Program version: 1.5.1, Extraction mode: UEFI
0x2EB9C: FormSet Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, Title: "Setup", Help: "Setup" { 0E A7 4A 10 59 7B 0D C0 58 41 87 FF F0 4D 63 96 A9 15 07 00 08 00 01 71 99 03 93 45 85 04 4B B4 5E 32 EB 83 26 04 0E }
0x2EBC3: 	Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Class, Class: 0x1 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 03 01 00 }
0x2EBD8: 	Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: SubClass, SubClass: 0x0 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 04 00 00 }
0x2EBED: 	DefaultStore DefaultId: 0x0, Name: "" { 5C 06 02 00 00 00 }
0x2EBF3: 	DefaultStore DefaultId: 0x1, Name: "" { 5C 06 02 00 01 00 }
0x2EBF9: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0xF101, Size: 0xCA7, Name: "Setup" { 24 1C 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 01 F1 A7 0C 53 65 74 75 70 00 }
0x2EC15: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0xF009, Size: 0x2, Name: "PlatformLang" { 24 23 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 09 F0 02 00 50 6C 61 74 66 6F 72 6D 4C 61 6E 67 00 }
0x2EC38: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0xF00A, Size: 0x2, Name: "PlatformLangCodes" { 24 28 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 0A F0 02 00 50 6C 61 74 66 6F 72 6D 4C 61 6E 67 43 6F 64 65 73 00 }
0x2EC60: 	VarStore Guid: E770BB69-BCB4-4D04-9E97-23FF9456FEAC, VarStoreId: 0xF000, Size: 0x1, Name: "SystemAccess" { 24 23 69 BB 70 E7 B4 BC 04 4D 9E 97 23 FF 94 56 FE AC 00 F0 01 00 53 79 73 74 65 6D 41 63 63 65 73 73 00 }
0x2EC83: 	VarStore Guid: 9CF0F18E-7C7D-49DE-B5AA-BBBAD6B21007, VarStoreId: 0xF002, Size: 0x2, Name: "AMICallback" { 24 22 8E F1 F0 9C 7D 7C DE 49 B5 AA BB BA D6 B2 10 07 02 F0 02 00 41 4D 49 43 61 6C 6C 62 61 63 6B 00 }
0x2ECA5: 	VarStore Guid: C811FA38-42C8-4579-A9BB-60E94EDDFB34, VarStoreId: 0xF013, Size: 0x51, Name: "AMITSESetup" { 24 22 38 FA 11 C8 C8 42 79 45 A9 BB 60 E9 4E DD FB 34 13 F0 51 00 41 4D 49 54 53 45 53 65 74 75 70 00 }
0x2ECC7: 	VarStore Guid: B4909CF3-7B93-4751-9BD8-5BA8220B9BB2, VarStoreId: 0xF003, Size: 0x2, Name: "BootManager" { 24 22 F3 9C 90 B4 93 7B 51 47 9B D8 5B A8 22 0B 9B B2 03 F0 02 00 42 6F 6F 74 4D 61 6E 61 67 65 72 00 }
0x2ECE9: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0xF005, Size: 0x2, Name: "Timeout" { 24 1E 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 05 F0 02 00 54 69 6D 65 6F 75 74 00 }
0x2ED07: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0xF006, Size: 0x2, Name: "BootOrder" { 24 20 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 06 F0 02 00 42 6F 6F 74 4F 72 64 65 72 00 }
0x2ED27: 	VarStore Guid: 19D96D3F-6A6A-47D2-B195-7B2432DA3BE2, VarStoreId: 0xF00D, Size: 0x11C, Name: "AddBootOption" { 24 24 3F 6D D9 19 6A 6A D2 47 B1 95 7B 24 32 DA 3B E2 0D F0 1C 01 41 64 64 42 6F 6F 74 4F 70 74 69 6F 6E 00 }
0x2ED4B: 	VarStore Guid: F6C73719-F34C-479C-B32F-277FCBBCFE4F, VarStoreId: 0xF00E, Size: 0x2, Name: "DelBootOption" { 24 24 19 37 C7 F6 4C F3 9C 47 B3 2F 27 7F CB BC FE 4F 0E F0 02 00 44 65 6C 42 6F 6F 74 4F 70 74 69 6F 6E 00 }
0x2ED6F: 	VarStore Guid: A56074DB-65FE-45F7-BD21-2D2BDD8E9652, VarStoreId: 0xF007, Size: 0x2, Name: "LegacyDev" { 24 20 DB 74 60 A5 FE 65 F7 45 BD 21 2D 2B DD 8E 96 52 07 F0 02 00 4C 65 67 61 63 79 44 65 76 00 }
0x2ED8F: 	VarStore Guid: A56074DB-65FE-45F7-BD21-2D2BDD8E9652, VarStoreId: 0xF016, Size: 0x2, Name: "LegacyGroup" { 24 22 DB 74 60 A5 FE 65 F7 45 BD 21 2D 2B DD 8E 96 52 16 F0 02 00 4C 65 67 61 63 79 47 72 6F 75 70 00 }
0x2EDB1: 	VarStore Guid: A56074DB-65FE-45F7-BD21-2D2BDD8E9652, VarStoreId: 0xF008, Size: 0x2, Name: "LegacyDevOrder" { 24 25 DB 74 60 A5 FE 65 F7 45 BD 21 2D 2B DD 8E 96 52 08 F0 02 00 4C 65 67 61 63 79 44 65 76 4F 72 64 65 72 00 }
0x2EDD6: 	VarStore Guid: 052E6EB0-F240-42C5-8309-45874545C6B4, VarStoreId: 0xF014, Size: 0x2, Name: "BootNowCount" { 24 23 B0 6E 2E 05 40 F2 C5 42 83 09 45 87 45 45 C6 B4 14 F0 02 00 42 6F 6F 74 4E 6F 77 43 6F 75 6E 74 00 }
0x2EDF9: 	VarStore Guid: C57AD6B7-0515-40A8-9D21-551652854E37, VarStoreId: 0xF00B, Size: 0x2, Name: "Shell" { 24 1C B7 D6 7A C5 15 05 A8 40 9D 21 55 16 52 85 4E 37 0B F0 02 00 53 68 65 6C 6C 00 }
0x2EE15: 	VarStore Guid: B08F97FF-E6E8-4193-A997-5E9E9B0ADB32, VarStoreId: 0x1, Size: 0x3C1, Name: "CpuSetup" { 24 1F FF 97 8F B0 E8 E6 93 41 A9 97 5E 9E 9B 0A DB 32 01 00 C1 03 43 70 75 53 65 74 75 70 00 }
0x2EE34: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x2, Size: 0x38, Name: "SetupCpuFeatures" { 24 27 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 02 00 38 00 53 65 74 75 70 43 70 75 46 65 61 74 75 72 65 73 00 }
0x2EE5B: 	VarStore Guid: B08F97FF-E6E8-4193-A997-5E9E9B0ADB32, VarStoreId: 0x3, Size: 0xB, Name: "CpuSetupVolatileData" { 24 2B FF 97 8F B0 E8 E6 93 41 A9 97 5E 9E 9B 0A DB 32 03 00 0B 00 43 70 75 53 65 74 75 70 56 6F 6C 61 74 69 6C 65 44 61 74 61 00 }
0x2EE86: 	VarStore Guid: 72C5E28C-7783-43A1-8767-FAD73FCCAFA4, VarStoreId: 0x4, Size: 0x578, Name: "SaSetup" { 24 1E 8C E2 C5 72 83 77 A1 43 87 67 FA D7 3F CC AF A4 04 00 78 05 53 61 53 65 74 75 70 00 }
0x2EEA4: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x5, Size: 0x6, Name: "TbtSetupVolatileData" { 24 2B 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 05 00 06 00 54 62 74 53 65 74 75 70 56 6F 6C 61 74 69 6C 65 44 61 74 61 00 }
0x2EECF: 	VarStore Guid: 4570B7F1-ADE8-4943-8DC3-406472842384, VarStoreId: 0x6, Size: 0x80F, Name: "PchSetup" { 24 1F F1 B7 70 45 E8 AD 43 49 8D C3 40 64 72 84 23 84 06 00 0F 08 50 63 68 53 65 74 75 70 00 }
0x2EEEE: 	VarStore Guid: A1D89A3A-4A90-429D-4365-1F64C3A29614, VarStoreId: 0x7, Size: 0x11, Name: "NhltEndpointsTableConfigurationVariable" { 24 3E 3A 9A D8 A1 90 4A 9D 42 43 65 1F 64 C3 A2 96 14 07 00 11 00 4E 68 6C 74 45 6E 64 70 6F 69 6E 74 73 54 61 62 6C 65 43 6F 6E 66 69 67 75 72 61 74 69 6F 6E 56 61 72 69 61 62 6C 65 00 }
0x2EF2C: 	VarStore Guid: 5432122D-D034-49D2-A6DE-65A829EB4C74, VarStoreId: 0x8, Size: 0x36, Name: "MeSetup" { 24 1E 2D 12 32 54 34 D0 D2 49 A6 DE 65 A8 29 EB 4C 74 08 00 36 00 4D 65 53 65 74 75 70 00 }
0x2EF4A: 	VarStore Guid: 5432122D-D034-49D2-A6DE-65A829EB4C74, VarStoreId: 0x9, Size: 0x12, Name: "MeSetupStorage" { 24 25 2D 12 32 54 34 D0 D2 49 A6 DE 65 A8 29 EB 4C 74 09 00 12 00 4D 65 53 65 74 75 70 53 74 6F 72 61 67 65 00 }
0x2EF6F: 	VarStore Guid: 1E785E1A-8EC4-49E4-8275-FBBDEDED18E7, VarStoreId: 0xA, Size: 0xF, Name: "BoardInfoSetup" { 24 25 1A 5E 78 1E C4 8E E4 49 82 75 FB BD ED ED 18 E7 0A 00 0F 00 42 6F 61 72 64 49 6E 66 6F 53 65 74 75 70 00 }
0x2EF94: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0xB, Size: 0x1, Name: "SetupAmtFeatures" { 24 27 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 0B 00 01 00 53 65 74 75 70 41 6D 74 46 65 61 74 75 72 65 73 00 }
0x2EFBB: 	VarStore Guid: 64192DCA-D034-49D2-A6DE-65A829EB4C74, VarStoreId: 0xC, Size: 0x8, Name: "IccAdvancedSetupDataVar" { 24 2E CA 2D 19 64 34 D0 D2 49 A6 DE 65 A8 29 EB 4C 74 0C 00 08 00 49 63 63 41 64 76 61 6E 63 65 64 53 65 74 75 70 44 61 74 61 56 61 72 00 }
0x2EFE9: 	VarStore Guid: AAF8E719-48F8-4099-A6F7-645FBD694C3D, VarStoreId: 0xD, Size: 0x7, Name: "SiSetup" { 24 1E 19 E7 F8 AA F8 48 99 40 A6 F7 64 5F BD 69 4C 3D 0D 00 07 00 53 69 53 65 74 75 70 00 }
0x2F007: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x28B7, Size: 0x4, Name: "DebugSetupVolatileData" { 24 2D 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 B7 28 04 00 44 65 62 75 67 53 65 74 75 70 56 6F 6C 61 74 69 6C 65 44 61 74 61 00 }
0x2F034: 	VarStore Guid: B5FBE0C8-A72A-408D-859C-0FD7537AAA5F, VarStoreId: 0x28B8, Size: 0xC, Name: "LpeSetup" { 24 1F C8 E0 FB B5 2A A7 8D 40 85 9C 0F D7 53 7A AA 5F B8 28 0C 00 4C 70 65 53 65 74 75 70 00 }
0x2F053: 	VarStore Guid: DE0A5E74-4E3E-3D96-A440-2C96ECBD3C97, VarStoreId: 0xE, Size: 0x11, Name: "DebugConfigData" { 24 26 74 5E 0A DE 3E 4E 96 3D A4 40 2C 96 EC BD 3C 97 0E 00 11 00 44 65 62 75 67 43 6F 6E 66 69 67 44 61 74 61 00 }
0x2F079: 	VarStore Guid: 279B9A61-F654-49E3-A252-A0B76B7C3865, VarStoreId: 0xF, Size: 0x3, Name: "TerminalPortsEnableVar" { 24 2D 61 9A 9B 27 54 F6 E3 49 A2 52 A0 B7 6B 7C 38 65 0F 00 03 00 54 65 72 6D 69 6E 61 6C 50 6F 72 74 73 45 6E 61 62 6C 65 56 61 72 00 }
0x2F0A6: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x10, Size: 0xE, Name: "NBPlatformData" { 24 25 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 10 00 0E 00 4E 42 50 6C 61 74 66 6F 72 6D 44 61 74 61 00 }
0x2F0CB: 	VarStore Guid: C61C31A3-CB5D-46DD-9FE5-8A82BBC72483, VarStoreId: 0x11, Size: 0x5, Name: "AmiWrapperSetup" { 24 26 A3 31 1C C6 5D CB DD 46 9F E5 8A 82 BB C7 24 83 11 00 05 00 41 6D 69 57 72 61 70 70 65 72 53 65 74 75 70 00 }
0x2F0F1: 	VarStore Guid: C0B4FB05-15E5-4588-9FE9-B3D39C067715, VarStoreId: 0x12, Size: 0x2, Name: "DriverManager" { 24 24 05 FB B4 C0 E5 15 88 45 9F E9 B3 D3 9C 06 77 15 12 00 02 00 44 72 69 76 65 72 4D 61 6E 61 67 65 72 00 }
0x2F115: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x13, Size: 0x2, Name: "DriverOrder" { 24 22 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 13 00 02 00 44 72 69 76 65 72 4F 72 64 65 72 00 }
0x2F137: 	VarStore Guid: C143929C-BF5D-423B-999B-0F2DD2B61FF7, VarStoreId: 0x14, Size: 0x2, Name: "AmiGopPolicySetupData" { 24 2C 9C 92 43 C1 5D BF 3B 42 99 9B 0F 2D D2 B6 1F F7 14 00 02 00 41 6D 69 47 6F 70 50 6F 6C 69 63 79 53 65 74 75 70 44 61 74 61 00 }
0x2F163: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x15, Size: 0x2, Name: "NBGopPlatformData" { 24 28 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 15 00 02 00 4E 42 47 6F 70 50 6C 61 74 66 6F 72 6D 44 61 74 61 00 }
0x2F18B: 	VarStore Guid: 6B0CC1BC-910F-411E-B6CB-0E314D0BB8C1, VarStoreId: 0x290A, Size: 0x1, Name: "SioSetupData" { 24 23 BC C1 0C 6B 0F 91 1E 41 B6 CB 0E 31 4D 0B B8 C1 0A 29 01 00 53 69 6F 53 65 74 75 70 44 61 74 61 00 }
0x2F1AE: 	VarStoreEfi Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x16, Attributes: 0x2, Size: 0x2, Name: "UsbMassDevNum" { 26 28 16 00 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 02 00 00 00 02 00 55 73 62 4D 61 73 73 44 65 76 4E 75 6D 00 }
0x2F1D6: 	VarStoreEfi Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x17, Attributes: 0x2, Size: 0x20, Name: "UsbMassDevValid" { 26 2A 17 00 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 02 00 00 00 20 00 55 73 62 4D 61 73 73 44 65 76 56 61 6C 69 64 00 }
0x2F200: 	VarStoreEfi Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x18, Attributes: 0x2, Size: 0x4, Name: "UsbControllerNum" { 26 2B 18 00 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 02 00 00 00 04 00 55 73 62 43 6F 6E 74 72 6F 6C 6C 65 72 4E 75 6D 00 }
0x2F22B: 	VarStoreEfi Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x19, Attributes: 0x3, Size: 0x31, Name: "UsbSupport" { 26 25 19 00 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 03 00 00 00 31 00 55 73 62 53 75 70 70 6F 72 74 00 }
0x2F250: 	VarStore Guid: D1405D16-7AFC-4695-BB12-41459D3695A2, VarStoreId: 0x1A, Size: 0x8, Name: "NetworkStackVar" { 24 26 16 5D 40 D1 FC 7A 95 46 BB 12 41 45 9D 36 95 A2 1A 00 08 00 4E 65 74 77 6F 72 6B 53 74 61 63 6B 56 61 72 00 }
0x2F276: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x29D3, Size: 0x52, Name: "SdioDevConfiguration" { 24 2B 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 D3 29 52 00 53 64 69 6F 44 65 76 43 6F 6E 66 69 67 75 72 61 74 69 6F 6E 00 }
0x2F2A1: 	VarStore Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, VarStoreId: 0x1B, Size: 0x7, Name: "SecureBootSetup" { 24 26 4A 10 59 7B 0D C0 58 41 87 FF F0 4D 63 96 A9 15 1B 00 07 00 53 65 63 75 72 65 42 6F 6F 74 53 65 74 75 70 00 }
0x2F2C7: 	VarStore Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, VarStoreId: 0x1C, Size: 0x6, Name: "SecureVarPresent" { 24 27 4A 10 59 7B 0D C0 58 41 87 FF F0 4D 63 96 A9 15 1C 00 06 00 53 65 63 75 72 65 56 61 72 50 72 65 73 65 6E 74 00 }
0x2F2EE: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x1D, Size: 0x1, Name: "VendorKeys" { 24 21 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 1D 00 01 00 56 65 6E 64 6F 72 4B 65 79 73 00 }
0x2F30F: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x1E, Size: 0x1, Name: "SetupMode" { 24 20 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 1E 00 01 00 53 65 74 75 70 4D 6F 64 65 00 }
0x2F32F: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x1F, Size: 0x1, Name: "SecureBoot" { 24 21 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 1F 00 01 00 53 65 63 75 72 65 42 6F 6F 74 00 }
0x2F350: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x20, Size: 0x1, Name: "AuditMode" { 24 20 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 20 00 01 00 41 75 64 69 74 4D 6F 64 65 00 }
0x2F370: 	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x21, Size: 0x1, Name: "DeployedMode" { 24 23 61 DF E4 8B CA 93 D2 11 AA 0D 00 E0 98 03 2B 8C 21 00 01 00 44 65 70 6C 6F 79 65 64 4D 6F 64 65 00 }
0x2F393: 	VarStore Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, VarStoreId: 0x22, Size: 0x1, Name: "AuthVarPreBootPhase" { 24 2A 4A 10 59 7B 0D C0 58 41 87 FF F0 4D 63 96 A9 15 22 00 01 00 41 75 74 68 56 61 72 50 72 65 42 6F 6F 74 50 68 61 73 65 00 }
0x2F3BD: 	VarStore Guid: 2798F49D-F760-480B-8055-916940C27740, VarStoreId: 0xDDDF, Size: 0x8C, Name: "TcgStorageDynamicSetupVar" { 24 30 9D F4 98 27 60 F7 0B 48 80 55 91 69 40 C2 77 40 DF DD 8C 00 54 63 67 53 74 6F 72 61 67 65 44 79 6E 61 6D 69 63 53 65 74 75 70 56 61 72 00 }
0x2F3ED: 	VarStore Guid: B63BF800-F267-4F55-9217-E97FB3B69846, VarStoreId: 0x23, Size: 0x2, Name: "DynamicPageCount" { 24 27 00 F8 3B B6 67 F2 55 4F 92 17 E9 7F B3 B6 98 46 23 00 02 00 44 79 6E 61 6D 69 63 50 61 67 65 43 6F 75 6E 74 00 }
0x2F414: 	VarStore Guid: 0885F288-418C-4BE1-A6AF-8BAD61DA08FE, VarStoreId: 0x24, Size: 0x2, Name: "DriverHlthEnable" { 24 27 88 F2 85 08 8C 41 E1 4B A6 AF 8B AD 61 DA 08 FE 24 00 02 00 44 72 69 76 65 72 48 6C 74 68 45 6E 61 62 6C 65 00 }
0x2F43B: 	VarStore Guid: 7459A7D4-6533-4480-BBA7-79E25A4443C9, VarStoreId: 0x25, Size: 0x2, Name: "DriverHealthCount" { 24 28 D4 A7 59 74 33 65 80 44 BB A7 79 E2 5A 44 43 C9 25 00 02 00 44 72 69 76 65 72 48 65 61 6C 74 68 43 6F 75 6E 74 00 }
0x2F463: 	VarStore Guid: 58279C2D-FB19-466E-B42E-CD437016DC25, VarStoreId: 0x26, Size: 0x2, Name: "DrvHealthCtrlCnt" { 24 27 2D 9C 27 58 19 FB 6E 46 B4 2E CD 43 70 16 DC 25 26 00 02 00 44 72 76 48 65 61 6C 74 68 43 74 72 6C 43 6E 74 00 }
0x2F48A: 	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x27, Size: 0x6D, Name: "SetupVolatileData" { 24 28 43 D6 87 EC A4 EB B5 4B A1 E5 3F 3E 36 B2 0D A9 27 00 6D 00 53 65 74 75 70 56 6F 6C 61 74 69 6C 65 44 61 74 61 00 }
0x2F4B2: 	Form FormId: 0x2710, Title: "Setup" { 01 86 10 27 07 00 }
0x2F4B8: 		Ref Prompt: "Main", Help: "", QuestionFlags: 0x0, QuestionId: 0x1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2717 { 0F 0F 09 00 02 00 01 00 00 00 FF FF 00 17 27 }
0x2F4C7: 		Ref Prompt: "Advanced", Help: "", QuestionFlags: 0x0, QuestionId: 0x2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2718 { 0F 0F 1E 00 02 00 02 00 00 00 FF FF 00 18 27 }
0x2F4D6: 		Ref Prompt: "Chipset", Help: "", QuestionFlags: 0x0, QuestionId: 0x3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2719 { 0F 0F 1F 00 02 00 03 00 00 00 FF FF 00 19 27 }
0x2F4E5: 		Ref Prompt: "Security", Help: "", QuestionFlags: 0x0, QuestionId: 0x4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271A { 0F 0F 3B 00 02 00 04 00 00 00 FF FF 00 1A 27 }
0x2F4F4: 		Ref Prompt: "Boot", Help: "", QuestionFlags: 0x0, QuestionId: 0x5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271B { 0F 0F 20 00 02 00 05 00 00 00 FF FF 00 1B 27 }
0x2F503: 		Ref Prompt: "Save & Exit", Help: "", QuestionFlags: 0x0, QuestionId: 0x6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 4E 00 02 00 06 00 00 00 FF FF 00 1C 27 }
0x2F512: 	End  { 29 02 }
0x2F514: 	Form FormId: 0x2711, Title: "Main" { 01 86 11 27 09 00 }
0x2F51A: 		Subtitle Prompt: "BIOS Information", Help: "", Flags: 0x0 { 02 87 0C 00 00 00 00 }
0x2F521: 		End  { 29 02 }
0x2F523: 		Text Prompt: "Project Name", Help: "", Text: "N/A" { 03 08 0B 23 02 00 0C 23 }
0x2F52B: 		Text Prompt: "BIOS FW Version", Help: "", Text: "N/A" { 03 08 0D 23 02 00 0E 23 }
0x2F533: 		Text Prompt: "Build Date and Time", Help: "", Text: "N/A" { 03 08 15 00 02 00 16 00 }
0x2F53B: 		Text Prompt: "EC FW Version", Help: "", Text: "N/A" { 03 08 0F 23 02 00 10 23 }
0x2F543: 		Text Prompt: "Build Version", Help: "", Text: "N/A" { 03 08 11 23 02 00 12 23 }
0x2F54B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F552: 		End  { 29 02 }
0x2F554: 		Subtitle Prompt: "Processor Information", Help: "", Flags: 0x0 { 02 87 5A 1B 00 00 00 }
0x2F55B: 		End  { 29 02 }
0x2F55D: 		Subtitle Prompt: "N/A", Help: "", Flags: 0x0 { 02 87 59 1B 00 00 00 }
0x2F564: 		End  { 29 02 }
0x2F566: 		Subtitle Prompt: "N/A", Help: "", Flags: 0x0 { 02 87 5D 1B 00 00 00 }
0x2F56D: 		End  { 29 02 }
0x2F56F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F576: 		End  { 29 02 }
0x2F578: 		Text Prompt: "ME FW Version", Help: "", Text: "N/A" { 03 08 89 1A 02 00 8A 1A }
0x2F580: 		Text Prompt: "ME Firmware SKU", Help: "", Text: "N/A" { 03 08 C0 19 02 00 C1 19 }
0x2F588: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F58F: 		End  { 29 02 }
0x2F591: 		SuppressIf  { 0A 82 }
0x2F593: 			EqIdVal QuestionId: 0x122E, Value: 0xFFFF { 12 06 2E 12 FF FF }
0x2F599: 			OneOf Prompt: "System Language", Help: "Choose the system default language", QuestionFlags: 0x0, QuestionId: 0x7, VarStoreId: 0xF009, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0 { 05 94 0B 00 0A 00 07 00 09 F0 00 00 00 11 00 00 01 00 00 00 }
0x2F5AD: 				OneOfOption Option: "" Value: 0 { 09 08 02 00 01 01 00 00 }
0x2F5B5: 				OneOfOption Option: "" Value: 1 { 09 08 02 00 01 01 01 00 }
0x2F5BD: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x2F5C4: 				Default DefaultId: 0x1 Value: 0 { 5B 07 01 00 01 00 00 }
0x2F5CB: 			End  { 29 02 }
0x2F5CD: 		End  { 29 02 }
0x2F5CF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F5D6: 		End  { 29 02 }
0x2F5D8: 		Date Prompt: "System Date", Help: "Set the Date. Use Tab to switch between Date elements.

Default Ranges: 

Year: 1998-9999 

Months: 1-12 

Days: Dependent on month

Range of Years may vary.", QuestionFlags: 0x0, QuestionId: 0x8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, Flags: 0x10 { 1A 8E 17 00 18 00 08 00 00 00 FF FF 00 10 }
0x2F5E6: 			Default DefaultId: 0x0 Value: 2014-01-01 { 5B 09 00 00 06 DE 07 01 01 }
0x2F5EF: 		End  { 29 02 }
0x2F5F1: 		Time Prompt: "System Time", Help: "Set the Time. Use Tab to switch between Time elements.", QuestionFlags: 0x0, QuestionId: 0x9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, Flags: 0x10 { 1B 8E 19 00 1A 00 09 00 00 00 FF FF 00 10 }
0x2F5FF: 			Default DefaultId: 0x0 Value: 00:00:00 { 5B 08 00 00 05 00 00 00 }
0x2F607: 		End  { 29 02 }
0x2F609: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F610: 		End  { 29 02 }
0x2F612: 		SuppressIf  { 0A 82 }
0x2F614: 			EqIdVal QuestionId: 0x110A, Value: 0x0 { 12 06 0A 11 00 00 }
0x2F61A: 			Text Prompt: "Access Level", Help: "", Text: "User" { 03 08 1B 00 02 00 1C 00 }
0x2F622: 		End  { 29 02 }
0x2F624: 		SuppressIf  { 0A 82 }
0x2F626: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x2F62C: 			Text Prompt: "Access Level", Help: "", Text: "Administrator" { 03 08 1B 00 02 00 1D 00 }
0x2F634: 		End  { 29 02 }
0x2F636: 	End  { 29 02 }
0x2F638: 	Form FormId: 0x2712, Title: "Advanced" { 01 86 12 27 1E 00 }
0x2F63E: 		SuppressIf  { 0A 82 }
0x2F640: 			EqIdValList QuestionId: 0x1229, Values: [65535] { 14 08 29 12 01 00 FF FF }
0x2F648: 			Ref Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2718 { 0F 0F 02 00 02 00 0A 00 00 00 FF FF 00 18 27 }
0x2F657: 		End  { 29 02 }
0x2F659: 		SuppressIf  { 0A 82 }
0x2F65B: 			EqIdVal QuestionId: 0x122D, Value: 0x1 { 12 06 2D 12 01 00 }
0x2F661: 			SuppressIf  { 0A 82 }
0x2F663: 				EqIdVal QuestionId: 0x122C, Value: 0x1 { 12 86 2C 12 01 00 }
0x2F669: 					EqIdVal QuestionId: 0x122B, Value: 0x1 { 12 06 2B 12 01 00 }
0x2F66F: 					Or  { 16 02 }
0x2F671: 				End  { 29 02 }
0x2F673: 				Ref Prompt: "Trusted Computing", Help: "Trusted Computing Settings", QuestionFlags: 0x0, QuestionId: 0xB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C2 { 0F 0F 87 22 88 22 0B 00 00 00 FF FF 00 C2 28 }
0x2F682: 			End  { 29 02 }
0x2F684: 			SuppressIf  { 0A 82 }
0x2F686: 				EqIdVal QuestionId: 0x122C, Value: 0x0 { 12 86 2C 12 00 00 }
0x2F68C: 					EqIdVal QuestionId: 0x122B, Value: 0x1 { 12 06 2B 12 01 00 }
0x2F692: 					Or  { 16 02 }
0x2F694: 				End  { 29 02 }
0x2F696: 				Ref Prompt: "Trusted Computing", Help: "Trusted Computing Settings", QuestionFlags: 0x0, QuestionId: 0xC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C3 { 0F 0F 87 22 88 22 0C 00 00 00 FF FF 00 C3 28 }
0x2F6A5: 			End  { 29 02 }
0x2F6A7: 			SuppressIf  { 0A 82 }
0x2F6A9: 				EqIdVal QuestionId: 0x122B, Value: 0x0 { 12 06 2B 12 00 00 }
0x2F6AF: 				Ref Prompt: "Trusted Computing", Help: "Trusted Computing Settings", QuestionFlags: 0x0, QuestionId: 0xD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C1 { 0F 0F 87 22 88 22 0D 00 00 00 FF FF 00 C1 28 }
0x2F6BE: 			End  { 29 02 }
0x2F6C0: 		End  { 29 02 }
0x2F6C2: 		Ref Prompt: "Onboard Device Configuration", Help: "Enable or disable onboard device. Command & Control can override this setting.", QuestionFlags: 0x0, QuestionId: 0xE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2AD8 { 0F 0F 45 1C 1C 23 0E 00 00 00 FF FF 00 D8 2A }
0x2F6D1: 		Ref Prompt: "SATA Configuration", Help: "SATA Device Options Settings", QuestionFlags: 0x0, QuestionId: 0xF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2AD9 { 0F 0F 99 16 9A 16 0F 00 00 00 FF FF 00 D9 2A }
0x2F6E0: 		Ref Prompt: "NVMe Configuration", Help: "NVMe Device Options Settings", QuestionFlags: 0x0, QuestionId: 0x10, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x1, RefQuestionId: 0x0, FormSetGuid: 5E39CF2E-6712-45AB-84C4-35D3C6A3686D { 0F 21 EE 21 EF 21 10 00 00 00 FF FF 00 01 00 00 00 2E CF 39 5E 12 67 AB 45 84 C4 35 D3 C6 A3 68 6D }
0x2F701: 		Ref Prompt: "USB Configuration", Help: "USB Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x11, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2ADA { 0F 0F 49 21 4A 21 11 00 00 00 FF FF 00 DA 2A }
0x2F710: 		OneOf Prompt: "Switchable Graphics device.", Help: "Switchable which of Graphics device to NVIDIA Discrete Graphics Or Intel Graphics With NVIDIA Optimus Technology.", QuestionFlags: 0x14, QuestionId: 0x2AD6, VarStoreId: 0xF101, VarOffset: 0xCA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 3B 23 3C 23 D6 2A 01 F1 A4 0C 14 10 00 02 00 }
0x2F721: 			OneOfOption Option: "Discrete" Value: 1 { 09 07 19 20 00 00 01 }
0x2F728: 			OneOfOption Option: "MSHybrid" Value: 2 { 09 07 1A 20 00 00 02 }
0x2F72F: 			OneOfOption Option: "Dynamic" Value: 0, Default, MfgDefault { 09 07 1B 20 30 00 00 }
0x2F736: 		End  { 29 02 }
0x2F738: 		OneOf Prompt: "Thunderbolt 5V Power Switch", Help: "Enable or Disable Thunderbolt 5 Voltage Power", QuestionFlags: 0x14, QuestionId: 0x2AD7, VarStoreId: 0xF101, VarOffset: 0xCA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 13 23 14 23 D7 2A 01 F1 A5 0C 14 10 00 01 00 }
0x2F749: 			OneOfOption Option: "ENABLED" Value: 1 { 09 07 15 23 00 00 01 }
0x2F750: 			OneOfOption Option: "DISABLED" Value: 0, Default, MfgDefault { 09 07 16 23 30 00 00 }
0x2F757: 		End  { 29 02 }
0x2F759: 		OneOf Prompt: "Network Stack", Help: "Enable/Disable UEFI Network Stack", QuestionFlags: 0x10, QuestionId: 0x12, VarStoreId: 0x1A, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 21 AA 21 12 00 1A 00 00 00 10 10 00 01 00 }
0x2F76A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x2F771: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x2F778: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x2F77E: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x2F784: 		End  { 29 02 }
0x2F786: 		SuppressIf  { 0A 82 }
0x2F788: 			EqIdVal QuestionId: 0x12, Value: 0x0 { 12 06 12 00 00 00 }
0x2F78E: 			OneOf Prompt: "IPv4 PXE Support", Help: "Enable/Disable IPv4 PXE boot support. If disabled, IPv4 PXE boot support will not be available.", QuestionFlags: 0x10, QuestionId: 0x13, VarStoreId: 0x1A, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 21 AE 21 13 00 1A 00 01 00 10 10 00 01 00 }
0x2F79F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x2F7A6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x2F7AD: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x2F7B3: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x2F7B9: 			End  { 29 02 }
0x2F7BB: 		End  { 29 02 }
0x2F7BD: 		SuppressIf  { 0A 82 }
0x2F7BF: 			EqIdVal QuestionId: 0x12, Value: 0x0 { 12 06 12 00 00 00 }
0x2F7C5: 			OneOf Prompt: "IPv6 PXE Support", Help: "Enable/Disable IPv6 PXE boot support. If disabled, IPv6 PXE boot support will not be available.", QuestionFlags: 0x10, QuestionId: 0x14, VarStoreId: 0x1A, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AF 21 B0 21 14 00 1A 00 02 00 10 10 00 01 00 }
0x2F7D6: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x2F7DD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x2F7E4: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x2F7EA: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x2F7F0: 			End  { 29 02 }
0x2F7F2: 		End  { 29 02 }
0x2F7F4: 		SuppressIf  { 0A 82 }
0x2F7F6: 			EqIdVal QuestionId: 0x12, Value: 0x0 { 12 06 12 00 00 00 }
0x2F7FC: 			Numeric Prompt: "PXE boot wait time", Help: "Wait time in seconds to press ESC key to abort the PXE boot. Use either +/- or numeric keys to set the value.", QuestionFlags: 0x10, QuestionId: 0x15, VarStoreId: 0x1A, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x1 { 07 91 B3 21 B4 21 15 00 1A 00 04 00 10 10 00 05 01 }
0x2F80D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x2F813: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x2F819: 			End  { 29 02 }
0x2F81B: 		End  { 29 02 }
0x2F81D: 		SuppressIf  { 0A 82 }
0x2F81F: 			EqIdVal QuestionId: 0x12, Value: 0x0 { 12 06 12 00 00 00 }
0x2F825: 			Numeric Prompt: "Media detect count", Help: "Number of times the presence of media will be checked. Use either +/- or numeric keys to set the value.", QuestionFlags: 0x10, QuestionId: 0x16, VarStoreId: 0x1A, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 B5 21 B6 21 16 00 1A 00 05 00 10 10 01 32 01 }
0x2F836: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x2F83C: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x2F842: 			End  { 29 02 }
0x2F844: 		End  { 29 02 }
0x2F846: 	End  { 29 02 }
0x2F848: 	Form FormId: 0x2AD8, Title: "Onboard Device Configuration" { 01 86 D8 2A 45 1C }
0x2F84E: 		Subtitle Prompt: "Onboard Device Configuration", Help: "", Flags: 0x0 { 02 87 45 1C 00 00 00 }
0x2F855: 		End  { 29 02 }
0x2F857: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F85E: 		End  { 29 02 }
0x2F860: 		OneOf Prompt: "Wireless Lan", Help: "Enable or disable onboard device. Command & Control can override this setting.", QuestionFlags: 0x10, QuestionId: 0x17, VarStoreId: 0xF101, VarOffset: 0xC9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1D 23 1C 23 17 00 01 F1 9E 0C 10 10 00 01 00 }
0x2F871: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x2F878: 			OneOfOption Option: "By Command & Control" Value: 0 { 09 07 1E 23 00 00 00 }
0x2F87F: 		End  { 29 02 }
0x2F881: 		OneOf Prompt: "RTC SUPPORT", Help: "Enable or disable S4/S5 RTC wake up.", QuestionFlags: 0x10, QuestionId: 0x18, VarStoreId: 0xF101, VarOffset: 0xC9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1F 23 20 23 18 00 01 F1 9F 0C 10 10 00 01 00 }
0x2F892: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x2F899: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x2F8A0: 		End  { 29 02 }
0x2F8A2: 		OneOf Prompt: "Wake on LAN Enable", Help: "Enable/Disable integrated LAN to wake the system.", QuestionFlags: 0x10, QuestionId: 0x19, VarStoreId: 0x6, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 11 33 11 19 00 06 00 0C 00 10 10 00 01 00 }
0x2F8B3: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x2F8BA: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x2F8C1: 		End  { 29 02 }
0x2F8C3: 		OneOf Prompt: "Webcam", Help: "Enable or disable onboard device. Command & Control can override this setting.", QuestionFlags: 0x10, QuestionId: 0x1A, VarStoreId: 0xF101, VarOffset: 0xCA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 21 23 1C 23 1A 00 01 F1 A0 0C 10 10 00 01 00 }
0x2F8D4: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x2F8DB: 			OneOfOption Option: "By Command & Control" Value: 0 { 09 07 1E 23 00 00 00 }
0x2F8E2: 		End  { 29 02 }
0x2F8E4: 		OneOf Prompt: "Hyper-Threading", Help: "Enable or Disable Hyper-Threading Technology.", QuestionFlags: 0x10, QuestionId: 0x1B, VarStoreId: 0x1, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 04 93 04 1B 00 01 00 05 00 10 10 00 01 00 }
0x2F8F5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x2F8FC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x2F903: 		End  { 29 02 }
0x2F905: 		OneOf Prompt: "Intel (VMX) Virtualization Technology", Help: "When enabled, a VMM can utilize the additional hardware capabilities provided by Vanderpool Technology.", QuestionFlags: 0x10, QuestionId: 0x1C, VarStoreId: 0x1, VarOffset: 0xB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 04 BC 04 1C 00 01 00 B9 00 10 10 00 01 00 }
0x2F916: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x2F91D: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x2F924: 		End  { 29 02 }
0x2F926: 		SuppressIf  { 0A 82 }
0x2F928: 			True  { 46 02 }
0x2F92A: 			OneOf Prompt: "Bluetooth", Help: "Enable or disable onboard device. Command & Control can override this setting.", QuestionFlags: 0x10, QuestionId: 0x1D, VarStoreId: 0xF101, VarOffset: 0xCA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 23 1C 23 1D 00 01 F1 A1 0C 10 10 00 01 00 }
0x2F93B: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x2F942: 				OneOfOption Option: "By Command & Control" Value: 0 { 09 07 1E 23 00 00 00 }
0x2F949: 			End  { 29 02 }
0x2F94B: 		End  { 29 02 }
0x2F94D: 		SuppressIf  { 0A 82 }
0x2F94F: 			True  { 46 02 }
0x2F951: 			OneOf Prompt: "Keyboard Language", Help: "Choose the system keyboard language 
 
 - English, Chinese. 
 - European, Korean. 
 - Japanese.", QuestionFlags: 0x10, QuestionId: 0x1E, VarStoreId: 0xF101, VarOffset: 0xCA2, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0 { 05 91 25 23 26 23 1E 00 01 F1 A2 0C 10 10 01 03 00 }
0x2F962: 				OneOfOption Option: "English" Value: 1, Default, MfgDefault { 09 07 27 23 30 00 01 }
0x2F969: 				OneOfOption Option: "European" Value: 2 { 09 07 28 23 00 00 02 }
0x2F970: 				OneOfOption Option: "Japanese" Value: 3 { 09 07 29 23 00 00 03 }
0x2F977: 			End  { 29 02 }
0x2F979: 		End  { 29 02 }
0x2F97B: 	End  { 29 02 }
0x2F97D: 	Form FormId: 0x2AD9, Title: "SATA Configuration" { 01 86 D9 2A 99 16 }
0x2F983: 		Subtitle Prompt: "SATA Configuration", Help: "", Flags: 0x0 { 02 87 99 16 00 00 00 }
0x2F98A: 		End  { 29 02 }
0x2F98C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F993: 		End  { 29 02 }
0x2F995: 		OneOf Prompt: "Aggressive LPM Support", Help: "Enable PCH to aggressively enter link power state.", QuestionFlags: 0x10, QuestionId: 0x1F, VarStoreId: 0x6, VarOffset: 0x92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 16 FB 16 1F 00 06 00 92 00 10 10 00 01 00 }
0x2F9A6: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x2F9AD: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x2F9B4: 		End  { 29 02 }
0x2F9B6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2F9BD: 		End  { 29 02 }
0x2F9BF: 		Text Prompt: "Serial ATA Port 1", Help: "", Text: "Empty" { 03 08 CF 16 C9 07 D0 16 }
0x2F9C7: 		Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 3E 17 }
0x2F9CF: 		Text Prompt: "Serial ATA Port 4", Help: "", Text: "Empty" { 03 08 D5 16 C9 07 D6 16 }
0x2F9D7: 		Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 41 17 }
0x2F9DF: 		Text Prompt: "Serial ATA Port 5", Help: "", Text: "Empty" { 03 08 D7 16 C9 07 D8 16 }
0x2F9E7: 		Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 42 17 }
0x2F9EF: 	End  { 29 02 }
0x2F9F1: 	Form FormId: 0x2ADA, Title: "USB Configuration" { 01 86 DA 2A 49 21 }
0x2F9F7: 		Subtitle Prompt: "USB Configuration", Help: "", Flags: 0x0 { 02 87 49 21 00 00 00 }
0x2F9FE: 		End  { 29 02 }
0x2FA00: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FA07: 		End  { 29 02 }
0x2FA09: 		Text Prompt: "USB Module Version", Help: "", Text: "00.00" { 03 08 7D 21 02 00 7C 21 }
0x2FA11: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FA18: 		End  { 29 02 }
0x2FA1A: 		Text Prompt: "USB Controllers:", Help: "", Text: "" { 03 08 51 21 02 00 00 00 }
0x2FA22: 		Subtitle Prompt: "N/A", Help: "", Flags: 0x0 { 02 87 52 21 00 00 00 }
0x2FA29: 		End  { 29 02 }
0x2FA2B: 		Text Prompt: "USB Devices:", Help: "", Text: "" { 03 08 53 21 02 00 00 00 }
0x2FA33: 		Subtitle Prompt: "N/A", Help: "", Flags: 0x0 { 02 87 54 21 00 00 00 }
0x2FA3A: 		End  { 29 02 }
0x2FA3C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FA43: 		End  { 29 02 }
0x2FA45: 		SuppressIf  { 0A 82 }
0x2FA47: 			EqIdId QuestionId: 0x576, OtherQuestionId: 0x576 { 13 06 76 05 76 05 }
0x2FA4D: 			GrayOutIf  { 19 82 }
0x2FA4F: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x2FA55: 				OneOf Prompt: "USB Support", Help: "USB Support Parameters", QuestionFlags: 0x10, QuestionId: 0x20, VarStoreId: 0x19, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4B 21 4C 21 20 00 19 00 00 00 10 10 00 01 00 }
0x2FA66: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 4E 21 00 00 00 }
0x2FA6D: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 4D 21 30 00 01 }
0x2FA74: 				End  { 29 02 }
0x2FA76: 			End  { 29 02 }
0x2FA78: 		End  { 29 02 }
0x2FA7A: 		SuppressIf  { 0A 82 }
0x2FA7C: 			EqIdVal QuestionId: 0x20, Value: 0x0 { 12 06 20 00 00 00 }
0x2FA82: 			GrayOutIf  { 19 82 }
0x2FA84: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x2FA8A: 				OneOf Prompt: "Legacy USB Support", Help: "Enables Legacy USB support. AUTO option disables legacy support if no USB devices are connected. DISABLE option will keep USB devices available only for EFI applications.", QuestionFlags: 0x10, QuestionId: 0x21, VarStoreId: 0x19, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 55 21 56 21 21 00 19 00 01 00 10 10 00 02 00 }
0x2FA9B: 					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 4D 21 30 00 00 }
0x2FAA2: 					OneOfOption Option: "Disabled" Value: 1 { 09 07 4E 21 00 00 01 }
0x2FAA9: 					OneOfOption Option: "Auto" Value: 2 { 09 07 4F 21 00 00 02 }
0x2FAB0: 				End  { 29 02 }
0x2FAB2: 			End  { 29 02 }
0x2FAB4: 		End  { 29 02 }
0x2FAB6: 	End  { 29 02 }
0x2FAB8: 	Form FormId: 0x2713, Title: "Chipset" { 01 86 13 27 1F 00 }
0x2FABE: 		Subtitle Prompt: "Memory Configuration", Help: "", Flags: 0x0 { 02 87 CD 07 00 00 00 }
0x2FAC5: 		End  { 29 02 }
0x2FAC7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FACE: 		End  { 29 02 }
0x2FAD0: 		Text Prompt: "DIMM#0", Help: "", Text: "" { 03 08 2A 23 02 00 02 00 }
0x2FAD8: 		SuppressIf  { 0A 82 }
0x2FADA: 			EqIdVal QuestionId: 0x1186, Value: 0x0 { 12 06 86 11 00 00 }
0x2FAE0: 			Text Prompt: "Memory Frequency", Help: "Displays the Frequency of Memory", Text: "N/A" { 03 08 EA 07 E9 07 EB 07 }
0x2FAE8: 			Text Prompt: "MC 0 Ch 0 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F1 07 EF 07 01 08 }
0x2FAF0: 		End  { 29 02 }
0x2FAF2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FAF9: 		End  { 29 02 }
0x2FAFB: 		Text Prompt: "DIMM#1", Help: "", Text: "" { 03 08 2B 23 02 00 02 00 }
0x2FB03: 		SuppressIf  { 0A 82 }
0x2FB05: 			EqIdVal QuestionId: 0x117E, Value: 0x0 { 12 06 7E 11 00 00 }
0x2FB0B: 			Text Prompt: "Memory Frequency", Help: "Displays the Frequency of Memory", Text: "N/A" { 03 08 EA 07 E9 07 EB 07 }
0x2FB13: 			Text Prompt: "MC 1 Ch 0 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F9 07 EF 07 09 08 }
0x2FB1B: 		End  { 29 02 }
0x2FB1D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FB24: 		End  { 29 02 }
0x2FB26: 		Text Prompt: "Total Memory", Help: "Total Memory in the System.", Text: "N/A" { 03 08 75 1B 77 1B 76 1B }
0x2FB2E: 	End  { 29 02 }
0x2FB30: 	Form FormId: 0x2714, Title: "Security" { 01 86 14 27 3B 00 }
0x2FB36: 		Subtitle Prompt: "Password Description", Help: "", Flags: 0x0 { 02 87 3C 00 00 00 00 }
0x2FB3D: 		End  { 29 02 }
0x2FB3F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FB46: 		End  { 29 02 }
0x2FB48: 		Subtitle Prompt: "If ONLY the Administrator's password is set,", Help: "", Flags: 0x0 { 02 87 3D 00 00 00 00 }
0x2FB4F: 		End  { 29 02 }
0x2FB51: 		Subtitle Prompt: "then this only limits access to Setup and is", Help: "", Flags: 0x0 { 02 87 3E 00 00 00 00 }
0x2FB58: 		End  { 29 02 }
0x2FB5A: 		Subtitle Prompt: "only asked for when entering Setup.", Help: "", Flags: 0x0 { 02 87 3F 00 00 00 00 }
0x2FB61: 		End  { 29 02 }
0x2FB63: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FB6A: 		End  { 29 02 }
0x2FB6C: 		Subtitle Prompt: "The password length must be", Help: "", Flags: 0x0 { 02 87 44 00 00 00 00 }
0x2FB73: 		End  { 29 02 }
0x2FB75: 		Subtitle Prompt: "in the following range:", Help: "", Flags: 0x0 { 02 87 45 00 00 00 00 }
0x2FB7C: 		End  { 29 02 }
0x2FB7E: 		Text Prompt: "Minimum length", Help: "", Text: "N/A" { 03 08 46 00 02 00 47 00 }
0x2FB86: 		Text Prompt: "Maximum length", Help: "", Text: "N/A" { 03 08 48 00 02 00 49 00 }
0x2FB8E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FB95: 		End  { 29 02 }
0x2FB97: 		GrayOutIf  { 19 82 }
0x2FB99: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x2FB9F: 			Password Prompt: "Administrator Password", Help: "Set Administrator Password", QuestionFlags: 0x0, QuestionId: 0x22, VarStoreId: 0xF013, VarStoreInfo: 0x28, MinSize: 0x3, MaxSize: 0x14 { 08 91 4A 00 4B 00 22 00 13 F0 28 00 00 03 00 14 00 }
0x2FBB0: 			End  { 29 02 }
0x2FBB2: 		End  { 29 02 }
0x2FBB4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FBBB: 		End  { 29 02 }
0x2FBBD: 		SuppressIf  { 0A 82 }
0x2FBBF: 			EqIdVal QuestionId: 0x110D, Value: 0x1 { 12 86 0D 11 01 00 }
0x2FBC5: 				Not  { 17 02 }
0x2FBC7: 			End  { 29 02 }
0x2FBC9: 			Text Prompt: "System Mode", Help: "", Text: "Deployed" { 03 08 17 22 02 00 1A 22 }
0x2FBD1: 		End  { 29 02 }
0x2FBD3: 		SuppressIf  { 0A 82 }
0x2FBD5: 			EqIdVal QuestionId: 0x110C, Value: 0x1 { 12 86 0C 11 01 00 }
0x2FBDB: 				Not  { 17 02 }
0x2FBDD: 			End  { 29 02 }
0x2FBDF: 			Text Prompt: "System Mode", Help: "", Text: "Audit" { 03 08 17 22 02 00 19 22 }
0x2FBE7: 		End  { 29 02 }
0x2FBE9: 		SuppressIf  { 0A 82 }
0x2FBEB: 			EqIdVal QuestionId: 0x110D, Value: 0x1 { 12 86 0D 11 01 00 }
0x2FBF1: 				EqIdVal QuestionId: 0x110C, Value: 0x1 { 12 06 0C 11 01 00 }
0x2FBF7: 				Or  { 16 02 }
0x2FBF9: 				EqIdVal QuestionId: 0x110B, Value: 0x0 { 12 06 0B 11 00 00 }
0x2FBFF: 				Or  { 16 02 }
0x2FC01: 			End  { 29 02 }
0x2FC03: 			Text Prompt: "System Mode", Help: "", Text: "Setup" { 03 08 17 22 02 00 07 00 }
0x2FC0B: 		End  { 29 02 }
0x2FC0D: 		SuppressIf  { 0A 82 }
0x2FC0F: 			EqIdVal QuestionId: 0x110D, Value: 0x1 { 12 86 0D 11 01 00 }
0x2FC15: 				EqIdVal QuestionId: 0x110C, Value: 0x1 { 12 06 0C 11 01 00 }
0x2FC1B: 				Or  { 16 02 }
0x2FC1D: 				EqIdVal QuestionId: 0x110B, Value: 0x1 { 12 06 0B 11 01 00 }
0x2FC23: 				Or  { 16 02 }
0x2FC25: 			End  { 29 02 }
0x2FC27: 			Text Prompt: "System Mode", Help: "", Text: "User" { 03 08 17 22 02 00 18 22 }
0x2FC2F: 		End  { 29 02 }
0x2FC31: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FC38: 		End  { 29 02 }
0x2FC3A: 		SuppressIf  { 0A 82 }
0x2FC3C: 			EqIdVal QuestionId: 0x1108, Value: 0x0 { 12 86 08 11 00 00 }
0x2FC42: 				Not  { 17 02 }
0x2FC44: 			End  { 29 02 }
0x2FC46: 			Ref Prompt: "Enroll all Factory Default keys", Help: "Force System to User Mode.
Install factory default Secure Boot key databases", QuestionFlags: 0x14, QuestionId: 0x2ADB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2714 { 0F 0F 2D 23 2D 22 DB 2A 00 00 FF FF 14 14 27 }
0x2FC55: 		End  { 29 02 }
0x2FC57: 		SuppressIf  { 0A 82 }
0x2FC59: 			EqIdVal QuestionId: 0x1108, Value: 0x1 { 12 86 08 11 01 00 }
0x2FC5F: 				Not  { 17 02 }
0x2FC61: 			End  { 29 02 }
0x2FC63: 			Ref Prompt: "Delete all Secure Boot variables", Help: "Delete all Secure Boot key databases from NVRAM", QuestionFlags: 0x14, QuestionId: 0x2ADC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2714 { 0F 0F 2C 23 2B 22 DC 2A 00 00 FF FF 14 14 27 }
0x2FC72: 		End  { 29 02 }
0x2FC74: 	End  { 29 02 }
0x2FC76: 	Form FormId: 0x2715, Title: "Boot" { 01 86 15 27 20 00 }
0x2FC7C: 		Subtitle Prompt: "Boot Configuration", Help: "", Flags: 0x0 { 02 87 25 00 00 00 00 }
0x2FC83: 		End  { 29 02 }
0x2FC85: 		OneOf Prompt: "Bootup NumLock State", Help: "Select the keyboard NumLock state", QuestionFlags: 0x10, QuestionId: 0x23, VarStoreId: 0xF101, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 00 29 00 23 00 01 F1 00 00 10 10 00 01 00 }
0x2FC96: 			OneOfOption Option: "On" Value: 1 { 09 07 2A 00 00 00 01 }
0x2FC9D: 			OneOfOption Option: "Off" Value: 0 { 09 07 2B 00 00 00 00 }
0x2FCA4: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x2FCAA: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x2FCB0: 		End  { 29 02 }
0x2FCB2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FCB9: 		End  { 29 02 }
0x2FCBB: 		Subtitle Prompt: "Boot Option Priorities", Help: "", Flags: 0x0 { 02 87 2C 00 00 00 00 }
0x2FCC2: 		End  { 29 02 }
0x2FCC4: 		SuppressIf  { 0A 82 }
0x2FCC6: 			EqIdValList QuestionId: 0x1100, Values: [65535] { 14 08 00 11 01 00 FF FF }
0x2FCCE: 			OneOf Prompt: "Boot Option #%d", Help: "Sets the system boot order", QuestionFlags: 0x0, QuestionId: 0x24, VarStoreId: 0xF006, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0 { 05 94 2D 00 2F 00 24 00 06 F0 00 00 00 11 00 00 01 00 00 00 }
0x2FCE2: 				OneOfOption Option: "" Value: 0 { 09 08 02 00 01 01 00 00 }
0x2FCEA: 				OneOfOption Option: "" Value: 1 { 09 08 02 00 01 01 01 00 }
0x2FCF2: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x2FCF9: 				Default DefaultId: 0x1 Value: 0 { 5B 07 01 00 01 00 00 }
0x2FD00: 			End  { 29 02 }
0x2FD02: 		End  { 29 02 }
0x2FD04: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FD0B: 		End  { 29 02 }
0x2FD0D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FD14: 		End  { 29 02 }
0x2FD16: 		SuppressIf  { 0A 82 }
0x2FD18: 			EqIdValList QuestionId: 0x10FE, Values: [65535] { 14 08 FE 10 01 00 FF FF }
0x2FD20: 			Ref Prompt: "", Help: "Set the order of the legacy devices in this group", QuestionFlags: 0x0, QuestionId: 0x25, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C0 { 0F 0F 02 00 35 00 25 00 00 00 FF FF 00 C0 28 }
0x2FD2F: 		End  { 29 02 }
0x2FD31: 	End  { 29 02 }
0x2FD33: 	Form FormId: 0x2716, Title: "Save & Exit" { 01 86 16 27 4E 00 }
0x2FD39: 		Subtitle Prompt: "Save Options", Help: "", Flags: 0x0 { 02 87 57 00 00 00 00 }
0x2FD40: 		End  { 29 02 }
0x2FD42: 		SuppressIf  { 0A 82 }
0x2FD44: 			EqIdVal QuestionId: 0x10FC, Value: 0x9 { 12 06 FC 10 09 00 }
0x2FD4A: 			Ref Prompt: "Save Changes and Reset", Help: "Reset the system after saving the changes.", QuestionFlags: 0x0, QuestionId: 0x26, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716 { 0F 0F 53 00 54 00 26 00 00 00 FF FF 00 16 27 }
0x2FD59: 		End  { 29 02 }
0x2FD5B: 		SuppressIf  { 0A 82 }
0x2FD5D: 			EqIdVal QuestionId: 0x10FC, Value: 0xA { 12 06 FC 10 0A 00 }
0x2FD63: 			Ref Prompt: "Discard Changes and Reset", Help: "Reset system setup without saving any changes.", QuestionFlags: 0x0, QuestionId: 0x27, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716 { 0F 0F 55 00 56 00 27 00 00 00 FF FF 00 16 27 }
0x2FD72: 		End  { 29 02 }
0x2FD74: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FD7B: 		End  { 29 02 }
0x2FD7D: 		SuppressIf  { 0A 82 }
0x2FD7F: 			EqIdVal QuestionId: 0x10FC, Value: 0x3 { 12 06 FC 10 03 00 }
0x2FD85: 			Ref Prompt: "Save Changes", Help: "Save Changes done so far to any of the setup options.", QuestionFlags: 0x0, QuestionId: 0x28, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716 { 0F 0F 58 00 59 00 28 00 00 00 FF FF 00 16 27 }
0x2FD94: 		End  { 29 02 }
0x2FD96: 		SuppressIf  { 0A 82 }
0x2FD98: 			EqIdVal QuestionId: 0x10FC, Value: 0x4 { 12 06 FC 10 04 00 }
0x2FD9E: 			Ref Prompt: "Discard Changes", Help: "Discard Changes done so far to any of the setup options.", QuestionFlags: 0x0, QuestionId: 0x29, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716 { 0F 0F 5A 00 5B 00 29 00 00 00 FF FF 00 16 27 }
0x2FDAD: 		End  { 29 02 }
0x2FDAF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FDB6: 		End  { 29 02 }
0x2FDB8: 		Subtitle Prompt: "Default Options", Help: "", Flags: 0x0 { 02 87 5C 00 00 00 00 }
0x2FDBF: 		End  { 29 02 }
0x2FDC1: 		SuppressIf  { 0A 82 }
0x2FDC3: 			EqIdVal QuestionId: 0x10FC, Value: 0x5 { 12 06 FC 10 05 00 }
0x2FDC9: 			Ref Prompt: "Restore Defaults", Help: "Restore/Load Default values for all the setup options.", QuestionFlags: 0x0, QuestionId: 0x2A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716 { 0F 0F 5D 00 5E 00 2A 00 00 00 FF FF 00 16 27 }
0x2FDD8: 		End  { 29 02 }
0x2FDDA: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FDE1: 		End  { 29 02 }
0x2FDE3: 	End  { 29 02 }
0x2FDE5: 	Form FormId: 0x2717, Title: "Main" { 01 86 17 27 09 00 }
0x2FDEB: 		Subtitle Prompt: "BIOS Information", Help: "", Flags: 0x0 { 02 87 0C 00 00 00 00 }
0x2FDF2: 		End  { 29 02 }
0x2FDF4: 		Text Prompt: "BIOS Vendor", Help: "", Text: "N/A" { 03 08 0D 00 02 00 0E 00 }
0x2FDFC: 		Text Prompt: "Core Version", Help: "", Text: "N/A" { 03 08 0F 00 02 00 10 00 }
0x2FE04: 		Text Prompt: "Compliancy", Help: "", Text: "N/A" { 03 08 11 00 02 00 12 00 }
0x2FE0C: 		Text Prompt: "Project Version", Help: "", Text: "N/A" { 03 08 13 00 02 00 14 00 }
0x2FE14: 		Text Prompt: "Build Date and Time", Help: "", Text: "N/A" { 03 08 15 00 02 00 16 00 }
0x2FE1C: 		SuppressIf  { 0A 82 }
0x2FE1E: 			EqIdVal QuestionId: 0x110A, Value: 0x0 { 12 06 0A 11 00 00 }
0x2FE24: 			Text Prompt: "Access Level", Help: "", Text: "User" { 03 08 1B 00 02 00 1C 00 }
0x2FE2C: 		End  { 29 02 }
0x2FE2E: 		SuppressIf  { 0A 82 }
0x2FE30: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x2FE36: 			Text Prompt: "Access Level", Help: "", Text: "Administrator" { 03 08 1B 00 02 00 1D 00 }
0x2FE3E: 		End  { 29 02 }
0x2FE40: 		Text Prompt: "Silicon Version", Help: "", Text: "N/A" { 03 08 DA 1F 02 00 DB 1F }
0x2FE48: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FE4F: 		End  { 29 02 }
0x2FE51: 		Subtitle Prompt: "FSP Information", Help: "", Flags: 0x0 { 02 87 DC 1F 00 00 00 }
0x2FE58: 		End  { 29 02 }
0x2FE5A: 		Text Prompt: "FSP version", Help: "FSP version information", Text: "N/A" { 03 08 DE 1F DD 1F DF 1F }
0x2FE62: 		Text Prompt: "RC version", Help: "RC version information", Text: "N/A" { 03 08 E4 1F E3 1F E5 1F }
0x2FE6A: 		Text Prompt: "Build Date", Help: "Build Date information", Text: "N/A" { 03 08 E7 1F E6 1F E8 1F }
0x2FE72: 		Text Prompt: "FSP Mode", Help: "FSP mode information, API or Dispatch", Text: "N/A" { 03 08 E1 1F E0 1F E2 1F }
0x2FE7A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FE81: 		End  { 29 02 }
0x2FE83: 		Subtitle Prompt: "Board Information", Help: "", Flags: 0x0 { 02 87 4A 1B 00 00 00 }
0x2FE8A: 		End  { 29 02 }
0x2FE8C: 		Text Prompt: "Board Name", Help: "Displays the Board Name.", Text: "N/A" { 03 08 4F 1B 4E 1B 50 1B }
0x2FE94: 		Text Prompt: "Board ID", Help: "Displays the Board ID.", Text: "N/A" { 03 08 4C 1B 4B 1B 4D 1B }
0x2FE9C: 		Text Prompt: "Fab ID", Help: "Displays the Fab ID", Text: "N/A" { 03 08 52 1B 51 1B 53 1B }
0x2FEA4: 		Text Prompt: "LAN PHY Revision", Help: "Displays LAN PHY Revision.", Text: "N/A" { 03 08 55 1B 54 1B 56 1B }
0x2FEAC: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FEB3: 		End  { 29 02 }
0x2FEB5: 		Subtitle Prompt: "Processor Information", Help: "", Flags: 0x0 { 02 87 5A 1B 00 00 00 }
0x2FEBC: 		End  { 29 02 }
0x2FEBE: 		Text Prompt: "Name", Help: "Displays the Processor Details.", Text: "N/A" { 03 08 58 1B 57 1B 59 1B }
0x2FEC6: 		Text Prompt: "Type", Help: "Displays the Processor Type.", Text: "N/A" { 03 08 5C 1B 5B 1B 5D 1B }
0x2FECE: 		Text Prompt: "Speed", Help: "Displays the Processor Speed.", Text: "N/A" { 03 08 5E 1B 60 1B 5F 1B }
0x2FED6: 		Text Prompt: "ID", Help: "Displays the Processor ID.", Text: "N/A" { 03 08 4E 04 50 04 4F 04 }
0x2FEDE: 		Text Prompt: "Stepping", Help: "Displays the Processor Stepping.", Text: "Unknown" { 03 08 61 1B 63 1B 62 1B }
0x2FEE6: 		Text Prompt: "Package", Help: "Displays the Processor Package.", Text: "N/A" { 03 08 64 1B 66 1B 65 1B }
0x2FEEE: 		Text Prompt: "Number of Efficient-cores", Help: "Displays number of CPU cores.", Text: "xCore(s) / yThread(s)" { 03 08 6A 1B 6E 1B 6C 1B }
0x2FEF6: 		Text Prompt: "Number of Performance-cores", Help: "Displays number of CPU cores.", Text: "xCore(s) / yThread(s)" { 03 08 6B 1B 6E 1B 6D 1B }
0x2FEFE: 		Text Prompt: "Microcode Revision", Help: "CPU Microcode Revision", Text: "Not loaded" { 03 08 67 1B 69 1B 68 1B }
0x2FF06: 		Text Prompt: "GT Info", Help: "Processor GT Info. Only valid if SNB stepping is D0 or above.", Text: "Not Applicable" { 03 08 6F 1B 71 1B 70 1B }
0x2FF0E: 		Text Prompt: "eDRAM Size", Help: "eDRAM Size supported by the SKU", Text: "N/A" { 03 08 72 1B 74 1B 73 1B }
0x2FF16: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FF1D: 		End  { 29 02 }
0x2FF1F: 		SuppressIf  { 0A 82 }
0x2FF21: 			EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x2FF27: 			Text Prompt: "IGFX GOP Version", Help: "IGFX GOP Version", Text: "N/A" { 03 08 B0 1A AF 1A B1 1A }
0x2FF2F: 		End  { 29 02 }
0x2FF31: 		Text Prompt: "PCIe GEN4 Dekel FW Version", Help: "Dekel Firmware Version used by PCIe Gen4 PHY", Text: "N/A" { 03 08 A7 1A A6 1A A8 1A }
0x2FF39: 		Text Prompt: "PCIe GEN5 HS-Phy Recipe Version", Help: "HS-Phy Recipe Version used by PCIe Gen5 PHY", Text: "N/A" { 03 08 AA 1A A9 1A AB 1A }
0x2FF41: 		Text Prompt: "PCIe GEN5 HS-Phy FW Version", Help: "HS-Phy Firmware Version used by PCIe Gen5 PHY", Text: "N/A" { 03 08 AD 1A AC 1A AE 1A }
0x2FF49: 		Text Prompt: "Memory RC Version", Help: "Memory RC Version", Text: "N/A" { 03 08 E7 07 E6 07 E8 07 }
0x2FF51: 		Text Prompt: "Total Memory", Help: "Total Memory in the System.", Text: "N/A" { 03 08 75 1B 77 1B 76 1B }
0x2FF59: 		Text Prompt: "Memory Frequency", Help: "Displays the Frequency of Memory", Text: "N/A" { 03 08 EA 07 E9 07 EB 07 }
0x2FF61: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FF68: 		End  { 29 02 }
0x2FF6A: 		Subtitle Prompt: "PCH Information", Help: "", Flags: 0x0 { 02 87 78 1B 00 00 00 }
0x2FF71: 		End  { 29 02 }
0x2FF73: 		Text Prompt: "Name", Help: "PCH Name", Text: "UnKnown" { 03 08 60 1A 5F 1A 61 1A }
0x2FF7B: 		Text Prompt: "PCH SKU", Help: "PCH SKU", Text: "UnKnown" { 03 08 63 1A 62 1A 64 1A }
0x2FF83: 		Text Prompt: "Stepping", Help: "PCH Stepping", Text: "UnKnown" { 03 08 66 1A 65 1A 67 1A }
0x2FF8B: 		Text Prompt: "ChipsetInit Intel Module Rev", Help: "ChipsetInit Intel Module Rev", Text: "Unknown" { 03 08 7A 1A 79 1A 7B 1A }
0x2FF93: 		Text Prompt: "ChipsetInit OEM Module Rev", Help: "ChipsetInit OEM Module Rev", Text: "Unknown" { 03 08 7D 1A 7C 1A 7E 1A }
0x2FF9B: 		Text Prompt: "Package", Help: "PCH Package", Text: "N/A" { 03 08 69 1A 68 1A 6A 1A }
0x2FFA3: 		Text Prompt: "TXT Capability of Platform/PCH", Help: "Platform/PCH TXT capability", Text: "Not Supported" { 03 08 6E 1A 6D 1A 6F 1A }
0x2FFAB: 		Text Prompt: "Production Type", Help: "Platform Production Type", Text: "Not Supported" { 03 08 71 1A 70 1A 72 1A }
0x2FFB3: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x2FFBA: 		End  { 29 02 }
0x2FFBC: 		Text Prompt: "Dual Output Fast Read support", Help: "Dual Output Fast Read support", Text: "N/A" { 03 08 8F 1A 8E 1A 90 1A }
0x2FFC4: 		Text Prompt: "Read ID/Status Clock Freq", Help: "Read ID and Read Status Clock Frequency", Text: "N/A" { 03 08 92 1A 91 1A 93 1A }
0x2FFCC: 		Text Prompt: "Write and Erase Clock Freq", Help: "Write and Erase Clock Frequency ", Text: "N/A" { 03 08 95 1A 94 1A 96 1A }
0x2FFD4: 		Text Prompt: "Fast Read Clock Freq", Help: "Fast Read Clock Frequency", Text: "N/A" { 03 08 98 1A 97 1A 99 1A }
0x2FFDC: 		Text Prompt: "Fast Read support", Help: "Fast Read support", Text: "N/A" { 03 08 9B 1A 9A 1A 9C 1A }
0x2FFE4: 		Text Prompt: "Number of Components", Help: "Number of Components", Text: "N/A" { 03 08 9E 1A 9D 1A 9F 1A }
0x2FFEC: 		SuppressIf  { 0A 82 }
0x2FFEE: 			EqIdVal QuestionId: 0x122F, Value: 0x0 { 12 06 2F 12 00 00 }
0x2FFF4: 			Text Prompt: "SPI Component 1 Density", Help: "SPI Component 1 Density", Text: "N/A" { 03 08 A1 1A A0 1A A2 1A }
0x2FFFC: 		End  { 29 02 }
0x2FFFE: 		Text Prompt: "SPI Component 0 Density", Help: "SPI Component 0 Density", Text: "N/A" { 03 08 A4 1A A3 1A A5 1A }
0x30006: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3000D: 		End  { 29 02 }
0x3000F: 		Text Prompt: "EC FW Version", Help: "EC FW Version", Text: "N/A" { 03 08 80 1A 7F 1A 81 1A }
0x30017: 		Text Prompt: "eSPI Flash Sharing Mode", Help: "eSPI Flash Sharing Mode", Text: "N/A" { 03 08 83 1A 82 1A 84 1A }
0x3001F: 		Text Prompt: "EC PECI Mode", Help: "Switch eSPI PECI Mode or Legacy PECI mode", Text: "N/A" { 03 08 86 1A 85 1A 87 1A }
0x30027: 		Text Prompt: "ME FW Version", Help: "ME Firmware Version", Text: "N/A" { 03 08 89 1A 88 1A 8A 1A }
0x3002F: 		Text Prompt: "ME Firmware SKU", Help: "ME Firmware SKU", Text: "N/A" { 03 08 C0 19 BF 19 C1 19 }
0x30037: 		Text Prompt: "PMC FW Version", Help: "PMC Firmware Version", Text: "N/A" { 03 08 8C 1A 8B 1A 8D 1A }
0x3003F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30046: 		End  { 29 02 }
0x30048: 		SuppressIf  { 0A 82 }
0x3004A: 			EqIdVal QuestionId: 0x122E, Value: 0xFFFF { 12 06 2E 12 FF FF }
0x30050: 			OneOf Prompt: "System Language", Help: "Choose the system default language", QuestionFlags: 0x0, QuestionId: 0x2B, VarStoreId: 0xF009, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0 { 05 94 0B 00 0A 00 2B 00 09 F0 00 00 00 11 00 00 01 00 00 00 }
0x30064: 				OneOfOption Option: "" Value: 0 { 09 08 02 00 01 01 00 00 }
0x3006C: 				OneOfOption Option: "" Value: 1 { 09 08 02 00 01 01 01 00 }
0x30074: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3007B: 				Default DefaultId: 0x1 Value: 0 { 5B 07 01 00 01 00 00 }
0x30082: 			End  { 29 02 }
0x30084: 		End  { 29 02 }
0x30086: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3008D: 		End  { 29 02 }
0x3008F: 		Date Prompt: "System Date", Help: "Set the Date. Use Tab to switch between Date elements.

Default Ranges: 

Year: 1998-9999 

Months: 1-12 

Days: Dependent on month

Range of Years may vary.", QuestionFlags: 0x0, QuestionId: 0x2C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, Flags: 0x10 { 1A 8E 17 00 18 00 2C 00 00 00 FF FF 00 10 }
0x3009D: 			Default DefaultId: 0x0 Value: 2014-01-01 { 5B 09 00 00 06 DE 07 01 01 }
0x300A6: 		End  { 29 02 }
0x300A8: 		Time Prompt: "System Time", Help: "Set the Time. Use Tab to switch between Time elements.", QuestionFlags: 0x0, QuestionId: 0x2D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, Flags: 0x10 { 1B 8E 19 00 1A 00 2D 00 00 00 FF FF 00 10 }
0x300B6: 			Default DefaultId: 0x0 Value: 00:00:00 { 5B 08 00 00 05 00 00 00 }
0x300BE: 		End  { 29 02 }
0x300C0: 	End  { 29 02 }
0x300C2: 	Form FormId: 0x2718, Title: "Advanced" { 01 86 18 27 1E 00 }
0x300C8: 		Ref Prompt: "RC ACPI Settings", Help: "System ACPI Parameters.", QuestionFlags: 0x0, QuestionId: 0x2E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271F { 0F 0F 43 01 44 01 2E 00 00 00 FF FF 00 1F 27 }
0x300D7: 		Ref Prompt: "Connectivity Configuration", Help: "Configure Connectivity related options", QuestionFlags: 0x0, QuestionId: 0x2F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2723 { 0F 0F C4 01 C5 01 2F 00 00 00 FF FF 00 23 27 }
0x300E6: 		Ref Prompt: "CPU Configuration", Help: "CPU Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x30, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275C { 0F 0F A3 03 A4 03 30 00 00 00 FF FF 00 5C 27 }
0x300F5: 		Ref Prompt: "Power & Performance", Help: "Power & Performance Options", QuestionFlags: 0x0, QuestionId: 0x31, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2761 { 0F 0F 86 04 87 04 31 00 00 00 FF FF 00 61 27 }
0x30104: 		Ref Prompt: "PCH-FW Configuration", Help: "Configure Management Engine Technology Parameters", QuestionFlags: 0x0, QuestionId: 0x32, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2865 { 0F 0F B2 19 B3 19 32 00 00 00 FF FF 00 65 28 }
0x30113: 		Ref Prompt: "Thermal Configuration", Help: "Thermal Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x33, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2876 { 0F 0F B4 1A B5 1A 33 00 00 00 FF FF 00 76 28 }
0x30122: 		Ref Prompt: "Platform Settings", Help: "Platform related settings", QuestionFlags: 0x0, QuestionId: 0x34, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x287B { 0F 0F 79 1B 7A 1B 34 00 00 00 FF FF 00 7B 28 }
0x30131: 		Ref Prompt: "ACPI D3Cold settings", Help: "ACPI D3Cold related settings", QuestionFlags: 0x0, QuestionId: 0x35, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x287C { 0F 0F 16 1C 17 1C 35 00 00 00 FF FF 00 7C 28 }
0x30140: 		Ref Prompt: "OverClocking Performance Menu", Help: "Performance Menu for Processor and Memory.", QuestionFlags: 0x0, QuestionId: 0x36, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2888 { 0F 0F AE 1C AF 1C 36 00 00 00 FF FF 00 88 28 }
0x3014F: 		Ref Prompt: "BCLK Configuration", Help: "BCLK Configuration", QuestionFlags: 0x0, QuestionId: 0x37, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x289C { 0F 0F B2 1E B2 1E 37 00 00 00 FF FF 00 9C 28 }
0x3015E: 		Ref Prompt: "Debug Settings", Help: "Debug interface Settings", QuestionFlags: 0x0, QuestionId: 0x38, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28B9 { 0F 0F 46 1F 47 1F 38 00 00 00 FF FF 00 B9 28 }
0x3016D: 		Ref Prompt: "Debug Configuration", Help: "Debug Message Settings", QuestionFlags: 0x0, QuestionId: 0x39, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28BD { 0F 0F 9F 1F A0 1F 39 00 00 00 FF FF 00 BD 28 }
0x3017C: 		SuppressIf  { 0A 82 }
0x3017E: 			EqIdVal QuestionId: 0x122D, Value: 0x1 { 12 06 2D 12 01 00 }
0x30184: 			SuppressIf  { 0A 82 }
0x30186: 				EqIdVal QuestionId: 0x122C, Value: 0x1 { 12 86 2C 12 01 00 }
0x3018C: 					EqIdVal QuestionId: 0x122B, Value: 0x1 { 12 06 2B 12 01 00 }
0x30192: 					Or  { 16 02 }
0x30194: 				End  { 29 02 }
0x30196: 				Ref Prompt: "Trusted Computing", Help: "Trusted Computing Settings", QuestionFlags: 0x0, QuestionId: 0x3A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C2 { 0F 0F 87 22 88 22 3A 00 00 00 FF FF 00 C2 28 }
0x301A5: 			End  { 29 02 }
0x301A7: 			SuppressIf  { 0A 82 }
0x301A9: 				EqIdVal QuestionId: 0x122C, Value: 0x0 { 12 86 2C 12 00 00 }
0x301AF: 					EqIdVal QuestionId: 0x122B, Value: 0x1 { 12 06 2B 12 01 00 }
0x301B5: 					Or  { 16 02 }
0x301B7: 				End  { 29 02 }
0x301B9: 				Ref Prompt: "Trusted Computing", Help: "Trusted Computing Settings", QuestionFlags: 0x0, QuestionId: 0x3B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C3 { 0F 0F 87 22 88 22 3B 00 00 00 FF FF 00 C3 28 }
0x301C8: 			End  { 29 02 }
0x301CA: 			SuppressIf  { 0A 82 }
0x301CC: 				EqIdVal QuestionId: 0x122B, Value: 0x0 { 12 06 2B 12 00 00 }
0x301D2: 				Ref Prompt: "Trusted Computing", Help: "Trusted Computing Settings", QuestionFlags: 0x0, QuestionId: 0x3C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C1 { 0F 0F 87 22 88 22 3C 00 00 00 FF FF 00 C1 28 }
0x301E1: 			End  { 29 02 }
0x301E3: 		End  { 29 02 }
0x301E5: 		Ref Prompt: "ACPI Settings", Help: "System ACPI Parameters.", QuestionFlags: 0x0, QuestionId: 0x3D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C4 { 0F 0F 1E 20 44 01 3D 00 00 00 FF FF 00 C4 28 }
0x301F4: 		Ref Prompt: "SMART Settings", Help: "System SMART Settings", QuestionFlags: 0x0, QuestionId: 0x3E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28E3 { 0F 0F EA 21 EB 21 3E 00 00 00 FF FF 00 E3 28 }
0x30203: 		Ref Prompt: "UEFI Variables Protection", Help: "NVRAM Runtime Variable Protection Settings", QuestionFlags: 0x0, QuestionId: 0x3F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28E4 { 0F 0F F0 1F F1 1F 3F 00 00 00 FF FF 00 E4 28 }
0x30212: 		Ref Prompt: "Serial Port Console Redirection", Help: "Serial Port Console Redirection", QuestionFlags: 0x0, QuestionId: 0x40, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28E5 { 0F 0F 60 20 60 20 40 00 00 00 FF FF 00 E5 28 }
0x30221: 		Ref Prompt: "Intel TXT Information", Help: "Display Intel TXT information", QuestionFlags: 0x0, QuestionId: 0x41, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F9 { 0F 0F 27 01 28 01 41 00 00 00 FF FF 00 F9 28 }
0x30230: 		Ref Prompt: "Acoustic Management Configuration", Help: "Option to Enable or Disable Automatic Acoustic Management", QuestionFlags: 0x0, QuestionId: 0x42, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x1, RefQuestionId: 0x0, FormSetGuid: C48AA1AC-F870-418D-A6EF-C1DD89C1CE19 { 0F 21 07 20 08 20 42 00 00 00 FF FF 00 01 00 00 00 AC A1 8A C4 70 F8 8D 41 A6 EF C1 DD 89 C1 CE 19 }
0x30251: 		Ref Prompt: "Switchable Graphics", Help: "Switchable Graphics selections", QuestionFlags: 0x0, QuestionId: 0x43, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FC { 0F 0F 09 20 0A 20 43 00 00 00 FF FF 00 FC 28 }
0x30260: 		SuppressIf  { 0A 82 }
0x30262: 			EqIdVal QuestionId: 0x122A, Value: 0x0 { 12 06 2A 12 00 00 }
0x30268: 			Ref Prompt: "AMI Graphic Output Protocol Policy", Help: "User Select Monitor Output by Graphic Output Protocol", QuestionFlags: 0x0, QuestionId: 0x44, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF { 0F 0F 26 20 27 20 44 00 00 00 FF FF 00 FF 28 }
0x30277: 		End  { 29 02 }
0x30279: 		Ref Prompt: "SIO Common Setting", Help: "SIO Common Setting", QuestionFlags: 0x0, QuestionId: 0x45, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x290B { 0F 0F 5A 20 5B 20 45 00 00 00 FF FF 00 0B 29 }
0x30288: 		Ref Prompt: "SIO Configuration", Help: "SIO Configuration", QuestionFlags: 0x0, QuestionId: 0x46, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x1, RefQuestionId: 0x0, FormSetGuid: 941BC855-BF7E-4FCB-882F-7AEAD15C9D47 { 0F 21 59 20 59 20 46 00 00 00 FF FF 00 01 00 00 00 55 C8 1B 94 7E BF CB 4F 88 2F 7A EA D1 5C 9D 47 }
0x302A9: 		Ref Prompt: "PCI Subsystem Settings", Help: "PCI Subsystem Settings", QuestionFlags: 0x0, QuestionId: 0x47, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x1, RefQuestionId: 0x0, FormSetGuid: ACA9F304-21E2-4852-9875-7FF4881D67A5 { 0F 21 5E 20 5E 20 47 00 00 00 FF FF 00 01 00 00 00 04 F3 A9 AC E2 21 52 48 98 75 7F F4 88 1D 67 A5 }
0x302CA: 		Ref Prompt: "USB Configuration", Help: "USB Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x48, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x290C { 0F 0F 49 21 4A 21 48 00 00 00 FF FF 00 0C 29 }
0x302D9: 		Ref Prompt: "Network Stack Configuration", Help: "Network Stack Settings", QuestionFlags: 0x0, QuestionId: 0x49, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x290F { 0F 0F AB 21 AC 21 49 00 00 00 FF FF 00 0F 29 }
0x302E8: 		Ref Prompt: "CSM Configuration", Help: "CSM configuration: Enable/Disable, Option ROM execution settings, etc.", QuestionFlags: 0x0, QuestionId: 0x4A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2911 { 0F 0F BB 21 BC 21 4A 00 00 00 FF FF 00 11 29 }
0x302F7: 		Ref Prompt: "NVMe Configuration", Help: "NVMe Device Options Settings", QuestionFlags: 0x0, QuestionId: 0x4B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x1, RefQuestionId: 0x0, FormSetGuid: 5E39CF2E-6712-45AB-84C4-35D3C6A3686D { 0F 21 EE 21 EF 21 4B 00 00 00 FF FF 00 01 00 00 00 2E CF 39 5E 12 67 AB 45 84 C4 35 D3 C6 A3 68 6D }
0x30318: 		Ref Prompt: "SDIO Configuration", Help: "SDIO Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x4C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29D4 { 0F 0F F0 21 F1 21 4C 00 00 00 FF FF 00 D4 29 }
0x30327: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3032E: 		End  { 29 02 }
0x30330: 		SuppressIf  { 0A 82 }
0x30332: 			EqIdValList QuestionId: 0x1229, Values: [65535] { 14 08 29 12 01 00 FF FF }
0x3033A: 			Ref Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x4D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2718 { 0F 0F 02 00 02 00 4D 00 00 00 FF FF 00 18 27 }
0x30349: 		End  { 29 02 }
0x3034B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30352: 		End  { 29 02 }
0x30354: 		SuppressIf  { 0A 82 }
0x30356: 			EqIdValList QuestionId: 0x1228, Values: [65535] { 14 08 28 12 01 00 FF FF }
0x3035E: 			Ref Prompt: "Driver Health", Help: "Provides Health Status for the Drivers/Controllers", QuestionFlags: 0x0, QuestionId: 0x4E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2AE0 { 0F 0F 68 00 69 00 4E 00 00 00 FF FF 00 E0 2A }
0x3036D: 		End  { 29 02 }
0x3036F: 	End  { 29 02 }
0x30371: 	Form FormId: 0x271F, Title: "RC ACPI Settings" { 01 86 1F 27 43 01 }
0x30377: 		Subtitle Prompt: "RC ACPI Settings", Help: "", Flags: 0x0 { 02 87 43 01 00 00 00 }
0x3037E: 		End  { 29 02 }
0x30380: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30387: 		End  { 29 02 }
0x30389: 		CheckBox Prompt: "PTID Support", Help: "PTID Support will be loaded if enabled.", QuestionFlags: 0x10, QuestionId: 0x4F, VarStoreId: 0xF101, VarOffset: 0x33, Flags: 0x3, Default: Enabled, MfgDefault: Enabled { 06 8E 52 01 53 01 4F 00 01 F1 33 00 10 03 }
0x30397: 		End  { 29 02 }
0x30399: 		OneOf Prompt: "PECI Access Method", Help: "PECI Access Method is Direct I/O or ACPI", QuestionFlags: 0x10, QuestionId: 0x50, VarStoreId: 0xF101, VarOffset: 0x3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 54 01 55 01 50 00 01 F1 3B 00 10 10 00 01 00 }
0x303AA: 			OneOfOption Option: "Direct I/O" Value: 0, Default, MfgDefault { 09 07 56 01 30 00 00 }
0x303B1: 			OneOfOption Option: "ACPI" Value: 1 { 09 07 57 01 00 00 01 }
0x303B8: 		End  { 29 02 }
0x303BA: 		SuppressIf  { 0A 82 }
0x303BC: 			EqIdVal QuestionId: 0xB67, Value: 0x0 { 12 06 67 0B 00 00 }
0x303C2: 			OneOf Prompt: "Native PCIE Enable", Help: "Bit - PCIe Native * control
 0 - ~ Hot Plug
 1 - SHPC Native Hot Plug control
 2 - ~ Power Management Events
 3 - PCIe Advanced Error Reporting control
 4 - PCIe Capability Structure control
 5 - Latency Tolerance Reporting control", QuestionFlags: 0x10, QuestionId: 0x51, VarStoreId: 0xF101, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 01 4F 01 51 00 01 F1 31 00 10 10 00 01 00 }
0x303D3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 42 01 00 00 00 }
0x303DA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 41 01 30 00 01 }
0x303E1: 			End  { 29 02 }
0x303E3: 		End  { 29 02 }
0x303E5: 		SuppressIf  { 0A 82 }
0x303E7: 			EqIdVal QuestionId: 0x51, Value: 0x0 { 12 06 51 00 00 00 }
0x303ED: 			OneOf Prompt: "Native ASPM", Help: "Enabled - OS Controlled ASPM, Disabled - BIOS Controlled ASPM", QuestionFlags: 0x10, QuestionId: 0x52, VarStoreId: 0xF101, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 50 01 51 01 52 00 01 F1 32 00 10 10 00 02 00 }
0x303FE: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 06 00 30 00 02 }
0x30405: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 41 01 00 00 01 }
0x3040C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 42 01 00 00 00 }
0x30413: 			End  { 29 02 }
0x30415: 		End  { 29 02 }
0x30417: 		OneOf Prompt: "BDAT ACPI Table Support", Help: "Enables support for the BDAT ACPI table.", QuestionFlags: 0x10, QuestionId: 0x53, VarStoreId: 0x4, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 01 47 01 53 00 04 00 01 00 10 10 00 01 00 }
0x30428: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3042E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 42 01 00 00 00 }
0x30435: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 41 01 00 00 01 }
0x3043C: 		End  { 29 02 }
0x3043E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30445: 		End  { 29 02 }
0x30447: 		OneOf Prompt: "Wake System from S5 via RTC", Help: "Enable or disable System wake on alarm event. When enabled, System will wake on the hr::min::sec specified", QuestionFlags: 0x10, QuestionId: 0x54, VarStoreId: 0xF101, VarOffset: 0x3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5D 01 5E 01 54 00 01 F1 3A 00 10 10 00 01 00 }
0x30458: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3045F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30466: 		End  { 29 02 }
0x30468: 		OneOf Prompt: "ACPI Debug", Help: "Open a memory buffer for storing debug strings. Reenter SETUP after enabling to see the buffer address. Use method ADBG to write strings to buffer.", QuestionFlags: 0x10, QuestionId: 0x55, VarStoreId: 0xF101, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 01 59 01 55 00 01 F1 34 00 10 10 00 01 00 }
0x30479: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30480: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30487: 		End  { 29 02 }
0x30489: 		SuppressIf  { 0A 82 }
0x3048B: 			EqIdVal QuestionId: 0x55, Value: 0x0 { 12 06 55 00 00 00 }
0x30491: 			Text Prompt: "  Acpi Memory Buffer Address", Help: "Acpi Memory Buffer Address", Text: "N/A" { 03 08 5B 01 5A 01 5C 01 }
0x30499: 		End  { 29 02 }
0x3049B: 		OneOf Prompt: "D3 Setting for Storage", Help: "RTD3 support for Storage. PCIE storage PEP constraint needs to be set as D0/F1 (Intel Advanced -> ACPI Settings -> PEP PCIe Storage) when this setup is disabled/D3Hot", QuestionFlags: 0x10, QuestionId: 0x56, VarStoreId: 0xF101, VarOffset: 0xAD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 61 01 62 01 56 00 01 F1 D2 0A 10 10 00 02 00 }
0x304AC: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x304B3: 			OneOfOption Option: "D3Hot" Value: 1 { 09 07 63 01 00 00 01 }
0x304BA: 			SuppressIf  { 0A 82 }
0x304BC: 				EqIdVal QuestionId: 0x2873, Value: 0x1 { 12 86 73 28 01 00 }
0x304C2: 					Not  { 17 02 }
0x304C4: 				End  { 29 02 }
0x304C6: 				OneOfOption Option: "D3Cold" Value: 2 { 09 07 64 01 00 00 02 }
0x304CD: 			End  { 29 02 }
0x304CF: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x304D4: 				Value  { 5A 82 }
0x304D6: 					Get VarStoreId: 0xF101, VarStoreInfo: 0x700, VarStoreType: 0x0 { 2B 87 01 F1 00 07 00 }
0x304DD: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x304E7: 						Equal  { 2F 02 }
0x304E9: 						Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x304F3: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x304FD: 						Conditional  { 50 02 }
0x304FF: 					End  { 29 02 }
0x30501: 				End  { 29 02 }
0x30503: 			End  { 29 02 }
0x30505: 		End  { 29 02 }
0x30507: 		OneOf Prompt: "Low Power S0 Idle Capability", Help: "This variable determines if we enable ACPI Lower Power S0 Idle Capability (Mutually exclusive with Smart connect). While this is enabled, it also disable 8254 timer for SLP_S0 support.", QuestionFlags: 0x14, QuestionId: 0x271D, VarStoreId: 0xF101, VarOffset: 0x3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 01 66 01 1D 27 01 F1 3C 00 14 10 00 01 00 }
0x30518: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3051E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30525: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3052C: 			WarningIf Timeout: 0x0, Warning: "Enable Low Power S0 Idle State will also enable HID Event Filter Driver in Platform Settings" { 63 85 BA 01 00 }
0x30531: 				EqIdVal QuestionId: 0x271D, Value: 0x1 { 12 06 1D 27 01 00 }
0x30537: 			End  { 29 02 }
0x30539: 		End  { 29 02 }
0x3053B: 		GrayOutIf  { 19 82 }
0x3053D: 			EqIdVal QuestionId: 0x271D, Value: 0x1 { 12 86 1D 27 01 00 }
0x30543: 				Not  { 17 02 }
0x30545: 			End  { 29 02 }
0x30547: 			OneOf Prompt: "PUIS Enable", Help: "Enable/Disable Power-Up In Standby (PUIS) feature set allows devices to be powered-up into the Standby power management state to minimize inrush current at power-up and to allow the host to sequence the spin-up of devices. 
", QuestionFlags: 0x10, QuestionId: 0x57, VarStoreId: 0xF101, VarOffset: 0x86E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 01 68 01 57 00 01 F1 6E 08 10 10 00 01 00 }
0x30558: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3055F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30566: 			End  { 29 02 }
0x30568: 		End  { 29 02 }
0x3056A: 		SuppressIf  { 0A 82 }
0x3056C: 			EqIdVal QuestionId: 0x271D, Value: 0x1 { 12 86 1D 27 01 00 }
0x30572: 				Not  { 17 02 }
0x30574: 			End  { 29 02 }
0x30576: 			OneOf Prompt: "EC Notification", Help: "Sends EC notification of Low Power S0 Idle State", QuestionFlags: 0x10, QuestionId: 0x58, VarStoreId: 0xF101, VarOffset: 0x51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 01 AF 01 58 00 01 F1 51 00 10 10 00 01 00 }
0x30587: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3058E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30595: 			End  { 29 02 }
0x30597: 			SuppressIf  { 0A 82 }
0x30599: 				EqIdVal QuestionId: 0x58, Value: 0x1 { 12 86 58 00 01 00 }
0x3059F: 					Not  { 17 02 }
0x305A1: 				End  { 29 02 }
0x305A3: 				OneOf Prompt: "EC CS Debug Light", Help: "When EC enters Low Power S0 Idle State, the CAPS LOCK light will be turned on", QuestionFlags: 0x14, QuestionId: 0x271E, VarStoreId: 0xF101, VarOffset: 0x52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 01 B1 01 1E 27 01 F1 52 00 14 10 00 01 00 }
0x305B4: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x305BB: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x305C2: 				End  { 29 02 }
0x305C4: 				OneOf Prompt: "EC Low Power Mode", Help: "This option controls whether EC will go to Low power mode during Low Power S0 Idle State", QuestionFlags: 0x10, QuestionId: 0x59, VarStoreId: 0xF101, VarOffset: 0x53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 01 B3 01 59 00 01 F1 53 00 10 10 00 01 00 }
0x305D5: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x305DC: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x305E3: 				End  { 29 02 }
0x305E5: 			End  { 29 02 }
0x305E7: 			OneOf Prompt: "Sensor Standby", Help: "Enable/Disable Sensor standby mode", QuestionFlags: 0x10, QuestionId: 0x5A, VarStoreId: 0xF101, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 01 B5 01 5A 00 01 F1 58 00 10 10 00 01 00 }
0x305F8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x305FF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30606: 			End  { 29 02 }
0x30608: 			OneOf Prompt: "CS PL1 Limit", Help: "Limit PL1 (Power Limit 1) while in Connected Standby", QuestionFlags: 0x10, QuestionId: 0x5B, VarStoreId: 0xF101, VarOffset: 0x59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 01 B7 01 5B 00 01 F1 59 00 10 10 00 01 00 }
0x30619: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30620: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30627: 			End  { 29 02 }
0x30629: 			SuppressIf  { 0A 82 }
0x3062B: 				EqIdVal QuestionId: 0x5B, Value: 0x1 { 12 86 5B 00 01 00 }
0x30631: 					Not  { 17 02 }
0x30633: 				End  { 29 02 }
0x30635: 				Numeric Prompt: "CS PL1 Value", Help: "PL1 value is in milliwatts with 125 step value", QuestionFlags: 0x0, QuestionId: 0x5C, VarStoreId: 0xF101, VarOffset: 0x5A, Flags: 0x11, Size: 16, Min: 0xBB8, Max: 0x4E20, Step: 0x7D { 07 94 B8 01 B9 01 5C 00 01 F1 5A 00 00 11 B8 0B 20 4E 7D 00 }
0x30649: 					Default DefaultId: 0x0 Value: 4500 { 5B 07 00 00 01 94 11 }
0x30650: 				End  { 29 02 }
0x30652: 			End  { 29 02 }
0x30654: 			Ref Prompt: "PEP Constraints Configuration", Help: "Control which controllers get included in PEP constraint list", QuestionFlags: 0x0, QuestionId: 0x5D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2720 { 0F 0F 69 01 6A 01 5D 00 00 00 FF FF 00 20 27 }
0x30663: 			OneOf Prompt: "LPIT Residency Counter", Help: "Select Residency Counter", QuestionFlags: 0x10, QuestionId: 0x5E, VarStoreId: 0xF101, VarOffset: 0x5E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x7, Step: 0x0 { 05 91 BB 01 BC 01 5E 00 01 F1 5E 00 10 10 01 07 00 }
0x30674: 				OneOfOption Option: "C10" Value: 1 { 09 07 BE 01 00 00 01 }
0x3067B: 				OneOfOption Option: "SLP S0" Value: 3, Default, MfgDefault { 09 07 BD 01 30 00 03 }
0x30682: 				SuppressIf  { 0A 82 }
0x30684: 					EqIdVal QuestionId: 0x1227, Value: 0x0 { 12 06 27 12 00 00 }
0x3068A: 					OneOfOption Option: "ATX Shutdown (PS_ON)" Value: 7 { 09 07 BF 01 00 00 07 }
0x30691: 				End  { 29 02 }
0x30693: 			End  { 29 02 }
0x30695: 		End  { 29 02 }
0x30697: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3069E: 		End  { 29 02 }
0x306A0: 		OneOf Prompt: "PCI Delay Optimization", Help: "Experimental ACPI additions for FW latency optimizations", QuestionFlags: 0x10, QuestionId: 0x5F, VarStoreId: 0xF101, VarOffset: 0x39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 01 C1 01 5F 00 01 F1 39 00 10 10 00 01 00 }
0x306B1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x306B8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x306BF: 		End  { 29 02 }
0x306C1: 		OneOf Prompt: "MSI enabled", Help: "When disabled, MSI support is disabled in FADT", QuestionFlags: 0x10, QuestionId: 0x60, VarStoreId: 0xF101, VarOffset: 0x7A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 01 C3 01 60 00 01 F1 A6 07 10 10 00 01 00 }
0x306D2: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x306D9: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x306E0: 		End  { 29 02 }
0x306E2: 	End  { 29 02 }
0x306E4: 	Form FormId: 0x2720, Title: "PEP Constraints Configuration" { 01 86 20 27 69 01 }
0x306EA: 		Subtitle Prompt: "PEP Constraints Configuration", Help: "", Flags: 0x0 { 02 87 69 01 00 00 00 }
0x306F1: 		End  { 29 02 }
0x306F3: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x306FA: 		End  { 29 02 }
0x306FC: 		OneOf Prompt: "PEP CPU", Help: "Add CPU in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x61, VarStoreId: 0xF101, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 01 6C 01 61 00 01 F1 3D 00 10 10 00 01 00 }
0x3070D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30714: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3071B: 		End  { 29 02 }
0x3071D: 		OneOf Prompt: "PEP Graphics", Help: "Add Gfx in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x62, VarStoreId: 0xF101, VarOffset: 0x3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 01 6E 01 62 00 01 F1 3E 00 10 10 00 01 00 }
0x3072E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30735: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3073C: 		End  { 29 02 }
0x3073E: 		OneOf Prompt: "PEP IPU", Help: "Add IPU in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x63, VarStoreId: 0xF101, VarOffset: 0x4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6F 01 70 01 63 00 01 F1 4A 00 10 10 00 01 00 }
0x3074F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30756: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3075D: 		End  { 29 02 }
0x3075F: 		OneOf Prompt: "PEP GNA", Help: "Add GNA in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x64, VarStoreId: 0xF101, VarOffset: 0x4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 71 01 72 01 64 00 01 F1 4B 00 10 10 00 01 00 }
0x30770: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30777: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3077E: 		End  { 29 02 }
0x30780: 		OneOf Prompt: "PEP SATA", Help: "Add Storage device in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x65, VarStoreId: 0xF101, VarOffset: 0x3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 73 01 74 01 65 00 01 F1 3F 00 10 10 00 03 00 }
0x30791: 			OneOfOption Option: "No Constraint" Value: 0 { 09 07 77 01 00 00 00 }
0x30798: 			OneOfOption Option: "Adapter D0/F1" Value: 1 { 09 07 75 01 00 00 01 }
0x3079F: 			OneOfOption Option: "Raid Volume0" Value: 2 { 09 07 89 01 00 00 02 }
0x307A6: 			OneOfOption Option: "Adapter D3" Value: 3, Default, MfgDefault { 09 07 76 01 30 00 03 }
0x307AD: 		End  { 29 02 }
0x307AF: 		OneOf Prompt: "PEP enumerated SATA ports", Help: "Add enumerated SATA ports in PEP Constraint list", QuestionFlags: 0x10, QuestionId: 0x66, VarStoreId: 0xF101, VarOffset: 0x9DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 01 79 01 66 00 01 F1 DB 09 10 10 00 01 00 }
0x307C0: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x307C7: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x307CE: 		End  { 29 02 }
0x307D0: 		OneOf Prompt: "PEP PCIe Storage", Help: "Add PCIe root ports (storage) in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x67, VarStoreId: 0xF101, VarOffset: 0x862, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 7A 01 7B 01 67 00 01 F1 62 08 10 10 00 03 00 }
0x307E1: 			OneOfOption Option: "No Constraint" Value: 0 { 09 07 7C 01 00 00 00 }
0x307E8: 			OneOfOption Option: "D0/F1" Value: 1 { 09 07 7D 01 00 00 01 }
0x307EF: 			OneOfOption Option: "D3" Value: 3, Default, MfgDefault { 09 07 7E 01 30 00 03 }
0x307F6: 		End  { 29 02 }
0x307F8: 		OneOf Prompt: "PEP PCIe LAN", Help: "Add PCIe root ports (LAN) in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x68, VarStoreId: 0xF101, VarOffset: 0xAA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 7F 01 80 01 68 00 01 F1 A0 0A 10 10 00 03 00 }
0x30809: 			OneOfOption Option: "No Constraint" Value: 0 { 09 07 7C 01 00 00 00 }
0x30810: 			OneOfOption Option: "D0/F1" Value: 1, Default, MfgDefault { 09 07 7D 01 30 00 01 }
0x30817: 			OneOfOption Option: "D3" Value: 3 { 09 07 7E 01 00 00 03 }
0x3081E: 		End  { 29 02 }
0x30820: 		OneOf Prompt: "PEP PCIe WLAN", Help: "", QuestionFlags: 0x10, QuestionId: 0x69, VarStoreId: 0xF101, VarOffset: 0xAA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 81 01 82 01 69 00 01 F1 A1 0A 10 10 00 03 00 }
0x30831: 			OneOfOption Option: "No Constraint" Value: 0 { 09 07 7C 01 00 00 00 }
0x30838: 			OneOfOption Option: "D0/F1" Value: 1, Default, MfgDefault { 09 07 7D 01 30 00 01 }
0x3083F: 			OneOfOption Option: "D3" Value: 3 { 09 07 7E 01 00 00 03 }
0x30846: 		End  { 29 02 }
0x30848: 		OneOf Prompt: "PEP PCIe GFX", Help: "", QuestionFlags: 0x10, QuestionId: 0x6A, VarStoreId: 0xF101, VarOffset: 0xAA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 83 01 84 01 6A 00 01 F1 A2 0A 10 10 00 03 00 }
0x30859: 			OneOfOption Option: "No Constraint" Value: 0 { 09 07 7C 01 00 00 00 }
0x30860: 			OneOfOption Option: "D0/F1" Value: 1, Default, MfgDefault { 09 07 7D 01 30 00 01 }
0x30867: 			OneOfOption Option: "D3" Value: 3 { 09 07 7E 01 00 00 03 }
0x3086E: 		End  { 29 02 }
0x30870: 		OneOf Prompt: "PEP PCIe Other", Help: "", QuestionFlags: 0x10, QuestionId: 0x6B, VarStoreId: 0xF101, VarOffset: 0xAA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 85 01 86 01 6B 00 01 F1 A3 0A 10 10 00 03 00 }
0x30881: 			OneOfOption Option: "No Constraint" Value: 0, Default, MfgDefault { 09 07 7C 01 30 00 00 }
0x30888: 			OneOfOption Option: "D0/F1" Value: 1 { 09 07 7D 01 00 00 01 }
0x3088F: 			OneOfOption Option: "D3" Value: 3 { 09 07 7E 01 00 00 03 }
0x30896: 		End  { 29 02 }
0x30898: 		GrayOutIf  { 19 82 }
0x3089A: 			EqIdVal QuestionId: 0xF79, Value: 0x0 { 12 86 79 0F 00 00 }
0x308A0: 				EqIdVal QuestionId: 0xF7A, Value: 0x0 { 12 06 7A 0F 00 00 }
0x308A6: 				And  { 15 02 }
0x308A8: 				EqIdVal QuestionId: 0xF7B, Value: 0x0 { 12 06 7B 0F 00 00 }
0x308AE: 				And  { 15 02 }
0x308B0: 			End  { 29 02 }
0x308B2: 			OneOf Prompt: "PEP UART", Help: "Add UART in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x6C, VarStoreId: 0xF101, VarOffset: 0x40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 01 8B 01 6C 00 01 F1 40 00 10 10 00 01 00 }
0x308C3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x308CA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x308D1: 			End  { 29 02 }
0x308D3: 		End  { 29 02 }
0x308D5: 		GrayOutIf  { 19 82 }
0x308D7: 			EqIdVal QuestionId: 0xF6A, Value: 0x0 { 12 06 6A 0F 00 00 }
0x308DD: 			OneOf Prompt: "PEP I2C0", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x6D, VarStoreId: 0xF101, VarOffset: 0x41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 01 96 01 6D 00 01 F1 41 00 10 10 00 01 00 }
0x308EE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x308F5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x308FC: 			End  { 29 02 }
0x308FE: 		End  { 29 02 }
0x30900: 		GrayOutIf  { 19 82 }
0x30902: 			EqIdVal QuestionId: 0xF6B, Value: 0x0 { 12 06 6B 0F 00 00 }
0x30908: 			OneOf Prompt: "PEP I2C1", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x6E, VarStoreId: 0xF101, VarOffset: 0x42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 01 96 01 6E 00 01 F1 42 00 10 10 00 01 00 }
0x30919: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30920: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30927: 			End  { 29 02 }
0x30929: 		End  { 29 02 }
0x3092B: 		GrayOutIf  { 19 82 }
0x3092D: 			EqIdVal QuestionId: 0xF6C, Value: 0x0 { 12 06 6C 0F 00 00 }
0x30933: 			OneOf Prompt: "PEP I2C2", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x6F, VarStoreId: 0xF101, VarOffset: 0x43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 01 96 01 6F 00 01 F1 43 00 10 10 00 01 00 }
0x30944: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3094B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30952: 			End  { 29 02 }
0x30954: 		End  { 29 02 }
0x30956: 		GrayOutIf  { 19 82 }
0x30958: 			EqIdVal QuestionId: 0xF6D, Value: 0x0 { 12 06 6D 0F 00 00 }
0x3095E: 			OneOf Prompt: "PEP I2C3", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x70, VarStoreId: 0xF101, VarOffset: 0x44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 01 96 01 70 00 01 F1 44 00 10 10 00 01 00 }
0x3096F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30976: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3097D: 			End  { 29 02 }
0x3097F: 		End  { 29 02 }
0x30981: 		GrayOutIf  { 19 82 }
0x30983: 			EqIdVal QuestionId: 0xF6E, Value: 0x0 { 12 06 6E 0F 00 00 }
0x30989: 			OneOf Prompt: "PEP I2C4", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x71, VarStoreId: 0xF101, VarOffset: 0x45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 01 96 01 71 00 01 F1 45 00 10 10 00 01 00 }
0x3099A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x309A1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x309A8: 			End  { 29 02 }
0x309AA: 		End  { 29 02 }
0x309AC: 		GrayOutIf  { 19 82 }
0x309AE: 			EqIdVal QuestionId: 0xF6F, Value: 0x0 { 12 06 6F 0F 00 00 }
0x309B4: 			OneOf Prompt: "PEP I2C5", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x72, VarStoreId: 0xF101, VarOffset: 0x46, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 01 96 01 72 00 01 F1 46 00 10 10 00 01 00 }
0x309C5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x309CC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x309D3: 			End  { 29 02 }
0x309D5: 		End  { 29 02 }
0x309D7: 		GrayOutIf  { 19 82 }
0x309D9: 			EqIdVal QuestionId: 0xF70, Value: 0x0 { 12 06 70 0F 00 00 }
0x309DF: 			OneOf Prompt: "PEP I2C6", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x73, VarStoreId: 0xF101, VarOffset: 0xB18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 01 96 01 73 00 01 F1 18 0B 10 10 00 01 00 }
0x309F0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x309F7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x309FE: 			End  { 29 02 }
0x30A00: 		End  { 29 02 }
0x30A02: 		GrayOutIf  { 19 82 }
0x30A04: 			EqIdVal QuestionId: 0xF71, Value: 0x0 { 12 06 71 0F 00 00 }
0x30A0A: 			OneOf Prompt: "PEP I2C7", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x74, VarStoreId: 0xF101, VarOffset: 0xB35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 01 96 01 74 00 01 F1 35 0B 10 10 00 01 00 }
0x30A1B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30A22: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30A29: 			End  { 29 02 }
0x30A2B: 		End  { 29 02 }
0x30A2D: 		GrayOutIf  { 19 82 }
0x30A2F: 			EqIdVal QuestionId: 0xF72, Value: 0x0 { 12 86 72 0F 00 00 }
0x30A35: 				EqIdVal QuestionId: 0xF73, Value: 0x0 { 12 06 73 0F 00 00 }
0x30A3B: 				And  { 15 02 }
0x30A3D: 				EqIdVal QuestionId: 0xF74, Value: 0x0 { 12 06 74 0F 00 00 }
0x30A43: 				And  { 15 02 }
0x30A45: 			End  { 29 02 }
0x30A47: 			OneOf Prompt: "PEP SPI", Help: "Add SPI in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x75, VarStoreId: 0xF101, VarOffset: 0x47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 01 8D 01 75 00 01 F1 47 00 10 10 00 01 00 }
0x30A58: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30A5F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30A66: 			End  { 29 02 }
0x30A68: 		End  { 29 02 }
0x30A6A: 		OneOf Prompt: "PEP XHCI", Help: "Add XHCI in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x76, VarStoreId: 0xF101, VarOffset: 0x48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 01 98 01 76 00 01 F1 48 00 10 10 00 01 00 }
0x30A7B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30A82: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30A89: 		End  { 29 02 }
0x30A8B: 		GrayOutIf  { 19 82 }
0x30A8D: 			EqIdVal QuestionId: 0xF0F, Value: 0x0 { 12 06 0F 0F 00 00 }
0x30A93: 			OneOf Prompt: "PEP Audio", Help: "Add Audio in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x77, VarStoreId: 0xF101, VarOffset: 0x49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 99 01 9A 01 77 00 01 F1 49 00 10 10 00 03 00 }
0x30AA4: 				OneOfOption Option: "No Constraint" Value: 0 { 09 07 7C 01 00 00 00 }
0x30AAB: 				OneOfOption Option: "D0/F1" Value: 1, Default, MfgDefault { 09 07 7D 01 30 00 01 }
0x30AB2: 				OneOfOption Option: "D3" Value: 3 { 09 07 7E 01 00 00 03 }
0x30AB9: 			End  { 29 02 }
0x30ABB: 		End  { 29 02 }
0x30ABD: 		OneOf Prompt: "PEP CSME", Help: "Add CSME in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x78, VarStoreId: 0xF101, VarOffset: 0x4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 01 9E 01 78 00 01 F1 4C 00 10 10 00 01 00 }
0x30ACE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30AD5: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30ADC: 		End  { 29 02 }
0x30ADE: 		OneOf Prompt: "PEP HECI3", Help: "Add HECI3 in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x79, VarStoreId: 0xF101, VarOffset: 0x9DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 01 A0 01 79 00 01 F1 DC 09 10 10 00 01 00 }
0x30AEF: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30AF6: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30AFD: 		End  { 29 02 }
0x30AFF: 		OneOf Prompt: "PEP LAN(GBE)", Help: "Add LAN(GBE) in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x7A, VarStoreId: 0xF101, VarOffset: 0x4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 01 A2 01 7A 00 01 F1 4D 00 10 10 00 01 00 }
0x30B10: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30B17: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30B1E: 		End  { 29 02 }
0x30B20: 		OneOf Prompt: "PEP THC0", Help: "Add THC in PEP mitigation list. Applies only if THCx has assigned port", QuestionFlags: 0x10, QuestionId: 0x7B, VarStoreId: 0xF101, VarOffset: 0x4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A3 01 A5 01 7B 00 01 F1 4E 00 10 10 00 01 00 }
0x30B31: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30B38: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30B3F: 		End  { 29 02 }
0x30B41: 		OneOf Prompt: "PEP THC1", Help: "Add THC in PEP mitigation list. Applies only if THCx has assigned port", QuestionFlags: 0x10, QuestionId: 0x7C, VarStoreId: 0xF101, VarOffset: 0x4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 01 A5 01 7C 00 01 F1 4F 00 10 10 00 01 00 }
0x30B52: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30B59: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30B60: 		End  { 29 02 }
0x30B62: 		OneOf Prompt: "PEP TCSS", Help: "Add TCSS IPs in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x7D, VarStoreId: 0xF101, VarOffset: 0x50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 01 AB 01 7D 00 01 F1 50 00 10 10 00 01 00 }
0x30B73: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30B7A: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30B81: 		End  { 29 02 }
0x30B83: 		GrayOutIf  { 19 82 }
0x30B85: 			EqIdVal QuestionId: 0x9B6, Value: 0x0 { 12 06 B6 09 00 00 }
0x30B8B: 			OneOf Prompt: "PEP VMD", Help: "Add VMD in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x7E, VarStoreId: 0xF101, VarOffset: 0x99D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 01 AD 01 7E 00 01 F1 9D 09 10 10 00 01 00 }
0x30B9C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30BA3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30BAA: 			End  { 29 02 }
0x30BAC: 		End  { 29 02 }
0x30BAE: 		SuppressIf  { 0A 82 }
0x30BB0: 			EqIdVal QuestionId: 0x1226, Value: 0x0 { 12 06 26 12 00 00 }
0x30BB6: 			OneOf Prompt: "PEP EMMC", Help: "Add EMMC in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x7F, VarStoreId: 0xF101, VarOffset: 0xB4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 01 9C 01 7F 00 01 F1 4E 0B 10 10 00 01 00 }
0x30BC7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30BCE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x30BD5: 			End  { 29 02 }
0x30BD7: 		End  { 29 02 }
0x30BD9: 	End  { 29 02 }
0x30BDB: 	Form FormId: 0x2723, Title: "Connectivity Configuration" { 01 86 23 27 C4 01 }
0x30BE1: 		Text Prompt: "CNVi CRF Present", Help: "[Yes] means CNVi is the active Connectivity Solution, [No] means CNVi was not discovered", Text: "No" { 03 08 C6 01 C7 01 C8 01 }
0x30BE9: 		Text Prompt: "CNVi Configuration", Help: "CNVi Configuration", Text: "" { 03 08 CA 01 CA 01 00 00 }
0x30BF1: 		OneOf Prompt: "  CNVi Mode", Help: "This option configures Connectivity. 
[Auto Detection] means that if Discrete solution is discovered it will be enabled by default. Otherwise Integrated solution (CNVi) will be enabled; 
[Disable Integrated] disables Integrated Solution. 
NOTE: When CNVi is present, the GPIO pins that are used for radio interface cannot be assigned to the other native function.", QuestionFlags: 0x10, QuestionId: 0x80, VarStoreId: 0x6, VarOffset: 0x734, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CB 01 CC 01 80 00 06 00 34 07 10 10 00 01 00 }
0x30C02: 			OneOfOption Option: "Disable Integrated" Value: 0, Default, MfgDefault { 09 07 CE 01 30 00 00 }
0x30C09: 			OneOfOption Option: "Auto Detection" Value: 1 { 09 07 CD 01 00 00 01 }
0x30C10: 		End  { 29 02 }
0x30C12: 		SuppressIf  { 0A 82 }
0x30C14: 			EqIdVal QuestionId: 0x80, Value: 0x0 { 12 06 80 00 00 00 }
0x30C1A: 			GrayOutIf  { 19 82 }
0x30C1C: 				StringRef1 String: "No" { 4E 84 C9 01 }
0x30C20: 					StringRef1 String: "No" { 4E 04 C8 01 }
0x30C24: 					Match  { 2A 02 }
0x30C26: 				End  { 29 02 }
0x30C28: 				OneOf Prompt: "  Wi-Fi Core", Help: "This is an option intended to Enable/Disable Wi-Fi Core in CNVi", QuestionFlags: 0x10, QuestionId: 0x81, VarStoreId: 0x6, VarOffset: 0x735, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 01 D0 01 81 00 06 00 35 07 10 10 00 01 00 }
0x30C39: 					OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x30C40: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30C47: 				End  { 29 02 }
0x30C49: 				OneOf Prompt: "  BT Core", Help: "This is an option intended to Enable/Disable BT Core in CNVi", QuestionFlags: 0x10, QuestionId: 0x82, VarStoreId: 0x6, VarOffset: 0x736, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 01 D2 01 82 00 06 00 36 07 10 10 00 01 00 }
0x30C5A: 					OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x30C61: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30C68: 				End  { 29 02 }
0x30C6A: 				GrayOutIf  { 19 82 }
0x30C6C: 					EqIdVal QuestionId: 0x82, Value: 0x0 { 12 06 82 00 00 00 }
0x30C72: 					Numeric Prompt: "  BT RF-Kill Delay Time", Help: "This is the delay Time to switch on/off BT RF-KILL signal during S3/S4 resume. Unit is ms", QuestionFlags: 0x0, QuestionId: 0x83, VarStoreId: 0xF101, VarOffset: 0xBB3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x400, Step: 0x1 { 07 94 D9 01 DA 01 83 00 01 F1 B3 0B 00 11 00 00 00 04 01 00 }
0x30C86: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x30C8D: 					End  { 29 02 }
0x30C8F: 				End  { 29 02 }
0x30C91: 			End  { 29 02 }
0x30C93: 		End  { 29 02 }
0x30C95: 		OneOf Prompt: "BT Audio Offload", Help: "This is an option to Enable/Disable BT Audio Offload which enables audio input from BT device to the audio DSP and enables power efficient audio output to BT device.", QuestionFlags: 0x14, QuestionId: 0x2721, VarStoreId: 0x6, VarOffset: 0x737, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D3 01 D4 01 21 27 06 00 37 07 14 10 00 01 00 }
0x30CA6: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x30CAD: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30CB4: 		End  { 29 02 }
0x30CB6: 		OneOf Prompt: "RFI Mitigation", Help: "This is an option intended to Enable/Disable DDR-RFIM feature for Connectivity
This RFI mitigation feature may result in temporary slowdown of the DDR speed.", QuestionFlags: 0x10, QuestionId: 0x84, VarStoreId: 0x6, VarOffset: 0x738, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D5 01 D6 01 84 00 06 00 38 07 10 10 00 01 00 }
0x30CC7: 			OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x30CCE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30CD5: 		End  { 29 02 }
0x30CD7: 		SuppressIf  { 0A 82 }
0x30CD9: 			EqIdVal QuestionId: 0x1113, Value: 0x0 { 12 06 13 11 00 00 }
0x30CDF: 			OneOf Prompt: "DLVR RFI Mitigation", Help: "This is an option intended to Enable/Disable DLVR RFIM feature for Connectivity
This option is only valid when global DLVR is enabled.", QuestionFlags: 0x10, QuestionId: 0x85, VarStoreId: 0xF101, VarOffset: 0xBC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D7 01 D8 01 85 00 01 F1 C7 0B 10 10 00 01 00 }
0x30CF0: 				OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x30CF7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30CFE: 			End  { 29 02 }
0x30D00: 		End  { 29 02 }
0x30D02: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30D09: 		End  { 29 02 }
0x30D0B: 		GrayOutIf  { 19 82 }
0x30D0D: 			EqIdVal QuestionId: 0x1DF, Value: 0x0 { 12 06 DF 01 00 00 }
0x30D13: 			OneOf Prompt: "CoExistence Manager", Help: "CoEx Manager mitigates radio coexistence issues between Intel WWAN (modem) and Intel WLAN (WiFi/BT).
This should be enabled only if both WWAN and WLAN solutions are based on Intel components", QuestionFlags: 0x10, QuestionId: 0x86, VarStoreId: 0xF101, VarOffset: 0x792, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 03 59 03 86 00 01 F1 92 07 10 10 00 01 00 }
0x30D24: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30D2B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30D32: 			End  { 29 02 }
0x30D34: 		End  { 29 02 }
0x30D36: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30D3D: 		End  { 29 02 }
0x30D3F: 		OneOf Prompt: "Preboot BLE", Help: "This will be used to enable Preboot Bluetooth function", QuestionFlags: 0x10, QuestionId: 0x87, VarStoreId: 0xF101, VarOffset: 0x793, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 03 8D 03 87 00 01 F1 93 07 10 10 00 01 00 }
0x30D50: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30D57: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30D5E: 		End  { 29 02 }
0x30D60: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30D67: 		End  { 29 02 }
0x30D69: 		OneOf Prompt: "Discrete Bluetooth Interface", Help: "SerialIo UART0 needs to be enabled to select BT interface", QuestionFlags: 0x10, QuestionId: 0x88, VarStoreId: 0xF101, VarOffset: 0x5F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DB 01 DC 01 88 00 01 F1 F2 05 10 10 00 02 00 }
0x30D7A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x30D81: 			OneOfOption Option: "USB" Value: 1, Default, MfgDefault { 09 07 DD 01 30 00 01 }
0x30D88: 			SuppressIf  { 0A 82 }
0x30D8A: 				EqIdVal QuestionId: 0xF79, Value: 0x0 { 12 06 79 0F 00 00 }
0x30D90: 				OneOfOption Option: "UART" Value: 2 { 09 07 DE 01 00 00 02 }
0x30D97: 			End  { 29 02 }
0x30D99: 		End  { 29 02 }
0x30D9B: 		SuppressIf  { 0A 82 }
0x30D9D: 			EqIdVal QuestionId: 0x88, Value: 0x2 { 12 86 88 00 02 00 }
0x30DA3: 				Not  { 17 02 }
0x30DA5: 			End  { 29 02 }
0x30DA7: 			OneOf Prompt: " BT Interrupt Mode", Help: "Selects routing of interrupt from BT Module", QuestionFlags: 0x10, QuestionId: 0x89, VarStoreId: 0xF101, VarOffset: 0x5F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 01 E0 01 89 00 01 F1 F3 05 10 10 00 01 00 }
0x30DB8: 				OneOfOption Option: "GPIO Interrupt" Value: 0, Default, MfgDefault { 09 07 80 17 30 00 00 }
0x30DBF: 				OneOfOption Option: "APIC Interrupt" Value: 1 { 09 07 7F 17 00 00 01 }
0x30DC6: 			End  { 29 02 }
0x30DC8: 		End  { 29 02 }
0x30DCA: 		OneOf Prompt: "BT Tile Mode", Help: "Enable/Disable Tile", QuestionFlags: 0x10, QuestionId: 0x8A, VarStoreId: 0xF101, VarOffset: 0xAC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5F 03 60 03 8A 00 01 F1 C9 0A 10 10 00 01 00 }
0x30DDB: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30DE2: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30DE9: 		End  { 29 02 }
0x30DEB: 		SuppressIf  { 0A 82 }
0x30DED: 			EqIdVal QuestionId: 0x8A, Value: 0x0 { 12 06 8A 00 00 00 }
0x30DF3: 			Numeric Prompt: " Tile S0", Help: "The activity of Tile in S0.
Bit0:Find My PC
Bit1:Ring Notification
Bit2:BT_LED# Signal", QuestionFlags: 0x0, QuestionId: 0x8B, VarStoreId: 0xF101, VarOffset: 0xACA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 61 03 62 03 8B 00 01 F1 CA 0A 00 10 00 07 01 }
0x30E04: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30E0A: 			End  { 29 02 }
0x30E0C: 			Numeric Prompt: " Tile S0ix", Help: "The activity of Tile in S0ix.
Bit0:Find My PC
Bit1:Ring Notification
Bit2:BT_LED# Signal", QuestionFlags: 0x0, QuestionId: 0x8C, VarStoreId: 0xF101, VarOffset: 0xACB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 63 03 64 03 8C 00 01 F1 CB 0A 00 10 00 07 01 }
0x30E1D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30E23: 			End  { 29 02 }
0x30E25: 			Numeric Prompt: " Tile S4", Help: "The activity of Tile in S4.
Bit0:Find My PC
Bit1:Ring Notification
Bit2:BT_LED# Signal", QuestionFlags: 0x0, QuestionId: 0x8D, VarStoreId: 0xF101, VarOffset: 0xACC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 65 03 66 03 8D 00 01 F1 CC 0A 00 10 00 07 01 }
0x30E36: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30E3C: 			End  { 29 02 }
0x30E3E: 			Numeric Prompt: " Tile S5", Help: "The activity of Tile in S5.
Bit0:Find My PC
Bit1:Ring Notification
Bit2:BT_LED# Signal", QuestionFlags: 0x0, QuestionId: 0x8E, VarStoreId: 0xF101, VarOffset: 0xACD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 67 03 68 03 8E 00 01 F1 CD 0A 00 10 00 07 01 }
0x30E4F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30E55: 			End  { 29 02 }
0x30E57: 			Numeric Prompt: "BT LED Config", Help: "BT LED Config
Bit0:Define LED to Tile Ring Notification
Bit1:Active High Polarity", QuestionFlags: 0x0, QuestionId: 0x8F, VarStoreId: 0xF101, VarOffset: 0xB3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x1 { 07 91 6F 03 70 03 8F 00 01 F1 3B 0B 00 10 00 03 01 }
0x30E68: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30E6E: 			End  { 29 02 }
0x30E70: 			Numeric Prompt: "BT LED Pulse Duration", Help: "LED Duration in milliseconds.
Min:1ms
Max:1000ms", QuestionFlags: 0x0, QuestionId: 0x90, VarStoreId: 0xF101, VarOffset: 0xB3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 71 03 72 03 90 00 01 F1 3C 0B 00 10 00 FF 01 }
0x30E81: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30E87: 			End  { 29 02 }
0x30E89: 			Numeric Prompt: "BT LED Pulse Interval", Help: "LED Pulse interval  in tens of milliseconds.
Min:10ms
Max:255ms", QuestionFlags: 0x0, QuestionId: 0x91, VarStoreId: 0xF101, VarOffset: 0xB3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0xA { 07 91 73 03 74 03 91 00 01 F1 3D 0B 00 10 00 FF 0A }
0x30E9A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x30EA0: 			End  { 29 02 }
0x30EA2: 		End  { 29 02 }
0x30EA4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x30EAB: 		End  { 29 02 }
0x30EAD: 		OneOf Prompt: "Advanced settings", Help: "Configure ACPI objects for wireless devices", QuestionFlags: 0x10, QuestionId: 0x92, VarStoreId: 0xF101, VarOffset: 0x739, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 01 E2 01 92 00 01 F1 39 07 10 10 00 01 00 }
0x30EBE: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x30EC5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x30ECC: 		End  { 29 02 }
0x30ECE: 		SuppressIf  { 0A 82 }
0x30ED0: 			EqIdVal QuestionId: 0x92, Value: 0x0 { 12 06 92 00 00 00 }
0x30ED6: 			OneOf Prompt: "Switched Antenna Diversity Selection", Help: "This allows WiFi modules which have only one antenna to use one of the 2 possible antennas with the options:
 0 - Antenna1
 1 - Antenna2
 2 - Diversity
 3 - Diversity Antenna1
 4 - Diversity Antenna2", QuestionFlags: 0x10, QuestionId: 0x93, VarStoreId: 0xF101, VarOffset: 0x791, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 85 03 86 03 93 00 01 F1 91 07 10 10 00 04 00 }
0x30EE7: 				OneOfOption Option: "Antenna1" Value: 0 { 09 07 87 03 00 00 00 }
0x30EEE: 				OneOfOption Option: "Antenna2" Value: 1 { 09 07 88 03 00 00 01 }
0x30EF5: 				OneOfOption Option: "Diversity" Value: 2, Default, MfgDefault { 09 07 89 03 30 00 02 }
0x30EFC: 				OneOfOption Option: "Diversity Antenna1" Value: 3 { 09 07 8A 03 00 00 03 }
0x30F03: 				OneOfOption Option: "Diversity Antenna2" Value: 4 { 09 07 8B 03 00 00 04 }
0x30F0A: 			End  { 29 02 }
0x30F0C: 			Text Prompt: "SPLC", Help: "SPLC", Text: "" { 03 08 98 1B 98 1B 00 00 }
0x30F14: 			Numeric Prompt: " Domain Type SPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x94, VarStoreId: 0xF101, VarOffset: 0x73A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1 { 07 91 9C 1B 9D 1B 94 00 01 F1 3A 07 00 10 00 14 01 }
0x30F25: 				Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x30F2B: 			End  { 29 02 }
0x30F2D: 			Numeric Prompt: " Default Power Limit", Help: "Power Limit in milli watts", QuestionFlags: 0x14, QuestionId: 0x2722, VarStoreId: 0xF101, VarOffset: 0x73B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1 { 07 94 E3 01 E4 01 22 27 01 F1 3B 07 14 11 01 00 FF FF 01 00 }
0x30F41: 				Default DefaultId: 0x0 Value: 65535 { 5B 07 00 00 01 FF FF }
0x30F48: 			End  { 29 02 }
0x30F4A: 			Numeric Prompt: " Default Time Window", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x95, VarStoreId: 0xF101, VarOffset: 0x73D, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1 { 07 9A E5 01 E6 01 95 00 01 F1 3D 07 00 12 01 00 00 00 A0 86 01 00 01 00 00 00 }
0x30F64: 				Default DefaultId: 0x0 Value: 30000 { 5B 09 00 00 02 30 75 00 00 }
0x30F6D: 			End  { 29 02 }
0x30F6F: 			Text Prompt: "WAND", Help: "WAND", Text: "" { 03 08 E7 01 E7 01 00 00 }
0x30F77: 			Numeric Prompt: " TRxDelay_A", Help: "Antenna A delay possible values: 1-100 in 10ths of nano seconds resolution", QuestionFlags: 0x0, QuestionId: 0x96, VarStoreId: 0xF101, VarOffset: 0x741, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1 { 07 91 E8 01 E9 01 96 00 01 F1 41 07 00 10 01 64 01 }
0x30F88: 				Default DefaultId: 0x0 Value: 50 { 5B 06 00 00 00 32 }
0x30F8E: 			End  { 29 02 }
0x30F90: 			Numeric Prompt: " TRxCableLength_A", Help: "Antenna A cable length possible values: 1-100cm in 1cm resolution", QuestionFlags: 0x0, QuestionId: 0x97, VarStoreId: 0xF101, VarOffset: 0x742, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1 { 07 91 EA 01 EB 01 97 00 01 F1 42 07 00 10 01 64 01 }
0x30FA1: 				Default DefaultId: 0x0 Value: 50 { 5B 06 00 00 00 32 }
0x30FA7: 			End  { 29 02 }
0x30FA9: 			Numeric Prompt: " TRxDelay_B", Help: "Antenna B delay possible values: 1-100 in 10ths of nano seconds resolution", QuestionFlags: 0x0, QuestionId: 0x98, VarStoreId: 0xF101, VarOffset: 0x743, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1 { 07 91 EC 01 ED 01 98 00 01 F1 43 07 00 10 01 64 01 }
0x30FBA: 				Default DefaultId: 0x0 Value: 50 { 5B 06 00 00 00 32 }
0x30FC0: 			End  { 29 02 }
0x30FC2: 			Numeric Prompt: " TRxCableLength_B", Help: "Antenna B cable length possible values: 1-100cm in 1cm resolution", QuestionFlags: 0x0, QuestionId: 0x99, VarStoreId: 0xF101, VarOffset: 0x744, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1 { 07 91 EE 01 EF 01 99 00 01 F1 44 07 00 10 01 64 01 }
0x30FD3: 				Default DefaultId: 0x0 Value: 50 { 5B 06 00 00 00 32 }
0x30FD9: 			End  { 29 02 }
0x30FDB: 			Text Prompt: "WRDD Package 1", Help: "WRDD Package 1", Text: "" { 03 08 F0 01 F0 01 00 00 }
0x30FE3: 			Numeric Prompt: " Domain Type", Help: "09h: Module; 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x9A, VarStoreId: 0xF101, VarOffset: 0x745, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1 { 07 91 F1 01 F2 01 9A 00 01 F1 45 07 00 10 00 64 01 }
0x30FF4: 				Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x30FFA: 			End  { 29 02 }
0x30FFC: 			Numeric Prompt: " Country Identifier", Help: "Country identifier as defined in ISO/IEC 3166-1 Alpha 2 code", QuestionFlags: 0x0, QuestionId: 0x9B, VarStoreId: 0xF101, VarOffset: 0x746, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1 { 07 94 F3 01 F4 01 9B 00 01 F1 46 07 00 11 01 00 FF FF 01 00 }
0x31010: 				Default DefaultId: 0x0 Value: 16720 { 5B 07 00 00 01 50 41 }
0x31017: 			End  { 29 02 }
0x31019: 			Text Prompt: "11Ax Control", Help: "11Ax Control", Text: "" { 03 08 35 03 35 03 00 00 }
0x31021: 			OneOf Prompt: " 11Ax Setting for Ukraine", Help: "11Ax Setting for Ukraine
Bit 0 - Apply changes to country Ukraine. 11Ax Setting within module certification
00 - None. Work with Wi-Fi FW/OTP definitions [Default]
01 - Apply changes", QuestionFlags: 0x10, QuestionId: 0x9C, VarStoreId: 0xF101, VarOffset: 0xA1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 36 03 37 03 9C 00 01 F1 1D 0A 10 10 00 01 00 }
0x31032: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x31039: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x31040: 			End  { 29 02 }
0x31042: 			GrayOutIf  { 19 82 }
0x31044: 				EqIdVal QuestionId: 0x9C, Value: 0x0 { 12 06 9C 00 00 00 }
0x3104A: 				OneOf Prompt: " 11Ax Mode for Ukraine", Help: "11Ax Mode for Ukraine
Bit 1 - 11Ax Mode. Effective only if Bit 0 set to 1
00 – Disable 11Ax on country Ukraine [Default]
01 – Enable 11Ax on country Ukraine", QuestionFlags: 0x10, QuestionId: 0x9D, VarStoreId: 0xF101, VarOffset: 0xA1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 03 39 03 9D 00 01 F1 1E 0A 10 10 00 01 00 }
0x3105B: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x31062: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x31069: 				End  { 29 02 }
0x3106B: 			End  { 29 02 }
0x3106D: 			OneOf Prompt: " 11Ax Setting for Russia", Help: "11Ax Setting for Russia
Bit 2 - Apply changes to country Russia. 11Ax Setting within module certification
00 - None. Work with Wi-Fi FW/OTP definitions [Default]
01 - Apply changes", QuestionFlags: 0x10, QuestionId: 0x9E, VarStoreId: 0xF101, VarOffset: 0xA1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 03 3B 03 9E 00 01 F1 1F 0A 10 10 00 01 00 }
0x3107E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x31085: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3108C: 			End  { 29 02 }
0x3108E: 			GrayOutIf  { 19 82 }
0x31090: 				EqIdVal QuestionId: 0x9E, Value: 0x0 { 12 06 9E 00 00 00 }
0x31096: 				OneOf Prompt: " 11Ax Mode for Russia", Help: "11Ax Mode for Russia
Bit 3 - 11Ax Mode. Effective only if Bit 2 set to 1
00 – Disable 11Ax on country Russia [Default]
01 – Enable 11Ax on country Russia", QuestionFlags: 0x10, QuestionId: 0x9F, VarStoreId: 0xF101, VarOffset: 0xA20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 03 3D 03 9F 00 01 F1 20 0A 10 10 00 01 00 }
0x310A7: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x310AE: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x310B5: 				End  { 29 02 }
0x310B7: 			End  { 29 02 }
0x310B9: 			Text Prompt: "WRDS Package", Help: "WRDS Package", Text: "" { 03 08 F5 01 F5 01 00 00 }
0x310C1: 			OneOf Prompt: " WiFi SAR", Help: "Enable/Disable WiFi SAR Tx Power Limit; DISABLE - Device ignores WiFi SAR Configuration Table; ENABLE - Device uses WiFi SAR Configuration Table", QuestionFlags: 0x10, QuestionId: 0xA0, VarStoreId: 0xF101, VarOffset: 0x74B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F6 01 F7 01 A0 00 01 F1 4B 07 10 10 00 01 00 }
0x310D2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x310D8: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x310DF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x310E6: 			End  { 29 02 }
0x310E8: 			SuppressIf  { 0A 82 }
0x310EA: 				EqIdVal QuestionId: 0xA0, Value: 0x0 { 12 06 A0 00 00 00 }
0x310F0: 				Numeric Prompt: " SAR 2400 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA1, VarStoreId: 0xF101, VarOffset: 0x74C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 07 02 06 02 A1 00 01 F1 4C 07 00 10 00 FF 01 }
0x31101: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31107: 				End  { 29 02 }
0x31109: 				Numeric Prompt: " SAR 5180-5320 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA2, VarStoreId: 0xF101, VarOffset: 0x74D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 08 02 06 02 A2 00 01 F1 4D 07 00 10 00 FF 01 }
0x3111A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31120: 				End  { 29 02 }
0x31122: 				Numeric Prompt: " SAR 5340-5440 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA3, VarStoreId: 0xF101, VarOffset: 0x74E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 09 02 06 02 A3 00 01 F1 4E 07 00 10 00 FF 01 }
0x31133: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31139: 				End  { 29 02 }
0x3113B: 				Numeric Prompt: " SAR 5460-5700 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA4, VarStoreId: 0xF101, VarOffset: 0x74F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0A 02 06 02 A4 00 01 F1 4F 07 00 10 00 FF 01 }
0x3114C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31152: 				End  { 29 02 }
0x31154: 				Numeric Prompt: " SAR 5720-5825 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA5, VarStoreId: 0xF101, VarOffset: 0x750, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0B 02 06 02 A5 00 01 F1 50 07 00 10 00 FF 01 }
0x31165: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3116B: 				End  { 29 02 }
0x3116D: 				Numeric Prompt: " SAR 5845-6135 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA6, VarStoreId: 0xF101, VarOffset: 0x751, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0C 02 06 02 A6 00 01 F1 51 07 00 10 00 FF 01 }
0x3117E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31184: 				End  { 29 02 }
0x31186: 				Numeric Prompt: " SAR 6155-6375 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA7, VarStoreId: 0xF101, VarOffset: 0x752, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0D 02 06 02 A7 00 01 F1 52 07 00 10 00 FF 01 }
0x31197: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3119D: 				End  { 29 02 }
0x3119F: 				Numeric Prompt: " SAR 6395-6495 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA8, VarStoreId: 0xF101, VarOffset: 0x753, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0E 02 06 02 A8 00 01 F1 53 07 00 10 00 FF 01 }
0x311B0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x311B6: 				End  { 29 02 }
0x311B8: 				Numeric Prompt: " SAR 6515-6675 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xA9, VarStoreId: 0xF101, VarOffset: 0x754, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0F 02 06 02 A9 00 01 F1 54 07 00 10 00 FF 01 }
0x311C9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x311CF: 				End  { 29 02 }
0x311D1: 				Numeric Prompt: " SAR 6695-6835 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xAA, VarStoreId: 0xF101, VarOffset: 0x755, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 10 02 06 02 AA 00 01 F1 55 07 00 10 00 FF 01 }
0x311E2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x311E8: 				End  { 29 02 }
0x311EA: 				Numeric Prompt: " SAR 6855-7095 MHz Set1 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xAB, VarStoreId: 0xF101, VarOffset: 0x9E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 11 02 06 02 AB 00 01 F1 E1 09 00 10 00 FF 01 }
0x311FB: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31201: 				End  { 29 02 }
0x31203: 				Numeric Prompt: " SAR 2400 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xAC, VarStoreId: 0xF101, VarOffset: 0x9E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 12 02 06 02 AC 00 01 F1 E2 09 00 10 00 FF 01 }
0x31214: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3121A: 				End  { 29 02 }
0x3121C: 				Numeric Prompt: " SAR 5180-5320 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xAD, VarStoreId: 0xF101, VarOffset: 0x9E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 13 02 06 02 AD 00 01 F1 E3 09 00 10 00 FF 01 }
0x3122D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31233: 				End  { 29 02 }
0x31235: 				Numeric Prompt: " SAR 5340-5440 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xAE, VarStoreId: 0xF101, VarOffset: 0x9E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 14 02 06 02 AE 00 01 F1 E4 09 00 10 00 FF 01 }
0x31246: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3124C: 				End  { 29 02 }
0x3124E: 				Numeric Prompt: " SAR 5460-5700 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xAF, VarStoreId: 0xF101, VarOffset: 0x9E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 15 02 06 02 AF 00 01 F1 E5 09 00 10 00 FF 01 }
0x3125F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31265: 				End  { 29 02 }
0x31267: 				Numeric Prompt: " SAR 5720-5825 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB0, VarStoreId: 0xF101, VarOffset: 0x9E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 16 02 06 02 B0 00 01 F1 E6 09 00 10 00 FF 01 }
0x31278: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3127E: 				End  { 29 02 }
0x31280: 				Numeric Prompt: " SAR 5845-6135 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB1, VarStoreId: 0xF101, VarOffset: 0x9E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 17 02 06 02 B1 00 01 F1 E7 09 00 10 00 FF 01 }
0x31291: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31297: 				End  { 29 02 }
0x31299: 				Numeric Prompt: " SAR 6155-6375 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB2, VarStoreId: 0xF101, VarOffset: 0x9E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 18 02 06 02 B2 00 01 F1 E8 09 00 10 00 FF 01 }
0x312AA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x312B0: 				End  { 29 02 }
0x312B2: 				Numeric Prompt: " SAR 6395-6495 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB3, VarStoreId: 0xF101, VarOffset: 0x9E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 19 02 06 02 B3 00 01 F1 E9 09 00 10 00 FF 01 }
0x312C3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x312C9: 				End  { 29 02 }
0x312CB: 				Numeric Prompt: " SAR 6515-6675 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB4, VarStoreId: 0xF101, VarOffset: 0x9EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1A 02 06 02 B4 00 01 F1 EA 09 00 10 00 FF 01 }
0x312DC: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x312E2: 				End  { 29 02 }
0x312E4: 				Numeric Prompt: " SAR 6695-6835 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB5, VarStoreId: 0xF101, VarOffset: 0x9EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1B 02 06 02 B5 00 01 F1 EB 09 00 10 00 FF 01 }
0x312F5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x312FB: 				End  { 29 02 }
0x312FD: 				Numeric Prompt: " SAR 6855-7095 MHz Set1 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB6, VarStoreId: 0xF101, VarOffset: 0x9EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1C 02 06 02 B6 00 01 F1 EC 09 00 10 00 FF 01 }
0x3130E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31314: 				End  { 29 02 }
0x31316: 				Numeric Prompt: " SAR CDB 2400 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB7, VarStoreId: 0xF101, VarOffset: 0xA2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 60 02 5F 02 B7 00 01 F1 2A 0A 00 10 00 FF 01 }
0x31327: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3132D: 				End  { 29 02 }
0x3132F: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB8, VarStoreId: 0xF101, VarOffset: 0xA2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 61 02 5F 02 B8 00 01 F1 2B 0A 00 10 00 FF 01 }
0x31340: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31346: 				End  { 29 02 }
0x31348: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xB9, VarStoreId: 0xF101, VarOffset: 0xA2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 62 02 5F 02 B9 00 01 F1 2C 0A 00 10 00 FF 01 }
0x31359: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3135F: 				End  { 29 02 }
0x31361: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xBA, VarStoreId: 0xF101, VarOffset: 0xA2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 63 02 5F 02 BA 00 01 F1 2D 0A 00 10 00 FF 01 }
0x31372: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31378: 				End  { 29 02 }
0x3137A: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xBB, VarStoreId: 0xF101, VarOffset: 0xA2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 64 02 5F 02 BB 00 01 F1 2E 0A 00 10 00 FF 01 }
0x3138B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31391: 				End  { 29 02 }
0x31393: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xBC, VarStoreId: 0xF101, VarOffset: 0xA2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 65 02 5F 02 BC 00 01 F1 2F 0A 00 10 00 FF 01 }
0x313A4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x313AA: 				End  { 29 02 }
0x313AC: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xBD, VarStoreId: 0xF101, VarOffset: 0xA30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 66 02 5F 02 BD 00 01 F1 30 0A 00 10 00 FF 01 }
0x313BD: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x313C3: 				End  { 29 02 }
0x313C5: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xBE, VarStoreId: 0xF101, VarOffset: 0xA31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 67 02 5F 02 BE 00 01 F1 31 0A 00 10 00 FF 01 }
0x313D6: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x313DC: 				End  { 29 02 }
0x313DE: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xBF, VarStoreId: 0xF101, VarOffset: 0xA32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 68 02 5F 02 BF 00 01 F1 32 0A 00 10 00 FF 01 }
0x313EF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x313F5: 				End  { 29 02 }
0x313F7: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC0, VarStoreId: 0xF101, VarOffset: 0xA33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 69 02 5F 02 C0 00 01 F1 33 0A 00 10 00 FF 01 }
0x31408: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3140E: 				End  { 29 02 }
0x31410: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set1 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC1, VarStoreId: 0xF101, VarOffset: 0xA34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 6A 02 5F 02 C1 00 01 F1 34 0A 00 10 00 FF 01 }
0x31421: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31427: 				End  { 29 02 }
0x31429: 				Numeric Prompt: " SAR CDB 2400 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC2, VarStoreId: 0xF101, VarOffset: 0xA35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 6B 02 5F 02 C2 00 01 F1 35 0A 00 10 00 FF 01 }
0x3143A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31440: 				End  { 29 02 }
0x31442: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC3, VarStoreId: 0xF101, VarOffset: 0xA36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 6C 02 5F 02 C3 00 01 F1 36 0A 00 10 00 FF 01 }
0x31453: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31459: 				End  { 29 02 }
0x3145B: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC4, VarStoreId: 0xF101, VarOffset: 0xA37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 6D 02 5F 02 C4 00 01 F1 37 0A 00 10 00 FF 01 }
0x3146C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31472: 				End  { 29 02 }
0x31474: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC5, VarStoreId: 0xF101, VarOffset: 0xA38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 6E 02 5F 02 C5 00 01 F1 38 0A 00 10 00 FF 01 }
0x31485: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3148B: 				End  { 29 02 }
0x3148D: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC6, VarStoreId: 0xF101, VarOffset: 0xA39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 6F 02 5F 02 C6 00 01 F1 39 0A 00 10 00 FF 01 }
0x3149E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x314A4: 				End  { 29 02 }
0x314A6: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC7, VarStoreId: 0xF101, VarOffset: 0xA3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 70 02 5F 02 C7 00 01 F1 3A 0A 00 10 00 FF 01 }
0x314B7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x314BD: 				End  { 29 02 }
0x314BF: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC8, VarStoreId: 0xF101, VarOffset: 0xA3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 71 02 5F 02 C8 00 01 F1 3B 0A 00 10 00 FF 01 }
0x314D0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x314D6: 				End  { 29 02 }
0x314D8: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xC9, VarStoreId: 0xF101, VarOffset: 0xA3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 72 02 5F 02 C9 00 01 F1 3C 0A 00 10 00 FF 01 }
0x314E9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x314EF: 				End  { 29 02 }
0x314F1: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xCA, VarStoreId: 0xF101, VarOffset: 0xA3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 73 02 5F 02 CA 00 01 F1 3D 0A 00 10 00 FF 01 }
0x31502: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31508: 				End  { 29 02 }
0x3150A: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xCB, VarStoreId: 0xF101, VarOffset: 0xA3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 74 02 5F 02 CB 00 01 F1 3E 0A 00 10 00 FF 01 }
0x3151B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31521: 				End  { 29 02 }
0x31523: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set1 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xCC, VarStoreId: 0xF101, VarOffset: 0xA3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 75 02 5F 02 CC 00 01 F1 3F 0A 00 10 00 FF 01 }
0x31534: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3153A: 				End  { 29 02 }
0x3153C: 			End  { 29 02 }
0x3153E: 			Text Prompt: "EWRD Package", Help: "EWRD Package", Text: "" { 03 08 F8 01 F8 01 00 00 }
0x31546: 			OneOf Prompt: " WiFi Dynamic SAR", Help: "Enable/Disable WiFi Dynamic SAR Tx Power Limit which shell be set dynamically accorting to the Proximity Sensor", QuestionFlags: 0x10, QuestionId: 0xCD, VarStoreId: 0xF101, VarOffset: 0x756, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 01 FA 01 CD 00 01 F1 56 07 10 10 00 01 00 }
0x31557: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3155E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x31565: 			End  { 29 02 }
0x31567: 			SuppressIf  { 0A 82 }
0x31569: 				EqIdVal QuestionId: 0xCD, Value: 0x0 { 12 06 CD 00 00 00 }
0x3156F: 				OneOf Prompt: " Extended SAR Range Sets", Help: "Defines the WiFi SAR Sets that can be used to set the power limts dynamically based on the Proximity Sensor,Set 1 is always present if WiFi SAR enabled and Set 2-3 are additinoal sets", QuestionFlags: 0x10, QuestionId: 0xCE, VarStoreId: 0xF101, VarOffset: 0x757, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 FB 01 FC 01 CE 00 01 F1 57 07 10 10 00 03 00 }
0x31580: 					OneOfOption Option: "No Additional sets" Value: 0, Default, MfgDefault { 09 07 FD 01 30 00 00 }
0x31587: 					OneOfOption Option: "Set 2" Value: 1 { 09 07 FF 01 00 00 01 }
0x3158E: 					OneOfOption Option: "Set 3" Value: 2 { 09 07 00 02 00 00 02 }
0x31595: 					OneOfOption Option: "Set 4" Value: 3 { 09 07 01 02 00 00 03 }
0x3159C: 				End  { 29 02 }
0x3159E: 				Numeric Prompt: " SAR 2400 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xCF, VarStoreId: 0xF101, VarOffset: 0x758, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1D 02 06 02 CF 00 01 F1 58 07 00 10 00 FF 01 }
0x315AF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x315B5: 				End  { 29 02 }
0x315B7: 				Numeric Prompt: " SAR 5180-5320 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD0, VarStoreId: 0xF101, VarOffset: 0x759, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1E 02 06 02 D0 00 01 F1 59 07 00 10 00 FF 01 }
0x315C8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x315CE: 				End  { 29 02 }
0x315D0: 				Numeric Prompt: " SAR 5340-5440 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD1, VarStoreId: 0xF101, VarOffset: 0x75A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1F 02 06 02 D1 00 01 F1 5A 07 00 10 00 FF 01 }
0x315E1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x315E7: 				End  { 29 02 }
0x315E9: 				Numeric Prompt: " SAR 5460-5700 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD2, VarStoreId: 0xF101, VarOffset: 0x75B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 20 02 06 02 D2 00 01 F1 5B 07 00 10 00 FF 01 }
0x315FA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31600: 				End  { 29 02 }
0x31602: 				Numeric Prompt: " SAR 5720-5825 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD3, VarStoreId: 0xF101, VarOffset: 0x75C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 21 02 06 02 D3 00 01 F1 5C 07 00 10 00 FF 01 }
0x31613: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31619: 				End  { 29 02 }
0x3161B: 				Numeric Prompt: " SAR 5845-6135 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD4, VarStoreId: 0xF101, VarOffset: 0x75D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 22 02 06 02 D4 00 01 F1 5D 07 00 10 00 FF 01 }
0x3162C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31632: 				End  { 29 02 }
0x31634: 				Numeric Prompt: " SAR 6155-6375 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD5, VarStoreId: 0xF101, VarOffset: 0x75E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 23 02 06 02 D5 00 01 F1 5E 07 00 10 00 FF 01 }
0x31645: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3164B: 				End  { 29 02 }
0x3164D: 				Numeric Prompt: " SAR 6395-6495 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD6, VarStoreId: 0xF101, VarOffset: 0x75F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 24 02 06 02 D6 00 01 F1 5F 07 00 10 00 FF 01 }
0x3165E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31664: 				End  { 29 02 }
0x31666: 				Numeric Prompt: " SAR 6515-6675 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD7, VarStoreId: 0xF101, VarOffset: 0x760, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 25 02 06 02 D7 00 01 F1 60 07 00 10 00 FF 01 }
0x31677: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3167D: 				End  { 29 02 }
0x3167F: 				Numeric Prompt: " SAR 6695-6835 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD8, VarStoreId: 0xF101, VarOffset: 0x761, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 26 02 06 02 D8 00 01 F1 61 07 00 10 00 FF 01 }
0x31690: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31696: 				End  { 29 02 }
0x31698: 				Numeric Prompt: " SAR 6855-7095 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xD9, VarStoreId: 0xF101, VarOffset: 0x9ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 27 02 06 02 D9 00 01 F1 ED 09 00 10 00 FF 01 }
0x316A9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x316AF: 				End  { 29 02 }
0x316B1: 				Numeric Prompt: " SAR 2400 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xDA, VarStoreId: 0xF101, VarOffset: 0x9EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 28 02 06 02 DA 00 01 F1 EE 09 00 10 00 FF 01 }
0x316C2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x316C8: 				End  { 29 02 }
0x316CA: 				Numeric Prompt: " SAR 5180-5320 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xDB, VarStoreId: 0xF101, VarOffset: 0x9EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 29 02 06 02 DB 00 01 F1 EF 09 00 10 00 FF 01 }
0x316DB: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x316E1: 				End  { 29 02 }
0x316E3: 				Numeric Prompt: " SAR 5340-5440 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xDC, VarStoreId: 0xF101, VarOffset: 0x9F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2A 02 06 02 DC 00 01 F1 F0 09 00 10 00 FF 01 }
0x316F4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x316FA: 				End  { 29 02 }
0x316FC: 				Numeric Prompt: " SAR 5460-5700 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xDD, VarStoreId: 0xF101, VarOffset: 0x9F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2B 02 06 02 DD 00 01 F1 F1 09 00 10 00 FF 01 }
0x3170D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31713: 				End  { 29 02 }
0x31715: 				Numeric Prompt: " SAR 5720-5825 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xDE, VarStoreId: 0xF101, VarOffset: 0x9F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2C 02 06 02 DE 00 01 F1 F2 09 00 10 00 FF 01 }
0x31726: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3172C: 				End  { 29 02 }
0x3172E: 				Numeric Prompt: " SAR 5845-6135 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xDF, VarStoreId: 0xF101, VarOffset: 0x9F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2D 02 06 02 DF 00 01 F1 F3 09 00 10 00 FF 01 }
0x3173F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31745: 				End  { 29 02 }
0x31747: 				Numeric Prompt: " SAR 6155-6375 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE0, VarStoreId: 0xF101, VarOffset: 0x9F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2E 02 06 02 E0 00 01 F1 F4 09 00 10 00 FF 01 }
0x31758: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3175E: 				End  { 29 02 }
0x31760: 				Numeric Prompt: " SAR 6395-6495 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE1, VarStoreId: 0xF101, VarOffset: 0x9F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2F 02 06 02 E1 00 01 F1 F5 09 00 10 00 FF 01 }
0x31771: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31777: 				End  { 29 02 }
0x31779: 				Numeric Prompt: " SAR 6515-6675 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE2, VarStoreId: 0xF101, VarOffset: 0x9F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 30 02 06 02 E2 00 01 F1 F6 09 00 10 00 FF 01 }
0x3178A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31790: 				End  { 29 02 }
0x31792: 				Numeric Prompt: " SAR 6695-6835 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE3, VarStoreId: 0xF101, VarOffset: 0x9F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 31 02 06 02 E3 00 01 F1 F7 09 00 10 00 FF 01 }
0x317A3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x317A9: 				End  { 29 02 }
0x317AB: 				Numeric Prompt: " SAR 6855-7095 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE4, VarStoreId: 0xF101, VarOffset: 0x9F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 32 02 06 02 E4 00 01 F1 F8 09 00 10 00 FF 01 }
0x317BC: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x317C2: 				End  { 29 02 }
0x317C4: 				Numeric Prompt: " SAR 2400 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE5, VarStoreId: 0xF101, VarOffset: 0x762, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 33 02 06 02 E5 00 01 F1 62 07 00 10 00 FF 01 }
0x317D5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x317DB: 				End  { 29 02 }
0x317DD: 				Numeric Prompt: " SAR 5180-5320 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE6, VarStoreId: 0xF101, VarOffset: 0x763, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 34 02 06 02 E6 00 01 F1 63 07 00 10 00 FF 01 }
0x317EE: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x317F4: 				End  { 29 02 }
0x317F6: 				Numeric Prompt: " SAR 5340-5440 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE7, VarStoreId: 0xF101, VarOffset: 0x764, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 35 02 06 02 E7 00 01 F1 64 07 00 10 00 FF 01 }
0x31807: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3180D: 				End  { 29 02 }
0x3180F: 				Numeric Prompt: " SAR 5460-5700 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE8, VarStoreId: 0xF101, VarOffset: 0x765, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 36 02 06 02 E8 00 01 F1 65 07 00 10 00 FF 01 }
0x31820: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31826: 				End  { 29 02 }
0x31828: 				Numeric Prompt: " SAR 5720-5825 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xE9, VarStoreId: 0xF101, VarOffset: 0x766, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 37 02 06 02 E9 00 01 F1 66 07 00 10 00 FF 01 }
0x31839: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3183F: 				End  { 29 02 }
0x31841: 				Numeric Prompt: " SAR 5845-6135 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xEA, VarStoreId: 0xF101, VarOffset: 0x767, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 38 02 06 02 EA 00 01 F1 67 07 00 10 00 FF 01 }
0x31852: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31858: 				End  { 29 02 }
0x3185A: 				Numeric Prompt: " SAR 6155-6375 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xEB, VarStoreId: 0xF101, VarOffset: 0x768, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 39 02 06 02 EB 00 01 F1 68 07 00 10 00 FF 01 }
0x3186B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31871: 				End  { 29 02 }
0x31873: 				Numeric Prompt: " SAR 6395-6495 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xEC, VarStoreId: 0xF101, VarOffset: 0x769, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 3A 02 06 02 EC 00 01 F1 69 07 00 10 00 FF 01 }
0x31884: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3188A: 				End  { 29 02 }
0x3188C: 				Numeric Prompt: " SAR 6515-6675 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xED, VarStoreId: 0xF101, VarOffset: 0x76A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 3B 02 06 02 ED 00 01 F1 6A 07 00 10 00 FF 01 }
0x3189D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x318A3: 				End  { 29 02 }
0x318A5: 				Numeric Prompt: " SAR 6695-6835 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xEE, VarStoreId: 0xF101, VarOffset: 0x76B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 3C 02 06 02 EE 00 01 F1 6B 07 00 10 00 FF 01 }
0x318B6: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x318BC: 				End  { 29 02 }
0x318BE: 				Numeric Prompt: " SAR 6855-7095 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xEF, VarStoreId: 0xF101, VarOffset: 0x9F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 3D 02 06 02 EF 00 01 F1 F9 09 00 10 00 FF 01 }
0x318CF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x318D5: 				End  { 29 02 }
0x318D7: 				Numeric Prompt: " SAR 2400 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF0, VarStoreId: 0xF101, VarOffset: 0x9FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 3E 02 06 02 F0 00 01 F1 FA 09 00 10 00 FF 01 }
0x318E8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x318EE: 				End  { 29 02 }
0x318F0: 				Numeric Prompt: " SAR 5180-5320 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF1, VarStoreId: 0xF101, VarOffset: 0x9FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 3F 02 06 02 F1 00 01 F1 FB 09 00 10 00 FF 01 }
0x31901: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31907: 				End  { 29 02 }
0x31909: 				Numeric Prompt: " SAR 5340-5440 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF2, VarStoreId: 0xF101, VarOffset: 0x9FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 40 02 06 02 F2 00 01 F1 FC 09 00 10 00 FF 01 }
0x3191A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31920: 				End  { 29 02 }
0x31922: 				Numeric Prompt: " SAR 5460-5700 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF3, VarStoreId: 0xF101, VarOffset: 0x9FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 41 02 06 02 F3 00 01 F1 FD 09 00 10 00 FF 01 }
0x31933: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31939: 				End  { 29 02 }
0x3193B: 				Numeric Prompt: " SAR 5720-5825 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF4, VarStoreId: 0xF101, VarOffset: 0x9FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 42 02 06 02 F4 00 01 F1 FE 09 00 10 00 FF 01 }
0x3194C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31952: 				End  { 29 02 }
0x31954: 				Numeric Prompt: " SAR 5845-6135 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF5, VarStoreId: 0xF101, VarOffset: 0x9FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 43 02 06 02 F5 00 01 F1 FF 09 00 10 00 FF 01 }
0x31965: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3196B: 				End  { 29 02 }
0x3196D: 				Numeric Prompt: " SAR 6155-6375 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF6, VarStoreId: 0xF101, VarOffset: 0xA00, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 44 02 06 02 F6 00 01 F1 00 0A 00 10 00 FF 01 }
0x3197E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31984: 				End  { 29 02 }
0x31986: 				Numeric Prompt: " SAR 6395-6495 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF7, VarStoreId: 0xF101, VarOffset: 0xA01, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 45 02 06 02 F7 00 01 F1 01 0A 00 10 00 FF 01 }
0x31997: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3199D: 				End  { 29 02 }
0x3199F: 				Numeric Prompt: " SAR 6515-6675 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF8, VarStoreId: 0xF101, VarOffset: 0xA02, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 46 02 06 02 F8 00 01 F1 02 0A 00 10 00 FF 01 }
0x319B0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x319B6: 				End  { 29 02 }
0x319B8: 				Numeric Prompt: " SAR 6695-6835 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xF9, VarStoreId: 0xF101, VarOffset: 0xA03, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 47 02 06 02 F9 00 01 F1 03 0A 00 10 00 FF 01 }
0x319C9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x319CF: 				End  { 29 02 }
0x319D1: 				Numeric Prompt: " SAR 6855-7095 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xFA, VarStoreId: 0xF101, VarOffset: 0xA04, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 48 02 06 02 FA 00 01 F1 04 0A 00 10 00 FF 01 }
0x319E2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x319E8: 				End  { 29 02 }
0x319EA: 				Numeric Prompt: " SAR 2400 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xFB, VarStoreId: 0xF101, VarOffset: 0x76C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 49 02 06 02 FB 00 01 F1 6C 07 00 10 00 FF 01 }
0x319FB: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A01: 				End  { 29 02 }
0x31A03: 				Numeric Prompt: " SAR 5180-5320 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xFC, VarStoreId: 0xF101, VarOffset: 0x76D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4A 02 06 02 FC 00 01 F1 6D 07 00 10 00 FF 01 }
0x31A14: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A1A: 				End  { 29 02 }
0x31A1C: 				Numeric Prompt: " SAR 5340-5440 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xFD, VarStoreId: 0xF101, VarOffset: 0x76E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4B 02 06 02 FD 00 01 F1 6E 07 00 10 00 FF 01 }
0x31A2D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A33: 				End  { 29 02 }
0x31A35: 				Numeric Prompt: " SAR 5460-5700 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xFE, VarStoreId: 0xF101, VarOffset: 0x76F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4C 02 06 02 FE 00 01 F1 6F 07 00 10 00 FF 01 }
0x31A46: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A4C: 				End  { 29 02 }
0x31A4E: 				Numeric Prompt: " SAR 5720-5825 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0xFF, VarStoreId: 0xF101, VarOffset: 0x770, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4D 02 06 02 FF 00 01 F1 70 07 00 10 00 FF 01 }
0x31A5F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A65: 				End  { 29 02 }
0x31A67: 				Numeric Prompt: " SAR 5845-6135 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x100, VarStoreId: 0xF101, VarOffset: 0x771, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4E 02 06 02 00 01 01 F1 71 07 00 10 00 FF 01 }
0x31A78: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A7E: 				End  { 29 02 }
0x31A80: 				Numeric Prompt: " SAR 6155-6375 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x101, VarStoreId: 0xF101, VarOffset: 0x772, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4F 02 06 02 01 01 01 F1 72 07 00 10 00 FF 01 }
0x31A91: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31A97: 				End  { 29 02 }
0x31A99: 				Numeric Prompt: " SAR 6395-6495 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x102, VarStoreId: 0xF101, VarOffset: 0x773, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 50 02 06 02 02 01 01 F1 73 07 00 10 00 FF 01 }
0x31AAA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31AB0: 				End  { 29 02 }
0x31AB2: 				Numeric Prompt: " SAR 6515-6675 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x103, VarStoreId: 0xF101, VarOffset: 0x774, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 51 02 06 02 03 01 01 F1 74 07 00 10 00 FF 01 }
0x31AC3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31AC9: 				End  { 29 02 }
0x31ACB: 				Numeric Prompt: " SAR 6695-6835 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x104, VarStoreId: 0xF101, VarOffset: 0x775, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 52 02 06 02 04 01 01 F1 75 07 00 10 00 FF 01 }
0x31ADC: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31AE2: 				End  { 29 02 }
0x31AE4: 				Numeric Prompt: " SAR 6855-7095 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x105, VarStoreId: 0xF101, VarOffset: 0xA05, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 53 02 06 02 05 01 01 F1 05 0A 00 10 00 FF 01 }
0x31AF5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31AFB: 				End  { 29 02 }
0x31AFD: 				Numeric Prompt: " SAR 2400 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x106, VarStoreId: 0xF101, VarOffset: 0xA06, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 54 02 06 02 06 01 01 F1 06 0A 00 10 00 FF 01 }
0x31B0E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31B14: 				End  { 29 02 }
0x31B16: 				Numeric Prompt: " SAR 5180-5320 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x107, VarStoreId: 0xF101, VarOffset: 0xA07, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 55 02 06 02 07 01 01 F1 07 0A 00 10 00 FF 01 }
0x31B27: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31B2D: 				End  { 29 02 }
0x31B2F: 				Numeric Prompt: " SAR 5340-5440 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x108, VarStoreId: 0xF101, VarOffset: 0xA08, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 56 02 06 02 08 01 01 F1 08 0A 00 10 00 FF 01 }
0x31B40: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31B46: 				End  { 29 02 }
0x31B48: 				Numeric Prompt: " SAR 5460-5700 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x109, VarStoreId: 0xF101, VarOffset: 0xA09, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 57 02 06 02 09 01 01 F1 09 0A 00 10 00 FF 01 }
0x31B59: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31B5F: 				End  { 29 02 }
0x31B61: 				Numeric Prompt: " SAR 5720-5825 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x10A, VarStoreId: 0xF101, VarOffset: 0xA0A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 58 02 06 02 0A 01 01 F1 0A 0A 00 10 00 FF 01 }
0x31B72: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31B78: 				End  { 29 02 }
0x31B7A: 				Numeric Prompt: " SAR 5845-6135 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x10B, VarStoreId: 0xF101, VarOffset: 0xA0B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 59 02 06 02 0B 01 01 F1 0B 0A 00 10 00 FF 01 }
0x31B8B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31B91: 				End  { 29 02 }
0x31B93: 				Numeric Prompt: " SAR 6155-6375 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x10C, VarStoreId: 0xF101, VarOffset: 0xA0C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 5A 02 06 02 0C 01 01 F1 0C 0A 00 10 00 FF 01 }
0x31BA4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31BAA: 				End  { 29 02 }
0x31BAC: 				Numeric Prompt: " SAR 6395-6495 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x10D, VarStoreId: 0xF101, VarOffset: 0xA0D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 5B 02 06 02 0D 01 01 F1 0D 0A 00 10 00 FF 01 }
0x31BBD: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31BC3: 				End  { 29 02 }
0x31BC5: 				Numeric Prompt: " SAR 6515-6675 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x10E, VarStoreId: 0xF101, VarOffset: 0xA0E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 5C 02 06 02 0E 01 01 F1 0E 0A 00 10 00 FF 01 }
0x31BD6: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31BDC: 				End  { 29 02 }
0x31BDE: 				Numeric Prompt: " SAR 6695-6835 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x10F, VarStoreId: 0xF101, VarOffset: 0xA0F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 5D 02 06 02 0F 01 01 F1 0F 0A 00 10 00 FF 01 }
0x31BEF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31BF5: 				End  { 29 02 }
0x31BF7: 				Numeric Prompt: " SAR 6855-7095 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x110, VarStoreId: 0xF101, VarOffset: 0xA10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 5E 02 06 02 10 01 01 F1 10 0A 00 10 00 FF 01 }
0x31C08: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31C0E: 				End  { 29 02 }
0x31C10: 				Numeric Prompt: " SAR CDB 2400 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x111, VarStoreId: 0xF101, VarOffset: 0xA40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 76 02 06 02 11 01 01 F1 40 0A 00 10 00 FF 01 }
0x31C21: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31C27: 				End  { 29 02 }
0x31C29: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x112, VarStoreId: 0xF101, VarOffset: 0xA41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 77 02 06 02 12 01 01 F1 41 0A 00 10 00 FF 01 }
0x31C3A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31C40: 				End  { 29 02 }
0x31C42: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x113, VarStoreId: 0xF101, VarOffset: 0xA42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 78 02 06 02 13 01 01 F1 42 0A 00 10 00 FF 01 }
0x31C53: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31C59: 				End  { 29 02 }
0x31C5B: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x114, VarStoreId: 0xF101, VarOffset: 0xA43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 79 02 06 02 14 01 01 F1 43 0A 00 10 00 FF 01 }
0x31C6C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31C72: 				End  { 29 02 }
0x31C74: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x115, VarStoreId: 0xF101, VarOffset: 0xA44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 7A 02 06 02 15 01 01 F1 44 0A 00 10 00 FF 01 }
0x31C85: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31C8B: 				End  { 29 02 }
0x31C8D: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x116, VarStoreId: 0xF101, VarOffset: 0xA45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 7B 02 06 02 16 01 01 F1 45 0A 00 10 00 FF 01 }
0x31C9E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31CA4: 				End  { 29 02 }
0x31CA6: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x117, VarStoreId: 0xF101, VarOffset: 0xA46, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 7C 02 06 02 17 01 01 F1 46 0A 00 10 00 FF 01 }
0x31CB7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31CBD: 				End  { 29 02 }
0x31CBF: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x118, VarStoreId: 0xF101, VarOffset: 0xA47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 7D 02 06 02 18 01 01 F1 47 0A 00 10 00 FF 01 }
0x31CD0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31CD6: 				End  { 29 02 }
0x31CD8: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x119, VarStoreId: 0xF101, VarOffset: 0xA48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 7E 02 06 02 19 01 01 F1 48 0A 00 10 00 FF 01 }
0x31CE9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31CEF: 				End  { 29 02 }
0x31CF1: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x11A, VarStoreId: 0xF101, VarOffset: 0xA49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 7F 02 06 02 1A 01 01 F1 49 0A 00 10 00 FF 01 }
0x31D02: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D08: 				End  { 29 02 }
0x31D0A: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set2 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x11B, VarStoreId: 0xF101, VarOffset: 0xA4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 80 02 06 02 1B 01 01 F1 4A 0A 00 10 00 FF 01 }
0x31D1B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D21: 				End  { 29 02 }
0x31D23: 				Numeric Prompt: " SAR CDB 2400 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x11C, VarStoreId: 0xF101, VarOffset: 0xA4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 81 02 06 02 1C 01 01 F1 4B 0A 00 10 00 FF 01 }
0x31D34: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D3A: 				End  { 29 02 }
0x31D3C: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x11D, VarStoreId: 0xF101, VarOffset: 0xA4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 82 02 06 02 1D 01 01 F1 4C 0A 00 10 00 FF 01 }
0x31D4D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D53: 				End  { 29 02 }
0x31D55: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x11E, VarStoreId: 0xF101, VarOffset: 0xA4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 83 02 06 02 1E 01 01 F1 4D 0A 00 10 00 FF 01 }
0x31D66: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D6C: 				End  { 29 02 }
0x31D6E: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x11F, VarStoreId: 0xF101, VarOffset: 0xA4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 84 02 06 02 1F 01 01 F1 4E 0A 00 10 00 FF 01 }
0x31D7F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D85: 				End  { 29 02 }
0x31D87: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x120, VarStoreId: 0xF101, VarOffset: 0xA4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 85 02 06 02 20 01 01 F1 4F 0A 00 10 00 FF 01 }
0x31D98: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31D9E: 				End  { 29 02 }
0x31DA0: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x121, VarStoreId: 0xF101, VarOffset: 0xA50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 86 02 06 02 21 01 01 F1 50 0A 00 10 00 FF 01 }
0x31DB1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31DB7: 				End  { 29 02 }
0x31DB9: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x122, VarStoreId: 0xF101, VarOffset: 0xA51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 87 02 06 02 22 01 01 F1 51 0A 00 10 00 FF 01 }
0x31DCA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31DD0: 				End  { 29 02 }
0x31DD2: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x123, VarStoreId: 0xF101, VarOffset: 0xA52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 88 02 06 02 23 01 01 F1 52 0A 00 10 00 FF 01 }
0x31DE3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31DE9: 				End  { 29 02 }
0x31DEB: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set2 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x124, VarStoreId: 0xF101, VarOffset: 0xA53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 89 02 06 02 24 01 01 F1 53 0A 00 10 00 FF 01 }
0x31DFC: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E02: 				End  { 29 02 }
0x31E04: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set2 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x125, VarStoreId: 0xF101, VarOffset: 0xA54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 8A 02 5F 02 25 01 01 F1 54 0A 00 10 00 FF 01 }
0x31E15: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E1B: 				End  { 29 02 }
0x31E1D: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set2 Chain B", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x126, VarStoreId: 0xF101, VarOffset: 0xA55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 8B 02 5F 02 26 01 01 F1 55 0A 00 10 00 FF 01 }
0x31E2E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E34: 				End  { 29 02 }
0x31E36: 				Numeric Prompt: " SAR CDB 2400 MHz Set3 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x127, VarStoreId: 0xF101, VarOffset: 0xA56, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 8C 02 5F 02 27 01 01 F1 56 0A 00 10 00 FF 01 }
0x31E47: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E4D: 				End  { 29 02 }
0x31E4F: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set3 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x128, VarStoreId: 0xF101, VarOffset: 0xA57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 8D 02 5F 02 28 01 01 F1 57 0A 00 10 00 FF 01 }
0x31E60: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E66: 				End  { 29 02 }
0x31E68: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set3 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x129, VarStoreId: 0xF101, VarOffset: 0xA58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 8E 02 5F 02 29 01 01 F1 58 0A 00 10 00 FF 01 }
0x31E79: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E7F: 				End  { 29 02 }
0x31E81: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set3 Chain A", Help: "Defines the WiFi CDB SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x12A, VarStoreId: 0xF101, VarOffset: 0xA59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 8F 02 5F 02 2A 01 01 F1 59 0A 00 10 00 FF 01 }
0x31E92: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31E98: 				End  { 29 02 }
0x31E9A: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x12B, VarStoreId: 0xF101, VarOffset: 0xA5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 90 02 06 02 2B 01 01 F1 5A 0A 00 10 00 FF 01 }
0x31EAB: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31EB1: 				End  { 29 02 }
0x31EB3: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x12C, VarStoreId: 0xF101, VarOffset: 0xA5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 91 02 06 02 2C 01 01 F1 5B 0A 00 10 00 FF 01 }
0x31EC4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31ECA: 				End  { 29 02 }
0x31ECC: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x12D, VarStoreId: 0xF101, VarOffset: 0xA5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 92 02 06 02 2D 01 01 F1 5C 0A 00 10 00 FF 01 }
0x31EDD: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31EE3: 				End  { 29 02 }
0x31EE5: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x12E, VarStoreId: 0xF101, VarOffset: 0xA5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 93 02 06 02 2E 01 01 F1 5D 0A 00 10 00 FF 01 }
0x31EF6: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31EFC: 				End  { 29 02 }
0x31EFE: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x12F, VarStoreId: 0xF101, VarOffset: 0xA5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 94 02 06 02 2F 01 01 F1 5E 0A 00 10 00 FF 01 }
0x31F0F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31F15: 				End  { 29 02 }
0x31F17: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x130, VarStoreId: 0xF101, VarOffset: 0xA5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 95 02 06 02 30 01 01 F1 5F 0A 00 10 00 FF 01 }
0x31F28: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31F2E: 				End  { 29 02 }
0x31F30: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set3 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x131, VarStoreId: 0xF101, VarOffset: 0xA60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 96 02 06 02 31 01 01 F1 60 0A 00 10 00 FF 01 }
0x31F41: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31F47: 				End  { 29 02 }
0x31F49: 				Numeric Prompt: " SAR CDB 2400 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x132, VarStoreId: 0xF101, VarOffset: 0xA61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 97 02 06 02 32 01 01 F1 61 0A 00 10 00 FF 01 }
0x31F5A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31F60: 				End  { 29 02 }
0x31F62: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x133, VarStoreId: 0xF101, VarOffset: 0xA62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 98 02 06 02 33 01 01 F1 62 0A 00 10 00 FF 01 }
0x31F73: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31F79: 				End  { 29 02 }
0x31F7B: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x134, VarStoreId: 0xF101, VarOffset: 0xA63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 99 02 06 02 34 01 01 F1 63 0A 00 10 00 FF 01 }
0x31F8C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31F92: 				End  { 29 02 }
0x31F94: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x135, VarStoreId: 0xF101, VarOffset: 0xA64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 9A 02 06 02 35 01 01 F1 64 0A 00 10 00 FF 01 }
0x31FA5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31FAB: 				End  { 29 02 }
0x31FAD: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x136, VarStoreId: 0xF101, VarOffset: 0xA65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 9B 02 06 02 36 01 01 F1 65 0A 00 10 00 FF 01 }
0x31FBE: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31FC4: 				End  { 29 02 }
0x31FC6: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x137, VarStoreId: 0xF101, VarOffset: 0xA66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 9C 02 06 02 37 01 01 F1 66 0A 00 10 00 FF 01 }
0x31FD7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31FDD: 				End  { 29 02 }
0x31FDF: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x138, VarStoreId: 0xF101, VarOffset: 0xA67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 9D 02 06 02 38 01 01 F1 67 0A 00 10 00 FF 01 }
0x31FF0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x31FF6: 				End  { 29 02 }
0x31FF8: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x139, VarStoreId: 0xF101, VarOffset: 0xA68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 9E 02 06 02 39 01 01 F1 68 0A 00 10 00 FF 01 }
0x32009: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3200F: 				End  { 29 02 }
0x32011: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x13A, VarStoreId: 0xF101, VarOffset: 0xA69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 9F 02 06 02 3A 01 01 F1 69 0A 00 10 00 FF 01 }
0x32022: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32028: 				End  { 29 02 }
0x3202A: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x13B, VarStoreId: 0xF101, VarOffset: 0xA6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A0 02 06 02 3B 01 01 F1 6A 0A 00 10 00 FF 01 }
0x3203B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32041: 				End  { 29 02 }
0x32043: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set3 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x13C, VarStoreId: 0xF101, VarOffset: 0xA6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A1 02 06 02 3C 01 01 F1 6B 0A 00 10 00 FF 01 }
0x32054: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3205A: 				End  { 29 02 }
0x3205C: 				Numeric Prompt: " SAR CDB 2400 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x13D, VarStoreId: 0xF101, VarOffset: 0xA6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A2 02 06 02 3D 01 01 F1 6C 0A 00 10 00 FF 01 }
0x3206D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32073: 				End  { 29 02 }
0x32075: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x13E, VarStoreId: 0xF101, VarOffset: 0xA6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A3 02 06 02 3E 01 01 F1 6D 0A 00 10 00 FF 01 }
0x32086: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3208C: 				End  { 29 02 }
0x3208E: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x13F, VarStoreId: 0xF101, VarOffset: 0xA6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A4 02 06 02 3F 01 01 F1 6E 0A 00 10 00 FF 01 }
0x3209F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x320A5: 				End  { 29 02 }
0x320A7: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x140, VarStoreId: 0xF101, VarOffset: 0xA6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A5 02 06 02 40 01 01 F1 6F 0A 00 10 00 FF 01 }
0x320B8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x320BE: 				End  { 29 02 }
0x320C0: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x141, VarStoreId: 0xF101, VarOffset: 0xA70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A6 02 06 02 41 01 01 F1 70 0A 00 10 00 FF 01 }
0x320D1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x320D7: 				End  { 29 02 }
0x320D9: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x142, VarStoreId: 0xF101, VarOffset: 0xA71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A7 02 06 02 42 01 01 F1 71 0A 00 10 00 FF 01 }
0x320EA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x320F0: 				End  { 29 02 }
0x320F2: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x143, VarStoreId: 0xF101, VarOffset: 0xA72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A8 02 06 02 43 01 01 F1 72 0A 00 10 00 FF 01 }
0x32103: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32109: 				End  { 29 02 }
0x3210B: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x144, VarStoreId: 0xF101, VarOffset: 0xA73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A9 02 06 02 44 01 01 F1 73 0A 00 10 00 FF 01 }
0x3211C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32122: 				End  { 29 02 }
0x32124: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x145, VarStoreId: 0xF101, VarOffset: 0xA74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 AA 02 06 02 45 01 01 F1 74 0A 00 10 00 FF 01 }
0x32135: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3213B: 				End  { 29 02 }
0x3213D: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x146, VarStoreId: 0xF101, VarOffset: 0xA75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 AB 02 06 02 46 01 01 F1 75 0A 00 10 00 FF 01 }
0x3214E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32154: 				End  { 29 02 }
0x32156: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set4 Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x147, VarStoreId: 0xF101, VarOffset: 0xA76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 AC 02 06 02 47 01 01 F1 76 0A 00 10 00 FF 01 }
0x32167: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3216D: 				End  { 29 02 }
0x3216F: 				Numeric Prompt: " SAR CDB 2400 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x148, VarStoreId: 0xF101, VarOffset: 0xA77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 AD 02 06 02 48 01 01 F1 77 0A 00 10 00 FF 01 }
0x32180: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32186: 				End  { 29 02 }
0x32188: 				Numeric Prompt: " SAR CDB 5180-5320 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x149, VarStoreId: 0xF101, VarOffset: 0xA78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 AE 02 06 02 49 01 01 F1 78 0A 00 10 00 FF 01 }
0x32199: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3219F: 				End  { 29 02 }
0x321A1: 				Numeric Prompt: " SAR CDB 5340-5440 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x14A, VarStoreId: 0xF101, VarOffset: 0xA79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 AF 02 06 02 4A 01 01 F1 79 0A 00 10 00 FF 01 }
0x321B2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x321B8: 				End  { 29 02 }
0x321BA: 				Numeric Prompt: " SAR CDB 5460-5700 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x14B, VarStoreId: 0xF101, VarOffset: 0xA7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B0 02 06 02 4B 01 01 F1 7A 0A 00 10 00 FF 01 }
0x321CB: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x321D1: 				End  { 29 02 }
0x321D3: 				Numeric Prompt: " SAR CDB 5720-5825 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x14C, VarStoreId: 0xF101, VarOffset: 0xA7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B1 02 06 02 4C 01 01 F1 7B 0A 00 10 00 FF 01 }
0x321E4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x321EA: 				End  { 29 02 }
0x321EC: 				Numeric Prompt: " SAR CDB 5845-6135 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x14D, VarStoreId: 0xF101, VarOffset: 0xA7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B2 02 06 02 4D 01 01 F1 7C 0A 00 10 00 FF 01 }
0x321FD: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32203: 				End  { 29 02 }
0x32205: 				Numeric Prompt: " SAR CDB 6155-6375 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x14E, VarStoreId: 0xF101, VarOffset: 0xA7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B3 02 06 02 4E 01 01 F1 7D 0A 00 10 00 FF 01 }
0x32216: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3221C: 				End  { 29 02 }
0x3221E: 				Numeric Prompt: " SAR CDB 6395-6495 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x14F, VarStoreId: 0xF101, VarOffset: 0xA7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B4 02 06 02 4F 01 01 F1 7E 0A 00 10 00 FF 01 }
0x3222F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32235: 				End  { 29 02 }
0x32237: 				Numeric Prompt: " SAR CDB 6515-6675 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x150, VarStoreId: 0xF101, VarOffset: 0xA7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B5 02 06 02 50 01 01 F1 7F 0A 00 10 00 FF 01 }
0x32248: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3224E: 				End  { 29 02 }
0x32250: 				Numeric Prompt: " SAR CDB 6695-6835 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x151, VarStoreId: 0xF101, VarOffset: 0xA80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B6 02 06 02 51 01 01 F1 80 0A 00 10 00 FF 01 }
0x32261: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32267: 				End  { 29 02 }
0x32269: 				Numeric Prompt: " SAR CDB 6855-7095 MHz Set4 Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x152, VarStoreId: 0xF101, VarOffset: 0xA81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 B7 02 06 02 52 01 01 F1 81 0A 00 10 00 FF 01 }
0x3227A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32280: 				End  { 29 02 }
0x32282: 			End  { 29 02 }
0x32284: 			SuppressIf  { 0A 82 }
0x32286: 				True  { 46 02 }
0x32288: 				OneOf Prompt: "Antenna A Current Set", Help: "Current Set to be used 0 :Default OTP table 1-3 SAR Sets ", QuestionFlags: 0x10, QuestionId: 0x153, VarStoreId: 0xF101, VarOffset: 0x788, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 03 02 05 02 53 01 01 F1 88 07 10 10 00 04 00 }
0x32299: 					OneOfOption Option: "Default OTP table" Value: 0, Default, MfgDefault { 09 07 02 02 30 00 00 }
0x322A0: 					OneOfOption Option: "Set 1" Value: 1 { 09 07 FE 01 00 00 01 }
0x322A7: 					OneOfOption Option: "Set 2" Value: 2 { 09 07 FF 01 00 00 02 }
0x322AE: 					OneOfOption Option: "Set 3" Value: 3 { 09 07 00 02 00 00 03 }
0x322B5: 					OneOfOption Option: "Set 4" Value: 4 { 09 07 01 02 00 00 04 }
0x322BC: 				End  { 29 02 }
0x322BE: 			End  { 29 02 }
0x322C0: 			SuppressIf  { 0A 82 }
0x322C2: 				True  { 46 02 }
0x322C4: 				OneOf Prompt: "Antenna B Current Set", Help: "Current Set to be used 0 :Default OTP table 1-3 SAR Sets ", QuestionFlags: 0x10, QuestionId: 0x154, VarStoreId: 0xF101, VarOffset: 0x789, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 04 02 05 02 54 01 01 F1 89 07 10 10 00 04 00 }
0x322D5: 					OneOfOption Option: "Default OTP table" Value: 0, Default, MfgDefault { 09 07 02 02 30 00 00 }
0x322DC: 					OneOfOption Option: "Set 1" Value: 1 { 09 07 FE 01 00 00 01 }
0x322E3: 					OneOfOption Option: "Set 2" Value: 2 { 09 07 FF 01 00 00 02 }
0x322EA: 					OneOfOption Option: "Set 3" Value: 3 { 09 07 00 02 00 00 03 }
0x322F1: 					OneOfOption Option: "Set 4" Value: 4 { 09 07 01 02 00 00 04 }
0x322F8: 				End  { 29 02 }
0x322FA: 			End  { 29 02 }
0x322FC: 			Text Prompt: "WGDS Package", Help: "WGDS Package", Text: "" { 03 08 CF 02 CF 02 00 00 }
0x32304: 			Numeric Prompt: " Number of Groups", Help: "The Number of Group that supported. The first 3 Mandatory. 4-7 OEMs customizations.", QuestionFlags: 0x0, QuestionId: 0x155, VarStoreId: 0xF101, VarOffset: 0xB58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x8, Step: 0x1 { 07 91 D1 02 D2 02 55 01 01 F1 58 0B 00 10 00 08 01 }
0x32315: 				Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x3231B: 			End  { 29 02 }
0x3231D: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x156, VarStoreId: 0xF101, VarOffset: 0x776, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D3 02 D0 02 56 01 01 F1 76 07 00 10 00 FF 01 }
0x3232E: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32334: 			End  { 29 02 }
0x32336: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x157, VarStoreId: 0xF101, VarOffset: 0x777, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D4 02 D0 02 57 01 01 F1 77 07 00 10 00 FF 01 }
0x32347: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3234D: 			End  { 29 02 }
0x3234F: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x158, VarStoreId: 0xF101, VarOffset: 0x778, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D5 02 D0 02 58 01 01 F1 78 07 00 10 00 FF 01 }
0x32360: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32366: 			End  { 29 02 }
0x32368: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x159, VarStoreId: 0xF101, VarOffset: 0x779, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D6 02 D0 02 59 01 01 F1 79 07 00 10 00 FF 01 }
0x32379: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3237F: 			End  { 29 02 }
0x32381: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x15A, VarStoreId: 0xF101, VarOffset: 0x77A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D7 02 D0 02 5A 01 01 F1 7A 07 00 10 00 FF 01 }
0x32392: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32398: 			End  { 29 02 }
0x3239A: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 1 (FCC)", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x15B, VarStoreId: 0xF101, VarOffset: 0x77B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D8 02 06 02 5B 01 01 F1 7B 07 00 10 00 FF 01 }
0x323AB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x323B1: 			End  { 29 02 }
0x323B3: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x15C, VarStoreId: 0xF101, VarOffset: 0xA21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 D9 02 D0 02 5C 01 01 F1 21 0A 00 10 00 FF 01 }
0x323C4: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x323CA: 			End  { 29 02 }
0x323CC: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 1 (FCC)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x15D, VarStoreId: 0xF101, VarOffset: 0xA22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 DA 02 D0 02 5D 01 01 F1 22 0A 00 10 00 FF 01 }
0x323DD: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x323E3: 			End  { 29 02 }
0x323E5: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 1 (FCC)", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x15E, VarStoreId: 0xF101, VarOffset: 0xA23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 DB 02 06 02 5E 01 01 F1 23 0A 00 10 00 FF 01 }
0x323F6: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x323FC: 			End  { 29 02 }
0x323FE: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x15F, VarStoreId: 0xF101, VarOffset: 0x77C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 DC 02 D0 02 5F 01 01 F1 7C 07 00 10 00 FF 01 }
0x3240F: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32415: 			End  { 29 02 }
0x32417: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x160, VarStoreId: 0xF101, VarOffset: 0x77D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 DD 02 D0 02 60 01 01 F1 7D 07 00 10 00 FF 01 }
0x32428: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3242E: 			End  { 29 02 }
0x32430: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x161, VarStoreId: 0xF101, VarOffset: 0x77E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 DE 02 D0 02 61 01 01 F1 7E 07 00 10 00 FF 01 }
0x32441: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32447: 			End  { 29 02 }
0x32449: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x162, VarStoreId: 0xF101, VarOffset: 0x77F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 DF 02 D0 02 62 01 01 F1 7F 07 00 10 00 FF 01 }
0x3245A: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32460: 			End  { 29 02 }
0x32462: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x163, VarStoreId: 0xF101, VarOffset: 0x780, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E0 02 D0 02 63 01 01 F1 80 07 00 10 00 FF 01 }
0x32473: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32479: 			End  { 29 02 }
0x3247B: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x164, VarStoreId: 0xF101, VarOffset: 0x781, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E1 02 D0 02 64 01 01 F1 81 07 00 10 00 FF 01 }
0x3248C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32492: 			End  { 29 02 }
0x32494: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x165, VarStoreId: 0xF101, VarOffset: 0xA24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E2 02 D0 02 65 01 01 F1 24 0A 00 10 00 FF 01 }
0x324A5: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x324AB: 			End  { 29 02 }
0x324AD: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x166, VarStoreId: 0xF101, VarOffset: 0xA25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E3 02 D0 02 66 01 01 F1 25 0A 00 10 00 FF 01 }
0x324BE: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x324C4: 			End  { 29 02 }
0x324C6: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 2 (EU Japan)", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x167, VarStoreId: 0xF101, VarOffset: 0xA26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E4 02 06 02 67 01 01 F1 26 0A 00 10 00 FF 01 }
0x324D7: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x324DD: 			End  { 29 02 }
0x324DF: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x168, VarStoreId: 0xF101, VarOffset: 0x782, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E5 02 D0 02 68 01 01 F1 82 07 00 10 00 FF 01 }
0x324F0: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x324F6: 			End  { 29 02 }
0x324F8: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x169, VarStoreId: 0xF101, VarOffset: 0x783, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E6 02 D0 02 69 01 01 F1 83 07 00 10 00 FF 01 }
0x32509: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3250F: 			End  { 29 02 }
0x32511: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x16A, VarStoreId: 0xF101, VarOffset: 0x784, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E7 02 D0 02 6A 01 01 F1 84 07 00 10 00 FF 01 }
0x32522: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32528: 			End  { 29 02 }
0x3252A: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x16B, VarStoreId: 0xF101, VarOffset: 0x785, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E8 02 D0 02 6B 01 01 F1 85 07 00 10 00 FF 01 }
0x3253B: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32541: 			End  { 29 02 }
0x32543: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x16C, VarStoreId: 0xF101, VarOffset: 0x786, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E9 02 D0 02 6C 01 01 F1 86 07 00 10 00 FF 01 }
0x32554: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3255A: 			End  { 29 02 }
0x3255C: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 3 (ROW)", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x16D, VarStoreId: 0xF101, VarOffset: 0x787, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EA 02 06 02 6D 01 01 F1 87 07 00 10 00 FF 01 }
0x3256D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32573: 			End  { 29 02 }
0x32575: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x16E, VarStoreId: 0xF101, VarOffset: 0xA27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EB 02 D0 02 6E 01 01 F1 27 0A 00 10 00 FF 01 }
0x32586: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3258C: 			End  { 29 02 }
0x3258E: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 3 (ROW)", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x16F, VarStoreId: 0xF101, VarOffset: 0xA28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EC 02 D0 02 6F 01 01 F1 28 0A 00 10 00 FF 01 }
0x3259F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x325A5: 			End  { 29 02 }
0x325A7: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 3 (ROW)", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x170, VarStoreId: 0xF101, VarOffset: 0xA29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 ED 02 06 02 70 01 01 F1 29 0A 00 10 00 FF 01 }
0x325B8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x325BE: 			End  { 29 02 }
0x325C0: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x171, VarStoreId: 0xF101, VarOffset: 0xB59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EE 02 D0 02 71 01 01 F1 59 0B 00 10 00 FF 01 }
0x325D1: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x325D7: 			End  { 29 02 }
0x325D9: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x172, VarStoreId: 0xF101, VarOffset: 0xB5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EF 02 D0 02 72 01 01 F1 5A 0B 00 10 00 FF 01 }
0x325EA: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x325F0: 			End  { 29 02 }
0x325F2: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x173, VarStoreId: 0xF101, VarOffset: 0xB5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F0 02 D0 02 73 01 01 F1 5B 0B 00 10 00 FF 01 }
0x32603: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32609: 			End  { 29 02 }
0x3260B: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x174, VarStoreId: 0xF101, VarOffset: 0xB5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F1 02 D0 02 74 01 01 F1 5C 0B 00 10 00 FF 01 }
0x3261C: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32622: 			End  { 29 02 }
0x32624: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x175, VarStoreId: 0xF101, VarOffset: 0xB5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F2 02 D0 02 75 01 01 F1 5D 0B 00 10 00 FF 01 }
0x32635: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3263B: 			End  { 29 02 }
0x3263D: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 4", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x176, VarStoreId: 0xF101, VarOffset: 0xB5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F3 02 06 02 76 01 01 F1 5E 0B 00 10 00 FF 01 }
0x3264E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32654: 			End  { 29 02 }
0x32656: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x177, VarStoreId: 0xF101, VarOffset: 0xB5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F4 02 D0 02 77 01 01 F1 5F 0B 00 10 00 FF 01 }
0x32667: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3266D: 			End  { 29 02 }
0x3266F: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 4", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x178, VarStoreId: 0xF101, VarOffset: 0xB60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F5 02 D0 02 78 01 01 F1 60 0B 00 10 00 FF 01 }
0x32680: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32686: 			End  { 29 02 }
0x32688: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 4", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x179, VarStoreId: 0xF101, VarOffset: 0xB61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F6 02 06 02 79 01 01 F1 61 0B 00 10 00 FF 01 }
0x32699: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3269F: 			End  { 29 02 }
0x326A1: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x17A, VarStoreId: 0xF101, VarOffset: 0xB62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F7 02 D0 02 7A 01 01 F1 62 0B 00 10 00 FF 01 }
0x326B2: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x326B8: 			End  { 29 02 }
0x326BA: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x17B, VarStoreId: 0xF101, VarOffset: 0xB63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F8 02 D0 02 7B 01 01 F1 63 0B 00 10 00 FF 01 }
0x326CB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x326D1: 			End  { 29 02 }
0x326D3: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x17C, VarStoreId: 0xF101, VarOffset: 0xB64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F9 02 D0 02 7C 01 01 F1 64 0B 00 10 00 FF 01 }
0x326E4: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x326EA: 			End  { 29 02 }
0x326EC: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x17D, VarStoreId: 0xF101, VarOffset: 0xB65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FA 02 D0 02 7D 01 01 F1 65 0B 00 10 00 FF 01 }
0x326FD: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32703: 			End  { 29 02 }
0x32705: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x17E, VarStoreId: 0xF101, VarOffset: 0xB66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FB 02 D0 02 7E 01 01 F1 66 0B 00 10 00 FF 01 }
0x32716: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3271C: 			End  { 29 02 }
0x3271E: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 5", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x17F, VarStoreId: 0xF101, VarOffset: 0xB67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FC 02 06 02 7F 01 01 F1 67 0B 00 10 00 FF 01 }
0x3272F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32735: 			End  { 29 02 }
0x32737: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x180, VarStoreId: 0xF101, VarOffset: 0xB68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FD 02 D0 02 80 01 01 F1 68 0B 00 10 00 FF 01 }
0x32748: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3274E: 			End  { 29 02 }
0x32750: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 5", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x181, VarStoreId: 0xF101, VarOffset: 0xB69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FE 02 D0 02 81 01 01 F1 69 0B 00 10 00 FF 01 }
0x32761: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32767: 			End  { 29 02 }
0x32769: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 5", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x182, VarStoreId: 0xF101, VarOffset: 0xB6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FF 02 06 02 82 01 01 F1 6A 0B 00 10 00 FF 01 }
0x3277A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32780: 			End  { 29 02 }
0x32782: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x183, VarStoreId: 0xF101, VarOffset: 0xB6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 00 03 D0 02 83 01 01 F1 6B 0B 00 10 00 FF 01 }
0x32793: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32799: 			End  { 29 02 }
0x3279B: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x184, VarStoreId: 0xF101, VarOffset: 0xB6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 01 03 D0 02 84 01 01 F1 6C 0B 00 10 00 FF 01 }
0x327AC: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x327B2: 			End  { 29 02 }
0x327B4: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x185, VarStoreId: 0xF101, VarOffset: 0xB6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 02 03 D0 02 85 01 01 F1 6D 0B 00 10 00 FF 01 }
0x327C5: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x327CB: 			End  { 29 02 }
0x327CD: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x186, VarStoreId: 0xF101, VarOffset: 0xB6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 03 03 D0 02 86 01 01 F1 6E 0B 00 10 00 FF 01 }
0x327DE: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x327E4: 			End  { 29 02 }
0x327E6: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x187, VarStoreId: 0xF101, VarOffset: 0xB6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 04 03 D0 02 87 01 01 F1 6F 0B 00 10 00 FF 01 }
0x327F7: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x327FD: 			End  { 29 02 }
0x327FF: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 6", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x188, VarStoreId: 0xF101, VarOffset: 0xB70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 05 03 06 02 88 01 01 F1 70 0B 00 10 00 FF 01 }
0x32810: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32816: 			End  { 29 02 }
0x32818: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x189, VarStoreId: 0xF101, VarOffset: 0xB71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 06 03 D0 02 89 01 01 F1 71 0B 00 10 00 FF 01 }
0x32829: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3282F: 			End  { 29 02 }
0x32831: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 6", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x18A, VarStoreId: 0xF101, VarOffset: 0xB72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 07 03 D0 02 8A 01 01 F1 72 0B 00 10 00 FF 01 }
0x32842: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32848: 			End  { 29 02 }
0x3284A: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 6", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x18B, VarStoreId: 0xF101, VarOffset: 0xB73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 08 03 06 02 8B 01 01 F1 73 0B 00 10 00 FF 01 }
0x3285B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32861: 			End  { 29 02 }
0x32863: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x18C, VarStoreId: 0xF101, VarOffset: 0xB74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 09 03 D0 02 8C 01 01 F1 74 0B 00 10 00 FF 01 }
0x32874: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3287A: 			End  { 29 02 }
0x3287C: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x18D, VarStoreId: 0xF101, VarOffset: 0xB75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0A 03 D0 02 8D 01 01 F1 75 0B 00 10 00 FF 01 }
0x3288D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32893: 			End  { 29 02 }
0x32895: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x18E, VarStoreId: 0xF101, VarOffset: 0xB76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0B 03 D0 02 8E 01 01 F1 76 0B 00 10 00 FF 01 }
0x328A6: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x328AC: 			End  { 29 02 }
0x328AE: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x18F, VarStoreId: 0xF101, VarOffset: 0xB77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0C 03 D0 02 8F 01 01 F1 77 0B 00 10 00 FF 01 }
0x328BF: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x328C5: 			End  { 29 02 }
0x328C7: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x190, VarStoreId: 0xF101, VarOffset: 0xB78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0D 03 D0 02 90 01 01 F1 78 0B 00 10 00 FF 01 }
0x328D8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x328DE: 			End  { 29 02 }
0x328E0: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 7", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x191, VarStoreId: 0xF101, VarOffset: 0xB79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0E 03 06 02 91 01 01 F1 79 0B 00 10 00 FF 01 }
0x328F1: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x328F7: 			End  { 29 02 }
0x328F9: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x192, VarStoreId: 0xF101, VarOffset: 0xB7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0F 03 D0 02 92 01 01 F1 7A 0B 00 10 00 FF 01 }
0x3290A: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x32910: 			End  { 29 02 }
0x32912: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 7", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x193, VarStoreId: 0xF101, VarOffset: 0xB7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 10 03 D0 02 93 01 01 F1 7B 0B 00 10 00 FF 01 }
0x32923: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32929: 			End  { 29 02 }
0x3292B: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 7", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x194, VarStoreId: 0xF101, VarOffset: 0xB7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 11 03 06 02 94 01 01 F1 7C 0B 00 10 00 FF 01 }
0x3293C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32942: 			End  { 29 02 }
0x32944: 			Numeric Prompt: " SAR 2400 MHz Max Allowed for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x195, VarStoreId: 0xF101, VarOffset: 0xB7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 12 03 D0 02 95 01 01 F1 7D 0B 00 10 00 FF 01 }
0x32955: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x3295B: 			End  { 29 02 }
0x3295D: 			Numeric Prompt: " SAR 2400 MHz Chain A Offset for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x196, VarStoreId: 0xF101, VarOffset: 0xB7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 13 03 D0 02 96 01 01 F1 7E 0B 00 10 00 FF 01 }
0x3296E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32974: 			End  { 29 02 }
0x32976: 			Numeric Prompt: " SAR 2400 MHz Chain B Offset for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x197, VarStoreId: 0xF101, VarOffset: 0xB7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 14 03 D0 02 97 01 01 F1 7F 0B 00 10 00 FF 01 }
0x32987: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3298D: 			End  { 29 02 }
0x3298F: 			Numeric Prompt: " SAR 5200 MHz Max Allowed for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x198, VarStoreId: 0xF101, VarOffset: 0xB80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 15 03 D0 02 98 01 01 F1 80 0B 00 10 00 FF 01 }
0x329A0: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x329A6: 			End  { 29 02 }
0x329A8: 			Numeric Prompt: " SAR 5200 MHz Chain A Offset for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x199, VarStoreId: 0xF101, VarOffset: 0xB81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 16 03 D0 02 99 01 01 F1 81 0B 00 10 00 FF 01 }
0x329B9: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x329BF: 			End  { 29 02 }
0x329C1: 			Numeric Prompt: " SAR 5200 MHz Chain B Offset for Group 8", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x19A, VarStoreId: 0xF101, VarOffset: 0xB82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 17 03 06 02 9A 01 01 F1 82 0B 00 10 00 FF 01 }
0x329D2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x329D8: 			End  { 29 02 }
0x329DA: 			Numeric Prompt: " SAR 6000-7000 MHz Max Allowed for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x19B, VarStoreId: 0xF101, VarOffset: 0xB83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 18 03 D0 02 9B 01 01 F1 83 0B 00 10 00 FF 01 }
0x329EB: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x329F1: 			End  { 29 02 }
0x329F3: 			Numeric Prompt: " SAR 6000-7000 MHz Chain A Offset for Group 8", Help: "Defines the WiFi SAR Delta Value to be applied - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x19C, VarStoreId: 0xF101, VarOffset: 0xB84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 19 03 D0 02 9C 01 01 F1 84 0B 00 10 00 FF 01 }
0x32A04: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32A0A: 			End  { 29 02 }
0x32A0C: 			Numeric Prompt: " SAR 6000-7000 MHz Chain B Offset for Group 8", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x19D, VarStoreId: 0xF101, VarOffset: 0xB85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1A 03 06 02 9D 01 01 F1 85 0B 00 10 00 FF 01 }
0x32A1D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32A23: 			End  { 29 02 }
0x32A25: 			OneOf Prompt: "External 32kHz Clock", Help: "This will be used to specify that platform does have valid External 32kHz clock or not..", QuestionFlags: 0x10, QuestionId: 0x19E, VarStoreId: 0xF101, VarOffset: 0x9A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 03 8F 03 9E 01 01 F1 A9 09 10 10 00 01 00 }
0x32A36: 				OneOfOption Option: "Not Valid" Value: 0, Default, MfgDefault { 09 07 91 03 30 00 00 }
0x32A3D: 				OneOfOption Option: "Valid" Value: 1 { 09 07 90 03 00 00 01 }
0x32A44: 			End  { 29 02 }
0x32A46: 			Text Prompt: "PPAG Package", Help: "PPAG Package", Text: "" { 03 08 1B 03 1B 03 00 00 }
0x32A4E: 			OneOf Prompt: " WiFi ANT Gain control", Help: "Enable / Disable WiFi Antenna Gain control.", QuestionFlags: 0x10, QuestionId: 0x19F, VarStoreId: 0xF101, VarOffset: 0x9AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1C 03 1D 03 9F 01 01 F1 AA 09 10 10 00 01 00 }
0x32A5F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x32A66: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x32A6D: 			End  { 29 02 }
0x32A6F: 			Numeric Prompt: " ANT Gain 2400 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A0, VarStoreId: 0xF101, VarOffset: 0x9AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1E 03 34 03 A0 01 01 F1 AB 09 00 10 00 FF 01 }
0x32A80: 				Default DefaultId: 0x0 Value: 24 { 5B 06 00 00 00 18 }
0x32A86: 			End  { 29 02 }
0x32A88: 			Numeric Prompt: " ANT Gain 5180-5320 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A1, VarStoreId: 0xF101, VarOffset: 0x9AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1F 03 34 03 A1 01 01 F1 AC 09 00 10 00 FF 01 }
0x32A99: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32A9F: 			End  { 29 02 }
0x32AA1: 			Numeric Prompt: " Ant Gain 5340-5440 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A2, VarStoreId: 0xF101, VarOffset: 0x9AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 20 03 34 03 A2 01 01 F1 AD 09 00 10 00 FF 01 }
0x32AB2: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32AB8: 			End  { 29 02 }
0x32ABA: 			Numeric Prompt: " Ant Gain 5460-5700 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A3, VarStoreId: 0xF101, VarOffset: 0x9AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 21 03 34 03 A3 01 01 F1 AE 09 00 10 00 FF 01 }
0x32ACB: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32AD1: 			End  { 29 02 }
0x32AD3: 			Numeric Prompt: " Ant Gain 5720-5825 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A4, VarStoreId: 0xF101, VarOffset: 0x9AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 22 03 34 03 A4 01 01 F1 AF 09 00 10 00 FF 01 }
0x32AE4: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32AEA: 			End  { 29 02 }
0x32AEC: 			Numeric Prompt: " Ant Gain 5845-6135 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A5, VarStoreId: 0xF101, VarOffset: 0xA11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 23 03 34 03 A5 01 01 F1 11 0A 00 10 00 FF 01 }
0x32AFD: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32B03: 			End  { 29 02 }
0x32B05: 			Numeric Prompt: " Ant Gain 6155-6375 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A6, VarStoreId: 0xF101, VarOffset: 0xA12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 24 03 34 03 A6 01 01 F1 12 0A 00 10 00 FF 01 }
0x32B16: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32B1C: 			End  { 29 02 }
0x32B1E: 			Numeric Prompt: " Ant Gain 6395-6495 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A7, VarStoreId: 0xF101, VarOffset: 0xA13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 25 03 34 03 A7 01 01 F1 13 0A 00 10 00 FF 01 }
0x32B2F: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32B35: 			End  { 29 02 }
0x32B37: 			Numeric Prompt: " Ant Gain 6515-6675 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A8, VarStoreId: 0xF101, VarOffset: 0xA14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 26 03 34 03 A8 01 01 F1 14 0A 00 10 00 FF 01 }
0x32B48: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32B4E: 			End  { 29 02 }
0x32B50: 			Numeric Prompt: " Ant Gain 6695-6835 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1A9, VarStoreId: 0xF101, VarOffset: 0xA15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 27 03 34 03 A9 01 01 F1 15 0A 00 10 00 FF 01 }
0x32B61: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32B67: 			End  { 29 02 }
0x32B69: 			Numeric Prompt: " Ant Gain 6855-7095 MHz Chain A", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1AA, VarStoreId: 0xF101, VarOffset: 0xA16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 28 03 34 03 AA 01 01 F1 16 0A 00 10 00 FF 01 }
0x32B7A: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32B80: 			End  { 29 02 }
0x32B82: 			Numeric Prompt: " Ant Gain 2400 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1AB, VarStoreId: 0xF101, VarOffset: 0x9B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 29 03 34 03 AB 01 01 F1 B0 09 00 10 00 FF 01 }
0x32B93: 				Default DefaultId: 0x0 Value: 24 { 5B 06 00 00 00 18 }
0x32B99: 			End  { 29 02 }
0x32B9B: 			Numeric Prompt: " Ant Gain 5180-5320 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1AC, VarStoreId: 0xF101, VarOffset: 0x9B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2A 03 34 03 AC 01 01 F1 B1 09 00 10 00 FF 01 }
0x32BAC: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32BB2: 			End  { 29 02 }
0x32BB4: 			Numeric Prompt: " Ant Gain 5340-5440 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1AD, VarStoreId: 0xF101, VarOffset: 0x9B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2B 03 34 03 AD 01 01 F1 B2 09 00 10 00 FF 01 }
0x32BC5: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32BCB: 			End  { 29 02 }
0x32BCD: 			Numeric Prompt: " Ant Gain 5460-5700 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1AE, VarStoreId: 0xF101, VarOffset: 0x9B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2C 03 34 03 AE 01 01 F1 B3 09 00 10 00 FF 01 }
0x32BDE: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32BE4: 			End  { 29 02 }
0x32BE6: 			Numeric Prompt: " Ant Gain 5720-5825 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1AF, VarStoreId: 0xF101, VarOffset: 0x9B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2D 03 34 03 AF 01 01 F1 B4 09 00 10 00 FF 01 }
0x32BF7: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32BFD: 			End  { 29 02 }
0x32BFF: 			Numeric Prompt: " Ant Gain 5845-6135 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B0, VarStoreId: 0xF101, VarOffset: 0xA17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2E 03 34 03 B0 01 01 F1 17 0A 00 10 00 FF 01 }
0x32C10: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32C16: 			End  { 29 02 }
0x32C18: 			Numeric Prompt: " Ant Gain 6155-6375 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B1, VarStoreId: 0xF101, VarOffset: 0xA18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2F 03 34 03 B1 01 01 F1 18 0A 00 10 00 FF 01 }
0x32C29: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32C2F: 			End  { 29 02 }
0x32C31: 			Numeric Prompt: " Ant Gain 6395-6495 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B2, VarStoreId: 0xF101, VarOffset: 0xA19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 30 03 34 03 B2 01 01 F1 19 0A 00 10 00 FF 01 }
0x32C42: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32C48: 			End  { 29 02 }
0x32C4A: 			Numeric Prompt: " Ant Gain 6515-6675 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B3, VarStoreId: 0xF101, VarOffset: 0xA1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 31 03 34 03 B3 01 01 F1 1A 0A 00 10 00 FF 01 }
0x32C5B: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32C61: 			End  { 29 02 }
0x32C63: 			Numeric Prompt: " Ant Gain 6695-6835 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B4, VarStoreId: 0xF101, VarOffset: 0xA1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 32 03 34 03 B4 01 01 F1 1B 0A 00 10 00 FF 01 }
0x32C74: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32C7A: 			End  { 29 02 }
0x32C7C: 			Numeric Prompt: " Ant Gain 6855-7095 MHz Chain B", Help: "Defines the WiFi ANT gain Delta Value to be applied - 8bit signed Two's complement 0.125dB. 0x80  = 0b10000000 = -16dB; 0x7F = 0b01111111 = 15.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B5, VarStoreId: 0xF101, VarOffset: 0xA1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 33 03 34 03 B5 01 01 F1 1C 0A 00 10 00 FF 01 }
0x32C8D: 				Default DefaultId: 0x0 Value: 40 { 5B 06 00 00 00 28 }
0x32C93: 			End  { 29 02 }
0x32C95: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x32C9C: 			End  { 29 02 }
0x32C9E: 			OneOf Prompt: "External 32kHz Clock", Help: "This will be used to specify that platform does have valid External 32kHz clock or not..", QuestionFlags: 0x10, QuestionId: 0x1B6, VarStoreId: 0xF101, VarOffset: 0x9A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 03 8F 03 B6 01 01 F1 A9 09 10 10 00 01 00 }
0x32CAF: 				OneOfOption Option: "Not Valid" Value: 0, Default, MfgDefault { 09 07 91 03 30 00 00 }
0x32CB6: 				OneOfOption Option: "Valid" Value: 1 { 09 07 90 03 00 00 01 }
0x32CBD: 			End  { 29 02 }
0x32CBF: 			OneOf Prompt: "Bluetooth SAR", Help: "Define the mode of SAR control to be used.

Disabled: Tx power shall be mandated by device NVM

Enabled: Tx power shall be the minimum between BIOS SAR table and BT Device NVM (either Module or Platform)", QuestionFlags: 0x10, QuestionId: 0x1B7, VarStoreId: 0xF101, VarOffset: 0x78A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 03 47 03 B7 01 01 F1 8A 07 10 10 00 01 00 }
0x32CD0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x32CD7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x32CDE: 			End  { 29 02 }
0x32CE0: 			SuppressIf  { 0A 82 }
0x32CE2: 				EqIdVal QuestionId: 0x1B7, Value: 0x0 { 12 06 B7 01 00 00 }
0x32CE8: 				SuppressIf  { 0A 82 }
0x32CEA: 					EqIdVal QuestionId: 0x1113, Value: 0x0 { 12 06 13 11 00 00 }
0x32CF0: 					OneOf Prompt: " Bluetooth Increased Power Mode", Help: "Defines Bluetooth Increased Power Mode.
SAR Limitation feature enablement/disablement", QuestionFlags: 0x10, QuestionId: 0x1B8, VarStoreId: 0xF101, VarOffset: 0xBC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 03 49 03 B8 01 01 F1 C8 0B 10 10 00 01 00 }
0x32D01: 						OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x32D08: 						OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x32D0F: 					End  { 29 02 }
0x32D11: 					SuppressIf  { 0A 82 }
0x32D13: 						EqIdVal QuestionId: 0x1B8, Value: 0x0 { 12 06 B8 01 00 00 }
0x32D19: 						Numeric Prompt: " Bluetooth SAR Power Limit 2400 Chain A ", Help: "Bluetooth SAR power restriction for the Lower Band (LB) - 2400MHz frequency Chain A. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x1B9, VarStoreId: 0xF101, VarOffset: 0xBC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4A 03 4B 03 B9 01 01 F1 C9 0B 00 10 00 FF 01 }
0x32D2A: 							Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32D30: 						End  { 29 02 }
0x32D32: 					End  { 29 02 }
0x32D34: 				End  { 29 02 }
0x32D36: 				Numeric Prompt: " Bluetooth SAR BR ", Help: "Defines the SAR power restriction for BR Modulation", QuestionFlags: 0x0, QuestionId: 0x1BA, VarStoreId: 0xF101, VarOffset: 0x78B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4C 03 4D 03 BA 01 01 F1 8B 07 00 10 00 FF 01 }
0x32D47: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32D4D: 				End  { 29 02 }
0x32D4F: 				Numeric Prompt: " Bluetooth SAR EDR2 ", Help: "Defines the SAR power restriction for EDR2 Modulation", QuestionFlags: 0x0, QuestionId: 0x1BB, VarStoreId: 0xF101, VarOffset: 0x78C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4E 03 4F 03 BB 01 01 F1 8C 07 00 10 00 FF 01 }
0x32D60: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32D66: 				End  { 29 02 }
0x32D68: 				Numeric Prompt: " Bluetooth SAR EDR3 ", Help: "Defines the SAR power restriction for EDR3 Modulation", QuestionFlags: 0x0, QuestionId: 0x1BC, VarStoreId: 0xF101, VarOffset: 0x78D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 50 03 51 03 BC 01 01 F1 8D 07 00 10 00 FF 01 }
0x32D79: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32D7F: 				End  { 29 02 }
0x32D81: 				Numeric Prompt: " Bluetooth SAR LE ", Help: "Defines the SAR power restriction for LE Modulation", QuestionFlags: 0x0, QuestionId: 0x1BD, VarStoreId: 0xF101, VarOffset: 0x78E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 52 03 53 03 BD 01 01 F1 8E 07 00 10 00 FF 01 }
0x32D92: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32D98: 				End  { 29 02 }
0x32D9A: 				Numeric Prompt: " Bluetooth SAR LE 2Mhz", Help: "Defines the SAR power restriction for LE 2Mhz Modulation", QuestionFlags: 0x0, QuestionId: 0x1BE, VarStoreId: 0xF101, VarOffset: 0x78F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 54 03 55 03 BE 01 01 F1 8F 07 00 10 00 FF 01 }
0x32DAB: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32DB1: 				End  { 29 02 }
0x32DB3: 				Numeric Prompt: " Bluetooth SAR LE LR", Help: "Defines the SAR power restriction for LE LR Modulation", QuestionFlags: 0x0, QuestionId: 0x1BF, VarStoreId: 0xF101, VarOffset: 0x790, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 56 03 57 03 BF 01 01 F1 90 07 00 10 00 FF 01 }
0x32DC4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32DCA: 				End  { 29 02 }
0x32DCC: 			End  { 29 02 }
0x32DCE: 			Numeric Prompt: "Disable SRD Active Channels", Help: "Enable/Disable SRD Active Channels

 00 - ETSI 5.8 GHz SRD Active Scan Enable
 01 - ETSI 5.8 GHz SRD Passive Scan Enable
 02 - ETSI 5.8 GHz SRD Disabled", QuestionFlags: 0x0, QuestionId: 0x1C0, VarStoreId: 0xF101, VarOffset: 0x9D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x1 { 07 91 B8 02 B9 02 C0 01 01 F1 D7 09 00 10 00 02 01 }
0x32DDF: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32DE5: 			End  { 29 02 }
0x32DE7: 			Numeric Prompt: "Supported Indonesia 5.15-5.35 GHz Band", Help: "Enable/Disable Indonesia 5.15-5.35 GHz

 00 - Set 5.15-5.35 GHz to Disable in Indonesia
 01 - Set 5.15-5.35 GHz to Enable (Passive) in Indonesia
 02 - Reserved", QuestionFlags: 0x0, QuestionId: 0x1C1, VarStoreId: 0xF101, VarOffset: 0x9D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x1 { 07 91 BA 02 BB 02 C1 01 01 F1 D8 09 00 10 00 02 01 }
0x32DF8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32DFE: 			End  { 29 02 }
0x32E00: 			Numeric Prompt: "Ultra High Band Support", Help: "Please input HEX value.

Bit0
 '0' No override [Default]
 '1' Only allow countries enabled in the following bits
Bit1 - USA
 '0' USA 6GHz disable
 '1' 6GHz allowed in USA
Bit2 - Rest of World
Bit3 - EU countries
Bit4 - South Korea
Bit5 - Brazil
Bit6 - Chile
Bit7 - Japan
Bit8 - Canada
Below bits only support on Rpl Family CPU:
Bit9 - Morocco
Bit10 - Mongolia
Bit11 - Malaysia
Bit31:12 - Reserved", QuestionFlags: 0x10, QuestionId: 0x1C2, VarStoreId: 0xF101, VarOffset: 0x9DD, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A BC 02 BD 02 C2 01 01 F1 DD 09 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32E1A: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32E23: 			End  { 29 02 }
0x32E25: 			OneOf Prompt: "Regulatory Configurations", Help: "Enabling DRS for China Location", QuestionFlags: 0x10, QuestionId: 0x1C3, VarStoreId: 0xF101, VarOffset: 0xB3E, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x1, Step: 0x0 { 05 9A BE 02 BF 02 C3 01 01 F1 3E 0B 10 12 00 00 00 00 01 00 00 00 00 00 00 00 }
0x32E3F: 				OneOfOption Option: "Disable DRS for China Location" Value: 0, Default, MfgDefault { 09 0A C0 02 32 02 00 00 00 00 }
0x32E49: 				OneOfOption Option: "Enable DRS for China Location" Value: 1 { 09 0A C1 02 02 02 01 00 00 00 }
0x32E53: 			End  { 29 02 }
0x32E55: 			OneOf Prompt: "UART Configurations", Help: "TBD", QuestionFlags: 0x10, QuestionId: 0x1C4, VarStoreId: 0xF101, VarOffset: 0xB42, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x0, Step: 0x0 { 05 9A C2 02 C3 02 C4 01 01 F1 42 0B 10 12 00 00 00 00 00 00 00 00 00 00 00 00 }
0x32E6F: 				OneOfOption Option: "Default" Value: 0, Default, MfgDefault { 09 0A C4 02 32 02 00 00 00 00 }
0x32E79: 			End  { 29 02 }
0x32E7B: 			Numeric Prompt: "UNII-4", Help: "Control Enablement UNII-4 over certificate modules
Please input HEX value.

FCC
Bit0 - Apply changes over FCC, UNII-4 setting within module certification (Default Intel module definitions)
 '0' Work with WiFi FW/OTP definitions
 '1' Apply changes
Bit1 - UNII-4 mode on FCC
 '0' Disable UNII-4
 '1' Enable UNII-4

ETSI
Bit2 - Apply changes over ETSI, UNII-4 setting within module certification (Default Intel module definitions)
Bit3 - UNII-4 mode on ETSI

Bit31:4 - Reserved shall set to zeros", QuestionFlags: 0x10, QuestionId: 0x1C5, VarStoreId: 0xF101, VarOffset: 0xB46, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A C5 02 C6 02 C5 01 01 F1 46 0B 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32E95: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32E9E: 			End  { 29 02 }
0x32EA0: 			Numeric Prompt: "Indoor Control", Help: "Device for Indoor Use Only (Solar Family onwards)
Please input HEX value.

Bit0 - EU
Bit1 - Japan
Bit2 - China, applied only in case of China BIOS or DRS in China Enabled
Bit3 - USA
Bit31:4 - Reserved shall set to zeros", QuestionFlags: 0x10, QuestionId: 0x1C6, VarStoreId: 0xF101, VarOffset: 0xB4A, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A C7 02 C8 02 C6 01 01 F1 4A 0B 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32EBA: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32EC3: 			End  { 29 02 }
0x32EC5: 			SuppressIf  { 0A 82 }
0x32EC7: 				EqIdVal QuestionId: 0x1113, Value: 0x0 { 12 06 13 11 00 00 }
0x32ECD: 				Numeric Prompt: "Wi-Fi Band Selection", Help: "Give the ability to selectively enable/disable Wi-Fi bands on platform.
Please input HEX value.

Bit value
 '0' Band selection Controlled by NIC [Default]
 '1' Force disable the band
Bit0 - 2.4 GHz
Bit1 - 5.2 GHz
Bit2 - 5.3 GHz
Bit3 - 5.5 GHz
Bit4 - 5.8 GHz
Bit5 - 5.9 GHz
Bit6 - 6.2 GHz
Bit7 - 6.5 GHz
Bit8 - 6.6 GHz
Bit9 - 6.8 GHz
Bit10 - 7.0 GHz
Bit31:11 - Reserved", QuestionFlags: 0x10, QuestionId: 0x1C7, VarStoreId: 0xF101, VarOffset: 0xBC3, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A C9 02 CA 02 C7 01 01 F1 C3 0B 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32EE7: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32EF0: 				End  { 29 02 }
0x32EF2: 			End  { 29 02 }
0x32EF4: 			SuppressIf  { 0A 82 }
0x32EF6: 				EqIdVal QuestionId: 0x1113, Value: 0x0 { 12 06 13 11 00 00 }
0x32EFC: 				Numeric Prompt: "Wi-Fi Energy Detection Threshold", Help: "Please input HEX value.

Bit value
 '0' Use default EDT method
 '1' Use new EDT method
Bit0:1 - Reserved
Bit2 - For ETSI
Bit3:4 - Reserved
Bit5 - For FCC
Bit6:8 - Reserved
Bit9 - For HB 5150-5350
Bit10 - For HB 5350-5470
Bit11 - For HB 5470-5725
Bit12 - For HB 5725-5945
Bit13 - For UHB 5945-6165
Bit14 - For UHB 6165-6405
Bit15 - For UHB 6405-6525
Bit16 - For UHB 6525-6705
Bit17 - For UHB 6705-6865
Bit18 - For UHB 6865-7105
Bit31:19 - Reserved", QuestionFlags: 0x10, QuestionId: 0x1C8, VarStoreId: 0xF101, VarOffset: 0xBBF, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A CB 02 CC 02 C8 01 01 F1 BF 0B 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32F16: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32F1F: 				End  { 29 02 }
0x32F21: 			End  { 29 02 }
0x32F23: 			SuppressIf  { 0A 82 }
0x32F25: 				EqIdVal QuestionId: 0x1113, Value: 0x0 { 12 06 13 11 00 00 }
0x32F2B: 				Numeric Prompt: "Wi-Fi 7 enablement/disablement", Help: "Please input HEX value.

Bit0
 '0' No override [Default]
 '1' Force disable all countries that are not defined in the following bits
Bit1 - USA
 '0' USA Wi-Fi disable
 '1' Wi-Fi 7 allowed in the USA
Bit31:2 - Reserved", QuestionFlags: 0x10, QuestionId: 0x1C9, VarStoreId: 0xF101, VarOffset: 0xBBA, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A CD 02 CE 02 C9 01 01 F1 BA 0B 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32F45: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32F4E: 				End  { 29 02 }
0x32F50: 			End  { 29 02 }
0x32F52: 			Text Prompt: "WiFi Time Average SAR - WTAS", Help: "WiFi Time Average SAR - WTAS", Text: "" { 03 08 3E 03 3E 03 00 00 }
0x32F5A: 			Numeric Prompt: " WTAS Selection", Help: "Please input HEX value.

Bit0 - Enable TAS feature.
 '0' TAS Disabled [Default]
 '1' TAS Enabled
Bit1 - IEC Optimization, override NIC configuration (BIOSoverideTASrIEC),Allow override NIC defaults.
 '0' No override, use device settings.
 '1' Override IEC Optimization, effected over certified NIC. The Value will set by Bit #2.
Bit2 - IEC Optimization Control Valve (BIOCenTrIC).This bit impact only incase that Bit #1 set to ‘1’ and the NIC is certified to support TAS over IEC.
 '0' Disabled TAS IEC optimization regulatory averaging time
 '1' Enabled TAS IEC optimization regulatory averaging time
Bit31:3 - Reserved", QuestionFlags: 0x10, QuestionId: 0x1CA, VarStoreId: 0xF101, VarOffset: 0xB89, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 3F 03 40 03 CA 01 01 F1 89 0B 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x32F74: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x32F7D: 			End  { 29 02 }
0x32F7F: 			SuppressIf  { 0A 82 }
0x32F81: 				EqIdVal QuestionId: 0x1CA, Value: 0x0 { 12 06 CA 01 00 00 }
0x32F87: 				Numeric Prompt: " WTAS List Entries", Help: "No. of blocked countries not approved by OEM to support this feature.", QuestionFlags: 0x0, QuestionId: 0x1CB, VarStoreId: 0xF101, VarOffset: 0xA9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 42 03 43 03 CB 01 01 F1 9D 0A 00 10 00 0F 01 }
0x32F98: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x32F9E: 				End  { 29 02 }
0x32FA0: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1CC, VarStoreId: 0xF101, VarOffset: 0xAA7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 44 03 45 03 CC 01 01 F1 A7 0A 00 11 00 00 FF FF 01 00 }
0x32FB4: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x32FBB: 				End  { 29 02 }
0x32FBD: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1CD, VarStoreId: 0xF101, VarOffset: 0xAA9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 93 03 45 03 CD 01 01 F1 A9 0A 00 11 00 00 FF FF 01 00 }
0x32FD1: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x32FD8: 				End  { 29 02 }
0x32FDA: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1CE, VarStoreId: 0xF101, VarOffset: 0xAAB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 94 03 45 03 CE 01 01 F1 AB 0A 00 11 00 00 FF FF 01 00 }
0x32FEE: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x32FF5: 				End  { 29 02 }
0x32FF7: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1CF, VarStoreId: 0xF101, VarOffset: 0xAAD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 95 03 45 03 CF 01 01 F1 AD 0A 00 11 00 00 FF FF 01 00 }
0x3300B: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x33012: 				End  { 29 02 }
0x33014: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D0, VarStoreId: 0xF101, VarOffset: 0xAAF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 96 03 45 03 D0 01 01 F1 AF 0A 00 11 00 00 FF FF 01 00 }
0x33028: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3302F: 				End  { 29 02 }
0x33031: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D1, VarStoreId: 0xF101, VarOffset: 0xAB1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 97 03 45 03 D1 01 01 F1 B1 0A 00 11 00 00 FF FF 01 00 }
0x33045: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3304C: 				End  { 29 02 }
0x3304E: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D2, VarStoreId: 0xF101, VarOffset: 0xAB3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 98 03 45 03 D2 01 01 F1 B3 0A 00 11 00 00 FF FF 01 00 }
0x33062: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x33069: 				End  { 29 02 }
0x3306B: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D3, VarStoreId: 0xF101, VarOffset: 0xAB5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 99 03 45 03 D3 01 01 F1 B5 0A 00 11 00 00 FF FF 01 00 }
0x3307F: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x33086: 				End  { 29 02 }
0x33088: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D4, VarStoreId: 0xF101, VarOffset: 0xAB7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9A 03 45 03 D4 01 01 F1 B7 0A 00 11 00 00 FF FF 01 00 }
0x3309C: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x330A3: 				End  { 29 02 }
0x330A5: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D5, VarStoreId: 0xF101, VarOffset: 0xAB9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9B 03 45 03 D5 01 01 F1 B9 0A 00 11 00 00 FF FF 01 00 }
0x330B9: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x330C0: 				End  { 29 02 }
0x330C2: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D6, VarStoreId: 0xF101, VarOffset: 0xABB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9C 03 45 03 D6 01 01 F1 BB 0A 00 11 00 00 FF FF 01 00 }
0x330D6: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x330DD: 				End  { 29 02 }
0x330DF: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D7, VarStoreId: 0xF101, VarOffset: 0xABD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9D 03 45 03 D7 01 01 F1 BD 0A 00 11 00 00 FF FF 01 00 }
0x330F3: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x330FA: 				End  { 29 02 }
0x330FC: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D8, VarStoreId: 0xF101, VarOffset: 0xABF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9E 03 45 03 D8 01 01 F1 BF 0A 00 11 00 00 FF FF 01 00 }
0x33110: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x33117: 				End  { 29 02 }
0x33119: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1D9, VarStoreId: 0xF101, VarOffset: 0xAC1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9F 03 45 03 D9 01 01 F1 C1 0A 00 11 00 00 FF FF 01 00 }
0x3312D: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x33134: 				End  { 29 02 }
0x33136: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1DA, VarStoreId: 0xF101, VarOffset: 0xAC3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 A0 03 45 03 DA 01 01 F1 C3 0A 00 11 00 00 FF FF 01 00 }
0x3314A: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x33151: 				End  { 29 02 }
0x33153: 				Numeric Prompt: " ISO country code to block", Help: "The decimal equivalent of country code (a two-ASCII-character) as specified in ISO_3166-1. Ex. for JP - 19024", QuestionFlags: 0x0, QuestionId: 0x1DB, VarStoreId: 0xF101, VarOffset: 0xAC5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 A1 03 45 03 DB 01 01 F1 C5 0A 00 11 00 00 FF FF 01 00 }
0x33167: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3316E: 				End  { 29 02 }
0x33170: 			End  { 29 02 }
0x33172: 			Text Prompt: "WLAN/WWAN Antenna Isolation", Help: "WLAN/WWAN Antenna Isolation", Text: "" { 03 08 5A 03 5A 03 00 00 }
0x3317A: 			Numeric Prompt: " WLAN/WWAN Low Band Isolation", Help: "Isolation between WLAN and WWAN in WiFi Low Band (2.4 GHz).
Range: 15 - 40 dB", QuestionFlags: 0x0, QuestionId: 0x1DC, VarStoreId: 0xF101, VarOffset: 0xB56, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x28, Step: 0x1 { 07 91 5B 03 5C 03 DC 01 01 F1 56 0B 00 10 0F 28 01 }
0x3318B: 				Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x33191: 			End  { 29 02 }
0x33193: 			Numeric Prompt: " WLAN/WWAN High Band Isolation", Help: "Isolation between WLAN and WWAN in WiFi High Band (5.2-7 GHz).
Range: 15 - 40 dB", QuestionFlags: 0x0, QuestionId: 0x1DD, VarStoreId: 0xF101, VarOffset: 0xB57, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x28, Step: 0x1 { 07 91 5D 03 5E 03 DD 01 01 F1 57 0B 00 10 0F 28 01 }
0x331A4: 				Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x331AA: 			End  { 29 02 }
0x331AC: 		End  { 29 02 }
0x331AE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x331B5: 		End  { 29 02 }
0x331B7: 		Ref Prompt: "WWAN Configuration", Help: "Configure WWAN related options", QuestionFlags: 0x0, QuestionId: 0x1DE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2724 { 0F 0F 75 03 76 03 DE 01 00 00 FF FF 00 24 27 }
0x331C6: 	End  { 29 02 }
0x331C8: 	Form FormId: 0x2724, Title: "WWAN Configuration" { 01 86 24 27 75 03 }
0x331CE: 		OneOf Prompt: "WWAN Device", Help: "Select the M.2 WWAN Device options to enable 4G - 7360/7560 (Intel), 5G - M80 (MediaTek) Modems", QuestionFlags: 0x10, QuestionId: 0x1DF, VarStoreId: 0xF101, VarOffset: 0x81D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 77 03 78 03 DF 01 01 F1 1D 08 10 10 00 02 00 }
0x331DF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x331E6: 			OneOfOption Option: "4G - 7360/7560" Value: 1 { 09 07 79 03 00 00 01 }
0x331ED: 			OneOfOption Option: "5G - M80" Value: 2 { 09 07 7A 03 00 00 02 }
0x331F4: 		End  { 29 02 }
0x331F6: 		SuppressIf  { 0A 82 }
0x331F8: 			EqIdVal QuestionId: 0x1DF, Value: 0x0 { 12 06 DF 01 00 00 }
0x331FE: 			OneOf Prompt: "Firmware Flash Device", Help: "Enable or Disable WWAN Firmware Flash Device", QuestionFlags: 0x10, QuestionId: 0x1E0, VarStoreId: 0xF101, VarOffset: 0xADB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 81 03 82 03 E0 01 01 F1 DB 0A 10 10 00 01 00 }
0x3320F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x33216: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3321D: 			End  { 29 02 }
0x3321F: 			OneOf Prompt: "Wireless CNV Config Device", Help: "Enable or Disable WCCD ACPI device node", QuestionFlags: 0x10, QuestionId: 0x1E1, VarStoreId: 0xF101, VarOffset: 0xB51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 83 03 84 03 E1 01 01 F1 51 0B 10 10 00 01 00 }
0x33230: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33237: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3323E: 			End  { 29 02 }
0x33240: 		End  { 29 02 }
0x33242: 		SuppressIf  { 0A 82 }
0x33244: 			EqIdVal QuestionId: 0x1DF, Value: 0x0 { 12 06 DF 01 00 00 }
0x3324A: 			OneOf Prompt: "WWAN Reset Workaround", Help: "Enabling this workardound will result in BIOS asserting FULL_CARD_POWER_OFF#, PERST# and RESET# WWAN signals before the WWAN Device Power-On Sequence is executed.
Disabling it has no impact.", QuestionFlags: 0x10, QuestionId: 0x1E2, VarStoreId: 0xF101, VarOffset: 0x86D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7B 03 7C 03 E2 01 01 F1 6D 08 10 10 00 01 00 }
0x3325B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33262: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33269: 			End  { 29 02 }
0x3326B: 		End  { 29 02 }
0x3326D: 		SuppressIf  { 0A 82 }
0x3326F: 			EqIdVal QuestionId: 0x1DF, Value: 0x2 { 12 86 DF 01 02 00 }
0x33275: 				Not  { 17 02 }
0x33277: 			End  { 29 02 }
0x33279: 			Numeric Prompt: "WA - WWAN OEM SVID", Help: "WWAN OEM Sub-Vendor ID", QuestionFlags: 0x10, QuestionId: 0x1E3, VarStoreId: 0xF101, VarOffset: 0xB37, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 7D 03 7E 03 E3 01 01 F1 37 0B 10 21 00 00 FF FF 01 00 }
0x3328D: 				Default DefaultId: 0x0 Value: 7416 { 5B 07 00 00 01 F8 1C }
0x33294: 			End  { 29 02 }
0x33296: 			Numeric Prompt: "WA - WWAN SVID Detect Timeout", Help: "The timeout value (ms) for detecting WWAN OEM SVID. Please notice it's workaround for OEM only.", QuestionFlags: 0x10, QuestionId: 0x1E4, VarStoreId: 0xF101, VarOffset: 0xB39, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 7F 03 80 03 E4 01 01 F1 39 0B 10 11 00 00 FF FF 01 00 }
0x332AA: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x332B1: 			End  { 29 02 }
0x332B3: 		End  { 29 02 }
0x332B5: 	End  { 29 02 }
0x332B7: 	Form FormId: 0x275C, Title: "CPU Configuration" { 01 86 5C 27 A3 03 }
0x332BD: 		Subtitle Prompt: "CPU Configuration", Help: "", Flags: 0x0 { 02 87 A3 03 00 00 00 }
0x332C4: 		End  { 29 02 }
0x332C6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x332CD: 		End  { 29 02 }
0x332CF: 		SuppressIf  { 0A 82 }
0x332D1: 			EqIdVal QuestionId: 0x11E5, Value: 0x0 { 12 86 E5 11 00 00 }
0x332D7: 				EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 06 ED 01 00 00 }
0x332DD: 				Or  { 16 02 }
0x332DF: 			End  { 29 02 }
0x332E1: 			Ref Prompt: "Efficient-core Information", Help: "Displays the E-core Information", QuestionFlags: 0x0, QuestionId: 0x1E5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275D { 0F 0F 9B 07 9C 07 E5 01 00 00 FF FF 00 5D 27 }
0x332F0: 		End  { 29 02 }
0x332F2: 		GrayOutIf  { 19 82 }
0x332F4: 			EqIdVal QuestionId: 0x1210, Value: 0x0 { 12 86 10 12 00 00 }
0x332FA: 				EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x33300: 				Or  { 16 02 }
0x33302: 			End  { 29 02 }
0x33304: 			Ref Prompt: "Performance-core Information", Help: "Displays the P-core Information", QuestionFlags: 0x0, QuestionId: 0x1E6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275E { 0F 0F 9D 07 9E 07 E6 01 00 00 FF FF 00 5E 27 }
0x33313: 		End  { 29 02 }
0x33315: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3331C: 		End  { 29 02 }
0x3331E: 		Text Prompt: "ID", Help: "Displays the Processor ID.", Text: "N/A" { 03 08 4E 04 50 04 4F 04 }
0x33326: 		Text Prompt: "Brand String", Help: "Brand String of the Performance Processor", Text: "N/A" { 03 08 4B 04 4C 04 4D 04 }
0x3332E: 		Text Prompt: "VMX", Help: "VMX Supported or Not", Text: "N/A" { 03 08 69 04 6A 04 6B 04 }
0x33336: 		Text Prompt: "SMX/TXT", Help: "SMX/TXT Supported or Not", Text: "N/A" { 03 08 6C 04 6D 04 6E 04 }
0x3333E: 		Text Prompt: "TXT Crash Code ", Help: "TXT Crash Code Register value", Text: "N/A" { 03 08 6F 04 70 04 71 04 }
0x33346: 		Text Prompt: "TXT SPAD ", Help: "TXT SPAD Register value", Text: "N/A" { 03 08 72 04 73 04 74 04 }
0x3334E: 		Text Prompt: "Boot Guard Status ", Help: "Boot Guard Status Register value", Text: "N/A" { 03 08 75 04 76 04 77 04 }
0x33356: 		Text Prompt: "Boot Guard ACM Policy Status ", Help: "Boot Guard ACM Policy Status value", Text: "N/A" { 03 08 78 04 79 04 7A 04 }
0x3335E: 		Text Prompt: "Boot Guard SACM Information ", Help: "Boot Guard SACM Info MSR value", Text: "N/A" { 03 08 7B 04 7C 04 7D 04 }
0x33366: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3336D: 		End  { 29 02 }
0x3336F: 		SuppressIf  { 0A 82 }
0x33371: 			EqIdVal QuestionId: 0x1225, Value: 0x0 { 12 06 25 12 00 00 }
0x33377: 			OneOf Prompt: "C6DRAM", Help: "Enable/Disable moving of DRAM contents to PRM memory when CPU is in C6 state", QuestionFlags: 0x10, QuestionId: 0x2725, VarStoreId: 0x1, VarOffset: 0x114, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 07 71 07 25 27 01 00 14 01 10 10 00 01 00 }
0x33388: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3338E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33395: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3339C: 			End  { 29 02 }
0x3339E: 		End  { 29 02 }
0x333A0: 		OneOf Prompt: "CPU Flex Ratio Override", Help: "Enable/Disable CPU Flex Ratio Programming", QuestionFlags: 0x10, QuestionId: 0x1E7, VarStoreId: 0x1, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 04 83 04 E7 01 01 00 03 00 10 10 00 01 00 }
0x333B1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x333B8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x333BF: 		End  { 29 02 }
0x333C1: 		GrayOutIf  { 19 82 }
0x333C3: 			EqIdVal QuestionId: 0x1E7, Value: 0x0 { 12 06 E7 01 00 00 }
0x333C9: 			Numeric Prompt: "CPU Flex Ratio Settings", Help: "This value must be between Max Efficiency Ratio (LFM) and Maximum non-turbo ratio set by Hardware (HFM).", QuestionFlags: 0x14, QuestionId: 0x2726, VarStoreId: 0x1, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x0 { 07 91 80 04 81 04 26 27 01 00 01 00 14 10 00 3F 00 }
0x333DA: 				Default DefaultId: 0x0 Value: 20 { 5B 06 00 00 00 14 }
0x333E0: 			End  { 29 02 }
0x333E2: 		End  { 29 02 }
0x333E4: 		OneOf Prompt: "Hardware Prefetcher", Help: "To turn on/off the MLC streamer prefetcher.", QuestionFlags: 0x10, QuestionId: 0x1E8, VarStoreId: 0x1, VarOffset: 0xBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 04 B8 04 E8 01 01 00 BF 00 10 10 00 01 00 }
0x333F5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x333FC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33403: 		End  { 29 02 }
0x33405: 		OneOf Prompt: "Adjacent Cache Line Prefetch", Help: "To turn on/off prefetching of adjacent cache lines.", QuestionFlags: 0x10, QuestionId: 0x1E9, VarStoreId: 0x1, VarOffset: 0xC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 04 BA 04 E9 01 01 00 C0 00 10 10 00 01 00 }
0x33416: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3341D: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33424: 		End  { 29 02 }
0x33426: 		SuppressIf  { 0A 82 }
0x33428: 			EqIdVal QuestionId: 0x1224, Value: 0x0 { 12 06 24 12 00 00 }
0x3342E: 			GrayOutIf  { 19 82 }
0x33430: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x33436: 				OneOf Prompt: "Intel (VMX) Virtualization Technology", Help: "When enabled, a VMM can utilize the additional hardware capabilities provided by Vanderpool Technology.", QuestionFlags: 0x10, QuestionId: 0x2727, VarStoreId: 0x1, VarOffset: 0xB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 04 BC 04 27 27 01 00 B9 00 10 10 00 01 00 }
0x33447: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3344E: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33455: 				End  { 29 02 }
0x33457: 			End  { 29 02 }
0x33459: 		End  { 29 02 }
0x3345B: 		OneOf Prompt: "PECI", Help: "Enable/Disable PECI", QuestionFlags: 0x10, QuestionId: 0x1EA, VarStoreId: 0x1, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 04 85 04 EA 01 01 00 04 00 10 10 00 01 00 }
0x3346C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33473: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3347A: 		End  { 29 02 }
0x3347C: 		OneOf Prompt: "AVX", Help: "Enable/Disable the Avx 2 Instructions. This is applicable for Performance-core only", QuestionFlags: 0x10, QuestionId: 0x1EB, VarStoreId: 0x1, VarOffset: 0x2DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 07 85 07 EB 01 01 00 DC 02 10 10 00 01 00 }
0x3348D: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x33494: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x3349B: 		End  { 29 02 }
0x3349D: 		GrayOutIf  { 19 82 }
0x3349F: 			EqIdVal QuestionId: 0x2729, Value: 0x1 { 12 06 29 27 01 00 }
0x334A5: 			SuppressIf  { 0A 82 }
0x334A7: 				EqIdVal QuestionId: 0x1210, Value: 0x0 { 12 06 10 12 00 00 }
0x334AD: 				GrayOutIf  { 19 82 }
0x334AF: 					EqIdVal QuestionId: 0x2882, Value: 0x1 { 12 06 82 28 01 00 }
0x334B5: 					OneOf Prompt: "Active Performance-cores", Help: "Number of P-cores to enable in each processor package. Note: Number of Cores and E-cores are looked at together. When both are {0,0}, Pcode will enable all cores.", QuestionFlags: 0x10, QuestionId: 0x1EC, VarStoreId: 0x1, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFF, Step: 0x0 { 05 91 A1 04 A2 04 EC 01 01 00 06 00 10 10 01 FF 00 }
0x334C6: 						OneOfOption Option: "All" Value: 255, Default, MfgDefault { 09 07 B6 04 30 00 FF }
0x334CD: 						SuppressIf  { 0A 82 }
0x334CF: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x334D3: 								Uint8 Value: 0x8 { 42 03 08 }
0x334D6: 								LessThan  { 33 02 }
0x334D8: 							End  { 29 02 }
0x334DA: 							OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x334E1: 						End  { 29 02 }
0x334E3: 						SuppressIf  { 0A 82 }
0x334E5: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x334E9: 								Uint8 Value: 0x7 { 42 03 07 }
0x334EC: 								LessThan  { 33 02 }
0x334EE: 							End  { 29 02 }
0x334F0: 							OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x334F7: 						End  { 29 02 }
0x334F9: 						SuppressIf  { 0A 82 }
0x334FB: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x334FF: 								Uint8 Value: 0x6 { 42 03 06 }
0x33502: 								LessThan  { 33 02 }
0x33504: 							End  { 29 02 }
0x33506: 							OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x3350D: 						End  { 29 02 }
0x3350F: 						SuppressIf  { 0A 82 }
0x33511: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x33515: 								Uint8 Value: 0x5 { 42 03 05 }
0x33518: 								LessThan  { 33 02 }
0x3351A: 							End  { 29 02 }
0x3351C: 							OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x33523: 						End  { 29 02 }
0x33525: 						SuppressIf  { 0A 82 }
0x33527: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x3352B: 								Uint8 Value: 0x4 { 42 03 04 }
0x3352E: 								LessThan  { 33 02 }
0x33530: 							End  { 29 02 }
0x33532: 							OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x33539: 						End  { 29 02 }
0x3353B: 						SuppressIf  { 0A 82 }
0x3353D: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x33541: 								Uint8 Value: 0x3 { 42 03 03 }
0x33544: 								LessThan  { 33 02 }
0x33546: 							End  { 29 02 }
0x33548: 							OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x3354F: 						End  { 29 02 }
0x33551: 						SuppressIf  { 0A 82 }
0x33553: 							QuestionRef1 QuestionId: 0x1210 { 40 84 10 12 }
0x33557: 								Uint8 Value: 0x2 { 42 03 02 }
0x3355A: 								LessThan  { 33 02 }
0x3355C: 							End  { 29 02 }
0x3355E: 							OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x33565: 						End  { 29 02 }
0x33567: 					End  { 29 02 }
0x33569: 				End  { 29 02 }
0x3356B: 			End  { 29 02 }
0x3356D: 			SuppressIf  { 0A 82 }
0x3356F: 				EqIdVal QuestionId: 0x11E5, Value: 0x0 { 12 06 E5 11 00 00 }
0x33575: 				GrayOutIf  { 19 82 }
0x33577: 					EqIdVal QuestionId: 0x2882, Value: 0x1 { 12 06 82 28 01 00 }
0x3357D: 					OneOf Prompt: "Active Efficient-cores", Help: "Number of E-cores to enable in each processor package. Note: Number of Cores and E-cores are looked at together. When both are {0,0}, Pcode will enable all cores.", QuestionFlags: 0x10, QuestionId: 0x1ED, VarStoreId: 0x1, VarOffset: 0x22F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A3 04 A4 04 ED 01 01 00 2F 02 10 10 00 FF 00 }
0x3358E: 						OneOfOption Option: "All" Value: 255, Default, MfgDefault { 09 07 B6 04 30 00 FF }
0x33595: 						SuppressIf  { 0A 82 }
0x33597: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x3359B: 								Uint8 Value: 0x10 { 42 03 10 }
0x3359E: 								LessThan  { 33 02 }
0x335A0: 							End  { 29 02 }
0x335A2: 							OneOfOption Option: "15" Value: 15 { 09 07 B4 04 00 00 0F }
0x335A9: 						End  { 29 02 }
0x335AB: 						SuppressIf  { 0A 82 }
0x335AD: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x335B1: 								Uint8 Value: 0xF { 42 03 0F }
0x335B4: 								LessThan  { 33 02 }
0x335B6: 							End  { 29 02 }
0x335B8: 							OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x335BF: 						End  { 29 02 }
0x335C1: 						SuppressIf  { 0A 82 }
0x335C3: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x335C7: 								Uint8 Value: 0xE { 42 03 0E }
0x335CA: 								LessThan  { 33 02 }
0x335CC: 							End  { 29 02 }
0x335CE: 							OneOfOption Option: "13" Value: 13 { 09 07 B2 04 00 00 0D }
0x335D5: 						End  { 29 02 }
0x335D7: 						SuppressIf  { 0A 82 }
0x335D9: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x335DD: 								Uint8 Value: 0xD { 42 03 0D }
0x335E0: 								LessThan  { 33 02 }
0x335E2: 							End  { 29 02 }
0x335E4: 							OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x335EB: 						End  { 29 02 }
0x335ED: 						SuppressIf  { 0A 82 }
0x335EF: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x335F3: 								Uint8 Value: 0xC { 42 03 0C }
0x335F6: 								LessThan  { 33 02 }
0x335F8: 							End  { 29 02 }
0x335FA: 							OneOfOption Option: "11" Value: 11 { 09 07 B0 04 00 00 0B }
0x33601: 						End  { 29 02 }
0x33603: 						SuppressIf  { 0A 82 }
0x33605: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x33609: 								Uint8 Value: 0xB { 42 03 0B }
0x3360C: 								LessThan  { 33 02 }
0x3360E: 							End  { 29 02 }
0x33610: 							OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x33617: 						End  { 29 02 }
0x33619: 						SuppressIf  { 0A 82 }
0x3361B: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x3361F: 								Uint8 Value: 0xA { 42 03 0A }
0x33622: 								LessThan  { 33 02 }
0x33624: 							End  { 29 02 }
0x33626: 							OneOfOption Option: "9" Value: 9 { 09 07 AE 04 00 00 09 }
0x3362D: 						End  { 29 02 }
0x3362F: 						SuppressIf  { 0A 82 }
0x33631: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x33635: 								Uint8 Value: 0x9 { 42 03 09 }
0x33638: 								LessThan  { 33 02 }
0x3363A: 							End  { 29 02 }
0x3363C: 							OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x33643: 						End  { 29 02 }
0x33645: 						SuppressIf  { 0A 82 }
0x33647: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x3364B: 								Uint8 Value: 0x8 { 42 03 08 }
0x3364E: 								LessThan  { 33 02 }
0x33650: 							End  { 29 02 }
0x33652: 							OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x33659: 						End  { 29 02 }
0x3365B: 						SuppressIf  { 0A 82 }
0x3365D: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x33661: 								Uint8 Value: 0x7 { 42 03 07 }
0x33664: 								LessThan  { 33 02 }
0x33666: 							End  { 29 02 }
0x33668: 							OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x3366F: 						End  { 29 02 }
0x33671: 						SuppressIf  { 0A 82 }
0x33673: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x33677: 								Uint8 Value: 0x6 { 42 03 06 }
0x3367A: 								LessThan  { 33 02 }
0x3367C: 							End  { 29 02 }
0x3367E: 							OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x33685: 						End  { 29 02 }
0x33687: 						SuppressIf  { 0A 82 }
0x33689: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x3368D: 								Uint8 Value: 0x5 { 42 03 05 }
0x33690: 								LessThan  { 33 02 }
0x33692: 							End  { 29 02 }
0x33694: 							OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x3369B: 						End  { 29 02 }
0x3369D: 						SuppressIf  { 0A 82 }
0x3369F: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x336A3: 								Uint8 Value: 0x4 { 42 03 04 }
0x336A6: 								LessThan  { 33 02 }
0x336A8: 							End  { 29 02 }
0x336AA: 							OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x336B1: 						End  { 29 02 }
0x336B3: 						SuppressIf  { 0A 82 }
0x336B5: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x336B9: 								Uint8 Value: 0x3 { 42 03 03 }
0x336BC: 								LessThan  { 33 02 }
0x336BE: 							End  { 29 02 }
0x336C0: 							OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x336C7: 						End  { 29 02 }
0x336C9: 						SuppressIf  { 0A 82 }
0x336CB: 							QuestionRef1 QuestionId: 0x11E5 { 40 84 E5 11 }
0x336CF: 								Uint8 Value: 0x2 { 42 03 02 }
0x336D2: 								LessThan  { 33 02 }
0x336D4: 							End  { 29 02 }
0x336D6: 							OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x336DD: 						End  { 29 02 }
0x336DF: 						OneOfOption Option: "0" Value: 0 { 09 07 A5 04 00 00 00 }
0x336E6: 					End  { 29 02 }
0x336E8: 				End  { 29 02 }
0x336EA: 			End  { 29 02 }
0x336EC: 		End  { 29 02 }
0x336EE: 		SuppressIf  { 0A 82 }
0x336F0: 			True  { 46 02 }
0x336F2: 			OneOf Prompt: "Limit CPUID Maximum", Help: "Disabled for Windows XP", QuestionFlags: 0x10, QuestionId: 0x1EE, VarStoreId: 0x11, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 07 A3 07 EE 01 11 00 02 00 10 10 00 01 00 }
0x33703: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3370A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33711: 			End  { 29 02 }
0x33713: 		End  { 29 02 }
0x33715: 		SuppressIf  { 0A 82 }
0x33717: 			EqIdVal QuestionId: 0x1221, Value: 0x0 { 12 06 21 12 00 00 }
0x3371D: 			GrayOutIf  { 19 82 }
0x3371F: 				EqIdVal QuestionId: 0x2729, Value: 0x1 { 12 06 29 27 01 00 }
0x33725: 				OneOf Prompt: "Hyper-Threading", Help: "Enable or Disable Hyper-Threading Technology.", QuestionFlags: 0x10, QuestionId: 0x2728, VarStoreId: 0x1, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 04 93 04 28 27 01 00 05 00 10 10 00 01 00 }
0x33736: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3373D: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33744: 				End  { 29 02 }
0x33746: 			End  { 29 02 }
0x33748: 		End  { 29 02 }
0x3374A: 		OneOf Prompt: "BIST", Help: "Enable/Disable BIST (Built-In Self Test) on reset", QuestionFlags: 0x10, QuestionId: 0x1EF, VarStoreId: 0x1, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 04 95 04 EF 01 01 00 07 00 10 10 00 01 00 }
0x3375B: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x33762: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33769: 		End  { 29 02 }
0x3376B: 		OneOf Prompt: "AP threads Idle Manner", Help: "AP threads Idle Manner for waiting signal to run", QuestionFlags: 0x10, QuestionId: 0x1F0, VarStoreId: 0x1, VarOffset: 0x120, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0 { 05 91 96 04 97 04 F0 01 01 00 20 01 10 10 01 03 00 }
0x3377C: 			OneOfOption Option: "HALT Loop" Value: 1 { 09 07 98 04 00 00 01 }
0x33783: 			OneOfOption Option: "MWAIT Loop" Value: 2, Default, MfgDefault { 09 07 99 04 30 00 02 }
0x3378A: 			OneOfOption Option: "RUN Loop" Value: 3 { 09 07 9A 04 00 00 03 }
0x33791: 		End  { 29 02 }
0x33793: 		GrayOutIf  { 19 82 }
0x33795: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3379B: 			OneOf Prompt: "AES", Help: "Enable/Disable AES (Advanced Encryption Standard)", QuestionFlags: 0x10, QuestionId: 0x1F1, VarStoreId: 0x1, VarOffset: 0xBA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 04 9C 04 F1 01 01 00 BA 00 10 10 00 01 00 }
0x337AC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x337B3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x337BA: 			End  { 29 02 }
0x337BC: 		End  { 29 02 }
0x337BE: 		OneOf Prompt: "MachineCheck", Help: "Enable/Disable Machine Check", QuestionFlags: 0x10, QuestionId: 0x1F2, VarStoreId: 0x1, VarOffset: 0xBB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 04 9E 04 F2 01 01 00 BB 00 10 10 00 01 00 }
0x337CF: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x337D6: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x337DD: 		End  { 29 02 }
0x337DF: 		OneOf Prompt: "MonitorMWait", Help: "Enable/Disable MonitorMWait, if Disable MonitorMwait, the AP threads Idle Manner should not set in MWAIT Loop", QuestionFlags: 0x10, QuestionId: 0x1F3, VarStoreId: 0x1, VarOffset: 0xBC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 04 A0 04 F3 01 01 00 BC 00 10 10 00 01 00 }
0x337F0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x337F7: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x337FE: 		End  { 29 02 }
0x33800: 		SuppressIf  { 0A 82 }
0x33802: 			EqIdVal QuestionId: 0x1223, Value: 0x0 { 12 06 23 12 00 00 }
0x33808: 			GrayOutIf  { 19 82 }
0x3380A: 				EqIdVal QuestionId: 0x2727, Value: 0x0 { 12 86 27 27 00 00 }
0x33810: 					EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x33816: 					Or  { 16 02 }
0x33818: 					EqIdVal QuestionId: 0x1175, Value: 0x1 { 12 06 75 11 01 00 }
0x3381E: 					Or  { 16 02 }
0x33820: 				End  { 29 02 }
0x33822: 				OneOf Prompt: "Intel Trusted Execution Technology", Help: "Enables utilization of additional hardware capabilities provided by Intel (R) Trusted Execution Technology.

Changes require a full power cycle to take effect.", QuestionFlags: 0x14, QuestionId: 0x2729, VarStoreId: 0x1, VarOffset: 0xC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 04 BE 04 29 27 01 00 C1 00 14 10 00 01 00 }
0x33833: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3383A: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33841: 				End  { 29 02 }
0x33843: 			End  { 29 02 }
0x33845: 		End  { 29 02 }
0x33847: 		SuppressIf  { 0A 82 }
0x33849: 			EqIdVal QuestionId: 0x1223, Value: 0x0 { 12 06 23 12 00 00 }
0x3384F: 			GrayOutIf  { 19 82 }
0x33851: 				EqIdVal QuestionId: 0x2729, Value: 0x0 { 12 06 29 27 00 00 }
0x33857: 				OneOf Prompt: "Alias Check Request", Help: "Enables Txt Alias Checking capability

Changes require full Txt capability before it will take effect.

 It is a one time only change, next reboot will be reset.", QuestionFlags: 0x10, QuestionId: 0x1F4, VarStoreId: 0x1, VarOffset: 0xC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 04 C0 04 F4 01 01 00 C4 00 10 10 00 01 00 }
0x33868: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3386F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33876: 				End  { 29 02 }
0x33878: 			End  { 29 02 }
0x3387A: 		End  { 29 02 }
0x3387C: 		SuppressIf  { 0A 82 }
0x3387E: 			EqIdVal QuestionId: 0x1223, Value: 0x0 { 12 06 23 12 00 00 }
0x33884: 			GrayOutIf  { 19 82 }
0x33886: 				EqIdVal QuestionId: 0x1222, Value: 0x1 { 12 86 22 12 01 00 }
0x3388C: 					EqIdVal QuestionId: 0x2727, Value: 0x0 { 12 06 27 27 00 00 }
0x33892: 					Or  { 16 02 }
0x33894: 					EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x3389A: 					Or  { 16 02 }
0x3389C: 					EqIdVal QuestionId: 0x2729, Value: 0x0 { 12 06 29 27 00 00 }
0x338A2: 					Or  { 16 02 }
0x338A4: 					EqIdVal QuestionId: 0x1EC, Value: 0xFF { 12 06 EC 01 FF 00 }
0x338AA: 					EqIdVal QuestionId: 0x1ED, Value: 0xFF { 12 06 ED 01 FF 00 }
0x338B0: 					And  { 15 02 }
0x338B2: 					Not  { 17 02 }
0x338B4: 					Or  { 16 02 }
0x338B6: 				End  { 29 02 }
0x338B8: 				Numeric Prompt: "DPR Memory Size (MB)", Help: "Reserve DPR memory size (0-255) MB", QuestionFlags: 0x0, QuestionId: 0x1F5, VarStoreId: 0x1, VarOffset: 0xBD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 94 7E 04 7F 04 F5 01 01 00 BD 00 00 11 00 00 FF 00 01 00 }
0x338CC: 					Default DefaultId: 0x0 Value: 4 { 5B 07 00 00 01 04 00 }
0x338D3: 				End  { 29 02 }
0x338D5: 			End  { 29 02 }
0x338D7: 		End  { 29 02 }
0x338D9: 		SuppressIf  { 0A 82 }
0x338DB: 			EqIdVal QuestionId: 0x1223, Value: 0x0 { 12 06 23 12 00 00 }
0x338E1: 			GrayOutIf  { 19 82 }
0x338E3: 				EqIdVal QuestionId: 0x1222, Value: 0x1 { 12 86 22 12 01 00 }
0x338E9: 					EqIdVal QuestionId: 0x2727, Value: 0x0 { 12 06 27 27 00 00 }
0x338EF: 					Or  { 16 02 }
0x338F1: 					EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x338F7: 					Or  { 16 02 }
0x338F9: 					EqIdVal QuestionId: 0x2729, Value: 0x1 { 12 06 29 27 01 00 }
0x338FF: 					Or  { 16 02 }
0x33901: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x33907: 					Not  { 17 02 }
0x33909: 					Or  { 16 02 }
0x3390B: 					EqIdVal QuestionId: 0x2728, Value: 0x0 { 12 06 28 27 00 00 }
0x33911: 					EqIdVal QuestionId: 0x1221, Value: 0x1 { 12 06 21 12 01 00 }
0x33917: 					And  { 15 02 }
0x33919: 					Or  { 16 02 }
0x3391B: 				End  { 29 02 }
0x3391D: 				OneOf Prompt: "Reset AUX Content", Help: "Reset TPM Aux content. Txt may not functional after AUX content gets reset.", QuestionFlags: 0x10, QuestionId: 0x1F6, VarStoreId: 0x1, VarOffset: 0xC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 07 47 07 F6 01 01 00 C3 00 10 10 00 01 00 }
0x3392E: 					OneOfOption Option: "yes" Value: 1 { 09 07 60 01 00 00 01 }
0x33935: 					OneOfOption Option: "no" Value: 0, Default, MfgDefault { 09 07 5F 01 30 00 00 }
0x3393C: 				End  { 29 02 }
0x3393E: 			End  { 29 02 }
0x33940: 		End  { 29 02 }
0x33942: 		Ref Prompt: "BIOS Guard", Help: "BIOS Guard", QuestionFlags: 0x0, QuestionId: 0x1F7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275F { 0F 0F 42 07 42 07 F7 01 00 00 FF FF 00 5F 27 }
0x33951: 		SuppressIf  { 0A 82 }
0x33953: 			EqIdVal QuestionId: 0x121E, Value: 0x0 { 12 06 1E 12 00 00 }
0x33959: 			Ref Prompt: "CPU SMM Enhancement", Help: "CPU SMM Enhancement", QuestionFlags: 0x0, QuestionId: 0x1F8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2760 { 0F 0F 88 07 89 07 F8 01 00 00 FF FF 00 60 27 }
0x33968: 		End  { 29 02 }
0x3396A: 		SuppressIf  { 0A 82 }
0x3396C: 			EqIdVal QuestionId: 0x1220, Value: 0x0 { 12 06 20 12 00 00 }
0x33972: 			OneOf Prompt: "FCLK Frequency for Early Power On", Help: "FCLK frequency can take values of 400MHz, 800MHz  and 1GHz (1GHz not supported for ULT/ULX SKUs)", QuestionFlags: 0x10, QuestionId: 0x1F9, VarStoreId: 0x1, VarOffset: 0x126, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 92 07 93 07 F9 01 01 00 26 01 10 10 00 03 00 }
0x33983: 				OneOfOption Option: "Normal (800Mhz)" Value: 0 { 09 07 94 07 00 00 00 }
0x3398A: 				OneOfOption Option: "1GHz" Value: 1 { 09 07 96 07 00 00 01 }
0x33991: 				OneOfOption Option: "400MHz" Value: 2 { 09 07 95 07 00 00 02 }
0x33998: 				OneOfOption Option: "Auto" Value: 3, Default, MfgDefault { 09 07 06 00 30 00 03 }
0x3399F: 			End  { 29 02 }
0x339A1: 		End  { 29 02 }
0x339A3: 		SuppressIf  { 0A 82 }
0x339A5: 			EqIdVal QuestionId: 0x121F, Value: 0x0 { 12 06 1F 12 00 00 }
0x339AB: 			OneOf Prompt: "Total Memory Encryption", Help: "Configure Total Memory Encryption (TME) to protect DRAM data from physical attacks.", QuestionFlags: 0x10, QuestionId: 0x272A, VarStoreId: 0x1, VarOffset: 0x229, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 07 9A 07 2A 27 01 00 29 02 10 10 00 01 00 }
0x339BC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x339C3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x339CA: 			End  { 29 02 }
0x339CC: 		End  { 29 02 }
0x339CE: 		OneOf Prompt: "Legacy Game Compatibility Mode", Help: "When enabled, Pressing the scroll lock key will toggle the Efficient-cores between being parked when Scroll Lock LED is on and un-parked when LED is off.", QuestionFlags: 0x14, QuestionId: 0x272B, VarStoreId: 0x1, VarOffset: 0x34D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 07 A0 07 2B 27 01 00 4D 03 14 10 00 01 00 }
0x339DF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x339E6: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x339ED: 			WarningIf Timeout: 0x0, Warning: "Enable Legacy Game Compatibility Mode will also enable PS2 Keyboard and Mouse in Platform Settings" { 63 85 A1 07 00 }
0x339F2: 				EqIdVal QuestionId: 0x272B, Value: 0x1 { 12 06 2B 27 01 00 }
0x339F8: 			End  { 29 02 }
0x339FA: 		End  { 29 02 }
0x339FC: 	End  { 29 02 }
0x339FE: 	Form FormId: 0x275D, Title: "Efficient-core Information" { 01 86 5D 27 9B 07 }
0x33A04: 		Subtitle Prompt: "Efficient-core Information", Help: "", Flags: 0x0 { 02 87 9B 07 00 00 00 }
0x33A0B: 		End  { 29 02 }
0x33A0D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x33A14: 		End  { 29 02 }
0x33A16: 		Text Prompt: "L1 Data Cache", Help: "Displays the Efficient-core L1 Data Cache size.", Text: "N/A" { 03 08 51 04 53 04 52 04 }
0x33A1E: 		Text Prompt: "L1 Instruction Cache", Help: "Displays the Efficient-core L1 Instruction Cache size.", Text: "N/A" { 03 08 54 04 56 04 55 04 }
0x33A26: 		Text Prompt: "L2 Cache", Help: "Displays the Efficient-core L2 Cache size.", Text: "N/A" { 03 08 57 04 59 04 58 04 }
0x33A2E: 		Text Prompt: "L3 Cache", Help: "Displays the Efficient-core L3 Cache size.", Text: "N/A" { 03 08 5A 04 5C 04 5B 04 }
0x33A36: 	End  { 29 02 }
0x33A38: 	Form FormId: 0x275E, Title: "Performance-core Information" { 01 86 5E 27 9D 07 }
0x33A3E: 		Subtitle Prompt: "Performance-core Information", Help: "", Flags: 0x0 { 02 87 9D 07 00 00 00 }
0x33A45: 		End  { 29 02 }
0x33A47: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x33A4E: 		End  { 29 02 }
0x33A50: 		Text Prompt: "L1 Data Cache", Help: "Displays the Performance-core L1 Data Cache size.", Text: "N/A" { 03 08 5D 04 5F 04 5E 04 }
0x33A58: 		Text Prompt: "L1 Instruction Cache", Help: "Displays the Performance-core L1 Instruction Cache size.", Text: "N/A" { 03 08 60 04 62 04 61 04 }
0x33A60: 		Text Prompt: "L2 Cache", Help: "Displays the Performance-core L2 Cache size.", Text: "N/A" { 03 08 63 04 65 04 64 04 }
0x33A68: 		Text Prompt: "L3 Cache", Help: "Displays the Performance-core L3 Cache size.", Text: "N/A" { 03 08 66 04 68 04 67 04 }
0x33A70: 	End  { 29 02 }
0x33A72: 	Form FormId: 0x275F, Title: "BIOS Guard" { 01 86 5F 27 43 07 }
0x33A78: 		Subtitle Prompt: "BIOS Guard", Help: "", Flags: 0x0 { 02 87 43 07 00 00 00 }
0x33A7F: 		End  { 29 02 }
0x33A81: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x33A88: 		End  { 29 02 }
0x33A8A: 		OneOf Prompt: "Enable Tools Interface", Help: "Configure Tools Interface. Options are: DISABLE - Disable Tools Interface; ENABLE - Enable Tools Interface.", QuestionFlags: 0x10, QuestionId: 0x1FA, VarStoreId: 0x1, VarOffset: 0x110, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 07 45 07 FA 01 01 00 10 01 10 10 00 01 00 }
0x33A9B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33AA2: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33AA9: 		End  { 29 02 }
0x33AAB: 	End  { 29 02 }
0x33AAD: 	SuppressIf  { 0A 82 }
0x33AAF: 		EqIdVal QuestionId: 0x121E, Value: 0x0 { 12 06 1E 12 00 00 }
0x33AB5: 		Form FormId: 0x2760, Title: "CPU SMM Enhancement" { 01 86 60 27 88 07 }
0x33ABB: 			Subtitle Prompt: "CPU SMM Enhancement", Help: "", Flags: 0x0 { 02 87 88 07 00 00 00 }
0x33AC2: 			End  { 29 02 }
0x33AC4: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x33ACB: 			End  { 29 02 }
0x33ACD: 			SuppressIf  { 0A 82 }
0x33ACF: 				EqIdVal QuestionId: 0x121D, Value: 0x0 { 12 06 1D 12 00 00 }
0x33AD5: 				OneOf Prompt: "SMM MSR Save State Enable", Help: "Enable/Disable support for MSR Save State", QuestionFlags: 0x10, QuestionId: 0x1FB, VarStoreId: 0x1, VarOffset: 0x22A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 07 8B 07 FB 01 01 00 2A 02 10 10 00 01 00 }
0x33AE6: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x33AED: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33AF4: 				End  { 29 02 }
0x33AF6: 			End  { 29 02 }
0x33AF8: 			SuppressIf  { 0A 82 }
0x33AFA: 				EqIdVal QuestionId: 0x121C, Value: 0x0 { 12 06 1C 12 00 00 }
0x33B00: 				OneOf Prompt: "SMM Use Delay Indication", Help: "Enable/Disable usage of SMM_DELAYED MSR for MP sync in SMI", QuestionFlags: 0x10, QuestionId: 0x1FC, VarStoreId: 0x1, VarOffset: 0x22B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 07 8D 07 FC 01 01 00 2B 02 10 10 00 01 00 }
0x33B11: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33B18: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33B1F: 				End  { 29 02 }
0x33B21: 			End  { 29 02 }
0x33B23: 			OneOf Prompt: "SMM Use Block Indication", Help: "Enable/Disable usage of SMM_BLOCKED MSR for MP sync in SMI", QuestionFlags: 0x10, QuestionId: 0x1FD, VarStoreId: 0x1, VarOffset: 0x22C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 07 8F 07 FD 01 01 00 2C 02 10 10 00 01 00 }
0x33B34: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33B3B: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33B42: 			End  { 29 02 }
0x33B44: 			SuppressIf  { 0A 82 }
0x33B46: 				EqIdVal QuestionId: 0x121B, Value: 0x0 { 12 06 1B 12 00 00 }
0x33B4C: 				OneOf Prompt: "SMM Use SMM en-US Indication", Help: "Enable/Disable usage of SMM_ENABLE MSR for MP sync in SMI", QuestionFlags: 0x10, QuestionId: 0x1FE, VarStoreId: 0x1, VarOffset: 0x22D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 07 91 07 FE 01 01 00 2D 02 10 10 00 01 00 }
0x33B5D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33B64: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33B6B: 				End  { 29 02 }
0x33B6D: 			End  { 29 02 }
0x33B6F: 		End  { 29 02 }
0x33B71: 	End  { 29 02 }
0x33B73: 	Form FormId: 0x2761, Title: "Power & Performance" { 01 86 61 27 86 04 }
0x33B79: 		Subtitle Prompt: "Power & Performance", Help: "", Flags: 0x0 { 02 87 86 04 00 00 00 }
0x33B80: 		End  { 29 02 }
0x33B82: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x33B89: 		End  { 29 02 }
0x33B8B: 		Ref Prompt: "CPU - Power Management Control", Help: "CPU - Power Management Control Options", QuestionFlags: 0x0, QuestionId: 0x1FF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2762 { 0F 0F 8C 04 8D 04 FF 01 00 00 FF FF 00 62 27 }
0x33B9A: 		Ref Prompt: "GT - Power Management Control", Help: "GT - Power Management Control Options", QuestionFlags: 0x0, QuestionId: 0x200, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B9 { 0F 0F 8E 04 8F 04 00 02 00 00 FF FF 00 B9 27 }
0x33BA9: 		SuppressIf  { 0A 82 }
0x33BAB: 			EqIdVal QuestionId: 0x1217, Value: 0x0 { 12 86 17 12 00 00 }
0x33BB1: 				EqIdVal QuestionId: 0x121A, Value: 0x0 { 12 06 1A 12 00 00 }
0x33BB7: 				Or  { 16 02 }
0x33BB9: 			End  { 29 02 }
0x33BBB: 			OneOf Prompt: "Intel(R) Speed Shift Technology Interrupt Control", Help: "Enable/Disable Intel(R) Speed Shift Technology Interrupts", QuestionFlags: 0x10, QuestionId: 0x201, VarStoreId: 0x1, VarOffset: 0x20C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 07 83 07 01 02 01 00 0C 02 10 10 00 01 00 }
0x33BCC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33BD3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33BDA: 			End  { 29 02 }
0x33BDC: 		End  { 29 02 }
0x33BDE: 	End  { 29 02 }
0x33BE0: 	Form FormId: 0x2762, Title: "CPU - Power Management Control" { 01 86 62 27 8C 04 }
0x33BE6: 		Subtitle Prompt: "CPU - Power Management Control", Help: "", Flags: 0x0 { 02 87 8C 04 00 00 00 }
0x33BED: 		End  { 29 02 }
0x33BEF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x33BF6: 		End  { 29 02 }
0x33BF8: 		SuppressIf  { 0A 82 }
0x33BFA: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x33C00: 				EqIdVal QuestionId: 0x1218, Value: 0x0 { 12 06 18 12 00 00 }
0x33C06: 				Or  { 16 02 }
0x33C08: 			End  { 29 02 }
0x33C0A: 			Text Prompt: "P0 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P0", Text: "N/A" { 03 08 0B 05 0C 05 0D 05 }
0x33C12: 			SuppressIf  { 0A 82 }
0x33C14: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33C18: 					Uint8 Value: 0x2 { 42 03 02 }
0x33C1B: 					LessThan  { 33 02 }
0x33C1D: 				End  { 29 02 }
0x33C1F: 				Text Prompt: "P1 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P1", Text: "N/A" { 03 08 0E 05 0F 05 10 05 }
0x33C27: 			End  { 29 02 }
0x33C29: 			SuppressIf  { 0A 82 }
0x33C2B: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33C2F: 					Uint8 Value: 0x3 { 42 03 03 }
0x33C32: 					LessThan  { 33 02 }
0x33C34: 				End  { 29 02 }
0x33C36: 				Text Prompt: "P2 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P2", Text: "N/A" { 03 08 11 05 12 05 13 05 }
0x33C3E: 			End  { 29 02 }
0x33C40: 			SuppressIf  { 0A 82 }
0x33C42: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33C46: 					Uint8 Value: 0x4 { 42 03 04 }
0x33C49: 					LessThan  { 33 02 }
0x33C4B: 				End  { 29 02 }
0x33C4D: 				Text Prompt: "P3 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P3", Text: "N/A" { 03 08 14 05 15 05 16 05 }
0x33C55: 			End  { 29 02 }
0x33C57: 			SuppressIf  { 0A 82 }
0x33C59: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33C5D: 					Uint8 Value: 0x5 { 42 03 05 }
0x33C60: 					LessThan  { 33 02 }
0x33C62: 				End  { 29 02 }
0x33C64: 				Text Prompt: "P4 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P4", Text: "N/A" { 03 08 17 05 18 05 19 05 }
0x33C6C: 			End  { 29 02 }
0x33C6E: 			SuppressIf  { 0A 82 }
0x33C70: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33C74: 					Uint8 Value: 0x6 { 42 03 06 }
0x33C77: 					LessThan  { 33 02 }
0x33C79: 				End  { 29 02 }
0x33C7B: 				Text Prompt: "P5 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P5", Text: "N/A" { 03 08 1A 05 1B 05 1C 05 }
0x33C83: 			End  { 29 02 }
0x33C85: 			SuppressIf  { 0A 82 }
0x33C87: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33C8B: 					Uint8 Value: 0x7 { 42 03 07 }
0x33C8E: 					LessThan  { 33 02 }
0x33C90: 				End  { 29 02 }
0x33C92: 				Text Prompt: "P6 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P6", Text: "N/A" { 03 08 1D 05 1E 05 1F 05 }
0x33C9A: 			End  { 29 02 }
0x33C9C: 			SuppressIf  { 0A 82 }
0x33C9E: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x33CA2: 					Uint8 Value: 0x8 { 42 03 08 }
0x33CA5: 					LessThan  { 33 02 }
0x33CA7: 				End  { 29 02 }
0x33CA9: 				Text Prompt: "P7 Fused Max Core Ratio", Help: "Displays Fused Max Core Ratio for P7", Text: "N/A" { 03 08 20 05 21 05 22 05 }
0x33CB1: 			End  { 29 02 }
0x33CB3: 		End  { 29 02 }
0x33CB5: 		OneOf Prompt: "Boot performance mode", Help: "Select the performance state that the BIOS will set starting from reset vector.", QuestionFlags: 0x14, QuestionId: 0x272C, VarStoreId: 0x1, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 23 05 24 05 2C 27 01 00 13 00 14 10 00 02 00 }
0x33CC6: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x33CCC: 			OneOfOption Option: "Max Battery" Value: 0 { 09 07 25 05 00 00 00 }
0x33CD3: 			OneOfOption Option: "Max Non-Turbo Performance" Value: 1 { 09 07 26 05 00 00 01 }
0x33CDA: 			SuppressIf  { 0A 82 }
0x33CDC: 				EqIdVal QuestionId: 0x1215, Value: 0x0 { 12 06 15 12 00 00 }
0x33CE2: 				OneOfOption Option: "Turbo Performance" Value: 2 { 09 07 27 05 00 00 02 }
0x33CE9: 			End  { 29 02 }
0x33CEB: 		End  { 29 02 }
0x33CED: 		SuppressIf  { 0A 82 }
0x33CEF: 			EqIdVal QuestionId: 0x1219, Value: 0x0 { 12 06 19 12 00 00 }
0x33CF5: 			OneOf Prompt: "Intel(R) SpeedStep(tm)", Help: "Allows more than two frequency ranges to be supported.", QuestionFlags: 0x10, QuestionId: 0x272D, VarStoreId: 0x1, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 04 C2 04 2D 27 01 00 09 00 10 10 00 01 00 }
0x33D06: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33D0D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33D14: 			End  { 29 02 }
0x33D16: 		End  { 29 02 }
0x33D18: 		OneOf Prompt: "Race To Halt (RTH)", Help: "Enable/Disable Race To Halt feature. RTH will dynamically increase CPU frequency in order to enter pkg C-State faster to reduce overall power. (RTH is controlled through MSR 1FC bit 20)", QuestionFlags: 0x10, QuestionId: 0x202, VarStoreId: 0x1, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 07 98 07 02 02 01 00 0A 00 10 10 00 01 00 }
0x33D29: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33D30: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33D37: 		End  { 29 02 }
0x33D39: 		OneOf Prompt: "Intel(R) Speed Shift Technology", Help: "Enable/Disable Intel(R) Speed Shift Technology support. Enabling will expose the CPPC v2 interface to allow for hardware controlled P-states.", QuestionFlags: 0x10, QuestionId: 0x272E, VarStoreId: 0x1, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 04 C6 04 2E 27 01 00 0B 00 10 10 00 01 00 }
0x33D4A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33D51: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33D58: 		End  { 29 02 }
0x33D5A: 		SuppressIf  { 0A 82 }
0x33D5C: 			EqIdVal QuestionId: 0x1217, Value: 0x0 { 12 86 17 12 00 00 }
0x33D62: 				EqIdVal QuestionId: 0x1218, Value: 0x0 { 12 06 18 12 00 00 }
0x33D68: 				Or  { 16 02 }
0x33D6A: 			End  { 29 02 }
0x33D6C: 			OneOf Prompt: "Intel(R) Turbo Boost Max Technology 3.0", Help: "Enable/Disable Intel(R) Turbo Boost Max Technology 3.0 support. Disabling will report the maximum ratio of the slowest core in _CPC object.", QuestionFlags: 0x10, QuestionId: 0x272F, VarStoreId: 0x1, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C7 04 C8 04 2F 27 01 00 0C 00 10 10 00 01 00 }
0x33D7D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33D84: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33D8B: 			End  { 29 02 }
0x33D8D: 		End  { 29 02 }
0x33D8F: 		OneOf Prompt: "Per Core P State OS control mode", Help: "Enable/Disable Per Core P state OS control mode. Disabling will set Bit 31 = 1 command 0x06. When set, the highest core request is used for all other core requests.", QuestionFlags: 0x10, QuestionId: 0x203, VarStoreId: 0x1, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C9 04 CA 04 03 02 01 00 0E 00 10 10 00 01 00 }
0x33DA0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33DA7: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33DAE: 		End  { 29 02 }
0x33DB0: 		SuppressIf  { 0A 82 }
0x33DB2: 			EqIdVal QuestionId: 0x1217, Value: 0x0 { 12 06 17 12 00 00 }
0x33DB8: 			OneOf Prompt: "HwP Autonomous Per Core P State", Help: "Disable Autonomous PCPS (Bit 30 = 1, command 0x11) Autonomous will request the same value for all cores all the time. Enable PCPS (default Bit 30 = 0, command 0x11)", QuestionFlags: 0x10, QuestionId: 0x204, VarStoreId: 0x1, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CB 04 CC 04 04 02 01 00 0F 00 10 10 00 01 00 }
0x33DC9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33DD0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33DD7: 			End  { 29 02 }
0x33DD9: 			OneOf Prompt: "HwP Autonomous EPP Grouping", Help: "Enable EPP grouping (default Bit 29 =0, command 0x11) Autonomous will request the same values for all cores with same EPP. Disable EPP grouping (Bit 29 =1 , command 0x11) autonomous will not necessarily request same values for all cores with same EPP.", QuestionFlags: 0x10, QuestionId: 0x205, VarStoreId: 0x1, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CD 04 CE 04 05 02 01 00 10 00 10 10 00 01 00 }
0x33DEA: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33DF1: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33DF8: 			End  { 29 02 }
0x33DFA: 			OneOf Prompt: "EPB override over PECI", Help: "Enable/Disable EPB override over PECI. Enable by sending pcode command 0x2b , subcommand 0x3 to 1. This will allow OOB EPB PECI override control", QuestionFlags: 0x10, QuestionId: 0x206, VarStoreId: 0x1, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 04 D0 04 06 02 01 00 11 00 10 10 00 01 00 }
0x33E0B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x33E12: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33E19: 			End  { 29 02 }
0x33E1B: 			SuppressIf  { 0A 82 }
0x33E1D: 				EqIdVal QuestionId: 0x1216, Value: 0x0 { 12 06 16 12 00 00 }
0x33E23: 				OneOf Prompt: "HwP Fast MSR Support", Help: "Enable/Disable HwP Fast MSR Support for IA32_HWP_REQUEST MSR.", QuestionFlags: 0x10, QuestionId: 0x207, VarStoreId: 0x1, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 04 D2 04 07 02 01 00 12 00 10 10 00 01 00 }
0x33E34: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x33E3B: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x33E42: 				End  { 29 02 }
0x33E44: 			End  { 29 02 }
0x33E46: 			OneOf Prompt: "HwP Lock", Help: "Enable/Disable HWP Lock support in Misc Power Management MSR.", QuestionFlags: 0x10, QuestionId: 0x208, VarStoreId: 0x1, VarOffset: 0x228, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D3 04 D4 04 08 02 01 00 28 02 10 10 00 01 00 }
0x33E57: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33E5E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33E65: 			End  { 29 02 }
0x33E67: 		End  { 29 02 }
0x33E69: 		OneOf Prompt: "HDC Control", Help: "This option allows HDC configuration.
 Disabled: Disable HDC
 Enabled:  Can be enabled by OS if OS native support is available.", QuestionFlags: 0x10, QuestionId: 0x209, VarStoreId: 0x1, VarOffset: 0x4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 07 87 07 09 02 01 00 4A 00 10 10 00 01 00 }
0x33E7A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33E81: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33E88: 		End  { 29 02 }
0x33E8A: 		SuppressIf  { 0A 82 }
0x33E8C: 			EqIdVal QuestionId: 0x272D, Value: 0x0 { 12 86 2D 27 00 00 }
0x33E92: 				EqIdVal QuestionId: 0x272E, Value: 0x0 { 12 06 2E 27 00 00 }
0x33E98: 				And  { 15 02 }
0x33E9A: 				EqIdVal QuestionId: 0x1215, Value: 0x0 { 12 06 15 12 00 00 }
0x33EA0: 				Or  { 16 02 }
0x33EA2: 			End  { 29 02 }
0x33EA4: 			OneOf Prompt: "  Turbo Mode", Help: "Enable/Disable processor Turbo Mode (requires EMTTM enabled too). AUTO means enabled.", QuestionFlags: 0x14, QuestionId: 0x2730, VarStoreId: 0x1, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 05 2D 05 30 27 01 00 16 00 14 10 00 01 00 }
0x33EB5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33EBC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33EC3: 			End  { 29 02 }
0x33EC5: 			Ref Prompt: "  View/Configure Turbo Options", Help: "View/Configure Turbo Options", QuestionFlags: 0x0, QuestionId: 0x20A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2765 { 0F 0F A5 03 A6 03 0A 02 00 00 FF FF 00 65 27 }
0x33ED4: 		End  { 29 02 }
0x33ED6: 		SuppressIf  { 0A 82 }
0x33ED8: 			EqIdVal QuestionId: 0x120F, Value: 0x0 { 12 06 0F 12 00 00 }
0x33EDE: 			Ref Prompt: "  Config TDP Configurations", Help: "Configurable Processor Base Power (cTDP) Configurations", QuestionFlags: 0x0, QuestionId: 0x20B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276D { 0F 0F EF 04 F1 04 0B 02 00 00 FF FF 00 6D 27 }
0x33EED: 		End  { 29 02 }
0x33EEF: 		Ref Prompt: "CPU VR Settings", Help: "CPU VR Settings", QuestionFlags: 0x0, QuestionId: 0x20C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2766 { 0F 0F AC 03 AC 03 0C 02 00 00 FF FF 00 66 27 }
0x33EFE: 		OneOf Prompt: "Platform PL1 Enable", Help: "Enable/Disable Platform Power Limit 1 programming. If this option is enabled, it activates the PL1 value to be used by the processor to limit the average power of given time window.", QuestionFlags: 0x10, QuestionId: 0x20D, VarStoreId: 0x1, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 05 2F 05 0D 02 01 00 31 00 10 10 00 01 00 }
0x33F0F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x33F16: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x33F1D: 		End  { 29 02 }
0x33F1F: 		SuppressIf  { 0A 82 }
0x33F21: 			EqIdVal QuestionId: 0x20D, Value: 0x0 { 12 06 0D 02 00 00 }
0x33F27: 			Numeric Prompt: "Platform PL1 Power", Help: "Platform Power Limit 1 Power in Milli Watts/Percent. BIOS will round to the nearest 1/8W when programming. Any value can be programmed between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). For example, if 12.50W, enter 12500, if 12%, enter 12000, if 50%, enter 50000. This setting will act as the new PL1 value for the Package RAPL algorithm.", QuestionFlags: 0x10, QuestionId: 0x20E, VarStoreId: 0x1, VarOffset: 0x32, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 30 05 31 05 0E 02 01 00 32 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x33F41: 				Default DefaultId: 0x0 Value: 325000 { 5B 09 00 00 02 88 F5 04 00 }
0x33F4A: 			End  { 29 02 }
0x33F4C: 			OneOf Prompt: "Platform PL1 Time Window", Help: "Platform Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default values. Indicates the time window over which Platform Processor Base Power (TDP) value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x20F, VarStoreId: 0x1, VarOffset: 0x36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0 { 05 91 32 05 33 05 0F 02 01 00 36 00 10 10 00 80 00 }
0x33F5D: 				OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 A5 04 30 00 00 }
0x33F64: 				OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x33F6B: 				OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x33F72: 				OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x33F79: 				OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x33F80: 				OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x33F87: 				OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x33F8E: 				OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x33F95: 				OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x33F9C: 				OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x33FA3: 				OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x33FAA: 				OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x33FB1: 				OneOfOption Option: "16" Value: 16 { 09 07 B5 04 00 00 10 }
0x33FB8: 				OneOfOption Option: "20" Value: 20 { 09 07 FE 1D 00 00 14 }
0x33FBF: 				OneOfOption Option: "24" Value: 24 { 09 07 FF 1D 00 00 18 }
0x33FC6: 				OneOfOption Option: "28" Value: 28 { 09 07 00 1E 00 00 1C }
0x33FCD: 				OneOfOption Option: "32" Value: 32 { 09 07 01 1E 00 00 20 }
0x33FD4: 				OneOfOption Option: "40" Value: 40 { 09 07 02 1E 00 00 28 }
0x33FDB: 				OneOfOption Option: "48" Value: 48 { 09 07 03 1E 00 00 30 }
0x33FE2: 				OneOfOption Option: "56" Value: 56 { 09 07 04 1E 00 00 38 }
0x33FE9: 				OneOfOption Option: "64" Value: 64 { 09 07 05 1E 00 00 40 }
0x33FF0: 				OneOfOption Option: "80" Value: 80 { 09 07 06 1E 00 00 50 }
0x33FF7: 				OneOfOption Option: "96" Value: 96 { 09 07 07 1E 00 00 60 }
0x33FFE: 				OneOfOption Option: "112" Value: 112 { 09 07 08 1E 00 00 70 }
0x34005: 				OneOfOption Option: "128" Value: 128 { 09 07 09 1E 00 00 80 }
0x3400C: 			End  { 29 02 }
0x3400E: 		End  { 29 02 }
0x34010: 		OneOf Prompt: "Platform PL2 Enable", Help: "Enable/Disable Platform Power Limit 2 programming. If this option is disabled, BIOS will program the default values for Platform Power Limit 2.", QuestionFlags: 0x10, QuestionId: 0x210, VarStoreId: 0x1, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 05 35 05 10 02 01 00 37 00 10 10 00 01 00 }
0x34021: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x34028: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3402F: 		End  { 29 02 }
0x34031: 		SuppressIf  { 0A 82 }
0x34033: 			EqIdVal QuestionId: 0x210, Value: 0x0 { 12 06 10 02 00 00 }
0x34039: 			Numeric Prompt: "Platform PL2 Power", Help: "Platform Power Limit 2 Power in Milli Watts / Milli Percent. BIOS will round to the nearest 1/8W or 1/8% when programming. Any value can be programmed between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR) or PMAX value in %. For example if 12%, enter 12000, if 50%, enter 50000. If the value is '0', will default to PACKAGE_POWER_SKU_MSR if Psys is in Watts. Recommended value is 97000 if Psys is in %. This setting will act as the new PL2 value for the Package RAPL algorithm.", QuestionFlags: 0x10, QuestionId: 0x211, VarStoreId: 0x1, VarOffset: 0x38, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 36 05 37 05 11 02 01 00 38 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x34053: 				Default DefaultId: 0x0 Value: 327000 { 5B 09 00 00 02 58 FD 04 00 }
0x3405C: 			End  { 29 02 }
0x3405E: 		End  { 29 02 }
0x34060: 		SuppressIf  { 0A 82 }
0x34062: 			EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x34068: 			OneOf Prompt: "ATX Telemetry Unit", Help: "ATX Telemetry Unit in Watts or Percentage.", QuestionFlags: 0x10, QuestionId: 0x212, VarStoreId: 0x1, VarOffset: 0x384, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 05 39 05 12 02 01 00 84 03 10 10 00 01 00 }
0x34079: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3407F: 				OneOfOption Option: "Watts" Value: 0 { 09 07 3A 05 00 00 00 }
0x34086: 				OneOfOption Option: "Percentage" Value: 1 { 09 07 3B 05 00 00 01 }
0x3408D: 			End  { 29 02 }
0x3408F: 		End  { 29 02 }
0x34091: 		OneOf Prompt: "Power Limit 4 Override", Help: "Enable/Disable Power Limit 4 override. If this option is disabled, BIOS will leave the default values for Power Limit 4.", QuestionFlags: 0x10, QuestionId: 0x213, VarStoreId: 0x1, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 05 62 05 13 02 01 00 2A 00 10 10 00 01 00 }
0x340A2: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x340A8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x340AF: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x340B6: 		End  { 29 02 }
0x340B8: 		SuppressIf  { 0A 82 }
0x340BA: 			EqIdVal QuestionId: 0x213, Value: 0x0 { 12 06 13 02 00 00 }
0x340C0: 			Numeric Prompt: "Power Limit 4", Help: "Power Limit 4 in Milli Watts. BIOS will round to the nearest 1/8W when programming. For 12.50W, enter 12500. If the value is 0, BIOS leaves default value", QuestionFlags: 0x10, QuestionId: 0x214, VarStoreId: 0x1, VarOffset: 0x2B, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 63 05 64 05 14 02 01 00 2B 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x340DA: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x340E3: 			End  { 29 02 }
0x340E5: 		End  { 29 02 }
0x340E7: 		SuppressIf  { 0A 82 }
0x340E9: 			EqIdVal QuestionId: 0x213, Value: 0x0 { 12 06 13 02 00 00 }
0x340EF: 			OneOf Prompt: "Power Limit 4 Lock", Help: "Power Limit 4 MSR 601h Lock. When enabled PL4 configurations are locked during OS. When disabled PL4 configuration can be changed during OS.", QuestionFlags: 0x10, QuestionId: 0x215, VarStoreId: 0x1, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 05 66 05 15 02 01 00 2F 00 10 10 00 01 00 }
0x34100: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x34107: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3410E: 			End  { 29 02 }
0x34110: 		End  { 29 02 }
0x34112: 		SuppressIf  { 0A 82 }
0x34114: 			EqIdVal QuestionId: 0x1213, Value: 0x0 { 12 06 13 12 00 00 }
0x3411A: 			OneOf Prompt: "C states", Help: "Enable/Disable CPU Power Management. Allows CPU to go to C states when it's not 100% utilized.", QuestionFlags: 0x10, QuestionId: 0x2731, VarStoreId: 0x1, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 05 29 05 31 27 01 00 14 00 10 10 00 01 00 }
0x3412B: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x34131: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x34138: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3413F: 			End  { 29 02 }
0x34141: 		End  { 29 02 }
0x34143: 		SuppressIf  { 0A 82 }
0x34145: 			EqIdVal QuestionId: 0x1213, Value: 0x0 { 12 86 13 12 00 00 }
0x3414B: 				EqIdVal QuestionId: 0x2731, Value: 0x0 { 12 06 31 27 00 00 }
0x34151: 				Or  { 16 02 }
0x34153: 				EqIdVal QuestionId: 0x1214, Value: 0x0 { 12 06 14 12 00 00 }
0x34159: 				Or  { 16 02 }
0x3415B: 			End  { 29 02 }
0x3415D: 			OneOf Prompt: "  Enhanced C-states", Help: "Enable/Disable C1E. When enabled, CPU will switch to minimum speed when all cores enter C-State.", QuestionFlags: 0x10, QuestionId: 0x216, VarStoreId: 0x1, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 05 2B 05 16 02 01 00 15 00 10 10 00 01 00 }
0x3416E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x34175: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3417C: 			End  { 29 02 }
0x3417E: 		End  { 29 02 }
0x34180: 		SuppressIf  { 0A 82 }
0x34182: 			EqIdVal QuestionId: 0x1213, Value: 0x0 { 12 86 13 12 00 00 }
0x34188: 				EqIdVal QuestionId: 0x2731, Value: 0x0 { 12 06 31 27 00 00 }
0x3418E: 				Or  { 16 02 }
0x34190: 			End  { 29 02 }
0x34192: 			OneOf Prompt: "  C-State Auto Demotion", Help: "Configure C-State Auto Demotion", QuestionFlags: 0x10, QuestionId: 0x217, VarStoreId: 0x1, VarOffset: 0x3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 05 03 05 17 02 01 00 3E 00 10 10 00 01 00 }
0x341A3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x341AA: 				OneOfOption Option: "C1" Value: 1, Default, MfgDefault { 09 07 04 05 30 00 01 }
0x341B1: 			End  { 29 02 }
0x341B3: 			OneOf Prompt: "  C-State Un-demotion", Help: "Configure C-State Un-demotion", QuestionFlags: 0x10, QuestionId: 0x218, VarStoreId: 0x1, VarOffset: 0x3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 05 05 06 05 18 02 01 00 3F 00 10 10 00 01 00 }
0x341C4: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x341CB: 				OneOfOption Option: "C1" Value: 1, Default, MfgDefault { 09 07 04 05 30 00 01 }
0x341D2: 			End  { 29 02 }
0x341D4: 			OneOf Prompt: "  Package C-State Demotion", Help: "  Package C-State Demotion", QuestionFlags: 0x10, QuestionId: 0x219, VarStoreId: 0x1, VarOffset: 0x40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 05 07 05 19 02 01 00 40 00 10 10 00 01 00 }
0x341E5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x341EC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x341F3: 			End  { 29 02 }
0x341F5: 			OneOf Prompt: "  Package C-State Un-demotion", Help: "  Package C-State Un-demotion", QuestionFlags: 0x10, QuestionId: 0x21A, VarStoreId: 0x1, VarOffset: 0x41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 05 08 05 1A 02 01 00 41 00 10 10 00 01 00 }
0x34206: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3420D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x34214: 			End  { 29 02 }
0x34216: 			OneOf Prompt: "CState Pre-Wake", Help: "Disable - Sets bit 30 of POWER_CTL MSR(0x1FC) to 1 to disable the Cstate Pre-Wake", QuestionFlags: 0x10, QuestionId: 0x21B, VarStoreId: 0x1, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 05 0A 05 1B 02 01 00 3D 00 10 10 00 01 00 }
0x34227: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3422E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x34235: 			End  { 29 02 }
0x34237: 			OneOf Prompt: "IO MWAIT Redirection", Help: "When set, will map IO_read instructions sent to IO registers PMG_IO_BASE_ADDRBASE+offset to MWAIT(offset)", QuestionFlags: 0x10, QuestionId: 0x21C, VarStoreId: 0x1, VarOffset: 0x48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 23 07 24 07 1C 02 01 00 48 00 10 10 00 01 00 }
0x34248: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3424E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x34255: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3425C: 			End  { 29 02 }
0x3425E: 			OneOf Prompt: "Package C State Limit", Help: "Maximum Package C State Limit Setting. Cpu Default: Leaves to Factory default value.Auto: Initializes to deepest available Package C State Limit.", QuestionFlags: 0x10, QuestionId: 0x21D, VarStoreId: 0x1, VarOffset: 0x4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 48 07 49 07 1D 02 01 00 4B 00 10 10 00 FF 00 }
0x3426F: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x34275: 				OneOfOption Option: "C0/C1" Value: 0 { 09 07 4A 07 00 00 00 }
0x3427C: 				OneOfOption Option: "C2" Value: 1 { 09 07 4B 07 00 00 01 }
0x34283: 				OneOfOption Option: "C3" Value: 2 { 09 07 4C 07 00 00 02 }
0x3428A: 				OneOfOption Option: "C6" Value: 3 { 09 07 4D 07 00 00 03 }
0x34291: 				OneOfOption Option: "C7" Value: 4 { 09 07 4E 07 00 00 04 }
0x34298: 				OneOfOption Option: "C7S" Value: 5 { 09 07 4F 07 00 00 05 }
0x3429F: 				OneOfOption Option: "C8" Value: 6 { 09 07 50 07 00 00 06 }
0x342A6: 				OneOfOption Option: "C9" Value: 7 { 09 07 51 07 00 00 07 }
0x342AD: 				OneOfOption Option: "C10" Value: 8 { 09 07 52 07 00 00 08 }
0x342B4: 				OneOfOption Option: "Cpu Default" Value: 254 { 09 07 53 07 00 00 FE }
0x342BB: 				OneOfOption Option: "Auto" Value: 255 { 09 07 54 07 00 00 FF }
0x342C2: 			End  { 29 02 }
0x342C4: 			Subtitle Prompt: "C6/C7 Short Latency Control(MSR 0x60B)", Help: "", Flags: 0x0 { 02 87 59 07 00 00 00 }
0x342CB: 			End  { 29 02 }
0x342CD: 			OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x21E, VarStoreId: 0x1, VarOffset: 0x4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 5E 07 63 07 1E 02 01 00 4C 00 10 10 00 05 00 }
0x342DE: 				OneOfOption Option: "1 ns" Value: 0 { 09 07 6A 07 00 00 00 }
0x342E5: 				OneOfOption Option: "32 ns" Value: 1 { 09 07 6B 07 00 00 01 }
0x342EC: 				OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 6C 07 30 00 02 }
0x342F3: 				OneOfOption Option: "32768 ns" Value: 3 { 09 07 6D 07 00 00 03 }
0x342FA: 				OneOfOption Option: "1048576 ns" Value: 4 { 09 07 6E 07 00 00 04 }
0x34301: 				OneOfOption Option: "33554432 ns" Value: 5 { 09 07 6F 07 00 00 05 }
0x34308: 			End  { 29 02 }
0x3430A: 			Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x21F, VarStoreId: 0x1, VarOffset: 0x51, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 64 07 69 07 1F 02 01 00 51 00 10 11 00 00 FF 03 01 00 }
0x3431E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x34325: 			End  { 29 02 }
0x34327: 			Subtitle Prompt: "C6/C7 Long Latency Control(MSR 0x60C)", Help: "", Flags: 0x0 { 02 87 5A 07 00 00 00 }
0x3432E: 			End  { 29 02 }
0x34330: 			OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x220, VarStoreId: 0x1, VarOffset: 0x4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 5F 07 63 07 20 02 01 00 4D 00 10 10 00 05 00 }
0x34341: 				OneOfOption Option: "1 ns" Value: 0 { 09 07 6A 07 00 00 00 }
0x34348: 				OneOfOption Option: "32 ns" Value: 1 { 09 07 6B 07 00 00 01 }
0x3434F: 				OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 6C 07 30 00 02 }
0x34356: 				OneOfOption Option: "32768 ns" Value: 3 { 09 07 6D 07 00 00 03 }
0x3435D: 				OneOfOption Option: "1048576 ns" Value: 4 { 09 07 6E 07 00 00 04 }
0x34364: 				OneOfOption Option: "33554432 ns" Value: 5 { 09 07 6F 07 00 00 05 }
0x3436B: 			End  { 29 02 }
0x3436D: 			Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x221, VarStoreId: 0x1, VarOffset: 0x53, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 65 07 69 07 21 02 01 00 53 00 10 11 00 00 FF 03 01 00 }
0x34381: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x34388: 			End  { 29 02 }
0x3438A: 			SuppressIf  { 0A 82 }
0x3438C: 				EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x34392: 					Not  { 17 02 }
0x34394: 				End  { 29 02 }
0x34396: 				Subtitle Prompt: "C8 Latency Control(MSR 0x633)", Help: "", Flags: 0x0 { 02 87 5B 07 00 00 00 }
0x3439D: 				End  { 29 02 }
0x3439F: 				OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x222, VarStoreId: 0x1, VarOffset: 0x4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 60 07 63 07 22 02 01 00 4E 00 10 10 00 05 00 }
0x343B0: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 6A 07 00 00 00 }
0x343B7: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 6B 07 00 00 01 }
0x343BE: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 6C 07 30 00 02 }
0x343C5: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 6D 07 00 00 03 }
0x343CC: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 6E 07 00 00 04 }
0x343D3: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 6F 07 00 00 05 }
0x343DA: 				End  { 29 02 }
0x343DC: 				Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x223, VarStoreId: 0x1, VarOffset: 0x55, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 66 07 69 07 23 02 01 00 55 00 10 11 00 00 FF 03 01 00 }
0x343F0: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x343F7: 				End  { 29 02 }
0x343F9: 				Subtitle Prompt: "C9 Latency Control(MSR 0x634)", Help: "", Flags: 0x0 { 02 87 5C 07 00 00 00 }
0x34400: 				End  { 29 02 }
0x34402: 				OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x224, VarStoreId: 0x1, VarOffset: 0x4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 61 07 63 07 24 02 01 00 4F 00 10 10 00 05 00 }
0x34413: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 6A 07 00 00 00 }
0x3441A: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 6B 07 00 00 01 }
0x34421: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 6C 07 30 00 02 }
0x34428: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 6D 07 00 00 03 }
0x3442F: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 6E 07 00 00 04 }
0x34436: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 6F 07 00 00 05 }
0x3443D: 				End  { 29 02 }
0x3443F: 				Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x225, VarStoreId: 0x1, VarOffset: 0x57, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 67 07 69 07 25 02 01 00 57 00 10 11 00 00 FF 03 01 00 }
0x34453: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3445A: 				End  { 29 02 }
0x3445C: 				Subtitle Prompt: "C10 Latency Control(MSR 0x635)", Help: "", Flags: 0x0 { 02 87 5D 07 00 00 00 }
0x34463: 				End  { 29 02 }
0x34465: 				OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x226, VarStoreId: 0x1, VarOffset: 0x50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 62 07 63 07 26 02 01 00 50 00 10 10 00 05 00 }
0x34476: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 6A 07 00 00 00 }
0x3447D: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 6B 07 00 00 01 }
0x34484: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 6C 07 30 00 02 }
0x3448B: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 6D 07 00 00 03 }
0x34492: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 6E 07 00 00 04 }
0x34499: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 6F 07 00 00 05 }
0x344A0: 				End  { 29 02 }
0x344A2: 				Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x227, VarStoreId: 0x1, VarOffset: 0x59, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 68 07 69 07 27 02 01 00 59 00 10 11 00 00 FF 03 01 00 }
0x344B6: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x344BD: 				End  { 29 02 }
0x344BF: 			End  { 29 02 }
0x344C1: 		End  { 29 02 }
0x344C3: 		OneOf Prompt: "Thermal Monitor ", Help: "Enable/Disable Thermal Monitor", QuestionFlags: 0x10, QuestionId: 0x228, VarStoreId: 0x1, VarOffset: 0x42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 55 07 56 07 28 02 01 00 42 00 10 10 00 01 00 }
0x344D4: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x344DB: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x344E2: 		End  { 29 02 }
0x344E4: 		OneOf Prompt: "Interrupt Redirection Mode Selection", Help: "Interrupt Redirection Mode Select for Logical Interrupts ", QuestionFlags: 0x10, QuestionId: 0x229, VarStoreId: 0x1, VarOffset: 0x49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 27 07 28 07 29 02 01 00 49 00 10 10 00 07 00 }
0x344F5: 			OneOfOption Option: "Fixed Priority" Value: 0, Default, MfgDefault { 09 07 29 07 30 00 00 }
0x344FC: 			OneOfOption Option: "Round robin" Value: 1 { 09 07 2A 07 00 00 01 }
0x34503: 			OneOfOption Option: "Hash Vector" Value: 2 { 09 07 2B 07 00 00 02 }
0x3450A: 			OneOfOption Option: "No Change" Value: 7 { 09 07 2C 07 00 00 07 }
0x34511: 		End  { 29 02 }
0x34513: 		SuppressIf  { 0A 82 }
0x34515: 			EqIdVal QuestionId: 0x1212, Value: 0x0 { 12 06 12 12 00 00 }
0x3451B: 			OneOf Prompt: "Timed MWAIT ", Help: "Enable/Disable Timed MWAIT Support", QuestionFlags: 0x10, QuestionId: 0x22A, VarStoreId: 0x1, VarOffset: 0x47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 57 07 58 07 2A 02 01 00 47 00 10 10 00 01 00 }
0x3452C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x34533: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3453A: 			End  { 29 02 }
0x3453C: 		End  { 29 02 }
0x3453E: 		Ref Prompt: "Custom P-state Table", Help: "Add Custom P-state Table", QuestionFlags: 0x0, QuestionId: 0x22B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2763 { 0F 0F 90 04 91 04 2B 02 00 00 FF FF 00 63 27 }
0x3454D: 		SuppressIf  { 0A 82 }
0x3454F: 			EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x34555: 				Not  { 17 02 }
0x34557: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x3455D: 				Not  { 17 02 }
0x3455F: 				And  { 15 02 }
0x34561: 				EqIdVal QuestionId: 0x1142, Value: 0x5 { 12 06 42 11 05 00 }
0x34567: 				Not  { 17 02 }
0x34569: 				And  { 15 02 }
0x3456B: 				EqIdVal QuestionId: 0x2730, Value: 0x0 { 12 06 30 27 00 00 }
0x34571: 				Or  { 16 02 }
0x34573: 			End  { 29 02 }
0x34575: 			OneOf Prompt: "EC Turbo Control Mode", Help: "Enable/Disable EC Turbo Control mode", QuestionFlags: 0x10, QuestionId: 0x22C, VarStoreId: 0x1, VarOffset: 0xC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 07 2E 07 2C 02 01 00 C7 00 10 10 00 01 00 }
0x34586: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3458D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x34594: 			End  { 29 02 }
0x34596: 		End  { 29 02 }
0x34598: 		SuppressIf  { 0A 82 }
0x3459A: 			EqIdVal QuestionId: 0x22C, Value: 0x0 { 12 06 2C 02 00 00 }
0x345A0: 			OneOf Prompt: "  AC Brick Capacity", Help: "Specify the AC Brick capacity", QuestionFlags: 0x10, QuestionId: 0x22D, VarStoreId: 0x1, VarOffset: 0xC8, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0 { 05 91 2F 07 30 07 2D 02 01 00 C8 00 10 10 01 03 00 }
0x345B1: 				OneOfOption Option: "90W AC Brick" Value: 1, Default, MfgDefault { 09 07 3D 07 30 00 01 }
0x345B8: 				OneOfOption Option: "65W AC Brick" Value: 2 { 09 07 3E 07 00 00 02 }
0x345BF: 				OneOfOption Option: "75W AC Brick" Value: 3 { 09 07 3F 07 00 00 03 }
0x345C6: 			End  { 29 02 }
0x345C8: 			Numeric Prompt: "  EC Polling Period", Help: "Count 1 to 255 for a range of 10ms to 2.55 seconds (1 count = 10ms)", QuestionFlags: 0x10, QuestionId: 0x22E, VarStoreId: 0x1, VarOffset: 0xC9, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFF, Step: 0x1 { 07 91 31 07 32 07 2E 02 01 00 C9 00 10 10 01 FF 01 }
0x345D9: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x345DF: 			End  { 29 02 }
0x345E1: 			Numeric Prompt: "  EC Guard Band Value", Help: "Count 1 to 20 for a range of 1 watt to 20 watts", QuestionFlags: 0x10, QuestionId: 0x22F, VarStoreId: 0x1, VarOffset: 0xCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1 { 07 91 33 07 34 07 2F 02 01 00 CA 00 10 10 00 14 01 }
0x345F2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x345F8: 			End  { 29 02 }
0x345FA: 			Numeric Prompt: "  EC Algorithm Selection", Help: "Count 1 to 10 for Algorithm Selection", QuestionFlags: 0x10, QuestionId: 0x230, VarStoreId: 0x1, VarOffset: 0xCB, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x1 { 07 91 35 07 36 07 30 02 01 00 CB 00 10 10 01 0A 01 }
0x3460B: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x34611: 			End  { 29 02 }
0x34613: 		End  { 29 02 }
0x34615: 		OneOf Prompt: "Energy Performance Gain", Help: "Enable/disable Energy Performance Gain.", QuestionFlags: 0x10, QuestionId: 0x231, VarStoreId: 0x4, VarOffset: 0x75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 37 07 38 07 31 02 04 00 75 00 10 10 00 01 00 }
0x34626: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3462D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x34634: 		End  { 29 02 }
0x34636: 		GrayOutIf  { 19 82 }
0x34638: 			EqIdVal QuestionId: 0x231, Value: 0x0 { 12 06 31 02 00 00 }
0x3463E: 			Numeric Prompt: "EPG DIMM Idd3N", Help: "Active standby current (Idd3N) in milliamps from datasheet. Must be calculated on a per DIMM basis.", QuestionFlags: 0x10, QuestionId: 0x232, VarStoreId: 0x4, VarOffset: 0x76, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 39 07 3A 07 32 02 04 00 76 00 10 11 00 00 D0 07 01 00 }
0x34652: 				Default DefaultId: 0x0 Value: 26 { 5B 07 00 00 01 1A 00 }
0x34659: 			End  { 29 02 }
0x3465B: 			Numeric Prompt: "EPG DIMM Idd3P", Help: "Active power-down current (Idd3P) in milliamps from datasheet. Must be calculated on a per DIMM basis.", QuestionFlags: 0x10, QuestionId: 0x233, VarStoreId: 0x4, VarOffset: 0x78, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 3B 07 3C 07 33 02 04 00 78 00 10 11 00 00 D0 07 01 00 }
0x3466F: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x34676: 			End  { 29 02 }
0x34678: 		End  { 29 02 }
0x3467A: 		Ref Prompt: "Power Limit 3 Settings", Help: "Power Limit 3 Settings", QuestionFlags: 0x0, QuestionId: 0x234, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276C { 0F 0F 51 05 52 05 34 02 00 00 FF FF 00 6C 27 }
0x34689: 		Ref Prompt: "CPU Lock Configuration", Help: "CPU Lock Configuration", QuestionFlags: 0x0, QuestionId: 0x235, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276E { 0F 0F 88 04 89 04 35 02 00 00 FF FF 00 6E 27 }
0x34698: 		SuppressIf  { 0A 82 }
0x3469A: 			EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 86 42 11 02 00 }
0x346A0: 				Not  { 17 02 }
0x346A2: 			End  { 29 02 }
0x346A4: 			GrayOutIf  { 19 82 }
0x346A6: 				EqIdVal QuestionId: 0x337, Value: 0x1 { 12 06 37 03 01 00 }
0x346AC: 				OneOf Prompt: "Dual Tau Boost", Help: "Enable Dual Tau Boost feature. This is only applicable for Desktop 35W/65W/125W sku. When DPTF is enabled this feature is ignored.", QuestionFlags: 0x10, QuestionId: 0x236, VarStoreId: 0x1, VarOffset: 0x2AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 04 8B 04 36 02 01 00 AD 02 10 10 00 01 00 }
0x346BD: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x346C4: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x346CB: 				End  { 29 02 }
0x346CD: 			End  { 29 02 }
0x346CF: 		End  { 29 02 }
0x346D1: 	End  { 29 02 }
0x346D3: 	Form FormId: 0x2763, Title: "Custom P-state Table" { 01 86 63 27 90 04 }
0x346D9: 		Subtitle Prompt: "Custom P-state Table", Help: "", Flags: 0x0 { 02 87 90 04 00 00 00 }
0x346E0: 		End  { 29 02 }
0x346E2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x346E9: 		End  { 29 02 }
0x346EB: 		Numeric Prompt: "Number of P states", Help: "Sets the number of custom P-states. At least 2 states must be present.", QuestionFlags: 0x10, QuestionId: 0x237, VarStoreId: 0x1, VarOffset: 0x80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x28, Step: 0x0 { 07 91 67 05 68 05 37 02 01 00 80 00 10 10 00 28 00 }
0x346FC: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34702: 		End  { 29 02 }
0x34704: 		SuppressIf  { 0A 82 }
0x34706: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3470A: 				Uint8 Value: 0x2 { 42 03 02 }
0x3470D: 				LessThan  { 33 02 }
0x3470F: 			End  { 29 02 }
0x34711: 			Numeric Prompt: "Max P-State Ratio", Help: "Maximum P-state ratio to use in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x238, VarStoreId: 0x1, VarOffset: 0x81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 69 05 6A 05 38 02 01 00 81 00 10 10 00 7F 00 }
0x34722: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34728: 			End  { 29 02 }
0x3472A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x239, VarStoreId: 0x1, VarOffset: 0x82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 6B 05 92 05 39 02 01 00 82 00 10 10 00 7F 00 }
0x3473B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34741: 			End  { 29 02 }
0x34743: 		End  { 29 02 }
0x34745: 		SuppressIf  { 0A 82 }
0x34747: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3474B: 				Uint8 Value: 0x3 { 42 03 03 }
0x3474E: 				LessThan  { 33 02 }
0x34750: 			End  { 29 02 }
0x34752: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x23A, VarStoreId: 0x1, VarOffset: 0x83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 6C 05 92 05 3A 02 01 00 83 00 10 10 00 7F 00 }
0x34763: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34769: 			End  { 29 02 }
0x3476B: 		End  { 29 02 }
0x3476D: 		SuppressIf  { 0A 82 }
0x3476F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34773: 				Uint8 Value: 0x4 { 42 03 04 }
0x34776: 				LessThan  { 33 02 }
0x34778: 			End  { 29 02 }
0x3477A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x23B, VarStoreId: 0x1, VarOffset: 0x84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 6D 05 92 05 3B 02 01 00 84 00 10 10 00 7F 00 }
0x3478B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34791: 			End  { 29 02 }
0x34793: 		End  { 29 02 }
0x34795: 		SuppressIf  { 0A 82 }
0x34797: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3479B: 				Uint8 Value: 0x5 { 42 03 05 }
0x3479E: 				LessThan  { 33 02 }
0x347A0: 			End  { 29 02 }
0x347A2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x23C, VarStoreId: 0x1, VarOffset: 0x85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 6E 05 92 05 3C 02 01 00 85 00 10 10 00 7F 00 }
0x347B3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x347B9: 			End  { 29 02 }
0x347BB: 		End  { 29 02 }
0x347BD: 		SuppressIf  { 0A 82 }
0x347BF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x347C3: 				Uint8 Value: 0x6 { 42 03 06 }
0x347C6: 				LessThan  { 33 02 }
0x347C8: 			End  { 29 02 }
0x347CA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x23D, VarStoreId: 0x1, VarOffset: 0x86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 6F 05 92 05 3D 02 01 00 86 00 10 10 00 7F 00 }
0x347DB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x347E1: 			End  { 29 02 }
0x347E3: 		End  { 29 02 }
0x347E5: 		SuppressIf  { 0A 82 }
0x347E7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x347EB: 				Uint8 Value: 0x7 { 42 03 07 }
0x347EE: 				LessThan  { 33 02 }
0x347F0: 			End  { 29 02 }
0x347F2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x23E, VarStoreId: 0x1, VarOffset: 0x87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 70 05 92 05 3E 02 01 00 87 00 10 10 00 7F 00 }
0x34803: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34809: 			End  { 29 02 }
0x3480B: 		End  { 29 02 }
0x3480D: 		SuppressIf  { 0A 82 }
0x3480F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34813: 				Uint8 Value: 0x8 { 42 03 08 }
0x34816: 				LessThan  { 33 02 }
0x34818: 			End  { 29 02 }
0x3481A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x23F, VarStoreId: 0x1, VarOffset: 0x88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 71 05 92 05 3F 02 01 00 88 00 10 10 00 7F 00 }
0x3482B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34831: 			End  { 29 02 }
0x34833: 		End  { 29 02 }
0x34835: 		SuppressIf  { 0A 82 }
0x34837: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3483B: 				Uint8 Value: 0x9 { 42 03 09 }
0x3483E: 				LessThan  { 33 02 }
0x34840: 			End  { 29 02 }
0x34842: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x240, VarStoreId: 0x1, VarOffset: 0x89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 72 05 92 05 40 02 01 00 89 00 10 10 00 7F 00 }
0x34853: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34859: 			End  { 29 02 }
0x3485B: 		End  { 29 02 }
0x3485D: 		SuppressIf  { 0A 82 }
0x3485F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34863: 				Uint8 Value: 0xA { 42 03 0A }
0x34866: 				LessThan  { 33 02 }
0x34868: 			End  { 29 02 }
0x3486A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x241, VarStoreId: 0x1, VarOffset: 0x8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 73 05 92 05 41 02 01 00 8A 00 10 10 00 7F 00 }
0x3487B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34881: 			End  { 29 02 }
0x34883: 		End  { 29 02 }
0x34885: 		SuppressIf  { 0A 82 }
0x34887: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3488B: 				Uint8 Value: 0xB { 42 03 0B }
0x3488E: 				LessThan  { 33 02 }
0x34890: 			End  { 29 02 }
0x34892: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x242, VarStoreId: 0x1, VarOffset: 0x8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 74 05 92 05 42 02 01 00 8B 00 10 10 00 7F 00 }
0x348A3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x348A9: 			End  { 29 02 }
0x348AB: 		End  { 29 02 }
0x348AD: 		SuppressIf  { 0A 82 }
0x348AF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x348B3: 				Uint8 Value: 0xC { 42 03 0C }
0x348B6: 				LessThan  { 33 02 }
0x348B8: 			End  { 29 02 }
0x348BA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x243, VarStoreId: 0x1, VarOffset: 0x8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 75 05 92 05 43 02 01 00 8C 00 10 10 00 7F 00 }
0x348CB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x348D1: 			End  { 29 02 }
0x348D3: 		End  { 29 02 }
0x348D5: 		SuppressIf  { 0A 82 }
0x348D7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x348DB: 				Uint8 Value: 0xD { 42 03 0D }
0x348DE: 				LessThan  { 33 02 }
0x348E0: 			End  { 29 02 }
0x348E2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x244, VarStoreId: 0x1, VarOffset: 0x8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 76 05 92 05 44 02 01 00 8D 00 10 10 00 7F 00 }
0x348F3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x348F9: 			End  { 29 02 }
0x348FB: 		End  { 29 02 }
0x348FD: 		SuppressIf  { 0A 82 }
0x348FF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34903: 				Uint8 Value: 0xE { 42 03 0E }
0x34906: 				LessThan  { 33 02 }
0x34908: 			End  { 29 02 }
0x3490A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x245, VarStoreId: 0x1, VarOffset: 0x8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 77 05 92 05 45 02 01 00 8E 00 10 10 00 7F 00 }
0x3491B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34921: 			End  { 29 02 }
0x34923: 		End  { 29 02 }
0x34925: 		SuppressIf  { 0A 82 }
0x34927: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3492B: 				Uint8 Value: 0xF { 42 03 0F }
0x3492E: 				LessThan  { 33 02 }
0x34930: 			End  { 29 02 }
0x34932: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x246, VarStoreId: 0x1, VarOffset: 0x8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 78 05 92 05 46 02 01 00 8F 00 10 10 00 7F 00 }
0x34943: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34949: 			End  { 29 02 }
0x3494B: 		End  { 29 02 }
0x3494D: 		SuppressIf  { 0A 82 }
0x3494F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34953: 				Uint8 Value: 0x10 { 42 03 10 }
0x34956: 				LessThan  { 33 02 }
0x34958: 			End  { 29 02 }
0x3495A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x247, VarStoreId: 0x1, VarOffset: 0x90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 79 05 92 05 47 02 01 00 90 00 10 10 00 7F 00 }
0x3496B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34971: 			End  { 29 02 }
0x34973: 		End  { 29 02 }
0x34975: 		SuppressIf  { 0A 82 }
0x34977: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x3497B: 				Uint8 Value: 0x11 { 42 03 11 }
0x3497E: 				LessThan  { 33 02 }
0x34980: 			End  { 29 02 }
0x34982: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x248, VarStoreId: 0x1, VarOffset: 0x91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 7A 05 92 05 48 02 01 00 91 00 10 10 00 7F 00 }
0x34993: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34999: 			End  { 29 02 }
0x3499B: 		End  { 29 02 }
0x3499D: 		SuppressIf  { 0A 82 }
0x3499F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x349A3: 				Uint8 Value: 0x12 { 42 03 12 }
0x349A6: 				LessThan  { 33 02 }
0x349A8: 			End  { 29 02 }
0x349AA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x249, VarStoreId: 0x1, VarOffset: 0x92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 7B 05 92 05 49 02 01 00 92 00 10 10 00 7F 00 }
0x349BB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x349C1: 			End  { 29 02 }
0x349C3: 		End  { 29 02 }
0x349C5: 		SuppressIf  { 0A 82 }
0x349C7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x349CB: 				Uint8 Value: 0x13 { 42 03 13 }
0x349CE: 				LessThan  { 33 02 }
0x349D0: 			End  { 29 02 }
0x349D2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x24A, VarStoreId: 0x1, VarOffset: 0x93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 7C 05 92 05 4A 02 01 00 93 00 10 10 00 7F 00 }
0x349E3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x349E9: 			End  { 29 02 }
0x349EB: 		End  { 29 02 }
0x349ED: 		SuppressIf  { 0A 82 }
0x349EF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x349F3: 				Uint8 Value: 0x14 { 42 03 14 }
0x349F6: 				LessThan  { 33 02 }
0x349F8: 			End  { 29 02 }
0x349FA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x24B, VarStoreId: 0x1, VarOffset: 0x94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 7D 05 92 05 4B 02 01 00 94 00 10 10 00 7F 00 }
0x34A0B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34A11: 			End  { 29 02 }
0x34A13: 		End  { 29 02 }
0x34A15: 		SuppressIf  { 0A 82 }
0x34A17: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34A1B: 				Uint8 Value: 0x15 { 42 03 15 }
0x34A1E: 				LessThan  { 33 02 }
0x34A20: 			End  { 29 02 }
0x34A22: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x24C, VarStoreId: 0x1, VarOffset: 0x95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 7E 05 92 05 4C 02 01 00 95 00 10 10 00 7F 00 }
0x34A33: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34A39: 			End  { 29 02 }
0x34A3B: 		End  { 29 02 }
0x34A3D: 		SuppressIf  { 0A 82 }
0x34A3F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34A43: 				Uint8 Value: 0x16 { 42 03 16 }
0x34A46: 				LessThan  { 33 02 }
0x34A48: 			End  { 29 02 }
0x34A4A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x24D, VarStoreId: 0x1, VarOffset: 0x96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 7F 05 92 05 4D 02 01 00 96 00 10 10 00 7F 00 }
0x34A5B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34A61: 			End  { 29 02 }
0x34A63: 		End  { 29 02 }
0x34A65: 		SuppressIf  { 0A 82 }
0x34A67: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34A6B: 				Uint8 Value: 0x17 { 42 03 17 }
0x34A6E: 				LessThan  { 33 02 }
0x34A70: 			End  { 29 02 }
0x34A72: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x24E, VarStoreId: 0x1, VarOffset: 0x97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 80 05 92 05 4E 02 01 00 97 00 10 10 00 7F 00 }
0x34A83: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34A89: 			End  { 29 02 }
0x34A8B: 		End  { 29 02 }
0x34A8D: 		SuppressIf  { 0A 82 }
0x34A8F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34A93: 				Uint8 Value: 0x18 { 42 03 18 }
0x34A96: 				LessThan  { 33 02 }
0x34A98: 			End  { 29 02 }
0x34A9A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x24F, VarStoreId: 0x1, VarOffset: 0x98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 81 05 92 05 4F 02 01 00 98 00 10 10 00 7F 00 }
0x34AAB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34AB1: 			End  { 29 02 }
0x34AB3: 		End  { 29 02 }
0x34AB5: 		SuppressIf  { 0A 82 }
0x34AB7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34ABB: 				Uint8 Value: 0x19 { 42 03 19 }
0x34ABE: 				LessThan  { 33 02 }
0x34AC0: 			End  { 29 02 }
0x34AC2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x250, VarStoreId: 0x1, VarOffset: 0x99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 82 05 92 05 50 02 01 00 99 00 10 10 00 7F 00 }
0x34AD3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34AD9: 			End  { 29 02 }
0x34ADB: 		End  { 29 02 }
0x34ADD: 		SuppressIf  { 0A 82 }
0x34ADF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34AE3: 				Uint8 Value: 0x1A { 42 03 1A }
0x34AE6: 				LessThan  { 33 02 }
0x34AE8: 			End  { 29 02 }
0x34AEA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x251, VarStoreId: 0x1, VarOffset: 0x9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 83 05 92 05 51 02 01 00 9A 00 10 10 00 7F 00 }
0x34AFB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34B01: 			End  { 29 02 }
0x34B03: 		End  { 29 02 }
0x34B05: 		SuppressIf  { 0A 82 }
0x34B07: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34B0B: 				Uint8 Value: 0x1B { 42 03 1B }
0x34B0E: 				LessThan  { 33 02 }
0x34B10: 			End  { 29 02 }
0x34B12: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x252, VarStoreId: 0x1, VarOffset: 0x9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 84 05 92 05 52 02 01 00 9B 00 10 10 00 7F 00 }
0x34B23: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34B29: 			End  { 29 02 }
0x34B2B: 		End  { 29 02 }
0x34B2D: 		SuppressIf  { 0A 82 }
0x34B2F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34B33: 				Uint8 Value: 0x1C { 42 03 1C }
0x34B36: 				LessThan  { 33 02 }
0x34B38: 			End  { 29 02 }
0x34B3A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x253, VarStoreId: 0x1, VarOffset: 0x9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 85 05 92 05 53 02 01 00 9C 00 10 10 00 7F 00 }
0x34B4B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34B51: 			End  { 29 02 }
0x34B53: 		End  { 29 02 }
0x34B55: 		SuppressIf  { 0A 82 }
0x34B57: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34B5B: 				Uint8 Value: 0x1D { 42 03 1D }
0x34B5E: 				LessThan  { 33 02 }
0x34B60: 			End  { 29 02 }
0x34B62: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x254, VarStoreId: 0x1, VarOffset: 0x9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 86 05 92 05 54 02 01 00 9D 00 10 10 00 7F 00 }
0x34B73: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34B79: 			End  { 29 02 }
0x34B7B: 		End  { 29 02 }
0x34B7D: 		SuppressIf  { 0A 82 }
0x34B7F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34B83: 				Uint8 Value: 0x1E { 42 03 1E }
0x34B86: 				LessThan  { 33 02 }
0x34B88: 			End  { 29 02 }
0x34B8A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x255, VarStoreId: 0x1, VarOffset: 0x9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 87 05 92 05 55 02 01 00 9E 00 10 10 00 7F 00 }
0x34B9B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34BA1: 			End  { 29 02 }
0x34BA3: 		End  { 29 02 }
0x34BA5: 		SuppressIf  { 0A 82 }
0x34BA7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34BAB: 				Uint8 Value: 0x1F { 42 03 1F }
0x34BAE: 				LessThan  { 33 02 }
0x34BB0: 			End  { 29 02 }
0x34BB2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x256, VarStoreId: 0x1, VarOffset: 0x9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 88 05 92 05 56 02 01 00 9F 00 10 10 00 7F 00 }
0x34BC3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34BC9: 			End  { 29 02 }
0x34BCB: 		End  { 29 02 }
0x34BCD: 		SuppressIf  { 0A 82 }
0x34BCF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34BD3: 				Uint8 Value: 0x20 { 42 03 20 }
0x34BD6: 				LessThan  { 33 02 }
0x34BD8: 			End  { 29 02 }
0x34BDA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x257, VarStoreId: 0x1, VarOffset: 0xA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 89 05 92 05 57 02 01 00 A0 00 10 10 00 7F 00 }
0x34BEB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34BF1: 			End  { 29 02 }
0x34BF3: 		End  { 29 02 }
0x34BF5: 		SuppressIf  { 0A 82 }
0x34BF7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34BFB: 				Uint8 Value: 0x21 { 42 03 21 }
0x34BFE: 				LessThan  { 33 02 }
0x34C00: 			End  { 29 02 }
0x34C02: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x258, VarStoreId: 0x1, VarOffset: 0xA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 8A 05 92 05 58 02 01 00 A1 00 10 10 00 7F 00 }
0x34C13: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34C19: 			End  { 29 02 }
0x34C1B: 		End  { 29 02 }
0x34C1D: 		SuppressIf  { 0A 82 }
0x34C1F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34C23: 				Uint8 Value: 0x22 { 42 03 22 }
0x34C26: 				LessThan  { 33 02 }
0x34C28: 			End  { 29 02 }
0x34C2A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x259, VarStoreId: 0x1, VarOffset: 0xA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 8B 05 92 05 59 02 01 00 A2 00 10 10 00 7F 00 }
0x34C3B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34C41: 			End  { 29 02 }
0x34C43: 		End  { 29 02 }
0x34C45: 		SuppressIf  { 0A 82 }
0x34C47: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34C4B: 				Uint8 Value: 0x23 { 42 03 23 }
0x34C4E: 				LessThan  { 33 02 }
0x34C50: 			End  { 29 02 }
0x34C52: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x25A, VarStoreId: 0x1, VarOffset: 0xA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 8C 05 92 05 5A 02 01 00 A3 00 10 10 00 7F 00 }
0x34C63: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34C69: 			End  { 29 02 }
0x34C6B: 		End  { 29 02 }
0x34C6D: 		SuppressIf  { 0A 82 }
0x34C6F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34C73: 				Uint8 Value: 0x24 { 42 03 24 }
0x34C76: 				LessThan  { 33 02 }
0x34C78: 			End  { 29 02 }
0x34C7A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x25B, VarStoreId: 0x1, VarOffset: 0xA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 8D 05 92 05 5B 02 01 00 A4 00 10 10 00 7F 00 }
0x34C8B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34C91: 			End  { 29 02 }
0x34C93: 		End  { 29 02 }
0x34C95: 		SuppressIf  { 0A 82 }
0x34C97: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34C9B: 				Uint8 Value: 0x25 { 42 03 25 }
0x34C9E: 				LessThan  { 33 02 }
0x34CA0: 			End  { 29 02 }
0x34CA2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x25C, VarStoreId: 0x1, VarOffset: 0xA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 8E 05 92 05 5C 02 01 00 A5 00 10 10 00 7F 00 }
0x34CB3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34CB9: 			End  { 29 02 }
0x34CBB: 		End  { 29 02 }
0x34CBD: 		SuppressIf  { 0A 82 }
0x34CBF: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34CC3: 				Uint8 Value: 0x26 { 42 03 26 }
0x34CC6: 				LessThan  { 33 02 }
0x34CC8: 			End  { 29 02 }
0x34CCA: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x25D, VarStoreId: 0x1, VarOffset: 0xA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 8F 05 92 05 5D 02 01 00 A6 00 10 10 00 7F 00 }
0x34CDB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34CE1: 			End  { 29 02 }
0x34CE3: 		End  { 29 02 }
0x34CE5: 		SuppressIf  { 0A 82 }
0x34CE7: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34CEB: 				Uint8 Value: 0x27 { 42 03 27 }
0x34CEE: 				LessThan  { 33 02 }
0x34CF0: 			End  { 29 02 }
0x34CF2: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x25E, VarStoreId: 0x1, VarOffset: 0xA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 90 05 92 05 5E 02 01 00 A7 00 10 10 00 7F 00 }
0x34D03: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34D09: 			End  { 29 02 }
0x34D0B: 		End  { 29 02 }
0x34D0D: 		SuppressIf  { 0A 82 }
0x34D0F: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34D13: 				Uint8 Value: 0x28 { 42 03 28 }
0x34D16: 				LessThan  { 33 02 }
0x34D18: 			End  { 29 02 }
0x34D1A: 			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0x25F, VarStoreId: 0x1, VarOffset: 0xA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 91 05 92 05 5F 02 01 00 A8 00 10 10 00 7F 00 }
0x34D2B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34D31: 			End  { 29 02 }
0x34D33: 		End  { 29 02 }
0x34D35: 		SuppressIf  { 0A 82 }
0x34D37: 			QuestionRef1 QuestionId: 0x237 { 40 84 37 02 }
0x34D3B: 				Uint8 Value: 0x11 { 42 03 11 }
0x34D3E: 				LessThan  { 33 02 }
0x34D40: 			End  { 29 02 }
0x34D42: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x34D49: 			End  { 29 02 }
0x34D4B: 			Subtitle Prompt: "Max 16 custom P-state Table", Help: "", Flags: 0x0 { 02 87 93 05 00 00 00 }
0x34D52: 			End  { 29 02 }
0x34D54: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x34D5B: 			End  { 29 02 }
0x34D5D: 			Numeric Prompt: "Max P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x260, VarStoreId: 0x1, VarOffset: 0xA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 94 05 A4 05 60 02 01 00 A9 00 10 10 00 7F 00 }
0x34D6E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34D74: 			End  { 29 02 }
0x34D76: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x261, VarStoreId: 0x1, VarOffset: 0xAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 95 05 A4 05 61 02 01 00 AA 00 10 10 00 7F 00 }
0x34D87: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34D8D: 			End  { 29 02 }
0x34D8F: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x262, VarStoreId: 0x1, VarOffset: 0xAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 96 05 A4 05 62 02 01 00 AB 00 10 10 00 7F 00 }
0x34DA0: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34DA6: 			End  { 29 02 }
0x34DA8: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x263, VarStoreId: 0x1, VarOffset: 0xAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 97 05 A4 05 63 02 01 00 AC 00 10 10 00 7F 00 }
0x34DB9: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34DBF: 			End  { 29 02 }
0x34DC1: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x264, VarStoreId: 0x1, VarOffset: 0xAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 98 05 A4 05 64 02 01 00 AD 00 10 10 00 7F 00 }
0x34DD2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34DD8: 			End  { 29 02 }
0x34DDA: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x265, VarStoreId: 0x1, VarOffset: 0xAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 99 05 A4 05 65 02 01 00 AE 00 10 10 00 7F 00 }
0x34DEB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34DF1: 			End  { 29 02 }
0x34DF3: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x266, VarStoreId: 0x1, VarOffset: 0xAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 9A 05 A4 05 66 02 01 00 AF 00 10 10 00 7F 00 }
0x34E04: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34E0A: 			End  { 29 02 }
0x34E0C: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x267, VarStoreId: 0x1, VarOffset: 0xB0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 9B 05 A4 05 67 02 01 00 B0 00 10 10 00 7F 00 }
0x34E1D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34E23: 			End  { 29 02 }
0x34E25: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x268, VarStoreId: 0x1, VarOffset: 0xB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 9C 05 A4 05 68 02 01 00 B1 00 10 10 00 7F 00 }
0x34E36: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34E3C: 			End  { 29 02 }
0x34E3E: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x269, VarStoreId: 0x1, VarOffset: 0xB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 9D 05 A4 05 69 02 01 00 B2 00 10 10 00 7F 00 }
0x34E4F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34E55: 			End  { 29 02 }
0x34E57: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x26A, VarStoreId: 0x1, VarOffset: 0xB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 9E 05 A4 05 6A 02 01 00 B3 00 10 10 00 7F 00 }
0x34E68: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34E6E: 			End  { 29 02 }
0x34E70: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x26B, VarStoreId: 0x1, VarOffset: 0xB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 9F 05 A4 05 6B 02 01 00 B4 00 10 10 00 7F 00 }
0x34E81: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34E87: 			End  { 29 02 }
0x34E89: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x26C, VarStoreId: 0x1, VarOffset: 0xB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 A0 05 A4 05 6C 02 01 00 B5 00 10 10 00 7F 00 }
0x34E9A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34EA0: 			End  { 29 02 }
0x34EA2: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x26D, VarStoreId: 0x1, VarOffset: 0xB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 A1 05 A4 05 6D 02 01 00 B6 00 10 10 00 7F 00 }
0x34EB3: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34EB9: 			End  { 29 02 }
0x34EBB: 			Numeric Prompt: "P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x26E, VarStoreId: 0x1, VarOffset: 0xB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 A2 05 A4 05 6E 02 01 00 B7 00 10 10 00 7F 00 }
0x34ECC: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34ED2: 			End  { 29 02 }
0x34ED4: 			Numeric Prompt: "Min P-State Ratio (Max 16 table)", Help: "P-state ratio for the given state in the Max 16 P-state table. Used if OS only supports 16 P-states", QuestionFlags: 0x10, QuestionId: 0x26F, VarStoreId: 0x1, VarOffset: 0xB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x0 { 07 91 A3 05 A4 05 6F 02 01 00 B8 00 10 10 00 7F 00 }
0x34EE5: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x34EEB: 			End  { 29 02 }
0x34EED: 		End  { 29 02 }
0x34EEF: 	End  { 29 02 }
0x34EF1: 	Form FormId: 0x2764, Title: "Turbo Ratio Limit Options" { 01 86 64 27 A9 03 }
0x34EF7: 		Subtitle Prompt: "Current Turbo Ratio Limit Settings", Help: "", Flags: 0x0 { 02 87 AB 03 00 00 00 }
0x34EFE: 		End  { 29 02 }
0x34F00: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x34F07: 		End  { 29 02 }
0x34F09: 		SuppressIf  { 0A 82 }
0x34F0B: 			EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 86 EC 01 00 00 }
0x34F11: 				EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 06 ED 01 00 00 }
0x34F17: 				Not  { 17 02 }
0x34F19: 				And  { 15 02 }
0x34F1B: 				EqIdVal QuestionId: 0x1210, Value: 0x0 { 12 06 10 12 00 00 }
0x34F21: 				Or  { 16 02 }
0x34F23: 			End  { 29 02 }
0x34F25: 			Text Prompt: "P-core Turbo Ratio Limit Numcore0", Help: "Performance-core Turbo Ratio Limit Numcore0 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio0. If value is zero, this entry is ignored.", Text: "" { 03 08 82 06 81 06 83 06 }
0x34F2D: 			Text Prompt: "P-core Turbo Ratio Limit Numcore1", Help: "Performance-core Turbo Ratio Limit Numcore1 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio1. If value is zero, this entry is ignored.", Text: "" { 03 08 85 06 84 06 86 06 }
0x34F35: 			Text Prompt: "P-core Turbo Ratio Limit Numcore2", Help: "Performance-core Turbo Ratio Limit Numcore2 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio2. If value is zero, this entry is ignored.", Text: "" { 03 08 88 06 87 06 89 06 }
0x34F3D: 			Text Prompt: "P-core Turbo Ratio Limit Numcore3", Help: "Performance-core Turbo Ratio Limit Numcore3 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio3. If value is zero, this entry is ignored.", Text: "" { 03 08 8B 06 8A 06 8C 06 }
0x34F45: 			Text Prompt: "P-core Turbo Ratio Limit Numcore4", Help: "Performance-core Turbo Ratio Limit Numcore4 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio4. If value is zero, this entry is ignored.", Text: "" { 03 08 8E 06 8D 06 8F 06 }
0x34F4D: 			Text Prompt: "P-core Turbo Ratio Limit Numcore5", Help: "Performance-core Turbo Ratio Limit Numcore5 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio5. If value is zero, this entry is ignored.", Text: "" { 03 08 91 06 90 06 92 06 }
0x34F55: 			Text Prompt: "P-core Turbo Ratio Limit Numcore6", Help: "Performance-core Turbo Ratio Limit Numcore6 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio6. If value is zero, this entry is ignored.", Text: "" { 03 08 94 06 93 06 95 06 }
0x34F5D: 			Text Prompt: "P-core Turbo Ratio Limit Numcore7", Help: "Performance-core Turbo Ratio Limit Numcore7 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio7. If value is zero, this entry is ignored.", Text: "" { 03 08 97 06 96 06 98 06 }
0x34F65: 			Text Prompt: "P-core Turbo Ratio Limit Ratio0", Help: "Performance-core Turbo Ratio Limit Ratio0 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore0.", Text: "" { 03 08 9A 06 99 06 9B 06 }
0x34F6D: 			Text Prompt: "P-core Turbo Ratio Limit Ratio1", Help: "Performance-core Turbo Ratio Limit Ratio1 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore1.", Text: "" { 03 08 9D 06 9C 06 9E 06 }
0x34F75: 			Text Prompt: "P-core Turbo Ratio Limit Ratio2", Help: "Performance-core Turbo Ratio Limit Ratio2 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore2.", Text: "" { 03 08 A0 06 9F 06 A1 06 }
0x34F7D: 			Text Prompt: "P-core Turbo Ratio Limit Ratio3", Help: "Performance-core Turbo Ratio Limit Ratio3 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore3.", Text: "" { 03 08 A3 06 A2 06 A4 06 }
0x34F85: 			Text Prompt: "P-core Turbo Ratio Limit Ratio4", Help: "Performance-core Turbo Ratio Limit Ratio4 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore4.", Text: "" { 03 08 A6 06 A5 06 A7 06 }
0x34F8D: 			Text Prompt: "P-core Turbo Ratio Limit Ratio5", Help: "Performance-core Turbo Ratio Limit Ratio5 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore5.", Text: "" { 03 08 A9 06 A8 06 AA 06 }
0x34F95: 			Text Prompt: "P-core Turbo Ratio Limit Ratio6", Help: "Performance-core Turbo Ratio Limit Ratio6 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore6.", Text: "" { 03 08 AC 06 AB 06 AD 06 }
0x34F9D: 			Text Prompt: "P-core Turbo Ratio Limit Ratio7", Help: "Performance-core Turbo Ratio Limit Ratio7 defines the turbo ratio, the core range is defined in Turbo Ratio Limit Numcore7.", Text: "" { 03 08 AF 06 AE 06 B0 06 }
0x34FA5: 		End  { 29 02 }
0x34FA7: 		SuppressIf  { 0A 82 }
0x34FA9: 			EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 86 ED 01 00 00 }
0x34FAF: 				EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x34FB5: 				Not  { 17 02 }
0x34FB7: 				And  { 15 02 }
0x34FB9: 				EqIdVal QuestionId: 0x11E5, Value: 0x0 { 12 06 E5 11 00 00 }
0x34FBF: 				Or  { 16 02 }
0x34FC1: 			End  { 29 02 }
0x34FC3: 			Text Prompt: "E-core Turbo Ratio Limit Numcore0", Help: "Efficient-core Turbo Ratio Limit Numcore0 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio0. If value is zero, this entry is ignored.", Text: "" { 03 08 B2 06 B1 06 B3 06 }
0x34FCB: 			Text Prompt: "E-core Turbo Ratio Limit Numcore1", Help: "Efficient-core Turbo Ratio Limit Numcore1 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio1. If value is zero, this entry is ignored.", Text: "" { 03 08 B5 06 B4 06 B6 06 }
0x34FD3: 			Text Prompt: "E-core Turbo Ratio Limit Numcore2", Help: "Efficient-core Turbo Ratio Limit Numcore2 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio2. If value is zero, this entry is ignored.", Text: "" { 03 08 B8 06 B7 06 B9 06 }
0x34FDB: 			Text Prompt: "E-core Turbo Ratio Limit Numcore3", Help: "Efficient-core Turbo Ratio Limit Numcore3 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio3. If value is zero, this entry is ignored.", Text: "" { 03 08 BB 06 BA 06 BC 06 }
0x34FE3: 			Text Prompt: "E-core Turbo Ratio Limit Numcore4", Help: "Efficient-core Turbo Ratio Limit Numcore4 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio4. If value is zero, this entry is ignored.", Text: "" { 03 08 BE 06 BD 06 BF 06 }
0x34FEB: 			Text Prompt: "E-core Turbo Ratio Limit Numcore5", Help: "Efficient-core Turbo Ratio Limit Numcore5 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio5. If value is zero, this entry is ignored.", Text: "" { 03 08 C1 06 C0 06 C2 06 }
0x34FF3: 			Text Prompt: "E-core Turbo Ratio Limit Numcore6", Help: "Efficient-core Turbo Ratio Limit Numcore6 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio6. If value is zero, this entry is ignored.", Text: "" { 03 08 C4 06 C3 06 C5 06 }
0x34FFB: 			Text Prompt: "E-core Turbo Ratio Limit Numcore7", Help: "Efficient-core Turbo Ratio Limit Numcore7 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio7. If value is zero, this entry is ignored.", Text: "" { 03 08 C7 06 C6 06 C8 06 }
0x35003: 			Text Prompt: "E-core Turbo Ratio Limit Ratio0", Help: "Efficient-core Turbo Ratio Limit Ratio0 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore0.", Text: "" { 03 08 CA 06 C9 06 CB 06 }
0x3500B: 			Text Prompt: "E-core Turbo Ratio Limit Ratio1", Help: "Efficient-core Turbo Ratio Limit Ratio1 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore1.", Text: "" { 03 08 CD 06 CC 06 CE 06 }
0x35013: 			Text Prompt: "E-core Turbo Ratio Limit Ratio2", Help: "Efficient-core Turbo Ratio Limit Ratio2 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore2.", Text: "" { 03 08 D0 06 CF 06 D1 06 }
0x3501B: 			Text Prompt: "E-core Turbo Ratio Limit Ratio3", Help: "Efficient-core Turbo Ratio Limit Ratio3 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore3.", Text: "" { 03 08 D3 06 D2 06 D4 06 }
0x35023: 			Text Prompt: "E-core Turbo Ratio Limit Ratio4", Help: "Efficient-core Turbo Ratio Limit Ratio4 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore4.", Text: "" { 03 08 D6 06 D5 06 D7 06 }
0x3502B: 			Text Prompt: "E-core Turbo Ratio Limit Ratio5", Help: "Efficient-core Turbo Ratio Limit Ratio5 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore5.", Text: "" { 03 08 D9 06 D8 06 DA 06 }
0x35033: 			Text Prompt: "E-core Turbo Ratio Limit Ratio6", Help: "Efficient-core Turbo Ratio Limit Ratio6 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore6.", Text: "" { 03 08 DC 06 DB 06 DD 06 }
0x3503B: 			Text Prompt: "E-core Turbo Ratio Limit Ratio7", Help: "Efficient-core Turbo Ratio Limit Ratio7 defines the turbo ratio, the core range is defined in E-core Turbo Ratio Limit Numcore7.", Text: "" { 03 08 DF 06 DE 06 E0 06 }
0x35043: 		End  { 29 02 }
0x35045: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3504C: 		End  { 29 02 }
0x3504E: 		SuppressIf  { 0A 82 }
0x35050: 			EqIdVal QuestionId: 0x1211, Value: 0x0 { 12 86 11 12 00 00 }
0x35056: 				EqIdVal QuestionId: 0x272D, Value: 0x0 { 12 06 2D 27 00 00 }
0x3505C: 				Or  { 16 02 }
0x3505E: 				EqIdVal QuestionId: 0x2730, Value: 0x0 { 12 06 30 27 00 00 }
0x35064: 				Or  { 16 02 }
0x35066: 			End  { 29 02 }
0x35068: 			SuppressIf  { 0A 82 }
0x3506A: 				EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 86 EC 01 00 00 }
0x35070: 					EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 06 ED 01 00 00 }
0x35076: 					Not  { 17 02 }
0x35078: 					And  { 15 02 }
0x3507A: 					EqIdVal QuestionId: 0x1210, Value: 0x0 { 12 06 10 12 00 00 }
0x35080: 					Or  { 16 02 }
0x35082: 				End  { 29 02 }
0x35084: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore0", Help: "Performance-core Turbo Ratio Limit Numcore0 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio0. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2732, VarStoreId: 0x1, VarOffset: 0xE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E2 06 E1 06 32 27 01 00 E6 00 14 10 00 FF 01 }
0x35095: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3509B: 				End  { 29 02 }
0x3509D: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore1", Help: "Performance-core Turbo Ratio Limit Numcore1 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio1. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2733, VarStoreId: 0x1, VarOffset: 0xE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E4 06 E3 06 33 27 01 00 E7 00 14 10 00 FF 01 }
0x350AE: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x350B4: 				End  { 29 02 }
0x350B6: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore2", Help: "Performance-core Turbo Ratio Limit Numcore2 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio2. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2734, VarStoreId: 0x1, VarOffset: 0xE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E6 06 E5 06 34 27 01 00 E8 00 14 10 00 FF 01 }
0x350C7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x350CD: 				End  { 29 02 }
0x350CF: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore3", Help: "Performance-core Turbo Ratio Limit Numcore3 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio3. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2735, VarStoreId: 0x1, VarOffset: 0xE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 E8 06 E7 06 35 27 01 00 E9 00 14 10 00 FF 01 }
0x350E0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x350E6: 				End  { 29 02 }
0x350E8: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore4", Help: "Performance-core Turbo Ratio Limit Numcore4 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio4. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2736, VarStoreId: 0x1, VarOffset: 0xEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EA 06 E9 06 36 27 01 00 EA 00 14 10 00 FF 01 }
0x350F9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x350FF: 				End  { 29 02 }
0x35101: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore5", Help: "Performance-core Turbo Ratio Limit Numcore5 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio5. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2737, VarStoreId: 0x1, VarOffset: 0xEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EC 06 EB 06 37 27 01 00 EB 00 14 10 00 FF 01 }
0x35112: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35118: 				End  { 29 02 }
0x3511A: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore6", Help: "Performance-core Turbo Ratio Limit Numcore6 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio6. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2738, VarStoreId: 0x1, VarOffset: 0xEC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 EE 06 ED 06 38 27 01 00 EC 00 14 10 00 FF 01 }
0x3512B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35131: 				End  { 29 02 }
0x35133: 				Numeric Prompt: "P-core Turbo Ratio Limit Numcore7", Help: "Performance-core Turbo Ratio Limit Numcore7 defines the core range, the turbo ratio is defined in Turbo Ratio Limit Ratio7. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2739, VarStoreId: 0x1, VarOffset: 0xED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F0 06 EF 06 39 27 01 00 ED 00 14 10 00 FF 01 }
0x35144: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3514A: 				End  { 29 02 }
0x3514C: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio0", Help: "Performance-core Turbo Ratio Limit Ratio0 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore0.", QuestionFlags: 0x14, QuestionId: 0x273A, VarStoreId: 0x1, VarOffset: 0xD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 F2 06 F1 06 3A 27 01 00 D6 00 14 10 00 78 01 }
0x3515D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35163: 				End  { 29 02 }
0x35165: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio1", Help: "Performance-core Turbo Ratio Limit Ratio1 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore1.", QuestionFlags: 0x14, QuestionId: 0x273B, VarStoreId: 0x1, VarOffset: 0xD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 F4 06 F3 06 3B 27 01 00 D7 00 14 10 00 78 01 }
0x35176: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3517C: 				End  { 29 02 }
0x3517E: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio2", Help: "Performance-core Turbo Ratio Limit Ratio2 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore2.", QuestionFlags: 0x14, QuestionId: 0x273C, VarStoreId: 0x1, VarOffset: 0xD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 F6 06 F5 06 3C 27 01 00 D8 00 14 10 00 78 01 }
0x3518F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35195: 				End  { 29 02 }
0x35197: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio3", Help: "Performance-core Turbo Ratio Limit Ratio3 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore3.", QuestionFlags: 0x14, QuestionId: 0x273D, VarStoreId: 0x1, VarOffset: 0xD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 F8 06 F7 06 3D 27 01 00 D9 00 14 10 00 78 01 }
0x351A8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x351AE: 				End  { 29 02 }
0x351B0: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio4", Help: "Performance-core Turbo Ratio Limit Ratio4 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore4.", QuestionFlags: 0x14, QuestionId: 0x273E, VarStoreId: 0x1, VarOffset: 0xDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 FA 06 F9 06 3E 27 01 00 DA 00 14 10 00 78 01 }
0x351C1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x351C7: 				End  { 29 02 }
0x351C9: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio5", Help: "Performance-core Turbo Ratio Limit Ratio5 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore5.", QuestionFlags: 0x14, QuestionId: 0x273F, VarStoreId: 0x1, VarOffset: 0xDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 FC 06 FB 06 3F 27 01 00 DB 00 14 10 00 78 01 }
0x351DA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x351E0: 				End  { 29 02 }
0x351E2: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio6", Help: "Performance-core Turbo Ratio Limit Ratio6 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore6.", QuestionFlags: 0x14, QuestionId: 0x2740, VarStoreId: 0x1, VarOffset: 0xDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 FE 06 FD 06 40 27 01 00 DC 00 14 10 00 78 01 }
0x351F3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x351F9: 				End  { 29 02 }
0x351FB: 				Numeric Prompt: "P-core Turbo Ratio Limit Ratio7", Help: "Performance-core Turbo Ratio Limit Ratio7 defines the turbo ratio (max is 85 in normal mode and 120 in core extension mode), the core range is defined in Turbo Ratio Limit Numcore7.", QuestionFlags: 0x14, QuestionId: 0x2741, VarStoreId: 0x1, VarOffset: 0xDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 00 07 FF 06 41 27 01 00 DD 00 14 10 00 78 01 }
0x3520C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35212: 				End  { 29 02 }
0x35214: 			End  { 29 02 }
0x35216: 			SuppressIf  { 0A 82 }
0x35218: 				EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 86 ED 01 00 00 }
0x3521E: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x35224: 					Not  { 17 02 }
0x35226: 					And  { 15 02 }
0x35228: 					EqIdVal QuestionId: 0x11E5, Value: 0x0 { 12 06 E5 11 00 00 }
0x3522E: 					Or  { 16 02 }
0x35230: 				End  { 29 02 }
0x35232: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore0", Help: "Efficient-core Turbo Ratio Limit Numcore0 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio0. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2742, VarStoreId: 0x1, VarOffset: 0x106, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 02 07 01 07 42 27 01 00 06 01 14 10 00 FF 01 }
0x35243: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35249: 				End  { 29 02 }
0x3524B: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore1", Help: "Efficient-core Turbo Ratio Limit Numcore1 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio1. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2743, VarStoreId: 0x1, VarOffset: 0x107, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 04 07 03 07 43 27 01 00 07 01 14 10 00 FF 01 }
0x3525C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35262: 				End  { 29 02 }
0x35264: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore2", Help: "Efficient-core Turbo Ratio Limit Numcore2 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio2. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2744, VarStoreId: 0x1, VarOffset: 0x108, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 06 07 05 07 44 27 01 00 08 01 14 10 00 FF 01 }
0x35275: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3527B: 				End  { 29 02 }
0x3527D: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore3", Help: "Efficient-core Turbo Ratio Limit Numcore3 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio3. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2745, VarStoreId: 0x1, VarOffset: 0x109, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 08 07 07 07 45 27 01 00 09 01 14 10 00 FF 01 }
0x3528E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35294: 				End  { 29 02 }
0x35296: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore4", Help: "Efficient-core Turbo Ratio Limit Numcore4 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio4. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2746, VarStoreId: 0x1, VarOffset: 0x10A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0A 07 09 07 46 27 01 00 0A 01 14 10 00 FF 01 }
0x352A7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x352AD: 				End  { 29 02 }
0x352AF: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore5", Help: "Efficient-core Turbo Ratio Limit Numcore5 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio5. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2747, VarStoreId: 0x1, VarOffset: 0x10B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0C 07 0B 07 47 27 01 00 0B 01 14 10 00 FF 01 }
0x352C0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x352C6: 				End  { 29 02 }
0x352C8: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore6", Help: "Efficient-core Turbo Ratio Limit Numcore6 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio6. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2748, VarStoreId: 0x1, VarOffset: 0x10C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0E 07 0D 07 48 27 01 00 0C 01 14 10 00 FF 01 }
0x352D9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x352DF: 				End  { 29 02 }
0x352E1: 				Numeric Prompt: "E-core Turbo Ratio Limit Numcore7", Help: "Efficient-core Turbo Ratio Limit Numcore7 defines the core range, the turbo ratio is defined in E-core Turbo Ratio Limit Ratio7. If value is zero, this entry is ignored.", QuestionFlags: 0x14, QuestionId: 0x2749, VarStoreId: 0x1, VarOffset: 0x10D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 10 07 0F 07 49 27 01 00 0D 01 14 10 00 FF 01 }
0x352F2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x352F8: 				End  { 29 02 }
0x352FA: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio0", Help: "Efficient-core Turbo Ratio Limit Ratio0 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore0.", QuestionFlags: 0x14, QuestionId: 0x274A, VarStoreId: 0x1, VarOffset: 0xF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 12 07 11 07 4A 27 01 00 F6 00 14 10 00 55 01 }
0x3530B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35311: 				End  { 29 02 }
0x35313: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio1", Help: "Efficient-core Turbo Ratio Limit Ratio1 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore1.", QuestionFlags: 0x14, QuestionId: 0x274B, VarStoreId: 0x1, VarOffset: 0xF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 14 07 13 07 4B 27 01 00 F7 00 14 10 00 55 01 }
0x35324: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3532A: 				End  { 29 02 }
0x3532C: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio2", Help: "Efficient-core Turbo Ratio Limit Ratio2 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore2.", QuestionFlags: 0x14, QuestionId: 0x274C, VarStoreId: 0x1, VarOffset: 0xF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 16 07 15 07 4C 27 01 00 F8 00 14 10 00 55 01 }
0x3533D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35343: 				End  { 29 02 }
0x35345: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio3", Help: "Efficient-core Turbo Ratio Limit Ratio3 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore3.", QuestionFlags: 0x14, QuestionId: 0x274D, VarStoreId: 0x1, VarOffset: 0xF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 18 07 17 07 4D 27 01 00 F9 00 14 10 00 55 01 }
0x35356: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3535C: 				End  { 29 02 }
0x3535E: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio4", Help: "Efficient-core Turbo Ratio Limit Ratio4 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore4.", QuestionFlags: 0x14, QuestionId: 0x274E, VarStoreId: 0x1, VarOffset: 0xFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 1A 07 19 07 4E 27 01 00 FA 00 14 10 00 55 01 }
0x3536F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35375: 				End  { 29 02 }
0x35377: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio5", Help: "Efficient-core Turbo Ratio Limit Ratio5 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore5.", QuestionFlags: 0x14, QuestionId: 0x274F, VarStoreId: 0x1, VarOffset: 0xFB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 1C 07 1B 07 4F 27 01 00 FB 00 14 10 00 55 01 }
0x35388: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3538E: 				End  { 29 02 }
0x35390: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio6", Help: "Efficient-core Turbo Ratio Limit Ratio6 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore6.", QuestionFlags: 0x14, QuestionId: 0x2750, VarStoreId: 0x1, VarOffset: 0xFC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 1E 07 1D 07 50 27 01 00 FC 00 14 10 00 55 01 }
0x353A1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x353A7: 				End  { 29 02 }
0x353A9: 				Numeric Prompt: "E-core Turbo Ratio Limit Ratio7", Help: "Efficient-core Turbo Ratio Limit Ratio7 defines the turbo ratio (max is 85 irrespective of the core extension mode), the core range is defined in E-core Turbo Ratio Limit Numcore7.", QuestionFlags: 0x14, QuestionId: 0x2751, VarStoreId: 0x1, VarOffset: 0xFD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 20 07 1F 07 51 27 01 00 FD 00 14 10 00 55 01 }
0x353BA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x353C0: 				End  { 29 02 }
0x353C2: 			End  { 29 02 }
0x353C4: 		End  { 29 02 }
0x353C6: 	End  { 29 02 }
0x353C8: 	Form FormId: 0x2765, Title: "  View/Configure Turbo Options" { 01 86 65 27 A5 03 }
0x353CE: 		Subtitle Prompt: "Current Turbo Settings", Help: "", Flags: 0x0 { 02 87 A8 03 00 00 00 }
0x353D5: 		End  { 29 02 }
0x353D7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x353DE: 		End  { 29 02 }
0x353E0: 		Text Prompt: "Max Turbo Power Limit", Help: "Max Turbo Power Limit", Text: "" { 03 08 A6 05 A5 05 A7 05 }
0x353E8: 		Text Prompt: "Min Turbo Power Limit", Help: "Min Turbo Power Limit", Text: "" { 03 08 A9 05 A8 05 AA 05 }
0x353F0: 		Text Prompt: "Package TDP Limit", Help: "Package Processor Base Power (TDP) Limit", Text: "" { 03 08 B2 05 B1 05 B3 05 }
0x353F8: 		Text Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and Processor Base Power (TDP) Limit. If value is 0, BIOS will program Processor Base Power (TDP) value.", Text: "" { 03 08 AC 05 44 05 AD 05 }
0x35400: 		Text Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. If the value is 0, BIOS will program this value as 1.25*Processor Base Power (TDP). For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", Text: "" { 03 08 AF 05 50 05 B0 05 }
0x35408: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3540F: 		End  { 29 02 }
0x35411: 		Ref Prompt: "Turbo Ratio Limit Options", Help: "View/Configure Turbo Ratio Limit Options", QuestionFlags: 0x0, QuestionId: 0x270, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2764 { 0F 0F A9 03 AA 03 70 02 00 00 FF FF 00 64 27 }
0x35420: 		SuppressIf  { 0A 82 }
0x35422: 			EqIdVal QuestionId: 0x272D, Value: 0x0 { 12 86 2D 27 00 00 }
0x35428: 				EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x3542E: 				Or  { 16 02 }
0x35430: 			End  { 29 02 }
0x35432: 			OneOf Prompt: "Energy Efficient P-state", Help: "Enable/Disable Energy Efficient P-state feature. When set to 0, will disable access to ENERGY_PERFORMANCE_BIAS MSR and CPUID Function 6 ECX[3] will read 0 indicating no support for Energy Efficient policy setting. When set to 1 will enable access to ENERGY_PERFORMANCE_BIAS MSR 1B0h and CPUID Function 6 ECX[3] will read 1 indicating Energy Efficient policy setting is supported.", QuestionFlags: 0x10, QuestionId: 0x271, VarStoreId: 0x1, VarOffset: 0x3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C3 04 C4 04 71 02 01 00 3C 00 10 10 00 01 00 }
0x35443: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3544A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x35451: 			End  { 29 02 }
0x35453: 		End  { 29 02 }
0x35455: 		SuppressIf  { 0A 82 }
0x35457: 			EqIdVal QuestionId: 0x272D, Value: 0x0 { 12 06 2D 27 00 00 }
0x3545D: 			OneOf Prompt: "Package Power Limit MSR Lock", Help: "Enable/Disable locking of Package Power Limit settings. When enabled, PACKAGE_POWER_LIMIT MSR will be locked and a reset will be required to unlock the register.", QuestionFlags: 0x10, QuestionId: 0x272, VarStoreId: 0x1, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 05 3D 05 72 02 01 00 30 00 10 10 00 01 00 }
0x3546E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x35475: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3547C: 			End  { 29 02 }
0x3547E: 		End  { 29 02 }
0x35480: 		SuppressIf  { 0A 82 }
0x35482: 			EqIdVal QuestionId: 0x120F, Value: 0x1 { 12 06 0F 12 01 00 }
0x35488: 			OneOf Prompt: "Power Limit 1 Override", Help: "Enable/Disable Power Limit 1 override. If this option is disabled, BIOS will program the default values for Power Limit 1 and Power Limit 1 Time Window.", QuestionFlags: 0x10, QuestionId: 0x273, VarStoreId: 0x1, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 05 3F 05 73 02 01 00 1B 00 10 10 00 01 00 }
0x35499: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3549F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x354A6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x354AD: 			End  { 29 02 }
0x354AF: 		End  { 29 02 }
0x354B1: 		SuppressIf  { 0A 82 }
0x354B3: 			EqIdVal QuestionId: 0x120F, Value: 0x1 { 12 86 0F 12 01 00 }
0x354B9: 				EqIdVal QuestionId: 0x273, Value: 0x0 { 12 06 73 02 00 00 }
0x354BF: 				Or  { 16 02 }
0x354C1: 			End  { 29 02 }
0x354C3: 			Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and Processor Base Power (TDP) Limit. If value is 0, BIOS will program Processor Base Power (TDP) value.", QuestionFlags: 0x10, QuestionId: 0x274, VarStoreId: 0x1, VarOffset: 0x17, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 40 05 44 05 74 02 01 00 17 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x354DD: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x354E6: 			End  { 29 02 }
0x354E8: 		End  { 29 02 }
0x354EA: 		SuppressIf  { 0A 82 }
0x354EC: 			EqIdVal QuestionId: 0x120F, Value: 0x1 { 12 86 0F 12 01 00 }
0x354F2: 				EqIdVal QuestionId: 0x273, Value: 0x0 { 12 06 73 02 00 00 }
0x354F8: 				Or  { 16 02 }
0x354FA: 			End  { 29 02 }
0x354FC: 			OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which Processor Base Power (TDP) value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x275, VarStoreId: 0x1, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0 { 05 91 45 05 49 05 75 02 01 00 1C 00 10 10 00 80 00 }
0x3550D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35513: 				OneOfOption Option: "0" Value: 0 { 09 07 A5 04 00 00 00 }
0x3551A: 				OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x35521: 				OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x35528: 				OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x3552F: 				OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x35536: 				OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x3553D: 				OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x35544: 				OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x3554B: 				OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x35552: 				OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x35559: 				OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x35560: 				OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x35567: 				OneOfOption Option: "16" Value: 16 { 09 07 B5 04 00 00 10 }
0x3556E: 				OneOfOption Option: "20" Value: 20 { 09 07 FE 1D 00 00 14 }
0x35575: 				OneOfOption Option: "24" Value: 24 { 09 07 FF 1D 00 00 18 }
0x3557C: 				OneOfOption Option: "28" Value: 28 { 09 07 00 1E 00 00 1C }
0x35583: 				OneOfOption Option: "32" Value: 32 { 09 07 01 1E 00 00 20 }
0x3558A: 				OneOfOption Option: "40" Value: 40 { 09 07 02 1E 00 00 28 }
0x35591: 				OneOfOption Option: "48" Value: 48 { 09 07 03 1E 00 00 30 }
0x35598: 				OneOfOption Option: "56" Value: 56 { 09 07 04 1E 00 00 38 }
0x3559F: 				OneOfOption Option: "64" Value: 64 { 09 07 05 1E 00 00 40 }
0x355A6: 				OneOfOption Option: "80" Value: 80 { 09 07 06 1E 00 00 50 }
0x355AD: 				OneOfOption Option: "96" Value: 96 { 09 07 07 1E 00 00 60 }
0x355B4: 				OneOfOption Option: "112" Value: 112 { 09 07 08 1E 00 00 70 }
0x355BB: 				OneOfOption Option: "128" Value: 128 { 09 07 09 1E 00 00 80 }
0x355C2: 			End  { 29 02 }
0x355C4: 		End  { 29 02 }
0x355C6: 		SuppressIf  { 0A 82 }
0x355C8: 			EqIdVal QuestionId: 0x120F, Value: 0x1 { 12 06 0F 12 01 00 }
0x355CE: 			OneOf Prompt: "Power Limit 2 Override", Help: "Enable/Disable Power Limit 2 override. If this option is disabled, BIOS will program the default values for Power Limit 2.", QuestionFlags: 0x10, QuestionId: 0x276, VarStoreId: 0x1, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4A 05 4B 05 76 02 01 00 1D 00 10 10 00 01 00 }
0x355DF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x355E6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x355ED: 			End  { 29 02 }
0x355EF: 		End  { 29 02 }
0x355F1: 		SuppressIf  { 0A 82 }
0x355F3: 			EqIdVal QuestionId: 0x120F, Value: 0x1 { 12 86 0F 12 01 00 }
0x355F9: 				EqIdVal QuestionId: 0x276, Value: 0x0 { 12 06 76 02 00 00 }
0x355FF: 				Or  { 16 02 }
0x35601: 			End  { 29 02 }
0x35603: 			Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. If the value is 0, BIOS will program this value as 1.25*Processor Base Power (TDP). For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x277, VarStoreId: 0x1, VarOffset: 0x1E, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 4C 05 50 05 77 02 01 00 1E 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x3561D: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x35626: 			End  { 29 02 }
0x35628: 		End  { 29 02 }
0x3562A: 		OneOf Prompt: "Energy Efficient Turbo", Help: "Enable/Disable Energy Efficient Turbo Feature. This feature will opportunistically lower the turbo frequency to increase efficiency. Recommended only to disable in overclocking situations where turbo frequency must remain constant. Otherwise, leave enabled.", QuestionFlags: 0x10, QuestionId: 0x278, VarStoreId: 0x1, VarOffset: 0x1D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 07 41 07 78 02 01 00 D5 01 10 10 00 01 00 }
0x3563B: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x35642: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x35649: 		End  { 29 02 }
0x3564B: 	End  { 29 02 }
0x3564D: 	Form FormId: 0x2766, Title: "CPU VR Settings" { 01 86 66 27 AC 03 }
0x35653: 		Subtitle Prompt: "CPU VR Settings", Help: "", Flags: 0x0 { 02 87 AD 03 00 00 00 }
0x3565A: 		End  { 29 02 }
0x3565C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x35663: 		End  { 29 02 }
0x35665: 		Text Prompt: "Current VccIn Aux Icc Max", Help: "Current VccIn Aux Icc Max", Text: "" { 03 08 E7 05 E6 05 E8 05 }
0x3566D: 		Numeric Prompt: "PSYS Slope", Help: "PSYS Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x9.", QuestionFlags: 0x10, QuestionId: 0x279, VarStoreId: 0x1, VarOffset: 0x127, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1 { 07 91 0D 06 0E 06 79 02 01 00 27 01 10 10 00 C8 01 }
0x3567E: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35684: 		End  { 29 02 }
0x35686: 		Numeric Prompt: "PSYS Offset", Help: "PSYS Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. PSYS Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x27A, VarStoreId: 0x1, VarOffset: 0x128, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1 { 07 94 0F 06 10 06 7A 02 01 00 28 01 10 11 00 00 FF F9 01 00 }
0x3569A: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x356A1: 		End  { 29 02 }
0x356A3: 		OneOf Prompt: "  PSYS Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x27B, VarStoreId: 0x1, VarOffset: 0x12A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 06 12 06 7B 02 01 00 2A 01 10 10 00 01 00 }
0x356B4: 			OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x356BB: 			OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x356C2: 		End  { 29 02 }
0x356C4: 		Numeric Prompt: "PSYS PMax Power", Help: "Psys Pmax power, defined in 1/8 Watt or 1/8 Percent increments. For Watts, range is 0-8191 (ex. For 125W, enter 1000). For ATX12VO Percent, Range is 0-1600 (ex. For recommended value of 200%, enter 1600). Uses BIOS VR mailbox command 0xB.", QuestionFlags: 0x10, QuestionId: 0x27C, VarStoreId: 0x1, VarOffset: 0x12B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1FFF, Step: 0x1 { 07 94 13 06 14 06 7C 02 01 00 2B 01 10 11 00 00 FF 1F 01 00 }
0x356D8: 			Default DefaultId: 0x0 Value: 2680 { 5B 07 00 00 01 78 0A }
0x356DF: 		End  { 29 02 }
0x356E1: 		OneOf Prompt: "Min Voltage Override", Help: "Min Voltage Override. Enable to override minimum voltage for runtime and for C8.", QuestionFlags: 0x10, QuestionId: 0x27D, VarStoreId: 0x1, VarOffset: 0x207, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7B 06 7C 06 7D 02 01 00 07 02 10 10 00 01 00 }
0x356F2: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x356F9: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x35700: 		End  { 29 02 }
0x35702: 		SuppressIf  { 0A 82 }
0x35704: 			EqIdVal QuestionId: 0x27D, Value: 0x0 { 12 06 7D 02 00 00 }
0x3570A: 			Numeric Prompt: "  Min Voltage Runtime", Help: "Min Voltage for Runtime. Range is 0 - 1999mV in 1/128 volt increments. Input is in mVolts.", QuestionFlags: 0x10, QuestionId: 0x27E, VarStoreId: 0x1, VarOffset: 0x208, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7CF, Step: 0x1 { 07 94 7D 06 7E 06 7E 02 01 00 08 02 10 11 00 00 CF 07 01 00 }
0x3571E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35725: 			End  { 29 02 }
0x35727: 			Numeric Prompt: "  Min Voltage C8", Help: "Min Voltage for Package C8. Range is 0 - 1999mV in 1/128 volt increments. Input is in mVolts.", QuestionFlags: 0x10, QuestionId: 0x27F, VarStoreId: 0x1, VarOffset: 0x20A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7CF, Step: 0x1 { 07 94 7F 06 80 06 7F 02 01 00 0A 02 10 11 00 00 CF 07 01 00 }
0x3573B: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35742: 			End  { 29 02 }
0x35744: 		End  { 29 02 }
0x35746: 		Numeric Prompt: "VccIn Aux Icc Max", Help: "Sets the Max Icc VccIn Aux value defined in 1/4A increments. Range is 0-512. For an IccMax 32A, enter 128(32*4).", QuestionFlags: 0x10, QuestionId: 0x280, VarStoreId: 0x1, VarOffset: 0x2E8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 15 06 16 06 80 02 01 00 E8 02 10 11 00 00 00 02 01 00 }
0x3575A: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35761: 		End  { 29 02 }
0x35763: 		Numeric Prompt: "VccIn Aux IMON Slope", Help: "VccIN Aux IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x18.", QuestionFlags: 0x10, QuestionId: 0x281, VarStoreId: 0x1, VarOffset: 0x2EA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xC8, Step: 0x1 { 07 94 17 06 18 06 81 02 01 00 EA 02 10 11 00 00 C8 00 01 00 }
0x35777: 			Default DefaultId: 0x0 Value: 100 { 5B 07 00 00 01 64 00 }
0x3577E: 		End  { 29 02 }
0x35780: 		Numeric Prompt: "VccIN Aux IMON Offset", Help: "VccIN Aux IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x18.", QuestionFlags: 0x10, QuestionId: 0x282, VarStoreId: 0x1, VarOffset: 0x2EC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1 { 07 94 19 06 1A 06 82 02 01 00 EC 02 10 11 00 00 FF F9 01 00 }
0x35794: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3579B: 		End  { 29 02 }
0x3579D: 		OneOf Prompt: "  VccIN Aux IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x283, VarStoreId: 0x1, VarOffset: 0x2EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1B 06 1C 06 83 02 01 00 EE 02 10 10 00 01 00 }
0x357AE: 			OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x357B5: 			OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x357BC: 		End  { 29 02 }
0x357BE: 		OneOf Prompt: "Vsys/Psys Critical", Help: "Vsys/Psys Critical Enable or disable", QuestionFlags: 0x10, QuestionId: 0x284, VarStoreId: 0x1, VarOffset: 0x2EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 1D 06 1E 06 84 02 01 00 EF 02 10 10 00 02 00 }
0x357CF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x357D6: 			OneOfOption Option: "Psys Critical" Value: 1 { 09 07 20 06 00 00 01 }
0x357DD: 			OneOfOption Option: "Vsys Critical" Value: 2 { 09 07 1F 06 00 00 02 }
0x357E4: 		End  { 29 02 }
0x357E6: 		SuppressIf  { 0A 82 }
0x357E8: 			EqIdVal QuestionId: 0x284, Value: 0x0 { 12 86 84 02 00 00 }
0x357EE: 				EqIdVal QuestionId: 0x284, Value: 0x2 { 12 06 84 02 02 00 }
0x357F4: 				Or  { 16 02 }
0x357F6: 			End  { 29 02 }
0x357F8: 			Numeric Prompt: "Vsys/Psys Full Scale", Help: "Input Vsys or Psys Full-Scale and Critical Threshold to program Vsys/Psys Critical (0x4A) register. Critical Limit Trigger = (Critical Threshold/Full-Scale) * 0xFF. Input for Vsys is in Milli-Volts. For Psys either in Milli-Watts or Milli-Percent. For ATX12VO systems, recommended value is 200000. ", QuestionFlags: 0x10, QuestionId: 0x285, VarStoreId: 0x1, VarOffset: 0x38D, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E418, Step: 0x1 { 07 9A 21 06 22 06 85 02 01 00 8D 03 10 12 00 00 00 00 18 E4 03 00 01 00 00 00 }
0x35812: 				Default DefaultId: 0x0 Value: 200000 { 5B 09 00 00 02 40 0D 03 00 }
0x3581B: 			End  { 29 02 }
0x3581D: 			Numeric Prompt: "Vsys/Psys Critical Threshold", Help: "Input Vsys or Psys Full-Scale and Critical Threshold to program Vsys/Psys Critical (0x4A) register. Critical Limit Trigger = (Critical Threshold/Full-Scale) * 0xFF. Input for Vsys is in Milli-Volts. For Psys either in Milli-Watts or Milli-Percent. For ATX12VO systems, recommended value is 120000. ", QuestionFlags: 0x10, QuestionId: 0x286, VarStoreId: 0x1, VarOffset: 0x391, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E418, Step: 0x1 { 07 9A 23 06 24 06 86 02 01 00 91 03 10 12 00 00 00 00 18 E4 03 00 01 00 00 00 }
0x35837: 				Default DefaultId: 0x0 Value: 130000 { 5B 09 00 00 02 D0 FB 01 00 }
0x35840: 			End  { 29 02 }
0x35842: 		End  { 29 02 }
0x35844: 		SuppressIf  { 0A 82 }
0x35846: 			EqIdVal QuestionId: 0x284, Value: 0x0 { 12 86 84 02 00 00 }
0x3584C: 				EqIdVal QuestionId: 0x284, Value: 0x1 { 12 06 84 02 01 00 }
0x35852: 				Or  { 16 02 }
0x35854: 			End  { 29 02 }
0x35856: 			Numeric Prompt: "Vsys/Psys Full Scale", Help: "Input Vsys or Psys Full-Scale and Critical Threshold to program Vsys/Psys Critical (0x4A) register. Critical Limit Trigger = (Critical Threshold/Full-Scale) * 0xFF. Input for Vsys is in Milli-Volts. For Psys either in Milli-Watts or Milli-Percent. For ATX12VO systems, recommended value is 200000. ", QuestionFlags: 0x10, QuestionId: 0x287, VarStoreId: 0x1, VarOffset: 0x385, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E418, Step: 0x1 { 07 9A B2 07 22 06 87 02 01 00 85 03 10 12 00 00 00 00 18 E4 03 00 01 00 00 00 }
0x35870: 				Default DefaultId: 0x0 Value: 24000 { 5B 09 00 00 02 C0 5D 00 00 }
0x35879: 			End  { 29 02 }
0x3587B: 			Numeric Prompt: "Vsys/Psys Critical Threshold", Help: "Input Vsys or Psys Full-Scale and Critical Threshold to program Vsys/Psys Critical (0x4A) register. Critical Limit Trigger = (Critical Threshold/Full-Scale) * 0xFF. Input for Vsys is in Milli-Volts. For Psys either in Milli-Watts or Milli-Percent. For ATX12VO systems, recommended value is 120000. ", QuestionFlags: 0x10, QuestionId: 0x288, VarStoreId: 0x1, VarOffset: 0x389, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E418, Step: 0x1 { 07 9A B3 07 24 06 88 02 01 00 89 03 10 12 00 00 00 00 18 E4 03 00 01 00 00 00 }
0x35895: 				Default DefaultId: 0x0 Value: 6000 { 5B 09 00 00 02 70 17 00 00 }
0x3589E: 			End  { 29 02 }
0x358A0: 		End  { 29 02 }
0x358A2: 		Numeric Prompt: "Assertion Deglitch Mantissa ", Help: "Assertion Deglitch Mantissa 0x4F[7-3]. Assertion Deglitch = 2µs * Mantissa * 2^(Exponent) ", QuestionFlags: 0x10, QuestionId: 0x289, VarStoreId: 0x1, VarOffset: 0x2F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 25 06 26 06 89 02 01 00 F2 02 10 10 00 FF 01 }
0x358B3: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x358B9: 		End  { 29 02 }
0x358BB: 		Numeric Prompt: "Assertion Deglitch Exponent ", Help: "Assertion Deglitch Exponent 0x4F[3-0]. Assertion Deglitch = 2µs * Mantissa * 2^(Exponent)", QuestionFlags: 0x10, QuestionId: 0x28A, VarStoreId: 0x1, VarOffset: 0x2F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 27 06 28 06 8A 02 01 00 F3 02 10 10 00 FF 01 }
0x358CC: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x358D2: 		End  { 29 02 }
0x358D4: 		Numeric Prompt: "De assertion Deglitch Mantissa", Help: "De Assertion Deglitch Mantissa 0x49[7-3]. Assertion Deglitch = 2µs * Mantissa * 2^(Exponent) ", QuestionFlags: 0x10, QuestionId: 0x28B, VarStoreId: 0x1, VarOffset: 0x2F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 29 06 2A 06 8B 02 01 00 F4 02 10 10 00 FF 01 }
0x358E5: 			Default DefaultId: 0x0 Value: 13 { 5B 06 00 00 00 0D }
0x358EB: 		End  { 29 02 }
0x358ED: 		Numeric Prompt: "De assertion Deglitch Exponent", Help: "De Assertion Deglitch Exponent 0x49[3-0]. Assertion Deglitch = 2µs * Mantissa * 2^(Exponent) ", QuestionFlags: 0x10, QuestionId: 0x28C, VarStoreId: 0x1, VarOffset: 0x2F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 2B 06 2C 06 8C 02 01 00 F5 02 10 10 00 FF 01 }
0x358FE: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x35904: 		End  { 29 02 }
0x35906: 		OneOf Prompt: "VR Power Delivery Design", Help: "Specifies the ADL Desktop board design used for the VR settings override values. By default, BIOS will override the default Desktop VR settings based on the board design. A value of AUTO(0) will use the board ID to determine the board design. Any other value will override the board id logic to provide a custom VR Power Delivery Design value. This is intended primarily for validation.", QuestionFlags: 0x14, QuestionId: 0x2752, VarStoreId: 0x1, VarOffset: 0x313, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF4, Step: 0x0 { 05 91 CF 03 D0 03 52 27 01 00 13 03 14 10 00 F4 00 }
0x35917: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3591D: 			OneOfOption Option: "AUTO" Value: 0 { 09 07 D1 03 00 00 00 }
0x35924: 			SuppressIf  { 0A 82 }
0x35926: 				EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 86 42 11 02 00 }
0x3592C: 					Not  { 17 02 }
0x3592E: 					EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x35934: 					Not  { 17 02 }
0x35936: 					And  { 15 02 }
0x35938: 				End  { 29 02 }
0x3593A: 				OneOfOption Option: "ADL S 881 35W" Value: 1 { 09 07 D2 03 00 00 01 }
0x35941: 				OneOfOption Option: "ADL S 881 65W" Value: 3 { 09 07 D3 03 00 00 03 }
0x35948: 				OneOfOption Option: "ADL S 881 125W" Value: 4 { 09 07 D4 03 00 00 04 }
0x3594F: 				OneOfOption Option: "ADL S 841 35W" Value: 6 { 09 07 D5 03 00 00 06 }
0x35956: 				OneOfOption Option: "ADL S 841 65W" Value: 8 { 09 07 D6 03 00 00 08 }
0x3595D: 				OneOfOption Option: "ADL S 841 125W" Value: 9 { 09 07 D7 03 00 00 09 }
0x35964: 				OneOfOption Option: "ADL S 641 35W" Value: 10 { 09 07 D8 03 00 00 0A }
0x3596B: 				OneOfOption Option: "ADL S 641 65W" Value: 11 { 09 07 D9 03 00 00 0B }
0x35972: 				OneOfOption Option: "ADL S 641 125W" Value: 12 { 09 07 DA 03 00 00 0C }
0x35979: 				OneOfOption Option: "ADL S 681 35W" Value: 13 { 09 07 DB 03 00 00 0D }
0x35980: 				OneOfOption Option: "ADL S 801 35W" Value: 15 { 09 07 DC 03 00 00 0F }
0x35987: 				OneOfOption Option: "ADL S 801 65W" Value: 16 { 09 07 DD 03 00 00 10 }
0x3598E: 				OneOfOption Option: "ADL S 401 35W" Value: 18 { 09 07 DE 03 00 00 12 }
0x35995: 				OneOfOption Option: "ADL S 401 65W" Value: 19 { 09 07 DF 03 00 00 13 }
0x3599C: 				OneOfOption Option: "ADL S 601 35W" Value: 21 { 09 07 E0 03 00 00 15 }
0x359A3: 				OneOfOption Option: "ADL S 601 65W" Value: 22 { 09 07 E1 03 00 00 16 }
0x359AA: 				OneOfOption Option: "ADL S 201 35W" Value: 23 { 09 07 E2 03 00 00 17 }
0x359B1: 				OneOfOption Option: "ADL S 201 46W" Value: 24 { 09 07 E3 03 00 00 18 }
0x359B8: 				OneOfOption Option: "ADL S 201 65W" Value: 25 { 09 07 E4 03 00 00 19 }
0x359BF: 				OneOfOption Option: "ADL S 401 58W" Value: 26 { 09 07 E5 03 00 00 1A }
0x359C6: 				OneOfOption Option: "ADL S 401 60W" Value: 27 { 09 07 E6 03 00 00 1B }
0x359CD: 				OneOfOption Option: "ADL S 401 63W" Value: 28 { 09 07 E7 03 00 00 1C }
0x359D4: 				OneOfOption Option: "ADL S BGA 881 65W" Value: 29 { 09 07 E8 03 00 00 1D }
0x359DB: 				OneOfOption Option: "ADL S BGA 841 65W" Value: 30 { 09 07 E9 03 00 00 1E }
0x359E2: 				OneOfOption Option: "ADL S BGA 441 65W" Value: 31 { 09 07 EA 03 00 00 1F }
0x359E9: 				OneOfOption Option: "ADL S BGA 601 65W" Value: 32 { 09 07 EB 03 00 00 20 }
0x359F0: 				OneOfOption Option: "ADL S BGA 681 65W" Value: 33 { 09 07 EC 03 00 00 21 }
0x359F7: 				OneOfOption Option: "ADL S BGA 401 65W" Value: 34 { 09 07 ED 03 00 00 22 }
0x359FE: 				OneOfOption Option: "ADL S Mobile BGA 881 55W" Value: 35 { 09 07 EE 03 00 00 23 }
0x35A05: 				OneOfOption Option: "ADL S Mobile BGA 681 55W" Value: 36 { 09 07 EF 03 00 00 24 }
0x35A0C: 				OneOfOption Option: "ADL S Mobile BGA 481 55W" Value: 37 { 09 07 F0 03 00 00 25 }
0x35A13: 				OneOfOption Option: "ADL S Mobile BGA 441 55W" Value: 38 { 09 07 F1 03 00 00 26 }
0x35A1A: 				OneOfOption Option: "RPL S 8161 35W" Value: 128 { 09 07 F2 03 00 00 80 }
0x35A21: 				OneOfOption Option: "RPL S 8161 65W" Value: 129 { 09 07 F3 03 00 00 81 }
0x35A28: 				OneOfOption Option: "RPL S 8161 95W" Value: 130 { 09 07 F4 03 00 00 82 }
0x35A2F: 				OneOfOption Option: "RPL S 8161 125W" Value: 131 { 09 07 F5 03 00 00 83 }
0x35A36: 				OneOfOption Option: "RPL S 8161 150W" Value: 132 { 09 07 F6 03 00 00 84 }
0x35A3D: 				OneOfOption Option: "RPL S 881 35W" Value: 133 { 09 07 F7 03 00 00 85 }
0x35A44: 				OneOfOption Option: "RPL S 881 65W" Value: 134 { 09 07 F8 03 00 00 86 }
0x35A4B: 				OneOfOption Option: "RPL S 881 125W" Value: 135 { 09 07 F9 03 00 00 87 }
0x35A52: 				OneOfOption Option: "RPL S 681 125W" Value: 136 { 09 07 FA 03 00 00 88 }
0x35A59: 				OneOfOption Option: "RPL S 641 65W" Value: 137 { 09 07 FB 03 00 00 89 }
0x35A60: 				OneOfOption Option: "RPL S 641 125W" Value: 138 { 09 07 FC 03 00 00 8A }
0x35A67: 				OneOfOption Option: "RPL S 801 80W" Value: 139 { 09 07 FD 03 00 00 8B }
0x35A6E: 				OneOfOption Option: "RPL S 801 95W" Value: 140 { 09 07 FE 03 00 00 8C }
0x35A75: 				OneOfOption Option: "RPL S 641 35W" Value: 143 { 09 07 FF 03 00 00 8F }
0x35A7C: 				OneOfOption Option: "RPL S 8121 35W" Value: 153 { 09 07 00 04 00 00 99 }
0x35A83: 				OneOfOption Option: "RPL S 8121 65W" Value: 154 { 09 07 01 04 00 00 9A }
0x35A8A: 				OneOfOption Option: "RPL S 8121 125W" Value: 155 { 09 07 02 04 00 00 9B }
0x35A91: 				OneOfOption Option: "RPL HX SBGA 8161 55W" Value: 160 { 09 07 03 04 00 00 A0 }
0x35A98: 				OneOfOption Option: "RPL HX SBGA 8121 55W" Value: 162 { 09 07 04 04 00 00 A2 }
0x35A9F: 				OneOfOption Option: "RPL HX SBGA 881 55W" Value: 164 { 09 07 05 04 00 00 A4 }
0x35AA6: 				OneOfOption Option: "RPL HX SBGA 681 55W" Value: 170 { 09 07 06 04 00 00 AA }
0x35AAD: 				OneOfOption Option: "RPL HX SBGA 641 55W" Value: 171 { 09 07 07 04 00 00 AB }
0x35AB4: 				OneOfOption Option: "RPL HX SBGA 441 55W" Value: 172 { 09 07 08 04 00 00 AC }
0x35ABB: 				OneOfOption Option: "RPL2 S 681 35W" Value: 224 { 09 07 09 04 00 00 E0 }
0x35AC2: 				OneOfOption Option: "RPL2 S 681 65W" Value: 225 { 09 07 0A 04 00 00 E1 }
0x35AC9: 				OneOfOption Option: "RPL2 S 641 35W" Value: 226 { 09 07 0B 04 00 00 E2 }
0x35AD0: 				OneOfOption Option: "RPL2 S 641 65W" Value: 227 { 09 07 0C 04 00 00 E3 }
0x35AD7: 				OneOfOption Option: "RPL2 S 401 35W" Value: 228 { 09 07 0D 04 00 00 E4 }
0x35ADE: 				OneOfOption Option: "RPL2 S 401 58W" Value: 229 { 09 07 0E 04 00 00 E5 }
0x35AE5: 				OneOfOption Option: "RPL2 S 401 60W" Value: 230 { 09 07 0F 04 00 00 E6 }
0x35AEC: 				OneOfOption Option: "RPL2 S 401 65W" Value: 231 { 09 07 10 04 00 00 E7 }
0x35AF3: 				OneOfOption Option: "RPL2 S 201 35W" Value: 232 { 09 07 11 04 00 00 E8 }
0x35AFA: 				OneOfOption Option: "RPL2 S 201 46W" Value: 233 { 09 07 12 04 00 00 E9 }
0x35B01: 				OneOfOption Option: "RPL2 S 201 65W" Value: 234 { 09 07 13 04 00 00 EA }
0x35B08: 				OneOfOption Option: "RPL2 S 601 65W" Value: 235 { 09 07 14 04 00 00 EB }
0x35B0F: 				OneOfOption Option: "RPL2 HX SBGA 881 55W" Value: 240 { 09 07 15 04 00 00 F0 }
0x35B16: 				OneOfOption Option: "RPL2 HX SBGA 681 55W" Value: 241 { 09 07 16 04 00 00 F1 }
0x35B1D: 				OneOfOption Option: "RPL2 HX SBGA 641 55W" Value: 242 { 09 07 17 04 00 00 F2 }
0x35B24: 				OneOfOption Option: "RPL2 HX SBGA 481 55W" Value: 243 { 09 07 18 04 00 00 F3 }
0x35B2B: 				OneOfOption Option: "RPL2 HX SBGA 441 55W" Value: 244 { 09 07 19 04 00 00 F4 }
0x35B32: 			End  { 29 02 }
0x35B34: 			SuppressIf  { 0A 82 }
0x35B36: 				EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x35B3C: 					Not  { 17 02 }
0x35B3E: 					EqIdVal QuestionId: 0x120D, Value: 0x0 { 12 06 0D 12 00 00 }
0x35B44: 					Not  { 17 02 }
0x35B46: 					Or  { 16 02 }
0x35B48: 				End  { 29 02 }
0x35B4A: 				OneOfOption Option: "ADL P 282 15W" Value: 48 { 09 07 1A 04 00 00 30 }
0x35B51: 				OneOfOption Option: "ADL P 482 28W" Value: 49 { 09 07 1B 04 00 00 31 }
0x35B58: 				OneOfOption Option: "ADL P 682 28W" Value: 50 { 09 07 1C 04 00 00 32 }
0x35B5F: 				OneOfOption Option: "ADL P 682 45W" Value: 53 { 09 07 1D 04 00 00 35 }
0x35B66: 				OneOfOption Option: "ADL P 142 15W" Value: 54 { 09 07 1E 04 00 00 36 }
0x35B6D: 				OneOfOption Option: "ADL P 242 15W" Value: 55 { 09 07 1F 04 00 00 37 }
0x35B74: 				OneOfOption Option: "ADL P 482 45W" Value: 56 { 09 07 20 04 00 00 38 }
0x35B7B: 				OneOfOption Option: "ADL P 442 45W" Value: 57 { 09 07 21 04 00 00 39 }
0x35B82: 				OneOfOption Option: "ADL P 442 28W" Value: 58 { 09 07 22 04 00 00 3A }
0x35B89: 				OneOfOption Option: "ADL P 282 28W" Value: 59 { 09 07 23 04 00 00 3B }
0x35B90: 				OneOfOption Option: "ADL P 242 28W" Value: 60 { 09 07 24 04 00 00 3C }
0x35B97: 				OneOfOption Option: "ADL P 142 28W" Value: 61 { 09 07 25 04 00 00 3D }
0x35B9E: 				OneOfOption Option: "ADL P 242 45W" Value: 62 { 09 07 26 04 00 00 3E }
0x35BA5: 				OneOfOption Option: "ADL P 182 28W" Value: 63 { 09 07 27 04 00 00 3F }
0x35BAC: 				OneOfOption Option: "ADL P 662 28W" Value: 64 { 09 07 28 04 00 00 40 }
0x35BB3: 				OneOfOption Option: "ADL P 642 28W" Value: 65 { 09 07 29 04 00 00 41 }
0x35BBA: 				OneOfOption Option: "ADL P 642 45W" Value: 66 { 09 07 2A 04 00 00 42 }
0x35BC1: 			End  { 29 02 }
0x35BC3: 			SuppressIf  { 0A 82 }
0x35BC5: 				EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x35BCB: 					Not  { 17 02 }
0x35BCD: 					EqIdVal QuestionId: 0x120D, Value: 0x0 { 12 06 0D 12 00 00 }
0x35BD3: 					Or  { 16 02 }
0x35BD5: 				End  { 29 02 }
0x35BD7: 				OneOfOption Option: "ADL M 18 7W PMIC" Value: 80 { 09 07 3D 04 00 00 50 }
0x35BDE: 				OneOfOption Option: "ADL M 18 5W PMIC" Value: 81 { 09 07 3E 04 00 00 51 }
0x35BE5: 				OneOfOption Option: "ADL M 14 5W PMIC" Value: 82 { 09 07 3F 04 00 00 52 }
0x35BEC: 				OneOfOption Option: "ADL M 14 7W PMIC" Value: 83 { 09 07 40 04 00 00 53 }
0x35BF3: 				OneOfOption Option: "ADL M 24 7W Discrete/Hybrid" Value: 84 { 09 07 41 04 00 00 54 }
0x35BFA: 				OneOfOption Option: "ADL M 28 7W Discrete/Hybrid" Value: 85 { 09 07 42 04 00 00 55 }
0x35C01: 				OneOfOption Option: "ADL M 18 7W Discrete/Hybrid" Value: 86 { 09 07 43 04 00 00 56 }
0x35C08: 				OneOfOption Option: "ADL M 28 9W Discrete/Hybrid" Value: 87 { 09 07 46 04 00 00 57 }
0x35C0F: 				OneOfOption Option: "ADL M 14 9W Discrete/Hybrid" Value: 88 { 09 07 44 04 00 00 58 }
0x35C16: 				OneOfOption Option: "ADL M 24 9W Discrete/Hybrid" Value: 89 { 09 07 45 04 00 00 59 }
0x35C1D: 				OneOfOption Option: "ADL M 14 12W Discrete/Hybrid" Value: 96 { 09 07 47 04 00 00 60 }
0x35C24: 				OneOfOption Option: "ADL M 24 12W Discrete/Hybrid" Value: 97 { 09 07 48 04 00 00 61 }
0x35C2B: 				OneOfOption Option: "ADL M 18 12W Discrete/Hybrid" Value: 98 { 09 07 4A 04 00 00 62 }
0x35C32: 				OneOfOption Option: "ADL M 28 12W Discrete/Hybrid" Value: 99 { 09 07 49 04 00 00 63 }
0x35C39: 			End  { 29 02 }
0x35C3B: 		End  { 29 02 }
0x35C3D: 		Ref Prompt: "Acoustic Noise Settings", Help: "Configure Acoustic Noise Settings for IA, GT and SA domains", QuestionFlags: 0x0, QuestionId: 0x28D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2767 { 0F 0F AE 03 AF 03 8D 02 00 00 FF FF 00 67 27 }
0x35C4C: 		SuppressIf  { 0A 82 }
0x35C4E: 			EqIdVal QuestionId: 0x11E4, Value: 0x1 { 12 06 E4 11 01 00 }
0x35C54: 			Ref Prompt: "Core/IA VR Settings", Help: "Core/IA VR Settings", QuestionFlags: 0x0, QuestionId: 0x28E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2768 { 0F 0F B4 03 B4 03 8E 02 00 00 FF FF 00 68 27 }
0x35C63: 		End  { 29 02 }
0x35C65: 		SuppressIf  { 0A 82 }
0x35C67: 			EqIdVal QuestionId: 0x11E3, Value: 0x1 { 12 06 E3 11 01 00 }
0x35C6D: 			Ref Prompt: "GT VR Settings", Help: "GT VR Settings", QuestionFlags: 0x0, QuestionId: 0x28F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2769 { 0F 0F B6 03 B6 03 8F 02 00 00 FF FF 00 69 27 }
0x35C7C: 		End  { 29 02 }
0x35C7E: 		SuppressIf  { 0A 82 }
0x35C80: 			EqIdVal QuestionId: 0x120E, Value: 0x1 { 12 86 0E 12 01 00 }
0x35C86: 				EqIdVal QuestionId: 0x120D, Value: 0x0 { 12 06 0D 12 00 00 }
0x35C8C: 				Or  { 16 02 }
0x35C8E: 			End  { 29 02 }
0x35C90: 			Ref Prompt: "SA VR Settings", Help: "SA VR Settings", QuestionFlags: 0x0, QuestionId: 0x290, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276A { 0F 0F B8 03 B8 03 90 02 00 00 FF FF 00 6A 27 }
0x35C9F: 		End  { 29 02 }
0x35CA1: 		SuppressIf  { 0A 82 }
0x35CA3: 			EqIdVal QuestionId: 0x120B, Value: 0x0 { 12 06 0B 12 00 00 }
0x35CA9: 			Ref Prompt: "RFI Settings", Help: "RFI Settings", QuestionFlags: 0x0, QuestionId: 0x291, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276B { 0F 0F BA 03 BA 03 91 02 00 00 FF FF 00 6B 27 }
0x35CB8: 		End  { 29 02 }
0x35CBA: 	End  { 29 02 }
0x35CBC: 	Form FormId: 0x2767, Title: "Acoustic Noise Settings" { 01 86 67 27 AE 03 }
0x35CC2: 		Subtitle Prompt: "Acoustic Noise Settings", Help: "", Flags: 0x0 { 02 87 B0 03 00 00 00 }
0x35CC9: 		End  { 29 02 }
0x35CCB: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x35CD2: 		End  { 29 02 }
0x35CD4: 		OneOf Prompt: "Acoustic Noise Mitigation", Help: "Enabling this option will help mitigate acoustic noise on certain SKUs when the CPU is in deeper C state", QuestionFlags: 0x10, QuestionId: 0x292, VarStoreId: 0x1, VarOffset: 0x1FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 06 2E 06 92 02 01 00 FC 01 10 10 00 01 00 }
0x35CE5: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x35CEC: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x35CF3: 		End  { 29 02 }
0x35CF5: 		GrayOutIf  { 19 82 }
0x35CF7: 			EqIdVal QuestionId: 0x292, Value: 0x0 { 12 06 92 02 00 00 }
0x35CFD: 			Numeric Prompt: "Pre Wake Time", Help: "Set the maximum Pre Wake randomization time in micro ticks. Range is 0-255. This is for acoustic noise mitigation Dynamic Perodicity Alteration (DPA) tuning.", QuestionFlags: 0x10, QuestionId: 0x293, VarStoreId: 0x1, VarOffset: 0x2D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 35 06 36 06 93 02 01 00 D9 02 10 10 00 FF 01 }
0x35D0E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35D14: 			End  { 29 02 }
0x35D16: 			Numeric Prompt: "Ramp Up Time", Help: "Set the maximum Ramp Up randomization time in micro ticks. Range is 0-255. This is for acoustic noise mitigation Dynamic Perodicity Alteration (DPA) tuning.", QuestionFlags: 0x10, QuestionId: 0x294, VarStoreId: 0x1, VarOffset: 0x2DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 37 06 38 06 94 02 01 00 DA 02 10 10 00 FF 01 }
0x35D27: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35D2D: 			End  { 29 02 }
0x35D2F: 			Numeric Prompt: "Ramp Down Time", Help: "Set the maximum Ramp Down randomization time in micro ticks. Range is 0-255. This is for acoustic noise mitigation Dynamic Perodicity Alteration (DPA) tuning.", QuestionFlags: 0x10, QuestionId: 0x295, VarStoreId: 0x1, VarOffset: 0x2DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 39 06 3A 06 95 02 01 00 DB 02 10 10 00 FF 01 }
0x35D40: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x35D46: 			End  { 29 02 }
0x35D48: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x35D4F: 			End  { 29 02 }
0x35D51: 			Subtitle Prompt: "IA VR Domain", Help: "", Flags: 0x0 { 02 87 B1 03 00 00 00 }
0x35D58: 			End  { 29 02 }
0x35D5A: 			OneOf Prompt: "Disable Fast PKG C State Ramp for IA Domain", Help: "This option needs to be configured to reduce acoustic noise during deeper C states. False: Don't disable Fast ramp during deeper C states; True: Disable Fast ramp during deeper C state", QuestionFlags: 0x10, QuestionId: 0x296, VarStoreId: 0x1, VarOffset: 0x1FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 06 32 06 96 02 01 00 FD 01 10 10 00 01 00 }
0x35D6B: 				OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault { 09 07 33 06 30 00 00 }
0x35D72: 				OneOfOption Option: "TRUE" Value: 1 { 09 07 34 06 00 00 01 }
0x35D79: 			End  { 29 02 }
0x35D7B: 			OneOf Prompt: "Slow Slew Rate for IA Domain", Help: "Set VR IA Slow Slew Rate for Deep Package C State ramp time; Slow slew rate equals to Fast divided by number, the number is 2, 4, 8, 16 to slow down the slew rate to help minimize acoustic noise", QuestionFlags: 0x10, QuestionId: 0x297, VarStoreId: 0x1, VarOffset: 0x202, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 3B 06 3C 06 97 02 01 00 02 02 10 10 00 03 00 }
0x35D8C: 				OneOfOption Option: "Fast/2" Value: 0, Default, MfgDefault { 09 07 3F 06 30 00 00 }
0x35D93: 				OneOfOption Option: "Fast/4" Value: 1 { 09 07 40 06 00 00 01 }
0x35D9A: 				OneOfOption Option: "Fast/8" Value: 2 { 09 07 41 06 00 00 02 }
0x35DA1: 				OneOfOption Option: "Fast/16" Value: 3 { 09 07 42 06 00 00 03 }
0x35DA8: 			End  { 29 02 }
0x35DAA: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x35DB1: 			End  { 29 02 }
0x35DB3: 			Subtitle Prompt: "GT VR Domain", Help: "", Flags: 0x0 { 02 87 B2 03 00 00 00 }
0x35DBA: 			End  { 29 02 }
0x35DBC: 			OneOf Prompt: "Disable Fast PKG C State Ramp for GT Domain", Help: "This option needs to be configured to reduce acoustic noise during deeper C states. False: Don't disable Fast ramp during deeper C states; True: Disable Fast ramp during deeper C state", QuestionFlags: 0x10, QuestionId: 0x298, VarStoreId: 0x1, VarOffset: 0x1FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 06 32 06 98 02 01 00 FE 01 10 10 00 01 00 }
0x35DCD: 				OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault { 09 07 33 06 30 00 00 }
0x35DD4: 				OneOfOption Option: "TRUE" Value: 1 { 09 07 34 06 00 00 01 }
0x35DDB: 			End  { 29 02 }
0x35DDD: 			OneOf Prompt: "Slow Slew Rate for GT Domain", Help: "Set VR GT Slow Slew Rate for Deep Package C State ramp time; Slow slew rate equals to Fast divided by number, the number is 2, 4, 8 to slow down the slew rate to help minimize acoustic noise; divide by 16 is disabled", QuestionFlags: 0x10, QuestionId: 0x299, VarStoreId: 0x1, VarOffset: 0x203, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 3D 06 3E 06 99 02 01 00 03 02 10 10 00 02 00 }
0x35DEE: 				OneOfOption Option: "Fast/2" Value: 0, Default, MfgDefault { 09 07 3F 06 30 00 00 }
0x35DF5: 				OneOfOption Option: "Fast/4" Value: 1 { 09 07 40 06 00 00 01 }
0x35DFC: 				OneOfOption Option: "Fast/8" Value: 2 { 09 07 41 06 00 00 02 }
0x35E03: 			End  { 29 02 }
0x35E05: 			SuppressIf  { 0A 82 }
0x35E07: 				EqIdVal QuestionId: 0x120D, Value: 0x0 { 12 06 0D 12 00 00 }
0x35E0D: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x35E14: 				End  { 29 02 }
0x35E16: 				Subtitle Prompt: "SA VR Domain", Help: "", Flags: 0x0 { 02 87 B3 03 00 00 00 }
0x35E1D: 				End  { 29 02 }
0x35E1F: 				OneOf Prompt: "Disable Fast PKG C State Ramp for SA Domain", Help: "This option needs to be configured to reduce acoustic noise during deeper C states. False: Don't disable Fast ramp during deeper C states; True: Disable Fast ramp during deeper C state", QuestionFlags: 0x10, QuestionId: 0x29A, VarStoreId: 0x1, VarOffset: 0x1FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 06 32 06 9A 02 01 00 FF 01 10 10 00 01 00 }
0x35E30: 					OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault { 09 07 33 06 30 00 00 }
0x35E37: 					OneOfOption Option: "TRUE" Value: 1 { 09 07 34 06 00 00 01 }
0x35E3E: 				End  { 29 02 }
0x35E40: 			End  { 29 02 }
0x35E42: 		End  { 29 02 }
0x35E44: 	End  { 29 02 }
0x35E46: 	Form FormId: 0x2768, Title: "Core/IA VR Settings" { 01 86 68 27 B4 03 }
0x35E4C: 		Subtitle Prompt: "Core/IA VR Domain", Help: "", Flags: 0x0 { 02 87 B5 03 00 00 00 }
0x35E53: 		End  { 29 02 }
0x35E55: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x35E5C: 		End  { 29 02 }
0x35E5E: 		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0x29B, VarStoreId: 0x1, VarOffset: 0x12D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 05 EA 05 9B 02 01 00 2D 01 10 10 00 01 00 }
0x35E6F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x35E76: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x35E7D: 		End  { 29 02 }
0x35E7F: 		SuppressIf  { 0A 82 }
0x35E81: 			EqIdVal QuestionId: 0x29B, Value: 0x0 { 12 06 9B 02 00 00 }
0x35E87: 			Text Prompt: "Current AC Loadline", Help: "Current AC Loadline", Text: "" { 03 08 B5 05 B4 05 B6 05 }
0x35E8F: 			Text Prompt: "Current DC Loadline", Help: "Current DC Loadline", Text: "" { 03 08 BA 05 B9 05 BB 05 }
0x35E97: 			Text Prompt: "Current Psi1 Threshold", Help: "Current Psi1 Threshold", Text: "" { 03 08 BF 05 BE 05 C0 05 }
0x35E9F: 			Text Prompt: "Current Psi2 Threshold", Help: "Current Psi2 Threshold", Text: "" { 03 08 C4 05 C3 05 C5 05 }
0x35EA7: 			Text Prompt: "Current Psi3 Threshold", Help: "Current Psi3 Threshold", Text: "" { 03 08 C9 05 C8 05 CA 05 }
0x35EAF: 			Text Prompt: "Current Imon Slope", Help: "Current Imon Slope", Text: "" { 03 08 CE 05 CD 05 CF 05 }
0x35EB7: 			Text Prompt: "Current Imon Offset", Help: "Current Imon Offset", Text: "" { 03 08 D3 05 D2 05 D4 05 }
0x35EBF: 			Text Prompt: "Current VR Current Limit", Help: "Current VR Current Limit (Current IccMax Value)", Text: "" { 03 08 D8 05 D7 05 D9 05 }
0x35EC7: 			Text Prompt: "Current Tdc Current Limit", Help: "Current Tdc Current Limit", Text: "" { 03 08 DD 05 DC 05 DE 05 }
0x35ECF: 			Text Prompt: "Current Voltage Limit", Help: "Current Voltage Limit", Text: "" { 03 08 E2 05 E1 05 E3 05 }
0x35ED7: 			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x29C, VarStoreId: 0x1, VarOffset: 0x132, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0 { 07 94 EB 05 EC 05 9C 02 01 00 32 01 10 11 00 00 24 F4 00 00 }
0x35EEB: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35EF2: 			End  { 29 02 }
0x35EF4: 			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x29D, VarStoreId: 0x1, VarOffset: 0x13C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0 { 07 94 ED 05 EE 05 9D 02 01 00 3C 01 10 11 00 00 24 F4 00 00 }
0x35F08: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35F0F: 			End  { 29 02 }
0x35F11: 			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x29E, VarStoreId: 0x1, VarOffset: 0x146, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 FB 05 FC 05 9E 02 01 00 46 01 10 11 00 00 00 02 01 00 }
0x35F25: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x35F2C: 			End  { 29 02 }
0x35F2E: 			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x29F, VarStoreId: 0x1, VarOffset: 0x150, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 FD 05 FE 05 9F 02 01 00 50 01 10 11 00 00 00 02 01 00 }
0x35F42: 				Default DefaultId: 0x0 Value: 20 { 5B 07 00 00 01 14 00 }
0x35F49: 			End  { 29 02 }
0x35F4B: 			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2A0, VarStoreId: 0x1, VarOffset: 0x15A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 FF 05 00 06 A0 02 01 00 5A 01 10 11 00 00 00 02 01 00 }
0x35F5F: 				Default DefaultId: 0x0 Value: 4 { 5B 07 00 00 01 04 00 }
0x35F66: 			End  { 29 02 }
0x35F68: 			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2A1, VarStoreId: 0x1, VarOffset: 0x164, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 06 02 06 A1 02 01 00 64 01 10 10 00 01 00 }
0x35F79: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x35F80: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x35F87: 			End  { 29 02 }
0x35F89: 			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0x2A2, VarStoreId: 0x1, VarOffset: 0x169, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 03 06 04 06 A2 02 01 00 69 01 10 10 00 01 00 }
0x35F9A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x35FA1: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x35FA8: 			End  { 29 02 }
0x35FAA: 			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x2A3, VarStoreId: 0x1, VarOffset: 0x16E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xC8, Step: 0x1 { 07 94 07 06 08 06 A3 02 01 00 6E 01 10 11 00 00 C8 00 01 00 }
0x35FBE: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35FC5: 			End  { 29 02 }
0x35FC7: 			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x2A4, VarStoreId: 0x1, VarOffset: 0x178, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1 { 07 94 09 06 0A 06 A4 02 01 00 78 01 10 11 00 00 FF F9 01 00 }
0x35FDB: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x35FE2: 			End  { 29 02 }
0x35FE4: 			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2A5, VarStoreId: 0x1, VarOffset: 0x182, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 06 0C 06 A5 02 01 00 82 01 10 10 00 01 00 }
0x35FF5: 				OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x35FFC: 				OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x36003: 			End  { 29 02 }
0x36005: 			GrayOutIf  { 19 82 }
0x36007: 				EqIdVal QuestionId: 0x2881, Value: 0x1 { 12 06 81 28 01 00 }
0x3600D: 				Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (IccMax). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x2A6, VarStoreId: 0x1, VarOffset: 0x187, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x800, Step: 0x1 { 07 94 EF 05 F0 05 A6 02 01 00 87 01 10 11 00 00 00 08 01 00 }
0x36021: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36028: 				End  { 29 02 }
0x3602A: 			End  { 29 02 }
0x3602C: 			SuppressIf  { 0A 82 }
0x3602E: 				EqIdVal QuestionId: 0x120C, Value: 0x0 { 12 06 0C 12 00 00 }
0x36034: 				OneOf Prompt: "Core VR Fast Vmode", Help: "Core VR Fast Vmode. Use to control Core Fast Vmode Enable/Disable. The value will only be effective by enabling the corresponding CEP..", QuestionFlags: 0x14, QuestionId: 0x2753, VarStoreId: 0x1, VarOffset: 0x379, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 05 F2 05 53 27 01 00 79 03 14 10 00 01 00 }
0x36045: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3604C: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x36053: 				End  { 29 02 }
0x36055: 				SuppressIf  { 0A 82 }
0x36057: 					EqIdVal QuestionId: 0x2753, Value: 0x0 { 12 06 53 27 00 00 }
0x3605D: 					Numeric Prompt: "  Fast Vmode Itrip ICC Limit", Help: "Voltage Regulator Fast Vmode Itrip ICC Limit. A value of 400 = 100A. A value of 0 corresponds to feature disabled (no reactive protection). This value represents the current threshold where the VR would initiate reactive protection if Fast Vmode is enabled. The value is represented in 1/4 A increments. Uses BIOS VR mailbox command 0x25.", QuestionFlags: 0x14, QuestionId: 0x2754, VarStoreId: 0x1, VarOffset: 0x32A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F8, Step: 0x1 { 07 94 F7 05 F8 05 54 27 01 00 2A 03 14 11 00 00 F8 07 01 00 }
0x36071: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36078: 					End  { 29 02 }
0x3607A: 				End  { 29 02 }
0x3607C: 			End  { 29 02 }
0x3607E: 			Numeric Prompt: "VR Voltage Limit", Help: "Voltage Limit (VMAX). This value represents the Maximum instantaneous voltage allowed at any given time. Range is 0 - 7999mV. Uses BIOS VR mailbox command 0x8.", QuestionFlags: 0x10, QuestionId: 0x2A7, VarStoreId: 0x1, VarOffset: 0x1BE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1 { 07 94 05 06 06 06 A7 02 01 00 BE 01 10 11 00 00 3F 1F 01 00 }
0x36092: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36099: 			End  { 29 02 }
0x3609B: 			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x2A8, VarStoreId: 0x1, VarOffset: 0x19B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 43 06 44 06 A8 02 01 00 9B 01 10 10 00 01 00 }
0x360AC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x360B3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x360BA: 			End  { 29 02 }
0x360BC: 			SuppressIf  { 0A 82 }
0x360BE: 				EqIdVal QuestionId: 0x2A8, Value: 0x0 { 12 06 A8 02 00 00 }
0x360C4: 				Numeric Prompt: "TDC Current Limit", Help: "TDC Current Limit, defined in 1/8A increments. Range 0-32767. For a TDC Current Limit of 125A, enter 1000. 0 = 0 Amps. Uses BIOS VR mailbox command 0x1A.", QuestionFlags: 0x10, QuestionId: 0x2A9, VarStoreId: 0x1, VarOffset: 0x191, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FFF, Step: 0x7D { 07 94 45 06 46 06 A9 02 01 00 91 01 10 11 00 00 FF 7F 7D 00 }
0x360D8: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x360DF: 				End  { 29 02 }
0x360E1: 				OneOf Prompt: "TDC Time Window", Help: "VR TDC Time Window, value in seconds. 1s is default. Range from 1s to 448s.", QuestionFlags: 0x10, QuestionId: 0x2AA, VarStoreId: 0x1, VarOffset: 0x1A0, Flags: 0x12, Size: 32, Min: 0x3E8, Max: 0x6D600, Step: 0x0 { 05 9A 47 06 48 06 AA 02 01 00 A0 01 10 12 E8 03 00 00 00 D6 06 00 00 00 00 00 }
0x360FB: 					OneOfOption Option: "1 sec" Value: 1000, Default, MfgDefault { 09 0A 58 06 32 02 E8 03 00 00 }
0x36105: 					OneOfOption Option: "2 sec" Value: 2000 { 09 0A 59 06 02 02 D0 07 00 00 }
0x3610F: 					OneOfOption Option: "3 sec" Value: 3000 { 09 0A 5A 06 02 02 B8 0B 00 00 }
0x36119: 					OneOfOption Option: "4 sec" Value: 4000 { 09 0A 5B 06 02 02 A0 0F 00 00 }
0x36123: 					OneOfOption Option: "5 sec" Value: 5000 { 09 0A 5C 06 02 02 88 13 00 00 }
0x3612D: 					OneOfOption Option: "6 sec" Value: 6000 { 09 0A 5D 06 02 02 70 17 00 00 }
0x36137: 					OneOfOption Option: "7 sec" Value: 7000 { 09 0A 5E 06 02 02 58 1B 00 00 }
0x36141: 					OneOfOption Option: "8 sec" Value: 8000 { 09 0A 5F 06 02 02 40 1F 00 00 }
0x3614B: 					OneOfOption Option: "10 sec" Value: 10000 { 09 0A 60 06 02 02 10 27 00 00 }
0x36155: 					OneOfOption Option: "12 sec" Value: 12000 { 09 0A 61 06 02 02 E0 2E 00 00 }
0x3615F: 					OneOfOption Option: "14 sec" Value: 14000 { 09 0A 62 06 02 02 B0 36 00 00 }
0x36169: 					OneOfOption Option: "16 sec" Value: 16000 { 09 0A 63 06 02 02 80 3E 00 00 }
0x36173: 					OneOfOption Option: "20 sec" Value: 20000 { 09 0A 64 06 02 02 20 4E 00 00 }
0x3617D: 					OneOfOption Option: "24 sec" Value: 24000 { 09 0A 65 06 02 02 C0 5D 00 00 }
0x36187: 					OneOfOption Option: "28 sec" Value: 28000 { 09 0A 66 06 02 02 60 6D 00 00 }
0x36191: 					OneOfOption Option: "32 sec" Value: 32000 { 09 0A 67 06 02 02 00 7D 00 00 }
0x3619B: 					OneOfOption Option: "40 sec" Value: 40000 { 09 0A 68 06 02 02 40 9C 00 00 }
0x361A5: 					OneOfOption Option: "48 sec" Value: 48000 { 09 0A 69 06 02 02 80 BB 00 00 }
0x361AF: 					OneOfOption Option: "56 sec" Value: 56000 { 09 0A 6A 06 02 02 C0 DA 00 00 }
0x361B9: 					OneOfOption Option: "64 sec" Value: 64000 { 09 0A 6B 06 02 02 00 FA 00 00 }
0x361C3: 					OneOfOption Option: "80 sec" Value: 80000 { 09 0A 6C 06 02 02 80 38 01 00 }
0x361CD: 					OneOfOption Option: "96 sec" Value: 96000 { 09 0A 6D 06 02 02 00 77 01 00 }
0x361D7: 					OneOfOption Option: "112 sec" Value: 112000 { 09 0A 6E 06 02 02 80 B5 01 00 }
0x361E1: 					OneOfOption Option: "128 sec" Value: 128000 { 09 0A 6F 06 02 02 00 F4 01 00 }
0x361EB: 					OneOfOption Option: "160 sec" Value: 160000 { 09 0A 70 06 02 02 00 71 02 00 }
0x361F5: 					OneOfOption Option: "192 sec" Value: 192000 { 09 0A 71 06 02 02 00 EE 02 00 }
0x361FF: 					OneOfOption Option: "224 sec" Value: 224000 { 09 0A 72 06 02 02 00 6B 03 00 }
0x36209: 					OneOfOption Option: "256 sec" Value: 256000 { 09 0A 73 06 02 02 00 E8 03 00 }
0x36213: 					OneOfOption Option: "320 sec" Value: 320000 { 09 0A 74 06 02 02 00 E2 04 00 }
0x3621D: 					OneOfOption Option: "384 sec" Value: 384000 { 09 0A 75 06 02 02 00 DC 05 00 }
0x36227: 					OneOfOption Option: "448 sec" Value: 448000 { 09 0A 76 06 02 02 00 D6 06 00 }
0x36231: 				End  { 29 02 }
0x36233: 				OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x2AB, VarStoreId: 0x1, VarOffset: 0x1B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 77 06 78 06 AB 02 01 00 B4 01 10 10 00 01 00 }
0x36244: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3624B: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36252: 				End  { 29 02 }
0x36254: 			End  { 29 02 }
0x36256: 			OneOf Prompt: "IRMS", Help: "Enable/Disable IRMS - Current root mean square", QuestionFlags: 0x10, QuestionId: 0x2AC, VarStoreId: 0x1, VarOffset: 0x1B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 79 06 7A 06 AC 02 01 00 B9 01 10 10 00 01 00 }
0x36267: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3626E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36275: 			End  { 29 02 }
0x36277: 		End  { 29 02 }
0x36279: 	End  { 29 02 }
0x3627B: 	Form FormId: 0x2769, Title: "GT VR Settings" { 01 86 69 27 B6 03 }
0x36281: 		Subtitle Prompt: "GT Domain", Help: "", Flags: 0x0 { 02 87 B7 03 00 00 00 }
0x36288: 		End  { 29 02 }
0x3628A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x36291: 		End  { 29 02 }
0x36293: 		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0x2AD, VarStoreId: 0x1, VarOffset: 0x12E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 07 EA 05 AD 02 01 00 2E 01 10 10 00 01 00 }
0x362A4: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x362AB: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x362B2: 		End  { 29 02 }
0x362B4: 		SuppressIf  { 0A 82 }
0x362B6: 			EqIdVal QuestionId: 0x2AD, Value: 0x0 { 12 06 AD 02 00 00 }
0x362BC: 			Text Prompt: "Current AC Loadline", Help: "Current AC Loadline", Text: "" { 03 08 B5 05 B4 05 B7 05 }
0x362C4: 			Text Prompt: "Current DC Loadline", Help: "Current DC Loadline", Text: "" { 03 08 BA 05 B9 05 BC 05 }
0x362CC: 			Text Prompt: "Current Psi1 Threshold", Help: "Current Psi1 Threshold", Text: "" { 03 08 BF 05 BE 05 C1 05 }
0x362D4: 			Text Prompt: "Current Psi2 Threshold", Help: "Current Psi2 Threshold", Text: "" { 03 08 C4 05 C3 05 C6 05 }
0x362DC: 			Text Prompt: "Current Psi3 Threshold", Help: "Current Psi3 Threshold", Text: "" { 03 08 C9 05 C8 05 CB 05 }
0x362E4: 			Text Prompt: "Current Imon Slope", Help: "Current Imon Slope", Text: "" { 03 08 CE 05 CD 05 D0 05 }
0x362EC: 			Text Prompt: "Current Imon Offset", Help: "Current Imon Offset", Text: "" { 03 08 D3 05 D2 05 D5 05 }
0x362F4: 			Text Prompt: "Current VR Current Limit", Help: "Current VR Current Limit (Current IccMax Value)", Text: "" { 03 08 D8 05 D7 05 DA 05 }
0x362FC: 			Text Prompt: "Current Tdc Current Limit", Help: "Current Tdc Current Limit", Text: "" { 03 08 DD 05 DC 05 DF 05 }
0x36304: 			Text Prompt: "Current Voltage Limit", Help: "Current Voltage Limit", Text: "" { 03 08 E2 05 E1 05 E4 05 }
0x3630C: 			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x2AE, VarStoreId: 0x1, VarOffset: 0x134, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0 { 07 94 A5 07 EC 05 AE 02 01 00 34 01 10 11 00 00 24 F4 00 00 }
0x36320: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36327: 			End  { 29 02 }
0x36329: 			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x2AF, VarStoreId: 0x1, VarOffset: 0x13E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0 { 07 94 A6 07 EE 05 AF 02 01 00 3E 01 10 11 00 00 24 F4 00 00 }
0x3633D: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36344: 			End  { 29 02 }
0x36346: 			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2B0, VarStoreId: 0x1, VarOffset: 0x148, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 A9 07 FC 05 B0 02 01 00 48 01 10 11 00 00 00 02 01 00 }
0x3635A: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x36361: 			End  { 29 02 }
0x36363: 			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2B1, VarStoreId: 0x1, VarOffset: 0x152, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 AA 07 FE 05 B1 02 01 00 52 01 10 11 00 00 00 02 01 00 }
0x36377: 				Default DefaultId: 0x0 Value: 20 { 5B 07 00 00 01 14 00 }
0x3637E: 			End  { 29 02 }
0x36380: 			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2B2, VarStoreId: 0x1, VarOffset: 0x15C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 AB 07 00 06 B2 02 01 00 5C 01 10 11 00 00 00 02 01 00 }
0x36394: 				Default DefaultId: 0x0 Value: 4 { 5B 07 00 00 01 04 00 }
0x3639B: 			End  { 29 02 }
0x3639D: 			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2B3, VarStoreId: 0x1, VarOffset: 0x165, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 07 02 06 B3 02 01 00 65 01 10 10 00 01 00 }
0x363AE: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x363B5: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x363BC: 			End  { 29 02 }
0x363BE: 			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0x2B4, VarStoreId: 0x1, VarOffset: 0x16A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 07 04 06 B4 02 01 00 6A 01 10 10 00 01 00 }
0x363CF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x363D6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x363DD: 			End  { 29 02 }
0x363DF: 			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x2B5, VarStoreId: 0x1, VarOffset: 0x170, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xC8, Step: 0x1 { 07 94 AF 07 08 06 B5 02 01 00 70 01 10 11 00 00 C8 00 01 00 }
0x363F3: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x363FA: 			End  { 29 02 }
0x363FC: 			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x2B6, VarStoreId: 0x1, VarOffset: 0x17A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1 { 07 94 B0 07 0A 06 B6 02 01 00 7A 01 10 11 00 00 FF F9 01 00 }
0x36410: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36417: 			End  { 29 02 }
0x36419: 			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2B7, VarStoreId: 0x1, VarOffset: 0x183, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 07 0C 06 B7 02 01 00 83 01 10 10 00 01 00 }
0x3642A: 				OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x36431: 				OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x36438: 			End  { 29 02 }
0x3643A: 			GrayOutIf  { 19 82 }
0x3643C: 				EqIdVal QuestionId: 0x2881, Value: 0x1 { 12 06 81 28 01 00 }
0x36442: 				Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (IccMax). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x2B8, VarStoreId: 0x1, VarOffset: 0x189, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x800, Step: 0x1 { 07 94 A7 07 F0 05 B8 02 01 00 89 01 10 11 00 00 00 08 01 00 }
0x36456: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3645D: 				End  { 29 02 }
0x3645F: 			End  { 29 02 }
0x36461: 			SuppressIf  { 0A 82 }
0x36463: 				EqIdVal QuestionId: 0x120C, Value: 0x0 { 12 06 0C 12 00 00 }
0x36469: 				OneOf Prompt: "GT VR Fast Vmode", Help: "GT VR Fast Vmode. Use to control GT Fast Vmode Enable/Disable.", QuestionFlags: 0x14, QuestionId: 0x2755, VarStoreId: 0x1, VarOffset: 0x37A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F3 05 F4 05 55 27 01 00 7A 03 14 10 00 01 00 }
0x3647A: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x36481: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36488: 				End  { 29 02 }
0x3648A: 				SuppressIf  { 0A 82 }
0x3648C: 					EqIdVal QuestionId: 0x2755, Value: 0x0 { 12 06 55 27 00 00 }
0x36492: 					Numeric Prompt: "  Fast Vmode Itrip ICC Limit", Help: "Voltage Regulator Fast Vmode Itrip ICC Limit. A value of 400 = 100A. A value of 0 corresponds to feature disabled (no reactive protection). This value represents the current threshold where the VR would initiate reactive protection if Fast Vmode is enabled. The value is represented in 1/4 A increments. Uses BIOS VR mailbox command 0x25.", QuestionFlags: 0x14, QuestionId: 0x2756, VarStoreId: 0x1, VarOffset: 0x32C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F8, Step: 0x1 { 07 94 A8 07 F8 05 56 27 01 00 2C 03 14 11 00 00 F8 07 01 00 }
0x364A6: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x364AD: 					End  { 29 02 }
0x364AF: 				End  { 29 02 }
0x364B1: 			End  { 29 02 }
0x364B3: 			Numeric Prompt: "VR Voltage Limit", Help: "Voltage Limit (VMAX). This value represents the Maximum instantaneous voltage allowed at any given time. Range is 0 - 7999mV. Uses BIOS VR mailbox command 0x8.", QuestionFlags: 0x10, QuestionId: 0x2B9, VarStoreId: 0x1, VarOffset: 0x1C0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1 { 07 94 AE 07 06 06 B9 02 01 00 C0 01 10 11 00 00 3F 1F 01 00 }
0x364C7: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x364CE: 			End  { 29 02 }
0x364D0: 			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x2BA, VarStoreId: 0x1, VarOffset: 0x19C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 07 44 06 BA 02 01 00 9C 01 10 10 00 01 00 }
0x364E1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x364E8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x364EF: 			End  { 29 02 }
0x364F1: 			SuppressIf  { 0A 82 }
0x364F3: 				EqIdVal QuestionId: 0x2BA, Value: 0x0 { 12 06 BA 02 00 00 }
0x364F9: 				Numeric Prompt: "TDC Current Limit", Help: "TDC Current Limit, defined in 1/8A increments. Range 0-32767. For a TDC Current Limit of 125A, enter 1000. 0 = 0 Amps. Uses BIOS VR mailbox command 0x1A.", QuestionFlags: 0x10, QuestionId: 0x2BB, VarStoreId: 0x1, VarOffset: 0x193, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FFF, Step: 0x7D { 07 94 B5 07 46 06 BB 02 01 00 93 01 10 11 00 00 FF 7F 7D 00 }
0x3650D: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36514: 				End  { 29 02 }
0x36516: 				OneOf Prompt: "TDC Time Window", Help: "VR TDC Time Window, value in seconds. 1s is default. Range from 1s to 448s.", QuestionFlags: 0x10, QuestionId: 0x2BC, VarStoreId: 0x1, VarOffset: 0x1A4, Flags: 0x12, Size: 32, Min: 0x3E8, Max: 0x6D600, Step: 0x0 { 05 9A B6 07 48 06 BC 02 01 00 A4 01 10 12 E8 03 00 00 00 D6 06 00 00 00 00 00 }
0x36530: 					OneOfOption Option: "1 sec" Value: 1000, Default, MfgDefault { 09 0A 58 06 32 02 E8 03 00 00 }
0x3653A: 					OneOfOption Option: "2 sec" Value: 2000 { 09 0A 59 06 02 02 D0 07 00 00 }
0x36544: 					OneOfOption Option: "3 sec" Value: 3000 { 09 0A 5A 06 02 02 B8 0B 00 00 }
0x3654E: 					OneOfOption Option: "4 sec" Value: 4000 { 09 0A 5B 06 02 02 A0 0F 00 00 }
0x36558: 					OneOfOption Option: "5 sec" Value: 5000 { 09 0A 5C 06 02 02 88 13 00 00 }
0x36562: 					OneOfOption Option: "6 sec" Value: 6000 { 09 0A 5D 06 02 02 70 17 00 00 }
0x3656C: 					OneOfOption Option: "7 sec" Value: 7000 { 09 0A 5E 06 02 02 58 1B 00 00 }
0x36576: 					OneOfOption Option: "8 sec" Value: 8000 { 09 0A 5F 06 02 02 40 1F 00 00 }
0x36580: 					OneOfOption Option: "10 sec" Value: 10000 { 09 0A 60 06 02 02 10 27 00 00 }
0x3658A: 					OneOfOption Option: "12 sec" Value: 12000 { 09 0A 61 06 02 02 E0 2E 00 00 }
0x36594: 					OneOfOption Option: "14 sec" Value: 14000 { 09 0A 62 06 02 02 B0 36 00 00 }
0x3659E: 					OneOfOption Option: "16 sec" Value: 16000 { 09 0A 63 06 02 02 80 3E 00 00 }
0x365A8: 					OneOfOption Option: "20 sec" Value: 20000 { 09 0A 64 06 02 02 20 4E 00 00 }
0x365B2: 					OneOfOption Option: "24 sec" Value: 24000 { 09 0A 65 06 02 02 C0 5D 00 00 }
0x365BC: 					OneOfOption Option: "28 sec" Value: 28000 { 09 0A 66 06 02 02 60 6D 00 00 }
0x365C6: 					OneOfOption Option: "32 sec" Value: 32000 { 09 0A 67 06 02 02 00 7D 00 00 }
0x365D0: 					OneOfOption Option: "40 sec" Value: 40000 { 09 0A 68 06 02 02 40 9C 00 00 }
0x365DA: 					OneOfOption Option: "48 sec" Value: 48000 { 09 0A 69 06 02 02 80 BB 00 00 }
0x365E4: 					OneOfOption Option: "56 sec" Value: 56000 { 09 0A 6A 06 02 02 C0 DA 00 00 }
0x365EE: 					OneOfOption Option: "64 sec" Value: 64000 { 09 0A 6B 06 02 02 00 FA 00 00 }
0x365F8: 					OneOfOption Option: "80 sec" Value: 80000 { 09 0A 6C 06 02 02 80 38 01 00 }
0x36602: 					OneOfOption Option: "96 sec" Value: 96000 { 09 0A 6D 06 02 02 00 77 01 00 }
0x3660C: 					OneOfOption Option: "112 sec" Value: 112000 { 09 0A 6E 06 02 02 80 B5 01 00 }
0x36616: 					OneOfOption Option: "128 sec" Value: 128000 { 09 0A 6F 06 02 02 00 F4 01 00 }
0x36620: 					OneOfOption Option: "160 sec" Value: 160000 { 09 0A 70 06 02 02 00 71 02 00 }
0x3662A: 					OneOfOption Option: "192 sec" Value: 192000 { 09 0A 71 06 02 02 00 EE 02 00 }
0x36634: 					OneOfOption Option: "224 sec" Value: 224000 { 09 0A 72 06 02 02 00 6B 03 00 }
0x3663E: 					OneOfOption Option: "256 sec" Value: 256000 { 09 0A 73 06 02 02 00 E8 03 00 }
0x36648: 					OneOfOption Option: "320 sec" Value: 320000 { 09 0A 74 06 02 02 00 E2 04 00 }
0x36652: 					OneOfOption Option: "384 sec" Value: 384000 { 09 0A 75 06 02 02 00 DC 05 00 }
0x3665C: 					OneOfOption Option: "448 sec" Value: 448000 { 09 0A 76 06 02 02 00 D6 06 00 }
0x36666: 				End  { 29 02 }
0x36668: 				OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x2BD, VarStoreId: 0x1, VarOffset: 0x1B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 07 78 06 BD 02 01 00 B5 01 10 10 00 01 00 }
0x36679: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x36680: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36687: 				End  { 29 02 }
0x36689: 			End  { 29 02 }
0x3668B: 		End  { 29 02 }
0x3668D: 	End  { 29 02 }
0x3668F: 	Form FormId: 0x276A, Title: "SA VR Settings" { 01 86 6A 27 B8 03 }
0x36695: 		Subtitle Prompt: "SA Domain", Help: "", Flags: 0x0 { 02 87 B9 03 00 00 00 }
0x3669C: 		End  { 29 02 }
0x3669E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x366A5: 		End  { 29 02 }
0x366A7: 		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0x2BE, VarStoreId: 0x1, VarOffset: 0x12F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 07 EA 05 BE 02 01 00 2F 01 10 10 00 01 00 }
0x366B8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x366BF: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x366C6: 		End  { 29 02 }
0x366C8: 		SuppressIf  { 0A 82 }
0x366CA: 			EqIdVal QuestionId: 0x2BE, Value: 0x0 { 12 06 BE 02 00 00 }
0x366D0: 			Text Prompt: "Current AC Loadline", Help: "Current AC Loadline", Text: "" { 03 08 B5 05 B4 05 B8 05 }
0x366D8: 			Text Prompt: "Current DC Loadline", Help: "Current DC Loadline", Text: "" { 03 08 BA 05 B9 05 BD 05 }
0x366E0: 			Text Prompt: "Current Psi1 Threshold", Help: "Current Psi1 Threshold", Text: "" { 03 08 BF 05 BE 05 C2 05 }
0x366E8: 			Text Prompt: "Current Psi2 Threshold", Help: "Current Psi2 Threshold", Text: "" { 03 08 C4 05 C3 05 C7 05 }
0x366F0: 			Text Prompt: "Current Psi3 Threshold", Help: "Current Psi3 Threshold", Text: "" { 03 08 C9 05 C8 05 CC 05 }
0x366F8: 			Text Prompt: "Current Imon Slope", Help: "Current Imon Slope", Text: "" { 03 08 CE 05 CD 05 D1 05 }
0x36700: 			Text Prompt: "Current Imon Offset", Help: "Current Imon Offset", Text: "" { 03 08 D3 05 D2 05 D6 05 }
0x36708: 			Text Prompt: "Current VR Current Limit", Help: "Current VR Current Limit (Current IccMax Value)", Text: "" { 03 08 D8 05 D7 05 DB 05 }
0x36710: 			Text Prompt: "Current Voltage Limit", Help: "Current Voltage Limit", Text: "" { 03 08 E2 05 E1 05 E5 05 }
0x36718: 			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x2BF, VarStoreId: 0x1, VarOffset: 0x136, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0 { 07 94 B9 07 EC 05 BF 02 01 00 36 01 10 11 00 00 24 F4 00 00 }
0x3672C: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36733: 			End  { 29 02 }
0x36735: 			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x2C0, VarStoreId: 0x1, VarOffset: 0x140, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0 { 07 94 BA 07 EE 05 C0 02 01 00 40 01 10 11 00 00 24 F4 00 00 }
0x36749: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36750: 			End  { 29 02 }
0x36752: 			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2C1, VarStoreId: 0x1, VarOffset: 0x14A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 BB 07 FC 05 C1 02 01 00 4A 01 10 11 00 00 00 02 01 00 }
0x36766: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x3676D: 			End  { 29 02 }
0x3676F: 			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2C2, VarStoreId: 0x1, VarOffset: 0x154, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 BC 07 FE 05 C2 02 01 00 54 01 10 11 00 00 00 02 01 00 }
0x36783: 				Default DefaultId: 0x0 Value: 20 { 5B 07 00 00 01 14 00 }
0x3678A: 			End  { 29 02 }
0x3678C: 			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2C3, VarStoreId: 0x1, VarOffset: 0x15E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1 { 07 94 BD 07 00 06 C3 02 01 00 5E 01 10 11 00 00 00 02 01 00 }
0x367A0: 				Default DefaultId: 0x0 Value: 4 { 5B 07 00 00 01 04 00 }
0x367A7: 			End  { 29 02 }
0x367A9: 			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x2C4, VarStoreId: 0x1, VarOffset: 0x166, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 07 02 06 C4 02 01 00 66 01 10 10 00 01 00 }
0x367BA: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x367C1: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x367C8: 			End  { 29 02 }
0x367CA: 			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0x2C5, VarStoreId: 0x1, VarOffset: 0x16B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 07 04 06 C5 02 01 00 6B 01 10 10 00 01 00 }
0x367DB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x367E2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x367E9: 			End  { 29 02 }
0x367EB: 			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x2C6, VarStoreId: 0x1, VarOffset: 0x172, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xC8, Step: 0x1 { 07 94 C0 07 08 06 C6 02 01 00 72 01 10 11 00 00 C8 00 01 00 }
0x367FF: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36806: 			End  { 29 02 }
0x36808: 			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x2C7, VarStoreId: 0x1, VarOffset: 0x17C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1 { 07 94 C1 07 0A 06 C7 02 01 00 7C 01 10 11 00 00 FF F9 01 00 }
0x3681C: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36823: 			End  { 29 02 }
0x36825: 			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2C8, VarStoreId: 0x1, VarOffset: 0x184, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 07 0C 06 C8 02 01 00 84 01 10 10 00 01 00 }
0x36836: 				OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3683D: 				OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x36844: 			End  { 29 02 }
0x36846: 			Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (IccMax). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x2C9, VarStoreId: 0x1, VarOffset: 0x18B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x800, Step: 0x1 { 07 94 C3 07 F0 05 C9 02 01 00 8B 01 10 11 00 00 00 08 01 00 }
0x3685A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x36861: 			End  { 29 02 }
0x36863: 			SuppressIf  { 0A 82 }
0x36865: 				EqIdVal QuestionId: 0x120C, Value: 0x0 { 12 06 0C 12 00 00 }
0x3686B: 				OneOf Prompt: "SA VR Fast Vmode", Help: "SA VR Fast Vmode. Use to control SA Fast Vmode Enable/Disable.", QuestionFlags: 0x14, QuestionId: 0x2757, VarStoreId: 0x1, VarOffset: 0x37B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 05 F6 05 57 27 01 00 7B 03 14 10 00 01 00 }
0x3687C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x36883: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3688A: 				End  { 29 02 }
0x3688C: 				SuppressIf  { 0A 82 }
0x3688E: 					EqIdVal QuestionId: 0x2757, Value: 0x0 { 12 06 57 27 00 00 }
0x36894: 					Numeric Prompt: "  Fast Vmode Itrip ICC Limit", Help: "Voltage Regulator Fast Vmode Itrip ICC Limit. A value of 400 = 100A. A value of 0 corresponds to feature disabled (no reactive protection). This value represents the current threshold where the VR would initiate reactive protection if Fast Vmode is enabled. The value is represented in 1/4 A increments. Uses BIOS VR mailbox command 0x25.", QuestionFlags: 0x14, QuestionId: 0x2758, VarStoreId: 0x1, VarOffset: 0x32E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F8, Step: 0x1 { 07 94 C4 07 F8 05 58 27 01 00 2E 03 14 11 00 00 F8 07 01 00 }
0x368A8: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x368AF: 					End  { 29 02 }
0x368B1: 				End  { 29 02 }
0x368B3: 			End  { 29 02 }
0x368B5: 			Numeric Prompt: "VR Voltage Limit", Help: "Voltage Limit (VMAX). This value represents the Maximum instantaneous voltage allowed at any given time. Range is 0 - 7999mV. Uses BIOS VR mailbox command 0x8.", QuestionFlags: 0x10, QuestionId: 0x2CA, VarStoreId: 0x1, VarOffset: 0x1C2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1 { 07 94 C5 07 06 06 CA 02 01 00 C2 01 10 11 00 00 3F 1F 01 00 }
0x368C9: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x368D0: 			End  { 29 02 }
0x368D2: 			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x2CB, VarStoreId: 0x1, VarOffset: 0x19D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 07 44 06 CB 02 01 00 9D 01 10 10 00 01 00 }
0x368E3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x368EA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x368F1: 			End  { 29 02 }
0x368F3: 			SuppressIf  { 0A 82 }
0x368F5: 				EqIdVal QuestionId: 0x2CB, Value: 0x0 { 12 06 CB 02 00 00 }
0x368FB: 				OneOf Prompt: "TDC Time Window", Help: "TDC Time Window 1, value in milliseconds. 1ms is default. Range from 1ms to 10ms, except for 9ms. 9ms has no valid encoding in the MSR definition.", QuestionFlags: 0x10, QuestionId: 0x2CC, VarStoreId: 0x1, VarOffset: 0x1A8, Flags: 0x12, Size: 32, Min: 0x1, Max: 0xA, Step: 0x0 { 05 9A C7 07 49 06 CC 02 01 00 A8 01 10 12 01 00 00 00 0A 00 00 00 00 00 00 00 }
0x36915: 					OneOfOption Option: "1 ms" Value: 1, Default, MfgDefault { 09 0A 4A 06 32 02 01 00 00 00 }
0x3691F: 					OneOfOption Option: "2 ms" Value: 2 { 09 0A 4B 06 02 02 02 00 00 00 }
0x36929: 					OneOfOption Option: "3 ms" Value: 3 { 09 0A 4C 06 02 02 03 00 00 00 }
0x36933: 					OneOfOption Option: "4 ms" Value: 4 { 09 0A 4D 06 02 02 04 00 00 00 }
0x3693D: 					OneOfOption Option: "5 ms" Value: 5 { 09 0A 4E 06 02 02 05 00 00 00 }
0x36947: 					OneOfOption Option: "6 ms" Value: 6 { 09 0A 4F 06 02 02 06 00 00 00 }
0x36951: 					OneOfOption Option: "7 ms" Value: 7 { 09 0A 50 06 02 02 07 00 00 00 }
0x3695B: 					OneOfOption Option: "8 ms" Value: 8 { 09 0A 51 06 02 02 08 00 00 00 }
0x36965: 					OneOfOption Option: "10 ms" Value: 10 { 09 0A 52 06 02 02 0A 00 00 00 }
0x3696F: 				End  { 29 02 }
0x36971: 				OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x2CD, VarStoreId: 0x1, VarOffset: 0x1B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 07 78 06 CD 02 01 00 B6 01 10 10 00 01 00 }
0x36982: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x36989: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36990: 				End  { 29 02 }
0x36992: 			End  { 29 02 }
0x36994: 		End  { 29 02 }
0x36996: 	End  { 29 02 }
0x36998: 	Form FormId: 0x276B, Title: "RFI Settings" { 01 86 6B 27 BA 03 }
0x3699E: 		Subtitle Prompt: "RFI Domain", Help: "", Flags: 0x0 { 02 87 BB 03 00 00 00 }
0x369A5: 		End  { 29 02 }
0x369A7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x369AE: 		End  { 29 02 }
0x369B0: 		SuppressIf  { 0A 82 }
0x369B2: 			EqIdVal QuestionId: 0x120B, Value: 0x0 { 12 06 0B 12 00 00 }
0x369B8: 			Text Prompt: "RFI Current Frequency", Help: "RFI Current Frequency", Text: "" { 03 08 CC 03 CB 03 BC 03 }
0x369C0: 			Numeric Prompt: "RFI Frequency", Help: "Set desired RFI frequency, in increments of 100KHz. (For a frequency of 100.6MHz, enter 1006.)", QuestionFlags: 0x10, QuestionId: 0x2CE, VarStoreId: 0x1, VarOffset: 0x1F9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x77E, Step: 0x0 { 07 94 CD 03 CE 03 CE 02 01 00 F9 01 10 11 00 00 7E 07 00 00 }
0x369D4: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x369DB: 			End  { 29 02 }
0x369DD: 			OneOf Prompt: "FIVR Spread Spectrum", Help: "Enable or Disable the FIVR Spread Spectrum", QuestionFlags: 0x10, QuestionId: 0x2CF, VarStoreId: 0x1, VarOffset: 0x2F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 03 C0 03 CF 02 01 00 F6 02 10 10 00 01 00 }
0x369EE: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x369F5: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x369FC: 			End  { 29 02 }
0x369FE: 			SuppressIf  { 0A 82 }
0x36A00: 				EqIdVal QuestionId: 0x2CF, Value: 0x0 { 12 06 CF 02 00 00 }
0x36A06: 				OneOf Prompt: "RFI Spread Spectrum", Help: "Set the Spread Spectrum", QuestionFlags: 0x10, QuestionId: 0x2D0, VarStoreId: 0x1, VarOffset: 0x1FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2C, Step: 0x0 { 05 91 C1 03 C2 03 D0 02 01 00 FB 01 10 10 00 2C 00 }
0x36A17: 					OneOfOption Option: "0.5%" Value: 0 { 09 07 C3 03 00 00 00 }
0x36A1E: 					OneOfOption Option: "1%" Value: 3 { 09 07 C4 03 00 00 03 }
0x36A25: 					OneOfOption Option: "1.5%" Value: 8, Default, MfgDefault { 09 07 C5 03 30 00 08 }
0x36A2C: 					OneOfOption Option: "2%" Value: 18 { 09 07 C6 03 00 00 12 }
0x36A33: 					OneOfOption Option: "3%" Value: 28 { 09 07 C7 03 00 00 1C }
0x36A3A: 					OneOfOption Option: "4%" Value: 34 { 09 07 C8 03 00 00 22 }
0x36A41: 					OneOfOption Option: "5%" Value: 39 { 09 07 C9 03 00 00 27 }
0x36A48: 					OneOfOption Option: "6%" Value: 44 { 09 07 CA 03 00 00 2C }
0x36A4F: 				End  { 29 02 }
0x36A51: 			End  { 29 02 }
0x36A53: 		End  { 29 02 }
0x36A55: 	End  { 29 02 }
0x36A57: 	Form FormId: 0x276C, Title: "Power Limit 3 Settings" { 01 86 6C 27 51 05 }
0x36A5D: 		OneOf Prompt: "Power Limit 3 Override ", Help: "Enable/DisablePower Limit 3 override. If this option is disabled, BIOS will leave the hardware default values for Power Limit 3 and Power Limit 3 Time Window.", QuestionFlags: 0x10, QuestionId: 0x2D1, VarStoreId: 0x1, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 53 05 54 05 D1 02 01 00 22 00 10 10 00 01 00 }
0x36A6E: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36A74: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x36A7B: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36A82: 		End  { 29 02 }
0x36A84: 		SuppressIf  { 0A 82 }
0x36A86: 			EqIdVal QuestionId: 0x2D1, Value: 0x0 { 12 06 D1 02 00 00 }
0x36A8C: 			Numeric Prompt: "Power Limit 3", Help: "Platform Power Limit 3 Power in Milli Watts / Milli Percent. BIOS will round to the nearest 1/8W or 1/8% when programming. For example if 12%, enter 12000, if 50%, enter 50000.  For all SKUs, limit must be less than Psys Pmax value (either in Watts or %). XE SKU: Any value up through Psys Pmax can be programmed. Overclocking SKU: value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and Processor Base Power (TDP). If the value is '0', will default to hardware default value. Recommended value is 100000 if Psys is in %.", QuestionFlags: 0x10, QuestionId: 0x2D2, VarStoreId: 0x1, VarOffset: 0x23, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 55 05 56 05 D2 02 01 00 23 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36AA6: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36AAF: 			End  { 29 02 }
0x36AB1: 		End  { 29 02 }
0x36AB3: 		SuppressIf  { 0A 82 }
0x36AB5: 			EqIdVal QuestionId: 0x2D1, Value: 0x0 { 12 06 D1 02 00 00 }
0x36ABB: 			OneOf Prompt: "Power Limit 3 Time Window", Help: "Power Limit 3 Time Window value in Milli seconds. The value may vary from 3 to 64(max). Indicates the time window over which Power Limit 3 value should be maintained. If the value is 0, BIOS leaves the hardware default value. For ATX12VO PSU systems, recommended value is 40.", QuestionFlags: 0x10, QuestionId: 0x2D3, VarStoreId: 0x1, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x0 { 05 91 57 05 58 05 D3 02 01 00 27 00 10 10 00 40 00 }
0x36ACC: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36AD2: 				OneOfOption Option: "0" Value: 0 { 09 07 A5 04 00 00 00 }
0x36AD9: 				OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x36AE0: 				OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x36AE7: 				OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x36AEE: 				OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x36AF5: 				OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x36AFC: 				OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x36B03: 				OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x36B0A: 				OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x36B11: 				OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x36B18: 				OneOfOption Option: "16" Value: 16 { 09 07 B5 04 00 00 10 }
0x36B1F: 				OneOfOption Option: "20" Value: 20 { 09 07 FE 1D 00 00 14 }
0x36B26: 				OneOfOption Option: "24" Value: 24 { 09 07 FF 1D 00 00 18 }
0x36B2D: 				OneOfOption Option: "28" Value: 28 { 09 07 00 1E 00 00 1C }
0x36B34: 				OneOfOption Option: "32" Value: 32 { 09 07 01 1E 00 00 20 }
0x36B3B: 				OneOfOption Option: "40" Value: 40 { 09 07 02 1E 00 00 28 }
0x36B42: 				OneOfOption Option: "48" Value: 48 { 09 07 03 1E 00 00 30 }
0x36B49: 				OneOfOption Option: "56" Value: 56 { 09 07 04 1E 00 00 38 }
0x36B50: 				OneOfOption Option: "64" Value: 64 { 09 07 05 1E 00 00 40 }
0x36B57: 			End  { 29 02 }
0x36B59: 		End  { 29 02 }
0x36B5B: 		SuppressIf  { 0A 82 }
0x36B5D: 			EqIdVal QuestionId: 0x2D1, Value: 0x0 { 12 06 D1 02 00 00 }
0x36B63: 			Numeric Prompt: "Power Limit 3 Duty Cycle", Help: "Specify the duty cycle in percentage that the CPU is required to maintain over the configured time window. Range is 0-100. For ATX12VO PSU systems, recommended value is 25.", QuestionFlags: 0x10, QuestionId: 0x2D4, VarStoreId: 0x1, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x0 { 07 91 5F 05 60 05 D4 02 01 00 28 00 10 10 00 64 00 }
0x36B74: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36B7A: 			End  { 29 02 }
0x36B7C: 		End  { 29 02 }
0x36B7E: 		SuppressIf  { 0A 82 }
0x36B80: 			EqIdVal QuestionId: 0x2D1, Value: 0x0 { 12 86 D1 02 00 00 }
0x36B86: 				EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x36B8C: 				Or  { 16 02 }
0x36B8E: 			End  { 29 02 }
0x36B90: 			OneOf Prompt: "Response Mode", Help: "Use Response Mode to adjust Psys_PL3 power reduction behavior. Battery-enabled systems use Gradual power reduction.", QuestionFlags: 0x10, QuestionId: 0x2D5, VarStoreId: 0x1, VarOffset: 0x383, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5B 05 5C 05 D5 02 01 00 83 03 10 10 00 01 00 }
0x36BA1: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36BA7: 				OneOfOption Option: "Gradual power reduction" Value: 0, Default, MfgDefault { 09 07 59 05 30 00 00 }
0x36BAE: 				OneOfOption Option: "Aggressive power reduction" Value: 1 { 09 07 5A 05 00 00 01 }
0x36BB5: 			End  { 29 02 }
0x36BB7: 		End  { 29 02 }
0x36BB9: 		SuppressIf  { 0A 82 }
0x36BBB: 			EqIdVal QuestionId: 0x2D1, Value: 0x0 { 12 06 D1 02 00 00 }
0x36BC1: 			OneOf Prompt: "Power Limit 3 Lock", Help: "Power Limit 3 MSR 615h Lock. When enabled PL3 configurations are locked during OS. When disabled PL3 configuration can be changed during OS.", QuestionFlags: 0x10, QuestionId: 0x2D6, VarStoreId: 0x1, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5D 05 5E 05 D6 02 01 00 29 00 10 10 00 01 00 }
0x36BD2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36BD8: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x36BDF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36BE6: 			End  { 29 02 }
0x36BE8: 		End  { 29 02 }
0x36BEA: 	End  { 29 02 }
0x36BEC: 	Form FormId: 0x276D, Title: "  Config TDP Configurations" { 01 86 6D 27 EF 04 }
0x36BF2: 		Subtitle Prompt: "Config TDP Configurations", Help: "", Flags: 0x0 { 02 87 F0 04 00 00 00 }
0x36BF9: 		End  { 29 02 }
0x36BFB: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x36C02: 		End  { 29 02 }
0x36C04: 		OneOf Prompt: "Enable Configurable TDP", Help: "Applies Configurable Processor Base Power (cTDP) initialization settings based on non-cTDP or cTDP. Default is 1: Applies to cTDP; if 0 then applies non-cTDP and BIOS will bypass cTDP initialzation flow", QuestionFlags: 0x10, QuestionId: 0x2D7, VarStoreId: 0x1, VarOffset: 0x227, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D5 04 D6 04 D7 02 01 00 27 02 10 10 00 01 00 }
0x36C15: 			OneOfOption Option: "Applies to non-cTDP" Value: 0 { 09 07 D7 04 00 00 00 }
0x36C1C: 			OneOfOption Option: "Applies to cTDP" Value: 1, Default, MfgDefault { 09 07 D8 04 30 00 01 }
0x36C23: 		End  { 29 02 }
0x36C25: 		OneOf Prompt: "Configurable TDP Boot Mode", Help: "Configurable Processor Base Power (cTDP) Mode as Nominal/Level/Leve2/Deactivate TDP selection. Deactivate option will set MSR to Nominal and MMIO to Zero.", QuestionFlags: 0x10, QuestionId: 0x2D8, VarStoreId: 0x1, VarOffset: 0x44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 D9 04 DA 04 D8 02 01 00 44 00 10 10 00 FF 00 }
0x36C36: 			OneOfOption Option: "Nominal" Value: 0, Default, MfgDefault { 09 07 DB 04 30 00 00 }
0x36C3D: 			SuppressIf  { 0A 82 }
0x36C3F: 				EqIdVal QuestionId: 0x120A, Value: 0x0 { 12 06 0A 12 00 00 }
0x36C45: 				OneOfOption Option: "Level1" Value: 1 { 09 07 DC 04 00 00 01 }
0x36C4C: 			End  { 29 02 }
0x36C4E: 			SuppressIf  { 0A 82 }
0x36C50: 				EqIdVal QuestionId: 0x1209, Value: 0x0 { 12 06 09 12 00 00 }
0x36C56: 				OneOfOption Option: "Level2" Value: 2 { 09 07 DD 04 00 00 02 }
0x36C5D: 			End  { 29 02 }
0x36C5F: 			OneOfOption Option: "Deactivate" Value: 255 { 09 07 DE 04 00 00 FF }
0x36C66: 		End  { 29 02 }
0x36C68: 		OneOf Prompt: "Configurable TDP Lock", Help: "Configurable Processor Base Power (cTDP) Mode Lock sets the Lock bits on TURBO_ACTIVATION_RATIO and CONFIG_TDP_CONTROL.                 Note: When CTDP Lock is enabled Custom ConfigTDP Count will be forced to 1 and Custom ConfigTDP Boot Index will be forced to 0.", QuestionFlags: 0x10, QuestionId: 0x2D9, VarStoreId: 0x1, VarOffset: 0x45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 04 E0 04 D9 02 01 00 45 00 10 10 00 01 00 }
0x36C79: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36C80: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x36C87: 		End  { 29 02 }
0x36C89: 		SuppressIf  { 0A 82 }
0x36C8B: 			EqIdVal QuestionId: 0x2D9, Value: 0x1 { 12 86 D9 02 01 00 }
0x36C91: 				EqIdVal QuestionId: 0x337, Value: 0x1 { 12 06 37 03 01 00 }
0x36C97: 				Or  { 16 02 }
0x36C99: 			End  { 29 02 }
0x36C9B: 			OneOf Prompt: "CTDP BIOS control", Help: "Enables Configurable Processor Base Power (cTDP) control via runtime ACPI BIOS methods. This "BIOS only" feature does not require EC or driver support.", QuestionFlags: 0x10, QuestionId: 0x2DA, VarStoreId: 0x1, VarOffset: 0x46, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 04 E2 04 DA 02 01 00 46 00 10 10 00 01 00 }
0x36CAC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x36CB3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x36CBA: 			End  { 29 02 }
0x36CBC: 		End  { 29 02 }
0x36CBE: 		Text Prompt: "ConfigTDP Levels", Help: "Configurable Processor Base Power (cTDP) Levels Supported from MSR", Text: "" { 03 08 E4 04 E3 04 E5 04 }
0x36CC6: 		Text Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Configurable Processor Base Power (cTDP) Turbo Activation Ratio values from MSR", Text: "N/A" { 03 08 F3 04 F2 04 F4 04 }
0x36CCE: 		Text Prompt: "Power Limit 1", Help: "Power Limit 1 values from MMIO", Text: "N/A" { 03 08 F6 04 F5 04 F7 04 }
0x36CD6: 		Text Prompt: "Power Limit 2", Help: "Power Limit 2 values from MMIO", Text: "N/A" { 03 08 F9 04 F8 04 FA 04 }
0x36CDE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x36CE5: 		End  { 29 02 }
0x36CE7: 		Subtitle Prompt: "Custom Settings Nominal", Help: "", Flags: 0x0 { 02 87 FB 04 00 00 00 }
0x36CEE: 		End  { 29 02 }
0x36CF0: 		Text Prompt: "ConfigTDP Nominal", Help: "Configurable Processor Base Power (cTDP) Nominal Ratio and Processor Base Power (TDP) from MSR", Text: "N/A" { 03 08 E7 04 E6 04 E8 04 }
0x36CF8: 		GrayOutIf  { 19 82 }
0x36CFA: 			EqIdVal QuestionId: 0x2D9, Value: 0x1 { 12 06 D9 02 01 00 }
0x36D00: 			Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and Processor Base Power (TDP) Limit.", QuestionFlags: 0x10, QuestionId: 0x2DB, VarStoreId: 0x1, VarOffset: 0x5B, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 41 05 AB 05 DB 02 01 00 5B 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36D1A: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36D23: 			End  { 29 02 }
0x36D25: 			Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x2DC, VarStoreId: 0x1, VarOffset: 0x5F, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 4D 05 AE 05 DC 02 01 00 5F 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36D3F: 				Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36D48: 			End  { 29 02 }
0x36D4A: 			OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which Processor Base Power (TDP) value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x2DD, VarStoreId: 0x1, VarOffset: 0x63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0 { 05 91 46 05 49 05 DD 02 01 00 63 00 10 10 00 80 00 }
0x36D5B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36D61: 				OneOfOption Option: "0" Value: 0 { 09 07 A5 04 00 00 00 }
0x36D68: 				OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x36D6F: 				OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x36D76: 				OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x36D7D: 				OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x36D84: 				OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x36D8B: 				OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x36D92: 				OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x36D99: 				OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x36DA0: 				OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x36DA7: 				OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x36DAE: 				OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x36DB5: 				OneOfOption Option: "16" Value: 16 { 09 07 B5 04 00 00 10 }
0x36DBC: 				OneOfOption Option: "20" Value: 20 { 09 07 FE 1D 00 00 14 }
0x36DC3: 				OneOfOption Option: "24" Value: 24 { 09 07 FF 1D 00 00 18 }
0x36DCA: 				OneOfOption Option: "28" Value: 28 { 09 07 00 1E 00 00 1C }
0x36DD1: 				OneOfOption Option: "32" Value: 32 { 09 07 01 1E 00 00 20 }
0x36DD8: 				OneOfOption Option: "40" Value: 40 { 09 07 02 1E 00 00 28 }
0x36DDF: 				OneOfOption Option: "48" Value: 48 { 09 07 03 1E 00 00 30 }
0x36DE6: 				OneOfOption Option: "56" Value: 56 { 09 07 04 1E 00 00 38 }
0x36DED: 				OneOfOption Option: "64" Value: 64 { 09 07 05 1E 00 00 40 }
0x36DF4: 				OneOfOption Option: "80" Value: 80 { 09 07 06 1E 00 00 50 }
0x36DFB: 				OneOfOption Option: "96" Value: 96 { 09 07 07 1E 00 00 60 }
0x36E02: 				OneOfOption Option: "112" Value: 112 { 09 07 08 1E 00 00 70 }
0x36E09: 				OneOfOption Option: "128" Value: 128 { 09 07 09 1E 00 00 80 }
0x36E10: 			End  { 29 02 }
0x36E12: 			Numeric Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Custom value for Turbo Activation Ratio. Needs to be configured with valid values from LFM to Max Turbo. 0 means don't use custom value.", QuestionFlags: 0x10, QuestionId: 0x2DE, VarStoreId: 0x1, VarOffset: 0x64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FE 04 01 05 DE 02 01 00 64 00 10 10 00 FF 01 }
0x36E23: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36E29: 			End  { 29 02 }
0x36E2B: 		End  { 29 02 }
0x36E2D: 		SuppressIf  { 0A 82 }
0x36E2F: 			EqIdVal QuestionId: 0x120A, Value: 0x0 { 12 06 0A 12 00 00 }
0x36E35: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x36E3C: 			End  { 29 02 }
0x36E3E: 			Subtitle Prompt: "Custom Settings Level1", Help: "", Flags: 0x0 { 02 87 FC 04 00 00 00 }
0x36E45: 			End  { 29 02 }
0x36E47: 			Text Prompt: "ConfigTDP Level1", Help: "Configurable Processor Base Power (cTDP) Level1 Ratio and Processor Base Power (TDP) from MSR", Text: "N/A" { 03 08 EA 04 E9 04 EB 04 }
0x36E4F: 			GrayOutIf  { 19 82 }
0x36E51: 				EqIdVal QuestionId: 0x2D9, Value: 0x1 { 12 06 D9 02 01 00 }
0x36E57: 				Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and Processor Base Power (TDP) Limit.", QuestionFlags: 0x10, QuestionId: 0x2DF, VarStoreId: 0x1, VarOffset: 0x65, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 42 05 AB 05 DF 02 01 00 65 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36E71: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36E7A: 				End  { 29 02 }
0x36E7C: 				Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x2E0, VarStoreId: 0x1, VarOffset: 0x69, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 4E 05 AE 05 E0 02 01 00 69 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36E96: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36E9F: 				End  { 29 02 }
0x36EA1: 				OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which Processor Base Power (TDP) value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x2E1, VarStoreId: 0x1, VarOffset: 0x6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0 { 05 91 47 05 49 05 E1 02 01 00 6D 00 10 10 00 80 00 }
0x36EB2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36EB8: 					OneOfOption Option: "0" Value: 0 { 09 07 A5 04 00 00 00 }
0x36EBF: 					OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x36EC6: 					OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x36ECD: 					OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x36ED4: 					OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x36EDB: 					OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x36EE2: 					OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x36EE9: 					OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x36EF0: 					OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x36EF7: 					OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x36EFE: 					OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x36F05: 					OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x36F0C: 					OneOfOption Option: "16" Value: 16 { 09 07 B5 04 00 00 10 }
0x36F13: 					OneOfOption Option: "20" Value: 20 { 09 07 FE 1D 00 00 14 }
0x36F1A: 					OneOfOption Option: "24" Value: 24 { 09 07 FF 1D 00 00 18 }
0x36F21: 					OneOfOption Option: "28" Value: 28 { 09 07 00 1E 00 00 1C }
0x36F28: 					OneOfOption Option: "32" Value: 32 { 09 07 01 1E 00 00 20 }
0x36F2F: 					OneOfOption Option: "40" Value: 40 { 09 07 02 1E 00 00 28 }
0x36F36: 					OneOfOption Option: "48" Value: 48 { 09 07 03 1E 00 00 30 }
0x36F3D: 					OneOfOption Option: "56" Value: 56 { 09 07 04 1E 00 00 38 }
0x36F44: 					OneOfOption Option: "64" Value: 64 { 09 07 05 1E 00 00 40 }
0x36F4B: 					OneOfOption Option: "80" Value: 80 { 09 07 06 1E 00 00 50 }
0x36F52: 					OneOfOption Option: "96" Value: 96 { 09 07 07 1E 00 00 60 }
0x36F59: 					OneOfOption Option: "112" Value: 112 { 09 07 08 1E 00 00 70 }
0x36F60: 					OneOfOption Option: "128" Value: 128 { 09 07 09 1E 00 00 80 }
0x36F67: 				End  { 29 02 }
0x36F69: 				Numeric Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Custom value for Turbo Activation Ratio. Needs to be configured with valid values from LFM to Max Turbo. 0 means don't use custom value.", QuestionFlags: 0x10, QuestionId: 0x2E2, VarStoreId: 0x1, VarOffset: 0x6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 FF 04 01 05 E2 02 01 00 6E 00 10 10 00 FF 01 }
0x36F7A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x36F80: 				End  { 29 02 }
0x36F82: 			End  { 29 02 }
0x36F84: 		End  { 29 02 }
0x36F86: 		SuppressIf  { 0A 82 }
0x36F88: 			EqIdVal QuestionId: 0x1209, Value: 0x0 { 12 06 09 12 00 00 }
0x36F8E: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x36F95: 			End  { 29 02 }
0x36F97: 			Subtitle Prompt: "Custom Settings Level2", Help: "", Flags: 0x0 { 02 87 FD 04 00 00 00 }
0x36F9E: 			End  { 29 02 }
0x36FA0: 			GrayOutIf  { 19 82 }
0x36FA2: 				EqIdVal QuestionId: 0x2D9, Value: 0x1 { 12 06 D9 02 01 00 }
0x36FA8: 				Text Prompt: "ConfigTDP Level2", Help: "Configurable Processor Base Power (cTDP) Level2 Ratio and Processor Base Power (TDP) from MSR", Text: "N/A" { 03 08 ED 04 EC 04 EE 04 }
0x36FB0: 				Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and Processor Base Power (TDP) Limit.", QuestionFlags: 0x10, QuestionId: 0x2E3, VarStoreId: 0x1, VarOffset: 0x6F, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 43 05 AB 05 E3 02 01 00 6F 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36FCA: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36FD3: 				End  { 29 02 }
0x36FD5: 				Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x2E4, VarStoreId: 0x1, VarOffset: 0x73, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D { 07 9A 4F 05 AE 05 E4 02 01 00 73 00 10 12 00 00 00 00 83 7F 3E 00 7D 00 00 00 }
0x36FEF: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x36FF8: 				End  { 29 02 }
0x36FFA: 				OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which Processor Base Power (TDP) value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x2E5, VarStoreId: 0x1, VarOffset: 0x77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0 { 05 91 48 05 49 05 E5 02 01 00 77 00 10 10 00 80 00 }
0x3700B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x37011: 					OneOfOption Option: "0" Value: 0 { 09 07 A5 04 00 00 00 }
0x37018: 					OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x3701F: 					OneOfOption Option: "2" Value: 2 { 09 07 A7 04 00 00 02 }
0x37026: 					OneOfOption Option: "3" Value: 3 { 09 07 A8 04 00 00 03 }
0x3702D: 					OneOfOption Option: "4" Value: 4 { 09 07 A9 04 00 00 04 }
0x37034: 					OneOfOption Option: "5" Value: 5 { 09 07 AA 04 00 00 05 }
0x3703B: 					OneOfOption Option: "6" Value: 6 { 09 07 AB 04 00 00 06 }
0x37042: 					OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x37049: 					OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x37050: 					OneOfOption Option: "10" Value: 10 { 09 07 AF 04 00 00 0A }
0x37057: 					OneOfOption Option: "12" Value: 12 { 09 07 B1 04 00 00 0C }
0x3705E: 					OneOfOption Option: "14" Value: 14 { 09 07 B3 04 00 00 0E }
0x37065: 					OneOfOption Option: "16" Value: 16 { 09 07 B5 04 00 00 10 }
0x3706C: 					OneOfOption Option: "20" Value: 20 { 09 07 FE 1D 00 00 14 }
0x37073: 					OneOfOption Option: "24" Value: 24 { 09 07 FF 1D 00 00 18 }
0x3707A: 					OneOfOption Option: "28" Value: 28 { 09 07 00 1E 00 00 1C }
0x37081: 					OneOfOption Option: "32" Value: 32 { 09 07 01 1E 00 00 20 }
0x37088: 					OneOfOption Option: "40" Value: 40 { 09 07 02 1E 00 00 28 }
0x3708F: 					OneOfOption Option: "48" Value: 48 { 09 07 03 1E 00 00 30 }
0x37096: 					OneOfOption Option: "56" Value: 56 { 09 07 04 1E 00 00 38 }
0x3709D: 					OneOfOption Option: "64" Value: 64 { 09 07 05 1E 00 00 40 }
0x370A4: 					OneOfOption Option: "80" Value: 80 { 09 07 06 1E 00 00 50 }
0x370AB: 					OneOfOption Option: "96" Value: 96 { 09 07 07 1E 00 00 60 }
0x370B2: 					OneOfOption Option: "112" Value: 112 { 09 07 08 1E 00 00 70 }
0x370B9: 					OneOfOption Option: "128" Value: 128 { 09 07 09 1E 00 00 80 }
0x370C0: 				End  { 29 02 }
0x370C2: 				Numeric Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Custom value for Turbo Activation Ratio. Needs to be configured with valid values from LFM to Max Turbo. 0 means don't use custom value.", QuestionFlags: 0x10, QuestionId: 0x2E6, VarStoreId: 0x1, VarOffset: 0x78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 00 05 01 05 E6 02 01 00 78 00 10 10 00 FF 01 }
0x370D3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x370D9: 				End  { 29 02 }
0x370DB: 			End  { 29 02 }
0x370DD: 		End  { 29 02 }
0x370DF: 	End  { 29 02 }
0x370E1: 	Form FormId: 0x276E, Title: "  View/Configure CPU Lock Options" { 01 86 6E 27 A7 03 }
0x370E7: 		OneOf Prompt: "CFG Lock", Help: "Configure MSR 0xE2[15], CFG Lock bit", QuestionFlags: 0x10, QuestionId: 0x2E7, VarStoreId: 0x1, VarOffset: 0x43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 25 07 26 07 E7 02 01 00 43 00 10 10 00 01 00 }
0x370F8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x370FF: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37106: 		End  { 29 02 }
0x37108: 		OneOf Prompt: "Overclocking Lock", Help: "Enable/Disable Overclocking Lock (BIT 20) in FLEX_RATIO(194) MSR ", QuestionFlags: 0x10, QuestionId: 0x2E8, VarStoreId: 0x1, VarOffset: 0x10E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 21 07 22 07 E8 02 01 00 0E 01 10 10 00 01 00 }
0x37119: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37120: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37127: 		End  { 29 02 }
0x37129: 	End  { 29 02 }
0x3712B: 	Form FormId: 0x2865, Title: "PCH-FW Configuration" { 01 86 65 28 B2 19 }
0x37131: 		SuppressIf  { 0A 82 }
0x37133: 			True  { 46 02 }
0x37135: 			Action Prompt: "None", Help: "None", QuestionFlags: 0x4, QuestionId: 0x2866, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: "" { 0C 8F 05 00 05 00 66 28 00 00 FF FF 04 00 00 }
0x37144: 			End  { 29 02 }
0x37146: 		End  { 29 02 }
0x37148: 		Text Prompt: "ME Firmware Version", Help: "ME Firmware Version", Text: "N/A" { 03 08 B5 19 B4 19 B6 19 }
0x37150: 		SuppressIf  { 0A 82 }
0x37152: 			EqIdVal QuestionId: 0x1208, Value: 0xFF { 12 86 08 12 FF 00 }
0x37158: 				Not  { 17 02 }
0x3715A: 			End  { 29 02 }
0x3715C: 			Text Prompt: "ME Firmware Mode", Help: "", Text: "Normal Mode" { 03 08 B8 19 02 00 BA 19 }
0x37164: 			Text Prompt: "ME Firmware Mode", Help: "", Text: "ME ALT Disabled" { 03 08 B8 19 02 00 BE 19 }
0x3716C: 			Text Prompt: "ME Firmware Mode", Help: "", Text: "ME Temporarily Disabled" { 03 08 B8 19 02 00 BC 19 }
0x37174: 			Text Prompt: "ME Firmware Mode", Help: "", Text: "Secovr Jmpr/Heci MSG" { 03 08 B8 19 02 00 BD 19 }
0x3717C: 			Text Prompt: "ME Firmware Mode", Help: "", Text: "ME Failed" { 03 08 B8 19 02 00 BB 19 }
0x37184: 		End  { 29 02 }
0x37186: 		Text Prompt: "ME Firmware Mode", Help: "ME Firmware Mode", Text: "N/A" { 03 08 B8 19 B7 19 B9 19 }
0x3718E: 		Text Prompt: "ME Firmware SKU", Help: "ME Firmware SKU", Text: "N/A" { 03 08 C0 19 BF 19 C1 19 }
0x37196: 		Text Prompt: "ME Firmware Status 1", Help: "ME Firmware Status 1", Text: "N/A" { 03 08 C3 19 C2 19 C4 19 }
0x3719E: 		Text Prompt: "ME Firmware Status 2", Help: "ME Firmware Status 2", Text: "N/A" { 03 08 C6 19 C5 19 C7 19 }
0x371A6: 		Text Prompt: "ME Firmware Status 3", Help: "ME Firmware Status 3", Text: "N/A" { 03 08 C9 19 C8 19 CA 19 }
0x371AE: 		Text Prompt: "ME Firmware Status 4", Help: "ME Firmware Status 4", Text: "N/A" { 03 08 CC 19 CB 19 CD 19 }
0x371B6: 		Text Prompt: "ME Firmware Status 5", Help: "ME Firmware Status 5", Text: "N/A" { 03 08 CF 19 CE 19 D0 19 }
0x371BE: 		Text Prompt: "ME Firmware Status 6", Help: "ME Firmware Status 6", Text: "N/A" { 03 08 D2 19 D1 19 D3 19 }
0x371C6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x371CD: 		End  { 29 02 }
0x371CF: 		GrayOutIf  { 19 82 }
0x371D1: 			EqIdVal QuestionId: 0x1175, Value: 0x1 { 12 86 75 11 01 00 }
0x371D7: 				EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x371DD: 				Or  { 16 02 }
0x371DF: 			End  { 29 02 }
0x371E1: 			OneOf Prompt: "ME State", Help: "When Disabled ME will be put into ME Temporarily Disabled Mode.", QuestionFlags: 0x10, QuestionId: 0x2E9, VarStoreId: 0x9, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D4 19 D5 19 E9 02 09 00 02 00 10 10 00 01 00 }
0x371F2: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x371F9: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37200: 			End  { 29 02 }
0x37202: 		End  { 29 02 }
0x37204: 		SuppressIf  { 0A 82 }
0x37206: 			EqIdVal QuestionId: 0x2E9, Value: 0x0 { 12 06 E9 02 00 00 }
0x3720C: 			SuppressIf  { 0A 82 }
0x3720E: 				EqIdVal QuestionId: 0x1202, Value: 0x4 { 12 86 02 12 04 00 }
0x37214: 					Not  { 17 02 }
0x37216: 					EqIdVal QuestionId: 0x1208, Value: 0x0 { 12 06 08 12 00 00 }
0x3721C: 					Not  { 17 02 }
0x3721E: 					Or  { 16 02 }
0x37220: 					EqIdVal QuestionId: 0x1207, Value: 0x0 { 12 06 07 12 00 00 }
0x37226: 					Or  { 16 02 }
0x37228: 				End  { 29 02 }
0x3722A: 				GrayOutIf  { 19 82 }
0x3722C: 					EqIdVal QuestionId: 0x1175, Value: 0x1 { 12 06 75 11 01 00 }
0x37232: 					GrayOutIf  { 19 82 }
0x37234: 						EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x3723A: 						OneOf Prompt: "Manageability Features State", Help: "Enable/Disable Intel(R) Manageability features.

NOTE:
This option disables/enables Manageability Features support in FW.
To disable support platform must be in an unprovisioned state first.", QuestionFlags: 0x14, QuestionId: 0x285C, VarStoreId: 0x9, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 19 D7 19 5C 28 09 00 00 00 14 10 00 01 00 }
0x3724B: 							OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37252: 							OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x37259: 						End  { 29 02 }
0x3725B: 					End  { 29 02 }
0x3725D: 					SuppressIf  { 0A 82 }
0x3725F: 						EqIdVal QuestionId: 0x285C, Value: 0x0 { 12 06 5C 28 00 00 }
0x37265: 						GrayOutIf  { 19 82 }
0x37267: 							EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x3726D: 							OneOf Prompt: "AMT BIOS Features", Help: "When disabled AMT BIOS Features are no longer supported and user is no longer able to access MEBx Setup.

Note:
This option does not disable Manageability Features in FW.", QuestionFlags: 0x10, QuestionId: 0x2EA, VarStoreId: 0x8, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D8 19 D9 19 EA 02 08 00 14 00 10 10 00 01 00 }
0x3727E: 								OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37285: 								OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x3728C: 							End  { 29 02 }
0x3728E: 						End  { 29 02 }
0x37290: 						GrayOutIf  { 19 82 }
0x37292: 							EqIdVal QuestionId: 0x2EA, Value: 0x0 { 12 06 EA 02 00 00 }
0x37298: 							Ref Prompt: "AMT Configuration", Help: "Configure Intel(R) Active Management Technology Parameters", QuestionFlags: 0x0, QuestionId: 0x2EB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2895 { 0F 0F 7D 1E 7E 1E EB 02 00 00 FF FF 00 95 28 }
0x372A7: 						End  { 29 02 }
0x372A9: 					End  { 29 02 }
0x372AB: 				End  { 29 02 }
0x372AD: 			End  { 29 02 }
0x372AF: 			SuppressIf  { 0A 82 }
0x372B1: 				EqIdVal QuestionId: 0x285C, Value: 0x0 { 12 86 5C 28 00 00 }
0x372B7: 					EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x372BD: 					Or  { 16 02 }
0x372BF: 				End  { 29 02 }
0x372C1: 				Ref Prompt: "Local Platform Erase Configuration", Help: "Local Platform Erase configuration menu", QuestionFlags: 0x0, QuestionId: 0x2EC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x286F { 0F 0F 3E 1A 3F 1A EC 02 00 00 FF FF 00 6F 28 }
0x372D0: 			End  { 29 02 }
0x372D2: 			SuppressIf  { 0A 82 }
0x372D4: 				EqIdVal QuestionId: 0x1206, Value: 0x1 { 12 86 06 12 01 00 }
0x372DA: 					Not  { 17 02 }
0x372DC: 				End  { 29 02 }
0x372DE: 				OneOf Prompt: "ME Unconfig on RTC Clear", Help: "When Disabled ME will not be unconfigured on RTC Clear", QuestionFlags: 0x10, QuestionId: 0x2ED, VarStoreId: 0x8, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DA 19 DB 19 ED 02 08 00 10 00 10 10 00 01 00 }
0x372EF: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x372F6: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x372FD: 				End  { 29 02 }
0x372FF: 			End  { 29 02 }
0x37301: 			OneOf Prompt: "Comms Hub Support", Help: "Enables/Disables support for Comms Hub.", QuestionFlags: 0x10, QuestionId: 0x2EE, VarStoreId: 0x8, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 19 DD 19 EE 02 08 00 04 00 10 10 00 01 00 }
0x37312: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37319: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37320: 			End  { 29 02 }
0x37322: 			OneOf Prompt: "JHI Support", Help: "Enable/Disable Intel(R) DAL Host Interface Service (JHI)", QuestionFlags: 0x10, QuestionId: 0x2EF, VarStoreId: 0x8, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 19 DF 19 EF 02 08 00 13 00 10 10 00 01 00 }
0x37333: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3733A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37341: 			End  { 29 02 }
0x37343: 			OneOf Prompt: "Core Bios Done Message", Help: "Enable/Disable Core Bios Done message sent to ME", QuestionFlags: 0x10, QuestionId: 0x2F0, VarStoreId: 0x8, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 19 E3 19 F0 02 08 00 11 00 10 10 00 01 00 }
0x37354: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3735B: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37362: 			End  { 29 02 }
0x37364: 			SuppressIf  { 0A 82 }
0x37366: 				EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x3736C: 				OneOf Prompt: "CSE Data Resilience Support", Help: "Enable/Disable CSE Data Resilience Support", QuestionFlags: 0x10, QuestionId: 0x2F1, VarStoreId: 0x8, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 1A 2D 1A F1 02 08 00 35 00 10 10 00 01 00 }
0x3737D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37384: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3738B: 				End  { 29 02 }
0x3738D: 			End  { 29 02 }
0x3738F: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x37396: 			End  { 29 02 }
0x37398: 			Ref Prompt: "Firmware Update Configuration", Help: "Configure Management Engine Technology Parameters", QuestionFlags: 0x0, QuestionId: 0x2F2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2869 { 0F 0F E9 19 EA 19 F2 02 00 00 FF FF 00 69 28 }
0x373A7: 			Ref Prompt: "PTT Configuration", Help: "Configure PTT", QuestionFlags: 0x0, QuestionId: 0x2F3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2867 { 0F 0F EF 19 F0 19 F3 02 00 00 FF FF 00 67 28 }
0x373B6: 			Ref Prompt: "FIPS Configuration", Help: "FIPS Mode help", QuestionFlags: 0x0, QuestionId: 0x2F4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x286D { 0F 0F F9 19 FA 19 F4 02 00 00 FF FF 00 6D 28 }
0x373C5: 			SuppressIf  { 0A 82 }
0x373C7: 				EqIdVal QuestionId: 0x1202, Value: 0x4 { 12 86 02 12 04 00 }
0x373CD: 					Not  { 17 02 }
0x373CF: 				End  { 29 02 }
0x373D1: 				GrayOutIf  { 19 82 }
0x373D3: 					EqIdVal QuestionId: 0x1205, Value: 0x0 { 12 06 05 12 00 00 }
0x373D9: 					Ref Prompt: "Unique Platform Id Configuration", Help: "Configure Unique Platform Id Feature", QuestionFlags: 0x0, QuestionId: 0x2F5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x286A { 0F 0F 0D 1A 0E 1A F5 02 00 00 FF FF 00 6A 28 }
0x373E8: 				End  { 29 02 }
0x373EA: 			End  { 29 02 }
0x373EC: 			Ref Prompt: "ME Debug Configuration", Help: "Configure ME debug options

NOTE:
This menu is provided for testing purposes. It is recommended to leave the options in their default states", QuestionFlags: 0x0, QuestionId: 0x2F6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x286B { 0F 0F E4 19 E5 19 F6 02 00 00 FF FF 00 6B 28 }
0x373FB: 			Ref Prompt: "Anti-Rollback SVN Configuration", Help: "Configure Anti-Rollback SVN", QuestionFlags: 0x0, QuestionId: 0x2F7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x286E { 0F 0F 01 1A 02 1A F7 02 00 00 FF FF 00 6E 28 }
0x3740A: 		End  { 29 02 }
0x3740C: 		OneOf Prompt: "Extend CSME Measurement to TPM-PCR", Help: "Enable/Disable Extend CSME Measurement to TPM-PCR[0] and AMT Config to TPM-PCR[1]", QuestionFlags: 0x10, QuestionId: 0x2F8, VarStoreId: 0x8, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 19 E1 19 F8 02 08 00 27 00 10 10 00 01 00 }
0x3741D: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37424: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3742B: 		End  { 29 02 }
0x3742D: 	End  { 29 02 }
0x3742F: 	Form FormId: 0x2867, Title: "PTT Configuration" { 01 86 67 28 EF 19 }
0x37435: 		SuppressIf  { 0A 82 }
0x37437: 			True  { 46 02 }
0x37439: 			Action Prompt: "None", Help: "None", QuestionFlags: 0x4, QuestionId: 0x2868, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: "" { 0C 8F 05 00 05 00 68 28 00 00 FF FF 04 00 00 }
0x37448: 			End  { 29 02 }
0x3744A: 		End  { 29 02 }
0x3744C: 		Text Prompt: "PTT Capability / State", Help: "Platform Trust Technology Capability / Enablement State", Text: "N/A" { 03 08 F1 19 F3 19 F2 19 }
0x37454: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3745B: 		End  { 29 02 }
0x3745D: 		GrayOutIf  { 19 82 }
0x3745F: 			EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x37465: 			OneOf Prompt: "TPM Device Selection", Help: "Selects TPM device: PTT or dTPM. PTT - Enables PTT in SkuMgr dTPM 1.2 - Disables PTT in SkuMgr Warning !  PTT/dTPM will be disabled and all data saved on it will be lost.", QuestionFlags: 0x10, QuestionId: 0x2F9, VarStoreId: 0x11, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 1A 2F 1A F9 02 11 00 03 00 10 10 00 01 00 }
0x37476: 				OneOfOption Option: "dTPM" Value: 0 { 09 07 31 1A 00 00 00 }
0x3747D: 				OneOfOption Option: "PTT" Value: 1, Default, MfgDefault { 09 07 30 1A 30 00 01 }
0x37484: 			End  { 29 02 }
0x37486: 		End  { 29 02 }
0x37488: 		GrayOutIf  { 19 82 }
0x3748A: 			EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x37490: 			SuppressIf  { 0A 82 }
0x37492: 				EqIdVal QuestionId: 0x1204, Value: 0x0 { 12 86 04 12 00 00 }
0x37498: 					EqIdVal QuestionId: 0x1203, Value: 0x0 { 12 06 03 12 00 00 }
0x3749E: 					Or  { 16 02 }
0x374A0: 				End  { 29 02 }
0x374A2: 				OneOf Prompt: "TPM 1.2 Deactivate", Help: "Enabling this option will invoke the TPM 1.2 De-activate flow", QuestionFlags: 0x10, QuestionId: 0x2FA, VarStoreId: 0x9, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F4 19 F5 19 FA 02 09 00 06 00 10 10 00 01 00 }
0x374B3: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x374BA: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x374C1: 				End  { 29 02 }
0x374C3: 			End  { 29 02 }
0x374C5: 		End  { 29 02 }
0x374C7: 	End  { 29 02 }
0x374C9: 	Form FormId: 0x2869, Title: "Firmware Update Configuration" { 01 86 69 28 E9 19 }
0x374CF: 		OneOf Prompt: "Me FW Image Re-Flash", Help: "Enable/Disable Me FW Image Re-Flash function.", QuestionFlags: 0x10, QuestionId: 0x2FB, VarStoreId: 0x8, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 19 EC 19 FB 02 08 00 03 00 10 10 00 01 00 }
0x374E0: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x374E7: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x374EE: 		End  { 29 02 }
0x374F0: 		GrayOutIf  { 19 82 }
0x374F2: 			EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x374F8: 			OneOf Prompt: "FW Update", Help: "Enable/Disable ME FW Update function.", QuestionFlags: 0x10, QuestionId: 0x2FC, VarStoreId: 0x9, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 ED 19 EE 19 FC 02 09 00 01 00 10 10 00 01 00 }
0x37509: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37510: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37517: 			End  { 29 02 }
0x37519: 		End  { 29 02 }
0x3751B: 	End  { 29 02 }
0x3751D: 	Form FormId: 0x286A, Title: "Unique Platform Id Configuration" { 01 86 6A 28 0D 1A }
0x37523: 		Text Prompt: "OEM Platform Id", Help: "OEM Platform Id", Text: "N/A" { 03 08 13 1A 13 1A 14 1A }
0x3752B: 		Text Prompt: "CSME Platform Id", Help: "CSME Platform Id", Text: "N/A" { 03 08 15 1A 15 1A 16 1A }
0x37533: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3753A: 		End  { 29 02 }
0x3753C: 		GrayOutIf  { 19 82 }
0x3753E: 			EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x37544: 			OneOf Prompt: "Upid State", Help: "Enable/Disable Upid Feature", QuestionFlags: 0x10, QuestionId: 0x2FD, VarStoreId: 0x9, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0F 1A 10 1A FD 02 09 00 0E 00 10 10 00 01 00 }
0x37555: 				OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x3755C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37563: 			End  { 29 02 }
0x37565: 			OneOf Prompt: "Upid OS Control State", Help: "Allows OS to enable/disable the Upid feature state", QuestionFlags: 0x10, QuestionId: 0x2FE, VarStoreId: 0x9, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 1A 12 1A FE 02 09 00 0F 00 10 10 00 01 00 }
0x37576: 				OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x3757D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37584: 			End  { 29 02 }
0x37586: 		End  { 29 02 }
0x37588: 	End  { 29 02 }
0x3758A: 	Form FormId: 0x286B, Title: "ME Debug Configuration" { 01 86 6B 28 E4 19 }
0x37590: 		CheckBox Prompt: "HECI Timeouts", Help: "Enable/Disable HECI Send/Receive Timeouts.", QuestionFlags: 0x10, QuestionId: 0x2FF, VarStoreId: 0x8, VarOffset: 0x5, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 17 1A 18 1A FF 02 08 00 05 00 10 01 }
0x3759E: 		End  { 29 02 }
0x375A0: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x375A7: 		End  { 29 02 }
0x375A9: 		OneOf Prompt: "Force ME DID Init Status", Help: "Forces the DID Initialization Status value.", QuestionFlags: 0x10, QuestionId: 0x300, VarStoreId: 0x8, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 19 1A 1A 1A 00 03 08 00 06 00 10 10 00 03 00 }
0x375BA: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x375C1: 			OneOfOption Option: "0 - Success" Value: 1 { 09 07 1B 1A 00 00 01 }
0x375C8: 			OneOfOption Option: "1 - No Memory in Channels" Value: 2 { 09 07 1C 1A 00 00 02 }
0x375CF: 			OneOfOption Option: "2 - Memory Init Error" Value: 3 { 09 07 1D 1A 00 00 03 }
0x375D6: 		End  { 29 02 }
0x375D8: 		OneOf Prompt: "CPU Replaced Polling Disable", Help: "Setting this option disables CPU replacement polling loop", QuestionFlags: 0x10, QuestionId: 0x301, VarStoreId: 0x8, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1E 1A 1F 1A 01 03 08 00 07 00 10 10 00 01 00 }
0x375E9: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x375F0: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x375F7: 		End  { 29 02 }
0x375F9: 		OneOf Prompt: "HECI Message check Disable", Help: "Setting this option disables message check for Bios Boot Path when sending", QuestionFlags: 0x10, QuestionId: 0x302, VarStoreId: 0x8, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 20 1A 21 1A 02 03 08 00 08 00 10 10 00 01 00 }
0x3760A: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x37611: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37618: 		End  { 29 02 }
0x3761A: 		OneOf Prompt: "MBP HOB Skip", Help: "Setting this option will skip MBP HOB", QuestionFlags: 0x10, QuestionId: 0x303, VarStoreId: 0x8, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 1A 23 1A 03 03 08 00 09 00 10 10 00 01 00 }
0x3762B: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x37632: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37639: 		End  { 29 02 }
0x3763B: 		CheckBox Prompt: "HECI2 Interface Communication", Help: "Adds and Removes HECI2 Device from PCI space.", QuestionFlags: 0x10, QuestionId: 0x304, VarStoreId: 0x8, VarOffset: 0xA, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 24 1A 25 1A 04 03 08 00 0A 00 10 00 }
0x37649: 		End  { 29 02 }
0x3764B: 		CheckBox Prompt: "KT Device", Help: "Enable/Disable KT Device", QuestionFlags: 0x10, QuestionId: 0x305, VarStoreId: 0x8, VarOffset: 0xB, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 26 1A 27 1A 05 03 08 00 0B 00 10 01 }
0x37659: 		End  { 29 02 }
0x3765B: 		OneOf Prompt: "End Of Post Message", Help: "Enable/Disable End of Post message sent to ME", QuestionFlags: 0x10, QuestionId: 0x306, VarStoreId: 0x8, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E6 19 E7 19 06 03 08 00 12 00 10 10 00 02 00 }
0x3766C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37673: 			OneOfOption Option: "Send in DXE" Value: 2, Default { 09 07 E8 19 10 00 02 }
0x3767A: 		End  { 29 02 }
0x3767C: 		OneOf Prompt: "D0I3 Setting for HECI Disable", Help: "Setting this option disables setting D0I3 bit for all HECI devices", QuestionFlags: 0x10, QuestionId: 0x307, VarStoreId: 0x8, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 1A 29 1A 07 03 08 00 0C 00 10 10 00 01 00 }
0x3768D: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x37694: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3769B: 		End  { 29 02 }
0x3769D: 		OneOf Prompt: "MCTP Broadcast Cycle", Help: "Enable/Disable Management Component Transport Protocol Broadcast Cycle and Set PMT as Bus Owner", QuestionFlags: 0x10, QuestionId: 0x308, VarStoreId: 0x8, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 1A 2B 1A 08 03 08 00 0D 00 10 10 00 01 00 }
0x376AE: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x376B5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x376BC: 		End  { 29 02 }
0x376BE: 		Ref Prompt: "SMBIOS type 130 OEM capabilities", Help: "This menu allows changing SMBIOS type 130 OEM capabilities", QuestionFlags: 0x0, QuestionId: 0x309, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x286C { 0F 0F 32 1A 33 1A 09 03 00 00 FF FF 00 6C 28 }
0x376CD: 	End  { 29 02 }
0x376CF: 	Form FormId: 0x286C, Title: "SMBIOS type 130 OEM capabilities" { 01 86 6C 28 32 1A }
0x376D5: 		CheckBox Prompt: "BIOS Reflash Capability State", Help: "Change BIOS Reflash Capability State", QuestionFlags: 0x10, QuestionId: 0x30A, VarStoreId: 0x8, VarOffset: 0x29, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 34 1A 35 1A 0A 03 08 00 29 00 10 01 }
0x376E3: 		End  { 29 02 }
0x376E5: 		CheckBox Prompt: "BIOS Boot to Setup Capability State", Help: "Change BIOS Boot to Setup Capability State", QuestionFlags: 0x10, QuestionId: 0x30B, VarStoreId: 0x8, VarOffset: 0x2A, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 36 1A 37 1A 0B 03 08 00 2A 00 10 01 }
0x376F3: 		End  { 29 02 }
0x376F5: 		CheckBox Prompt: "BIOS Pause Before Booting Capability State", Help: "Change BIOS Pause Before Booting Capability State", QuestionFlags: 0x10, QuestionId: 0x30C, VarStoreId: 0x8, VarOffset: 0x2B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 38 1A 39 1A 0C 03 08 00 2B 00 10 00 }
0x37703: 		End  { 29 02 }
0x37705: 		CheckBox Prompt: "BIOS Secure Boot Capability Exposure to FW State", Help: "Change BIOS Secure Capability Exposure State to FW. This does not affect SecureBoot as such", QuestionFlags: 0x10, QuestionId: 0x30D, VarStoreId: 0x8, VarOffset: 0x2C, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 3A 1A 3B 1A 0D 03 08 00 2C 00 10 01 }
0x37713: 		End  { 29 02 }
0x37715: 		SuppressIf  { 0A 82 }
0x37717: 			EqIdVal QuestionId: 0x1202, Value: 0x4 { 12 86 02 12 04 00 }
0x3771D: 				Not  { 17 02 }
0x3771F: 			End  { 29 02 }
0x37721: 			CheckBox Prompt: "vPro TBT Dock Support", Help: "Enable/Disable vPro TBT Dock Support. Note: for the change to take effect, need to put system into G3 state then resume.", QuestionFlags: 0x10, QuestionId: 0x30E, VarStoreId: 0x8, VarOffset: 0x2D, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 3C 1A 3D 1A 0E 03 08 00 2D 00 10 01 }
0x3772F: 			End  { 29 02 }
0x37731: 		End  { 29 02 }
0x37733: 	End  { 29 02 }
0x37735: 	Form FormId: 0x286D, Title: "FIPS Mode" { 01 86 6D 28 F6 19 }
0x3773B: 		OneOf Prompt: "FIPS Mode Select", Help: "FIPS Mode configuration", QuestionFlags: 0x10, QuestionId: 0x30F, VarStoreId: 0x9, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F7 19 F8 19 0F 03 09 00 0A 00 10 10 00 01 00 }
0x3774C: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37753: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3775A: 		End  { 29 02 }
0x3775C: 		Text Prompt: "Current FIPS mode", Help: "N/A", Text: "Current mode unavailable" { 03 08 FB 19 FC 19 FD 19 }
0x37764: 		Text Prompt: "Crypto driver FIPS version", Help: "N/A", Text: "Version unavailable" { 03 08 FE 19 FF 19 00 1A }
0x3776C: 	End  { 29 02 }
0x3776E: 	Form FormId: 0x286E, Title: "Anti-Rollback SVN Configuration" { 01 86 6E 28 01 1A }
0x37774: 		Text Prompt: "Minimal Allowed Anti-Rollback SVN", Help: "Minimum ARB-SVN allowed on this platform. ME FW with lower ARB-SVN will not boot.", Text: "N/A" { 03 08 03 1A 04 1A 05 1A }
0x3777C: 		Text Prompt: "Executing Anti-Rollback SVN", Help: "ARB-SVN of executing ME FW", Text: "N/A" { 03 08 06 1A 07 1A 08 1A }
0x37784: 		GrayOutIf  { 19 82 }
0x37786: 			EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x3778C: 			OneOf Prompt: "Automatic HW-Enforced Anti-Rollback SVN", Help: "When enabled, hardware-enforced Anti-Rollback mechanism is automatically activated: once ME FW was successfully run on a platform, FW with lower ARB-SVN will be blocked from execution", QuestionFlags: 0x10, QuestionId: 0x310, VarStoreId: 0x8, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 1A 0A 1A 10 03 08 00 28 00 10 10 00 01 00 }
0x3779D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x377A4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x377AB: 			End  { 29 02 }
0x377AD: 			SuppressIf  { 0A 82 }
0x377AF: 				EqIdVal QuestionId: 0x310, Value: 0x1 { 12 06 10 03 01 00 }
0x377B5: 				OneOf Prompt: "Set HW-Enforced Anti-Rollback for Current SVN", Help: "Enable hardware-enforced Anti-Rollback mechanism for current ARB-SVN value. FW with lower ARB-SVN will be blocked from execution. The value will be restored to disable after the command is sent.", QuestionFlags: 0x4, QuestionId: 0x311, VarStoreId: 0x9, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 1A 0C 1A 11 03 09 00 0B 00 04 10 00 01 00 }
0x377C6: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x377CD: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x377D4: 				End  { 29 02 }
0x377D6: 			End  { 29 02 }
0x377D8: 		End  { 29 02 }
0x377DA: 	End  { 29 02 }
0x377DC: 	SuppressIf  { 0A 82 }
0x377DE: 		EqIdVal QuestionId: 0x285C, Value: 0x0 { 12 06 5C 28 00 00 }
0x377E4: 		Form FormId: 0x286F, Title: "Local Platform Erase Configuration" { 01 86 6F 28 3E 1A }
0x377EA: 			OneOf Prompt: "Perform Platform Erase Operations", Help: "Enabling this Feature will trigger Platform Erase Operations on the Next Boot", QuestionFlags: 0x14, QuestionId: 0x285D, VarStoreId: 0x28B8, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 1A 47 1A 5D 28 B8 28 01 00 14 10 00 01 00 }
0x377FB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37802: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37809: 				WarningIf Timeout: 0x0, Warning: " This options clears SSD, TPM, NVM variables and Loads the BIOS default Config " { 63 85 4A 1A 00 }
0x3780E: 					EqIdVal QuestionId: 0x285D, Value: 0x1 { 12 06 5D 28 01 00 }
0x37814: 				End  { 29 02 }
0x37816: 			End  { 29 02 }
0x37818: 			SuppressIf  { 0A 82 }
0x3781A: 				EqIdVal QuestionId: 0x285D, Value: 0x0 { 12 06 5D 28 00 00 }
0x37820: 				OneOf Prompt: "Erase All", Help: "Performs SSD Erase, TPM Clear,
Reload BIOS golden config, Clear NVME and 
OEM Custom actions", QuestionFlags: 0x14, QuestionId: 0x285E, VarStoreId: 0x28B8, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 1A 49 1A 5E 28 B8 28 02 00 14 10 00 01 00 }
0x37831: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37838: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3783F: 				End  { 29 02 }
0x37841: 				CheckBox Prompt: "   Storage Device Erase", Help: "Perform SSD/Nvme Erase", QuestionFlags: 0x14, QuestionId: 0x285F, VarStoreId: 0x28B8, VarOffset: 0x3, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 4B 1A 4C 1A 5F 28 B8 28 03 00 14 00 }
0x3784F: 				End  { 29 02 }
0x37851: 				SuppressIf  { 0A 82 }
0x37853: 					EqIdVal QuestionId: 0x285F, Value: 0x0 { 12 06 5F 28 00 00 }
0x37859: 					OneOf Prompt: "   SSD Erase Mode", Help: "Change LPE SSD Erase Action behavior:
Simulated: Performs LPE SSD Erase flow without erasing SSD
Real: Erase SSD.
*** If SATA device is used, OEM could use SECURE_ERASE_HOOK_PROTOCOL to remove SATA power to skip G3 cycle. ***", QuestionFlags: 0x10, QuestionId: 0x312, VarStoreId: 0x28B8, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 1A 41 1A 12 03 B8 28 09 00 10 10 00 01 00 }
0x3786A: 						OneOfOption Option: "Simulated" Value: 0, Default, MfgDefault { 09 07 42 1A 30 00 00 }
0x37871: 						OneOfOption Option: "Real" Value: 1 { 09 07 43 1A 00 00 01 }
0x37878: 					End  { 29 02 }
0x3787A: 					SuppressIf  { 0A 82 }
0x3787C: 						EqIdVal QuestionId: 0x312, Value: 0x0 { 12 86 12 03 00 00 }
0x37882: 							EqIdVal QuestionId: 0x1201, Value: 0x0 { 12 06 01 12 00 00 }
0x37888: 							Or  { 16 02 }
0x3788A: 						End  { 29 02 }
0x3788C: 						OneOf Prompt: "   Storage Erase Verification", Help: "Perform storage erase verification", QuestionFlags: 0x10, QuestionId: 0x313, VarStoreId: 0x28B8, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 1A 45 1A 13 03 B8 28 0A 00 10 10 00 01 00 }
0x3789D: 							OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x378A4: 							OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x378AB: 						End  { 29 02 }
0x378AD: 					End  { 29 02 }
0x378AF: 				End  { 29 02 }
0x378B1: 				CheckBox Prompt: "   TPM CLEAR", Help: "Perform SSD/Nvme Erase", QuestionFlags: 0x14, QuestionId: 0x2860, VarStoreId: 0x28B8, VarOffset: 0x4, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 4D 1A 4C 1A 60 28 B8 28 04 00 14 00 }
0x378BF: 				End  { 29 02 }
0x378C1: 				CheckBox Prompt: "   OEM Custom Actions", Help: "OEM Custom Actions", QuestionFlags: 0x10, QuestionId: 0x314, VarStoreId: 0x28B8, VarOffset: 0x5, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 4E 1A 4F 1A 14 03 B8 28 05 00 10 00 }
0x378CF: 				End  { 29 02 }
0x378D1: 				CheckBox Prompt: "   Clear NVM Variable", Help: "Clears NVM Varibles", QuestionFlags: 0x14, QuestionId: 0x2861, VarStoreId: 0x28B8, VarOffset: 0x6, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 50 1A 51 1A 61 28 B8 28 06 00 14 00 }
0x378DF: 				End  { 29 02 }
0x378E1: 				CheckBox Prompt: "   BIOS Reload Golden Config", Help: "Load BIOS default config", QuestionFlags: 0x14, QuestionId: 0x2862, VarStoreId: 0x28B8, VarOffset: 0x7, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 52 1A 53 1A 62 28 B8 28 07 00 14 00 }
0x378EF: 				End  { 29 02 }
0x378F1: 				CheckBox Prompt: "Unconfigure CSME", Help: "This option Unconfigure CSME Firmware and Unprovision AMT.", QuestionFlags: 0x10, QuestionId: 0x315, VarStoreId: 0x28B8, VarOffset: 0x8, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 54 1A 55 1A 15 03 B8 28 08 00 10 00 }
0x378FF: 					WarningIf Timeout: 0x0, Warning: "Performing this Action disconnect AMT Remote Access and require Admin to provision AMT" { 63 85 56 1A 00 }
0x37904: 						EqIdVal QuestionId: 0x315, Value: 0x1 { 12 06 15 03 01 00 }
0x3790A: 					End  { 29 02 }
0x3790C: 				End  { 29 02 }
0x3790E: 			End  { 29 02 }
0x37910: 		End  { 29 02 }
0x37912: 	End  { 29 02 }
0x37914: 	Form FormId: 0x2876, Title: "Thermal Configuration" { 01 86 76 28 B4 1A }
0x3791A: 		Subtitle Prompt: "Thermal Configuration", Help: "", Flags: 0x0 { 02 87 B4 1A 00 00 00 }
0x37921: 		End  { 29 02 }
0x37923: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3792A: 		End  { 29 02 }
0x3792C: 		OneOf Prompt: "Enable All Thermal Functions", Help: "Enable All Thermal Functions" is Enabled it Enables 'Memory Thermal Management','Active Trip Points', 'Critical Trip Points'.Set to disabled for Manual Configuration", QuestionFlags: 0x14, QuestionId: 0x2870, VarStoreId: 0x1, VarOffset: 0x1F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 1A B3 1A 70 28 01 00 F1 01 14 10 00 01 00 }
0x3793D: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x37943: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3794A: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37951: 		End  { 29 02 }
0x37953: 		Ref Prompt: "CPU Thermal Configuration", Help: "CPU Thermal Configuration options", QuestionFlags: 0x0, QuestionId: 0x316, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2877 { 0F 0F 59 1A 5A 1A 16 03 00 00 FF FF 00 77 28 }
0x37962: 		Ref Prompt: "Platform Thermal Configuration", Help: "Platform Thermal Configuration options", QuestionFlags: 0x0, QuestionId: 0x317, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2878 { 0F 0F 57 1A 58 1A 17 03 00 00 FF FF 00 78 28 }
0x37971: 		Ref Prompt: "Intel(R) Dynamic Tuning Technology Configuration", Help: "Intel(R) Dynamic Tuning Technology Configuration options", QuestionFlags: 0x0, QuestionId: 0x318, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2879 { 0F 0F 5B 1A 5C 1A 18 03 00 00 FF FF 00 79 28 }
0x37980: 	End  { 29 02 }
0x37982: 	Form FormId: 0x2877, Title: "Cpu Thermal Configuration" { 01 86 77 28 33 1B }
0x37988: 		Subtitle Prompt: "Cpu Thermal Configuration", Help: "", Flags: 0x0 { 02 87 33 1B 00 00 00 }
0x3798F: 		End  { 29 02 }
0x37991: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x37998: 		End  { 29 02 }
0x3799A: 		Text Prompt: "Current Tcc Activation Offset", Help: "Offset from factory set Tcc activation temprature at which the Thermal Control Circuit must be activated. Tcc will be activated at: Tcc Activation Temp - Tcc Activation Offset. Tcc Activation Offset range is 0 to 63.", Text: "" { 03 08 35 1B 37 1B 34 1B }
0x379A2: 		Numeric Prompt: "Tcc Activation Offset", Help: "Offset from factory set Tcc activation temprature at which the Thermal Control Circuit must be activated. Tcc will be activated at: Tcc Activation Temp - Tcc Activation Offset. Tcc Activation Offset range is 0 to 63.", QuestionFlags: 0x10, QuestionId: 0x319, VarStoreId: 0x1, VarOffset: 0x7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x0 { 07 91 36 1B 37 1B 19 03 01 00 7F 00 10 10 00 3F 00 }
0x379B3: 			Default DefaultId: 0x0 Value: 10 { 5B 06 00 00 00 0A }
0x379B9: 		End  { 29 02 }
0x379BB: 		OneOf Prompt: "Tcc Offset Time Window", Help: "Tcc Offset Time Window for Running Average Temperature Limit(RATL) feature. The Tcc offset time window can range from 5ms to 448s.", QuestionFlags: 0x10, QuestionId: 0x31A, VarStoreId: 0x1, VarOffset: 0x1C8, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x6D600, Step: 0x0 { 05 9A 38 1B 39 1B 1A 03 01 00 C8 01 10 12 00 00 00 00 00 D6 06 00 00 00 00 00 }
0x379D5: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 0A 04 00 32 02 00 00 00 00 }
0x379DF: 			OneOfOption Option: "5 ms" Value: 5 { 09 0A 4E 06 02 02 05 00 00 00 }
0x379E9: 			OneOfOption Option: "10 ms" Value: 10 { 09 0A 52 06 02 02 0A 00 00 00 }
0x379F3: 			OneOfOption Option: "55 ms" Value: 55 { 09 0A 53 06 02 02 37 00 00 00 }
0x379FD: 			OneOfOption Option: "156 ms" Value: 156 { 09 0A 54 06 02 02 9C 00 00 00 }
0x37A07: 			OneOfOption Option: "375 ms" Value: 375 { 09 0A 55 06 02 02 77 01 00 00 }
0x37A11: 			OneOfOption Option: "500 ms" Value: 500 { 09 0A 56 06 02 02 F4 01 00 00 }
0x37A1B: 			OneOfOption Option: "750 ms" Value: 750 { 09 0A 57 06 02 02 EE 02 00 00 }
0x37A25: 			OneOfOption Option: "1 sec" Value: 1000 { 09 0A 58 06 02 02 E8 03 00 00 }
0x37A2F: 			OneOfOption Option: "2 sec" Value: 2000 { 09 0A 59 06 02 02 D0 07 00 00 }
0x37A39: 			OneOfOption Option: "3 sec" Value: 3000 { 09 0A 5A 06 02 02 B8 0B 00 00 }
0x37A43: 			OneOfOption Option: "4 sec" Value: 4000 { 09 0A 5B 06 02 02 A0 0F 00 00 }
0x37A4D: 			OneOfOption Option: "5 sec" Value: 5000 { 09 0A 5C 06 02 02 88 13 00 00 }
0x37A57: 			OneOfOption Option: "6 sec" Value: 6000 { 09 0A 5D 06 02 02 70 17 00 00 }
0x37A61: 			OneOfOption Option: "7 sec" Value: 7000 { 09 0A 5E 06 02 02 58 1B 00 00 }
0x37A6B: 			OneOfOption Option: "8 sec" Value: 8000 { 09 0A 5F 06 02 02 40 1F 00 00 }
0x37A75: 			OneOfOption Option: "10 sec" Value: 10000 { 09 0A 60 06 02 02 10 27 00 00 }
0x37A7F: 			OneOfOption Option: "12 sec" Value: 12000 { 09 0A 61 06 02 02 E0 2E 00 00 }
0x37A89: 			OneOfOption Option: "14 sec" Value: 14000 { 09 0A 62 06 02 02 B0 36 00 00 }
0x37A93: 			OneOfOption Option: "16 sec" Value: 16000 { 09 0A 63 06 02 02 80 3E 00 00 }
0x37A9D: 			OneOfOption Option: "20 sec" Value: 20000 { 09 0A 64 06 02 02 20 4E 00 00 }
0x37AA7: 			OneOfOption Option: "24 sec" Value: 24000 { 09 0A 65 06 02 02 C0 5D 00 00 }
0x37AB1: 			OneOfOption Option: "28 sec" Value: 28000 { 09 0A 66 06 02 02 60 6D 00 00 }
0x37ABB: 			OneOfOption Option: "32 sec" Value: 32000 { 09 0A 67 06 02 02 00 7D 00 00 }
0x37AC5: 			OneOfOption Option: "40 sec" Value: 40000 { 09 0A 68 06 02 02 40 9C 00 00 }
0x37ACF: 			OneOfOption Option: "48 sec" Value: 48000 { 09 0A 69 06 02 02 80 BB 00 00 }
0x37AD9: 			OneOfOption Option: "56 sec" Value: 56000 { 09 0A 6A 06 02 02 C0 DA 00 00 }
0x37AE3: 			OneOfOption Option: "64 sec" Value: 64000 { 09 0A 6B 06 02 02 00 FA 00 00 }
0x37AED: 			OneOfOption Option: "80 sec" Value: 80000 { 09 0A 6C 06 02 02 80 38 01 00 }
0x37AF7: 			OneOfOption Option: "96 sec" Value: 96000 { 09 0A 6D 06 02 02 00 77 01 00 }
0x37B01: 			OneOfOption Option: "112 sec" Value: 112000 { 09 0A 6E 06 02 02 80 B5 01 00 }
0x37B0B: 			OneOfOption Option: "128 sec" Value: 128000 { 09 0A 6F 06 02 02 00 F4 01 00 }
0x37B15: 			OneOfOption Option: "160 sec" Value: 160000 { 09 0A 70 06 02 02 00 71 02 00 }
0x37B1F: 			OneOfOption Option: "192 sec" Value: 192000 { 09 0A 71 06 02 02 00 EE 02 00 }
0x37B29: 			OneOfOption Option: "224 sec" Value: 224000 { 09 0A 72 06 02 02 00 6B 03 00 }
0x37B33: 			OneOfOption Option: "256 sec" Value: 256000 { 09 0A 73 06 02 02 00 E8 03 00 }
0x37B3D: 			OneOfOption Option: "320 sec" Value: 320000 { 09 0A 74 06 02 02 00 E2 04 00 }
0x37B47: 			OneOfOption Option: "384 sec" Value: 384000 { 09 0A 75 06 02 02 00 DC 05 00 }
0x37B51: 			OneOfOption Option: "448 sec" Value: 448000 { 09 0A 76 06 02 02 00 D6 06 00 }
0x37B5B: 		End  { 29 02 }
0x37B5D: 		OneOf Prompt: "Tcc Offset Clamp Enable", Help: "Tcc Offset Clamp bit Enable for Running Average Temperature Limit(RATL) feature to allow CPU to throttle below P1.", QuestionFlags: 0x10, QuestionId: 0x31B, VarStoreId: 0x1, VarOffset: 0x1CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 1B 3B 1B 1B 03 01 00 CC 01 10 10 00 01 00 }
0x37B6E: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37B75: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37B7C: 		End  { 29 02 }
0x37B7E: 		OneOf Prompt: "Tcc Offset Lock Enable", Help: "Lock Enable for Running Average Temperature Limit(RATL) feature to lock Temperature Target MSR.", QuestionFlags: 0x10, QuestionId: 0x31C, VarStoreId: 0x1, VarOffset: 0x1CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 1B 3D 1B 1C 03 01 00 CD 01 10 10 00 01 00 }
0x37B8F: 			OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x37B96: 			OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x37B9D: 		End  { 29 02 }
0x37B9F: 		OneOf Prompt: "Bi-directional PROCHOT#", Help: "When a processor thermal sensor trips (either core), the PROCHOT# will be driven.
If bi-direction is enabled, external agents can drive PROCHOT# to throttle the processor.", QuestionFlags: 0x10, QuestionId: 0x31D, VarStoreId: 0x1, VarOffset: 0x7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 1B 3F 1B 1D 03 01 00 7A 00 10 10 00 01 00 }
0x37BB0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37BB7: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37BBE: 		End  { 29 02 }
0x37BC0: 		SuppressIf  { 0A 82 }
0x37BC2: 			EqIdVal QuestionId: 0x31D, Value: 0x0 { 12 06 1D 03 00 00 }
0x37BC8: 			OneOf Prompt: "Disable PROCHOT# Output", Help: "Enable/Disable PROCHOT# Output", QuestionFlags: 0x10, QuestionId: 0x31E, VarStoreId: 0x1, VarOffset: 0x7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 1B 41 1B 1E 03 01 00 7B 00 10 10 00 01 00 }
0x37BD9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37BE0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37BE7: 			End  { 29 02 }
0x37BE9: 		End  { 29 02 }
0x37BEB: 		OneOf Prompt: "Disable VR Thermal Alert", Help: "Enable/Disable VR Thermal Alert", QuestionFlags: 0x10, QuestionId: 0x31F, VarStoreId: 0x1, VarOffset: 0x7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 1B 45 1B 1F 03 01 00 7C 00 10 10 00 01 00 }
0x37BFC: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37C03: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37C0A: 		End  { 29 02 }
0x37C0C: 		OneOf Prompt: "PROCHOT Response", Help: "Enable/Disable PROCHOT Response", QuestionFlags: 0x10, QuestionId: 0x320, VarStoreId: 0x1, VarOffset: 0x7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 1B 47 1B 20 03 01 00 7E 00 10 10 00 01 00 }
0x37C1D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37C24: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37C2B: 		End  { 29 02 }
0x37C2D: 		OneOf Prompt: "PROCHOT Lock ", Help: "Enable/Disable PROCHOT Lock", QuestionFlags: 0x10, QuestionId: 0x321, VarStoreId: 0x1, VarOffset: 0x7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 1B 43 1B 21 03 01 00 7D 00 10 10 00 01 00 }
0x37C3E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37C45: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37C4C: 		End  { 29 02 }
0x37C4E: 		CheckBox Prompt: "ACPI T-States", Help: "Enable/Disable ACPI T-States.", QuestionFlags: 0x10, QuestionId: 0x322, VarStoreId: 0x1, VarOffset: 0x79, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 48 1B 49 1B 22 03 01 00 79 00 10 00 }
0x37C5C: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x37C62: 		End  { 29 02 }
0x37C64: 	End  { 29 02 }
0x37C66: 	Form FormId: 0x2878, Title: "Platform Thermal Configuration" { 01 86 78 28 57 1A }
0x37C6C: 		Subtitle Prompt: "Platform Thermal Configuration", Help: "", Flags: 0x0 { 02 87 57 1A 00 00 00 }
0x37C73: 		End  { 29 02 }
0x37C75: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x37C7C: 		End  { 29 02 }
0x37C7E: 		SuppressIf  { 0A 82 }
0x37C80: 			EqIdVal QuestionId: 0x2870, Value: 0x0 { 12 06 70 28 00 00 }
0x37C86: 			OneOf Prompt: "Critical Trip Point", Help: "This value controls the temperature of the ACPI Critical Trip Point - the point in which the OS will shut the system off.

NOTE:  119C is the Plan Of Record (POR) for all Intel mobile processors.", QuestionFlags: 0x10, QuestionId: 0x323, VarStoreId: 0xF101, VarOffset: 0x6BC, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x82, Step: 0x0 { 05 91 BC 1A BD 1A 23 03 01 F1 BC 06 10 10 0F 82 00 }
0x37C97: 				Default DefaultId: 0x0 Value: 119 { 5B 06 00 00 00 77 }
0x37C9D: 				OneOfOption Option: "15 C" Value: 15 { 09 07 BE 1A 00 00 0F }
0x37CA4: 				OneOfOption Option: "23 C" Value: 23 { 09 07 BF 1A 00 00 17 }
0x37CAB: 				OneOfOption Option: "31 C" Value: 31 { 09 07 C0 1A 00 00 1F }
0x37CB2: 				OneOfOption Option: "39 C" Value: 39 { 09 07 C1 1A 00 00 27 }
0x37CB9: 				OneOfOption Option: "47 C" Value: 47 { 09 07 C2 1A 00 00 2F }
0x37CC0: 				OneOfOption Option: "55 C" Value: 55 { 09 07 C3 1A 00 00 37 }
0x37CC7: 				OneOfOption Option: "63 C" Value: 63 { 09 07 C4 1A 00 00 3F }
0x37CCE: 				OneOfOption Option: "71 C" Value: 71 { 09 07 C5 1A 00 00 47 }
0x37CD5: 				OneOfOption Option: "79 C" Value: 79 { 09 07 C6 1A 00 00 4F }
0x37CDC: 				OneOfOption Option: "87 C" Value: 87 { 09 07 C7 1A 00 00 57 }
0x37CE3: 				OneOfOption Option: "95 C" Value: 95 { 09 07 C8 1A 00 00 5F }
0x37CEA: 				OneOfOption Option: "100 C" Value: 100 { 09 07 C9 1A 00 00 64 }
0x37CF1: 				OneOfOption Option: "103 C" Value: 103 { 09 07 CA 1A 00 00 67 }
0x37CF8: 				OneOfOption Option: "111 C" Value: 111 { 09 07 CB 1A 00 00 6F }
0x37CFF: 				OneOfOption Option: "119 C (POR)" Value: 119 { 09 07 CC 1A 00 00 77 }
0x37D06: 				OneOfOption Option: "127 C" Value: 127 { 09 07 CD 1A 00 00 7F }
0x37D0D: 				OneOfOption Option: "130 C" Value: 130 { 09 07 CE 1A 00 00 82 }
0x37D14: 			End  { 29 02 }
0x37D16: 		End  { 29 02 }
0x37D18: 		OneOf Prompt: "Active Trip Point 0", Help: "This value controls the temperature of the ACPI Active Trip Point 0 - the point in which the OS will turn the processor fan on Active Trip Point 0 Fan Speed.", QuestionFlags: 0x10, QuestionId: 0x324, VarStoreId: 0xF101, VarOffset: 0x6B8, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0 { 05 91 B8 1A B9 1A 24 03 01 F1 B8 06 10 10 0F 7F 00 }
0x37D29: 			OneOfOption Option: "Disabled" Value: 127 { 09 07 04 00 00 00 7F }
0x37D30: 			OneOfOption Option: "15 C" Value: 15 { 09 07 BE 1A 00 00 0F }
0x37D37: 			OneOfOption Option: "23 C" Value: 23 { 09 07 BF 1A 00 00 17 }
0x37D3E: 			OneOfOption Option: "31 C" Value: 31 { 09 07 C0 1A 00 00 1F }
0x37D45: 			OneOfOption Option: "39 C" Value: 39 { 09 07 C1 1A 00 00 27 }
0x37D4C: 			OneOfOption Option: "47 C" Value: 47 { 09 07 C2 1A 00 00 2F }
0x37D53: 			OneOfOption Option: "55 C" Value: 55 { 09 07 C3 1A 00 00 37 }
0x37D5A: 			OneOfOption Option: "63 C" Value: 63 { 09 07 C4 1A 00 00 3F }
0x37D61: 			OneOfOption Option: "71 C" Value: 71, Default, MfgDefault { 09 07 C5 1A 30 00 47 }
0x37D68: 			OneOfOption Option: "79 C" Value: 79 { 09 07 C6 1A 00 00 4F }
0x37D6F: 			OneOfOption Option: "87 C" Value: 87 { 09 07 C7 1A 00 00 57 }
0x37D76: 			OneOfOption Option: "95 C" Value: 95 { 09 07 C8 1A 00 00 5F }
0x37D7D: 			OneOfOption Option: "103 C" Value: 103 { 09 07 CA 1A 00 00 67 }
0x37D84: 			OneOfOption Option: "111 C" Value: 111 { 09 07 CB 1A 00 00 6F }
0x37D8B: 			OneOfOption Option: "119 C (POR)" Value: 119 { 09 07 CC 1A 00 00 77 }
0x37D92: 		End  { 29 02 }
0x37D94: 		Numeric Prompt: "Active Trip Point 0 Fan Speed", Help: "Active Trip Point 0 Fan Speed in percentage. Value must be between 0 (Fan off) - 100 (Max fan speed). This is the speed at which fan will run when Active Trip Point 0 is crossed.", QuestionFlags: 0x0, QuestionId: 0x325, VarStoreId: 0xF101, VarOffset: 0x6BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1 { 07 91 D5 1A D6 1A 25 03 01 F1 BA 06 00 10 00 64 01 }
0x37DA5: 			Default DefaultId: 0x0 Value: 100 { 5B 06 00 00 00 64 }
0x37DAB: 		End  { 29 02 }
0x37DAD: 		OneOf Prompt: "Active Trip Point 1", Help: "This value controls the temperature of the ACPI Active Trip Point 1 - the point in which the OS will turn the processor fan on Active Trip Point 1 Fan Speed.", QuestionFlags: 0x10, QuestionId: 0x326, VarStoreId: 0xF101, VarOffset: 0x6B7, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0 { 05 91 B6 1A B7 1A 26 03 01 F1 B7 06 10 10 0F 7F 00 }
0x37DBE: 			OneOfOption Option: "Disabled" Value: 127 { 09 07 04 00 00 00 7F }
0x37DC5: 			OneOfOption Option: "15 C" Value: 15 { 09 07 BE 1A 00 00 0F }
0x37DCC: 			OneOfOption Option: "23 C" Value: 23 { 09 07 BF 1A 00 00 17 }
0x37DD3: 			OneOfOption Option: "31 C" Value: 31 { 09 07 C0 1A 00 00 1F }
0x37DDA: 			OneOfOption Option: "39 C" Value: 39 { 09 07 C1 1A 00 00 27 }
0x37DE1: 			OneOfOption Option: "47 C" Value: 47 { 09 07 C2 1A 00 00 2F }
0x37DE8: 			OneOfOption Option: "55 C" Value: 55, Default, MfgDefault { 09 07 C3 1A 30 00 37 }
0x37DEF: 			OneOfOption Option: "63 C" Value: 63 { 09 07 C4 1A 00 00 3F }
0x37DF6: 			OneOfOption Option: "71 C" Value: 71 { 09 07 C5 1A 00 00 47 }
0x37DFD: 			OneOfOption Option: "79 C" Value: 79 { 09 07 C6 1A 00 00 4F }
0x37E04: 			OneOfOption Option: "87 C" Value: 87 { 09 07 C7 1A 00 00 57 }
0x37E0B: 			OneOfOption Option: "95 C" Value: 95 { 09 07 C8 1A 00 00 5F }
0x37E12: 			OneOfOption Option: "103 C" Value: 103 { 09 07 CA 1A 00 00 67 }
0x37E19: 			OneOfOption Option: "111 C" Value: 111 { 09 07 CB 1A 00 00 6F }
0x37E20: 			OneOfOption Option: "119 C (POR)" Value: 119 { 09 07 CC 1A 00 00 77 }
0x37E27: 		End  { 29 02 }
0x37E29: 		Numeric Prompt: "Active Trip Point 1 Fan Speed", Help: "Active Trip Point 1 Fan Speed in percentage. Value must be between 0 (Fan off) - 100 (Max fan speed). This value must be less than Active Trip Point 0 Fan speed. This is the speed at which fan will run when Active Trip 1 is crossed.", QuestionFlags: 0x0, QuestionId: 0x327, VarStoreId: 0xF101, VarOffset: 0x6B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1 { 07 91 D7 1A D8 1A 27 03 01 F1 B9 06 00 10 00 64 01 }
0x37E3A: 			Default DefaultId: 0x0 Value: 75 { 5B 06 00 00 00 4B }
0x37E40: 		End  { 29 02 }
0x37E42: 		OneOf Prompt: "Passive Trip Point", Help: "This value controls the temperature of the ACPI Passive Trip Point - the point in which the OS will begin throttling the processor.", QuestionFlags: 0x10, QuestionId: 0x328, VarStoreId: 0xF101, VarOffset: 0x6BB, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0 { 05 91 BA 1A BB 1A 28 03 01 F1 BB 06 10 10 0F 7F 00 }
0x37E53: 			Default DefaultId: 0x0 Value: 95 { 5B 06 00 00 00 5F }
0x37E59: 			OneOfOption Option: "Disabled" Value: 127 { 09 07 04 00 00 00 7F }
0x37E60: 			OneOfOption Option: "15 C" Value: 15 { 09 07 BE 1A 00 00 0F }
0x37E67: 			OneOfOption Option: "23 C" Value: 23 { 09 07 BF 1A 00 00 17 }
0x37E6E: 			OneOfOption Option: "31 C" Value: 31 { 09 07 C0 1A 00 00 1F }
0x37E75: 			OneOfOption Option: "39 C" Value: 39 { 09 07 C1 1A 00 00 27 }
0x37E7C: 			OneOfOption Option: "47 C" Value: 47 { 09 07 C2 1A 00 00 2F }
0x37E83: 			OneOfOption Option: "55 C" Value: 55 { 09 07 C3 1A 00 00 37 }
0x37E8A: 			OneOfOption Option: "63 C" Value: 63 { 09 07 C4 1A 00 00 3F }
0x37E91: 			OneOfOption Option: "71 C" Value: 71 { 09 07 C5 1A 00 00 47 }
0x37E98: 			OneOfOption Option: "79 C" Value: 79 { 09 07 C6 1A 00 00 4F }
0x37E9F: 			OneOfOption Option: "87 C" Value: 87 { 09 07 C7 1A 00 00 57 }
0x37EA6: 			OneOfOption Option: "95 C" Value: 95 { 09 07 C8 1A 00 00 5F }
0x37EAD: 			OneOfOption Option: "103 C" Value: 103 { 09 07 CA 1A 00 00 67 }
0x37EB4: 			OneOfOption Option: "111 C" Value: 111 { 09 07 CB 1A 00 00 6F }
0x37EBB: 			OneOfOption Option: "119 C (POR)" Value: 119 { 09 07 CC 1A 00 00 77 }
0x37EC2: 		End  { 29 02 }
0x37EC4: 		Numeric Prompt: "  Passive TC1 Value", Help: "This value sets the TC1 value for the ACPI Passive Cooling Formula. Range 1 - 16", QuestionFlags: 0x0, QuestionId: 0x329, VarStoreId: 0xF101, VarOffset: 0x6BD, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x10, Step: 0x1 { 07 91 D9 1A DA 1A 29 03 01 F1 BD 06 00 10 01 10 01 }
0x37ED5: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x37EDB: 		End  { 29 02 }
0x37EDD: 		Numeric Prompt: "  Passive TC2 Value", Help: "This value sets the TC2 value for the ACPI Passive Cooling Formula. Range 1 - 16", QuestionFlags: 0x0, QuestionId: 0x32A, VarStoreId: 0xF101, VarOffset: 0x6BE, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x10, Step: 0x1 { 07 91 DB 1A DC 1A 2A 03 01 F1 BE 06 00 10 01 10 01 }
0x37EEE: 			Default DefaultId: 0x0 Value: 5 { 5B 06 00 00 00 05 }
0x37EF4: 		End  { 29 02 }
0x37EF6: 		Numeric Prompt: "  Passive TSP Value", Help: "This item sets the TSP value for the ACPI Passive Cooling Formula.  It represents in tenths of a second how often the OS will read the temperature when passive cooling is enabled. Range 2 - 32", QuestionFlags: 0x0, QuestionId: 0x32B, VarStoreId: 0xF101, VarOffset: 0x6BF, Flags: 0x10, Size: 8, Min: 0x2, Max: 0x20, Step: 0x2 { 07 91 DD 1A DE 1A 2B 03 01 F1 BF 06 00 10 02 20 02 }
0x37F07: 			Default DefaultId: 0x0 Value: 10 { 5B 06 00 00 00 0A }
0x37F0D: 		End  { 29 02 }
0x37F0F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x37F16: 		End  { 29 02 }
0x37F18: 		OneOf Prompt: "Active Trip Points", Help: "Disable Active Trip Points", QuestionFlags: 0x10, QuestionId: 0x32C, VarStoreId: 0xF101, VarOffset: 0x6C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 1A E0 1A 2C 03 01 F1 C0 06 10 10 00 01 00 }
0x37F29: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37F30: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37F37: 		End  { 29 02 }
0x37F39: 		OneOf Prompt: "Passive Trip Points", Help: "Disable Passive Trip Points", QuestionFlags: 0x10, QuestionId: 0x32D, VarStoreId: 0xF101, VarOffset: 0x6C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 1A E2 1A 2D 03 01 F1 C1 06 10 10 00 01 00 }
0x37F4A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37F51: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37F58: 		End  { 29 02 }
0x37F5A: 		OneOf Prompt: "Critical Trip Points", Help: "Disable Critical Trip Points", QuestionFlags: 0x10, QuestionId: 0x32E, VarStoreId: 0xF101, VarOffset: 0x6C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 1A E4 1A 2E 03 01 F1 C2 06 10 10 00 01 00 }
0x37F6B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x37F72: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x37F79: 		End  { 29 02 }
0x37F7B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x37F82: 		End  { 29 02 }
0x37F84: 		CheckBox Prompt: "PCH Temp Read", Help: "PCH Temperature Read Enable", QuestionFlags: 0x10, QuestionId: 0x32F, VarStoreId: 0xF101, VarOffset: 0x6CB, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E EF 1A F0 1A 2F 03 01 F1 CB 06 10 01 }
0x37F92: 		End  { 29 02 }
0x37F94: 		CheckBox Prompt: "CPU Energy Read", Help: "CPU Energy Read Enable", QuestionFlags: 0x10, QuestionId: 0x330, VarStoreId: 0xF101, VarOffset: 0x6CA, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E ED 1A EE 1A 30 03 01 F1 CA 06 10 01 }
0x37FA2: 		End  { 29 02 }
0x37FA4: 		CheckBox Prompt: "CPU Temp Read", Help: "CPU Temperature Read Enable", QuestionFlags: 0x10, QuestionId: 0x331, VarStoreId: 0xF101, VarOffset: 0x6C9, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E EB 1A EC 1A 31 03 01 F1 C9 06 10 01 }
0x37FB2: 		End  { 29 02 }
0x37FB4: 		OneOf Prompt: "Alert Enable Lock", Help: "Lock all Alert Enable settings", QuestionFlags: 0x10, QuestionId: 0x332, VarStoreId: 0xF101, VarOffset: 0x6CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E5 1A E6 1A 32 03 01 F1 CC 06 10 10 00 01 00 }
0x37FC5: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37FCC: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37FD3: 		End  { 29 02 }
0x37FD5: 		SuppressIf  { 0A 82 }
0x37FD7: 			EqIdVal QuestionId: 0x332, Value: 0x0 { 12 06 32 03 00 00 }
0x37FDD: 			OneOf Prompt: " PCH Alert", Help: "PCH Alert pin enable", QuestionFlags: 0x10, QuestionId: 0x333, VarStoreId: 0xF101, VarOffset: 0x6CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E7 1A E8 1A 33 03 01 F1 CD 06 10 10 00 01 00 }
0x37FEE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x37FF5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x37FFC: 			End  { 29 02 }
0x37FFE: 			OneOf Prompt: " DIMM Alert", Help: "DIMM Alert pin enable", QuestionFlags: 0x10, QuestionId: 0x334, VarStoreId: 0xF101, VarOffset: 0x6CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 1A EA 1A 34 03 01 F1 CE 06 10 10 00 01 00 }
0x3800F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38016: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3801D: 			End  { 29 02 }
0x3801F: 		End  { 29 02 }
0x38021: 		Numeric Prompt: "CPU Temp", Help: "Fail Safe temp that EC will use if OS is hung", QuestionFlags: 0x0, QuestionId: 0x335, VarStoreId: 0xF101, VarOffset: 0x6CF, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x6E, Step: 0x1 { 07 91 F1 1A F2 1A 35 03 01 F1 CF 06 00 10 01 6E 01 }
0x38032: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x38037: 				Value  { 5A 82 }
0x38039: 					Uint64 Value: 0x48 { 45 0A 48 00 00 00 00 00 00 00 }
0x38043: 				End  { 29 02 }
0x38045: 			End  { 29 02 }
0x38047: 		End  { 29 02 }
0x38049: 		Numeric Prompt: "CPU Fan Speed", Help: "Fan speed that EC will use if OS is hung", QuestionFlags: 0x0, QuestionId: 0x336, VarStoreId: 0xF101, VarOffset: 0x6D0, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1 { 07 91 F3 1A F4 1A 36 03 01 F1 D0 06 00 10 01 64 01 }
0x3805A: 			Default DefaultId: 0x0 Value: 65 { 5B 06 00 00 00 41 }
0x38060: 		End  { 29 02 }
0x38062: 	End  { 29 02 }
0x38064: 	Form FormId: 0x2879, Title: "Intel(R) Dynamic Tuning Technology Configuration" { 01 86 79 28 5B 1A }
0x3806A: 		Subtitle Prompt: "Intel(R) Dynamic Tuning Technology Configuration", Help: "", Flags: 0x0 { 02 87 5B 1A 00 00 00 }
0x38071: 		End  { 29 02 }
0x38073: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3807A: 		End  { 29 02 }
0x3807C: 		GrayOutIf  { 19 82 }
0x3807E: 			EqIdVal QuestionId: 0x236, Value: 0x1 { 12 06 36 02 01 00 }
0x38084: 			OneOf Prompt: "Intel(R) Dynamic Tuning Technology", Help: "Enable/Disable Intel Dynamic Platform Thermal Framework", QuestionFlags: 0x10, QuestionId: 0x337, VarStoreId: 0xF101, VarOffset: 0x6D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 1A F6 1A 37 03 01 F1 D1 06 10 10 00 01 00 }
0x38095: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3809B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x380A2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x380A9: 			End  { 29 02 }
0x380AB: 		End  { 29 02 }
0x380AD: 		SuppressIf  { 0A 82 }
0x380AF: 			EqIdVal QuestionId: 0x337, Value: 0x0 { 12 06 37 03 00 00 }
0x380B5: 			OneOf Prompt: "INT3400 Device", Help: "Enable/Disable the INT3400 Device.", QuestionFlags: 0x10, QuestionId: 0x338, VarStoreId: 0xF101, VarOffset: 0x6E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 10 1B 11 1B 38 03 01 F1 E1 06 10 10 00 01 00 }
0x380C6: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x380CD: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x380D4: 			End  { 29 02 }
0x380D6: 			OneOf Prompt: "Processor Thermal Device", Help: "Enable/Disable Processor Thermal Device.", QuestionFlags: 0x10, QuestionId: 0x339, VarStoreId: 0xF101, VarOffset: 0x6D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 1A FA 1A 39 03 01 F1 D3 06 10 10 00 01 00 }
0x380E7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x380EE: 				OneOfOption Option: "SA Thermal Device" Value: 1, Default, MfgDefault { 09 07 FB 1A 30 00 01 }
0x380F5: 			End  { 29 02 }
0x380F7: 			SuppressIf  { 0A 82 }
0x380F9: 				EqIdVal QuestionId: 0x339, Value: 0x0 { 12 06 39 03 00 00 }
0x380FF: 				OneOf Prompt: " PPCC Step Size", Help: "Step size for Turbo power limit (RAPL) control", QuestionFlags: 0x10, QuestionId: 0x33A, VarStoreId: 0xF101, VarOffset: 0x6D4, Flags: 0x12, Size: 32, Min: 0x1F4, Max: 0x7D0, Step: 0x0 { 05 9A CF 1A D0 1A 3A 03 01 F1 D4 06 10 12 F4 01 00 00 D0 07 00 00 00 00 00 00 }
0x38119: 					OneOfOption Option: "0.5 Watts" Value: 500, Default, MfgDefault { 09 0A D1 1A 32 02 F4 01 00 00 }
0x38123: 					OneOfOption Option: "1.0 Watts" Value: 1000 { 09 0A D2 1A 02 02 E8 03 00 00 }
0x3812D: 					OneOfOption Option: "1.5 Watts" Value: 1500 { 09 0A D3 1A 02 02 DC 05 00 00 }
0x38137: 					OneOfOption Option: "2.0 Watts" Value: 2000 { 09 0A D4 1A 02 02 D0 07 00 00 }
0x38141: 				End  { 29 02 }
0x38143: 			End  { 29 02 }
0x38145: 			Numeric Prompt: "Intel(R) Dynamic Tuning Technology Configuration", Help: "An Integer containing the Intel(R) Dynamic Tuning Technology Configuration bitmap:   BIT0[Generic UI Access Control](0=enable,1=disable) BIT1[Restricted UI Access Control](0=enable,1=disable) BIT2[shell Access Control](0=enable,1=disable) BIT3[Environment Monitoring Report Control](0=report,1=silent) BIT4[Thermal Mitigation Report Control](0=silent,1=report)  BIT5[Thermal Policy Report Control](0=silent,1=report)", QuestionFlags: 0x10, QuestionId: 0x33B, VarStoreId: 0xF101, VarOffset: 0x6D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F7 1A F8 1A 3B 03 01 F1 D2 06 10 10 00 FF 01 }
0x38156: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3815C: 			End  { 29 02 }
0x3815E: 			GrayOutIf  { 19 82 }
0x38160: 				EqIdVal QuestionId: 0x1200, Value: 0x0 { 12 06 00 12 00 00 }
0x38166: 				OneOf Prompt: "FAN1 Device", Help: "Enable the Fan1 device.", QuestionFlags: 0x10, QuestionId: 0x33C, VarStoreId: 0xF101, VarOffset: 0x6DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 1A FE 1A 3C 03 01 F1 DB 06 10 10 00 01 00 }
0x38177: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3817E: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x38185: 				End  { 29 02 }
0x38187: 			End  { 29 02 }
0x38189: 			GrayOutIf  { 19 82 }
0x3818B: 				EqIdVal QuestionId: 0x11FF, Value: 0x0 { 12 06 FF 11 00 00 }
0x38191: 				OneOf Prompt: "FAN2 Device", Help: "Enable the Fan2 device.", QuestionFlags: 0x10, QuestionId: 0x33D, VarStoreId: 0xF101, VarOffset: 0xA98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FF 1A 00 1B 3D 03 01 F1 98 0A 10 10 00 01 00 }
0x381A2: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x381A9: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x381B0: 				End  { 29 02 }
0x381B2: 			End  { 29 02 }
0x381B4: 			GrayOutIf  { 19 82 }
0x381B6: 				EqIdVal QuestionId: 0x11FE, Value: 0x0 { 12 06 FE 11 00 00 }
0x381BC: 				OneOf Prompt: "FAN3 Device", Help: "Enable the Fan3 device.", QuestionFlags: 0x10, QuestionId: 0x33E, VarStoreId: 0xF101, VarOffset: 0xA99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 1B 02 1B 3E 03 01 F1 99 0A 10 10 00 01 00 }
0x381CD: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x381D4: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x381DB: 				End  { 29 02 }
0x381DD: 			End  { 29 02 }
0x381DF: 			OneOf Prompt: "Charger participant", Help: "Enable/Disable Charger device", QuestionFlags: 0x10, QuestionId: 0x33F, VarStoreId: 0xF101, VarOffset: 0x6DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 1B 25 1B 3F 03 01 F1 DC 06 10 10 00 01 00 }
0x381F0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x381F7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x381FE: 			End  { 29 02 }
0x38200: 			OneOf Prompt: "Power participant", Help: "Enable/Disable the Power participant.", QuestionFlags: 0x10, QuestionId: 0x340, VarStoreId: 0xF101, VarOffset: 0x6DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 1B 0B 1B 40 03 01 F1 DD 06 10 10 00 01 00 }
0x38211: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38218: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3821F: 			End  { 29 02 }
0x38221: 			OneOf Prompt: "Battery Participant", Help: "Enable/Disable the Battery Participant.", QuestionFlags: 0x10, QuestionId: 0x341, VarStoreId: 0xF101, VarOffset: 0x6E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 1B 0F 1B 41 03 01 F1 E0 06 10 10 00 01 00 }
0x38232: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38239: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38240: 			End  { 29 02 }
0x38242: 			SuppressIf  { 0A 82 }
0x38244: 				EqIdVal QuestionId: 0x341, Value: 0x0 { 12 06 41 03 00 00 }
0x3824A: 				Numeric Prompt: "Intel(R) Dynamic Tuning Technology Battery Sampling Period", Help: "This battery sampling period for the Battery Participant Object.", QuestionFlags: 0x10, QuestionId: 0x342, VarStoreId: 0xF101, VarOffset: 0x6DE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 0C 1B 0D 1B 42 03 01 F1 DE 06 10 11 00 00 E8 03 01 00 }
0x3825E: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x38265: 				End  { 29 02 }
0x38267: 			End  { 29 02 }
0x38269: 			OneOf Prompt: "PCH FIVR Participant", Help: "Enable/Disable PCH FIVR Participant", QuestionFlags: 0x10, QuestionId: 0x343, VarStoreId: 0xF101, VarOffset: 0x6ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 1B 27 1B 43 03 01 F1 ED 06 10 10 00 01 00 }
0x3827A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38281: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38288: 			End  { 29 02 }
0x3828A: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x38291: 			End  { 29 02 }
0x38293: 			GrayOutIf  { 19 82 }
0x38295: 				EqIdVal QuestionId: 0x11FD, Value: 0x0 { 12 06 FD 11 00 00 }
0x3829B: 				OneOf Prompt: "Sensor Device 1", Help: "Enable/Disable Memory Thermal Device", QuestionFlags: 0x10, QuestionId: 0x344, VarStoreId: 0xF101, VarOffset: 0x6E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 1B FC 1A 44 03 01 F1 E8 06 10 10 00 01 00 }
0x382AC: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x382B3: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x382BA: 				End  { 29 02 }
0x382BC: 			End  { 29 02 }
0x382BE: 			GrayOutIf  { 19 82 }
0x382C0: 				EqIdVal QuestionId: 0x11FC, Value: 0x0 { 12 06 FC 11 00 00 }
0x382C6: 				OneOf Prompt: "Sensor Device 2", Help: "Enable/Disable VR Hotspot Q50 sensor", QuestionFlags: 0x10, QuestionId: 0x345, VarStoreId: 0xF101, VarOffset: 0x6E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 29 1B 2F 1B 45 03 01 F1 E9 06 10 10 00 01 00 }
0x382D7: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x382DE: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x382E5: 				End  { 29 02 }
0x382E7: 			End  { 29 02 }
0x382E9: 			GrayOutIf  { 19 82 }
0x382EB: 				EqIdVal QuestionId: 0x11FB, Value: 0x0 { 12 06 FB 11 00 00 }
0x382F1: 				OneOf Prompt: "Sensor Device 3", Help: "Enable/Disable Skin Hotspot U50 sensor", QuestionFlags: 0x10, QuestionId: 0x346, VarStoreId: 0xF101, VarOffset: 0x6EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 1B 30 1B 46 03 01 F1 EA 06 10 10 00 01 00 }
0x38302: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38309: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38310: 				End  { 29 02 }
0x38312: 			End  { 29 02 }
0x38314: 			GrayOutIf  { 19 82 }
0x38316: 				EqIdVal QuestionId: 0x11FA, Value: 0x0 { 12 06 FA 11 00 00 }
0x3831C: 				OneOf Prompt: "Sensor Device 4", Help: "Enable/Disable PMIC-MCP Hotspot Q16 sensor", QuestionFlags: 0x10, QuestionId: 0x347, VarStoreId: 0xF101, VarOffset: 0x6EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2B 1B 31 1B 47 03 01 F1 EB 06 10 10 00 01 00 }
0x3832D: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38334: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3833B: 				End  { 29 02 }
0x3833D: 			End  { 29 02 }
0x3833F: 			GrayOutIf  { 19 82 }
0x38341: 				EqIdVal QuestionId: 0x11F9, Value: 0x0 { 12 06 F9 11 00 00 }
0x38347: 				OneOf Prompt: "Sensor Device 5", Help: "Enable/Disable C-Skin Chassis U50 IR sensor", QuestionFlags: 0x10, QuestionId: 0x348, VarStoreId: 0xF101, VarOffset: 0x6EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 1B 32 1B 48 03 01 F1 EC 06 10 10 00 01 00 }
0x38358: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3835F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38366: 				End  { 29 02 }
0x38368: 			End  { 29 02 }
0x3836A: 			SuppressIf  { 0A 82 }
0x3836C: 				EqIdVal QuestionId: 0x11F8, Value: 0x1 { 12 86 F8 11 01 00 }
0x38372: 					Not  { 17 02 }
0x38374: 					EqIdVal QuestionId: 0x11F7, Value: 0x1 { 12 06 F7 11 01 00 }
0x3837A: 					Not  { 17 02 }
0x3837C: 					And  { 15 02 }
0x3837E: 				End  { 29 02 }
0x38380: 				OneOf Prompt: "Discret Graphics Sensor Device", Help: "Enable/Disable DGPU Thermal Sensor", QuestionFlags: 0x10, QuestionId: 0x349, VarStoreId: 0xF101, VarOffset: 0xA9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 1B 2E 1B 49 03 01 F1 9A 0A 10 10 00 01 00 }
0x38391: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38398: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3839F: 				End  { 29 02 }
0x383A1: 			End  { 29 02 }
0x383A3: 		End  { 29 02 }
0x383A5: 		SuppressIf  { 0A 82 }
0x383A7: 			EqIdVal QuestionId: 0x337, Value: 0x0 { 12 06 37 03 00 00 }
0x383AD: 			Ref Prompt: "OEM variable and Object", Help: "OEM variable and Object options", QuestionFlags: 0x0, QuestionId: 0x34A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x287A { 0F 0F 5D 1A 5E 1A 4A 03 00 00 FF FF 00 7A 28 }
0x383BC: 		End  { 29 02 }
0x383BE: 	End  { 29 02 }
0x383C0: 	Form FormId: 0x287A, Title: "OEM variable and Object" { 01 86 7A 28 5D 1A }
0x383C6: 		Subtitle Prompt: "OEM variable and Object", Help: "", Flags: 0x0 { 02 87 5D 1A 00 00 00 }
0x383CD: 		End  { 29 02 }
0x383CF: 		Numeric Prompt: "Design Variable 0", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize Intel(R) Dynamic Tuning Technology behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x34B, VarStoreId: 0xF101, VarOffset: 0x6FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 03 1B 09 1B 4B 03 01 F1 FA 06 00 10 00 FF 01 }
0x383E0: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x383E6: 		End  { 29 02 }
0x383E8: 		Numeric Prompt: "Design Variable 1", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize Intel(R) Dynamic Tuning Technology behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x34C, VarStoreId: 0xF101, VarOffset: 0x6FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 04 1B 09 1B 4C 03 01 F1 FB 06 00 10 00 FF 01 }
0x383F9: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x383FF: 		End  { 29 02 }
0x38401: 		Numeric Prompt: "Design Variable 2", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize Intel(R) Dynamic Tuning Technology behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x34D, VarStoreId: 0xF101, VarOffset: 0x6FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 05 1B 09 1B 4D 03 01 F1 FC 06 00 10 00 FF 01 }
0x38412: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x38418: 		End  { 29 02 }
0x3841A: 		Numeric Prompt: "Design Variable 3", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize Intel(R) Dynamic Tuning Technology behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x34E, VarStoreId: 0xF101, VarOffset: 0x6FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 06 1B 09 1B 4E 03 01 F1 FD 06 00 10 00 FF 01 }
0x3842B: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x38431: 		End  { 29 02 }
0x38433: 		Numeric Prompt: "Design Variable 4", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize Intel(R) Dynamic Tuning Technology behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x34F, VarStoreId: 0xF101, VarOffset: 0x6FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 07 1B 09 1B 4F 03 01 F1 FE 06 00 10 00 FF 01 }
0x38444: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3844A: 		End  { 29 02 }
0x3844C: 		Numeric Prompt: "Design Variable 5", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize Intel(R) Dynamic Tuning Technology behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x350, VarStoreId: 0xF101, VarOffset: 0x6FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 08 1B 09 1B 50 03 01 F1 FF 06 00 10 00 FF 01 }
0x3845D: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x38463: 		End  { 29 02 }
0x38465: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3846C: 		End  { 29 02 }
0x3846E: 		OneOf Prompt: "PPCC Object", Help: "Enable/Disable PPCC object for validation.", QuestionFlags: 0x10, QuestionId: 0x351, VarStoreId: 0xF101, VarOffset: 0x6EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 12 1B 13 1B 51 03 01 F1 EE 06 10 10 00 01 00 }
0x3847F: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x38486: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x3848D: 		End  { 29 02 }
0x3848F: 		OneOf Prompt: "ARTG Object", Help: "Enable/Disable ARTG object for validation.", QuestionFlags: 0x10, QuestionId: 0x352, VarStoreId: 0xF101, VarOffset: 0x6EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 1B 15 1B 52 03 01 F1 EF 06 10 10 00 01 00 }
0x384A0: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x384A7: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x384AE: 		End  { 29 02 }
0x384B0: 		OneOf Prompt: "PMAX Object", Help: "Enable/Disable PMAX object for validation.", QuestionFlags: 0x10, QuestionId: 0x353, VarStoreId: 0xF101, VarOffset: 0x6F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 16 1B 17 1B 53 03 01 F1 F0 06 10 10 00 01 00 }
0x384C1: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x384C8: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x384CF: 		End  { 29 02 }
0x384D1: 		SuppressIf  { 0A 82 }
0x384D3: 			EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x384D9: 				Not  { 17 02 }
0x384DB: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x384E1: 				Not  { 17 02 }
0x384E3: 				And  { 15 02 }
0x384E5: 			End  { 29 02 }
0x384E7: 			OneOf Prompt: "PMAX Device", Help: "Enable/Disable PMAX device for validation.", QuestionFlags: 0x10, QuestionId: 0x354, VarStoreId: 0xF101, VarOffset: 0xAD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 18 1B 19 1B 54 03 01 F1 D3 0A 10 10 00 01 00 }
0x384F8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x384FF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38506: 			End  { 29 02 }
0x38508: 			SuppressIf  { 0A 82 }
0x3850A: 				EqIdVal QuestionId: 0x354, Value: 0x0 { 12 06 54 03 00 00 }
0x38510: 				OneOf Prompt: "PMAX Audio codec", Help: "Enable/Disable PMAX Audio codec for validation.", QuestionFlags: 0x10, QuestionId: 0x355, VarStoreId: 0xF101, VarOffset: 0xAD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1A 1B 1B 1B 55 03 01 F1 D4 0A 10 10 00 01 00 }
0x38521: 					OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x38528: 					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x3852F: 				End  { 29 02 }
0x38531: 				OneOf Prompt: "PMAX WF Camera", Help: "Enable/Disable PMAX WF Camera for validation.", QuestionFlags: 0x10, QuestionId: 0x356, VarStoreId: 0xF101, VarOffset: 0xAD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1C 1B 1D 1B 56 03 01 F1 D5 0A 10 10 00 01 00 }
0x38542: 					OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x38549: 					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x38550: 				End  { 29 02 }
0x38552: 				OneOf Prompt: "PMAX UF Camera", Help: "Enable/Disable PMAX UF Camera for validation.", QuestionFlags: 0x10, QuestionId: 0x357, VarStoreId: 0xF101, VarOffset: 0xAD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1E 1B 1F 1B 57 03 01 F1 D6 0A 10 10 00 01 00 }
0x38563: 					OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x3856A: 					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x38571: 				End  { 29 02 }
0x38573: 				OneOf Prompt: "PMAX Flash device", Help: "Enable/Disable PMAX Flash device for validation.", QuestionFlags: 0x10, QuestionId: 0x358, VarStoreId: 0xF101, VarOffset: 0xAD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 20 1B 21 1B 58 03 01 F1 D7 0A 10 10 00 01 00 }
0x38584: 					OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x3858B: 					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x38592: 				End  { 29 02 }
0x38594: 			End  { 29 02 }
0x38596: 		End  { 29 02 }
0x38598: 		Text Prompt: "Processor Thermal Device", Help: "Intel(R) Dynamic Tuning Technology Configuration options", Text: "" { 03 08 F9 1A 5C 1A 00 00 }
0x385A0: 		SuppressIf  { 0A 82 }
0x385A2: 			True  { 46 02 }
0x385A4: 			OneOf Prompt: "Optional Objects", Help: "Enable/Disable PIPR/PAPR for processor participant.", QuestionFlags: 0x10, QuestionId: 0x359, VarStoreId: 0xF101, VarOffset: 0x6F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 1B 23 1B 59 03 01 F1 F9 06 10 10 00 01 00 }
0x385B5: 				OneOfOption Option: "Disabled" Value: 1, Default, MfgDefault { 09 07 04 00 30 00 01 }
0x385BC: 				OneOfOption Option: "Enabled" Value: 0 { 09 07 03 00 00 00 00 }
0x385C3: 			End  { 29 02 }
0x385C5: 		End  { 29 02 }
0x385C7: 	End  { 29 02 }
0x385C9: 	Form FormId: 0x287B, Title: "Platform Settings" { 01 86 7B 28 79 1B }
0x385CF: 		Subtitle Prompt: "Platform Settings", Help: "", Flags: 0x0 { 02 87 7B 1B 00 00 00 }
0x385D6: 		End  { 29 02 }
0x385D8: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x385DF: 		End  { 29 02 }
0x385E1: 		OneOf Prompt: "Charging Method", Help: "Select charging method as Normal Charging or Fast Charging.", QuestionFlags: 0x10, QuestionId: 0x35A, VarStoreId: 0xF101, VarOffset: 0x850, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 66 1C 67 1C 5A 03 01 F1 50 08 10 10 00 01 00 }
0x385F2: 			OneOfOption Option: "Normal Charging" Value: 0, Default, MfgDefault { 09 07 68 1C 30 00 00 }
0x385F9: 			OneOfOption Option: "Fast Charging" Value: 1 { 09 07 69 1C 00 00 01 }
0x38600: 		End  { 29 02 }
0x38602: 		SuppressIf  { 0A 82 }
0x38604: 			EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x3860A: 				Not  { 17 02 }
0x3860C: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x38612: 				Not  { 17 02 }
0x38614: 				And  { 15 02 }
0x38616: 			End  { 29 02 }
0x38618: 			OneOf Prompt: "Pseudo G3", Help: "Enable/Disable Pseudo G3", QuestionFlags: 0x14, QuestionId: 0x35B, VarStoreId: 0xF101, VarOffset: 0x5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 1C 83 1C 5B 03 01 F1 5F 00 14 10 00 01 00 }
0x38629: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38630: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x38637: 			End  { 29 02 }
0x38639: 		End  { 29 02 }
0x3863B: 		SuppressIf  { 0A 82 }
0x3863D: 			EqIdVal QuestionId: 0x11F6, Value: 0x1 { 12 86 F6 11 01 00 }
0x38643: 				Not  { 17 02 }
0x38645: 			End  { 29 02 }
0x38647: 			OneOf Prompt: "RP08 D3 cold Support", Help: "Enable - RP08 D3cold entry is disabled .Disabled -RP08 D3Cold entry is enabled", QuestionFlags: 0x10, QuestionId: 0x35C, VarStoreId: 0xF101, VarOffset: 0xB87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 1C 85 1C 5C 03 01 F1 87 0B 10 10 00 01 00 }
0x38658: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3865F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38666: 			End  { 29 02 }
0x38668: 			OneOf Prompt: "Rp08 Wake Rework Support", Help: "Enable - Wake Enabled on RP08.Disabled - Wake Enabled on PEG10", QuestionFlags: 0x10, QuestionId: 0x35D, VarStoreId: 0xF101, VarOffset: 0xB88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 1C 87 1C 5D 03 01 F1 88 0B 10 10 00 01 00 }
0x38679: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38680: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38687: 			End  { 29 02 }
0x38689: 		End  { 29 02 }
0x3868B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x38692: 		End  { 29 02 }
0x38694: 		OneOf Prompt: "Firmware Configuration", Help: "Firmware Configuration options.
NOTE:Ignore Policy Update(STR_FW_CONFIG_DEFAULT_VALUE) is to skip policy update and will ONLY WORK ON A PLATFORM.", QuestionFlags: 0x10, QuestionId: 0x35E, VarStoreId: 0xF101, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A9 1C AA 1C 5E 03 01 F1 30 00 10 10 00 02 00 }
0x386A5: 			OneOfOption Option: "Ignore Policy Update" Value: 0 { 09 07 AB 1C 00 00 00 }
0x386AC: 			OneOfOption Option: "Production" Value: 1 { 09 07 AC 1C 00 00 01 }
0x386B3: 			OneOfOption Option: "Test" Value: 2, Default { 09 07 AD 1C 10 00 02 }
0x386BA: 		End  { 29 02 }
0x386BC: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x386C3: 		End  { 29 02 }
0x386C5: 		OneOf Prompt: "Scan Matrix Keyboard Support", Help: "Enable Scan Matrix Keyboard Support", QuestionFlags: 0x10, QuestionId: 0x2871, VarStoreId: 0xF101, VarOffset: 0x6B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 1C 62 1C 71 28 01 F1 B5 06 10 10 00 01 00 }
0x386D6: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x386DB: 				Value  { 5A 82 }
0x386DD: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x386E7: 				End  { 29 02 }
0x386E9: 			End  { 29 02 }
0x386EB: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x386F2: 			SuppressIf  { 0A 82 }
0x386F4: 				EqIdVal QuestionId: 0x272B, Value: 0x1 { 12 06 2B 27 01 00 }
0x386FA: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x38701: 			End  { 29 02 }
0x38703: 		End  { 29 02 }
0x38705: 		SuppressIf  { 0A 82 }
0x38707: 			EqIdVal QuestionId: 0x11F5, Value: 0x1 { 12 06 F5 11 01 00 }
0x3870D: 			OneOf Prompt: "EC PECI Mode", Help: "Switch eSPI PECI Mode or Legacy PECI mode", QuestionFlags: 0x14, QuestionId: 0x2872, VarStoreId: 0xF101, VarOffset: 0x55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 1C 85 1A 72 28 01 F1 55 00 14 10 00 01 00 }
0x3871E: 				OneOfOption Option: "Legacy PECI mode" Value: 0, Default { 09 07 64 1C 10 00 00 }
0x38725: 				OneOfOption Option: "PECI over eSPI mode" Value: 1 { 09 07 65 1C 00 00 01 }
0x3872C: 			End  { 29 02 }
0x3872E: 		End  { 29 02 }
0x38730: 		OneOf Prompt: "Power Loss Notification Feature", Help: "Enable/Disable Power Loss Notification Feature", QuestionFlags: 0x10, QuestionId: 0x35F, VarStoreId: 0xF101, VarOffset: 0xA9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 6A 1C 6B 1C 5F 03 01 F1 9E 0A 10 10 00 02 00 }
0x38741: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x38748: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3874F: 			OneOfOption Option: "Default" Value: 2, Default, MfgDefault { 09 07 6C 1C 30 00 02 }
0x38756: 		End  { 29 02 }
0x38758: 		CheckBox Prompt: "Device password support", Help: "Support device password feature", QuestionFlags: 0x10, QuestionId: 0x360, VarStoreId: 0xF101, VarOffset: 0x99C, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 5F 1C 60 1C 60 03 01 F1 9C 09 10 01 }
0x38766: 		End  { 29 02 }
0x38768: 		OneOf Prompt: "Pmic Vcc IO Level", Help: "Select the Pmic Vcc IO Voltage Level", QuestionFlags: 0x10, QuestionId: 0x361, VarStoreId: 0xF101, VarOffset: 0x6C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 7C 1B 7D 1B 61 03 01 F1 C3 06 10 10 00 07 00 }
0x38779: 			OneOfOption Option: "Disabled" Value: 7, Default, MfgDefault { 09 07 85 1B 30 00 07 }
0x38780: 			OneOfOption Option: "1.05V" Value: 0 { 09 07 7E 1B 00 00 00 }
0x38787: 			OneOfOption Option: "1.071V" Value: 1 { 09 07 7F 1B 00 00 01 }
0x3878E: 			OneOfOption Option: "1.023V" Value: 2 { 09 07 80 1B 00 00 02 }
0x38795: 			OneOfOption Option: "0.997V" Value: 3 { 09 07 81 1B 00 00 03 }
0x3879C: 			OneOfOption Option: "0.850V" Value: 4 { 09 07 82 1B 00 00 04 }
0x387A3: 			OneOfOption Option: "0.900V" Value: 5 { 09 07 83 1B 00 00 05 }
0x387AA: 			OneOfOption Option: "0.950V" Value: 6 { 09 07 84 1B 00 00 06 }
0x387B1: 		End  { 29 02 }
0x387B3: 		OneOf Prompt: "Pmic Vddq Level", Help: "Select the Pmic Vddq Voltage Level", QuestionFlags: 0x10, QuestionId: 0x362, VarStoreId: 0xF101, VarOffset: 0x6C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x8, Step: 0x0 { 05 91 86 1B 87 1B 62 03 01 F1 C4 06 10 10 00 08 00 }
0x387C4: 			OneOfOption Option: "Disabled" Value: 8, Default, MfgDefault { 09 07 85 1B 30 00 08 }
0x387CB: 			OneOfOption Option: "0" Value: 0 { 09 07 88 1B 00 00 00 }
0x387D2: 			OneOfOption Option: "1" Value: 1 { 09 07 89 1B 00 00 01 }
0x387D9: 			OneOfOption Option: "2" Value: 2 { 09 07 8A 1B 00 00 02 }
0x387E0: 			OneOfOption Option: "3" Value: 3 { 09 07 8B 1B 00 00 03 }
0x387E7: 			OneOfOption Option: "4" Value: 4 { 09 07 8C 1B 00 00 04 }
0x387EE: 			OneOfOption Option: "5" Value: 5 { 09 07 8D 1B 00 00 05 }
0x387F5: 			OneOfOption Option: "6" Value: 6 { 09 07 8E 1B 00 00 06 }
0x387FC: 			OneOfOption Option: "7" Value: 7 { 09 07 8F 1B 00 00 07 }
0x38803: 		End  { 29 02 }
0x38805: 		OneOf Prompt: "CSC Pmic NVM Update Support", Help: "Enable/Disable CastroCove Pmic Nvm Update", QuestionFlags: 0x10, QuestionId: 0x363, VarStoreId: 0xF101, VarOffset: 0x6C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 1B 93 1B 63 03 01 F1 C6 06 10 10 00 01 00 }
0x38816: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3881D: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38824: 		End  { 29 02 }
0x38826: 		SuppressIf  { 0A 82 }
0x38828: 			EqIdVal QuestionId: 0x363, Value: 0x0 { 12 06 63 03 00 00 }
0x3882E: 			OneOf Prompt: "CSC Pmic Customization Nvm Update Support", Help: "Enable/Disable CastroCove Pmic Customization Nvm Update", QuestionFlags: 0x10, QuestionId: 0x364, VarStoreId: 0xF101, VarOffset: 0x6C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 1B 95 1B 64 03 01 F1 C7 06 10 10 00 01 00 }
0x3883F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38846: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3884D: 			End  { 29 02 }
0x3884F: 		End  { 29 02 }
0x38851: 		OneOf Prompt: "Pmic NVM Write Lock Support", Help: "Enable/Disable WarrenCove/CastroCove Pmic Nvm Write Lock", QuestionFlags: 0x10, QuestionId: 0x365, VarStoreId: 0xF101, VarOffset: 0x6C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 96 1B 97 1B 65 03 01 F1 C8 06 10 10 00 01 00 }
0x38862: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38869: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38870: 		End  { 29 02 }
0x38872: 		SuppressIf  { 0A 82 }
0x38874: 			EqIdVal QuestionId: 0x11F4, Value: 0x1 { 12 86 F4 11 01 00 }
0x3887A: 				Not  { 17 02 }
0x3887C: 			End  { 29 02 }
0x3887E: 			Numeric Prompt: "HEBC value", Help: "HEBC value 32bit ", QuestionFlags: 0x0, QuestionId: 0x366, VarStoreId: 0xF101, VarOffset: 0x818, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 6B 1A 6C 1A 66 03 01 F1 18 08 00 12 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x38898: 				Default DefaultId: 0x0 Value: 144371 { 5B 09 00 00 02 F3 33 02 00 }
0x388A1: 			End  { 29 02 }
0x388A3: 		End  { 29 02 }
0x388A5: 		OneOf Prompt: "Pmic SlpS0 VM Support", Help: "Support to auto check Primium PMIC and disable SlpS0 voltage.", QuestionFlags: 0x10, QuestionId: 0x367, VarStoreId: 0xF101, VarOffset: 0x816, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 1B 91 1B 67 03 01 F1 16 08 10 10 00 01 00 }
0x388B6: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x388BD: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x388C4: 		End  { 29 02 }
0x388C6: 		OneOf Prompt: "Power Sharing Manager", Help: "Configure the PSM ACPI objects.", QuestionFlags: 0x10, QuestionId: 0x368, VarStoreId: 0xF101, VarOffset: 0x71F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 1B 9A 1B 68 03 01 F1 1F 07 10 10 00 01 00 }
0x388D7: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x388DE: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x388E5: 		End  { 29 02 }
0x388E7: 		SuppressIf  { 0A 82 }
0x388E9: 			EqIdVal QuestionId: 0x368, Value: 0x0 { 12 06 68 03 00 00 }
0x388EF: 			Numeric Prompt: " Domain Type SPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x369, VarStoreId: 0xF101, VarOffset: 0x720, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 9B 1B 9D 1B 69 03 01 F1 20 07 00 10 01 32 01 }
0x38900: 				Default DefaultId: 0x0 Value: 9 { 5B 06 00 00 00 09 }
0x38906: 			End  { 29 02 }
0x38908: 			Numeric Prompt: " Default Power Limit 1 SPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x36A, VarStoreId: 0xF101, VarOffset: 0x721, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x2710, Step: 0x1 { 07 9A 9E 1B E4 01 6A 03 01 F1 21 07 00 12 01 00 00 00 10 27 00 00 01 00 00 00 }
0x38922: 				Default DefaultId: 0x0 Value: 4000 { 5B 09 00 00 02 A0 0F 00 00 }
0x3892B: 			End  { 29 02 }
0x3892D: 			Numeric Prompt: " Default Time Window 1 SPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x36B, VarStoreId: 0xF101, VarOffset: 0x725, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1 { 07 9A 9F 1B E6 01 6B 03 01 F1 25 07 00 12 01 00 00 00 A0 86 01 00 01 00 00 00 }
0x38947: 				Default DefaultId: 0x0 Value: 30000 { 5B 09 00 00 02 30 75 00 00 }
0x38950: 			End  { 29 02 }
0x38952: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x38959: 			End  { 29 02 }
0x3895B: 			Numeric Prompt: " Domain Type DPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x36C, VarStoreId: 0xF101, VarOffset: 0x729, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 A0 1B 9D 1B 6C 03 01 F1 29 07 00 10 01 32 01 }
0x3896C: 				Default DefaultId: 0x0 Value: 9 { 5B 06 00 00 00 09 }
0x38972: 			End  { 29 02 }
0x38974: 			Numeric Prompt: " Domain Preference DPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x36D, VarStoreId: 0xF101, VarOffset: 0x72A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 A1 1B 9D 1B 6D 03 01 F1 2A 07 00 10 01 32 01 }
0x38985: 				Default DefaultId: 0x0 Value: 9 { 5B 06 00 00 00 09 }
0x3898B: 			End  { 29 02 }
0x3898D: 			Numeric Prompt: " Power Limit Index 1 DPLC", Help: "Index of the specific power limit range information", QuestionFlags: 0x0, QuestionId: 0x36E, VarStoreId: 0xF101, VarOffset: 0x72B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xA, Step: 0x1 { 07 94 A2 1B A3 1B 6E 03 01 F1 2B 07 00 11 00 00 0A 00 01 00 }
0x389A1: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x389A8: 			End  { 29 02 }
0x389AA: 			Numeric Prompt: " Default Power Limit 1 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x36F, VarStoreId: 0xF101, VarOffset: 0x72D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1 { 07 94 A4 1B E4 01 6F 03 01 F1 2D 07 00 11 01 00 10 27 01 00 }
0x389BE: 				Default DefaultId: 0x0 Value: 1200 { 5B 07 00 00 01 B0 04 }
0x389C5: 			End  { 29 02 }
0x389C7: 			Numeric Prompt: " Default Time Window 1 DPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x370, VarStoreId: 0xF101, VarOffset: 0x72F, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1 { 07 9A A5 1B E6 01 70 03 01 F1 2F 07 00 12 01 00 00 00 A0 86 01 00 01 00 00 00 }
0x389E1: 				Default DefaultId: 0x0 Value: 30000 { 5B 09 00 00 02 30 75 00 00 }
0x389EA: 			End  { 29 02 }
0x389EC: 			Numeric Prompt: " Minimum Power Limit 1 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x371, VarStoreId: 0xF101, VarOffset: 0x733, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1 { 07 94 A6 1B E4 01 71 03 01 F1 33 07 00 11 01 00 10 27 01 00 }
0x38A00: 				Default DefaultId: 0x0 Value: 1200 { 5B 07 00 00 01 B0 04 }
0x38A07: 			End  { 29 02 }
0x38A09: 			Numeric Prompt: " Maximum Power Limit 1 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x372, VarStoreId: 0xF101, VarOffset: 0x735, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1 { 07 94 A7 1B E4 01 72 03 01 F1 35 07 00 11 01 00 10 27 01 00 }
0x38A1D: 				Default DefaultId: 0x0 Value: 1200 { 5B 07 00 00 01 B0 04 }
0x38A24: 			End  { 29 02 }
0x38A26: 			Numeric Prompt: " Maximum Time Window 1 DPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x373, VarStoreId: 0xF101, VarOffset: 0x737, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1 { 07 94 A8 1B E6 01 73 03 01 F1 37 07 00 11 01 00 10 27 01 00 }
0x38A3A: 				Default DefaultId: 0x0 Value: 1000 { 5B 07 00 00 01 E8 03 }
0x38A41: 			End  { 29 02 }
0x38A43: 		End  { 29 02 }
0x38A45: 		OneOf Prompt: "Enable FFU Support", Help: "Enable/Disable FFU Support.", QuestionFlags: 0x10, QuestionId: 0x374, VarStoreId: 0xF101, VarOffset: 0x794, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 1B AA 1B 74 03 01 F1 94 07 10 10 00 01 00 }
0x38A56: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38A5D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38A64: 		End  { 29 02 }
0x38A66: 		OneOf Prompt: "HID Event Filter Driver", Help: "Enables/Disables HID Event Filter Driver interface to OS.", QuestionFlags: 0x10, QuestionId: 0x375, VarStoreId: 0xF101, VarOffset: 0x815, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 1C 47 1C 75 03 01 F1 15 08 10 10 00 01 00 }
0x38A77: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38A7E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38A85: 		End  { 29 02 }
0x38A87: 		SuppressIf  { 0A 82 }
0x38A89: 			EqIdVal QuestionId: 0x1DF, Value: 0x0 { 12 06 DF 01 00 00 }
0x38A8F: 			Numeric Prompt: "Delay to wait for WWAN device to be ready before SAR reset.", Help: "Value between 0-255 seconds. Default is 8. Will result in Responsiveness impact. ", QuestionFlags: 0x0, QuestionId: 0x376, VarStoreId: 0xF101, VarOffset: 0x81C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 4D 1C 4E 1C 76 03 01 F1 1C 08 00 10 00 FF 01 }
0x38AA0: 				Default DefaultId: 0x0 Value: 8 { 5B 06 00 00 00 08 }
0x38AA6: 			End  { 29 02 }
0x38AA8: 		End  { 29 02 }
0x38AAA: 		OneOf Prompt: "System Time and Alarm Source", Help: "Select source of system time and alarm functions. ACPI Time and Alarm (default, legacy RTC disabled) or Legacy RTC support only", QuestionFlags: 0x10, QuestionId: 0x377, VarStoreId: 0xF101, VarOffset: 0x853, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4F 1C 50 1C 77 03 01 F1 53 08 10 10 00 01 00 }
0x38ABB: 			OneOfOption Option: "ACPI Time and Alarm Device" Value: 0, Default, MfgDefault { 09 07 51 1C 30 00 00 }
0x38AC2: 			OneOfOption Option: "Legacy RTC" Value: 1 { 09 07 52 1C 00 00 01 }
0x38AC9: 		End  { 29 02 }
0x38ACB: 		SuppressIf  { 0A 82 }
0x38ACD: 			EqIdVal QuestionId: 0x11F3, Value: 0x1 { 12 86 F3 11 01 00 }
0x38AD3: 				Not  { 17 02 }
0x38AD5: 			End  { 29 02 }
0x38AD7: 			OneOf Prompt: "Enable xdpclock ", Help: "Enable xdpclock routing on slot1 CMU_ONE_DWORD0 bits muxsel_itpxdp ", QuestionFlags: 0x10, QuestionId: 0x378, VarStoreId: 0xF101, VarOffset: 0x85E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 57 1C 58 1C 78 03 01 F1 5E 08 10 10 00 01 00 }
0x38AE8: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x38AEF: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x38AF6: 			End  { 29 02 }
0x38AF8: 		End  { 29 02 }
0x38AFA: 		OneOf Prompt: "DG Platform Support", Help: "DG is supported as MotherBoard Down OR Add In Card", QuestionFlags: 0x10, QuestionId: 0x379, VarStoreId: 0xF101, VarOffset: 0xAA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 59 1C 5A 1C 79 03 01 F1 A6 0A 10 10 00 01 00 }
0x38B0B: 			OneOfOption Option: "Add In Card" Value: 0, Default, MfgDefault { 09 07 5B 1C 30 00 00 }
0x38B12: 			OneOfOption Option: "MB Down" Value: 1 { 09 07 5C 1C 00 00 01 }
0x38B19: 		End  { 29 02 }
0x38B1B: 		OneOf Prompt: "Enable PowerMeter", Help: "", QuestionFlags: 0x10, QuestionId: 0x37A, VarStoreId: 0xF101, VarOffset: 0x86C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5D 1C 5E 1C 7A 03 01 F1 6C 08 10 10 00 01 00 }
0x38B2C: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38B33: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38B3A: 		End  { 29 02 }
0x38B3C: 		OneOf Prompt: "Intel Trusted Device Setup Boot", Help: "Enables/Disables a Intel Trusted Device Setup Boot on the next boot", QuestionFlags: 0x10, QuestionId: 0x37B, VarStoreId: 0xF101, VarOffset: 0x854, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4A 1C 4B 1C 7B 03 01 F1 54 08 10 10 00 01 00 }
0x38B4D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38B54: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x38B5B: 		End  { 29 02 }
0x38B5D: 		OneOf Prompt: "MPDT Support", Help: "Enable(Sensor_BOM1,Sensor_BOM2 and Sensor_BOM1 with Companion Chip)/Disable MPDT Support in BIOS", QuestionFlags: 0x10, QuestionId: 0x37C, VarStoreId: 0xF101, VarOffset: 0xAD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 E9 1F EA 1F 7C 03 01 F1 D9 0A 10 10 00 03 00 }
0x38B6E: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x38B75: 			OneOfOption Option: "Sensor_BOM1" Value: 1 { 09 07 EB 1F 00 00 01 }
0x38B7C: 			OneOfOption Option: "Sensor_BOM2" Value: 2 { 09 07 EC 1F 00 00 02 }
0x38B83: 			OneOfOption Option: "Sensor_BOM1 with Companion Chip" Value: 3 { 09 07 ED 1F 00 00 03 }
0x38B8A: 		End  { 29 02 }
0x38B8C: 		SuppressIf  { 0A 82 }
0x38B8E: 			EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 86 42 11 02 00 }
0x38B94: 				Not  { 17 02 }
0x38B96: 			End  { 29 02 }
0x38B98: 			SuppressIf  { 0A 82 }
0x38B9A: 				EqIdVal QuestionId: 0xA7F, Value: 0x1 { 12 86 7F 0A 01 00 }
0x38BA0: 					Not  { 17 02 }
0x38BA2: 				End  { 29 02 }
0x38BA4: 				Numeric Prompt: "Aux Rail Budget (Watt)", Help: "Total aux rail budget avaiable per RVP. Value must be between 0 (Min Watt) - 10 (Max Watt)", QuestionFlags: 0x10, QuestionId: 0x37D, VarStoreId: 0xF101, VarOffset: 0xAA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 80 1C 81 1C 7D 03 01 F1 A4 0A 10 10 00 0A 01 }
0x38BB5: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x38BBA: 						Value  { 5A 82 }
0x38BBC: 							Uint64 Value: 0x6 { 45 0A 06 00 00 00 00 00 00 00 }
0x38BC6: 						End  { 29 02 }
0x38BC8: 					End  { 29 02 }
0x38BCA: 				End  { 29 02 }
0x38BCC: 			End  { 29 02 }
0x38BCE: 		End  { 29 02 }
0x38BD0: 		Ref Prompt: "VTIO", Help: "Configure settings for VTIO", QuestionFlags: 0x0, QuestionId: 0x37E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x287D { 0F 0F AB 1B AC 1B 7E 03 00 00 FF FF 00 7D 28 }
0x38BDF: 		Ref Prompt: "TCSS Platform Setting", Help: "Configure TCSS Platform Setting", QuestionFlags: 0x0, QuestionId: 0x37F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2880 { 0F 0F E2 1B E3 1B 7F 03 00 00 FF FF 00 80 28 }
0x38BEE: 	End  { 29 02 }
0x38BF0: 	Form FormId: 0x287C, Title: "ACPI D3Cold settings" { 01 86 7C 28 18 1C }
0x38BF6: 		Subtitle Prompt: "ACPI D3Cold settings", Help: "", Flags: 0x0 { 02 87 18 1C 00 00 00 }
0x38BFD: 		End  { 29 02 }
0x38BFF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x38C06: 		End  { 29 02 }
0x38C08: 		OneOf Prompt: "ACPI D3Cold Support", Help: "Enable/Disable ACPI D3Cold support to be executed on D3 entry and exit

Note: Disable it would affect the Storage D3 setting", QuestionFlags: 0x14, QuestionId: 0x2873, VarStoreId: 0xF101, VarOffset: 0x700, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 1C 15 1C 73 28 01 F1 00 07 14 10 00 01 00 }
0x38C19: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x38C20: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x38C27: 		End  { 29 02 }
0x38C29: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x38C30: 		End  { 29 02 }
0x38C32: 		SuppressIf  { 0A 82 }
0x38C34: 			EqIdVal QuestionId: 0x2873, Value: 0x0 { 12 06 73 28 00 00 }
0x38C3A: 			Numeric Prompt: "VR Ramp up delay", Help: "Delay between subsequent VR ramp ups if they are all Turn ON at the same time", QuestionFlags: 0x0, QuestionId: 0x380, VarStoreId: 0xF101, VarOffset: 0x70C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x64, Step: 0x10 { 07 94 19 1C 1A 1C 80 03 01 F1 0C 07 00 11 00 00 64 00 10 00 }
0x38C4E: 				Default DefaultId: 0x0 Value: 16 { 5B 07 00 00 01 10 00 }
0x38C55: 			End  { 29 02 }
0x38C57: 			Numeric Prompt: "PCIE Slot 5 Device Power-on delay in ms", Help: "Delay between applying core power and Deasserting PERST#", QuestionFlags: 0x0, QuestionId: 0x381, VarStoreId: 0xF101, VarOffset: 0x701, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x10 { 07 91 1B 1C 1C 1C 81 03 01 F1 01 07 00 10 00 C8 10 }
0x38C68: 				Default DefaultId: 0x0 Value: 100 { 5B 06 00 00 00 64 }
0x38C6E: 			End  { 29 02 }
0x38C70: 			SuppressIf  { 0A 82 }
0x38C72: 				EqIdVal QuestionId: 0xF0F, Value: 0x0 { 12 06 0F 0F 00 00 }
0x38C78: 				Numeric Prompt: "Audio Delay", Help: "Delay after applying power to HD Audio(Realtek) codec device.", QuestionFlags: 0x0, QuestionId: 0x382, VarStoreId: 0xF101, VarOffset: 0x704, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x10 { 07 94 1D 1C 1E 1C 82 03 01 F1 04 07 00 11 00 00 E8 03 10 00 }
0x38C8C: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x38C93: 				End  { 29 02 }
0x38C95: 			End  { 29 02 }
0x38C97: 			Numeric Prompt: "SensorHub", Help: "Delay after applying power to SensorHub device.", QuestionFlags: 0x0, QuestionId: 0x383, VarStoreId: 0xF101, VarOffset: 0x70A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x10 { 07 94 23 1C 24 1C 83 03 01 F1 0A 07 00 11 00 00 E8 03 10 00 }
0x38CAB: 				Default DefaultId: 0x0 Value: 68 { 5B 07 00 00 01 44 00 }
0x38CB2: 			End  { 29 02 }
0x38CB4: 			Numeric Prompt: "TouchPad", Help: "Delay after applying power to TouchPad device.", QuestionFlags: 0x0, QuestionId: 0x384, VarStoreId: 0xF101, VarOffset: 0x706, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x10 { 07 94 1F 1C 20 1C 84 03 01 F1 06 07 00 11 00 00 E8 03 10 00 }
0x38CC8: 				Default DefaultId: 0x0 Value: 68 { 5B 07 00 00 01 44 00 }
0x38CCF: 			End  { 29 02 }
0x38CD1: 			Numeric Prompt: "TouchPanel", Help: "Delay in PR _ON after applying power to TouchPanel device.", QuestionFlags: 0x0, QuestionId: 0x385, VarStoreId: 0xF101, VarOffset: 0x708, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x10 { 07 94 21 1C 22 1C 85 03 01 F1 08 07 00 11 00 00 E8 03 10 00 }
0x38CE5: 				Default DefaultId: 0x0 Value: 68 { 5B 07 00 00 01 44 00 }
0x38CEC: 			End  { 29 02 }
0x38CEE: 			OneOf Prompt: "P-state Capping", Help: "Set _PPC and send ACPI notification", QuestionFlags: 0x10, QuestionId: 0x386, VarStoreId: 0xF101, VarOffset: 0x70E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 25 1C 26 1C 86 03 01 F1 0E 07 10 10 00 01 00 }
0x38CFF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38D06: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38D0D: 			End  { 29 02 }
0x38D0F: 			OneOf Prompt: "USB Port 1", Help: "USB RTD3 support. Super Speed : USB3.0 devices will be exposed as RTD3 capable. High Speed: USB2.0 devices will be exposed as RTD3 capable. Disabled : USB RTD3 support disabled.

 For SawtoothPeak USB Port1(Below) is Superspeed and Port2(Top) is HighSpeed. Check respective board configuration to know about USB port position.", QuestionFlags: 0x10, QuestionId: 0x387, VarStoreId: 0xF101, VarOffset: 0x702, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 36 1C 3A 1C 87 03 01 F1 02 07 10 10 00 02 00 }
0x38D20: 				OneOfOption Option: "High Speed" Value: 1 { 09 07 38 1C 00 00 01 }
0x38D27: 				OneOfOption Option: "Super Speed" Value: 2 { 09 07 39 1C 00 00 02 }
0x38D2E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38D35: 			End  { 29 02 }
0x38D37: 			OneOf Prompt: "USB Port 2", Help: "USB RTD3 support. Super Speed : USB3.0 devices will be exposed as RTD3 capable. High Speed: USB2.0 devices will be exposed as RTD3 capable. Disabled : USB RTD3 support disabled.

 For SawtoothPeak USB Port1(Below) is Superspeed and Port2(Top) is HighSpeed. Check respective board configuration to know about USB port position.", QuestionFlags: 0x10, QuestionId: 0x388, VarStoreId: 0xF101, VarOffset: 0x703, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 37 1C 3A 1C 88 03 01 F1 03 07 10 10 00 04 00 }
0x38D48: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38D4F: 				OneOfOption Option: "High Speed" Value: 1 { 09 07 38 1C 00 00 01 }
0x38D56: 				OneOfOption Option: "Super Speed" Value: 2 { 09 07 39 1C 00 00 02 }
0x38D5D: 				SuppressIf  { 0A 82 }
0x38D5F: 					EqIdVal QuestionId: 0x38A, Value: 0x0 { 12 06 8A 03 00 00 }
0x38D65: 					OneOfOption Option: "Super Speed WWAN" Value: 4 { 09 07 4C 1C 00 00 04 }
0x38D6C: 				End  { 29 02 }
0x38D6E: 			End  { 29 02 }
0x38D70: 			SuppressIf  { 0A 82 }
0x38D72: 				EqIdVal QuestionId: 0x11F2, Value: 0x1 { 12 06 F2 11 01 00 }
0x38D78: 				OneOf Prompt: "ZPODD", Help: "Zero Power ODD option is applicable only for the board with ZPODD support.", QuestionFlags: 0x10, QuestionId: 0x389, VarStoreId: 0xF101, VarOffset: 0x710, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 1C 28 1C 89 03 01 F1 10 07 10 10 00 01 00 }
0x38D89: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38D90: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38D97: 				End  { 29 02 }
0x38D99: 			End  { 29 02 }
0x38D9B: 			GrayOutIf  { 19 82 }
0x38D9D: 				EqIdVal QuestionId: 0x1DF, Value: 0x0 { 12 06 DF 01 00 00 }
0x38DA3: 				OneOf Prompt: "WWAN", Help: "Enable/Disable RTD3 support for WWAN", QuestionFlags: 0x10, QuestionId: 0x38A, VarStoreId: 0xF101, VarOffset: 0x711, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 29 1C 2A 1C 8A 03 01 F1 11 07 10 10 00 03 00 }
0x38DB4: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x38DBB: 					OneOfOption Option: "D0/L1.2" Value: 1 { 09 07 2C 1C 00 00 01 }
0x38DC2: 					OneOfOption Option: "D3/L2" Value: 3, Default, MfgDefault { 09 07 2B 1C 30 00 03 }
0x38DC9: 				End  { 29 02 }
0x38DCB: 			End  { 29 02 }
0x38DCD: 			OneOf Prompt: "Sata Port 0", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x38B, VarStoreId: 0xF101, VarOffset: 0x712, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 1C 35 1C 8B 03 01 F1 12 07 10 10 00 01 00 }
0x38DDE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38DE5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38DEC: 			End  { 29 02 }
0x38DEE: 			OneOf Prompt: "Sata Port 1", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x38C, VarStoreId: 0xF101, VarOffset: 0x713, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 1C 35 1C 8C 03 01 F1 13 07 10 10 00 01 00 }
0x38DFF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38E06: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38E0D: 			End  { 29 02 }
0x38E0F: 			OneOf Prompt: "Sata Port 2", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x38D, VarStoreId: 0xF101, VarOffset: 0x714, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 1C 35 1C 8D 03 01 F1 14 07 10 10 00 01 00 }
0x38E20: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38E27: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38E2E: 			End  { 29 02 }
0x38E30: 			OneOf Prompt: "Sata Port 3", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x38E, VarStoreId: 0xF101, VarOffset: 0x715, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 1C 35 1C 8E 03 01 F1 15 07 10 10 00 01 00 }
0x38E41: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38E48: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38E4F: 			End  { 29 02 }
0x38E51: 			OneOf Prompt: "Sata Port 4", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x38F, VarStoreId: 0xF101, VarOffset: 0x716, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 1C 35 1C 8F 03 01 F1 16 07 10 10 00 01 00 }
0x38E62: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38E69: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38E70: 			End  { 29 02 }
0x38E72: 			OneOf Prompt: "Sata Port 5", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x390, VarStoreId: 0xF101, VarOffset: 0x717, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 1C 35 1C 90 03 01 F1 17 07 10 10 00 01 00 }
0x38E83: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38E8A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38E91: 			End  { 29 02 }
0x38E93: 			OneOf Prompt: "Sata Port 6", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x391, VarStoreId: 0xF101, VarOffset: 0x718, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 1C 35 1C 91 03 01 F1 18 07 10 10 00 01 00 }
0x38EA4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38EAB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38EB2: 			End  { 29 02 }
0x38EB4: 			OneOf Prompt: "Sata Port 7", Help: "Setup option to control the SATA port RTD3 functionality", QuestionFlags: 0x10, QuestionId: 0x392, VarStoreId: 0xF101, VarOffset: 0x719, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 1C 35 1C 92 03 01 F1 19 07 10 10 00 01 00 }
0x38EC5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38ECC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38ED3: 			End  { 29 02 }
0x38ED5: 			SuppressIf  { 0A 82 }
0x38ED7: 				EqIdVal QuestionId: 0x289F, Value: 0x1 { 12 86 9F 28 01 00 }
0x38EDD: 					Not  { 17 02 }
0x38EDF: 				End  { 29 02 }
0x38EE1: 				GrayOutIf  { 19 82 }
0x38EE3: 					EqIdVal QuestionId: 0x28A4, Value: 0x2 { 12 86 A4 28 02 00 }
0x38EE9: 						Not  { 17 02 }
0x38EEB: 					End  { 29 02 }
0x38EED: 					OneOf Prompt: "DTBT RTD3 Enable", Help: "Enables or Disables DTBT RTD3 support", QuestionFlags: 0x10, QuestionId: 0x393, VarStoreId: 0xF101, VarOffset: 0x99E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3B 1C 3C 1C 93 03 01 F1 9E 09 10 10 00 01 00 }
0x38EFE: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38F05: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38F0C: 					End  { 29 02 }
0x38F0E: 				End  { 29 02 }
0x38F10: 				SuppressIf  { 0A 82 }
0x38F12: 					EqIdVal QuestionId: 0x393, Value: 0x1 { 12 86 93 03 01 00 }
0x38F18: 						Not  { 17 02 }
0x38F1A: 					End  { 29 02 }
0x38F1C: 					OneOf Prompt: "TBT Power-off delay Optimization", Help: "Enables or Disables TBT Power-off delay Optimization support", QuestionFlags: 0x10, QuestionId: 0x394, VarStoreId: 0xF101, VarOffset: 0xAC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 1C 3E 1C 94 03 01 F1 C7 0A 10 10 00 01 00 }
0x38F2D: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x38F34: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x38F3B: 					End  { 29 02 }
0x38F3D: 					Numeric Prompt: "TBT Power-off delay in ms", Help: "Specify delay in ms necessary after removing TBT power", QuestionFlags: 0x0, QuestionId: 0x395, VarStoreId: 0xF101, VarOffset: 0x99F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3A98, Step: 0x1 { 07 94 3F 1C 40 1C 95 03 01 F1 9F 09 00 11 00 00 98 3A 01 00 }
0x38F51: 						Default DefaultId: 0x0 Value: 5000 { 5B 07 00 00 01 88 13 }
0x38F58: 					End  { 29 02 }
0x38F5A: 					OneOf Prompt: "DTBT RTD3 CLKREQ Enable", Help: "Enables or Disables DTBT RTD3 CLKREQ mask", QuestionFlags: 0x10, QuestionId: 0x396, VarStoreId: 0xF101, VarOffset: 0x9A1, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x1, Step: 0x0 { 05 9A 41 1C 42 1C 96 03 01 F1 A1 09 10 12 00 00 00 00 01 00 00 00 00 00 00 00 }
0x38F74: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 0A 04 00 32 02 00 00 00 00 }
0x38F7E: 						OneOfOption Option: "Enabled" Value: 1 { 09 0A 03 00 02 02 01 00 00 00 }
0x38F88: 					End  { 29 02 }
0x38F8A: 					Numeric Prompt: "DTBT RTD3 CLKREQ Delay value", Help: "Specify delay in ms necessary after CLKREQ mask state is changed.", QuestionFlags: 0x0, QuestionId: 0x397, VarStoreId: 0xF101, VarOffset: 0x9A5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 43 1C 44 1C 97 03 01 F1 A5 09 00 11 00 00 D0 07 01 00 }
0x38F9E: 						Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x38FA5: 					End  { 29 02 }
0x38FA7: 				End  { 29 02 }
0x38FA9: 			End  { 29 02 }
0x38FAB: 		End  { 29 02 }
0x38FAD: 	End  { 29 02 }
0x38FAF: 	Form FormId: 0x287D, Title: "VTIO" { 01 86 7D 28 AB 1B }
0x38FB5: 		Subtitle Prompt: "VTIO", Help: "", Flags: 0x0 { 02 87 AD 1B 00 00 00 }
0x38FBC: 		End  { 29 02 }
0x38FBE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x38FC5: 		End  { 29 02 }
0x38FC7: 		OneOf Prompt: "Enable VTIO Support", Help: "Enable/Disable VTIO Support.", QuestionFlags: 0x10, QuestionId: 0x398, VarStoreId: 0xF101, VarOffset: 0x82B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 1B AF 1B 98 03 01 F1 2B 08 10 10 00 01 00 }
0x38FD8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x38FDF: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x38FE6: 		End  { 29 02 }
0x38FE8: 		SuppressIf  { 0A 82 }
0x38FEA: 			EqIdVal QuestionId: 0x398, Value: 0x0 { 12 06 98 03 00 00 }
0x38FF0: 			SuppressIf  { 0A 82 }
0x38FF2: 				True  { 46 02 }
0x38FF4: 				OneOf Prompt: "Expose CIO2 SDEV Entry", Help: "CIO2 Entry in SDEV table will be exposed based on this option", QuestionFlags: 0x10, QuestionId: 0x399, VarStoreId: 0xF101, VarOffset: 0x82C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 1B B6 1B 99 03 01 F1 2C 08 10 10 00 01 00 }
0x39005: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3900C: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39013: 				End  { 29 02 }
0x39015: 			End  { 29 02 }
0x39017: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3901E: 			End  { 29 02 }
0x39020: 			OneOf Prompt: "Expose ISP SDEV Entry", Help: "ISP Entry in SDEV table will be exposed based on this option", QuestionFlags: 0x10, QuestionId: 0x39A, VarStoreId: 0xF101, VarOffset: 0x82D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 1B B8 1B 9A 03 01 F1 2D 08 10 10 00 01 00 }
0x39031: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39038: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3903F: 			End  { 29 02 }
0x39041: 			SuppressIf  { 0A 82 }
0x39043: 				EqIdVal QuestionId: 0x39A, Value: 0x0 { 12 06 9A 03 00 00 }
0x39049: 				Numeric Prompt: "  Number of Sensor Entries", Help: "An array of Sensors Entries", QuestionFlags: 0x10, QuestionId: 0x39B, VarStoreId: 0xF101, VarOffset: 0x834, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x2, Step: 0x0 { 07 94 B0 1B B1 1B 9B 03 01 F1 34 08 10 21 00 00 02 00 00 00 }
0x3905D: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39062: 						Value  { 5A 82 }
0x39064: 							Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x3906E: 						End  { 29 02 }
0x39070: 					End  { 29 02 }
0x39072: 				End  { 29 02 }
0x39074: 				SuppressIf  { 0A 82 }
0x39076: 					EqIdVal QuestionId: 0x39B, Value: 0x0 { 12 06 9B 03 00 00 }
0x3907C: 					Numeric Prompt: "  Flags", Help: "Enter HEX value

BIT[0] - Allow handoff to non-secure OS
", QuestionFlags: 0x10, QuestionId: 0x39C, VarStoreId: 0xF101, VarOffset: 0x997, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 07 91 73 1C 74 1C 9C 03 01 F1 97 09 10 20 00 01 00 }
0x3908D: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39092: 							Value  { 5A 82 }
0x39094: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3909E: 							End  { 29 02 }
0x390A0: 						End  { 29 02 }
0x390A2: 					End  { 29 02 }
0x390A4: 					Numeric Prompt: "  Sensor Entry 1", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x39D, VarStoreId: 0xF101, VarOffset: 0x83E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B2 1B B4 1B 9D 03 01 F1 3E 08 10 21 00 00 FF FF 00 00 }
0x390B8: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x390BD: 							Value  { 5A 82 }
0x390BF: 								Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x390C9: 							End  { 29 02 }
0x390CB: 						End  { 29 02 }
0x390CD: 					End  { 29 02 }
0x390CF: 				End  { 29 02 }
0x390D1: 				SuppressIf  { 0A 82 }
0x390D3: 					QuestionRef1 QuestionId: 0x39B { 40 84 9B 03 }
0x390D7: 						Uint8 Value: 0x1 { 42 03 01 }
0x390DA: 						LessEqual  { 34 02 }
0x390DC: 					End  { 29 02 }
0x390DE: 					Numeric Prompt: "  Sensor Entry 2", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x39E, VarStoreId: 0xF101, VarOffset: 0x848, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B3 1B B4 1B 9E 03 01 F1 48 08 10 21 00 00 FF FF 00 00 }
0x390F2: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x390F7: 							Value  { 5A 82 }
0x390F9: 								Uint64 Value: 0x85 { 45 0A 85 00 00 00 00 00 00 00 }
0x39103: 							End  { 29 02 }
0x39105: 						End  { 29 02 }
0x39107: 					End  { 29 02 }
0x39109: 				End  { 29 02 }
0x3910B: 			End  { 29 02 }
0x3910D: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x39114: 			End  { 29 02 }
0x39116: 			OneOf Prompt: "Expose HECI SDEV Entry", Help: "HECI Entry in SDEV table will be exposed based on this option", QuestionFlags: 0x10, QuestionId: 0x39F, VarStoreId: 0xF101, VarOffset: 0x82E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 1B BA 1B 9F 03 01 F1 2E 08 10 10 00 01 00 }
0x39127: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3912E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39135: 			End  { 29 02 }
0x39137: 			SuppressIf  { 0A 82 }
0x39139: 				EqIdVal QuestionId: 0x39F, Value: 0x0 { 12 06 9F 03 00 00 }
0x3913F: 				Numeric Prompt: "  Number of Sensor Entries", Help: "An array of Sensors Entries", QuestionFlags: 0x10, QuestionId: 0x3A0, VarStoreId: 0xF101, VarOffset: 0x836, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x2, Step: 0x0 { 07 94 8C 1C B1 1B A0 03 01 F1 36 08 10 21 00 00 02 00 00 00 }
0x39153: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39158: 						Value  { 5A 82 }
0x3915A: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39164: 						End  { 29 02 }
0x39166: 					End  { 29 02 }
0x39168: 				End  { 29 02 }
0x3916A: 				SuppressIf  { 0A 82 }
0x3916C: 					EqIdVal QuestionId: 0x3A0, Value: 0x0 { 12 06 A0 03 00 00 }
0x39172: 					Numeric Prompt: "  Flags", Help: "Enter HEX value

BIT[0] - Allow handoff to non-secure OS
", QuestionFlags: 0x10, QuestionId: 0x3A1, VarStoreId: 0xF101, VarOffset: 0x998, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 07 91 8D 1C 74 1C A1 03 01 F1 98 09 10 20 00 01 00 }
0x39183: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39188: 							Value  { 5A 82 }
0x3918A: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39194: 							End  { 29 02 }
0x39196: 						End  { 29 02 }
0x39198: 					End  { 29 02 }
0x3919A: 					Numeric Prompt: "  Sensor Entry 1", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x3A2, VarStoreId: 0xF101, VarOffset: 0x840, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 8E 1C B4 1B A2 03 01 F1 40 08 10 21 00 00 FF FF 00 00 }
0x391AE: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x391B3: 							Value  { 5A 82 }
0x391B5: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x391BF: 							End  { 29 02 }
0x391C1: 						End  { 29 02 }
0x391C3: 					End  { 29 02 }
0x391C5: 				End  { 29 02 }
0x391C7: 				SuppressIf  { 0A 82 }
0x391C9: 					QuestionRef1 QuestionId: 0x3A0 { 40 84 A0 03 }
0x391CD: 						Uint8 Value: 0x1 { 42 03 01 }
0x391D0: 						LessEqual  { 34 02 }
0x391D2: 					End  { 29 02 }
0x391D4: 					Numeric Prompt: "  Sensor Entry 2", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x3A3, VarStoreId: 0xF101, VarOffset: 0x84A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 8F 1C B4 1B A3 03 01 F1 4A 08 10 21 00 00 FF FF 00 00 }
0x391E8: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x391ED: 							Value  { 5A 82 }
0x391EF: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x391F9: 							End  { 29 02 }
0x391FB: 						End  { 29 02 }
0x391FD: 					End  { 29 02 }
0x391FF: 				End  { 29 02 }
0x39201: 			End  { 29 02 }
0x39203: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3920A: 			End  { 29 02 }
0x3920C: 			OneOf Prompt: "Expose SPI1 Dev 1E Fun 2 SDEV Entry", Help: "SPI1 Entry in SDEV table will be exposed based on this option", QuestionFlags: 0x10, QuestionId: 0x3A4, VarStoreId: 0xF101, VarOffset: 0x82F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 1B BC 1B A4 03 01 F1 2F 08 10 10 00 01 00 }
0x3921D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39224: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3922B: 			End  { 29 02 }
0x3922D: 			SuppressIf  { 0A 82 }
0x3922F: 				EqIdVal QuestionId: 0x3A4, Value: 0x0 { 12 06 A4 03 00 00 }
0x39235: 				Numeric Prompt: "  Number of Sensor Entries", Help: "An array of Sensors Entries", QuestionFlags: 0x10, QuestionId: 0x3A5, VarStoreId: 0xF101, VarOffset: 0x838, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x2, Step: 0x0 { 07 94 90 1C B1 1B A5 03 01 F1 38 08 10 21 00 00 02 00 00 00 }
0x39249: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3924E: 						Value  { 5A 82 }
0x39250: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3925A: 						End  { 29 02 }
0x3925C: 					End  { 29 02 }
0x3925E: 				End  { 29 02 }
0x39260: 				SuppressIf  { 0A 82 }
0x39262: 					EqIdVal QuestionId: 0x3A5, Value: 0x0 { 12 06 A5 03 00 00 }
0x39268: 					Numeric Prompt: "  Flags", Help: "Enter HEX value

BIT[0] - Allow handoff to non-secure OS
", QuestionFlags: 0x10, QuestionId: 0x3A6, VarStoreId: 0xF101, VarOffset: 0x999, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 07 91 91 1C 74 1C A6 03 01 F1 99 09 10 20 00 01 00 }
0x39279: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3927E: 							Value  { 5A 82 }
0x39280: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3928A: 							End  { 29 02 }
0x3928C: 						End  { 29 02 }
0x3928E: 					End  { 29 02 }
0x39290: 					Numeric Prompt: "  Sensor Entry 1", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x3A7, VarStoreId: 0xF101, VarOffset: 0x842, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 92 1C B4 1B A7 03 01 F1 42 08 10 21 00 00 FF FF 00 00 }
0x392A4: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x392A9: 							Value  { 5A 82 }
0x392AB: 								Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x392B5: 							End  { 29 02 }
0x392B7: 						End  { 29 02 }
0x392B9: 					End  { 29 02 }
0x392BB: 				End  { 29 02 }
0x392BD: 				SuppressIf  { 0A 82 }
0x392BF: 					QuestionRef1 QuestionId: 0x3A5 { 40 84 A5 03 }
0x392C3: 						Uint8 Value: 0x1 { 42 03 01 }
0x392C6: 						LessEqual  { 34 02 }
0x392C8: 					End  { 29 02 }
0x392CA: 					Numeric Prompt: "  Sensor Entry 2", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x3A8, VarStoreId: 0xF101, VarOffset: 0x84C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 93 1C B4 1B A8 03 01 F1 4C 08 10 21 00 00 FF FF 00 00 }
0x392DE: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x392E3: 							Value  { 5A 82 }
0x392E5: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x392EF: 							End  { 29 02 }
0x392F1: 						End  { 29 02 }
0x392F3: 					End  { 29 02 }
0x392F5: 				End  { 29 02 }
0x392F7: 			End  { 29 02 }
0x392F9: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x39300: 			End  { 29 02 }
0x39302: 			OneOf Prompt: "Expose SPI2 Dev 1E Fun 3 SDEV Entry", Help: "SPI2 Entry in SDEV table will be exposed based on this option", QuestionFlags: 0x10, QuestionId: 0x3A9, VarStoreId: 0xF101, VarOffset: 0x830, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 1B BE 1B A9 03 01 F1 30 08 10 10 00 01 00 }
0x39313: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3931A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39321: 			End  { 29 02 }
0x39323: 			SuppressIf  { 0A 82 }
0x39325: 				EqIdVal QuestionId: 0x3A9, Value: 0x0 { 12 06 A9 03 00 00 }
0x3932B: 				Numeric Prompt: "  Number of Sensor Entries", Help: "An array of Sensors Entries", QuestionFlags: 0x10, QuestionId: 0x3AA, VarStoreId: 0xF101, VarOffset: 0x83A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x2, Step: 0x0 { 07 94 94 1C B1 1B AA 03 01 F1 3A 08 10 21 00 00 02 00 00 00 }
0x3933F: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39344: 						Value  { 5A 82 }
0x39346: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x39350: 						End  { 29 02 }
0x39352: 					End  { 29 02 }
0x39354: 				End  { 29 02 }
0x39356: 				SuppressIf  { 0A 82 }
0x39358: 					EqIdVal QuestionId: 0x3AA, Value: 0x0 { 12 06 AA 03 00 00 }
0x3935E: 					Numeric Prompt: "  Flags", Help: "Enter HEX value

BIT[0] - Allow handoff to non-secure OS
", QuestionFlags: 0x10, QuestionId: 0x3AB, VarStoreId: 0xF101, VarOffset: 0x99A, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 07 91 95 1C 74 1C AB 03 01 F1 9A 09 10 20 00 01 00 }
0x3936F: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39374: 							Value  { 5A 82 }
0x39376: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39380: 							End  { 29 02 }
0x39382: 						End  { 29 02 }
0x39384: 					End  { 29 02 }
0x39386: 					Numeric Prompt: "  Sensor Entry 1", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x3AC, VarStoreId: 0xF101, VarOffset: 0x844, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 96 1C B4 1B AC 03 01 F1 44 08 10 21 00 00 FF FF 00 00 }
0x3939A: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3939F: 							Value  { 5A 82 }
0x393A1: 								Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x393AB: 							End  { 29 02 }
0x393AD: 						End  { 29 02 }
0x393AF: 					End  { 29 02 }
0x393B1: 				End  { 29 02 }
0x393B3: 				SuppressIf  { 0A 82 }
0x393B5: 					QuestionRef1 QuestionId: 0x3AA { 40 84 AA 03 }
0x393B9: 						Uint8 Value: 0x1 { 42 03 01 }
0x393BC: 						LessEqual  { 34 02 }
0x393BE: 					End  { 29 02 }
0x393C0: 					Numeric Prompt: "  Sensor Entry 2", Help: "Enter HEX value

BIT[8:7] - Camera type
BIT[6]   - Plug-N-Play supported
BIT[5:2] - Port ID
BIT[1]   - Privacy Enabled Sensor present
BIT[0]   - Embedded Sensor present
", QuestionFlags: 0x10, QuestionId: 0x3AD, VarStoreId: 0xF101, VarOffset: 0x84E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 97 1C B4 1B AD 03 01 F1 4E 08 10 21 00 00 FF FF 00 00 }
0x393D4: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x393D9: 							Value  { 5A 82 }
0x393DB: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x393E5: 							End  { 29 02 }
0x393E7: 						End  { 29 02 }
0x393E9: 					End  { 29 02 }
0x393EB: 				End  { 29 02 }
0x393ED: 			End  { 29 02 }
0x393EF: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x393F6: 			End  { 29 02 }
0x393F8: 			OneOf Prompt: "Expose XHCI SDEV Entry", Help: "XHCI Entry in SDEV table will be exposed based on this option", QuestionFlags: 0x10, QuestionId: 0x3AE, VarStoreId: 0xF101, VarOffset: 0x831, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 1B C0 1B AE 03 01 F1 31 08 10 10 00 01 00 }
0x39409: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39410: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39417: 			End  { 29 02 }
0x39419: 			SuppressIf  { 0A 82 }
0x3941B: 				EqIdVal QuestionId: 0x3AE, Value: 0x0 { 12 06 AE 03 00 00 }
0x39421: 				Numeric Prompt: "  Number of USB Devices", Help: "Number of USB Devices", QuestionFlags: 0x10, QuestionId: 0x3AF, VarStoreId: 0xF101, VarOffset: 0x86F, Flags: 0x20, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 07 91 C1 1B C2 1B AF 03 01 F1 6F 08 10 20 01 02 00 }
0x39432: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39437: 						Value  { 5A 82 }
0x39439: 							Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x39443: 						End  { 29 02 }
0x39445: 					End  { 29 02 }
0x39447: 				End  { 29 02 }
0x39449: 				Numeric Prompt: "  Flags", Help: "Enter HEX value

BIT[0] - Allow handoff to non-secure OS
", QuestionFlags: 0x10, QuestionId: 0x3B0, VarStoreId: 0xF101, VarOffset: 0x99B, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 07 91 98 1C 74 1C B0 03 01 F1 9B 09 10 20 00 01 00 }
0x3945A: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3945F: 						Value  { 5A 82 }
0x39461: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3946B: 						End  { 29 02 }
0x3946D: 					End  { 29 02 }
0x3946F: 				End  { 29 02 }
0x39471: 				Text Prompt: "  USB Device 1", Help: "  USB Device 1", Text: "" { 03 08 C3 1B C3 1B 00 00 }
0x39479: 				Numeric Prompt: "  Attributes", Help: "Enter HEX value

BIT[7:1] - Reserved.
BIT[0]   - USB Composite Device
0x0 - A single interface USB device
0x1 - A function on a USB composite device
", QuestionFlags: 0x10, QuestionId: 0x3B1, VarStoreId: 0xF101, VarOffset: 0x870, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 C5 1B C6 1B B1 03 01 F1 70 08 10 20 00 FF 00 }
0x3948A: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3948F: 						Value  { 5A 82 }
0x39491: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3949B: 						End  { 29 02 }
0x3949D: 					End  { 29 02 }
0x3949F: 				End  { 29 02 }
0x394A1: 				Numeric Prompt: "  Root Port Number", Help: "Root port number on which the secure device is attached to the root hub.", QuestionFlags: 0x10, QuestionId: 0x3B2, VarStoreId: 0xF101, VarOffset: 0x872, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 C7 1B C8 1B B2 03 01 F1 72 08 10 20 00 FF 00 }
0x394B2: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x394B7: 						Value  { 5A 82 }
0x394B9: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x394C3: 						End  { 29 02 }
0x394C5: 					End  { 29 02 }
0x394C7: 				End  { 29 02 }
0x394C9: 				Numeric Prompt: "  VID", Help: "Vendor ID", QuestionFlags: 0x10, QuestionId: 0x3B3, VarStoreId: 0xF101, VarOffset: 0x874, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 C9 1B CA 1B B3 03 01 F1 74 08 10 21 00 00 FF FF 00 00 }
0x394DD: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x394E2: 						Value  { 5A 82 }
0x394E4: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x394EE: 						End  { 29 02 }
0x394F0: 					End  { 29 02 }
0x394F2: 				End  { 29 02 }
0x394F4: 				Numeric Prompt: "  PID", Help: "Product ID", QuestionFlags: 0x10, QuestionId: 0x3B4, VarStoreId: 0xF101, VarOffset: 0x878, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 CB 1B CC 1B B4 03 01 F1 78 08 10 21 00 00 FF FF 00 00 }
0x39508: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3950D: 						Value  { 5A 82 }
0x3950F: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39519: 						End  { 29 02 }
0x3951B: 					End  { 29 02 }
0x3951D: 				End  { 29 02 }
0x3951F: 				Numeric Prompt: "  Revision", Help: "Revision", QuestionFlags: 0x10, QuestionId: 0x3B5, VarStoreId: 0xF101, VarOffset: 0x87C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 CD 1B CE 1B B5 03 01 F1 7C 08 10 21 00 00 FF FF 00 00 }
0x39533: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39538: 						Value  { 5A 82 }
0x3953A: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39544: 						End  { 29 02 }
0x39546: 					End  { 29 02 }
0x39548: 				End  { 29 02 }
0x3954A: 				Numeric Prompt: "  Interface Number", Help: "Interface number (0-based) of the interface on the device that this entry corresponds to. This field is considered valid only if the Attributes indicates that the device is a composite device.", QuestionFlags: 0x10, QuestionId: 0x3B6, VarStoreId: 0xF101, VarOffset: 0x880, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 CF 1B D0 1B B6 03 01 F1 80 08 10 20 00 FF 00 }
0x3955B: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39560: 						Value  { 5A 82 }
0x39562: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3956C: 						End  { 29 02 }
0x3956E: 					End  { 29 02 }
0x39570: 				End  { 29 02 }
0x39572: 				Numeric Prompt: "  Class", Help: "Class Number of the secure device", QuestionFlags: 0x10, QuestionId: 0x3B7, VarStoreId: 0xF101, VarOffset: 0x882, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 D1 1B D2 1B B7 03 01 F1 82 08 10 20 00 FF 00 }
0x39583: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39588: 						Value  { 5A 82 }
0x3958A: 							Uint64 Value: 0xE { 45 0A 0E 00 00 00 00 00 00 00 }
0x39594: 						End  { 29 02 }
0x39596: 					End  { 29 02 }
0x39598: 				End  { 29 02 }
0x3959A: 				Numeric Prompt: "  Subclass", Help: "Subclass Number of the secure device", QuestionFlags: 0x10, QuestionId: 0x3B8, VarStoreId: 0xF101, VarOffset: 0x884, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 D3 1B D4 1B B8 03 01 F1 84 08 10 20 00 FF 00 }
0x395AB: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x395B0: 						Value  { 5A 82 }
0x395B2: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x395BC: 						End  { 29 02 }
0x395BE: 					End  { 29 02 }
0x395C0: 				End  { 29 02 }
0x395C2: 				Numeric Prompt: "  Protocol", Help: "Protocol Number of the secure device", QuestionFlags: 0x10, QuestionId: 0x3B9, VarStoreId: 0xF101, VarOffset: 0x886, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 D5 1B D6 1B B9 03 01 F1 86 08 10 20 00 FF 00 }
0x395D3: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x395D8: 						Value  { 5A 82 }
0x395DA: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x395E4: 						End  { 29 02 }
0x395E6: 					End  { 29 02 }
0x395E8: 				End  { 29 02 }
0x395EA: 				Numeric Prompt: "  ACPI Path String Offset", Help: "Offset for fully qualified ACPI path name of the secure device from the beginning of this table", QuestionFlags: 0x10, QuestionId: 0x3BA, VarStoreId: 0xF101, VarOffset: 0x888, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 D7 1B D8 1B BA 03 01 F1 88 08 10 21 00 00 FF FF 00 00 }
0x395FE: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39603: 						Value  { 5A 82 }
0x39605: 							Uint64 Value: 0x34 { 45 0A 34 00 00 00 00 00 00 00 }
0x3960F: 						End  { 29 02 }
0x39611: 					End  { 29 02 }
0x39613: 				End  { 29 02 }
0x39615: 				GrayOutIf  { 19 82 }
0x39617: 					True  { 46 02 }
0x39619: 					Numeric Prompt: "  ACPI Path String Length", Help: "Length of fully qualified, null terminated ACPI path name of the secure device, The length includes the NULL terminator.", QuestionFlags: 0x10, QuestionId: 0x3BB, VarStoreId: 0xF101, VarOffset: 0x88C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 D9 1B DA 1B BB 03 01 F1 8C 08 10 21 00 00 FF FF 00 00 }
0x3962D: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39632: 							Value  { 5A 82 }
0x39634: 								Uint64 Value: 0x1D { 45 0A 1D 00 00 00 00 00 00 00 }
0x3963E: 							End  { 29 02 }
0x39640: 						End  { 29 02 }
0x39642: 					End  { 29 02 }
0x39644: 				End  { 29 02 }
0x39646: 				Numeric Prompt: "  Firmware Hash [255:192]", Help: "  Firmware Hash [255:192]", QuestionFlags: 0x10, QuestionId: 0x3BC, VarStoreId: 0xF101, VarOffset: 0x8A8, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 DC 1B DC 1B BC 03 01 F1 A8 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x3966C: 					Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x39679: 				End  { 29 02 }
0x3967B: 				Numeric Prompt: "  Firmware Hash [191:128]", Help: "  Firmware Hash [191:128]", QuestionFlags: 0x10, QuestionId: 0x3BD, VarStoreId: 0xF101, VarOffset: 0x8A0, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 DD 1B DD 1B BD 03 01 F1 A0 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x396A1: 					Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x396AE: 				End  { 29 02 }
0x396B0: 				Numeric Prompt: "  Firmware Hash [127:64]", Help: "  Firmware Hash [127:64]", QuestionFlags: 0x10, QuestionId: 0x3BE, VarStoreId: 0xF101, VarOffset: 0x898, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 DE 1B DE 1B BE 03 01 F1 98 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x396D6: 					Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x396E3: 				End  { 29 02 }
0x396E5: 				Numeric Prompt: "  Firmware Hash [63:0]", Help: "  Firmware Hash [63:0]", QuestionFlags: 0x10, QuestionId: 0x3BF, VarStoreId: 0xF101, VarOffset: 0x890, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 DF 1B DF 1B BF 03 01 F1 90 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x3970B: 					Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x39718: 				End  { 29 02 }
0x3971A: 				String Prompt: "  ACPI Path Name", Help: "ACPI Path Name. 
 The default value is: \_SB.PC00.XHCI.RHUB.HS00.CRGB", QuestionFlags: 0x14, QuestionId: 0x287E, VarStoreId: 0xF101, VarStoreInfo: 0x8D0, MinSize: 0x1, MaxSize: 0x30, Flags: 0x0 { 1C 90 DB 1B E0 1B 7E 28 01 F1 D0 08 14 01 30 00 }
0x3972A: 				End  { 29 02 }
0x3972C: 				SuppressIf  { 0A 82 }
0x3972E: 					QuestionRef1 QuestionId: 0x3AF { 40 84 AF 03 }
0x39732: 						Uint8 Value: 0x1 { 42 03 01 }
0x39735: 						LessEqual  { 34 02 }
0x39737: 					End  { 29 02 }
0x39739: 					Text Prompt: "  USB Device 2", Help: "  USB Device 2", Text: "" { 03 08 C4 1B C4 1B 00 00 }
0x39741: 					Numeric Prompt: "  Attributes", Help: "Enter HEX value

BIT[7:1] - Reserved.
BIT[0]   - USB Composite Device
0x0 - A single interface USB device
0x1 - A function on a USB composite device
", QuestionFlags: 0x10, QuestionId: 0x3C0, VarStoreId: 0xF101, VarOffset: 0x871, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 99 1C C6 1B C0 03 01 F1 71 08 10 20 00 FF 00 }
0x39752: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39757: 							Value  { 5A 82 }
0x39759: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39763: 							End  { 29 02 }
0x39765: 						End  { 29 02 }
0x39767: 					End  { 29 02 }
0x39769: 					Numeric Prompt: "  Root Port Number", Help: "Root port number on which the secure device is attached to the root hub.", QuestionFlags: 0x10, QuestionId: 0x3C1, VarStoreId: 0xF101, VarOffset: 0x873, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 9A 1C C8 1B C1 03 01 F1 73 08 10 20 00 FF 00 }
0x3977A: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3977F: 							Value  { 5A 82 }
0x39781: 								Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3978B: 							End  { 29 02 }
0x3978D: 						End  { 29 02 }
0x3978F: 					End  { 29 02 }
0x39791: 					Numeric Prompt: "  VID", Help: "Vendor ID", QuestionFlags: 0x10, QuestionId: 0x3C2, VarStoreId: 0xF101, VarOffset: 0x876, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 9B 1C CA 1B C2 03 01 F1 76 08 10 21 00 00 FF FF 00 00 }
0x397A5: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x397AA: 							Value  { 5A 82 }
0x397AC: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x397B6: 							End  { 29 02 }
0x397B8: 						End  { 29 02 }
0x397BA: 					End  { 29 02 }
0x397BC: 					Numeric Prompt: "  PID", Help: "Product ID", QuestionFlags: 0x10, QuestionId: 0x3C3, VarStoreId: 0xF101, VarOffset: 0x87A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 9C 1C CC 1B C3 03 01 F1 7A 08 10 21 00 00 FF FF 00 00 }
0x397D0: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x397D5: 							Value  { 5A 82 }
0x397D7: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x397E1: 							End  { 29 02 }
0x397E3: 						End  { 29 02 }
0x397E5: 					End  { 29 02 }
0x397E7: 					Numeric Prompt: "  Revision", Help: "Revision", QuestionFlags: 0x10, QuestionId: 0x3C4, VarStoreId: 0xF101, VarOffset: 0x87E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 9D 1C CE 1B C4 03 01 F1 7E 08 10 21 00 00 FF FF 00 00 }
0x397FB: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39800: 							Value  { 5A 82 }
0x39802: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3980C: 							End  { 29 02 }
0x3980E: 						End  { 29 02 }
0x39810: 					End  { 29 02 }
0x39812: 					Numeric Prompt: "  Interface Number", Help: "Interface number (0-based) of the interface on the device that this entry corresponds to. This field is considered valid only if the Attributes indicates that the device is a composite device.", QuestionFlags: 0x10, QuestionId: 0x3C5, VarStoreId: 0xF101, VarOffset: 0x881, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 9E 1C D0 1B C5 03 01 F1 81 08 10 20 00 FF 00 }
0x39823: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39828: 							Value  { 5A 82 }
0x3982A: 								Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x39834: 							End  { 29 02 }
0x39836: 						End  { 29 02 }
0x39838: 					End  { 29 02 }
0x3983A: 					Numeric Prompt: "  Class", Help: "Class Number of the secure device", QuestionFlags: 0x10, QuestionId: 0x3C6, VarStoreId: 0xF101, VarOffset: 0x883, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 9F 1C D2 1B C6 03 01 F1 83 08 10 20 00 FF 00 }
0x3984B: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39850: 							Value  { 5A 82 }
0x39852: 								Uint64 Value: 0xE { 45 0A 0E 00 00 00 00 00 00 00 }
0x3985C: 							End  { 29 02 }
0x3985E: 						End  { 29 02 }
0x39860: 					End  { 29 02 }
0x39862: 					Numeric Prompt: "  Subclass", Help: "Subclass Number of the secure device", QuestionFlags: 0x10, QuestionId: 0x3C7, VarStoreId: 0xF101, VarOffset: 0x885, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 A0 1C D4 1B C7 03 01 F1 85 08 10 20 00 FF 00 }
0x39873: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x39878: 							Value  { 5A 82 }
0x3987A: 								Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x39884: 							End  { 29 02 }
0x39886: 						End  { 29 02 }
0x39888: 					End  { 29 02 }
0x3988A: 					Numeric Prompt: "  Protocol", Help: "Protocol Number of the secure device", QuestionFlags: 0x10, QuestionId: 0x3C8, VarStoreId: 0xF101, VarOffset: 0x887, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 A1 1C D6 1B C8 03 01 F1 87 08 10 20 00 FF 00 }
0x3989B: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x398A0: 							Value  { 5A 82 }
0x398A2: 								Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x398AC: 							End  { 29 02 }
0x398AE: 						End  { 29 02 }
0x398B0: 					End  { 29 02 }
0x398B2: 					Numeric Prompt: "  ACPI Path String Offset", Help: "Offset for fully qualified ACPI path name of the secure device from the beginning of this table", QuestionFlags: 0x10, QuestionId: 0x3C9, VarStoreId: 0xF101, VarOffset: 0x88A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 A2 1C D8 1B C9 03 01 F1 8A 08 10 21 00 00 FF FF 00 00 }
0x398C6: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x398CB: 							Value  { 5A 82 }
0x398CD: 								Uint64 Value: 0x34 { 45 0A 34 00 00 00 00 00 00 00 }
0x398D7: 							End  { 29 02 }
0x398D9: 						End  { 29 02 }
0x398DB: 					End  { 29 02 }
0x398DD: 					GrayOutIf  { 19 82 }
0x398DF: 						True  { 46 02 }
0x398E1: 						Numeric Prompt: "  ACPI Path String Length", Help: "Length of fully qualified, null terminated ACPI path name of the secure device, The length includes the NULL terminator.", QuestionFlags: 0x10, QuestionId: 0x3CA, VarStoreId: 0xF101, VarOffset: 0x88E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 A3 1C DA 1B CA 03 01 F1 8E 08 10 21 00 00 FF FF 00 00 }
0x398F5: 							Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x398FA: 								Value  { 5A 82 }
0x398FC: 									Uint64 Value: 0x1C { 45 0A 1C 00 00 00 00 00 00 00 }
0x39906: 								End  { 29 02 }
0x39908: 							End  { 29 02 }
0x3990A: 						End  { 29 02 }
0x3990C: 					End  { 29 02 }
0x3990E: 					Numeric Prompt: "  Firmware Hash [255:192]", Help: "  Firmware Hash [255:192]", QuestionFlags: 0x10, QuestionId: 0x3CB, VarStoreId: 0xF101, VarOffset: 0x8C8, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 A4 1C DC 1B CB 03 01 F1 C8 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x39934: 						Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x39941: 					End  { 29 02 }
0x39943: 					Numeric Prompt: "  Firmware Hash [191:128]", Help: "  Firmware Hash [191:128]", QuestionFlags: 0x10, QuestionId: 0x3CC, VarStoreId: 0xF101, VarOffset: 0x8C0, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 A5 1C DD 1B CC 03 01 F1 C0 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x39969: 						Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x39976: 					End  { 29 02 }
0x39978: 					Numeric Prompt: "  Firmware Hash [127:64]", Help: "  Firmware Hash [127:64]", QuestionFlags: 0x10, QuestionId: 0x3CD, VarStoreId: 0xF101, VarOffset: 0x8B8, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 A6 1C DE 1B CD 03 01 F1 B8 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x3999E: 						Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x399AB: 					End  { 29 02 }
0x399AD: 					Numeric Prompt: "  Firmware Hash [63:0]", Help: "  Firmware Hash [63:0]", QuestionFlags: 0x10, QuestionId: 0x3CE, VarStoreId: 0xF101, VarOffset: 0x8B0, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1 { 07 A6 A7 1C DF 1B CE 03 01 F1 B0 08 10 23 00 00 00 00 00 00 00 00 FF FF FF FF FF FF FF FF 01 00 00 00 00 00 00 00 }
0x399D3: 						Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x399E0: 					End  { 29 02 }
0x399E2: 					String Prompt: "  ACPI Path Name", Help: "ACPI Path Name. 
 The default value is: \_SB.PC00.XHCI.RHUB.HS01.CIR", QuestionFlags: 0x14, QuestionId: 0x287F, VarStoreId: 0xF101, VarStoreInfo: 0x932, MinSize: 0x1, MaxSize: 0x30, Flags: 0x0 { 1C 90 A8 1C E1 1B 7F 28 01 F1 32 09 14 01 30 00 }
0x399F2: 					End  { 29 02 }
0x399F4: 				End  { 29 02 }
0x399F6: 			End  { 29 02 }
0x399F8: 		End  { 29 02 }
0x399FA: 	End  { 29 02 }
0x399FC: 	Form FormId: 0x2880, Title: "TCSS Platform Setting" { 01 86 80 28 E2 1B }
0x39A02: 		Subtitle Prompt: "TCSS Platform Setting", Help: "", Flags: 0x0 { 02 87 E4 1B 00 00 00 }
0x39A09: 		End  { 29 02 }
0x39A0B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x39A12: 		End  { 29 02 }
0x39A14: 		SuppressIf  { 0A 82 }
0x39A16: 			EqIdVal QuestionId: 0x1174, Value: 0x0 { 12 06 74 11 00 00 }
0x39A1C: 			GrayOutIf  { 19 82 }
0x39A1E: 				EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x39A24: 				OneOf Prompt: "Disable TBT PCIE Tree BME", Help: "Disable TBT PCIE RP and child device Tree BME to Enable VTD Base Security", QuestionFlags: 0x14, QuestionId: 0x3CF, VarStoreId: 0xF101, VarOffset: 0xAC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 1C 49 1C CF 03 01 F1 C8 0A 14 10 00 01 00 }
0x39A35: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x39A3C: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x39A43: 				End  { 29 02 }
0x39A45: 			End  { 29 02 }
0x39A47: 		End  { 29 02 }
0x39A49: 		OneOf Prompt: "USBC connector manager selection", Help: "Select UCSI or UCMC device in ACPI support based on configuration", QuestionFlags: 0x10, QuestionId: 0x3D0, VarStoreId: 0xF101, VarOffset: 0x861, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E5 1B E6 1B D0 03 01 F1 61 08 10 10 00 02 00 }
0x39A5A: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39A60: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39A67: 			OneOfOption Option: "Enable UCSI Device" Value: 1 { 09 07 E7 1B 00 00 01 }
0x39A6E: 			OneOfOption Option: "Enable UCMC Device" Value: 2 { 09 07 E8 1B 00 00 02 }
0x39A75: 		End  { 29 02 }
0x39A77: 		OneOf Prompt: "USBC and USBA Wake Capability", Help: "USBC and USBA Wake Capability", QuestionFlags: 0x14, QuestionId: 0x2874, VarStoreId: 0xF101, VarOffset: 0x9DA, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x4, Step: 0x0 { 05 91 F3 1B F4 1B 74 28 01 F1 DA 09 14 10 03 04 00 }
0x39A88: 			OneOfOption Option: "S3" Value: 3 { 09 07 F5 1B 00 00 03 }
0x39A8F: 			OneOfOption Option: "S4" Value: 4, Default, MfgDefault { 09 07 F6 1B 30 00 04 }
0x39A96: 		End  { 29 02 }
0x39A98: 		OneOf Prompt: "PD PS_ON mode selection", Help: "Select TCSS PD Policy on Low Power Entry", QuestionFlags: 0x10, QuestionId: 0x3D1, VarStoreId: 0xF101, VarOffset: 0xA9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 75 1C 76 1C D1 03 01 F1 9F 0A 10 10 00 02 00 }
0x39AA9: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39AB0: 			OneOfOption Option: "Enable PD PS_ON" Value: 1 { 09 07 77 1C 00 00 01 }
0x39AB7: 			OneOfOption Option: "Enable PD PS_ON Override" Value: 2 { 09 07 78 1C 00 00 02 }
0x39ABE: 		End  { 29 02 }
0x39AC0: 		OneOf Prompt: "USBC DataRole Swap Platform Disable Option", Help: "Enable/Disable setting USBC DataRole Swap Platform Disable Option", QuestionFlags: 0x10, QuestionId: 0x3D2, VarStoreId: 0xF101, VarOffset: 0xAF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7E 1C 7F 1C D2 03 01 F1 F4 0A 10 10 00 01 00 }
0x39AD1: 			OneOfOption Option: "TRUE" Value: 1, Default, MfgDefault { 09 07 34 06 30 00 01 }
0x39AD8: 			OneOfOption Option: "FALSE" Value: 0 { 09 07 33 06 00 00 00 }
0x39ADF: 		End  { 29 02 }
0x39AE1: 		Ref Prompt: "Thunderbolt(TM) Configuration", Help: "Thunderbolt(TM) Related Configuration", QuestionFlags: 0x0, QuestionId: 0x3D3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28AB { 0F 0F BF 1E C0 1E D3 03 00 00 FF FF 00 AB 28 }
0x39AF0: 		SuppressIf  { 0A 82 }
0x39AF2: 			EqIdVal QuestionId: 0x11F1, Value: 0x0 { 12 06 F1 11 00 00 }
0x39AF8: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x39AFF: 			End  { 29 02 }
0x39B01: 			Subtitle Prompt: "PD Information", Help: "", Flags: 0x0 { 02 87 01 1C 00 00 00 }
0x39B08: 			End  { 29 02 }
0x39B0A: 			SuppressIf  { 0A 82 }
0x39B0C: 				EqIdVal QuestionId: 0x11F0, Value: 0x1 { 12 86 F0 11 01 00 }
0x39B12: 					Not  { 17 02 }
0x39B14: 				End  { 29 02 }
0x39B16: 				Text Prompt: "PD0 Application name", Help: "PD0 Application name", Text: "N/A" { 03 08 03 1C 02 1C 04 1C }
0x39B1E: 				Text Prompt: "PD0 External Circuit Specific Version", Help: "PD0 External Circuit Specific Version", Text: "N/A" { 03 08 06 1C 05 1C 07 1C }
0x39B26: 			End  { 29 02 }
0x39B28: 			Text Prompt: "PD0 Version", Help: "PD0 Version", Text: "N/A" { 03 08 09 1C 08 1C 0A 1C }
0x39B30: 			SuppressIf  { 0A 82 }
0x39B32: 				EqIdVal QuestionId: 0x11F0, Value: 0x1 { 12 86 F0 11 01 00 }
0x39B38: 					Not  { 17 02 }
0x39B3A: 				End  { 29 02 }
0x39B3C: 				Text Prompt: "PD1 Application name", Help: "PD1 Application name", Text: "N/A" { 03 08 0C 1C 0B 1C 0D 1C }
0x39B44: 				Text Prompt: "PD1 External Circuit Specific Version", Help: "PD1 External Circuit Specific Version", Text: "N/A" { 03 08 0F 1C 0E 1C 10 1C }
0x39B4C: 			End  { 29 02 }
0x39B4E: 			Text Prompt: "PD1 Version", Help: "PD1 Version", Text: "N/A" { 03 08 12 1C 11 1C 13 1C }
0x39B56: 		End  { 29 02 }
0x39B58: 	End  { 29 02 }
0x39B5A: 	Form FormId: 0x2888, Title: "OverClocking Performance Menu" { 01 86 88 28 AE 1C }
0x39B60: 		Subtitle Prompt: "OverClocking Performance Menu", Help: "", Flags: 0x0 { 02 87 AE 1C 00 00 00 }
0x39B67: 		End  { 29 02 }
0x39B69: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x39B70: 		End  { 29 02 }
0x39B72: 		OneOf Prompt: "OverClocking Feature", Help: "Performance Menu for Processor and Memory.", QuestionFlags: 0x14, QuestionId: 0x2881, VarStoreId: 0x1, VarOffset: 0x1D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 1C B1 1C 81 28 01 00 D9 01 14 10 00 01 00 }
0x39B83: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39B8A: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39B91: 		End  { 29 02 }
0x39B93: 		SuppressIf  { 0A 82 }
0x39B95: 			EqIdVal QuestionId: 0x2881, Value: 0x0 { 12 86 81 28 00 00 }
0x39B9B: 				EqIdVal QuestionId: 0x11EF, Value: 0x0 { 12 06 EF 11 00 00 }
0x39BA1: 				Or  { 16 02 }
0x39BA3: 			End  { 29 02 }
0x39BA5: 			OneOf Prompt: "UnderVolt Protection", Help: "When UnderVolt Protection is enabled, user will not be able to program under voltage in OS runtime. Recommended to keep it enabled by default. Enabled: Allow BIOS undervolting, but enable UnderVolt Protection in Runtime. Disabled: No UnderVolt Protection in Runtime.", QuestionFlags: 0x10, QuestionId: 0x3D4, VarStoreId: 0x1, VarOffset: 0x381, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4F 1E 50 1E D4 03 01 00 81 03 10 10 00 01 00 }
0x39BB6: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x39BBD: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x39BC4: 			End  { 29 02 }
0x39BC6: 		End  { 29 02 }
0x39BC8: 		SuppressIf  { 0A 82 }
0x39BCA: 			EqIdVal QuestionId: 0x11EE, Value: 0x0 { 12 86 EE 11 00 00 }
0x39BD0: 				EqIdVal QuestionId: 0x2881, Value: 0x0 { 12 06 81 28 00 00 }
0x39BD6: 				Or  { 16 02 }
0x39BD8: 			End  { 29 02 }
0x39BDA: 			Numeric Prompt: "Per-core HT Disable", Help: "", QuestionFlags: 0x14, QuestionId: 0x3D5, VarStoreId: 0x1, VarOffset: 0x230, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 94 B2 1C B3 1C D5 03 01 00 30 02 14 21 00 00 FF 00 01 00 }
0x39BEE: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x39BF5: 			End  { 29 02 }
0x39BF7: 		End  { 29 02 }
0x39BF9: 		OneOf Prompt: "WDT Enable", Help: "Enable/Disable WatchDog Timer. Note: This option is ignored on debug BIOS.", QuestionFlags: 0x10, QuestionId: 0x3D6, VarStoreId: 0x6, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 1C B5 1C D6 03 06 00 24 00 10 10 00 01 00 }
0x39C0A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39C11: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39C18: 		End  { 29 02 }
0x39C1A: 		Text Prompt: "BCLK Frequency", Help: "", Text: "100.00 MHz" { 03 08 2D 1E C9 07 2E 1E }
0x39C22: 		SuppressIf  { 0A 82 }
0x39C24: 			EqIdVal QuestionId: 0x2881, Value: 0x0 { 12 06 81 28 00 00 }
0x39C2A: 			SuppressIf  { 0A 82 }
0x39C2C: 				EqIdVal QuestionId: 0x1188, Value: 0x1 { 12 06 88 11 01 00 }
0x39C32: 				GrayOutIf  { 19 82 }
0x39C34: 					EqIdVal QuestionId: 0x11DC, Value: 0x1 { 12 06 DC 11 01 00 }
0x39C3A: 					Numeric Prompt: "CPU BCLK OC Frequency", Help: "CPU BCLK Frequency in 10kHz increments. Specifies new CPU BCLK frequency to be applied. Frequency is rounded to nearest valid value. Allowed range is limited by the Max/Min supported frequencies. Changes are not applied until settings are saved and platform resets. Example: For 125.70MHz, enter 12570.", QuestionFlags: 0x10, QuestionId: 0x3D7, VarStoreId: 0x1, VarOffset: 0x2F7, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xC350, Step: 0x1 { 07 9A 2F 1E 30 1E D7 03 01 00 F7 02 10 12 00 00 00 00 50 C3 00 00 01 00 00 00 }
0x39C54: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x39C5D: 					End  { 29 02 }
0x39C5F: 				End  { 29 02 }
0x39C61: 				OneOf Prompt: "BCLK Aware Adaptive Voltage", Help: "BCLK Aware Adaptive Voltage enable/disable. When enabled, pcode will be aware of the BCLK frequency when calculating the CPU V/F curves. This is ideal for BCLK OC to avoid high voltage overrides. Uses OC Mailbox command 0x15.", QuestionFlags: 0x10, QuestionId: 0x3D8, VarStoreId: 0x1, VarOffset: 0x20D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D3 1D D4 1D D8 03 01 00 0D 02 10 10 00 01 00 }
0x39C72: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x39C79: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x39C80: 				End  { 29 02 }
0x39C82: 			End  { 29 02 }
0x39C84: 			SuppressIf  { 0A 82 }
0x39C86: 				EqIdVal QuestionId: 0x1112, Value: 0x1 { 12 86 12 11 01 00 }
0x39C8C: 					Not  { 17 02 }
0x39C8E: 				End  { 29 02 }
0x39C90: 				Numeric Prompt: "PVD Ratio Threshold", Help: "Select PVD Ratio Threshold Value from Range 1 to 40. 0 - Auto/HW default", QuestionFlags: 0x10, QuestionId: 0x3D9, VarStoreId: 0x1, VarOffset: 0x1DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x28, Step: 0x1 { 07 91 31 1E 32 1E D9 03 01 00 DC 01 10 10 00 28 01 }
0x39CA1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39CA7: 				End  { 29 02 }
0x39CA9: 			End  { 29 02 }
0x39CAB: 			OneOf Prompt: "FLL Overclock Mode Enable", Help: "Enable FLL Overclock Mode, Default is Disable", QuestionFlags: 0x10, QuestionId: 0x3DA, VarStoreId: 0x1, VarOffset: 0x352, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 49 1E 4A 1E DA 03 01 00 52 03 10 10 00 01 00 }
0x39CBC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39CC3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39CCA: 			End  { 29 02 }
0x39CCC: 			SuppressIf  { 0A 82 }
0x39CCE: 				EqIdVal QuestionId: 0x3DA, Value: 0x0 { 12 06 DA 03 00 00 }
0x39CD4: 				Numeric Prompt: "  FLL Overclock Mode Select", Help: "Select FLL Mode Value from Range 1 to 3. 0x0 = no overclocking, 0x1 = ratio overclocking with nominal (0.5-1x) reference clock frequency, 0x2 = BCLK overclocking with elevated (1-3x) reference clock frequency, 0x3 = BCLK overclocking with extreme elevated (3-5x) reference clock frequency and ratio limited to 63", QuestionFlags: 0x10, QuestionId: 0x3DB, VarStoreId: 0x1, VarOffset: 0x353, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x1 { 07 91 4B 1E 4C 1E DB 03 01 00 53 03 10 10 00 03 01 }
0x39CE5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39CEB: 				End  { 29 02 }
0x39CED: 			End  { 29 02 }
0x39CEF: 			OneOf Prompt: "SA PLL Frequency Override", Help: "Configure Sa PLL Frequency.", QuestionFlags: 0x10, QuestionId: 0x3DC, VarStoreId: 0x1, VarOffset: 0x342, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 1D 0B 1D DC 03 01 00 42 03 10 10 00 01 00 }
0x39D00: 				OneOfOption Option: "3200 MHz" Value: 0, Default, MfgDefault { 09 07 0C 1D 30 00 00 }
0x39D07: 				OneOfOption Option: "1600 MHz" Value: 1 { 09 07 0D 1D 00 00 01 }
0x39D0E: 			End  { 29 02 }
0x39D10: 			OneOf Prompt: "BCLK TSC HW Fixup", Help: "BCLK TSC HW Fixup disable during TSC copy from PMA to APIC", QuestionFlags: 0x10, QuestionId: 0x3DD, VarStoreId: 0x1, VarOffset: 0x344, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 1D 0F 1D DD 03 01 00 44 03 10 10 00 01 00 }
0x39D21: 				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x39D28: 				OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x39D2F: 			End  { 29 02 }
0x39D31: 		End  { 29 02 }
0x39D33: 		SuppressIf  { 0A 82 }
0x39D35: 			EqIdVal QuestionId: 0x2881, Value: 0x0 { 12 06 81 28 00 00 }
0x39D3B: 			Ref Prompt: "Processor", Help: "Processor Bus Ratio Override and Bus Speed Override.", QuestionFlags: 0x0, QuestionId: 0x3DE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2889 { 0F 0F B8 1C B9 1C DE 03 00 00 FF FF 00 89 28 }
0x39D4A: 			SuppressIf  { 0A 82 }
0x39D4C: 				EqIdVal QuestionId: 0x11E5, Value: 0x0 { 12 86 E5 11 00 00 }
0x39D52: 					EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 06 ED 01 00 00 }
0x39D58: 					Or  { 16 02 }
0x39D5A: 				End  { 29 02 }
0x39D5C: 				Ref Prompt: "E-core L2 Configurations", Help: "Efficient-core L2 Bus Ratio Override and Bus Speed Override.", QuestionFlags: 0x0, QuestionId: 0x3DF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x288B { 0F 0F BB 1C BC 1C DF 03 00 00 FF FF 00 8B 28 }
0x39D6B: 			End  { 29 02 }
0x39D6D: 			Ref Prompt: "Ring", Help: "Ring Ratio and Voltage Settings", QuestionFlags: 0x0, QuestionId: 0x3E0, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x288C { 0F 0F BD 1C BE 1C E0 03 00 00 FF FF 00 8C 28 }
0x39D7C: 			Ref Prompt: "GT", Help: "GT Ratio Override and Delta voltage programming", QuestionFlags: 0x0, QuestionId: 0x3E1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x288D { 0F 0F 0A 1E 0B 1E E1 03 00 00 FF FF 00 8D 28 }
0x39D8B: 			Ref Prompt: "Voltage PLL Trim Controls", Help: "Voltage PLL Trim Controls Menu", QuestionFlags: 0x0, QuestionId: 0x3E2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2890 { 0F 0F B6 1C B7 1C E2 03 00 00 FF FF 00 90 28 }
0x39D9A: 			SuppressIf  { 0A 82 }
0x39D9C: 				EqIdVal QuestionId: 0x1188, Value: 0x1 { 12 06 88 11 01 00 }
0x39DA2: 				Ref Prompt: "Platform Voltage Overrides", Help: "Platform Voltages related Overclocking Menu", QuestionFlags: 0x0, QuestionId: 0x3E3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x288F { 0F 0F F0 1D F1 1D E3 03 00 00 FF FF 00 8F 28 }
0x39DB1: 			End  { 29 02 }
0x39DB3: 			Ref Prompt: "CEP Disable", Help: "CEP (Current Excursion Protection) Disable Menu", QuestionFlags: 0x0, QuestionId: 0x3E4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2891 { 0F 0F BD 1D BE 1D E4 03 00 00 FF FF 00 91 28 }
0x39DC2: 			Ref Prompt: "VR ICCMAX Current Override", Help: "VR ICCMAX Current Override Menu", QuestionFlags: 0x0, QuestionId: 0x3E5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2892 { 0F 0F C3 1D C4 1D E5 03 00 00 FF FF 00 92 28 }
0x39DD1: 		End  { 29 02 }
0x39DD3: 		SuppressIf  { 0A 82 }
0x39DD5: 			EqIdVal QuestionId: 0x11ED, Value: 0x0 { 12 06 ED 11 00 00 }
0x39DDB: 			Ref Prompt: "Uncore", Help: "Uncore Overclocking Menu", QuestionFlags: 0x0, QuestionId: 0x3E6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x288E { 0F 0F 23 1E 24 1E E6 03 00 00 FF FF 00 8E 28 }
0x39DEA: 		End  { 29 02 }
0x39DEC: 	End  { 29 02 }
0x39DEE: 	Form FormId: 0x2889, Title: "Processor" { 01 86 89 28 B8 1C }
0x39DF4: 		Subtitle Prompt: "Processor", Help: "", Flags: 0x0 { 02 87 B8 1C 00 00 00 }
0x39DFB: 		End  { 29 02 }
0x39DFD: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x39E04: 		End  { 29 02 }
0x39E06: 		OneOf Prompt: "Per Core Disable Configuration", Help: "Enable/Disable Per Core Disable. When Per Core Disable Configuration is enabled, selction of Active Cores and Active Efficient-cores will be disabled.", QuestionFlags: 0x14, QuestionId: 0x2882, VarStoreId: 0x1, VarOffset: 0x34C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 1C C5 1C 82 28 01 00 4C 03 14 10 00 01 00 }
0x39E17: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39E1E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39E25: 		End  { 29 02 }
0x39E27: 		SuppressIf  { 0A 82 }
0x39E29: 			EqIdVal QuestionId: 0x2882, Value: 0x1 { 12 86 82 28 01 00 }
0x39E2F: 				Not  { 17 02 }
0x39E31: 			End  { 29 02 }
0x39E33: 			Ref Prompt: "  Processor Disable", Help: "Processor Disable Control", QuestionFlags: 0x0, QuestionId: 0x3E7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2893 { 0F 0F C6 1C C7 1C E7 03 00 00 FF FF 00 93 28 }
0x39E42: 		End  { 29 02 }
0x39E44: 		SuppressIf  { 0A 82 }
0x39E46: 			EqIdVal QuestionId: 0x1112, Value: 0x1 { 12 86 12 11 01 00 }
0x39E4C: 				Not  { 17 02 }
0x39E4E: 			End  { 29 02 }
0x39E50: 			OneOf Prompt: "Core Ratio Extension Mode", Help: "Enable / Disable Core Ratio Above 85 Extension Mode. Enable - Max Overclocking Ratio Limit as specified by OCMB 0x1 command is 120; Disable - Max Overclocking Ratio Limit as specified by OCMB 0x1 command is 85.", QuestionFlags: 0x10, QuestionId: 0x3E8, VarStoreId: 0x1, VarOffset: 0x1DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 1D 09 1D E8 03 01 00 DA 01 10 10 00 01 00 }
0x39E61: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39E68: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39E6F: 			End  { 29 02 }
0x39E71: 		End  { 29 02 }
0x39E73: 		Numeric Prompt: "Core Max OC Ratio", Help: "Sets the maximum OC Ratio for the CPU Core. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range non-turbo max - 85 (Previously max turbo is 83).", QuestionFlags: 0x10, QuestionId: 0x3E9, VarStoreId: 0x1, VarOffset: 0x1DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 10 1D 11 1D E9 03 01 00 DB 01 10 10 00 78 01 }
0x39E84: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39E8A: 		End  { 29 02 }
0x39E8C: 		OneOf Prompt: "Per Core Ratio Override", Help: "Enable / Disable Per Core Ratio Override. Enable - Set maximum OC ratio to specific core by OCMB 0x1D command; Disable - Set maximum OC ratio to all cores by OCMB command 0x11. Reminding: It's expeced we should manual change the "Turbo Ratio Limit(TRL) MSR 0x1AD / 0x1AE" settings based on here max core ratio changed", QuestionFlags: 0x10, QuestionId: 0x3EA, VarStoreId: 0x1, VarOffset: 0x2BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 1C C3 1C EA 03 01 00 BB 02 10 10 00 01 00 }
0x39E9D: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x39EA4: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x39EAB: 		End  { 29 02 }
0x39EAD: 		SuppressIf  { 0A 82 }
0x39EAF: 			EqIdVal QuestionId: 0x3EA, Value: 0x0 { 12 06 EA 03 00 00 }
0x39EB5: 			Numeric Prompt: "  Core 0 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 0.", QuestionFlags: 0x10, QuestionId: 0x3EB, VarStoreId: 0x1, VarOffset: 0x2BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 12 1D 13 1D EB 03 01 00 BC 02 10 10 00 78 01 }
0x39EC6: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39ECC: 			End  { 29 02 }
0x39ECE: 			SuppressIf  { 0A 82 }
0x39ED0: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x39ED4: 					Uint8 Value: 0x2 { 42 03 02 }
0x39ED7: 					LessThan  { 33 02 }
0x39ED9: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x39EDD: 					Uint8 Value: 0x2 { 42 03 02 }
0x39EE0: 					LessThan  { 33 02 }
0x39EE2: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x39EE8: 					Not  { 17 02 }
0x39EEA: 					And  { 15 02 }
0x39EEC: 					Or  { 16 02 }
0x39EEE: 				End  { 29 02 }
0x39EF0: 				Numeric Prompt: "  Core 1 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 1.", QuestionFlags: 0x10, QuestionId: 0x3EC, VarStoreId: 0x1, VarOffset: 0x2BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 14 1D 15 1D EC 03 01 00 BD 02 10 10 00 78 01 }
0x39F01: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39F07: 				End  { 29 02 }
0x39F09: 			End  { 29 02 }
0x39F0B: 			SuppressIf  { 0A 82 }
0x39F0D: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x39F11: 					Uint8 Value: 0x3 { 42 03 03 }
0x39F14: 					LessThan  { 33 02 }
0x39F16: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x39F1A: 					Uint8 Value: 0x3 { 42 03 03 }
0x39F1D: 					LessThan  { 33 02 }
0x39F1F: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x39F25: 					Not  { 17 02 }
0x39F27: 					And  { 15 02 }
0x39F29: 					Or  { 16 02 }
0x39F2B: 				End  { 29 02 }
0x39F2D: 				Numeric Prompt: "  Core 2 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 2.", QuestionFlags: 0x10, QuestionId: 0x3ED, VarStoreId: 0x1, VarOffset: 0x2BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 16 1D 17 1D ED 03 01 00 BE 02 10 10 00 78 01 }
0x39F3E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39F44: 				End  { 29 02 }
0x39F46: 			End  { 29 02 }
0x39F48: 			SuppressIf  { 0A 82 }
0x39F4A: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x39F4E: 					Uint8 Value: 0x4 { 42 03 04 }
0x39F51: 					LessThan  { 33 02 }
0x39F53: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x39F57: 					Uint8 Value: 0x4 { 42 03 04 }
0x39F5A: 					LessThan  { 33 02 }
0x39F5C: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x39F62: 					Not  { 17 02 }
0x39F64: 					And  { 15 02 }
0x39F66: 					Or  { 16 02 }
0x39F68: 				End  { 29 02 }
0x39F6A: 				Numeric Prompt: "  Core 3 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 3.", QuestionFlags: 0x10, QuestionId: 0x3EE, VarStoreId: 0x1, VarOffset: 0x2BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 18 1D 19 1D EE 03 01 00 BF 02 10 10 00 78 01 }
0x39F7B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39F81: 				End  { 29 02 }
0x39F83: 			End  { 29 02 }
0x39F85: 			SuppressIf  { 0A 82 }
0x39F87: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x39F8B: 					Uint8 Value: 0x5 { 42 03 05 }
0x39F8E: 					LessThan  { 33 02 }
0x39F90: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x39F94: 					Uint8 Value: 0x5 { 42 03 05 }
0x39F97: 					LessThan  { 33 02 }
0x39F99: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x39F9F: 					Not  { 17 02 }
0x39FA1: 					And  { 15 02 }
0x39FA3: 					Or  { 16 02 }
0x39FA5: 				End  { 29 02 }
0x39FA7: 				Numeric Prompt: "  Core 4 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 4.", QuestionFlags: 0x10, QuestionId: 0x3EF, VarStoreId: 0x1, VarOffset: 0x2C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 1A 1D 1B 1D EF 03 01 00 C0 02 10 10 00 78 01 }
0x39FB8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39FBE: 				End  { 29 02 }
0x39FC0: 			End  { 29 02 }
0x39FC2: 			SuppressIf  { 0A 82 }
0x39FC4: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x39FC8: 					Uint8 Value: 0x6 { 42 03 06 }
0x39FCB: 					LessThan  { 33 02 }
0x39FCD: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x39FD1: 					Uint8 Value: 0x6 { 42 03 06 }
0x39FD4: 					LessThan  { 33 02 }
0x39FD6: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x39FDC: 					Not  { 17 02 }
0x39FDE: 					And  { 15 02 }
0x39FE0: 					Or  { 16 02 }
0x39FE2: 				End  { 29 02 }
0x39FE4: 				Numeric Prompt: "  Core 5 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 5.", QuestionFlags: 0x10, QuestionId: 0x3F0, VarStoreId: 0x1, VarOffset: 0x2C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 1C 1D 1D 1D F0 03 01 00 C1 02 10 10 00 78 01 }
0x39FF5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x39FFB: 				End  { 29 02 }
0x39FFD: 			End  { 29 02 }
0x39FFF: 			SuppressIf  { 0A 82 }
0x3A001: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A005: 					Uint8 Value: 0x7 { 42 03 07 }
0x3A008: 					LessThan  { 33 02 }
0x3A00A: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x3A00E: 					Uint8 Value: 0x7 { 42 03 07 }
0x3A011: 					LessThan  { 33 02 }
0x3A013: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x3A019: 					Not  { 17 02 }
0x3A01B: 					And  { 15 02 }
0x3A01D: 					Or  { 16 02 }
0x3A01F: 				End  { 29 02 }
0x3A021: 				Numeric Prompt: "  Core 6 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 6.", QuestionFlags: 0x10, QuestionId: 0x3F1, VarStoreId: 0x1, VarOffset: 0x2C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 1E 1D 1F 1D F1 03 01 00 C2 02 10 10 00 78 01 }
0x3A032: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3A038: 				End  { 29 02 }
0x3A03A: 			End  { 29 02 }
0x3A03C: 			SuppressIf  { 0A 82 }
0x3A03E: 				QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A042: 					Uint8 Value: 0x8 { 42 03 08 }
0x3A045: 					LessThan  { 33 02 }
0x3A047: 					QuestionRef1 QuestionId: 0x1EC { 40 04 EC 01 }
0x3A04B: 					Uint8 Value: 0x8 { 42 03 08 }
0x3A04E: 					LessThan  { 33 02 }
0x3A050: 					EqIdVal QuestionId: 0x1EC, Value: 0x0 { 12 06 EC 01 00 00 }
0x3A056: 					Not  { 17 02 }
0x3A058: 					And  { 15 02 }
0x3A05A: 					Or  { 16 02 }
0x3A05C: 				End  { 29 02 }
0x3A05E: 				Numeric Prompt: "  Core 7 Max Ratio", Help: "Override current maximum OC Ratio for the CPU Core 7.", QuestionFlags: 0x10, QuestionId: 0x3F2, VarStoreId: 0x1, VarOffset: 0x2C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 20 1D 21 1D F2 03 01 00 C3 02 10 10 00 78 01 }
0x3A06F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3A075: 				End  { 29 02 }
0x3A077: 			End  { 29 02 }
0x3A079: 			SuppressIf  { 0A 82 }
0x3A07B: 				QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A07F: 					Uint8 Value: 0x1 { 42 03 01 }
0x3A082: 					LessThan  { 33 02 }
0x3A084: 				End  { 29 02 }
0x3A086: 				Numeric Prompt: "  Cluster 0 Max Ratio", Help: "Override Efficient-cores 0 - 3 Maximum OC Ratio, maximum value up to 120.Note. E-cores 0 - 3 are in the same Cluster and their max core ratio will be aligned.", QuestionFlags: 0x10, QuestionId: 0x3F3, VarStoreId: 0x1, VarOffset: 0x2B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 22 1D 23 1D F3 03 01 00 B7 02 10 10 00 78 01 }
0x3A097: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3A09D: 				End  { 29 02 }
0x3A09F: 			End  { 29 02 }
0x3A0A1: 			SuppressIf  { 0A 82 }
0x3A0A3: 				QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A0A7: 					Uint8 Value: 0x2 { 42 03 02 }
0x3A0AA: 					LessThan  { 33 02 }
0x3A0AC: 				End  { 29 02 }
0x3A0AE: 				Numeric Prompt: "  Cluster 1 Max Ratio", Help: "Override Efficient-cores 4 - 7 Maximum OC Ratio, maximum value up to 120.Note. E-cores 4 - 7 are in the same Cluster and their max core ratio will be aligned.", QuestionFlags: 0x10, QuestionId: 0x3F4, VarStoreId: 0x1, VarOffset: 0x2B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 24 1D 25 1D F4 03 01 00 B8 02 10 10 00 78 01 }
0x3A0BF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3A0C5: 				End  { 29 02 }
0x3A0C7: 			End  { 29 02 }
0x3A0C9: 			SuppressIf  { 0A 82 }
0x3A0CB: 				QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A0CF: 					Uint8 Value: 0x3 { 42 03 03 }
0x3A0D2: 					LessThan  { 33 02 }
0x3A0D4: 				End  { 29 02 }
0x3A0D6: 				Numeric Prompt: "  Cluster 2 Max Ratio", Help: "Override Efficient-cores 8 - 11 Maximum OC Ratio, maximum value up to 120.Note. E-cores 8 - 11 are in the same Cluster and their max core ratio will be aligned.", QuestionFlags: 0x10, QuestionId: 0x3F5, VarStoreId: 0x1, VarOffset: 0x2B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 26 1D 27 1D F5 03 01 00 B9 02 10 10 00 78 01 }
0x3A0E7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3A0ED: 				End  { 29 02 }
0x3A0EF: 			End  { 29 02 }
0x3A0F1: 			SuppressIf  { 0A 82 }
0x3A0F3: 				QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A0F7: 					Uint8 Value: 0x4 { 42 03 04 }
0x3A0FA: 					LessThan  { 33 02 }
0x3A0FC: 				End  { 29 02 }
0x3A0FE: 				Numeric Prompt: "  Cluster 3 Max Ratio", Help: "Override Efficient-cores 12 - 15 Maximum OC Ratio, maximum value up to 120.Note. E-cores 12 - 15 are in the same Cluster and their max core ratio will be aligned.", QuestionFlags: 0x10, QuestionId: 0x3F6, VarStoreId: 0x1, VarOffset: 0x2BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x78, Step: 0x1 { 07 91 28 1D 29 1D F6 03 01 00 BA 02 10 10 00 78 01 }
0x3A10F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3A115: 				End  { 29 02 }
0x3A117: 			End  { 29 02 }
0x3A119: 		End  { 29 02 }
0x3A11B: 		GrayOutIf  { 19 82 }
0x3A11D: 			EqIdVal QuestionId: 0x11EA, Value: 0x0 { 12 06 EA 11 00 00 }
0x3A123: 			OneOf Prompt: "VF Offset Mode", Help: "Selects between Legacy and Selection modes. Need Reset System after enabling OverClocking Feature to Initialize the default value. In Legacy Mode, setting a global offset for the entire VF curve. In Selection modes, setting a selected VF point.", QuestionFlags: 0x10, QuestionId: 0x3F7, VarStoreId: 0x1, VarOffset: 0x232, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5B 1D 5C 1D F7 03 01 00 32 02 10 10 00 01 00 }
0x3A134: 				OneOfOption Option: "Legacy" Value: 0, Default, MfgDefault { 09 07 D7 1D 30 00 00 }
0x3A13B: 				OneOfOption Option: "Selection" Value: 1 { 09 07 D8 1D 00 00 01 }
0x3A142: 			End  { 29 02 }
0x3A144: 		End  { 29 02 }
0x3A146: 		SuppressIf  { 0A 82 }
0x3A148: 			EqIdVal QuestionId: 0x3F7, Value: 0x1 { 12 06 F7 03 01 00 }
0x3A14E: 			OneOf Prompt: "Core Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x3F8, VarStoreId: 0x1, VarOffset: 0x1DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 59 1D 5A 1D F8 03 01 00 DD 01 10 10 00 01 00 }
0x3A15F: 				OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault { 09 07 D5 1D 30 00 00 }
0x3A166: 				OneOfOption Option: "Override" Value: 1 { 09 07 D6 1D 00 00 01 }
0x3A16D: 			End  { 29 02 }
0x3A16F: 			SuppressIf  { 0A 82 }
0x3A171: 				EqIdVal QuestionId: 0x3F8, Value: 0x0 { 12 06 F8 03 00 00 }
0x3A177: 				Numeric Prompt: "P-core Voltage Override", Help: "Specifies the Override Voltage applied to the Performance-core domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV.", QuestionFlags: 0x10, QuestionId: 0x3F9, VarStoreId: 0x1, VarOffset: 0x1DE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 5F 1D 60 1D F9 03 01 00 DE 01 10 11 00 00 D0 07 01 00 }
0x3A18B: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A192: 				End  { 29 02 }
0x3A194: 			End  { 29 02 }
0x3A196: 			SuppressIf  { 0A 82 }
0x3A198: 				EqIdVal QuestionId: 0x3F8, Value: 0x1 { 12 06 F8 03 01 00 }
0x3A19E: 				Numeric Prompt: "P-core Voltage Target Override", Help: "Specifies the extra turbo voltage applied while Performance-core is operating in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x3FA, VarStoreId: 0x1, VarOffset: 0x1E3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 B1 1D B2 1D FA 03 01 00 E3 01 10 11 00 00 D0 07 01 00 }
0x3A1B2: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A1B9: 				End  { 29 02 }
0x3A1BB: 			End  { 29 02 }
0x3A1BD: 		End  { 29 02 }
0x3A1BF: 		SuppressIf  { 0A 82 }
0x3A1C1: 			EqIdVal QuestionId: 0x3F7, Value: 0x1 { 12 06 F7 03 01 00 }
0x3A1C7: 			OneOf Prompt: "VF Configuration Scope", Help: "Alows both all cores VF curve or per-core VF curve configuration.", QuestionFlags: 0x10, QuestionId: 0x3FB, VarStoreId: 0x1, VarOffset: 0x261, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5D 1D 5E 1D FB 03 01 00 61 02 10 10 00 01 00 }
0x3A1D8: 				OneOfOption Option: "All-core" Value: 0, Default, MfgDefault { 09 07 D9 1D 30 00 00 }
0x3A1DF: 				OneOfOption Option: "Per-core" Value: 1 { 09 07 DA 1D 00 00 01 }
0x3A1E6: 			End  { 29 02 }
0x3A1E8: 			SuppressIf  { 0A 82 }
0x3A1EA: 				EqIdVal QuestionId: 0x3FB, Value: 0x1 { 12 06 FB 03 01 00 }
0x3A1F0: 				Numeric Prompt: "P-core Voltage Offset", Help: "Specifies the Offset Voltage applied to the Global Performance-core domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x3FC, VarStoreId: 0x1, VarOffset: 0x1E0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 61 1D 62 1D FC 03 01 00 E0 01 10 11 00 00 E8 03 01 00 }
0x3A204: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A20B: 				End  { 29 02 }
0x3A20D: 				OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x3FD, VarStoreId: 0x1, VarOffset: 0x1E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DB 1D EF 1D FD 03 01 00 E2 01 10 10 00 01 00 }
0x3A21E: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A225: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A22C: 				End  { 29 02 }
0x3A22E: 			End  { 29 02 }
0x3A230: 			SuppressIf  { 0A 82 }
0x3A232: 				EqIdVal QuestionId: 0x3FB, Value: 0x0 { 12 06 FB 03 00 00 }
0x3A238: 				SuppressIf  { 0A 82 }
0x3A23A: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A23E: 						Uint8 Value: 0x1 { 42 03 01 }
0x3A241: 						LessThan  { 33 02 }
0x3A243: 					End  { 29 02 }
0x3A245: 					Numeric Prompt: "P-core 0 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 0 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x3FE, VarStoreId: 0x1, VarOffset: 0x262, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 63 1D 64 1D FE 03 01 00 62 02 10 11 00 00 E8 03 01 00 }
0x3A259: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A260: 					End  { 29 02 }
0x3A262: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x3FF, VarStoreId: 0x1, VarOffset: 0x272, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 1E EF 1D FF 03 01 00 72 02 10 10 00 01 00 }
0x3A273: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A27A: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A281: 					End  { 29 02 }
0x3A283: 				End  { 29 02 }
0x3A285: 				SuppressIf  { 0A 82 }
0x3A287: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A28B: 						Uint8 Value: 0x2 { 42 03 02 }
0x3A28E: 						LessThan  { 33 02 }
0x3A290: 					End  { 29 02 }
0x3A292: 					Numeric Prompt: "P-core 1 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 1 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x400, VarStoreId: 0x1, VarOffset: 0x264, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 65 1D 66 1D 00 04 01 00 64 02 10 11 00 00 E8 03 01 00 }
0x3A2A6: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A2AD: 					End  { 29 02 }
0x3A2AF: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x401, VarStoreId: 0x1, VarOffset: 0x273, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 62 1E EF 1D 01 04 01 00 73 02 10 10 00 01 00 }
0x3A2C0: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A2C7: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A2CE: 					End  { 29 02 }
0x3A2D0: 				End  { 29 02 }
0x3A2D2: 				SuppressIf  { 0A 82 }
0x3A2D4: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A2D8: 						Uint8 Value: 0x3 { 42 03 03 }
0x3A2DB: 						LessThan  { 33 02 }
0x3A2DD: 					End  { 29 02 }
0x3A2DF: 					Numeric Prompt: "P-core 2 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 2 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x402, VarStoreId: 0x1, VarOffset: 0x266, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 67 1D 68 1D 02 04 01 00 66 02 10 11 00 00 E8 03 01 00 }
0x3A2F3: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A2FA: 					End  { 29 02 }
0x3A2FC: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x403, VarStoreId: 0x1, VarOffset: 0x274, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 1E EF 1D 03 04 01 00 74 02 10 10 00 01 00 }
0x3A30D: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A314: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A31B: 					End  { 29 02 }
0x3A31D: 				End  { 29 02 }
0x3A31F: 				SuppressIf  { 0A 82 }
0x3A321: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A325: 						Uint8 Value: 0x4 { 42 03 04 }
0x3A328: 						LessThan  { 33 02 }
0x3A32A: 					End  { 29 02 }
0x3A32C: 					Numeric Prompt: "P-core 3 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 3 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x404, VarStoreId: 0x1, VarOffset: 0x268, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 69 1D 6A 1D 04 04 01 00 68 02 10 11 00 00 E8 03 01 00 }
0x3A340: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A347: 					End  { 29 02 }
0x3A349: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x405, VarStoreId: 0x1, VarOffset: 0x275, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 64 1E EF 1D 05 04 01 00 75 02 10 10 00 01 00 }
0x3A35A: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A361: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A368: 					End  { 29 02 }
0x3A36A: 				End  { 29 02 }
0x3A36C: 				SuppressIf  { 0A 82 }
0x3A36E: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A372: 						Uint8 Value: 0x5 { 42 03 05 }
0x3A375: 						LessThan  { 33 02 }
0x3A377: 					End  { 29 02 }
0x3A379: 					Numeric Prompt: "P-core 4 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 4 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x406, VarStoreId: 0x1, VarOffset: 0x26A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 6B 1D 6C 1D 06 04 01 00 6A 02 10 11 00 00 E8 03 01 00 }
0x3A38D: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A394: 					End  { 29 02 }
0x3A396: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x407, VarStoreId: 0x1, VarOffset: 0x276, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 1E EF 1D 07 04 01 00 76 02 10 10 00 01 00 }
0x3A3A7: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A3AE: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A3B5: 					End  { 29 02 }
0x3A3B7: 				End  { 29 02 }
0x3A3B9: 				SuppressIf  { 0A 82 }
0x3A3BB: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A3BF: 						Uint8 Value: 0x6 { 42 03 06 }
0x3A3C2: 						LessThan  { 33 02 }
0x3A3C4: 					End  { 29 02 }
0x3A3C6: 					Numeric Prompt: "P-core 5 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 5 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x408, VarStoreId: 0x1, VarOffset: 0x26C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 6D 1D 6E 1D 08 04 01 00 6C 02 10 11 00 00 E8 03 01 00 }
0x3A3DA: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A3E1: 					End  { 29 02 }
0x3A3E3: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x409, VarStoreId: 0x1, VarOffset: 0x277, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 66 1E EF 1D 09 04 01 00 77 02 10 10 00 01 00 }
0x3A3F4: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A3FB: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A402: 					End  { 29 02 }
0x3A404: 				End  { 29 02 }
0x3A406: 				SuppressIf  { 0A 82 }
0x3A408: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A40C: 						Uint8 Value: 0x7 { 42 03 07 }
0x3A40F: 						LessThan  { 33 02 }
0x3A411: 					End  { 29 02 }
0x3A413: 					Numeric Prompt: "P-core 6 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 6 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x40A, VarStoreId: 0x1, VarOffset: 0x26E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 6F 1D 70 1D 0A 04 01 00 6E 02 10 11 00 00 E8 03 01 00 }
0x3A427: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A42E: 					End  { 29 02 }
0x3A430: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x40B, VarStoreId: 0x1, VarOffset: 0x278, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 1E EF 1D 0B 04 01 00 78 02 10 10 00 01 00 }
0x3A441: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A448: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A44F: 					End  { 29 02 }
0x3A451: 				End  { 29 02 }
0x3A453: 				SuppressIf  { 0A 82 }
0x3A455: 					QuestionRef1 QuestionId: 0x11EC { 40 84 EC 11 }
0x3A459: 						Uint8 Value: 0x8 { 42 03 08 }
0x3A45C: 						LessThan  { 33 02 }
0x3A45E: 					End  { 29 02 }
0x3A460: 					Numeric Prompt: "P-core 7 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Performance-core 7 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x40C, VarStoreId: 0x1, VarOffset: 0x270, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 71 1D 72 1D 0C 04 01 00 70 02 10 11 00 00 E8 03 01 00 }
0x3A474: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A47B: 					End  { 29 02 }
0x3A47D: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x40D, VarStoreId: 0x1, VarOffset: 0x279, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 1E EF 1D 0D 04 01 00 79 02 10 10 00 01 00 }
0x3A48E: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A495: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A49C: 					End  { 29 02 }
0x3A49E: 				End  { 29 02 }
0x3A4A0: 				SuppressIf  { 0A 82 }
0x3A4A2: 					QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A4A6: 						Uint8 Value: 0x1 { 42 03 01 }
0x3A4A9: 						LessThan  { 33 02 }
0x3A4AB: 					End  { 29 02 }
0x3A4AD: 					Numeric Prompt: "Cluster 0 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Efficient-core Cluster 0 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x40E, VarStoreId: 0x1, VarOffset: 0x315, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 33 1D 34 1D 0E 04 01 00 15 03 10 11 00 00 E8 03 01 00 }
0x3A4C1: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A4C8: 					End  { 29 02 }
0x3A4CA: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x40F, VarStoreId: 0x1, VarOffset: 0x31D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 1E EF 1D 0F 04 01 00 1D 03 10 10 00 01 00 }
0x3A4DB: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A4E2: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A4E9: 					End  { 29 02 }
0x3A4EB: 				End  { 29 02 }
0x3A4ED: 				SuppressIf  { 0A 82 }
0x3A4EF: 					QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A4F3: 						Uint8 Value: 0x2 { 42 03 02 }
0x3A4F6: 						LessThan  { 33 02 }
0x3A4F8: 					End  { 29 02 }
0x3A4FA: 					Numeric Prompt: "Cluster 1 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Efficient-core Cluster 1 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x410, VarStoreId: 0x1, VarOffset: 0x317, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 35 1D 36 1D 10 04 01 00 17 03 10 11 00 00 E8 03 01 00 }
0x3A50E: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A515: 					End  { 29 02 }
0x3A517: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x411, VarStoreId: 0x1, VarOffset: 0x31E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6A 1E EF 1D 11 04 01 00 1E 03 10 10 00 01 00 }
0x3A528: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A52F: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A536: 					End  { 29 02 }
0x3A538: 				End  { 29 02 }
0x3A53A: 				SuppressIf  { 0A 82 }
0x3A53C: 					QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A540: 						Uint8 Value: 0x3 { 42 03 03 }
0x3A543: 						LessThan  { 33 02 }
0x3A545: 					End  { 29 02 }
0x3A547: 					Numeric Prompt: "Cluster 2 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Efficient-core Cluster 2 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x412, VarStoreId: 0x1, VarOffset: 0x319, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 37 1D 38 1D 12 04 01 00 19 03 10 11 00 00 E8 03 01 00 }
0x3A55B: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A562: 					End  { 29 02 }
0x3A564: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x413, VarStoreId: 0x1, VarOffset: 0x31F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 1E EF 1D 13 04 01 00 1F 03 10 10 00 01 00 }
0x3A575: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A57C: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A583: 					End  { 29 02 }
0x3A585: 				End  { 29 02 }
0x3A587: 				SuppressIf  { 0A 82 }
0x3A589: 					QuestionRef1 QuestionId: 0x11EB { 40 84 EB 11 }
0x3A58D: 						Uint8 Value: 0x4 { 42 03 04 }
0x3A590: 						LessThan  { 33 02 }
0x3A592: 					End  { 29 02 }
0x3A594: 					Numeric Prompt: "Cluster 3 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Efficient-core Cluster 3 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x414, VarStoreId: 0x1, VarOffset: 0x31B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 39 1D 3A 1D 14 04 01 00 1B 03 10 11 00 00 E8 03 01 00 }
0x3A5A8: 						Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A5AF: 					End  { 29 02 }
0x3A5B1: 					OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x415, VarStoreId: 0x1, VarOffset: 0x320, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 1E EF 1D 15 04 01 00 20 03 10 10 00 01 00 }
0x3A5C2: 						OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A5C9: 						OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A5D0: 					End  { 29 02 }
0x3A5D2: 				End  { 29 02 }
0x3A5D4: 			End  { 29 02 }
0x3A5D6: 		End  { 29 02 }
0x3A5D8: 		SuppressIf  { 0A 82 }
0x3A5DA: 			EqIdVal QuestionId: 0x3F7, Value: 0x0 { 12 06 F7 03 00 00 }
0x3A5E0: 			SuppressIf  { 0A 82 }
0x3A5E2: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A5E6: 					Uint8 Value: 0x1 { 42 03 01 }
0x3A5E9: 					LessThan  { 33 02 }
0x3A5EB: 				End  { 29 02 }
0x3A5ED: 				Numeric Prompt: "VF Point 1 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 1. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x1. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x416, VarStoreId: 0x1, VarOffset: 0x234, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 73 1D 74 1D 16 04 01 00 34 02 10 11 00 00 E8 03 01 00 }
0x3A601: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A608: 				End  { 29 02 }
0x3A60A: 				OneOf Prompt: "  VF Point 1 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x417, VarStoreId: 0x1, VarOffset: 0x252, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 1D EF 1D 17 04 01 00 52 02 10 10 00 01 00 }
0x3A61B: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A622: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A629: 				End  { 29 02 }
0x3A62B: 				Text Prompt: "  VF Point 1 Ratio", Help: "", Text: "N/A" { 03 08 3B 1D C9 07 3C 1D }
0x3A633: 			End  { 29 02 }
0x3A635: 			SuppressIf  { 0A 82 }
0x3A637: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A63B: 					Uint8 Value: 0x2 { 42 03 02 }
0x3A63E: 					LessThan  { 33 02 }
0x3A640: 				End  { 29 02 }
0x3A642: 				Numeric Prompt: "VF Point 2 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 2. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x2. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x418, VarStoreId: 0x1, VarOffset: 0x236, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 75 1D 76 1D 18 04 01 00 36 02 10 11 00 00 E8 03 01 00 }
0x3A656: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A65D: 				End  { 29 02 }
0x3A65F: 				OneOf Prompt: "  VF Point 2 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x419, VarStoreId: 0x1, VarOffset: 0x253, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DD 1D EF 1D 19 04 01 00 53 02 10 10 00 01 00 }
0x3A670: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A677: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A67E: 				End  { 29 02 }
0x3A680: 				Text Prompt: "  VF Point 2 Ratio", Help: "", Text: "N/A" { 03 08 3D 1D C9 07 3E 1D }
0x3A688: 			End  { 29 02 }
0x3A68A: 			SuppressIf  { 0A 82 }
0x3A68C: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A690: 					Uint8 Value: 0x3 { 42 03 03 }
0x3A693: 					LessThan  { 33 02 }
0x3A695: 				End  { 29 02 }
0x3A697: 				Numeric Prompt: "VF Point 3 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 3. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x3. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x41A, VarStoreId: 0x1, VarOffset: 0x238, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 77 1D 78 1D 1A 04 01 00 38 02 10 11 00 00 E8 03 01 00 }
0x3A6AB: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A6B2: 				End  { 29 02 }
0x3A6B4: 				OneOf Prompt: "  VF Point 3 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x41B, VarStoreId: 0x1, VarOffset: 0x254, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 1D EF 1D 1B 04 01 00 54 02 10 10 00 01 00 }
0x3A6C5: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A6CC: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A6D3: 				End  { 29 02 }
0x3A6D5: 				Text Prompt: "  VF Point 3 Ratio", Help: "", Text: "N/A" { 03 08 3F 1D C9 07 40 1D }
0x3A6DD: 			End  { 29 02 }
0x3A6DF: 			SuppressIf  { 0A 82 }
0x3A6E1: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A6E5: 					Uint8 Value: 0x4 { 42 03 04 }
0x3A6E8: 					LessThan  { 33 02 }
0x3A6EA: 				End  { 29 02 }
0x3A6EC: 				Numeric Prompt: "VF Point 4 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 4. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x4. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x41C, VarStoreId: 0x1, VarOffset: 0x23A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 79 1D 7A 1D 1C 04 01 00 3A 02 10 11 00 00 E8 03 01 00 }
0x3A700: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A707: 				End  { 29 02 }
0x3A709: 				OneOf Prompt: "  VF Point 4 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x41D, VarStoreId: 0x1, VarOffset: 0x255, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 1D EF 1D 1D 04 01 00 55 02 10 10 00 01 00 }
0x3A71A: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A721: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A728: 				End  { 29 02 }
0x3A72A: 				Text Prompt: "  VF Point 4 Ratio", Help: "", Text: "N/A" { 03 08 41 1D C9 07 42 1D }
0x3A732: 			End  { 29 02 }
0x3A734: 			SuppressIf  { 0A 82 }
0x3A736: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A73A: 					Uint8 Value: 0x5 { 42 03 05 }
0x3A73D: 					LessThan  { 33 02 }
0x3A73F: 				End  { 29 02 }
0x3A741: 				Numeric Prompt: "VF Point 5 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 5. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x5. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x41E, VarStoreId: 0x1, VarOffset: 0x23C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 7B 1D 7C 1D 1E 04 01 00 3C 02 10 11 00 00 E8 03 01 00 }
0x3A755: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A75C: 				End  { 29 02 }
0x3A75E: 				OneOf Prompt: "  VF Point 5 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x41F, VarStoreId: 0x1, VarOffset: 0x256, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 1D EF 1D 1F 04 01 00 56 02 10 10 00 01 00 }
0x3A76F: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A776: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A77D: 				End  { 29 02 }
0x3A77F: 				Text Prompt: "  VF Point 5 Ratio", Help: "", Text: "N/A" { 03 08 43 1D C9 07 44 1D }
0x3A787: 			End  { 29 02 }
0x3A789: 			SuppressIf  { 0A 82 }
0x3A78B: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A78F: 					Uint8 Value: 0x6 { 42 03 06 }
0x3A792: 					LessThan  { 33 02 }
0x3A794: 				End  { 29 02 }
0x3A796: 				Numeric Prompt: "VF Point 6 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 6. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x6. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x420, VarStoreId: 0x1, VarOffset: 0x23E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 7D 1D 7E 1D 20 04 01 00 3E 02 10 11 00 00 E8 03 01 00 }
0x3A7AA: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A7B1: 				End  { 29 02 }
0x3A7B3: 				OneOf Prompt: "  VF Point 6 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x421, VarStoreId: 0x1, VarOffset: 0x257, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 1D EF 1D 21 04 01 00 57 02 10 10 00 01 00 }
0x3A7C4: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A7CB: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A7D2: 				End  { 29 02 }
0x3A7D4: 				Text Prompt: "  VF Point 6 Ratio", Help: "", Text: "N/A" { 03 08 45 1D C9 07 46 1D }
0x3A7DC: 			End  { 29 02 }
0x3A7DE: 			SuppressIf  { 0A 82 }
0x3A7E0: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A7E4: 					Uint8 Value: 0x7 { 42 03 07 }
0x3A7E7: 					LessThan  { 33 02 }
0x3A7E9: 				End  { 29 02 }
0x3A7EB: 				Numeric Prompt: "VF Point 7 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 7. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x7. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x422, VarStoreId: 0x1, VarOffset: 0x240, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 7F 1D 80 1D 22 04 01 00 40 02 10 11 00 00 E8 03 01 00 }
0x3A7FF: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A806: 				End  { 29 02 }
0x3A808: 				OneOf Prompt: "  VF Point 7 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x423, VarStoreId: 0x1, VarOffset: 0x258, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 1D EF 1D 23 04 01 00 58 02 10 10 00 01 00 }
0x3A819: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A820: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A827: 				End  { 29 02 }
0x3A829: 				Text Prompt: "  VF Point 7 Ratio", Help: "", Text: "N/A" { 03 08 47 1D C9 07 48 1D }
0x3A831: 			End  { 29 02 }
0x3A833: 			SuppressIf  { 0A 82 }
0x3A835: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A839: 					Uint8 Value: 0x8 { 42 03 08 }
0x3A83C: 					LessThan  { 33 02 }
0x3A83E: 				End  { 29 02 }
0x3A840: 				Numeric Prompt: "VF Point 8 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 8. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x8. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x424, VarStoreId: 0x1, VarOffset: 0x242, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 81 1D 82 1D 24 04 01 00 42 02 10 11 00 00 E8 03 01 00 }
0x3A854: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A85B: 				End  { 29 02 }
0x3A85D: 				OneOf Prompt: "  VF Point 8 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x425, VarStoreId: 0x1, VarOffset: 0x259, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 1D EF 1D 25 04 01 00 59 02 10 10 00 01 00 }
0x3A86E: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A875: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A87C: 				End  { 29 02 }
0x3A87E: 				Text Prompt: "  VF Point 8 Ratio", Help: "", Text: "N/A" { 03 08 49 1D C9 07 4A 1D }
0x3A886: 			End  { 29 02 }
0x3A888: 			SuppressIf  { 0A 82 }
0x3A88A: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A88E: 					Uint8 Value: 0x9 { 42 03 09 }
0x3A891: 					LessThan  { 33 02 }
0x3A893: 				End  { 29 02 }
0x3A895: 				Numeric Prompt: "VF Point 9 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 9. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x9. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x426, VarStoreId: 0x1, VarOffset: 0x244, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 83 1D 84 1D 26 04 01 00 44 02 10 11 00 00 E8 03 01 00 }
0x3A8A9: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A8B0: 				End  { 29 02 }
0x3A8B2: 				OneOf Prompt: "  VF Point 9 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x427, VarStoreId: 0x1, VarOffset: 0x25A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 1D EF 1D 27 04 01 00 5A 02 10 10 00 01 00 }
0x3A8C3: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A8CA: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A8D1: 				End  { 29 02 }
0x3A8D3: 				Text Prompt: "  VF Point 9 Ratio", Help: "", Text: "N/A" { 03 08 4B 1D C9 07 4C 1D }
0x3A8DB: 			End  { 29 02 }
0x3A8DD: 			SuppressIf  { 0A 82 }
0x3A8DF: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A8E3: 					Uint8 Value: 0xA { 42 03 0A }
0x3A8E6: 					LessThan  { 33 02 }
0x3A8E8: 				End  { 29 02 }
0x3A8EA: 				Numeric Prompt: "VF Point 10 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 10. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xA. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x428, VarStoreId: 0x1, VarOffset: 0x246, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 85 1D 86 1D 28 04 01 00 46 02 10 11 00 00 E8 03 01 00 }
0x3A8FE: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A905: 				End  { 29 02 }
0x3A907: 				OneOf Prompt: "  VF Point 10 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x429, VarStoreId: 0x1, VarOffset: 0x25B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E5 1D EF 1D 29 04 01 00 5B 02 10 10 00 01 00 }
0x3A918: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A91F: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A926: 				End  { 29 02 }
0x3A928: 				Text Prompt: "  VF Point 10 Ratio", Help: "", Text: "N/A" { 03 08 4D 1D C9 07 4E 1D }
0x3A930: 			End  { 29 02 }
0x3A932: 			SuppressIf  { 0A 82 }
0x3A934: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A938: 					Uint8 Value: 0xB { 42 03 0B }
0x3A93B: 					LessThan  { 33 02 }
0x3A93D: 				End  { 29 02 }
0x3A93F: 				Numeric Prompt: "VF Point 11 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 11. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xB. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x42A, VarStoreId: 0x1, VarOffset: 0x248, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 87 1D 88 1D 2A 04 01 00 48 02 10 11 00 00 E8 03 01 00 }
0x3A953: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A95A: 				End  { 29 02 }
0x3A95C: 				OneOf Prompt: "  VF Point 11 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x42B, VarStoreId: 0x1, VarOffset: 0x25C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E6 1D EF 1D 2B 04 01 00 5C 02 10 10 00 01 00 }
0x3A96D: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A974: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A97B: 				End  { 29 02 }
0x3A97D: 				Text Prompt: "  VF Point 11 Ratio", Help: "", Text: "N/A" { 03 08 4F 1D C9 07 50 1D }
0x3A985: 			End  { 29 02 }
0x3A987: 			SuppressIf  { 0A 82 }
0x3A989: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A98D: 					Uint8 Value: 0xC { 42 03 0C }
0x3A990: 					LessThan  { 33 02 }
0x3A992: 				End  { 29 02 }
0x3A994: 				Numeric Prompt: "VF Point 12 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 12. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xC. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x42C, VarStoreId: 0x1, VarOffset: 0x24A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 89 1D 8A 1D 2C 04 01 00 4A 02 10 11 00 00 E8 03 01 00 }
0x3A9A8: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3A9AF: 				End  { 29 02 }
0x3A9B1: 				OneOf Prompt: "  VF Point 12 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x42D, VarStoreId: 0x1, VarOffset: 0x25D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E7 1D EF 1D 2D 04 01 00 5D 02 10 10 00 01 00 }
0x3A9C2: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3A9C9: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3A9D0: 				End  { 29 02 }
0x3A9D2: 				Text Prompt: "  VF Point 12 Ratio", Help: "", Text: "N/A" { 03 08 51 1D C9 07 52 1D }
0x3A9DA: 			End  { 29 02 }
0x3A9DC: 			SuppressIf  { 0A 82 }
0x3A9DE: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3A9E2: 					Uint8 Value: 0xD { 42 03 0D }
0x3A9E5: 					LessThan  { 33 02 }
0x3A9E7: 				End  { 29 02 }
0x3A9E9: 				Numeric Prompt: "VF Point 13 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 13. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xD. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x42E, VarStoreId: 0x1, VarOffset: 0x24C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 8B 1D 8C 1D 2E 04 01 00 4C 02 10 11 00 00 E8 03 01 00 }
0x3A9FD: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AA04: 				End  { 29 02 }
0x3AA06: 				OneOf Prompt: "  VF Point 13 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x42F, VarStoreId: 0x1, VarOffset: 0x25E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 1D EF 1D 2F 04 01 00 5E 02 10 10 00 01 00 }
0x3AA17: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AA1E: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AA25: 				End  { 29 02 }
0x3AA27: 				Text Prompt: "  VF Point 13 Ratio", Help: "", Text: "N/A" { 03 08 53 1D C9 07 54 1D }
0x3AA2F: 			End  { 29 02 }
0x3AA31: 			SuppressIf  { 0A 82 }
0x3AA33: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3AA37: 					Uint8 Value: 0xE { 42 03 0E }
0x3AA3A: 					LessThan  { 33 02 }
0x3AA3C: 				End  { 29 02 }
0x3AA3E: 				Numeric Prompt: "VF Point 14 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 14. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xE. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x430, VarStoreId: 0x1, VarOffset: 0x24E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 8D 1D 8E 1D 30 04 01 00 4E 02 10 11 00 00 E8 03 01 00 }
0x3AA52: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AA59: 				End  { 29 02 }
0x3AA5B: 				OneOf Prompt: "  VF Point 14 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x431, VarStoreId: 0x1, VarOffset: 0x25F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 1D EF 1D 31 04 01 00 5F 02 10 10 00 01 00 }
0x3AA6C: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AA73: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AA7A: 				End  { 29 02 }
0x3AA7C: 				Text Prompt: "  VF Point 14 Ratio", Help: "", Text: "N/A" { 03 08 55 1D C9 07 56 1D }
0x3AA84: 			End  { 29 02 }
0x3AA86: 			SuppressIf  { 0A 82 }
0x3AA88: 				QuestionRef1 QuestionId: 0x11EA { 40 84 EA 11 }
0x3AA8C: 					Uint8 Value: 0xF { 42 03 0F }
0x3AA8F: 					LessThan  { 33 02 }
0x3AA91: 				End  { 29 02 }
0x3AA93: 				Numeric Prompt: "VF Point 15 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 15. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xF. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x432, VarStoreId: 0x1, VarOffset: 0x250, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 8F 1D 90 1D 32 04 01 00 50 02 10 11 00 00 E8 03 01 00 }
0x3AAA7: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AAAE: 				End  { 29 02 }
0x3AAB0: 				OneOf Prompt: "  VF Point 15 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x433, VarStoreId: 0x1, VarOffset: 0x260, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 1D EF 1D 33 04 01 00 60 02 10 10 00 01 00 }
0x3AAC1: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AAC8: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AACF: 				End  { 29 02 }
0x3AAD1: 				Text Prompt: "  VF Point 15 Ratio", Help: "", Text: "N/A" { 03 08 57 1D C9 07 58 1D }
0x3AAD9: 			End  { 29 02 }
0x3AADB: 		End  { 29 02 }
0x3AADD: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3AAE4: 		End  { 29 02 }
0x3AAE6: 		Numeric Prompt: "AVX2 Ratio Offset", Help: "AVX2 Ratio Offset. Specifies number of bins to decrease AVX ratio vs. Core Ratio. AVX is a more stressful workload, it is helpful to lower the AVX ratio to ensure maximum possible ratio for SSE workloads. Uses Mailbox MSR 0x150, cmd 0x1B. Range 0 - 31. 0 = No offset.", QuestionFlags: 0x10, QuestionId: 0x434, VarStoreId: 0x1, VarOffset: 0x1E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 B3 1D B4 1D 34 04 01 00 E5 01 10 10 00 1F 01 }
0x3AAF7: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3AAFD: 		End  { 29 02 }
0x3AAFF: 		Numeric Prompt: "AVX2 Voltage Guardband Scale Factor", Help: "AVX2 Voltage Guardband Scale Factor. Controls the voltage guardband applied to AVX workloads. Range 0 - 200 in 1/100 units, where 125 = 1.25 scale factor. A default value of 100 applies the default voltage guardband scale factor of 1.0. A value > 100 will increase the votlage guardband, and < 100 will decrease the voltage guardband.", QuestionFlags: 0x10, QuestionId: 0x435, VarStoreId: 0x1, VarOffset: 0x225, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1 { 07 91 B5 1D B6 1D 35 04 01 00 25 02 10 10 00 C8 01 }
0x3AB10: 			Default DefaultId: 0x0 Value: 100 { 5B 06 00 00 00 64 }
0x3AB16: 		End  { 29 02 }
0x3AB18: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3AB1F: 		End  { 29 02 }
0x3AB21: 		Numeric Prompt: "TjMax Offset", Help: "TjMax Offset. Specified value here is clipped by pCode (125 - TjMax Offset) to support TjMax in the range of 62 to 115 deg Celsius. Uses Mailbox MSR 0x37, command 0x01. Range 10 - 63. 0 = No offset.", QuestionFlags: 0x10, QuestionId: 0x436, VarStoreId: 0x1, VarOffset: 0x1F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 B7 1D B8 1D 36 04 01 00 F8 01 10 10 00 3F 01 }
0x3AB32: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3AB38: 		End  { 29 02 }
0x3AB3A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3AB41: 		End  { 29 02 }
0x3AB43: 		Subtitle Prompt: "Thermal Velocity Boost (TVB)", Help: "", Flags: 0x0 { 02 87 BA 1C 00 00 00 }
0x3AB4A: 		End  { 29 02 }
0x3AB4C: 		OneOf Prompt: "Thermal Velocity Boost", Help: "This service controls Core frequency reduction caused by high package temperatures for processors that implement the Intel Thermal Velocity Boost (TVB) feature. It is required to be disabled for supporting overclocking at frequencies higher than the default max turbo frequency. Default is disabled. Uses Overclocking Mailbox command 0x18/0x19.", QuestionFlags: 0x10, QuestionId: 0x437, VarStoreId: 0x1, VarOffset: 0x2E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 1D BA 1D 37 04 01 00 E3 02 10 10 00 01 00 }
0x3AB5D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3AB64: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3AB6B: 		End  { 29 02 }
0x3AB6D: 		SuppressIf  { 0A 82 }
0x3AB6F: 			EqIdVal QuestionId: 0x437, Value: 0x0 { 12 06 37 04 00 00 }
0x3AB75: 			Numeric Prompt: "Down Bins (delta) for Temperature Threshold 0", Help: "When running above Temperature Threshold 0, the ratio will be clipped to (Max_Ratio-This Down Bins value)", QuestionFlags: 0x10, QuestionId: 0x438, VarStoreId: 0x1, VarOffset: 0x34E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 41 1E 42 1E 38 04 01 00 4E 03 10 10 00 0A 01 }
0x3AB86: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3AB8C: 			End  { 29 02 }
0x3AB8E: 			Numeric Prompt: "TVB Temperature Threshold 0 (degrees C)", Help: "Running ABOVE this temperature will clip delta Down Bins for Threshold 0 from the resolved OC Ratio", QuestionFlags: 0x10, QuestionId: 0x439, VarStoreId: 0x1, VarOffset: 0x34F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1 { 07 91 45 1E 46 1E 39 04 01 00 4F 03 10 10 00 64 01 }
0x3AB9F: 				Default DefaultId: 0x0 Value: 70 { 5B 06 00 00 00 46 }
0x3ABA5: 			End  { 29 02 }
0x3ABA7: 			Numeric Prompt: "TVB Temperature Threshold 1 (degrees C)", Help: "Running ABOVE this temperature will clip delta Down Bins for Threshold 1 from the resolved OC Ratio", QuestionFlags: 0x10, QuestionId: 0x43A, VarStoreId: 0x1, VarOffset: 0x350, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1 { 07 91 47 1E 48 1E 3A 04 01 00 50 03 10 10 00 64 01 }
0x3ABB8: 				Default DefaultId: 0x0 Value: 100 { 5B 06 00 00 00 64 }
0x3ABBE: 			End  { 29 02 }
0x3ABC0: 			Numeric Prompt: "Down Bins (delta) for Temperature Threshold 1", Help: "When running above Temperature Threshold 1, the ratio will be clipped to (Max_Ratio-This Down Bins value)", QuestionFlags: 0x10, QuestionId: 0x43B, VarStoreId: 0x1, VarOffset: 0x351, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 43 1E 44 1E 3B 04 01 00 51 03 10 10 00 0A 01 }
0x3ABD1: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x3ABD7: 			End  { 29 02 }
0x3ABD9: 		End  { 29 02 }
0x3ABDB: 		OneOf Prompt: "TVB Voltage Optimizations", Help: "This service controls thermal based voltage optimizations for processors that implement the Intel Thermal Velocity Boost (TVB) feature. Default is enabled. Uses Overclocking Mailbox command 0x18/0x19.", QuestionFlags: 0x10, QuestionId: 0x43C, VarStoreId: 0x1, VarOffset: 0x2E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 1D BC 1D 3C 04 01 00 E4 02 10 10 00 01 00 }
0x3ABEC: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3ABF3: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3ABFA: 		End  { 29 02 }
0x3ABFC: 		OneOf Prompt: "Enhanced Thermal Velocity Boost", Help: "If enabled the user will be clipped when the temperatures reach the default threshold on supported products.  Recommended to disable for overclocking.", QuestionFlags: 0x10, QuestionId: 0x43D, VarStoreId: 0x1, VarOffset: 0x378, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4D 1E 4E 1E 3D 04 01 00 78 03 10 10 00 01 00 }
0x3AC0D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3AC14: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3AC1B: 		End  { 29 02 }
0x3AC1D: 		SuppressIf  { 0A 82 }
0x3AC1F: 			EqIdVal QuestionId: 0x11E9, Value: 0x0 { 12 86 E9 11 00 00 }
0x3AC25: 				EqIdVal QuestionId: 0x11E8, Value: 0x0 { 12 06 E8 11 00 00 }
0x3AC2B: 				Or  { 16 02 }
0x3AC2D: 			End  { 29 02 }
0x3AC2F: 			Text Prompt: "Expected CPU Freq", Help: "Expected Processor frequency calculated using Bus ratio and Bus speed.", Text: "" { 03 08 BF 1C C1 1C C0 1C }
0x3AC37: 			SuppressIf  { 0A 82 }
0x3AC39: 				True  { 46 02 }
0x3AC3B: 				SuppressIf  { 0A 82 }
0x3AC3D: 					EqIdVal QuestionId: 0x10FC, Value: 0xB { 12 06 FC 10 0B 00 }
0x3AC43: 					Action Prompt: "Expected CPU Freq", Help: "Expected Processor frequency calculated using Bus ratio and Bus speed.", QuestionFlags: 0x4, QuestionId: 0x288A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: "" { 0C 8F BF 1C C1 1C 8A 28 00 00 FF FF 04 00 00 }
0x3AC52: 					End  { 29 02 }
0x3AC54: 				End  { 29 02 }
0x3AC56: 			End  { 29 02 }
0x3AC58: 		End  { 29 02 }
0x3AC5A: 	End  { 29 02 }
0x3AC5C: 	Form FormId: 0x288B, Title: "E-core L2 Configurations" { 01 86 8B 28 BB 1C }
0x3AC62: 		Subtitle Prompt: "E-core L2 Configurations", Help: "", Flags: 0x0 { 02 87 BB 1C 00 00 00 }
0x3AC69: 		End  { 29 02 }
0x3AC6B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3AC72: 		End  { 29 02 }
0x3AC74: 		OneOf Prompt: "E-core L2 Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x43E, VarStoreId: 0x1, VarOffset: 0x2AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 1D 2B 1D 3E 04 01 00 AF 02 10 10 00 01 00 }
0x3AC85: 			OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault { 09 07 D5 1D 30 00 00 }
0x3AC8C: 			OneOfOption Option: "Override" Value: 1 { 09 07 D6 1D 00 00 01 }
0x3AC93: 		End  { 29 02 }
0x3AC95: 		SuppressIf  { 0A 82 }
0x3AC97: 			EqIdVal QuestionId: 0x43E, Value: 0x0 { 12 06 3E 04 00 00 }
0x3AC9D: 			Numeric Prompt: "E-core L2 Voltage Override", Help: "Specifies the Override Voltage applied to the Efficient-core L2 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV.", QuestionFlags: 0x10, QuestionId: 0x43F, VarStoreId: 0x1, VarOffset: 0x2B0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 2C 1D 2D 1D 3F 04 01 00 B0 02 10 11 00 00 D0 07 01 00 }
0x3ACB1: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3ACB8: 			End  { 29 02 }
0x3ACBA: 		End  { 29 02 }
0x3ACBC: 		SuppressIf  { 0A 82 }
0x3ACBE: 			EqIdVal QuestionId: 0x43E, Value: 0x1 { 12 06 3E 04 01 00 }
0x3ACC4: 			Numeric Prompt: "E-core L2 Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while Efficient-core L2 is operating in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x440, VarStoreId: 0x1, VarOffset: 0x2B5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 30 1D 31 1D 40 04 01 00 B5 02 10 11 00 00 D0 07 01 00 }
0x3ACD8: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3ACDF: 			End  { 29 02 }
0x3ACE1: 		End  { 29 02 }
0x3ACE3: 		Numeric Prompt: "E-core L2 Voltage Offset", Help: "Specifies the Offset Voltage applied to the Efficient-core L2 domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x441, VarStoreId: 0x1, VarOffset: 0x2B2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 2E 1D 2F 1D 41 04 01 00 B2 02 10 11 00 00 E8 03 01 00 }
0x3ACF7: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3ACFE: 		End  { 29 02 }
0x3AD00: 		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x442, VarStoreId: 0x1, VarOffset: 0x2B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 1D EF 1D 42 04 01 00 B4 02 10 10 00 01 00 }
0x3AD11: 			OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AD18: 			OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AD1F: 		End  { 29 02 }
0x3AD21: 	End  { 29 02 }
0x3AD23: 	Form FormId: 0x288C, Title: "Ring" { 01 86 8C 28 BD 1C }
0x3AD29: 		Subtitle Prompt: "Ring", Help: "", Flags: 0x0 { 02 87 BD 1C 00 00 00 }
0x3AD30: 		End  { 29 02 }
0x3AD32: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3AD39: 		End  { 29 02 }
0x3AD3B: 		Numeric Prompt: "Ring Max OC Ratio", Help: "Sets the maximum OC Ratio for the CPU Ring. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range non-turbo max - 85.", QuestionFlags: 0x14, QuestionId: 0x2885, VarStoreId: 0x1, VarOffset: 0x1E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 A0 1D A1 1D 85 28 01 00 E7 01 14 10 00 55 01 }
0x3AD4C: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3AD52: 		End  { 29 02 }
0x3AD54: 		GrayOutIf  { 19 82 }
0x3AD56: 			EqIdVal QuestionId: 0x11E7, Value: 0x0 { 12 06 E7 11 00 00 }
0x3AD5C: 			OneOf Prompt: "VF Offset Mode", Help: "Selects between Legacy and Selection modes. Need Reset System after enabling OverClocking Feature to Initialize the default value. In Legacy Mode, setting a global offset for the entire VF curve. In Selection modes, setting a selected VF point.", QuestionFlags: 0x10, QuestionId: 0x443, VarStoreId: 0x1, VarOffset: 0x27C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 51 1E 5C 1D 43 04 01 00 7C 02 10 10 00 01 00 }
0x3AD6D: 				OneOfOption Option: "Legacy" Value: 0, Default, MfgDefault { 09 07 D7 1D 30 00 00 }
0x3AD74: 				OneOfOption Option: "Selection" Value: 1 { 09 07 D8 1D 00 00 01 }
0x3AD7B: 			End  { 29 02 }
0x3AD7D: 		End  { 29 02 }
0x3AD7F: 		SuppressIf  { 0A 82 }
0x3AD81: 			EqIdVal QuestionId: 0x443, Value: 0x1 { 12 06 43 04 01 00 }
0x3AD87: 			OneOf Prompt: "Ring Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x444, VarStoreId: 0x1, VarOffset: 0x1E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 1D A3 1D 44 04 01 00 E9 01 10 10 00 01 00 }
0x3AD98: 				OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault { 09 07 D5 1D 30 00 00 }
0x3AD9F: 				OneOfOption Option: "Override" Value: 1 { 09 07 D6 1D 00 00 01 }
0x3ADA6: 			End  { 29 02 }
0x3ADA8: 			SuppressIf  { 0A 82 }
0x3ADAA: 				EqIdVal QuestionId: 0x444, Value: 0x0 { 12 06 44 04 00 00 }
0x3ADB0: 				Numeric Prompt: "Ring Voltage Override", Help: "Specifies the Override Voltage applied to the Ring domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV.", QuestionFlags: 0x10, QuestionId: 0x445, VarStoreId: 0x1, VarOffset: 0x1EA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 A4 1D A5 1D 45 04 01 00 EA 01 10 11 00 00 D0 07 01 00 }
0x3ADC4: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3ADCB: 				End  { 29 02 }
0x3ADCD: 			End  { 29 02 }
0x3ADCF: 			SuppressIf  { 0A 82 }
0x3ADD1: 				EqIdVal QuestionId: 0x444, Value: 0x1 { 12 06 44 04 01 00 }
0x3ADD7: 				Numeric Prompt: "Ring Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while ring is operating in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x446, VarStoreId: 0x1, VarOffset: 0x1EF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 A8 1D A9 1D 46 04 01 00 EF 01 10 11 00 00 D0 07 01 00 }
0x3ADEB: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3ADF2: 				End  { 29 02 }
0x3ADF4: 			End  { 29 02 }
0x3ADF6: 			Numeric Prompt: "Ring Voltage Offset", Help: "Specifies the Offset Voltage applied to the Ring domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x447, VarStoreId: 0x1, VarOffset: 0x1EC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 A6 1D A7 1D 47 04 01 00 EC 01 10 11 00 00 E8 03 01 00 }
0x3AE0A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AE11: 			End  { 29 02 }
0x3AE13: 			OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x448, VarStoreId: 0x1, VarOffset: 0x1EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 1D EF 1D 48 04 01 00 EE 01 10 10 00 01 00 }
0x3AE24: 				OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AE2B: 				OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AE32: 			End  { 29 02 }
0x3AE34: 		End  { 29 02 }
0x3AE36: 		SuppressIf  { 0A 82 }
0x3AE38: 			EqIdVal QuestionId: 0x443, Value: 0x0 { 12 06 43 04 00 00 }
0x3AE3E: 			SuppressIf  { 0A 82 }
0x3AE40: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3AE44: 					Uint8 Value: 0x1 { 42 03 01 }
0x3AE47: 					LessThan  { 33 02 }
0x3AE49: 				End  { 29 02 }
0x3AE4B: 				Numeric Prompt: "VF Point 1 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 1. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x1. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x449, VarStoreId: 0x1, VarOffset: 0x27E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 52 1E 74 1D 49 04 01 00 7E 02 10 11 00 00 E8 03 01 00 }
0x3AE5F: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AE66: 				End  { 29 02 }
0x3AE68: 				OneOf Prompt: "  VF Point 1 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x44A, VarStoreId: 0x1, VarOffset: 0x29C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 1E EF 1D 4A 04 01 00 9C 02 10 10 00 01 00 }
0x3AE79: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AE80: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AE87: 				End  { 29 02 }
0x3AE89: 				Text Prompt: "  VF Point 1 Ratio", Help: "", Text: "N/A" { 03 08 3B 1D C9 07 91 1D }
0x3AE91: 			End  { 29 02 }
0x3AE93: 			SuppressIf  { 0A 82 }
0x3AE95: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3AE99: 					Uint8 Value: 0x2 { 42 03 02 }
0x3AE9C: 					LessThan  { 33 02 }
0x3AE9E: 				End  { 29 02 }
0x3AEA0: 				Numeric Prompt: "VF Point 2 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 2. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x2. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x44B, VarStoreId: 0x1, VarOffset: 0x280, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 53 1E 76 1D 4B 04 01 00 80 02 10 11 00 00 E8 03 01 00 }
0x3AEB4: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AEBB: 				End  { 29 02 }
0x3AEBD: 				OneOf Prompt: "  VF Point 2 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x44C, VarStoreId: 0x1, VarOffset: 0x29D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 1E EF 1D 4C 04 01 00 9D 02 10 10 00 01 00 }
0x3AECE: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AED5: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AEDC: 				End  { 29 02 }
0x3AEDE: 				Text Prompt: "  VF Point 2 Ratio", Help: "", Text: "N/A" { 03 08 3D 1D C9 07 92 1D }
0x3AEE6: 			End  { 29 02 }
0x3AEE8: 			SuppressIf  { 0A 82 }
0x3AEEA: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3AEEE: 					Uint8 Value: 0x3 { 42 03 03 }
0x3AEF1: 					LessThan  { 33 02 }
0x3AEF3: 				End  { 29 02 }
0x3AEF5: 				Numeric Prompt: "VF Point 3 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 3. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x3. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x44D, VarStoreId: 0x1, VarOffset: 0x282, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 54 1E 78 1D 4D 04 01 00 82 02 10 11 00 00 E8 03 01 00 }
0x3AF09: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AF10: 				End  { 29 02 }
0x3AF12: 				OneOf Prompt: "  VF Point 3 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x44E, VarStoreId: 0x1, VarOffset: 0x29E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6F 1E EF 1D 4E 04 01 00 9E 02 10 10 00 01 00 }
0x3AF23: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AF2A: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AF31: 				End  { 29 02 }
0x3AF33: 				Text Prompt: "  VF Point 3 Ratio", Help: "", Text: "N/A" { 03 08 3F 1D C9 07 93 1D }
0x3AF3B: 			End  { 29 02 }
0x3AF3D: 			SuppressIf  { 0A 82 }
0x3AF3F: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3AF43: 					Uint8 Value: 0x4 { 42 03 04 }
0x3AF46: 					LessThan  { 33 02 }
0x3AF48: 				End  { 29 02 }
0x3AF4A: 				Numeric Prompt: "VF Point 4 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 4. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x4. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x44F, VarStoreId: 0x1, VarOffset: 0x284, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 55 1E 7A 1D 4F 04 01 00 84 02 10 11 00 00 E8 03 01 00 }
0x3AF5E: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AF65: 				End  { 29 02 }
0x3AF67: 				OneOf Prompt: "  VF Point 4 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x450, VarStoreId: 0x1, VarOffset: 0x29F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 1E EF 1D 50 04 01 00 9F 02 10 10 00 01 00 }
0x3AF78: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AF7F: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AF86: 				End  { 29 02 }
0x3AF88: 				Text Prompt: "  VF Point 4 Ratio", Help: "", Text: "N/A" { 03 08 41 1D C9 07 94 1D }
0x3AF90: 			End  { 29 02 }
0x3AF92: 			SuppressIf  { 0A 82 }
0x3AF94: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3AF98: 					Uint8 Value: 0x5 { 42 03 05 }
0x3AF9B: 					LessThan  { 33 02 }
0x3AF9D: 				End  { 29 02 }
0x3AF9F: 				Numeric Prompt: "VF Point 5 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 5. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x5. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x451, VarStoreId: 0x1, VarOffset: 0x286, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 56 1E 7C 1D 51 04 01 00 86 02 10 11 00 00 E8 03 01 00 }
0x3AFB3: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3AFBA: 				End  { 29 02 }
0x3AFBC: 				OneOf Prompt: "  VF Point 5 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x452, VarStoreId: 0x1, VarOffset: 0x2A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 71 1E EF 1D 52 04 01 00 A0 02 10 10 00 01 00 }
0x3AFCD: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3AFD4: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3AFDB: 				End  { 29 02 }
0x3AFDD: 				Text Prompt: "  VF Point 5 Ratio", Help: "", Text: "N/A" { 03 08 43 1D C9 07 95 1D }
0x3AFE5: 			End  { 29 02 }
0x3AFE7: 			SuppressIf  { 0A 82 }
0x3AFE9: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3AFED: 					Uint8 Value: 0x6 { 42 03 06 }
0x3AFF0: 					LessThan  { 33 02 }
0x3AFF2: 				End  { 29 02 }
0x3AFF4: 				Numeric Prompt: "VF Point 6 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 6. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x6. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x453, VarStoreId: 0x1, VarOffset: 0x288, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 57 1E 7E 1D 53 04 01 00 88 02 10 11 00 00 E8 03 01 00 }
0x3B008: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B00F: 				End  { 29 02 }
0x3B011: 				OneOf Prompt: "  VF Point 6 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x454, VarStoreId: 0x1, VarOffset: 0x2A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 1E EF 1D 54 04 01 00 A1 02 10 10 00 01 00 }
0x3B022: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B029: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B030: 				End  { 29 02 }
0x3B032: 				Text Prompt: "  VF Point 6 Ratio", Help: "", Text: "N/A" { 03 08 45 1D C9 07 96 1D }
0x3B03A: 			End  { 29 02 }
0x3B03C: 			SuppressIf  { 0A 82 }
0x3B03E: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B042: 					Uint8 Value: 0x7 { 42 03 07 }
0x3B045: 					LessThan  { 33 02 }
0x3B047: 				End  { 29 02 }
0x3B049: 				Numeric Prompt: "VF Point 7 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 7. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x7. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x455, VarStoreId: 0x1, VarOffset: 0x28A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 58 1E 80 1D 55 04 01 00 8A 02 10 11 00 00 E8 03 01 00 }
0x3B05D: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B064: 				End  { 29 02 }
0x3B066: 				OneOf Prompt: "  VF Point 7 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x456, VarStoreId: 0x1, VarOffset: 0x2A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 73 1E EF 1D 56 04 01 00 A2 02 10 10 00 01 00 }
0x3B077: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B07E: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B085: 				End  { 29 02 }
0x3B087: 				Text Prompt: "  VF Point 7 Ratio", Help: "", Text: "N/A" { 03 08 47 1D C9 07 97 1D }
0x3B08F: 			End  { 29 02 }
0x3B091: 			SuppressIf  { 0A 82 }
0x3B093: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B097: 					Uint8 Value: 0x8 { 42 03 08 }
0x3B09A: 					LessThan  { 33 02 }
0x3B09C: 				End  { 29 02 }
0x3B09E: 				Numeric Prompt: "VF Point 8 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 8. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x8. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x457, VarStoreId: 0x1, VarOffset: 0x28C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 59 1E 82 1D 57 04 01 00 8C 02 10 11 00 00 E8 03 01 00 }
0x3B0B2: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B0B9: 				End  { 29 02 }
0x3B0BB: 				OneOf Prompt: "  VF Point 8 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x458, VarStoreId: 0x1, VarOffset: 0x2A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 1E EF 1D 58 04 01 00 A3 02 10 10 00 01 00 }
0x3B0CC: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B0D3: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B0DA: 				End  { 29 02 }
0x3B0DC: 				Text Prompt: "  VF Point 8 Ratio", Help: "", Text: "N/A" { 03 08 49 1D C9 07 98 1D }
0x3B0E4: 			End  { 29 02 }
0x3B0E6: 			SuppressIf  { 0A 82 }
0x3B0E8: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B0EC: 					Uint8 Value: 0x9 { 42 03 09 }
0x3B0EF: 					LessThan  { 33 02 }
0x3B0F1: 				End  { 29 02 }
0x3B0F3: 				Numeric Prompt: "VF Point 9 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 9. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0x9. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x459, VarStoreId: 0x1, VarOffset: 0x28E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 5A 1E 84 1D 59 04 01 00 8E 02 10 11 00 00 E8 03 01 00 }
0x3B107: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B10E: 				End  { 29 02 }
0x3B110: 				OneOf Prompt: "  VF Point 9 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x45A, VarStoreId: 0x1, VarOffset: 0x2A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 75 1E EF 1D 5A 04 01 00 A4 02 10 10 00 01 00 }
0x3B121: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B128: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B12F: 				End  { 29 02 }
0x3B131: 				Text Prompt: "  VF Point 9 Ratio", Help: "", Text: "N/A" { 03 08 4B 1D C9 07 99 1D }
0x3B139: 			End  { 29 02 }
0x3B13B: 			SuppressIf  { 0A 82 }
0x3B13D: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B141: 					Uint8 Value: 0xA { 42 03 0A }
0x3B144: 					LessThan  { 33 02 }
0x3B146: 				End  { 29 02 }
0x3B148: 				Numeric Prompt: "VF Point 10 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 10. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xA. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x45B, VarStoreId: 0x1, VarOffset: 0x290, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 5B 1E 86 1D 5B 04 01 00 90 02 10 11 00 00 E8 03 01 00 }
0x3B15C: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B163: 				End  { 29 02 }
0x3B165: 				OneOf Prompt: "  VF Point 10 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x45C, VarStoreId: 0x1, VarOffset: 0x2A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 1E EF 1D 5C 04 01 00 A5 02 10 10 00 01 00 }
0x3B176: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B17D: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B184: 				End  { 29 02 }
0x3B186: 				Text Prompt: "  VF Point 10 Ratio", Help: "", Text: "N/A" { 03 08 4D 1D C9 07 9A 1D }
0x3B18E: 			End  { 29 02 }
0x3B190: 			SuppressIf  { 0A 82 }
0x3B192: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B196: 					Uint8 Value: 0xB { 42 03 0B }
0x3B199: 					LessThan  { 33 02 }
0x3B19B: 				End  { 29 02 }
0x3B19D: 				Numeric Prompt: "VF Point 11 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 11. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xB. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x45D, VarStoreId: 0x1, VarOffset: 0x292, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 5C 1E 88 1D 5D 04 01 00 92 02 10 11 00 00 E8 03 01 00 }
0x3B1B1: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B1B8: 				End  { 29 02 }
0x3B1BA: 				OneOf Prompt: "  VF Point 11 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x45E, VarStoreId: 0x1, VarOffset: 0x2A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 77 1E EF 1D 5E 04 01 00 A6 02 10 10 00 01 00 }
0x3B1CB: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B1D2: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B1D9: 				End  { 29 02 }
0x3B1DB: 				Text Prompt: "  VF Point 11 Ratio", Help: "", Text: "N/A" { 03 08 4F 1D C9 07 9B 1D }
0x3B1E3: 			End  { 29 02 }
0x3B1E5: 			SuppressIf  { 0A 82 }
0x3B1E7: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B1EB: 					Uint8 Value: 0xC { 42 03 0C }
0x3B1EE: 					LessThan  { 33 02 }
0x3B1F0: 				End  { 29 02 }
0x3B1F2: 				Numeric Prompt: "VF Point 12 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 12. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xC. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x45F, VarStoreId: 0x1, VarOffset: 0x294, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 5D 1E 8A 1D 5F 04 01 00 94 02 10 11 00 00 E8 03 01 00 }
0x3B206: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B20D: 				End  { 29 02 }
0x3B20F: 				OneOf Prompt: "  VF Point 12 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x460, VarStoreId: 0x1, VarOffset: 0x2A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 1E EF 1D 60 04 01 00 A7 02 10 10 00 01 00 }
0x3B220: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B227: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B22E: 				End  { 29 02 }
0x3B230: 				Text Prompt: "  VF Point 12 Ratio", Help: "", Text: "N/A" { 03 08 51 1D C9 07 9C 1D }
0x3B238: 			End  { 29 02 }
0x3B23A: 			SuppressIf  { 0A 82 }
0x3B23C: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B240: 					Uint8 Value: 0xD { 42 03 0D }
0x3B243: 					LessThan  { 33 02 }
0x3B245: 				End  { 29 02 }
0x3B247: 				Numeric Prompt: "VF Point 13 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 13. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xD. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x461, VarStoreId: 0x1, VarOffset: 0x296, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 5E 1E 8C 1D 61 04 01 00 96 02 10 11 00 00 E8 03 01 00 }
0x3B25B: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B262: 				End  { 29 02 }
0x3B264: 				OneOf Prompt: "  VF Point 13 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x462, VarStoreId: 0x1, VarOffset: 0x2A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 79 1E EF 1D 62 04 01 00 A8 02 10 10 00 01 00 }
0x3B275: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B27C: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B283: 				End  { 29 02 }
0x3B285: 				Text Prompt: "  VF Point 13 Ratio", Help: "", Text: "N/A" { 03 08 53 1D C9 07 9D 1D }
0x3B28D: 			End  { 29 02 }
0x3B28F: 			SuppressIf  { 0A 82 }
0x3B291: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B295: 					Uint8 Value: 0xE { 42 03 0E }
0x3B298: 					LessThan  { 33 02 }
0x3B29A: 				End  { 29 02 }
0x3B29C: 				Numeric Prompt: "VF Point 14 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 14. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xE. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x463, VarStoreId: 0x1, VarOffset: 0x298, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 5F 1E 8E 1D 63 04 01 00 98 02 10 11 00 00 E8 03 01 00 }
0x3B2B0: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B2B7: 				End  { 29 02 }
0x3B2B9: 				OneOf Prompt: "  VF Point 14 Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x464, VarStoreId: 0x1, VarOffset: 0x2A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 1E EF 1D 64 04 01 00 A9 02 10 10 00 01 00 }
0x3B2CA: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B2D1: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B2D8: 				End  { 29 02 }
0x3B2DA: 				Text Prompt: "  VF Point 14 Ratio", Help: "", Text: "N/A" { 03 08 55 1D C9 07 9E 1D }
0x3B2E2: 			End  { 29 02 }
0x3B2E4: 			SuppressIf  { 0A 82 }
0x3B2E6: 				QuestionRef1 QuestionId: 0x11E7 { 40 84 E7 11 }
0x3B2EA: 					Uint8 Value: 0xF { 42 03 0F }
0x3B2ED: 					LessThan  { 33 02 }
0x3B2EF: 				End  { 29 02 }
0x3B2F1: 				Numeric Prompt: "VF Point 15 Offset", Help: "Specifies the Offset Voltage applied to the Selected VF Point 15. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11, Param1 0:Core 2:Ring, Param2 0xF. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x465, VarStoreId: 0x1, VarOffset: 0x29A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 60 1E 90 1D 65 04 01 00 9A 02 10 11 00 00 E8 03 01 00 }
0x3B305: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B30C: 				End  { 29 02 }
0x3B30E: 				OneOf Prompt: "", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x466, VarStoreId: 0x1, VarOffset: 0x2AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7B 1E EF 1D 66 04 01 00 AA 02 10 10 00 01 00 }
0x3B31F: 					OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B326: 					OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B32D: 				End  { 29 02 }
0x3B32F: 				Text Prompt: "  VF Point 15 Ratio", Help: "", Text: "N/A" { 03 08 57 1D C9 07 9F 1D }
0x3B337: 			End  { 29 02 }
0x3B339: 		End  { 29 02 }
0x3B33B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B342: 		End  { 29 02 }
0x3B344: 		OneOf Prompt: "Ring Down Bin", Help: "Enable/Disable Ring Downbin feature. Enabled - CPU will down bin the ring ratio, which means the requested max ring ratio will not be observed. Disable - CPU will not down bin the ring ratio and the requested ring ratio limit will be observed. Default for Overclocking is "Disabled" to allow for a predictable ring ratio. Uses OC mailbox command 0x19.", QuestionFlags: 0x10, QuestionId: 0x467, VarStoreId: 0x1, VarOffset: 0x1E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1D 1E 1E 1E 67 04 01 00 E8 01 10 10 00 01 00 }
0x3B355: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3B35C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3B363: 		End  { 29 02 }
0x3B365: 		Numeric Prompt: "Min Ring Ratio Limit", Help: "This sets the minimum ring ratio limit. 0 - Auto/HW default. 1-LFM are invalid ratio settings.", QuestionFlags: 0x14, QuestionId: 0x2886, VarStoreId: 0x1, VarOffset: 0x210, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 1F 1E 20 1E 86 28 01 00 10 02 14 10 00 55 01 }
0x3B376: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B37C: 		End  { 29 02 }
0x3B37E: 		Numeric Prompt: "Max Ring Ratio Limit", Help: "This sets the maximum ring ratio limit. 0 - Auto/HW default. 1-LFM are invalid ratio settings.", QuestionFlags: 0x14, QuestionId: 0x2887, VarStoreId: 0x1, VarOffset: 0x211, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x55, Step: 0x1 { 07 91 21 1E 22 1E 87 28 01 00 11 02 14 10 00 55 01 }
0x3B38F: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B395: 		End  { 29 02 }
0x3B397: 	End  { 29 02 }
0x3B399: 	Form FormId: 0x288D, Title: "GT" { 01 86 8D 28 0A 1E }
0x3B39F: 		Subtitle Prompt: "GT Domain", Help: "", Flags: 0x0 { 02 87 0F 1E 00 00 00 }
0x3B3A6: 		End  { 29 02 }
0x3B3A8: 		Numeric Prompt: "GT OverClocking Frequency", Help: "Overclocked RP0 Frequency (MLC Clk) in multiples of 50 MHz", QuestionFlags: 0x10, QuestionId: 0x468, VarStoreId: 0x4, VarOffset: 0x262, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2A, Step: 0x1 { 07 91 0C 1E 0E 1E 68 04 04 00 62 02 10 10 00 2A 01 }
0x3B3B9: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B3BF: 		End  { 29 02 }
0x3B3C1: 		OneOf Prompt: "  GT Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x469, VarStoreId: 0x4, VarOffset: 0x263, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 1E 13 1E 69 04 04 00 63 02 10 10 00 01 00 }
0x3B3D2: 			OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault { 09 07 D5 1D 30 00 00 }
0x3B3D9: 			OneOfOption Option: "Override" Value: 1 { 09 07 D6 1D 00 00 01 }
0x3B3E0: 		End  { 29 02 }
0x3B3E2: 		SuppressIf  { 0A 82 }
0x3B3E4: 			EqIdVal QuestionId: 0x469, Value: 0x0 { 12 06 69 04 00 00 }
0x3B3EA: 			Numeric Prompt: "  GT Voltage Override", Help: "Specifies the Override Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x46A, VarStoreId: 0x4, VarOffset: 0x267, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 14 1E 16 1E 6A 04 04 00 67 02 10 11 00 00 D0 07 01 00 }
0x3B3FE: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B405: 			End  { 29 02 }
0x3B407: 		End  { 29 02 }
0x3B409: 		SuppressIf  { 0A 82 }
0x3B40B: 			EqIdVal QuestionId: 0x469, Value: 0x1 { 12 06 69 04 01 00 }
0x3B411: 			Numeric Prompt: "  GT Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while GT is operating in turbo mode. Unit is in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x46B, VarStoreId: 0x4, VarOffset: 0x269, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 1A 1E 1C 1E 6B 04 04 00 69 02 10 11 00 00 D0 07 01 00 }
0x3B425: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B42C: 			End  { 29 02 }
0x3B42E: 		End  { 29 02 }
0x3B430: 		Numeric Prompt: "  GT Voltage Offset", Help: "Specifies the Offset Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -1000 to 1000 mV", QuestionFlags: 0x10, QuestionId: 0x46C, VarStoreId: 0x4, VarOffset: 0x264, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 17 1E 19 1E 6C 04 04 00 64 02 10 11 00 00 E8 03 01 00 }
0x3B444: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B44B: 		End  { 29 02 }
0x3B44D: 		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x46D, VarStoreId: 0x4, VarOffset: 0x266, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EC 1D EF 1D 6D 04 04 00 66 02 10 10 00 01 00 }
0x3B45E: 			OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B465: 			OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B46C: 		End  { 29 02 }
0x3B46E: 		SuppressIf  { 0A 82 }
0x3B470: 			EqIdVal QuestionId: 0x11E6, Value: 0x0 { 12 06 E6 11 00 00 }
0x3B476: 			Subtitle Prompt: "GT Unslice Domain", Help: "", Flags: 0x0 { 02 87 10 1E 00 00 00 }
0x3B47D: 			End  { 29 02 }
0x3B47F: 			Numeric Prompt: "GT OverClocking Frequency", Help: "Overclocked RP0 Frequency (MLC Clk) in multiples of 50 MHz", QuestionFlags: 0x10, QuestionId: 0x46E, VarStoreId: 0x4, VarOffset: 0x26B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2A, Step: 0x1 { 07 91 0D 1E 0E 1E 6E 04 04 00 6B 02 10 10 00 2A 01 }
0x3B490: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B496: 			End  { 29 02 }
0x3B498: 			OneOf Prompt: "  GT Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x46F, VarStoreId: 0x4, VarOffset: 0x26C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 12 1E 13 1E 6F 04 04 00 6C 02 10 10 00 01 00 }
0x3B4A9: 				OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault { 09 07 D5 1D 30 00 00 }
0x3B4B0: 				OneOfOption Option: "Override" Value: 1 { 09 07 D6 1D 00 00 01 }
0x3B4B7: 			End  { 29 02 }
0x3B4B9: 			SuppressIf  { 0A 82 }
0x3B4BB: 				EqIdVal QuestionId: 0x46F, Value: 0x0 { 12 06 6F 04 00 00 }
0x3B4C1: 				Numeric Prompt: "  GT Voltage Override", Help: "Specifies the Override Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x470, VarStoreId: 0x4, VarOffset: 0x270, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 15 1E 16 1E 70 04 04 00 70 02 10 11 00 00 D0 07 01 00 }
0x3B4D5: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B4DC: 				End  { 29 02 }
0x3B4DE: 			End  { 29 02 }
0x3B4E0: 			SuppressIf  { 0A 82 }
0x3B4E2: 				EqIdVal QuestionId: 0x46F, Value: 0x1 { 12 06 6F 04 01 00 }
0x3B4E8: 				Numeric Prompt: "  GT Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while GT is operating in turbo mode. Unit is in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x471, VarStoreId: 0x4, VarOffset: 0x272, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 1B 1E 1C 1E 71 04 04 00 72 02 10 11 00 00 D0 07 01 00 }
0x3B4FC: 					Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B503: 				End  { 29 02 }
0x3B505: 			End  { 29 02 }
0x3B507: 			Numeric Prompt: "  GTU Voltage Offset", Help: "Specifies the Offset Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -1000 to 1000 mV", QuestionFlags: 0x10, QuestionId: 0x472, VarStoreId: 0x4, VarOffset: 0x26D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 18 1E 19 1E 72 04 04 00 6D 02 10 11 00 00 E8 03 01 00 }
0x3B51B: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B522: 			End  { 29 02 }
0x3B524: 			OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x473, VarStoreId: 0x4, VarOffset: 0x26F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 ED 1D EF 1D 73 04 04 00 6F 02 10 10 00 01 00 }
0x3B535: 				OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B53C: 				OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B543: 			End  { 29 02 }
0x3B545: 		End  { 29 02 }
0x3B547: 	End  { 29 02 }
0x3B549: 	Form FormId: 0x288E, Title: "Uncore" { 01 86 8E 28 23 1E }
0x3B54F: 		Subtitle Prompt: "Uncore", Help: "", Flags: 0x0 { 02 87 23 1E 00 00 00 }
0x3B556: 		End  { 29 02 }
0x3B558: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B55F: 		End  { 29 02 }
0x3B561: 		OneOf Prompt: "Uncore Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x474, VarStoreId: 0x1, VarOffset: 0x2DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 1E 28 1E 74 04 01 00 DE 02 10 10 00 01 00 }
0x3B572: 			OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault { 09 07 D5 1D 30 00 00 }
0x3B579: 			OneOfOption Option: "Override" Value: 1 { 09 07 D6 1D 00 00 01 }
0x3B580: 		End  { 29 02 }
0x3B582: 		SuppressIf  { 0A 82 }
0x3B584: 			EqIdVal QuestionId: 0x474, Value: 0x0 { 12 06 74 04 00 00 }
0x3B58A: 			Numeric Prompt: "Uncore Voltage Override", Help: "Specifies the Override Voltage applied to the SA Uncore domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV.", QuestionFlags: 0x10, QuestionId: 0x475, VarStoreId: 0x1, VarOffset: 0x2DF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 29 1E 2A 1E 75 04 01 00 DF 02 10 11 00 00 D0 07 01 00 }
0x3B59E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B5A5: 			End  { 29 02 }
0x3B5A7: 		End  { 29 02 }
0x3B5A9: 		SuppressIf  { 0A 82 }
0x3B5AB: 			EqIdVal QuestionId: 0x474, Value: 0x1 { 12 06 74 04 01 00 }
0x3B5B1: 			Numeric Prompt: "Uncore Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while SA Uncore is operating in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x476, VarStoreId: 0x1, VarOffset: 0x2E1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1 { 07 94 2B 1E 2C 1E 76 04 01 00 E1 02 10 11 00 00 D0 07 01 00 }
0x3B5C5: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B5CC: 			End  { 29 02 }
0x3B5CE: 		End  { 29 02 }
0x3B5D0: 		Numeric Prompt: "Uncore Voltage Offset", Help: "Specifies the Offset Voltage applied to the Uncore domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -1000 to 1000 mV", QuestionFlags: 0x10, QuestionId: 0x477, VarStoreId: 0x4, VarOffset: 0x25F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1 { 07 94 25 1E 26 1E 77 04 04 00 5F 02 10 11 00 00 E8 03 01 00 }
0x3B5E4: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3B5EB: 		End  { 29 02 }
0x3B5ED: 		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x478, VarStoreId: 0x4, VarOffset: 0x261, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EE 1D EF 1D 78 04 04 00 61 02 10 10 00 01 00 }
0x3B5FE: 			OneOfOption Option: "+" Value: 0, Default, MfgDefault { 09 07 BD 03 30 00 00 }
0x3B605: 			OneOfOption Option: "-" Value: 1 { 09 07 BE 03 00 00 01 }
0x3B60C: 		End  { 29 02 }
0x3B60E: 	End  { 29 02 }
0x3B610: 	Form FormId: 0x288F, Title: "Platform Voltage Overrides" { 01 86 8F 28 F0 1D }
0x3B616: 		Subtitle Prompt: "Platform Voltage Overrides", Help: "", Flags: 0x0 { 02 87 F0 1D 00 00 00 }
0x3B61D: 		End  { 29 02 }
0x3B61F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B626: 		End  { 29 02 }
0x3B628: 		OneOf Prompt: "Vcc1p8 Override Enable", Help: "Overrides the Vcc1p8 voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x479, VarStoreId: 0x1, VarOffset: 0x321, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F2 1D F3 1D 79 04 01 00 21 03 10 10 00 01 00 }
0x3B639: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B640: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B647: 		End  { 29 02 }
0x3B649: 		SuppressIf  { 0A 82 }
0x3B64B: 			EqIdVal QuestionId: 0x479, Value: 0x0 { 12 06 79 04 00 00 }
0x3B651: 			Numeric Prompt: "  Vcc1p8", Help: "Range of Vcc1p8 voltage - Default is 1800 mV", QuestionFlags: 0x10, QuestionId: 0x47A, VarStoreId: 0x1, VarOffset: 0x322, Flags: 0x11, Size: 16, Min: 0x320, Max: 0x9F6, Step: 0xA { 07 94 F4 1D F5 1D 7A 04 01 00 22 03 10 11 20 03 F6 09 0A 00 }
0x3B665: 				Default DefaultId: 0x0 Value: 1800 { 5B 07 00 00 01 08 07 }
0x3B66C: 			End  { 29 02 }
0x3B66E: 		End  { 29 02 }
0x3B670: 		OneOf Prompt: "Vcc1p05 Override Enable", Help: "Overrides the Vcc1p05 voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x47B, VarStoreId: 0x1, VarOffset: 0x324, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F6 1D F7 1D 7B 04 01 00 24 03 10 10 00 01 00 }
0x3B681: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B688: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B68F: 		End  { 29 02 }
0x3B691: 		SuppressIf  { 0A 82 }
0x3B693: 			EqIdVal QuestionId: 0x47B, Value: 0x0 { 12 06 7B 04 00 00 }
0x3B699: 			Numeric Prompt: "  Vcc1p05", Help: "Range of Vcc1p05 voltage - Default is 1050 mV", QuestionFlags: 0x10, QuestionId: 0x47C, VarStoreId: 0x1, VarOffset: 0x325, Flags: 0x11, Size: 16, Min: 0x320, Max: 0x9F6, Step: 0xA { 07 94 F8 1D F9 1D 7C 04 01 00 25 03 10 11 20 03 F6 09 0A 00 }
0x3B6AD: 				Default DefaultId: 0x0 Value: 1050 { 5B 07 00 00 01 1A 04 }
0x3B6B4: 			End  { 29 02 }
0x3B6B6: 		End  { 29 02 }
0x3B6B8: 		OneOf Prompt: "VccDD2 Override Enable", Help: "Overrides the VccDD2 voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x47D, VarStoreId: 0x1, VarOffset: 0x327, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 1D FB 1D 7D 04 01 00 27 03 10 10 00 01 00 }
0x3B6C9: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B6D0: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B6D7: 		End  { 29 02 }
0x3B6D9: 		SuppressIf  { 0A 82 }
0x3B6DB: 			EqIdVal QuestionId: 0x47D, Value: 0x0 { 12 06 7D 04 00 00 }
0x3B6E1: 			Numeric Prompt: "  VccDD2", Help: "Range of VccDD2 voltage - Default is 1100 mV", QuestionFlags: 0x10, QuestionId: 0x47E, VarStoreId: 0x1, VarOffset: 0x328, Flags: 0x11, Size: 16, Min: 0x320, Max: 0x9F6, Step: 0xA { 07 94 FC 1D FD 1D 7E 04 01 00 28 03 10 11 20 03 F6 09 0A 00 }
0x3B6F5: 				Default DefaultId: 0x0 Value: 1100 { 5B 07 00 00 01 4C 04 }
0x3B6FC: 			End  { 29 02 }
0x3B6FE: 		End  { 29 02 }
0x3B700: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B707: 		End  { 29 02 }
0x3B709: 		OneOf Prompt: "VCCIN AUX CPU Overrides Enable", Help: "VCCIN AUX CPU Voltage Overrides from SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x47F, VarStoreId: 0x1, VarOffset: 0x336, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 1E 34 1E 7F 04 01 00 36 03 10 10 00 01 00 }
0x3B71A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B721: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B728: 		End  { 29 02 }
0x3B72A: 		SuppressIf  { 0A 82 }
0x3B72C: 			EqIdVal QuestionId: 0x47F, Value: 0x0 { 12 06 7F 04 00 00 }
0x3B732: 			Numeric Prompt: "  VCCIN AUX CPU", Help: "Voltage Range of VCCIN AUX CPU from 1620mV - 1900mV; Default is 1800 mV", QuestionFlags: 0x10, QuestionId: 0x480, VarStoreId: 0x1, VarOffset: 0x337, Flags: 0x11, Size: 16, Min: 0x654, Max: 0x76C, Step: 0xA { 07 94 35 1E 36 1E 80 04 01 00 37 03 10 11 54 06 6C 07 0A 00 }
0x3B746: 				Default DefaultId: 0x0 Value: 1800 { 5B 07 00 00 01 08 07 }
0x3B74D: 			End  { 29 02 }
0x3B74F: 		End  { 29 02 }
0x3B751: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B758: 		End  { 29 02 }
0x3B75A: 		OneOf Prompt: "RichTek VccIA Control Overrides", Help: "VccIA Voltage can be overrides from Richtek SMBUS/PMBUS VR. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x481, VarStoreId: 0x1, VarOffset: 0x339, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 1E 3A 1E 81 04 01 00 39 03 10 10 00 01 00 }
0x3B76B: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B772: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B779: 		End  { 29 02 }
0x3B77B: 		SuppressIf  { 0A 82 }
0x3B77D: 			EqIdVal QuestionId: 0x481, Value: 0x0 { 12 06 81 04 00 00 }
0x3B783: 			OneOf Prompt: " Fixed VID Mode", Help: "Fixed VID Mode Enabled for the VccIA/VccGT Voltage rail Overrides from Richtek SMBUS/PMBUS VR. When Disabled, voltage rail will use IMVP from SVID BUS.", QuestionFlags: 0x10, QuestionId: 0x482, VarStoreId: 0x1, VarOffset: 0x33B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 37 1E 38 1E 82 04 01 00 3B 03 10 10 00 01 00 }
0x3B794: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B79B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B7A2: 			End  { 29 02 }
0x3B7A4: 			SuppressIf  { 0A 82 }
0x3B7A6: 				EqIdVal QuestionId: 0x482, Value: 0x0 { 12 06 82 04 00 00 }
0x3B7AC: 				Numeric Prompt: "  VccIA (mV)", Help: "Voltage Range of RichTek VccIA from 250mV - 2170mV; Default is 1200 mV", QuestionFlags: 0x10, QuestionId: 0x483, VarStoreId: 0x1, VarOffset: 0x33D, Flags: 0x11, Size: 16, Min: 0xFA, Max: 0x87A, Step: 0xA { 07 94 3B 1E 3C 1E 83 04 01 00 3D 03 10 11 FA 00 7A 08 0A 00 }
0x3B7C0: 					Default DefaultId: 0x0 Value: 1200 { 5B 07 00 00 01 B0 04 }
0x3B7C7: 				End  { 29 02 }
0x3B7C9: 			End  { 29 02 }
0x3B7CB: 		End  { 29 02 }
0x3B7CD: 		OneOf Prompt: "RichTek VccGT Control Overrides", Help: "VccGT Voltage can be overrides from Richtek SMBUS/PMBUS VR. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x484, VarStoreId: 0x1, VarOffset: 0x33A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 1E 3E 1E 84 04 01 00 3A 03 10 10 00 01 00 }
0x3B7DE: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B7E5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B7EC: 		End  { 29 02 }
0x3B7EE: 		SuppressIf  { 0A 82 }
0x3B7F0: 			EqIdVal QuestionId: 0x484, Value: 0x0 { 12 06 84 04 00 00 }
0x3B7F6: 			OneOf Prompt: " Fixed VID Mode", Help: "Fixed VID Mode Enabled for the VccIA/VccGT Voltage rail Overrides from Richtek SMBUS/PMBUS VR. When Disabled, voltage rail will use IMVP from SVID BUS.", QuestionFlags: 0x10, QuestionId: 0x485, VarStoreId: 0x1, VarOffset: 0x33C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7C 1E 38 1E 85 04 01 00 3C 03 10 10 00 01 00 }
0x3B807: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B80E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B815: 			End  { 29 02 }
0x3B817: 			SuppressIf  { 0A 82 }
0x3B819: 				EqIdVal QuestionId: 0x485, Value: 0x0 { 12 06 85 04 00 00 }
0x3B81F: 				Numeric Prompt: "  VccGT (mV)", Help: "Voltage Range of RichTek VccGT from 250mV - 2170mV; Default is 1200 mV", QuestionFlags: 0x10, QuestionId: 0x486, VarStoreId: 0x1, VarOffset: 0x33F, Flags: 0x11, Size: 16, Min: 0xFA, Max: 0x87A, Step: 0xA { 07 94 3F 1E 40 1E 86 04 01 00 3F 03 10 11 FA 00 7A 08 0A 00 }
0x3B833: 					Default DefaultId: 0x0 Value: 1200 { 5B 07 00 00 01 B0 04 }
0x3B83A: 				End  { 29 02 }
0x3B83C: 			End  { 29 02 }
0x3B83E: 		End  { 29 02 }
0x3B840: 	End  { 29 02 }
0x3B842: 	Form FormId: 0x2890, Title: "Voltage PLL Trim Controls" { 01 86 90 28 B6 1C }
0x3B848: 		Subtitle Prompt: "Voltage PLL Trim Controls", Help: "", Flags: 0x0 { 02 87 B6 1C 00 00 00 }
0x3B84F: 		End  { 29 02 }
0x3B851: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B858: 		End  { 29 02 }
0x3B85A: 		Numeric Prompt: "Core PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-15. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x487, VarStoreId: 0x1, VarOffset: 0x1F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 AA 1D B0 1D 87 04 01 00 F2 01 10 10 00 0F 01 }
0x3B86B: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B871: 		End  { 29 02 }
0x3B873: 		Numeric Prompt: "GT PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-15. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x488, VarStoreId: 0x1, VarOffset: 0x1F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 AB 1D B0 1D 88 04 01 00 F3 01 10 10 00 0F 01 }
0x3B884: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B88A: 		End  { 29 02 }
0x3B88C: 		Numeric Prompt: "Ring PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-15. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x489, VarStoreId: 0x1, VarOffset: 0x1F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 AC 1D B0 1D 89 04 01 00 F4 01 10 10 00 0F 01 }
0x3B89D: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B8A3: 		End  { 29 02 }
0x3B8A5: 		Numeric Prompt: "System Agent PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-15. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x48A, VarStoreId: 0x1, VarOffset: 0x1F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 AD 1D B0 1D 8A 04 01 00 F5 01 10 10 00 0F 01 }
0x3B8B6: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B8BC: 		End  { 29 02 }
0x3B8BE: 		SuppressIf  { 0A 82 }
0x3B8C0: 			EqIdVal QuestionId: 0x11E5, Value: 0x0 { 12 86 E5 11 00 00 }
0x3B8C6: 				EqIdVal QuestionId: 0x1ED, Value: 0x0 { 12 06 ED 01 00 00 }
0x3B8CC: 				Or  { 16 02 }
0x3B8CE: 			End  { 29 02 }
0x3B8D0: 			Numeric Prompt: "Efficient-core PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-15. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x48B, VarStoreId: 0x1, VarOffset: 0x1F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 AE 1D B0 1D 8B 04 01 00 F6 01 10 10 00 0F 01 }
0x3B8E1: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B8E7: 			End  { 29 02 }
0x3B8E9: 		End  { 29 02 }
0x3B8EB: 		Numeric Prompt: "Memory Controller PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-15. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x48C, VarStoreId: 0x1, VarOffset: 0x1F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 AF 1D B0 1D 8C 04 01 00 F7 01 10 10 00 0F 01 }
0x3B8FC: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3B902: 		End  { 29 02 }
0x3B904: 	End  { 29 02 }
0x3B906: 	Form FormId: 0x2891, Title: "CEP Disable" { 01 86 91 28 BD 1D }
0x3B90C: 		Subtitle Prompt: "CEP Disable", Help: "", Flags: 0x0 { 02 87 BD 1D 00 00 00 }
0x3B913: 		End  { 29 02 }
0x3B915: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B91C: 		End  { 29 02 }
0x3B91E: 		OneOf Prompt: "IA CEP Enable", Help: "Enable/Disable IA CEP (Current Excursion Protection) Support. Uses pCode Mailbox Command 0x37, Sub-command 0x1. Set Data bit2 to 1.", QuestionFlags: 0x10, QuestionId: 0x48D, VarStoreId: 0x1, VarOffset: 0x334, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 1D C0 1D 8D 04 01 00 34 03 10 10 00 01 00 }
0x3B92F: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3B936: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3B93D: 		End  { 29 02 }
0x3B93F: 		OneOf Prompt: "GT CEP Enable", Help: "Enable/Disable GT CEP (Current Excursion Protection) Support. Uses pCode Mailbox Command 0x37, Sub-command 0x1. Set Data bit3 to 1.", QuestionFlags: 0x10, QuestionId: 0x48E, VarStoreId: 0x1, VarOffset: 0x335, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 1D C2 1D 8E 04 01 00 35 03 10 10 00 01 00 }
0x3B950: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3B957: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3B95E: 		End  { 29 02 }
0x3B960: 	End  { 29 02 }
0x3B962: 	Form FormId: 0x2892, Title: "VR ICCMAX Current Override" { 01 86 92 28 C3 1D }
0x3B968: 		Subtitle Prompt: "VR ICCMAX Current Override", Help: "", Flags: 0x0 { 02 87 C3 1D 00 00 00 }
0x3B96F: 		End  { 29 02 }
0x3B971: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B978: 		End  { 29 02 }
0x3B97A: 		SuppressIf  { 0A 82 }
0x3B97C: 			EqIdVal QuestionId: 0x11E4, Value: 0x1 { 12 06 E4 11 01 00 }
0x3B982: 			Text Prompt: "Current IA VR Current Limit", Help: "Current IA VR Current Limit", Text: "" { 03 08 C6 1D C5 1D C7 1D }
0x3B98A: 		End  { 29 02 }
0x3B98C: 		SuppressIf  { 0A 82 }
0x3B98E: 			EqIdVal QuestionId: 0x11E3, Value: 0x1 { 12 06 E3 11 01 00 }
0x3B994: 			Text Prompt: "Current GT VR Current Limit", Help: "Current GT VR Current Limit", Text: "" { 03 08 C9 1D C8 1D CA 1D }
0x3B99C: 		End  { 29 02 }
0x3B99E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3B9A5: 		End  { 29 02 }
0x3B9A7: 		GrayOutIf  { 19 82 }
0x3B9A9: 			EqIdVal QuestionId: 0x11E4, Value: 0x1 { 12 06 E4 11 01 00 }
0x3B9AF: 			GrayOutIf  { 19 82 }
0x3B9B1: 				EqIdVal QuestionId: 0x490, Value: 0x1 { 12 06 90 04 01 00 }
0x3B9B7: 				Numeric Prompt: "IA ICC Max Current Limit Override", Help: "IA Voltage Regulator Current Limit (Icc Max). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. Range is 4 to 2047. Uses OC mailbox command 0x17", QuestionFlags: 0x10, QuestionId: 0x48F, VarStoreId: 0x1, VarOffset: 0x347, Flags: 0x11, Size: 16, Min: 0x4, Max: 0x7FF, Step: 0x1 { 07 94 CB 1D CC 1D 8F 04 01 00 47 03 10 11 04 00 FF 07 01 00 }
0x3B9CB: 					Default DefaultId: 0x0 Value: 4 { 5B 07 00 00 01 04 00 }
0x3B9D2: 				End  { 29 02 }
0x3B9D4: 			End  { 29 02 }
0x3B9D6: 			OneOf Prompt: "IA ICC Unlimited Mode", Help: "Enable/Disable IA Unlimited ICCMAX. When Enabled, IA VR ICCMAX value is set to max ICC current 512A.", QuestionFlags: 0x10, QuestionId: 0x490, VarStoreId: 0x1, VarOffset: 0x346, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CD 1D CE 1D 90 04 01 00 46 03 10 10 00 01 00 }
0x3B9E7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3B9EE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3B9F5: 			End  { 29 02 }
0x3B9F7: 		End  { 29 02 }
0x3B9F9: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3BA00: 		End  { 29 02 }
0x3BA02: 		GrayOutIf  { 19 82 }
0x3BA04: 			EqIdVal QuestionId: 0x11E3, Value: 0x1 { 12 06 E3 11 01 00 }
0x3BA0A: 			GrayOutIf  { 19 82 }
0x3BA0C: 				EqIdVal QuestionId: 0x492, Value: 0x1 { 12 06 92 04 01 00 }
0x3BA12: 				Numeric Prompt: "GT ICC Max Current Limit Override", Help: "GT Voltage Regulator Current Limit (Icc Max). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. Range is 4 to 2047. Uses OC mailbox command 0x17", QuestionFlags: 0x10, QuestionId: 0x491, VarStoreId: 0x1, VarOffset: 0x34A, Flags: 0x11, Size: 16, Min: 0x4, Max: 0x7FF, Step: 0x1 { 07 94 CF 1D D0 1D 91 04 01 00 4A 03 10 11 04 00 FF 07 01 00 }
0x3BA26: 					Default DefaultId: 0x0 Value: 4 { 5B 07 00 00 01 04 00 }
0x3BA2D: 				End  { 29 02 }
0x3BA2F: 			End  { 29 02 }
0x3BA31: 			OneOf Prompt: "GT ICC Unlimited Mode", Help: "Enable/Disable GT Unlimited ICCMAX. When Enabled, GT VR ICCMAX value is set to max ICC current 512A.", QuestionFlags: 0x10, QuestionId: 0x492, VarStoreId: 0x1, VarOffset: 0x349, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 1D D2 1D 92 04 01 00 49 03 10 10 00 01 00 }
0x3BA42: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3BA49: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3BA50: 			End  { 29 02 }
0x3BA52: 		End  { 29 02 }
0x3BA54: 	End  { 29 02 }
0x3BA56: 	Form FormId: 0x2893, Title: "  Processor Disable" { 01 86 93 28 C6 1C }
0x3BA5C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3BA63: 		End  { 29 02 }
0x3BA65: 		SuppressIf  { 0A 82 }
0x3BA67: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BA6E: 				Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3BA78: 				BitwiseAnd  { 35 02 }
0x3BA7A: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BA84: 				NotEqual  { 30 02 }
0x3BA86: 			End  { 29 02 }
0x3BA88: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x493, VarStoreId: 0x1, VarOffset: 0x358, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E C8 1C E8 1C 93 04 01 00 58 03 10 00 }
0x3BA96: 			End  { 29 02 }
0x3BA98: 		End  { 29 02 }
0x3BA9A: 		SuppressIf  { 0A 82 }
0x3BA9C: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BAA3: 				Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x3BAAD: 				BitwiseAnd  { 35 02 }
0x3BAAF: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BAB9: 				NotEqual  { 30 02 }
0x3BABB: 			End  { 29 02 }
0x3BABD: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x494, VarStoreId: 0x1, VarOffset: 0x359, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E C9 1C E9 1C 94 04 01 00 59 03 10 00 }
0x3BACB: 			End  { 29 02 }
0x3BACD: 		End  { 29 02 }
0x3BACF: 		SuppressIf  { 0A 82 }
0x3BAD1: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BAD8: 				Uint64 Value: 0x4 { 45 0A 04 00 00 00 00 00 00 00 }
0x3BAE2: 				BitwiseAnd  { 35 02 }
0x3BAE4: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BAEE: 				NotEqual  { 30 02 }
0x3BAF0: 			End  { 29 02 }
0x3BAF2: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x495, VarStoreId: 0x1, VarOffset: 0x35A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CA 1C EA 1C 95 04 01 00 5A 03 10 00 }
0x3BB00: 			End  { 29 02 }
0x3BB02: 		End  { 29 02 }
0x3BB04: 		SuppressIf  { 0A 82 }
0x3BB06: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BB0D: 				Uint64 Value: 0x8 { 45 0A 08 00 00 00 00 00 00 00 }
0x3BB17: 				BitwiseAnd  { 35 02 }
0x3BB19: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BB23: 				NotEqual  { 30 02 }
0x3BB25: 			End  { 29 02 }
0x3BB27: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x496, VarStoreId: 0x1, VarOffset: 0x35B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CB 1C EB 1C 96 04 01 00 5B 03 10 00 }
0x3BB35: 			End  { 29 02 }
0x3BB37: 		End  { 29 02 }
0x3BB39: 		SuppressIf  { 0A 82 }
0x3BB3B: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BB42: 				Uint64 Value: 0x10 { 45 0A 10 00 00 00 00 00 00 00 }
0x3BB4C: 				BitwiseAnd  { 35 02 }
0x3BB4E: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BB58: 				NotEqual  { 30 02 }
0x3BB5A: 			End  { 29 02 }
0x3BB5C: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x497, VarStoreId: 0x1, VarOffset: 0x35C, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CC 1C EC 1C 97 04 01 00 5C 03 10 00 }
0x3BB6A: 			End  { 29 02 }
0x3BB6C: 		End  { 29 02 }
0x3BB6E: 		SuppressIf  { 0A 82 }
0x3BB70: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BB77: 				Uint64 Value: 0x20 { 45 0A 20 00 00 00 00 00 00 00 }
0x3BB81: 				BitwiseAnd  { 35 02 }
0x3BB83: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BB8D: 				NotEqual  { 30 02 }
0x3BB8F: 			End  { 29 02 }
0x3BB91: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x498, VarStoreId: 0x1, VarOffset: 0x35D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CD 1C ED 1C 98 04 01 00 5D 03 10 00 }
0x3BB9F: 			End  { 29 02 }
0x3BBA1: 		End  { 29 02 }
0x3BBA3: 		SuppressIf  { 0A 82 }
0x3BBA5: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BBAC: 				Uint64 Value: 0x40 { 45 0A 40 00 00 00 00 00 00 00 }
0x3BBB6: 				BitwiseAnd  { 35 02 }
0x3BBB8: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BBC2: 				NotEqual  { 30 02 }
0x3BBC4: 			End  { 29 02 }
0x3BBC6: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x499, VarStoreId: 0x1, VarOffset: 0x35E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CE 1C EE 1C 99 04 01 00 5E 03 10 00 }
0x3BBD4: 			End  { 29 02 }
0x3BBD6: 		End  { 29 02 }
0x3BBD8: 		SuppressIf  { 0A 82 }
0x3BBDA: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BBE1: 				Uint64 Value: 0x80 { 45 0A 80 00 00 00 00 00 00 00 }
0x3BBEB: 				BitwiseAnd  { 35 02 }
0x3BBED: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BBF7: 				NotEqual  { 30 02 }
0x3BBF9: 			End  { 29 02 }
0x3BBFB: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x49A, VarStoreId: 0x1, VarOffset: 0x35F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CF 1C EF 1C 9A 04 01 00 5F 03 10 00 }
0x3BC09: 			End  { 29 02 }
0x3BC0B: 		End  { 29 02 }
0x3BC0D: 		SuppressIf  { 0A 82 }
0x3BC0F: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BC16: 				Uint64 Value: 0x100 { 45 0A 00 01 00 00 00 00 00 00 }
0x3BC20: 				BitwiseAnd  { 35 02 }
0x3BC22: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BC2C: 				NotEqual  { 30 02 }
0x3BC2E: 			End  { 29 02 }
0x3BC30: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x49B, VarStoreId: 0x1, VarOffset: 0x360, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D0 1C F0 1C 9B 04 01 00 60 03 10 00 }
0x3BC3E: 			End  { 29 02 }
0x3BC40: 		End  { 29 02 }
0x3BC42: 		SuppressIf  { 0A 82 }
0x3BC44: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BC4B: 				Uint64 Value: 0x200 { 45 0A 00 02 00 00 00 00 00 00 }
0x3BC55: 				BitwiseAnd  { 35 02 }
0x3BC57: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BC61: 				NotEqual  { 30 02 }
0x3BC63: 			End  { 29 02 }
0x3BC65: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x49C, VarStoreId: 0x1, VarOffset: 0x361, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D1 1C F1 1C 9C 04 01 00 61 03 10 00 }
0x3BC73: 			End  { 29 02 }
0x3BC75: 		End  { 29 02 }
0x3BC77: 		SuppressIf  { 0A 82 }
0x3BC79: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BC80: 				Uint64 Value: 0x400 { 45 0A 00 04 00 00 00 00 00 00 }
0x3BC8A: 				BitwiseAnd  { 35 02 }
0x3BC8C: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BC96: 				NotEqual  { 30 02 }
0x3BC98: 			End  { 29 02 }
0x3BC9A: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x49D, VarStoreId: 0x1, VarOffset: 0x362, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D2 1C F2 1C 9D 04 01 00 62 03 10 00 }
0x3BCA8: 			End  { 29 02 }
0x3BCAA: 		End  { 29 02 }
0x3BCAC: 		SuppressIf  { 0A 82 }
0x3BCAE: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BCB5: 				Uint64 Value: 0x800 { 45 0A 00 08 00 00 00 00 00 00 }
0x3BCBF: 				BitwiseAnd  { 35 02 }
0x3BCC1: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BCCB: 				NotEqual  { 30 02 }
0x3BCCD: 			End  { 29 02 }
0x3BCCF: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x49E, VarStoreId: 0x1, VarOffset: 0x363, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D3 1C F3 1C 9E 04 01 00 63 03 10 00 }
0x3BCDD: 			End  { 29 02 }
0x3BCDF: 		End  { 29 02 }
0x3BCE1: 		SuppressIf  { 0A 82 }
0x3BCE3: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BCEA: 				Uint64 Value: 0x1000 { 45 0A 00 10 00 00 00 00 00 00 }
0x3BCF4: 				BitwiseAnd  { 35 02 }
0x3BCF6: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BD00: 				NotEqual  { 30 02 }
0x3BD02: 			End  { 29 02 }
0x3BD04: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x49F, VarStoreId: 0x1, VarOffset: 0x364, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D4 1C F4 1C 9F 04 01 00 64 03 10 00 }
0x3BD12: 			End  { 29 02 }
0x3BD14: 		End  { 29 02 }
0x3BD16: 		SuppressIf  { 0A 82 }
0x3BD18: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BD1F: 				Uint64 Value: 0x2000 { 45 0A 00 20 00 00 00 00 00 00 }
0x3BD29: 				BitwiseAnd  { 35 02 }
0x3BD2B: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BD35: 				NotEqual  { 30 02 }
0x3BD37: 			End  { 29 02 }
0x3BD39: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A0, VarStoreId: 0x1, VarOffset: 0x365, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D5 1C F5 1C A0 04 01 00 65 03 10 00 }
0x3BD47: 			End  { 29 02 }
0x3BD49: 		End  { 29 02 }
0x3BD4B: 		SuppressIf  { 0A 82 }
0x3BD4D: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BD54: 				Uint64 Value: 0x4000 { 45 0A 00 40 00 00 00 00 00 00 }
0x3BD5E: 				BitwiseAnd  { 35 02 }
0x3BD60: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BD6A: 				NotEqual  { 30 02 }
0x3BD6C: 			End  { 29 02 }
0x3BD6E: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A1, VarStoreId: 0x1, VarOffset: 0x366, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D6 1C F6 1C A1 04 01 00 66 03 10 00 }
0x3BD7C: 			End  { 29 02 }
0x3BD7E: 		End  { 29 02 }
0x3BD80: 		SuppressIf  { 0A 82 }
0x3BD82: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BD89: 				Uint64 Value: 0x8000 { 45 0A 00 80 00 00 00 00 00 00 }
0x3BD93: 				BitwiseAnd  { 35 02 }
0x3BD95: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BD9F: 				NotEqual  { 30 02 }
0x3BDA1: 			End  { 29 02 }
0x3BDA3: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A2, VarStoreId: 0x1, VarOffset: 0x367, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D7 1C F7 1C A2 04 01 00 67 03 10 00 }
0x3BDB1: 			End  { 29 02 }
0x3BDB3: 		End  { 29 02 }
0x3BDB5: 		SuppressIf  { 0A 82 }
0x3BDB7: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BDBE: 				Uint64 Value: 0x10000 { 45 0A 00 00 01 00 00 00 00 00 }
0x3BDC8: 				BitwiseAnd  { 35 02 }
0x3BDCA: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BDD4: 				NotEqual  { 30 02 }
0x3BDD6: 			End  { 29 02 }
0x3BDD8: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A3, VarStoreId: 0x1, VarOffset: 0x368, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D8 1C F8 1C A3 04 01 00 68 03 10 00 }
0x3BDE6: 			End  { 29 02 }
0x3BDE8: 		End  { 29 02 }
0x3BDEA: 		SuppressIf  { 0A 82 }
0x3BDEC: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BDF3: 				Uint64 Value: 0x20000 { 45 0A 00 00 02 00 00 00 00 00 }
0x3BDFD: 				BitwiseAnd  { 35 02 }
0x3BDFF: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BE09: 				NotEqual  { 30 02 }
0x3BE0B: 			End  { 29 02 }
0x3BE0D: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A4, VarStoreId: 0x1, VarOffset: 0x369, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D9 1C F9 1C A4 04 01 00 69 03 10 00 }
0x3BE1B: 			End  { 29 02 }
0x3BE1D: 		End  { 29 02 }
0x3BE1F: 		SuppressIf  { 0A 82 }
0x3BE21: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BE28: 				Uint64 Value: 0x40000 { 45 0A 00 00 04 00 00 00 00 00 }
0x3BE32: 				BitwiseAnd  { 35 02 }
0x3BE34: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BE3E: 				NotEqual  { 30 02 }
0x3BE40: 			End  { 29 02 }
0x3BE42: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A5, VarStoreId: 0x1, VarOffset: 0x36A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DA 1C FA 1C A5 04 01 00 6A 03 10 00 }
0x3BE50: 			End  { 29 02 }
0x3BE52: 		End  { 29 02 }
0x3BE54: 		SuppressIf  { 0A 82 }
0x3BE56: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BE5D: 				Uint64 Value: 0x80000 { 45 0A 00 00 08 00 00 00 00 00 }
0x3BE67: 				BitwiseAnd  { 35 02 }
0x3BE69: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BE73: 				NotEqual  { 30 02 }
0x3BE75: 			End  { 29 02 }
0x3BE77: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A6, VarStoreId: 0x1, VarOffset: 0x36B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DB 1C FB 1C A6 04 01 00 6B 03 10 00 }
0x3BE85: 			End  { 29 02 }
0x3BE87: 		End  { 29 02 }
0x3BE89: 		SuppressIf  { 0A 82 }
0x3BE8B: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BE92: 				Uint64 Value: 0x100000 { 45 0A 00 00 10 00 00 00 00 00 }
0x3BE9C: 				BitwiseAnd  { 35 02 }
0x3BE9E: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BEA8: 				NotEqual  { 30 02 }
0x3BEAA: 			End  { 29 02 }
0x3BEAC: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A7, VarStoreId: 0x1, VarOffset: 0x36C, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DC 1C FC 1C A7 04 01 00 6C 03 10 00 }
0x3BEBA: 			End  { 29 02 }
0x3BEBC: 		End  { 29 02 }
0x3BEBE: 		SuppressIf  { 0A 82 }
0x3BEC0: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BEC7: 				Uint64 Value: 0x200000 { 45 0A 00 00 20 00 00 00 00 00 }
0x3BED1: 				BitwiseAnd  { 35 02 }
0x3BED3: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BEDD: 				NotEqual  { 30 02 }
0x3BEDF: 			End  { 29 02 }
0x3BEE1: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A8, VarStoreId: 0x1, VarOffset: 0x36D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DD 1C FD 1C A8 04 01 00 6D 03 10 00 }
0x3BEEF: 			End  { 29 02 }
0x3BEF1: 		End  { 29 02 }
0x3BEF3: 		SuppressIf  { 0A 82 }
0x3BEF5: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BEFC: 				Uint64 Value: 0x400000 { 45 0A 00 00 40 00 00 00 00 00 }
0x3BF06: 				BitwiseAnd  { 35 02 }
0x3BF08: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BF12: 				NotEqual  { 30 02 }
0x3BF14: 			End  { 29 02 }
0x3BF16: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4A9, VarStoreId: 0x1, VarOffset: 0x36E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DE 1C FE 1C A9 04 01 00 6E 03 10 00 }
0x3BF24: 			End  { 29 02 }
0x3BF26: 		End  { 29 02 }
0x3BF28: 		SuppressIf  { 0A 82 }
0x3BF2A: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BF31: 				Uint64 Value: 0x800000 { 45 0A 00 00 80 00 00 00 00 00 }
0x3BF3B: 				BitwiseAnd  { 35 02 }
0x3BF3D: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BF47: 				NotEqual  { 30 02 }
0x3BF49: 			End  { 29 02 }
0x3BF4B: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4AA, VarStoreId: 0x1, VarOffset: 0x36F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DF 1C FF 1C AA 04 01 00 6F 03 10 00 }
0x3BF59: 			End  { 29 02 }
0x3BF5B: 		End  { 29 02 }
0x3BF5D: 		SuppressIf  { 0A 82 }
0x3BF5F: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BF66: 				Uint64 Value: 0x1000000 { 45 0A 00 00 00 01 00 00 00 00 }
0x3BF70: 				BitwiseAnd  { 35 02 }
0x3BF72: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BF7C: 				NotEqual  { 30 02 }
0x3BF7E: 			End  { 29 02 }
0x3BF80: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4AB, VarStoreId: 0x1, VarOffset: 0x370, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E0 1C 00 1D AB 04 01 00 70 03 10 00 }
0x3BF8E: 			End  { 29 02 }
0x3BF90: 		End  { 29 02 }
0x3BF92: 		SuppressIf  { 0A 82 }
0x3BF94: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BF9B: 				Uint64 Value: 0x2000000 { 45 0A 00 00 00 02 00 00 00 00 }
0x3BFA5: 				BitwiseAnd  { 35 02 }
0x3BFA7: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BFB1: 				NotEqual  { 30 02 }
0x3BFB3: 			End  { 29 02 }
0x3BFB5: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4AC, VarStoreId: 0x1, VarOffset: 0x371, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E1 1C 01 1D AC 04 01 00 71 03 10 00 }
0x3BFC3: 			End  { 29 02 }
0x3BFC5: 		End  { 29 02 }
0x3BFC7: 		SuppressIf  { 0A 82 }
0x3BFC9: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3BFD0: 				Uint64 Value: 0x4000000 { 45 0A 00 00 00 04 00 00 00 00 }
0x3BFDA: 				BitwiseAnd  { 35 02 }
0x3BFDC: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3BFE6: 				NotEqual  { 30 02 }
0x3BFE8: 			End  { 29 02 }
0x3BFEA: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4AD, VarStoreId: 0x1, VarOffset: 0x372, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E2 1C 02 1D AD 04 01 00 72 03 10 00 }
0x3BFF8: 			End  { 29 02 }
0x3BFFA: 		End  { 29 02 }
0x3BFFC: 		SuppressIf  { 0A 82 }
0x3BFFE: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3C005: 				Uint64 Value: 0x8000000 { 45 0A 00 00 00 08 00 00 00 00 }
0x3C00F: 				BitwiseAnd  { 35 02 }
0x3C011: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3C01B: 				NotEqual  { 30 02 }
0x3C01D: 			End  { 29 02 }
0x3C01F: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4AE, VarStoreId: 0x1, VarOffset: 0x373, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E3 1C 03 1D AE 04 01 00 73 03 10 00 }
0x3C02D: 			End  { 29 02 }
0x3C02F: 		End  { 29 02 }
0x3C031: 		SuppressIf  { 0A 82 }
0x3C033: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3C03A: 				Uint64 Value: 0x10000000 { 45 0A 00 00 00 10 00 00 00 00 }
0x3C044: 				BitwiseAnd  { 35 02 }
0x3C046: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3C050: 				NotEqual  { 30 02 }
0x3C052: 			End  { 29 02 }
0x3C054: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4AF, VarStoreId: 0x1, VarOffset: 0x374, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E4 1C 04 1D AF 04 01 00 74 03 10 00 }
0x3C062: 			End  { 29 02 }
0x3C064: 		End  { 29 02 }
0x3C066: 		SuppressIf  { 0A 82 }
0x3C068: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3C06F: 				Uint64 Value: 0x20000000 { 45 0A 00 00 00 20 00 00 00 00 }
0x3C079: 				BitwiseAnd  { 35 02 }
0x3C07B: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3C085: 				NotEqual  { 30 02 }
0x3C087: 			End  { 29 02 }
0x3C089: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4B0, VarStoreId: 0x1, VarOffset: 0x375, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E5 1C 05 1D B0 04 01 00 75 03 10 00 }
0x3C097: 			End  { 29 02 }
0x3C099: 		End  { 29 02 }
0x3C09B: 		SuppressIf  { 0A 82 }
0x3C09D: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3C0A4: 				Uint64 Value: 0x40000000 { 45 0A 00 00 00 40 00 00 00 00 }
0x3C0AE: 				BitwiseAnd  { 35 02 }
0x3C0B0: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3C0BA: 				NotEqual  { 30 02 }
0x3C0BC: 			End  { 29 02 }
0x3C0BE: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4B1, VarStoreId: 0x1, VarOffset: 0x376, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E6 1C 06 1D B1 04 01 00 76 03 10 00 }
0x3C0CC: 			End  { 29 02 }
0x3C0CE: 		End  { 29 02 }
0x3C0D0: 		SuppressIf  { 0A 82 }
0x3C0D2: 			Get VarStoreId: 0x1, VarStoreInfo: 0x354, VarStoreType: 0x2 { 2B 87 01 00 54 03 02 }
0x3C0D9: 				Uint64 Value: 0x80000000 { 45 0A 00 00 00 80 00 00 00 00 }
0x3C0E3: 				BitwiseAnd  { 35 02 }
0x3C0E5: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3C0EF: 				NotEqual  { 30 02 }
0x3C0F1: 			End  { 29 02 }
0x3C0F3: 			CheckBox Prompt: "N/A", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0x4B2, VarStoreId: 0x1, VarOffset: 0x377, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E7 1C 07 1D B2 04 01 00 77 03 10 00 }
0x3C101: 			End  { 29 02 }
0x3C103: 		End  { 29 02 }
0x3C105: 	End  { 29 02 }
0x3C107: 	Form FormId: 0x2895, Title: "AMT Configuration" { 01 86 95 28 7D 1E }
0x3C10D: 		SuppressIf  { 0A 82 }
0x3C10F: 			True  { 46 02 }
0x3C111: 			Action Prompt: "None", Help: "None", QuestionFlags: 0x4, QuestionId: 0x2896, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: "" { 0C 8F 05 00 05 00 96 28 00 00 FF FF 04 00 00 }
0x3C120: 			End  { 29 02 }
0x3C122: 		End  { 29 02 }
0x3C124: 		OneOf Prompt: "USB Provisioning of AMT", Help: "Enable/Disable of AMT USB Provisioning.", QuestionFlags: 0x10, QuestionId: 0x4B3, VarStoreId: 0x8, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7F 1E 80 1E B3 04 08 00 1C 00 10 10 00 01 00 }
0x3C135: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3C13C: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C143: 		End  { 29 02 }
0x3C145: 		OneOf Prompt: "MAC Pass Through", Help: "Enable/Disable MAC Pass Through function.", QuestionFlags: 0x10, QuestionId: 0x4B4, VarStoreId: 0x8, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 1E 9A 1E B4 04 08 00 2E 00 10 10 00 01 00 }
0x3C156: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3C15D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C164: 		End  { 29 02 }
0x3C166: 		SuppressIf  { 0A 82 }
0x3C168: 			EqIdVal QuestionId: 0x11E2, Value: 0x0 { 12 06 E2 11 00 00 }
0x3C16E: 			GrayOutIf  { 19 82 }
0x3C170: 				EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x3C176: 				OneOf Prompt: "Dynamic Lan Switch", Help: "Allow switching AMT support from Integrated LAN to Discrete LAN.", QuestionFlags: 0x10, QuestionId: 0x4B5, VarStoreId: 0x9, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AD 1E AE 1E B5 04 09 00 10 00 10 10 00 02 00 }
0x3C187: 					OneOfOption Option: "As defined in FIT" Value: 0, Default, MfgDefault { 09 07 AF 1E 30 00 00 }
0x3C18E: 					OneOfOption Option: "Integrated LAN" Value: 1 { 09 07 B0 1E 00 00 01 }
0x3C195: 					OneOfOption Option: "Discrete LAN" Value: 2 { 09 07 B1 1E 00 00 02 }
0x3C19C: 				End  { 29 02 }
0x3C19E: 			End  { 29 02 }
0x3C1A0: 		End  { 29 02 }
0x3C1A2: 		CheckBox Prompt: "Activate Remote Assistance Process", Help: "Trigger CIRA boot

Note:
Network Access must be activated first from MEBx Setup.", QuestionFlags: 0x10, QuestionId: 0x4B6, VarStoreId: 0x8, VarOffset: 0x1A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 83 1E 84 1E B6 04 08 00 1A 00 10 00 }
0x3C1B0: 		End  { 29 02 }
0x3C1B2: 		CheckBox Prompt: "Unconfigure ME", Help: "Unconfigure ME with resetting MEBx password to default on next boot.", QuestionFlags: 0x10, QuestionId: 0x4B7, VarStoreId: 0x8, VarOffset: 0x19, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 81 1E 82 1E B7 04 08 00 19 00 10 00 }
0x3C1C0: 		End  { 29 02 }
0x3C1C2: 		Ref Prompt: "ASF Configuration", Help: "Configure Alert Standard Format parameters.", QuestionFlags: 0x0, QuestionId: 0x4B8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2897 { 0F 0F 85 1E 86 1E B8 04 00 00 FF FF 00 97 28 }
0x3C1D1: 		Ref Prompt: "Secure Erase Configuration", Help: "Secure Erase configuration menu", QuestionFlags: 0x0, QuestionId: 0x4B9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2898 { 0F 0F 91 1E 92 1E B9 04 00 00 FF FF 00 98 28 }
0x3C1E0: 		Ref Prompt: "One Click Recovery(OCR) Configuration", Help: "Configuration setting for One Click Recovery.  This allows access for AMT to boot a recovery OS application.", QuestionFlags: 0x0, QuestionId: 0x4BA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2899 { 0F 0F 9B 1E 9C 1E BA 04 00 00 FF FF 00 99 28 }
0x3C1EF: 		SuppressIf  { 0A 82 }
0x3C1F1: 			EqIdVal QuestionId: 0x11E1, Value: 0x0 { 12 06 E1 11 00 00 }
0x3C1F7: 			Ref Prompt: "Remote Platform Erase Configuration", Help: "Remote Platform Erase configuration menu", QuestionFlags: 0x0, QuestionId: 0x4BB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x289A { 0F 0F A5 1E A6 1E BB 04 00 00 FF FF 00 9A 28 }
0x3C206: 		End  { 29 02 }
0x3C208: 	End  { 29 02 }
0x3C20A: 	Form FormId: 0x2897, Title: "ASF Configuration" { 01 86 97 28 85 1E }
0x3C210: 		OneOf Prompt: "PET Progress", Help: "Enable/Disable PET Events Progress to receive PET Events.", QuestionFlags: 0x10, QuestionId: 0x4BC, VarStoreId: 0x8, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 1E 88 1E BC 04 08 00 1D 00 10 10 00 01 00 }
0x3C221: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C228: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C22F: 		End  { 29 02 }
0x3C231: 		OneOf Prompt: "WatchDog", Help: "Enable/Disable WatchDog Timer.", QuestionFlags: 0x10, QuestionId: 0x4BD, VarStoreId: 0x8, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 1E 8A 1E BD 04 08 00 1F 00 10 10 00 01 00 }
0x3C242: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3C249: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C250: 		End  { 29 02 }
0x3C252: 		GrayOutIf  { 19 82 }
0x3C254: 			EqIdVal QuestionId: 0x4BD, Value: 0x0 { 12 06 BD 04 00 00 }
0x3C25A: 			Numeric Prompt: "OS Timer", Help: "Set OS watchdog timer.", QuestionFlags: 0x0, QuestionId: 0x4BE, VarStoreId: 0x8, VarOffset: 0x20, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 8B 1E 8C 1E BE 04 08 00 20 00 00 11 00 00 FF FF 01 00 }
0x3C26E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3C275: 			End  { 29 02 }
0x3C277: 			Numeric Prompt: "BIOS Timer", Help: "Set BIOS watchdog timer.", QuestionFlags: 0x0, QuestionId: 0x4BF, VarStoreId: 0x8, VarOffset: 0x22, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 8D 1E 8E 1E BF 04 08 00 22 00 00 11 00 00 FF FF 01 00 }
0x3C28B: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3C292: 			End  { 29 02 }
0x3C294: 		End  { 29 02 }
0x3C296: 		OneOf Prompt: "ASF Sensors Table", Help: "Adds ASF Sensor Table into ASF! ACPI Table", QuestionFlags: 0x10, QuestionId: 0x4C0, VarStoreId: 0x8, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 1E 90 1E C0 04 08 00 1E 00 10 10 00 01 00 }
0x3C2A7: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3C2AE: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C2B5: 		End  { 29 02 }
0x3C2B7: 	End  { 29 02 }
0x3C2B9: 	Form FormId: 0x2898, Title: "Secure Erase Configuration" { 01 86 98 28 91 1E }
0x3C2BF: 		OneOf Prompt: "Secure Erase mode", Help: "Change Secure Erase module behavior:
Simulated: Performs SE flow without erasing SSD
Real: Erase SSD.
*** If SATA device is used, OEM could use SECURE_ERASE_HOOK_PROTOCOL to remove SATA power to skip G3 cycle. ***", QuestionFlags: 0x0, QuestionId: 0x4C1, VarStoreId: 0xF101, VarOffset: 0x813, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 1E 94 1E C1 04 01 F1 13 08 00 10 00 01 00 }
0x3C2D0: 			OneOfOption Option: "Simulated" Value: 0, Default { 09 07 95 1E 10 00 00 }
0x3C2D7: 			OneOfOption Option: "Real" Value: 1 { 09 07 96 1E 00 00 01 }
0x3C2DE: 		End  { 29 02 }
0x3C2E0: 		OneOf Prompt: "Force Secure Erase", Help: "Force Secure Erase on next boot", QuestionFlags: 0x10, QuestionId: 0x4C2, VarStoreId: 0xF101, VarOffset: 0x814, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 1E 98 1E C2 04 01 F1 14 08 10 10 00 01 00 }
0x3C2F1: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x3C2F8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C2FF: 		End  { 29 02 }
0x3C301: 	End  { 29 02 }
0x3C303: 	Form FormId: 0x2899, Title: "One Click Recovery(OCR) Configuration" { 01 86 99 28 9B 1E }
0x3C309: 		SuppressIf  { 0A 82 }
0x3C30B: 			EqIdVal QuestionId: 0x11E0, Value: 0x0 { 12 06 E0 11 00 00 }
0x3C311: 			OneOf Prompt: "OCR Https Boot", Help: "Enable/Disable One Click Recovery Https Boot", QuestionFlags: 0x10, QuestionId: 0x4C3, VarStoreId: 0x8, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 1E 9E 1E C3 04 08 00 2F 00 10 10 00 01 00 }
0x3C322: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C329: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C330: 			End  { 29 02 }
0x3C332: 		End  { 29 02 }
0x3C334: 		SuppressIf  { 0A 82 }
0x3C336: 			EqIdVal QuestionId: 0x11DF, Value: 0x0 { 12 06 DF 11 00 00 }
0x3C33C: 			OneOf Prompt: "OCR PBA Boot", Help: "Enable/Disable One Click Recovery PBA Boot", QuestionFlags: 0x10, QuestionId: 0x4C4, VarStoreId: 0x8, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 1E A0 1E C4 04 08 00 30 00 10 10 00 01 00 }
0x3C34D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C354: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C35B: 			End  { 29 02 }
0x3C35D: 		End  { 29 02 }
0x3C35F: 		SuppressIf  { 0A 82 }
0x3C361: 			EqIdVal QuestionId: 0x11DE, Value: 0x0 { 12 06 DE 11 00 00 }
0x3C367: 			OneOf Prompt: "OCR Windows Recovery Boot", Help: "Enable/Disable One Click Recovery Windows Recovery Boot", QuestionFlags: 0x10, QuestionId: 0x4C5, VarStoreId: 0x8, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 1E A2 1E C5 04 08 00 31 00 10 10 00 01 00 }
0x3C378: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C37F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C386: 			End  { 29 02 }
0x3C388: 		End  { 29 02 }
0x3C38A: 		SuppressIf  { 0A 82 }
0x3C38C: 			EqIdVal QuestionId: 0x11DD, Value: 0x0 { 12 06 DD 11 00 00 }
0x3C392: 			OneOf Prompt: "OCR Disable Secure Boot", Help: "Allows CSME to request SecureBoot to be disabled for One Click Recovery", QuestionFlags: 0x10, QuestionId: 0x4C6, VarStoreId: 0x8, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A3 1E A4 1E C6 04 08 00 32 00 10 10 00 01 00 }
0x3C3A3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C3AA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C3B1: 			End  { 29 02 }
0x3C3B3: 		End  { 29 02 }
0x3C3B5: 	End  { 29 02 }
0x3C3B7: 	Form FormId: 0x289A, Title: "Remote Platform Erase Configuration" { 01 86 9A 28 A5 1E }
0x3C3BD: 		OneOf Prompt: "Enable Remote Platform Erase Feature", Help: "Enable/Disable Remote Platform Erase Feature", QuestionFlags: 0x10, QuestionId: 0x4C7, VarStoreId: 0x8, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AB 1E AC 1E C7 04 08 00 33 00 10 10 00 01 00 }
0x3C3CE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C3D5: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C3DC: 		End  { 29 02 }
0x3C3DE: 		GrayOutIf  { 19 82 }
0x3C3E0: 			EqIdVal QuestionId: 0x4C7, Value: 0x0 { 12 06 C7 04 00 00 }
0x3C3E6: 			OneOf Prompt: "SSD Erase Mode", Help: "Change RPE SSD Erase Action behavior:
Simulated: Performs RPE SSD Erase flow without erasing SSD
Real: Erase SSD.
*** If SATA device is used, OEM could use SECURE_ERASE_HOOK_PROTOCOL to remove SATA power to skip G3 cycle. ***", QuestionFlags: 0x10, QuestionId: 0x4C8, VarStoreId: 0x8, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A7 1E A8 1E C8 04 08 00 34 00 10 10 00 01 00 }
0x3C3F7: 				OneOfOption Option: "Simulated" Value: 0, Default, MfgDefault { 09 07 A9 1E 30 00 00 }
0x3C3FE: 				OneOfOption Option: "Real" Value: 1 { 09 07 AA 1E 00 00 01 }
0x3C405: 			End  { 29 02 }
0x3C407: 		End  { 29 02 }
0x3C409: 	End  { 29 02 }
0x3C40B: 	Form FormId: 0x289C, Title: "BCLK Configuration" { 01 86 9C 28 B2 1E }
0x3C411: 		Text Prompt: "BCLK Source Config", Help: "CPU BCLK is only BCLK Source for ADL.", Text: "CPU BCLK" { 03 08 B3 1E B4 1E B5 1E }
0x3C419: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3C420: 		End  { 29 02 }
0x3C422: 		Subtitle Prompt: "CPU - BCLK Clock Settings", Help: "", Flags: 0x0 { 02 87 B6 1E 00 00 00 }
0x3C429: 		End  { 29 02 }
0x3C42B: 		Text Prompt: "BCLK Frequency", Help: "", Text: "100.00 MHz" { 03 08 2D 1E C9 07 2E 1E }
0x3C433: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3C43A: 		End  { 29 02 }
0x3C43C: 		SuppressIf  { 0A 82 }
0x3C43E: 			EqIdVal QuestionId: 0x11DC, Value: 0x0 { 12 06 DC 11 00 00 }
0x3C444: 			Text Prompt: "Current CPU Bclk Frequency", Help: "", Text: "100 MHz" { 03 08 B7 1E C9 07 B8 1E }
0x3C44C: 			Numeric Prompt: "Discrete CPU Bclk Frequency", Help: "Config Discrete Clock Frequency in MHz. Range from 80 MHz up to MAX 530 MHz.", QuestionFlags: 0x10, QuestionId: 0x4C9, VarStoreId: 0xF101, VarOffset: 0xAF0, Flags: 0x11, Size: 16, Min: 0x50, Max: 0x212, Step: 0x1 { 07 94 B9 1E BA 1E C9 04 01 F1 F0 0A 10 11 50 00 12 02 01 00 }
0x3C460: 				Default DefaultId: 0x0 Value: 100 { 5B 07 00 00 01 64 00 }
0x3C467: 			End  { 29 02 }
0x3C469: 			Text Prompt: "Current Peg/Dmi Clk Frequency", Help: "", Text: "100 MHz" { 03 08 BB 1E C9 07 BC 1E }
0x3C471: 			Numeric Prompt: "Discrete Peg/Dmi Clk Frequency", Help: "Config Peg/Dmi Clock Frequency in MHz. Range from 80 MHz up to MAX 200 MHz.", QuestionFlags: 0x10, QuestionId: 0x4CA, VarStoreId: 0xF101, VarOffset: 0xAF2, Flags: 0x10, Size: 8, Min: 0x50, Max: 0xC8, Step: 0x1 { 07 91 BD 1E BE 1E CA 04 01 F1 F2 0A 10 10 50 C8 01 }
0x3C482: 				Default DefaultId: 0x0 Value: 100 { 5B 06 00 00 00 64 }
0x3C488: 			End  { 29 02 }
0x3C48A: 		End  { 29 02 }
0x3C48C: 	End  { 29 02 }
0x3C48E: 	Form FormId: 0x28AB, Title: "Thunderbolt(TM) Configuration" { 01 86 AB 28 BF 1E }
0x3C494: 		OneOf Prompt: "PCIE Tunneling over USB4", Help: "Enable or disable PCIE Tunneling over USB4", QuestionFlags: 0x14, QuestionId: 0x4CB, VarStoreId: 0xF101, VarOffset: 0x9A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C7 1E C8 1E CB 04 01 F1 A8 09 14 10 00 01 00 }
0x3C4A5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C4AC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C4B3: 		End  { 29 02 }
0x3C4B5: 		SuppressIf  { 0A 82 }
0x3C4B7: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3C4BD: 				EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x3C4C3: 				Or  { 16 02 }
0x3C4C5: 			End  { 29 02 }
0x3C4C7: 			OneOf Prompt: "USB4 CM Mode", Help: "FW CM only - The system boots with FW CM only in both BIOS and OS phase.
SW CM first - The system boots with SW CM in BIOS phase all the time, then boot to OS based on OS preference for backward and forward compatible.
OS dependent - The system will boot with SW CM in BIOS phase after saving this setting, then boot to OS based on OS preference the reflect to CM setting to next BIOS boot.
CM debug - The system with boot without any CM in BIOS phase, then boot to OS with the CM based on OS' preference by every boot.", QuestionFlags: 0x14, QuestionId: 0x289D, VarStoreId: 0xF101, VarOffset: 0xADD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 C9 1E CA 1E 9D 28 01 F1 DD 0A 14 10 00 03 00 }
0x3C4D8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3C4DE: 				OneOfOption Option: "Firmware CM Only" Value: 0 { 09 07 CB 1E 00 00 00 }
0x3C4E5: 				OneOfOption Option: "Software CM first" Value: 1 { 09 07 CC 1E 00 00 01 }
0x3C4EC: 				OneOfOption Option: "OS Dependent" Value: 2 { 09 07 CD 1E 00 00 02 }
0x3C4F3: 				OneOfOption Option: "CM Debug" Value: 3 { 09 07 CE 1E 00 00 03 }
0x3C4FA: 			End  { 29 02 }
0x3C4FC: 			OneOf Prompt: "USB4 CM ver2 Support", Help: "Enable or Disable USB4 CM version 2 Support", QuestionFlags: 0x14, QuestionId: 0x4CC, VarStoreId: 0xF101, VarOffset: 0xBCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 1E D0 1E CC 04 01 F1 CA 0B 14 10 00 01 00 }
0x3C50D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3C513: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C51A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C521: 			End  { 29 02 }
0x3C523: 			SuppressIf  { 0A 82 }
0x3C525: 				EqIdVal QuestionId: 0x4CC, Value: 0x0 { 12 06 CC 04 00 00 }
0x3C52B: 				OneOf Prompt: "USB4 Host Router Class Code", Help: "Option for class code to be applied to Host Router for loading different driver. Auto: Determined by OSPM USB support, Intel USB4 Ver2: Intel USB4 Ver2 driver, USB4 Standard: OS inbox driver", QuestionFlags: 0x14, QuestionId: 0x4CD, VarStoreId: 0xF101, VarOffset: 0xBCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D1 1E D2 1E CD 04 01 F1 CB 0B 14 10 00 02 00 }
0x3C53C: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3C542: 					OneOfOption Option: "Auto" Value: 0 { 09 07 D3 1E 00 00 00 }
0x3C549: 					OneOfOption Option: "Intel USB4 Ver2" Value: 1 { 09 07 D4 1E 00 00 01 }
0x3C550: 					OneOfOption Option: "USB4 Standard" Value: 2 { 09 07 D5 1E 00 00 02 }
0x3C557: 				End  { 29 02 }
0x3C559: 			End  { 29 02 }
0x3C55B: 		End  { 29 02 }
0x3C55D: 		SuppressIf  { 0A 82 }
0x3C55F: 			EqIdVal QuestionId: 0x11DA, Value: 0x1 { 12 86 DA 11 01 00 }
0x3C565: 				Not  { 17 02 }
0x3C567: 			End  { 29 02 }
0x3C569: 			OneOf Prompt: "Discrete Thunderbolt(TM) Support", Help: "Enable or Disable Discrete Thunderbolt(TM) Support.", QuestionFlags: 0x14, QuestionId: 0x289F, VarStoreId: 0xF101, VarOffset: 0x79A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 1E C6 1E 9F 28 01 F1 9A 07 14 10 00 01 00 }
0x3C57A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3C580: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C587: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C58E: 			End  { 29 02 }
0x3C590: 		End  { 29 02 }
0x3C592: 		SuppressIf  { 0A 82 }
0x3C594: 			EqIdVal QuestionId: 0x289F, Value: 0x0 { 12 86 9F 28 00 00 }
0x3C59A: 				EqIdVal QuestionId: 0x11DB, Value: 0x0 { 12 06 DB 11 00 00 }
0x3C5A0: 				And  { 15 02 }
0x3C5A2: 			End  { 29 02 }
0x3C5A4: 			CheckBox Prompt: "Wake From Thunderbolt(TM) Devices", Help: "Enable or disable system wake from Thunderbolt(TM) devices.", QuestionFlags: 0x10, QuestionId: 0x4CE, VarStoreId: 0xF101, VarOffset: 0x79F, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E E2 1E E3 1E CE 04 01 F1 9F 07 10 01 }
0x3C5B2: 			End  { 29 02 }
0x3C5B4: 		End  { 29 02 }
0x3C5B6: 		SuppressIf  { 0A 82 }
0x3C5B8: 			EqIdVal QuestionId: 0x11DB, Value: 0x0 { 12 06 DB 11 00 00 }
0x3C5BE: 			Ref Prompt: "Integrated Thunderbolt(TM) Configuration", Help: "Integrated Thunderbolt(TM) Related Configuration", QuestionFlags: 0x0, QuestionId: 0x4CF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28AC { 0F 0F 0F 1F 10 1F CF 04 00 00 FF FF 00 AC 28 }
0x3C5CD: 		End  { 29 02 }
0x3C5CF: 		SuppressIf  { 0A 82 }
0x3C5D1: 			EqIdVal QuestionId: 0x11DA, Value: 0x1 { 12 86 DA 11 01 00 }
0x3C5D7: 				Not  { 17 02 }
0x3C5D9: 			End  { 29 02 }
0x3C5DB: 			SuppressIf  { 0A 82 }
0x3C5DD: 				EqIdVal QuestionId: 0x289F, Value: 0x0 { 12 06 9F 28 00 00 }
0x3C5E3: 				SuppressIf  { 0A 82 }
0x3C5E5: 					EqIdVal QuestionId: 0x11D9, Value: 0x1 { 12 86 D9 11 01 00 }
0x3C5EB: 						Not  { 17 02 }
0x3C5ED: 					End  { 29 02 }
0x3C5EF: 					OneOf Prompt: "Discrete DpIn Connection Policy", Help: "Configure the Dp Mux Connection setting.
 Internal Only: All display ports are for internal only.
 External First: All display ports are for external only.
 Runtime switch: Dynamic one-time switch from iGFx to dGFx after boot to OS", QuestionFlags: 0x10, QuestionId: 0x4D0, VarStoreId: 0xF101, VarOffset: 0xADE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 79 1C 7A 1C D0 04 01 F1 DE 0A 10 10 00 02 00 }
0x3C600: 						OneOfOption Option: "Internal Only" Value: 0 { 09 07 7B 1C 00 00 00 }
0x3C607: 						OneOfOption Option: "External Only" Value: 1, Default, MfgDefault { 09 07 7C 1C 30 00 01 }
0x3C60E: 						OneOfOption Option: "Runtime Switch" Value: 2 { 09 07 7D 1C 00 00 02 }
0x3C615: 					End  { 29 02 }
0x3C617: 				End  { 29 02 }
0x3C619: 				Ref Prompt: "Discrete Thunderbolt(TM) Configuration", Help: "Discrete Thunderbolt(TM) Related Configuration", QuestionFlags: 0x0, QuestionId: 0x4D1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28B1 { 0F 0F C1 1E C2 1E D1 04 00 00 FF FF 00 B1 28 }
0x3C628: 			End  { 29 02 }
0x3C62A: 		End  { 29 02 }
0x3C62C: 	End  { 29 02 }
0x3C62E: 	Form FormId: 0x28AC, Title: "Integrated Thunderbolt(TM) Configuration" { 01 86 AC 28 0F 1F }
0x3C634: 		Subtitle Prompt: "Integrated Thunderbolt(TM) Configuration", Help: "", Flags: 0x0 { 02 87 0F 1F 00 00 00 }
0x3C63B: 		End  { 29 02 }
0x3C63D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3C644: 		End  { 29 02 }
0x3C646: 		OneOf Prompt: "Os Native Resource Balance", Help: "Os Native Resource Balance", QuestionFlags: 0x10, QuestionId: 0x4D2, VarStoreId: 0xF101, VarOffset: 0x7C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 1F 3B 1F D2 04 01 F1 C4 07 10 10 00 01 00 }
0x3C657: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3C65E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C665: 		End  { 29 02 }
0x3C667: 		Numeric Prompt: "Connect Topology Timeout value for ITBT", Help: "Connect Topology Timeout value for Integrated Thunderbolt(TM) Controller", QuestionFlags: 0x14, QuestionId: 0x4D3, VarStoreId: 0xF101, VarOffset: 0x7FF, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1 { 07 94 DE 1E DF 1E D3 04 01 F1 FF 07 14 11 01 00 FF FF 01 00 }
0x3C67B: 			Default DefaultId: 0x0 Value: 5000 { 5B 07 00 00 01 88 13 }
0x3C682: 		End  { 29 02 }
0x3C684: 		Numeric Prompt: "Force Poweron Timeout value for ITBT", Help: "Force Poweron Timeout value for Integrated Thunderbolt(TM)", QuestionFlags: 0x14, QuestionId: 0x4D4, VarStoreId: 0xF101, VarOffset: 0x7FD, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1 { 07 94 D8 1E D9 1E D4 04 01 F1 FD 07 14 11 01 00 FF FF 01 00 }
0x3C698: 			Default DefaultId: 0x0 Value: 500 { 5B 07 00 00 01 F4 01 }
0x3C69F: 		End  { 29 02 }
0x3C6A1: 		OneOf Prompt: "ITBT RTD3", Help: "ITBT RTD3 Enable/Disable. Note: ITBT RTD3 Disabled is not supported when SW CM is applied for OS", QuestionFlags: 0x10, QuestionId: 0x4D5, VarStoreId: 0xF101, VarOffset: 0x865, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DA 1E DB 1E D5 04 01 F1 65 08 10 10 00 01 00 }
0x3C6B2: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C6B9: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3C6C0: 		End  { 29 02 }
0x3C6C2: 		Numeric Prompt: "ITBT RTD3 EXIT DELAY", Help: "ITBT RTD3 EXIT DELAY (milli seconds)", QuestionFlags: 0x14, QuestionId: 0x4D6, VarStoreId: 0xF101, VarOffset: 0x866, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x4E20, Step: 0x1 { 07 94 DC 1E DD 1E D6 04 01 F1 66 08 14 11 00 00 20 4E 01 00 }
0x3C6D6: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3C6DD: 		End  { 29 02 }
0x3C6DF: 		SuppressIf  { 0A 82 }
0x3C6E1: 			QuestionRef1 QuestionId: 0x11D5 { 40 84 D5 11 }
0x3C6E5: 				Uint8 Value: 0x1 { 42 03 01 }
0x3C6E8: 				GreaterEqual  { 32 02 }
0x3C6EA: 				Not  { 17 02 }
0x3C6EC: 			End  { 29 02 }
0x3C6EE: 			SuppressIf  { 0A 82 }
0x3C6F0: 				EqIdVal QuestionId: 0x11D8, Value: 0x0 { 12 06 D8 11 00 00 }
0x3C6F6: 				Ref Prompt: " ITBT Root Port 0 Configuration", Help: " ITBT Root Port 0 Configuration", QuestionFlags: 0x0, QuestionId: 0x4D7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28AD { 0F 0F 11 1F 11 1F D7 04 00 00 FF FF 00 AD 28 }
0x3C705: 			End  { 29 02 }
0x3C707: 		End  { 29 02 }
0x3C709: 		SuppressIf  { 0A 82 }
0x3C70B: 			QuestionRef1 QuestionId: 0x11D5 { 40 84 D5 11 }
0x3C70F: 				Uint8 Value: 0x2 { 42 03 02 }
0x3C712: 				GreaterEqual  { 32 02 }
0x3C714: 				Not  { 17 02 }
0x3C716: 			End  { 29 02 }
0x3C718: 			SuppressIf  { 0A 82 }
0x3C71A: 				EqIdVal QuestionId: 0x11D7, Value: 0x0 { 12 06 D7 11 00 00 }
0x3C720: 				Ref Prompt: " ITBT Root Port 1 Configuration", Help: " ITBT Root Port 1 Configuration", QuestionFlags: 0x0, QuestionId: 0x4D8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28AE { 0F 0F 12 1F 12 1F D8 04 00 00 FF FF 00 AE 28 }
0x3C72F: 			End  { 29 02 }
0x3C731: 		End  { 29 02 }
0x3C733: 		SuppressIf  { 0A 82 }
0x3C735: 			QuestionRef1 QuestionId: 0x11D5 { 40 84 D5 11 }
0x3C739: 				Uint8 Value: 0x3 { 42 03 03 }
0x3C73C: 				GreaterEqual  { 32 02 }
0x3C73E: 				Not  { 17 02 }
0x3C740: 			End  { 29 02 }
0x3C742: 			SuppressIf  { 0A 82 }
0x3C744: 				EqIdVal QuestionId: 0x11D6, Value: 0x0 { 12 06 D6 11 00 00 }
0x3C74A: 				Ref Prompt: " ITBT Root Port 2 Configuration", Help: " ITBT Root Port 2 Configuration", QuestionFlags: 0x0, QuestionId: 0x4D9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28AF { 0F 0F 13 1F 13 1F D9 04 00 00 FF FF 00 AF 28 }
0x3C759: 			End  { 29 02 }
0x3C75B: 		End  { 29 02 }
0x3C75D: 		SuppressIf  { 0A 82 }
0x3C75F: 			QuestionRef1 QuestionId: 0x11D5 { 40 84 D5 11 }
0x3C763: 				Uint8 Value: 0x4 { 42 03 04 }
0x3C766: 				GreaterEqual  { 32 02 }
0x3C768: 				Not  { 17 02 }
0x3C76A: 			End  { 29 02 }
0x3C76C: 			SuppressIf  { 0A 82 }
0x3C76E: 				EqIdVal QuestionId: 0x11D4, Value: 0x0 { 12 06 D4 11 00 00 }
0x3C774: 				Ref Prompt: " ITBT Root Port 3 Configuration", Help: " ITBT Root Port 3 Configuration", QuestionFlags: 0x0, QuestionId: 0x4DA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28B0 { 0F 0F 14 1F 14 1F DA 04 00 00 FF FF 00 B0 28 }
0x3C783: 			End  { 29 02 }
0x3C785: 		End  { 29 02 }
0x3C787: 	End  { 29 02 }
0x3C789: 	Form FormId: 0x28AD, Title: " ITBT Root Port 0 Configuration" { 01 86 AD 28 11 1F }
0x3C78F: 		OneOf Prompt: "ITBT Root Port 0", Help: "AUTO - Default(Platform Specific) ", QuestionFlags: 0x14, QuestionId: 0x28A0, VarStoreId: 0xF101, VarOffset: 0x7CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 15 1F 16 1F A0 28 01 F1 CD 07 14 10 00 01 00 }
0x3C7A0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C7A7: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C7AE: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3C7B4: 		End  { 29 02 }
0x3C7B6: 		Subtitle Prompt: "Root Port 0 Resource Allocation", Help: "", Flags: 0x0 { 02 87 1D 1F 00 00 00 }
0x3C7BD: 		End  { 29 02 }
0x3C7BF: 		Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42.
Extra Bus Reserved is required for each layer = (Extra Bus Reserved on the previous layer - 2 - the number of non-hot-plug ports in the current layer) / the number of hot-plug ports in the current layer
Example:
2 non-hot-plug ports and 3 hot-plug ports per connected device have
Recommend below setting
1 device = 7
2 device = 25
3 device = 79, disable one iTBT root port
4 device = 224, disable three iTBT root port, and not every hotplug port supports connecting to the next layer of devices
etc ...", QuestionFlags: 0x14, QuestionId: 0x4DB, VarStoreId: 0xF101, VarOffset: 0x7D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE0, Step: 0x1 { 07 91 1E 1F 1F 1F DB 04 01 F1 D3 07 14 10 00 E0 01 }
0x3C7D0: 			Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3C7D6: 		End  { 29 02 }
0x3C7D8: 		Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4DC, VarStoreId: 0xF101, VarOffset: 0x7D9, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 20 1F 21 1F DC 04 01 F1 D9 07 14 11 01 00 00 10 01 00 }
0x3C7EC: 			Default DefaultId: 0x0 Value: 194 { 5B 07 00 00 01 C2 00 }
0x3C7F3: 		End  { 29 02 }
0x3C7F5: 		Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4DD, VarStoreId: 0xF101, VarOffset: 0x7E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 22 1F 23 1F DD 04 01 F1 E5 07 14 10 00 1F 01 }
0x3C806: 			Default DefaultId: 0x0 Value: 25 { 5B 06 00 00 00 19 }
0x3C80C: 		End  { 29 02 }
0x3C80E: 		Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4DE, VarStoreId: 0xF101, VarOffset: 0x7EB, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 24 1F 25 1F DE 04 01 F1 EB 07 14 11 01 00 00 10 01 00 }
0x3C822: 			Default DefaultId: 0x0 Value: 448 { 5B 07 00 00 01 C0 01 }
0x3C829: 		End  { 29 02 }
0x3C82B: 		Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4DF, VarStoreId: 0xF101, VarOffset: 0x7F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 26 1F 27 1F DF 04 01 F1 F7 07 14 10 00 1F 01 }
0x3C83C: 			Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3C842: 		End  { 29 02 }
0x3C844: 	End  { 29 02 }
0x3C846: 	Form FormId: 0x28AE, Title: " ITBT Root Port 1 Configuration" { 01 86 AE 28 12 1F }
0x3C84C: 		OneOf Prompt: "ITBT Root Port 1", Help: "None", QuestionFlags: 0x14, QuestionId: 0x28A1, VarStoreId: 0xF101, VarOffset: 0x7CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 17 1F 18 1F A1 28 01 F1 CE 07 14 10 00 01 00 }
0x3C85D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C864: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C86B: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3C871: 		End  { 29 02 }
0x3C873: 		Subtitle Prompt: "Root Port 1 Resource Allocation", Help: "", Flags: 0x0 { 02 87 28 1F 00 00 00 }
0x3C87A: 		End  { 29 02 }
0x3C87C: 		Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42.
Extra Bus Reserved is required for each layer = (Extra Bus Reserved on the previous layer - 2 - the number of non-hot-plug ports in the current layer) / the number of hot-plug ports in the current layer
Example:
2 non-hot-plug ports and 3 hot-plug ports per connected device have
Recommend below setting
1 device = 7
2 device = 25
3 device = 79, disable one iTBT root port
4 device = 224, disable three iTBT root port, and not every hotplug port supports connecting to the next layer of devices
etc ...", QuestionFlags: 0x14, QuestionId: 0x4E0, VarStoreId: 0xF101, VarOffset: 0x7D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE0, Step: 0x1 { 07 91 29 1F 1F 1F E0 04 01 F1 D4 07 14 10 00 E0 01 }
0x3C88D: 			Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3C893: 		End  { 29 02 }
0x3C895: 		Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4E1, VarStoreId: 0xF101, VarOffset: 0x7DB, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 2A 1F 21 1F E1 04 01 F1 DB 07 14 11 01 00 00 10 01 00 }
0x3C8A9: 			Default DefaultId: 0x0 Value: 194 { 5B 07 00 00 01 C2 00 }
0x3C8B0: 		End  { 29 02 }
0x3C8B2: 		Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4E2, VarStoreId: 0xF101, VarOffset: 0x7E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 2B 1F 23 1F E2 04 01 F1 E6 07 14 10 00 1F 01 }
0x3C8C3: 			Default DefaultId: 0x0 Value: 25 { 5B 06 00 00 00 19 }
0x3C8C9: 		End  { 29 02 }
0x3C8CB: 		Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4E3, VarStoreId: 0xF101, VarOffset: 0x7ED, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 2C 1F 25 1F E3 04 01 F1 ED 07 14 11 01 00 00 10 01 00 }
0x3C8DF: 			Default DefaultId: 0x0 Value: 448 { 5B 07 00 00 01 C0 01 }
0x3C8E6: 		End  { 29 02 }
0x3C8E8: 		Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4E4, VarStoreId: 0xF101, VarOffset: 0x7F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 2D 1F 27 1F E4 04 01 F1 F8 07 14 10 00 1F 01 }
0x3C8F9: 			Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3C8FF: 		End  { 29 02 }
0x3C901: 	End  { 29 02 }
0x3C903: 	Form FormId: 0x28AF, Title: " ITBT Root Port 2 Configuration" { 01 86 AF 28 13 1F }
0x3C909: 		OneOf Prompt: "ITBT Root Port 2", Help: "None", QuestionFlags: 0x14, QuestionId: 0x28A2, VarStoreId: 0xF101, VarOffset: 0x7CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 19 1F 1A 1F A2 28 01 F1 CF 07 14 10 00 01 00 }
0x3C91A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C921: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C928: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3C92E: 		End  { 29 02 }
0x3C930: 		Subtitle Prompt: "Root Port 2 Resource Allocation", Help: "", Flags: 0x0 { 02 87 2E 1F 00 00 00 }
0x3C937: 		End  { 29 02 }
0x3C939: 		Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42.
Extra Bus Reserved is required for each layer = (Extra Bus Reserved on the previous layer - 2 - the number of non-hot-plug ports in the current layer) / the number of hot-plug ports in the current layer
Example:
2 non-hot-plug ports and 3 hot-plug ports per connected device have
Recommend below setting
1 device = 7
2 device = 25
3 device = 79, disable one iTBT root port
4 device = 224, disable three iTBT root port, and not every hotplug port supports connecting to the next layer of devices
etc ...", QuestionFlags: 0x14, QuestionId: 0x4E5, VarStoreId: 0xF101, VarOffset: 0x7D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE0, Step: 0x1 { 07 91 2F 1F 1F 1F E5 04 01 F1 D5 07 14 10 00 E0 01 }
0x3C94A: 			Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3C950: 		End  { 29 02 }
0x3C952: 		Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4E6, VarStoreId: 0xF101, VarOffset: 0x7DD, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 30 1F 21 1F E6 04 01 F1 DD 07 14 11 01 00 00 10 01 00 }
0x3C966: 			Default DefaultId: 0x0 Value: 194 { 5B 07 00 00 01 C2 00 }
0x3C96D: 		End  { 29 02 }
0x3C96F: 		Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4E7, VarStoreId: 0xF101, VarOffset: 0x7E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 31 1F 23 1F E7 04 01 F1 E7 07 14 10 00 1F 01 }
0x3C980: 			Default DefaultId: 0x0 Value: 25 { 5B 06 00 00 00 19 }
0x3C986: 		End  { 29 02 }
0x3C988: 		Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4E8, VarStoreId: 0xF101, VarOffset: 0x7EF, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 32 1F 25 1F E8 04 01 F1 EF 07 14 11 01 00 00 10 01 00 }
0x3C99C: 			Default DefaultId: 0x0 Value: 448 { 5B 07 00 00 01 C0 01 }
0x3C9A3: 		End  { 29 02 }
0x3C9A5: 		Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4E9, VarStoreId: 0xF101, VarOffset: 0x7F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 33 1F 27 1F E9 04 01 F1 F9 07 14 10 00 1F 01 }
0x3C9B6: 			Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3C9BC: 		End  { 29 02 }
0x3C9BE: 	End  { 29 02 }
0x3C9C0: 	Form FormId: 0x28B0, Title: " ITBT Root Port 3 Configuration" { 01 86 B0 28 14 1F }
0x3C9C6: 		OneOf Prompt: "ITBT Root Port 3", Help: "None", QuestionFlags: 0x14, QuestionId: 0x28A3, VarStoreId: 0xF101, VarOffset: 0x7D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1B 1F 1C 1F A3 28 01 F1 D0 07 14 10 00 01 00 }
0x3C9D7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3C9DE: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3C9E5: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3C9EB: 		End  { 29 02 }
0x3C9ED: 		Subtitle Prompt: "Root Port 3 Resource Allocation", Help: "", Flags: 0x0 { 02 87 34 1F 00 00 00 }
0x3C9F4: 		End  { 29 02 }
0x3C9F6: 		Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42.
Extra Bus Reserved is required for each layer = (Extra Bus Reserved on the previous layer - 2 - the number of non-hot-plug ports in the current layer) / the number of hot-plug ports in the current layer
Example:
2 non-hot-plug ports and 3 hot-plug ports per connected device have
Recommend below setting
1 device = 7
2 device = 25
3 device = 79, disable one iTBT root port
4 device = 224, disable three iTBT root port, and not every hotplug port supports connecting to the next layer of devices
etc ...", QuestionFlags: 0x14, QuestionId: 0x4EA, VarStoreId: 0xF101, VarOffset: 0x7D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE0, Step: 0x1 { 07 91 35 1F 1F 1F EA 04 01 F1 D6 07 14 10 00 E0 01 }
0x3CA07: 			Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3CA0D: 		End  { 29 02 }
0x3CA0F: 		Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4EB, VarStoreId: 0xF101, VarOffset: 0x7DF, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 36 1F 21 1F EB 04 01 F1 DF 07 14 11 01 00 00 10 01 00 }
0x3CA23: 			Default DefaultId: 0x0 Value: 194 { 5B 07 00 00 01 C2 00 }
0x3CA2A: 		End  { 29 02 }
0x3CA2C: 		Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4EC, VarStoreId: 0xF101, VarOffset: 0x7E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 37 1F 23 1F EC 04 01 F1 E8 07 14 10 00 1F 01 }
0x3CA3D: 			Default DefaultId: 0x0 Value: 25 { 5B 06 00 00 00 19 }
0x3CA43: 		End  { 29 02 }
0x3CA45: 		Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4ED, VarStoreId: 0xF101, VarOffset: 0x7F1, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 38 1F 25 1F ED 04 01 F1 F1 07 14 11 01 00 00 10 01 00 }
0x3CA59: 			Default DefaultId: 0x0 Value: 448 { 5B 07 00 00 01 C0 01 }
0x3CA60: 		End  { 29 02 }
0x3CA62: 		Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4EE, VarStoreId: 0xF101, VarOffset: 0x7FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 39 1F 27 1F EE 04 01 F1 FA 07 14 10 00 1F 01 }
0x3CA73: 			Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3CA79: 		End  { 29 02 }
0x3CA7B: 	End  { 29 02 }
0x3CA7D: 	Form FormId: 0x28B1, Title: "Discrete Thunderbolt(TM) Configuration" { 01 86 B1 28 C1 1E }
0x3CA83: 		Subtitle Prompt: "Discrete Thunderbolt(TM) Configuration", Help: "", Flags: 0x0 { 02 87 C1 1E 00 00 00 }
0x3CA8A: 		End  { 29 02 }
0x3CA8C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3CA93: 		End  { 29 02 }
0x3CA95: 		SuppressIf  { 0A 82 }
0x3CA97: 			EqIdVal QuestionId: 0x289F, Value: 0x0 { 12 06 9F 28 00 00 }
0x3CA9D: 			OneOf Prompt: "Thunderbolt Boot Support", Help: "Enabled allows boot from Bootable devices which is present behind Thunderbolt", QuestionFlags: 0x14, QuestionId: 0x4EF, VarStoreId: 0xF101, VarOffset: 0x79E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 1E E1 1E EF 04 01 F1 9E 07 14 10 00 01 00 }
0x3CAAE: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3CAB4: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3CABB: 				OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x3CAC2: 			End  { 29 02 }
0x3CAC4: 			SuppressIf  { 0A 82 }
0x3CAC6: 				EqIdVal QuestionId: 0x1114, Value: 0x0 { 12 06 14 11 00 00 }
0x3CACC: 				CheckBox Prompt: "GPIO3 Force Pwr", Help: "Set GPIO3 to 1/0", QuestionFlags: 0x10, QuestionId: 0x4F0, VarStoreId: 0xF101, VarOffset: 0x7A0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E F5 1E F6 1E F0 04 01 F1 A0 07 10 00 }
0x3CADA: 				End  { 29 02 }
0x3CADC: 			End  { 29 02 }
0x3CADE: 			OneOf Prompt: "GPIO filter", Help: "GPIO filter is needed to avoid electrical noise on PCH GPIOs during hotplug of 12V USB devices", QuestionFlags: 0x10, QuestionId: 0x4F1, VarStoreId: 0xF101, VarOffset: 0x7A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 1E E5 1E F1 04 01 F1 A4 07 10 10 00 01 00 }
0x3CAEF: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CAF5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3CAFC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3CB03: 			End  { 29 02 }
0x3CB05: 			OneOf Prompt: "DTBT Go2Sx Command", Help: "Command to put DTBT into Sx state while system going into Sx", QuestionFlags: 0x10, QuestionId: 0x4F2, VarStoreId: 0xF101, VarOffset: 0x9A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E6 1E E7 1E F2 04 01 F1 A7 09 10 10 00 01 00 }
0x3CB16: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3CB1C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3CB23: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3CB2A: 			End  { 29 02 }
0x3CB2C: 			OneOf Prompt: "Windows 10 Thunderbolt support", Help: "Windows 10 Thunderbolt support", QuestionFlags: 0x14, QuestionId: 0x28A4, VarStoreId: 0xF101, VarOffset: 0x7C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 0B 1F 0E 1F A4 28 01 F1 C0 07 14 10 00 02 00 }
0x3CB3D: 				OneOfOption Option: "Enable + RTD3" Value: 2, Default { 09 07 0D 1F 10 00 02 }
0x3CB44: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 0C 1F 00 00 00 }
0x3CB4B: 			End  { 29 02 }
0x3CB4D: 			SuppressIf  { 0A 82 }
0x3CB4F: 				QuestionRef1 QuestionId: 0x11D3 { 40 84 D3 11 }
0x3CB53: 					Uint8 Value: 0x1 { 42 03 01 }
0x3CB56: 					GreaterEqual  { 32 02 }
0x3CB58: 					Not  { 17 02 }
0x3CB5A: 				End  { 29 02 }
0x3CB5C: 				Ref Prompt: " DTBT Controller 0 Configuration", Help: " DTBT Controller 0 Configuration", QuestionFlags: 0x0, QuestionId: 0x4F3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28B2 { 0F 0F C3 1E C3 1E F3 04 00 00 FF FF 00 B2 28 }
0x3CB6B: 			End  { 29 02 }
0x3CB6D: 			SuppressIf  { 0A 82 }
0x3CB6F: 				QuestionRef1 QuestionId: 0x11D3 { 40 84 D3 11 }
0x3CB73: 					Uint8 Value: 0x2 { 42 03 02 }
0x3CB76: 					GreaterEqual  { 32 02 }
0x3CB78: 					Not  { 17 02 }
0x3CB7A: 				End  { 29 02 }
0x3CB7C: 				Ref Prompt: " DTBT Controller 1 Configuration", Help: " DTBT Controller 1 Configuration", QuestionFlags: 0x0, QuestionId: 0x4F4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28B3 { 0F 0F C4 1E C4 1E F4 04 00 00 FF FF 00 B3 28 }
0x3CB8B: 			End  { 29 02 }
0x3CB8D: 		End  { 29 02 }
0x3CB8F: 	End  { 29 02 }
0x3CB91: 	Form FormId: 0x28B2, Title: " DTBT Controller 0 Configuration" { 01 86 B2 28 C3 1E }
0x3CB97: 		OneOf Prompt: "DTBT Controller 0", Help: "AUTO - Default, Enable - RVP3 PCIe Root Port1, CNL RVP5 - PCIe Root Port5, CNL SDS - PCIe Root Port5", QuestionFlags: 0x14, QuestionId: 0x28A5, VarStoreId: 0xF101, VarOffset: 0x7A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 1E E9 1E A5 28 01 F1 A7 07 14 10 00 01 00 }
0x3CBA8: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CBAE: 			OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x3CBB5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3CBBC: 		End  { 29 02 }
0x3CBBE: 		SuppressIf  { 0A 82 }
0x3CBC0: 			EqIdVal QuestionId: 0x11D2, Value: 0x1 { 12 86 D2 11 01 00 }
0x3CBC6: 				Not  { 17 02 }
0x3CBC8: 			End  { 29 02 }
0x3CBCA: 			OneOf Prompt: "DTbt Root Port Type", Help: "Select the TBT Root Port Type. PCH or PEG", QuestionFlags: 0x14, QuestionId: 0x28A6, VarStoreId: 0xF101, VarOffset: 0x7A9, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 05 91 EC 1E ED 1E A6 28 01 F1 A9 07 14 10 01 02 00 }
0x3CBDB: 				OneOfOption Option: "PCH Root Port" Value: 1, Default, MfgDefault { 09 07 EE 1E 30 00 01 }
0x3CBE2: 				OneOfOption Option: "PEG Root Port" Value: 2 { 09 07 EF 1E 00 00 02 }
0x3CBE9: 			End  { 29 02 }
0x3CBEB: 		End  { 29 02 }
0x3CBED: 		OneOf Prompt: "TBT Host Router", Help: "Enable the host router based on ports available.", QuestionFlags: 0x14, QuestionId: 0x28A7, VarStoreId: 0xF101, VarOffset: 0x7AE, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 05 91 F0 1E F2 1E A7 28 01 F1 AE 07 14 10 01 02 00 }
0x3CBFE: 			OneOfOption Option: "One port" Value: 1, Default, MfgDefault { 09 07 F3 1E 30 00 01 }
0x3CC05: 			OneOfOption Option: "Two port" Value: 2 { 09 07 F4 1E 00 00 02 }
0x3CC0C: 		End  { 29 02 }
0x3CC0E: 		SuppressIf  { 0A 82 }
0x3CC10: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CC16: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42-One port Host,81-Two port Host.", QuestionFlags: 0x14, QuestionId: 0x4F5, VarStoreId: 0xF101, VarOffset: 0x7B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F7 1E F9 1E F5 04 01 F1 B0 07 14 10 00 FF 01 }
0x3CC27: 				Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3CC2D: 			End  { 29 02 }
0x3CC2F: 		End  { 29 02 }
0x3CC31: 		SuppressIf  { 0A 82 }
0x3CC33: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CC39: 				Not  { 17 02 }
0x3CC3B: 			End  { 29 02 }
0x3CC3D: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42-One port Host,81-Two port Host.", QuestionFlags: 0x14, QuestionId: 0x4F6, VarStoreId: 0xF101, VarOffset: 0x7B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F7 1E F9 1E F6 04 01 F1 B0 07 14 10 00 FF 01 }
0x3CC4E: 				Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3CC54: 			End  { 29 02 }
0x3CC56: 		End  { 29 02 }
0x3CC58: 		Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4F7, VarStoreId: 0xF101, VarOffset: 0x7B2, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 FA 1E FB 1E F7 04 01 F1 B2 07 14 11 01 00 00 10 01 00 }
0x3CC6C: 			SuppressIf  { 0A 82 }
0x3CC6E: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CC74: 				Default DefaultId: 0x0 Value: 96 { 5B 07 00 00 01 60 00 }
0x3CC7B: 			End  { 29 02 }
0x3CC7D: 			SuppressIf  { 0A 82 }
0x3CC7F: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CC85: 					Not  { 17 02 }
0x3CC87: 				End  { 29 02 }
0x3CC89: 				Default DefaultId: 0x0 Value: 356 { 5B 07 00 00 01 64 01 }
0x3CC90: 			End  { 29 02 }
0x3CC92: 		End  { 29 02 }
0x3CC94: 		Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4F8, VarStoreId: 0xF101, VarOffset: 0x7B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 FC 1E FD 1E F8 04 01 F1 B8 07 14 10 00 1F 01 }
0x3CCA5: 			SuppressIf  { 0A 82 }
0x3CCA7: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CCAD: 				Default DefaultId: 0x0 Value: 26 { 5B 06 00 00 00 1A }
0x3CCB3: 			End  { 29 02 }
0x3CCB5: 			SuppressIf  { 0A 82 }
0x3CCB7: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CCBD: 					Not  { 17 02 }
0x3CCBF: 				End  { 29 02 }
0x3CCC1: 				Default DefaultId: 0x0 Value: 26 { 5B 06 00 00 00 1A }
0x3CCC7: 			End  { 29 02 }
0x3CCC9: 		End  { 29 02 }
0x3CCCB: 		SuppressIf  { 0A 82 }
0x3CCCD: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CCD3: 			Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory per port for this Root Bridge (1-32768) MB. Reserved memory will be twice for two port host.", QuestionFlags: 0x14, QuestionId: 0x4F9, VarStoreId: 0xF101, VarOffset: 0x7BA, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x8000, Step: 0x1 { 07 94 FE 1E 00 1F F9 04 01 F1 BA 07 14 11 01 00 00 80 01 00 }
0x3CCE7: 				Default DefaultId: 0x0 Value: 32768 { 5B 07 00 00 01 00 80 }
0x3CCEE: 			End  { 29 02 }
0x3CCF0: 		End  { 29 02 }
0x3CCF2: 		SuppressIf  { 0A 82 }
0x3CCF4: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CCFA: 				Not  { 17 02 }
0x3CCFC: 			End  { 29 02 }
0x3CCFE: 			Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory per port for this Root Bridge (1-32768) MB. Reserved memory will be twice for two port host.", QuestionFlags: 0x14, QuestionId: 0x4FA, VarStoreId: 0xF101, VarOffset: 0x7BA, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x8000, Step: 0x1 { 07 94 FE 1E 00 1F FA 04 01 F1 BA 07 14 11 01 00 00 80 01 00 }
0x3CD12: 				Default DefaultId: 0x0 Value: 32768 { 5B 07 00 00 01 00 80 }
0x3CD19: 			End  { 29 02 }
0x3CD1B: 		End  { 29 02 }
0x3CD1D: 		Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x4FB, VarStoreId: 0xF101, VarOffset: 0x7BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 01 1F 02 1F FB 04 01 F1 BE 07 14 10 00 1F 01 }
0x3CD2E: 			SuppressIf  { 0A 82 }
0x3CD30: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CD36: 				Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3CD3C: 			End  { 29 02 }
0x3CD3E: 			SuppressIf  { 0A 82 }
0x3CD40: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CD46: 					Not  { 17 02 }
0x3CD48: 				End  { 29 02 }
0x3CD4A: 				Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3CD50: 			End  { 29 02 }
0x3CD52: 		End  { 29 02 }
0x3CD54: 		Numeric Prompt: "Reserved I/O", Help: "Reserved I/O", QuestionFlags: 0x14, QuestionId: 0x4FC, VarStoreId: 0xF101, VarOffset: 0x7B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3C, Step: 0x4 { 07 91 03 1F 04 1F FC 04 01 F1 B6 07 14 10 00 3C 04 }
0x3CD65: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CD6B: 		End  { 29 02 }
0x3CD6D: 	End  { 29 02 }
0x3CD6F: 	Form FormId: 0x28B3, Title: " DTBT Controller 1 Configuration" { 01 86 B3 28 C4 1E }
0x3CD75: 		OneOf Prompt: "DTBT Controller 1", Help: "None", QuestionFlags: 0x14, QuestionId: 0x28A8, VarStoreId: 0xF101, VarOffset: 0x7A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 1E EB 1E A8 28 01 F1 A8 07 14 10 00 01 00 }
0x3CD86: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CD8C: 			OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x3CD93: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3CD9A: 		End  { 29 02 }
0x3CD9C: 		SuppressIf  { 0A 82 }
0x3CD9E: 			EqIdVal QuestionId: 0x11D2, Value: 0x1 { 12 86 D2 11 01 00 }
0x3CDA4: 				Not  { 17 02 }
0x3CDA6: 			End  { 29 02 }
0x3CDA8: 			OneOf Prompt: "DTbt Root Port Type", Help: "Select the TBT Root Port Type. PCH or PEG", QuestionFlags: 0x14, QuestionId: 0x28A9, VarStoreId: 0xF101, VarOffset: 0x7AA, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 05 91 3C 1F ED 1E A9 28 01 F1 AA 07 14 10 01 02 00 }
0x3CDB9: 				OneOfOption Option: "PCH Root Port" Value: 1, Default, MfgDefault { 09 07 EE 1E 30 00 01 }
0x3CDC0: 				OneOfOption Option: "PEG Root Port" Value: 2 { 09 07 EF 1E 00 00 02 }
0x3CDC7: 			End  { 29 02 }
0x3CDC9: 		End  { 29 02 }
0x3CDCB: 		OneOf Prompt: "TBT Host Router", Help: "Enable the host router based on ports available.", QuestionFlags: 0x14, QuestionId: 0x28AA, VarStoreId: 0xF101, VarOffset: 0x7AF, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 05 91 F1 1E F2 1E AA 28 01 F1 AF 07 14 10 01 02 00 }
0x3CDDC: 			OneOfOption Option: "One port" Value: 1, Default, MfgDefault { 09 07 F3 1E 30 00 01 }
0x3CDE3: 			OneOfOption Option: "Two port" Value: 2 { 09 07 F4 1E 00 00 02 }
0x3CDEA: 		End  { 29 02 }
0x3CDEC: 		SuppressIf  { 0A 82 }
0x3CDEE: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CDF4: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42-One port Host,81-Two port Host.", QuestionFlags: 0x14, QuestionId: 0x4FD, VarStoreId: 0xF101, VarOffset: 0x7B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 05 1F F9 1E FD 04 01 F1 B1 07 14 10 00 FF 01 }
0x3CE05: 				Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3CE0B: 			End  { 29 02 }
0x3CE0D: 		End  { 29 02 }
0x3CE0F: 		SuppressIf  { 0A 82 }
0x3CE11: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CE17: 				Not  { 17 02 }
0x3CE19: 			End  { 29 02 }
0x3CE1B: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 42-One port Host,81-Two port Host.", QuestionFlags: 0x14, QuestionId: 0x4FE, VarStoreId: 0xF101, VarOffset: 0x7B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 05 1F F9 1E FE 04 01 F1 B1 07 14 10 00 FF 01 }
0x3CE2C: 				Default DefaultId: 0x0 Value: 42 { 5B 06 00 00 00 2A }
0x3CE32: 			End  { 29 02 }
0x3CE34: 		End  { 29 02 }
0x3CE36: 		Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x4FF, VarStoreId: 0xF101, VarOffset: 0x7B4, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1 { 07 94 06 1F FB 1E FF 04 01 F1 B4 07 14 11 01 00 00 10 01 00 }
0x3CE4A: 			SuppressIf  { 0A 82 }
0x3CE4C: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CE52: 				Default DefaultId: 0x0 Value: 96 { 5B 07 00 00 01 60 00 }
0x3CE59: 			End  { 29 02 }
0x3CE5B: 			SuppressIf  { 0A 82 }
0x3CE5D: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CE63: 					Not  { 17 02 }
0x3CE65: 				End  { 29 02 }
0x3CE67: 				Default DefaultId: 0x0 Value: 356 { 5B 07 00 00 01 64 01 }
0x3CE6E: 			End  { 29 02 }
0x3CE70: 		End  { 29 02 }
0x3CE72: 		Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x500, VarStoreId: 0xF101, VarOffset: 0x7B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 07 1F FD 1E 00 05 01 F1 B9 07 14 10 00 1F 01 }
0x3CE83: 			SuppressIf  { 0A 82 }
0x3CE85: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CE8B: 				Default DefaultId: 0x0 Value: 26 { 5B 06 00 00 00 1A }
0x3CE91: 			End  { 29 02 }
0x3CE93: 			SuppressIf  { 0A 82 }
0x3CE95: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CE9B: 					Not  { 17 02 }
0x3CE9D: 				End  { 29 02 }
0x3CE9F: 				Default DefaultId: 0x0 Value: 26 { 5B 06 00 00 00 1A }
0x3CEA5: 			End  { 29 02 }
0x3CEA7: 		End  { 29 02 }
0x3CEA9: 		SuppressIf  { 0A 82 }
0x3CEAB: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CEB1: 			Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory per port for this Root Bridge (1-32768) MB. Reserved memory will be twice for two port host.", QuestionFlags: 0x14, QuestionId: 0x501, VarStoreId: 0xF101, VarOffset: 0x7BC, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x8000, Step: 0x1 { 07 94 08 1F 00 1F 01 05 01 F1 BC 07 14 11 01 00 00 80 01 00 }
0x3CEC5: 				Default DefaultId: 0x0 Value: 32768 { 5B 07 00 00 01 00 80 }
0x3CECC: 			End  { 29 02 }
0x3CECE: 		End  { 29 02 }
0x3CED0: 		SuppressIf  { 0A 82 }
0x3CED2: 			EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CED8: 				Not  { 17 02 }
0x3CEDA: 			End  { 29 02 }
0x3CEDC: 			Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory per port for this Root Bridge (1-32768) MB. Reserved memory will be twice for two port host.", QuestionFlags: 0x14, QuestionId: 0x502, VarStoreId: 0xF101, VarOffset: 0x7BC, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x8000, Step: 0x1 { 07 94 08 1F 00 1F 02 05 01 F1 BC 07 14 11 01 00 00 80 01 00 }
0x3CEF0: 				Default DefaultId: 0x0 Value: 32768 { 5B 07 00 00 01 00 80 }
0x3CEF7: 			End  { 29 02 }
0x3CEF9: 		End  { 29 02 }
0x3CEFB: 		Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x503, VarStoreId: 0xF101, VarOffset: 0x7BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 09 1F 02 1F 03 05 01 F1 BF 07 14 10 00 1F 01 }
0x3CF0C: 			SuppressIf  { 0A 82 }
0x3CF0E: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 06 D1 11 00 00 }
0x3CF14: 				Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3CF1A: 			End  { 29 02 }
0x3CF1C: 			SuppressIf  { 0A 82 }
0x3CF1E: 				EqIdVal QuestionId: 0x11D1, Value: 0x0 { 12 86 D1 11 00 00 }
0x3CF24: 					Not  { 17 02 }
0x3CF26: 				End  { 29 02 }
0x3CF28: 				Default DefaultId: 0x0 Value: 28 { 5B 06 00 00 00 1C }
0x3CF2E: 			End  { 29 02 }
0x3CF30: 		End  { 29 02 }
0x3CF32: 		Numeric Prompt: "Reserved I/O", Help: "Reserved I/O", QuestionFlags: 0x14, QuestionId: 0x504, VarStoreId: 0xF101, VarOffset: 0x7B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3C, Step: 0x4 { 07 91 0A 1F 04 1F 04 05 01 F1 B7 07 14 10 00 3C 04 }
0x3CF43: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CF49: 		End  { 29 02 }
0x3CF4B: 	End  { 29 02 }
0x3CF4D: 	Form FormId: 0x28B9, Title: "Debug Settings" { 01 86 B9 28 46 1F }
0x3CF53: 		Subtitle Prompt: "Debug Settings", Help: "", Flags: 0x0 { 02 87 46 1F 00 00 00 }
0x3CF5A: 		End  { 29 02 }
0x3CF5C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3CF63: 		End  { 29 02 }
0x3CF65: 		OneOf Prompt: "Kernel Debug Serial Port", Help: "Select Kernel Debug Port and report in ACPI DBG2 table", QuestionFlags: 0x10, QuestionId: 0x505, VarStoreId: 0x6, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 4A 1F 50 1F 05 05 06 00 08 00 10 10 00 03 00 }
0x3CF76: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CF7C: 			OneOfOption Option: "Legacy UART" Value: 0 { 09 07 4B 1F 00 00 00 }
0x3CF83: 			OneOfOption Option: "SERIALIO UART2" Value: 3 { 09 07 4D 1F 00 00 03 }
0x3CF8A: 		End  { 29 02 }
0x3CF8C: 		SuppressIf  { 0A 82 }
0x3CF8E: 			EqIdVal QuestionId: 0x505, Value: 0x0 { 12 06 05 05 00 00 }
0x3CF94: 			OneOf Prompt: "Serial Io Uart Debug Power Gating", Help: "For S0iX support with Kernel Debugger Enabled.
BIOS needs to change DBG2 Port Sub Type as value of 0x14 (0x0014 Intel LPSS)
Note: Requires OS support", QuestionFlags: 0x10, QuestionId: 0x506, VarStoreId: 0x6, VarOffset: 0x786, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 1F 4F 1F 06 05 06 00 86 07 10 10 00 01 00 }
0x3CFA5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3CFAC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3CFB3: 			End  { 29 02 }
0x3CFB5: 		End  { 29 02 }
0x3CFB7: 		OneOf Prompt: "Kernel Debug Patch", Help: "Enable/Disable Kernel Debug Patch", QuestionFlags: 0x10, QuestionId: 0x507, VarStoreId: 0xF101, VarOffset: 0x864, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 51 1F 52 1F 07 05 01 F1 64 08 10 10 00 01 00 }
0x3CFC8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3CFCF: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3CFD6: 		End  { 29 02 }
0x3CFD8: 		Text Prompt: "Debug Token is present", Help: "Debug Token is present", Text: "N/A" { 03 08 53 1F 53 1F 54 1F }
0x3CFE0: 		GrayOutIf  { 19 82 }
0x3CFE2: 			EqIdVal QuestionId: 0x11D0, Value: 0x1 { 12 06 D0 11 01 00 }
0x3CFE8: 			OneOf Prompt: "Platform Debug Consent", Help: "Enabled(All Probes+TraceHub) supports all probes with TraceHub enabled and blocks s0ix

Enabled(Low Power) Tracehub is powergated by default, s0ix is viable

Manual:user needs to configure Advanced Debug Settings manually, aimed at advanced users", QuestionFlags: 0x14, QuestionId: 0x28B4, VarStoreId: 0xD, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 55 1F 56 1F B4 28 0D 00 01 00 14 10 00 07 00 }
0x3CFF9: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3CFFF: 				OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x3D006: 				OneOfOption Option: "Enabled (All Probes+TraceHub)" Value: 2 { 09 07 57 1F 00 00 02 }
0x3D00D: 				OneOfOption Option: "Enabled (Low Power)" Value: 6 { 09 07 58 1F 00 00 06 }
0x3D014: 				OneOfOption Option: "Manual" Value: 7 { 09 07 59 1F 00 00 07 }
0x3D01B: 			End  { 29 02 }
0x3D01D: 		End  { 29 02 }
0x3D01F: 		Ref Prompt: "VT-d Debug Settings", Help: "Vt-d Debug Settings", QuestionFlags: 0x0, QuestionId: 0x508, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28BA { 0F 0F 9D 1F 9E 1F 08 05 00 00 FF FF 00 BA 28 }
0x3D02E: 		Ref Prompt: "Advanced Debug Settings", Help: "Advanced Debug Settings", QuestionFlags: 0x0, QuestionId: 0x509, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28BB { 0F 0F 48 1F 49 1F 09 05 00 00 FF FF 00 BB 28 }
0x3D03D: 	End  { 29 02 }
0x3D03F: 	Form FormId: 0x28BA, Title: "VT-d Debug Settings" { 01 86 BA 28 9D 1F }
0x3D045: 		GrayOutIf  { 19 82 }
0x3D047: 			EqIdVal QuestionId: 0x1174, Value: 0x0 { 12 86 74 11 00 00 }
0x3D04D: 				EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x3D053: 				Or  { 16 02 }
0x3D055: 			End  { 29 02 }
0x3D057: 			OneOf Prompt: "IGD VTD Enable", Help: "Enable/Disable IGD VTD", QuestionFlags: 0x10, QuestionId: 0x50A, VarStoreId: 0x4, VarOffset: 0x88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 0D BA 0D 0A 05 04 00 88 00 10 10 00 01 00 }
0x3D068: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x3D06F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x3D076: 			End  { 29 02 }
0x3D078: 			OneOf Prompt: "IPU VTD Enable", Help: "Enable/Disable IPU VTD", QuestionFlags: 0x10, QuestionId: 0x50B, VarStoreId: 0x4, VarOffset: 0x89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 0D BC 0D 0B 05 04 00 89 00 10 10 00 01 00 }
0x3D089: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x3D090: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x3D097: 			End  { 29 02 }
0x3D099: 			OneOf Prompt: "IOP VTD Enable", Help: "Enable/Disable IOP VTD", QuestionFlags: 0x10, QuestionId: 0x50C, VarStoreId: 0x4, VarOffset: 0x8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 0D BE 0D 0C 05 04 00 8A 00 10 10 00 01 00 }
0x3D0AA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x3D0B1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x3D0B8: 			End  { 29 02 }
0x3D0BA: 		End  { 29 02 }
0x3D0BC: 	End  { 29 02 }
0x3D0BE: 	Form FormId: 0x28BB, Title: "Advanced Debug Settings" { 01 86 BB 28 48 1F }
0x3D0C4: 		OneOf Prompt: "USB3 Type-C UFP2DFP Kernel/Platform Debug Support", Help: "This BIOS option enables kernel and platform debug for USB3 interface over a UFP Type-C receptacle, select 'No Change' will do nothing to UFP2DFP setting", QuestionFlags: 0x10, QuestionId: 0x50D, VarStoreId: 0x6, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 74 1F 75 1F 0D 05 06 00 0A 00 10 10 00 02 00 }
0x3D0D5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D0DC: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D0E3: 			OneOfOption Option: "No Change" Value: 2, Default, MfgDefault { 09 07 72 1F 30 00 02 }
0x3D0EA: 		End  { 29 02 }
0x3D0EC: 		OneOf Prompt: "USB DbC Enable Mode", Help: "Disabled:Clear both USB2/3DBCEN
USB2:Set USB2DBCEN
USB3:Set USB3DBCEN
Both:Set both USB2/3DBCEN
No Change:Comply with HW value", QuestionFlags: 0x10, QuestionId: 0x50E, VarStoreId: 0x6, VarOffset: 0x73F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5C 1F 5D 1F 0E 05 06 00 3F 07 10 10 00 04 00 }
0x3D0FD: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D104: 			OneOfOption Option: "USB2" Value: 1 { 09 07 5E 1F 00 00 01 }
0x3D10B: 			OneOfOption Option: "USB3" Value: 2 { 09 07 5F 1F 00 00 02 }
0x3D112: 			OneOfOption Option: "Both" Value: 3 { 09 07 60 1F 00 00 03 }
0x3D119: 			OneOfOption Option: "No Change" Value: 4, Default, MfgDefault { 09 07 72 1F 30 00 04 }
0x3D120: 		End  { 29 02 }
0x3D122: 		GrayOutIf  { 19 82 }
0x3D124: 			EqIdVal QuestionId: 0x28B4, Value: 0x7 { 12 86 B4 28 07 00 }
0x3D12A: 				Not  { 17 02 }
0x3D12C: 			End  { 29 02 }
0x3D12E: 			SuppressIf  { 0A 82 }
0x3D130: 				EqIdVal QuestionId: 0x28B4, Value: 0x0 { 12 06 B4 28 00 00 }
0x3D136: 				OneOf Prompt: "DCI Enable", Help: "Determine if to enable DCI debug from host", QuestionFlags: 0x10, QuestionId: 0x50F, VarStoreId: 0x6, VarOffset: 0x73E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5A 1F 5B 1F 0F 05 06 00 3E 07 10 10 00 01 00 }
0x3D147: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D14E: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D155: 				End  { 29 02 }
0x3D157: 			End  { 29 02 }
0x3D159: 			GrayOutIf  { 19 82 }
0x3D15B: 				EqIdVal QuestionId: 0x11CF, Value: 0x1 { 12 06 CF 11 01 00 }
0x3D161: 				OneOf Prompt: "PCH Trace Hub Enable Mode", Help: "Select 'Host Debugger' if Trace Hub is used with host debugger tool or 'Target Debugger' if Trace Hub is used by target debugger software.
Note: If 'Host Debugger' is selected, Platform Debug Consent has to be ENABLED because DCI is one of the primary trace data output paths.", QuestionFlags: 0x10, QuestionId: 0x510, VarStoreId: 0x6, VarOffset: 0x714, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 78 1F 79 1F 10 05 06 00 14 07 10 10 00 02 00 }
0x3D172: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D179: 					OneOfOption Option: "Target Debugger" Value: 1 { 09 07 80 1F 00 00 01 }
0x3D180: 					OneOfOption Option: "Host Debugger" Value: 2 { 09 07 81 1F 00 00 02 }
0x3D187: 				End  { 29 02 }
0x3D189: 			End  { 29 02 }
0x3D18B: 			SuppressIf  { 0A 82 }
0x3D18D: 				EqIdVal QuestionId: 0x510, Value: 0x0 { 12 06 10 05 00 00 }
0x3D193: 				OneOf Prompt: "PCH TH Mem Buffer Size 0", Help: "Select size of memory region 0 buffer. Choose None/OS if OS-supported memory or trace forwarding is desired
Note : Limit of total buffer size (PCH + CPU) is 512MB when iTBT disabled, 256MB when iTBT enabled", QuestionFlags: 0x10, QuestionId: 0x511, VarStoreId: 0x6, VarOffset: 0x715, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 7A 1F 7E 1F 11 05 06 00 15 07 10 10 00 06 00 }
0x3D1A4: 					OneOfOption Option: "None/OS" Value: 0, Default, MfgDefault { 09 07 82 1F 30 00 00 }
0x3D1AB: 					OneOfOption Option: "1MB" Value: 1 { 09 07 83 1F 00 00 01 }
0x3D1B2: 					OneOfOption Option: "8MB" Value: 2 { 09 07 84 1F 00 00 02 }
0x3D1B9: 					OneOfOption Option: "64MB" Value: 3 { 09 07 85 1F 00 00 03 }
0x3D1C0: 					OneOfOption Option: "128MB" Value: 4 { 09 07 86 1F 00 00 04 }
0x3D1C7: 					OneOfOption Option: "256MB" Value: 5 { 09 07 87 1F 00 00 05 }
0x3D1CE: 					OneOfOption Option: "512MB" Value: 6 { 09 07 88 1F 00 00 06 }
0x3D1D5: 				End  { 29 02 }
0x3D1D7: 				OneOf Prompt: "PCH TH Mem Buffer Size 1", Help: "Select size of memory region 1 buffer. Choose None/OS if OS-supported memory or trace forwarding is desired
Note : Limit of total buffer size (PCH + CPU) is 512MB when iTBT disabled, 256MB when iTBT enabled", QuestionFlags: 0x10, QuestionId: 0x512, VarStoreId: 0x6, VarOffset: 0x716, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 7B 1F 7F 1F 12 05 06 00 16 07 10 10 00 06 00 }
0x3D1E8: 					OneOfOption Option: "None/OS" Value: 0, Default, MfgDefault { 09 07 82 1F 30 00 00 }
0x3D1EF: 					OneOfOption Option: "1MB" Value: 1 { 09 07 83 1F 00 00 01 }
0x3D1F6: 					OneOfOption Option: "8MB" Value: 2 { 09 07 84 1F 00 00 02 }
0x3D1FD: 					OneOfOption Option: "64MB" Value: 3 { 09 07 85 1F 00 00 03 }
0x3D204: 					OneOfOption Option: "128MB" Value: 4 { 09 07 86 1F 00 00 04 }
0x3D20B: 					OneOfOption Option: "256MB" Value: 5 { 09 07 87 1F 00 00 05 }
0x3D212: 					OneOfOption Option: "512MB" Value: 6 { 09 07 88 1F 00 00 06 }
0x3D219: 				End  { 29 02 }
0x3D21B: 			End  { 29 02 }
0x3D21D: 			OneOf Prompt: "CPU Trace Hub Enable Mode", Help: "Select 'Host Debugger' if Trace Hub is used with host debugger tool or 'Target Debugger' if Trace Hub is used by target debugger software.
Note: If 'Host Debugger' is selected, Platform Debug Consent has to be ENABLED because DCI is one of the primary trace data output paths.", QuestionFlags: 0x10, QuestionId: 0x513, VarStoreId: 0x4, VarOffset: 0x83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 89 1F 79 1F 13 05 04 00 83 00 10 10 00 02 00 }
0x3D22E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D235: 				OneOfOption Option: "Target Debugger" Value: 1 { 09 07 80 1F 00 00 01 }
0x3D23C: 				OneOfOption Option: "Host Debugger" Value: 2 { 09 07 81 1F 00 00 02 }
0x3D243: 			End  { 29 02 }
0x3D245: 			SuppressIf  { 0A 82 }
0x3D247: 				EqIdVal QuestionId: 0x513, Value: 0x0 { 12 06 13 05 00 00 }
0x3D24D: 				OneOf Prompt: "CPU TH Mem Buffer Size 0", Help: "Select size of memory region 0 buffer. Choose None/OS if OS-supported memory or trace forwarding is desired
Note : Limit of total buffer size (PCH + CPU) is 512MB when iTBT disabled, 256MB when iTBT enabled", QuestionFlags: 0x10, QuestionId: 0x514, VarStoreId: 0x4, VarOffset: 0x84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 7C 1F 7E 1F 14 05 04 00 84 00 10 10 00 06 00 }
0x3D25E: 					OneOfOption Option: "None/OS" Value: 0, Default, MfgDefault { 09 07 82 1F 30 00 00 }
0x3D265: 					OneOfOption Option: "1MB" Value: 1 { 09 07 83 1F 00 00 01 }
0x3D26C: 					OneOfOption Option: "8MB" Value: 2 { 09 07 84 1F 00 00 02 }
0x3D273: 					OneOfOption Option: "64MB" Value: 3 { 09 07 85 1F 00 00 03 }
0x3D27A: 					OneOfOption Option: "128MB" Value: 4 { 09 07 86 1F 00 00 04 }
0x3D281: 					OneOfOption Option: "256MB" Value: 5 { 09 07 87 1F 00 00 05 }
0x3D288: 					OneOfOption Option: "512MB" Value: 6 { 09 07 88 1F 00 00 06 }
0x3D28F: 				End  { 29 02 }
0x3D291: 				SuppressIf  { 0A 82 }
0x3D293: 					EqIdVal QuestionId: 0x11CE, Value: 0x1 { 12 06 CE 11 01 00 }
0x3D299: 					OneOf Prompt: "CPU TH Mem Buffer Size 1", Help: "Select size of memory region 1 buffer. Choose None/OS if OS-supported memory or trace forwarding is desired
Note : Limit of total buffer size (PCH + CPU) is 512MB when iTBT disabled, 256MB when iTBT enabled", QuestionFlags: 0x10, QuestionId: 0x515, VarStoreId: 0x4, VarOffset: 0x85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 7D 1F 7F 1F 15 05 04 00 85 00 10 10 00 06 00 }
0x3D2AA: 						OneOfOption Option: "None/OS" Value: 0, Default, MfgDefault { 09 07 82 1F 30 00 00 }
0x3D2B1: 						OneOfOption Option: "1MB" Value: 1 { 09 07 83 1F 00 00 01 }
0x3D2B8: 						OneOfOption Option: "8MB" Value: 2 { 09 07 84 1F 00 00 02 }
0x3D2BF: 						OneOfOption Option: "64MB" Value: 3 { 09 07 85 1F 00 00 03 }
0x3D2C6: 						OneOfOption Option: "128MB" Value: 4 { 09 07 86 1F 00 00 04 }
0x3D2CD: 						OneOfOption Option: "256MB" Value: 5 { 09 07 87 1F 00 00 05 }
0x3D2D4: 						OneOfOption Option: "512MB" Value: 6 { 09 07 88 1F 00 00 06 }
0x3D2DB: 					End  { 29 02 }
0x3D2DD: 				End  { 29 02 }
0x3D2DF: 			End  { 29 02 }
0x3D2E1: 		End  { 29 02 }
0x3D2E3: 		SuppressIf  { 0A 82 }
0x3D2E5: 			EqIdVal QuestionId: 0x11CD, Value: 0x0 { 12 06 CD 11 00 00 }
0x3D2EB: 			OneOf Prompt: "CPU Run Control ", Help: "Enable/Disable CPU Run Control Support; No Change : Comply with HW value", QuestionFlags: 0x10, QuestionId: 0x516, VarStoreId: 0x1, VarOffset: 0x111, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 61 1F 62 1F 16 05 01 00 11 01 10 10 00 02 00 }
0x3D2FC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x3D303: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x3D30A: 				OneOfOption Option: "No Change" Value: 2, Default, MfgDefault { 09 07 73 1F 30 00 02 }
0x3D311: 			End  { 29 02 }
0x3D313: 			SuppressIf  { 0A 82 }
0x3D315: 				EqIdVal QuestionId: 0x516, Value: 0x2 { 12 06 16 05 02 00 }
0x3D31B: 				OneOf Prompt: "CPU Run Control Lock ", Help: "Enable/Disable CPU Run Control Lock", QuestionFlags: 0x10, QuestionId: 0x517, VarStoreId: 0x1, VarOffset: 0x112, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 1F 64 1F 17 05 01 00 12 01 10 10 00 01 00 }
0x3D32C: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D333: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3D33A: 				End  { 29 02 }
0x3D33C: 			End  { 29 02 }
0x3D33E: 		End  { 29 02 }
0x3D340: 		GrayOutIf  { 19 82 }
0x3D342: 			EqIdVal QuestionId: 0x11CC, Value: 0x1 { 12 06 CC 11 01 00 }
0x3D348: 			OneOf Prompt: "USB Overcurrent Override for VISA", Help: "This option overrides USB Over Current enablement state that USB OC will be disabled after enabling this option. Enable when VISA pin is muxed with USB OC", QuestionFlags: 0x10, QuestionId: 0x518, VarStoreId: 0x6, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 1F 77 1F 18 05 06 00 0B 00 10 10 00 01 00 }
0x3D359: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D360: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D367: 			End  { 29 02 }
0x3D369: 		End  { 29 02 }
0x3D36B: 		SuppressIf  { 0A 82 }
0x3D36D: 			EqIdVal QuestionId: 0x11CB, Value: 0x0 { 12 06 CB 11 00 00 }
0x3D373: 			OneOf Prompt: "Processor trace memory allocation", Help: "Disable or Select Processor trace memory region Size: from 4KB ~ 128MB", QuestionFlags: 0x10, QuestionId: 0x519, VarStoreId: 0x1, VarOffset: 0x122, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 66 1F 67 1F 19 05 01 00 22 01 10 10 00 FF 00 }
0x3D384: 				OneOfOption Option: "Disabled" Value: 255, Default, MfgDefault { 09 07 04 00 30 00 FF }
0x3D38B: 				OneOfOption Option: "4KB" Value: 0 { 09 07 74 07 00 00 00 }
0x3D392: 				OneOfOption Option: "8KB" Value: 1 { 09 07 75 07 00 00 01 }
0x3D399: 				OneOfOption Option: "16KB" Value: 2 { 09 07 76 07 00 00 02 }
0x3D3A0: 				OneOfOption Option: "32KB" Value: 3 { 09 07 77 07 00 00 03 }
0x3D3A7: 				OneOfOption Option: "64KB" Value: 4 { 09 07 78 07 00 00 04 }
0x3D3AE: 				OneOfOption Option: "128KB" Value: 5 { 09 07 79 07 00 00 05 }
0x3D3B5: 				OneOfOption Option: "256KB" Value: 6 { 09 07 7A 07 00 00 06 }
0x3D3BC: 				OneOfOption Option: "512KB" Value: 7 { 09 07 7B 07 00 00 07 }
0x3D3C3: 				OneOfOption Option: "1MB" Value: 8 { 09 07 7C 07 00 00 08 }
0x3D3CA: 				OneOfOption Option: "2MB" Value: 9 { 09 07 7D 07 00 00 09 }
0x3D3D1: 				OneOfOption Option: "4MB" Value: 10 { 09 07 7E 07 00 00 0A }
0x3D3D8: 				OneOfOption Option: "8MB" Value: 11 { 09 07 7F 07 00 00 0B }
0x3D3DF: 				OneOfOption Option: "16MB" Value: 12 { 09 07 80 07 00 00 0C }
0x3D3E6: 				OneOfOption Option: "32MB" Value: 13 { 09 07 81 07 00 00 0D }
0x3D3ED: 				OneOfOption Option: "64MB" Value: 14 { 09 07 8D 00 00 00 0E }
0x3D3F4: 				OneOfOption Option: "128MB" Value: 15 { 09 07 8E 00 00 00 0F }
0x3D3FB: 			End  { 29 02 }
0x3D3FD: 		End  { 29 02 }
0x3D3FF: 		SuppressIf  { 0A 82 }
0x3D401: 			EqIdVal QuestionId: 0x11CB, Value: 0x0 { 12 86 CB 11 00 00 }
0x3D407: 				EqIdVal QuestionId: 0x519, Value: 0xFF { 12 06 19 05 FF 00 }
0x3D40D: 				Or  { 16 02 }
0x3D40F: 			End  { 29 02 }
0x3D411: 			OneOf Prompt: "Processor trace", Help: "Enable/Disable processor trace feature from CPU MSR. Enabling this feature will immediately start trace collection.", QuestionFlags: 0x10, QuestionId: 0x51A, VarStoreId: 0x1, VarOffset: 0x123, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 1F 69 1F 1A 05 01 00 23 01 10 10 00 01 00 }
0x3D422: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x3D429: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x3D430: 			End  { 29 02 }
0x3D432: 			OneOf Prompt: "Processor Trace OutPut Scheme", Help: "Select Single Range Output scheme or ToPA table Output scheme", QuestionFlags: 0x10, QuestionId: 0x51B, VarStoreId: 0x1, VarOffset: 0x121, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6A 1F 6B 1F 1B 05 01 00 21 01 10 10 00 01 00 }
0x3D443: 				OneOfOption Option: "Single Range Output" Value: 0, Default, MfgDefault { 09 07 72 07 30 00 00 }
0x3D44A: 				OneOfOption Option: "ToPA Output" Value: 1 { 09 07 73 07 00 00 01 }
0x3D451: 			End  { 29 02 }
0x3D453: 			OneOf Prompt: "SMM Processor Trace", Help: "Enable/Disable usage of Processor Trace in SMM", QuestionFlags: 0x10, QuestionId: 0x51C, VarStoreId: 0x1, VarOffset: 0x22E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 1F 6D 1F 1C 05 01 00 2E 02 10 10 00 01 00 }
0x3D464: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D46B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D472: 			End  { 29 02 }
0x3D474: 		End  { 29 02 }
0x3D476: 		GrayOutIf  { 19 82 }
0x3D478: 			EqIdVal QuestionId: 0x11CA, Value: 0x1 { 12 06 CA 11 01 00 }
0x3D47E: 			OneOf Prompt: "JTAG C10 Power Gate", Help: "When Enabled, JTAG is power gated in C10 state. When Disabled, keeps the JTAG power up during C10 and deeper power states for debug purpose. ", QuestionFlags: 0x10, QuestionId: 0x51D, VarStoreId: 0x1, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 1F 6F 1F 1D 05 01 00 08 00 10 10 00 01 00 }
0x3D48F: 				OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x3D496: 				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x3D49D: 			End  { 29 02 }
0x3D49F: 		End  { 29 02 }
0x3D4A1: 		OneOf Prompt: "Three Strike Counter", Help: "Enable/Disable Three Strike Counter", QuestionFlags: 0x10, QuestionId: 0x51E, VarStoreId: 0x1, VarOffset: 0x125, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 1F 71 1F 1E 05 01 00 25 01 10 10 00 01 00 }
0x3D4B2: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 04 00 00 00 01 }
0x3D4B9: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 03 00 30 00 00 }
0x3D4C0: 		End  { 29 02 }
0x3D4C2: 		OneOf Prompt: "CrashLog Feature", Help: "The feature helps collecting crash data from PMC SSRAM", QuestionFlags: 0x10, QuestionId: 0x51F, VarStoreId: 0xF101, VarOffset: 0x856, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 1F 8B 1F 1F 05 01 F1 56 08 10 10 00 01 00 }
0x3D4D3: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D4DA: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3D4E1: 		End  { 29 02 }
0x3D4E3: 		SuppressIf  { 0A 82 }
0x3D4E5: 			EqIdVal QuestionId: 0x51F, Value: 0x0 { 12 06 1F 05 00 00 }
0x3D4EB: 			OneOf Prompt: "CrashLog On All Reset", Help: "Option to invoke CrashLog collection on all reset", QuestionFlags: 0x10, QuestionId: 0x520, VarStoreId: 0xF101, VarOffset: 0x857, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 1F 8D 1F 20 05 01 F1 57 08 10 10 00 01 00 }
0x3D4FC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D503: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D50A: 			End  { 29 02 }
0x3D50C: 		End  { 29 02 }
0x3D50E: 		SuppressIf  { 0A 82 }
0x3D510: 			EqIdVal QuestionId: 0x51F, Value: 0x0 { 12 06 1F 05 00 00 }
0x3D516: 			OneOf Prompt: "CrashLog PMC Rearm", Help: "Option to invoke crashlog re-arm", QuestionFlags: 0x10, QuestionId: 0x521, VarStoreId: 0xF101, VarOffset: 0xBB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 1F 91 1F 21 05 01 F1 B8 0B 10 10 00 01 00 }
0x3D527: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D52E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3D535: 			End  { 29 02 }
0x3D537: 			OneOf Prompt: "CrashLog PMC Clear", Help: "Option to invoke CrashLog clear", QuestionFlags: 0x10, QuestionId: 0x522, VarStoreId: 0xF101, VarOffset: 0xBB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 1F 95 1F 22 05 01 F1 B7 0B 10 10 00 01 00 }
0x3D548: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D54F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3D556: 			End  { 29 02 }
0x3D558: 		End  { 29 02 }
0x3D55A: 		SuppressIf  { 0A 82 }
0x3D55C: 			EqIdVal QuestionId: 0x51F, Value: 0x0 { 12 06 1F 05 00 00 }
0x3D562: 			OneOf Prompt: "CrashLog Cdie Rearm", Help: "Option to invoke crashlog re-arm", QuestionFlags: 0x10, QuestionId: 0x523, VarStoreId: 0xF101, VarOffset: 0xBB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 1F 8F 1F 23 05 01 F1 B6 0B 10 10 00 01 00 }
0x3D573: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D57A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x3D581: 			End  { 29 02 }
0x3D583: 			OneOf Prompt: "CrashLog Cdie Clear", Help: "Option to invoke CrashLog clear", QuestionFlags: 0x10, QuestionId: 0x524, VarStoreId: 0xF101, VarOffset: 0xBB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 1F 93 1F 24 05 01 F1 B5 0B 10 10 00 01 00 }
0x3D594: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D59B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D5A2: 			End  { 29 02 }
0x3D5A4: 		End  { 29 02 }
0x3D5A6: 		SuppressIf  { 0A 82 }
0x3D5A8: 			EqIdVal QuestionId: 0x51F, Value: 0x0 { 12 06 1F 05 00 00 }
0x3D5AE: 			SuppressIf  { 0A 82 }
0x3D5B0: 				EqIdVal QuestionId: 0x11C9, Value: 0x0 { 12 86 C9 11 00 00 }
0x3D5B6: 					EqIdVal QuestionId: 0x11C8, Value: 0x670 { 12 06 C8 11 70 06 }
0x3D5BC: 					And  { 15 02 }
0x3D5BE: 				End  { 29 02 }
0x3D5C0: 				OneOf Prompt: "CrashLog GPRs", Help: "Helps collecting crash data from PMC SSRAM. Enabling this may expose personal or confidential information that may be held in the GPRs at the time of the Crash trigger", QuestionFlags: 0x10, QuestionId: 0x525, VarStoreId: 0x1, VarOffset: 0x314, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 96 1F 97 1F 25 05 01 00 14 03 10 10 00 02 00 }
0x3D5D1: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D5D8: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D5DF: 					OneOfOption Option: "Gprs Enabled, Smm Gprs Disabled" Value: 2 { 09 07 98 1F 00 00 02 }
0x3D5E6: 				End  { 29 02 }
0x3D5E8: 			End  { 29 02 }
0x3D5EA: 		End  { 29 02 }
0x3D5EC: 		OneOf Prompt: "PMC Debug Message Enable", Help: "When Enabled, PMC HW will send debug messages to trace hub; When Disabled, PMC HW will never send debug meesages to trace hub. Noted: When Enabled, may not enter S0ix", QuestionFlags: 0x10, QuestionId: 0x526, VarStoreId: 0x6, VarOffset: 0x741, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 1F 9A 1F 26 05 06 00 41 07 10 10 00 01 00 }
0x3D5FD: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x3D604: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D60B: 		End  { 29 02 }
0x3D60D: 		GrayOutIf  { 19 82 }
0x3D60F: 			EqIdVal QuestionId: 0x11C7, Value: 0x1 { 12 06 C7 11 01 00 }
0x3D615: 			OneOf Prompt: "Delayed Authentication Mode", Help: "Enable/Disable Delayed Authentication Mode", QuestionFlags: 0x14, QuestionId: 0x28B5, VarStoreId: 0x9, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 1F 9C 1F B5 28 09 00 09 00 14 10 00 01 00 }
0x3D626: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x3D62D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3D634: 			End  { 29 02 }
0x3D636: 		End  { 29 02 }
0x3D638: 	End  { 29 02 }
0x3D63A: 	Form FormId: 0x28BD, Title: "Debug Configuration" { 01 86 BD 28 9F 1F }
0x3D640: 		Subtitle Prompt: "Debug Configuration", Help: "", Flags: 0x0 { 02 87 9F 1F 00 00 00 }
0x3D647: 		End  { 29 02 }
0x3D649: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3D650: 		End  { 29 02 }
0x3D652: 		CheckBox Prompt: "RAM", Help: "Debug Messages Interface", QuestionFlags: 0x10, QuestionId: 0x527, VarStoreId: 0xE, VarOffset: 0x3, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E B1 1F A1 1F 27 05 0E 00 03 00 10 00 }
0x3D660: 		End  { 29 02 }
0x3D662: 		CheckBox Prompt: "Legacy UART", Help: "Debug Messages Interface", QuestionFlags: 0x10, QuestionId: 0x528, VarStoreId: 0xE, VarOffset: 0x4, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E B2 1F A1 1F 28 05 0E 00 04 00 10 01 }
0x3D670: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3D675: 				Value  { 5A 82 }
0x3D677: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x3D681: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3D68B: 						Equal  { 2F 02 }
0x3D68D: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3D697: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3D6A1: 						Conditional  { 50 02 }
0x3D6A3: 					End  { 29 02 }
0x3D6A5: 				End  { 29 02 }
0x3D6A7: 			End  { 29 02 }
0x3D6A9: 		End  { 29 02 }
0x3D6AB: 		CheckBox Prompt: "USB3", Help: "Debug Messages Interface", QuestionFlags: 0x10, QuestionId: 0x529, VarStoreId: 0xE, VarOffset: 0x5, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E B3 1F A1 1F 29 05 0E 00 05 00 10 00 }
0x3D6B9: 		End  { 29 02 }
0x3D6BB: 		CheckBox Prompt: "Serial IO UART", Help: "Debug Messages Interface", QuestionFlags: 0x10, QuestionId: 0x52A, VarStoreId: 0xE, VarOffset: 0x6, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E B4 1F A1 1F 2A 05 0E 00 06 00 10 01 }
0x3D6C9: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3D6CE: 				Value  { 5A 82 }
0x3D6D0: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x3D6DA: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3D6E4: 						Equal  { 2F 02 }
0x3D6E6: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3D6F0: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3D6FA: 						Conditional  { 50 02 }
0x3D6FC: 					End  { 29 02 }
0x3D6FE: 				End  { 29 02 }
0x3D700: 			End  { 29 02 }
0x3D702: 		End  { 29 02 }
0x3D704: 		CheckBox Prompt: "Trace Hub", Help: "Debug Messages Interface", QuestionFlags: 0x10, QuestionId: 0x52B, VarStoreId: 0xE, VarOffset: 0x7, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E B5 1F A1 1F 2B 05 0E 00 07 00 10 01 }
0x3D712: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3D717: 				Value  { 5A 82 }
0x3D719: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3D723: 				End  { 29 02 }
0x3D725: 			End  { 29 02 }
0x3D727: 		End  { 29 02 }
0x3D729: 		OneOf Prompt: "MRC Serial Debug Messages", Help: "Enable/Disable MRC Serial Debug Messages", QuestionFlags: 0x10, QuestionId: 0x52C, VarStoreId: 0xE, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 A4 1F A5 1F 2C 05 0E 00 00 00 10 10 00 05 00 }
0x3D73A: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3D740: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D747: 			OneOfOption Option: "Error Only" Value: 1 { 09 07 AC 1F 00 00 01 }
0x3D74E: 			OneOfOption Option: "Error & Warnings" Value: 2 { 09 07 AD 1F 00 00 02 }
0x3D755: 			OneOfOption Option: "Load, Error, Warnings & Info" Value: 3 { 09 07 AE 1F 00 00 03 }
0x3D75C: 			OneOfOption Option: "Load, Error, Warnings, Info & Event" Value: 4 { 09 07 AF 1F 00 00 04 }
0x3D763: 			OneOfOption Option: "Load, Error, Warnings, Info & Verbose" Value: 5 { 09 07 B0 1F 00 00 05 }
0x3D76A: 		End  { 29 02 }
0x3D76C: 		OneOf Prompt: "Serial Debug Messages", Help: "Enable/Disable some Platform Serial Debug Messages", QuestionFlags: 0x10, QuestionId: 0x52D, VarStoreId: 0xE, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 A2 1F A3 1F 2D 05 0E 00 01 00 10 10 00 05 00 }
0x3D77D: 			Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x3D783: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3D78A: 			OneOfOption Option: "Error Only" Value: 1 { 09 07 AC 1F 00 00 01 }
0x3D791: 			OneOfOption Option: "Error & Warnings" Value: 2 { 09 07 AD 1F 00 00 02 }
0x3D798: 			OneOfOption Option: "Load, Error, Warnings & Info" Value: 3 { 09 07 AE 1F 00 00 03 }
0x3D79F: 			OneOfOption Option: "Load, Error, Warnings, Info & Event" Value: 4 { 09 07 AF 1F 00 00 04 }
0x3D7A6: 			OneOfOption Option: "Load, Error, Warnings, Info & Verbose" Value: 5 { 09 07 B0 1F 00 00 05 }
0x3D7AD: 		End  { 29 02 }
0x3D7AF: 		OneOf Prompt: "Serial Debug Message Baud Rate", Help: "Baud Rate for Serial Debug Messages", QuestionFlags: 0x10, QuestionId: 0x52E, VarStoreId: 0xE, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x7, Step: 0x0 { 05 91 A6 1F A7 1F 2E 05 0E 00 02 00 10 10 03 07 00 }
0x3D7C0: 			OneOfOption Option: "9600" Value: 3 { 09 07 A8 1F 00 00 03 }
0x3D7C7: 			OneOfOption Option: "19200" Value: 4 { 09 07 A9 1F 00 00 04 }
0x3D7CE: 			OneOfOption Option: "57600" Value: 6 { 09 07 AA 1F 00 00 06 }
0x3D7D5: 			OneOfOption Option: "115200" Value: 7, Default, MfgDefault { 09 07 AB 1F 30 00 07 }
0x3D7DC: 		End  { 29 02 }
0x3D7DE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3D7E5: 		End  { 29 02 }
0x3D7E7: 		SuppressIf  { 0A 82 }
0x3D7E9: 			EqIdVal QuestionId: 0x52A, Value: 0x0 { 12 06 2A 05 00 00 }
0x3D7EF: 			Subtitle Prompt: "Serial IO Debug Controller Configuration", Help: "", Flags: 0x0 { 02 87 B6 1F 00 00 00 }
0x3D7F6: 			End  { 29 02 }
0x3D7F8: 			OneOf Prompt: "Controller Number", Help: "Pch Integrated UART controller number", QuestionFlags: 0x10, QuestionId: 0x52F, VarStoreId: 0xE, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D5 1F D6 1F 2F 05 0E 00 08 00 10 10 00 02 00 }
0x3D809: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x3D80F: 				OneOfOption Option: "Serial IO UART 0" Value: 0 { 09 07 D7 1F 00 00 00 }
0x3D816: 				OneOfOption Option: "Serial IO UART 1" Value: 1 { 09 07 D8 1F 00 00 01 }
0x3D81D: 				OneOfOption Option: "Serial IO UART 2" Value: 2 { 09 07 D9 1F 00 00 02 }
0x3D824: 			End  { 29 02 }
0x3D826: 			OneOf Prompt: "Baud Rate", Help: "Serial IO transmission speed in baud [Bd] per second", QuestionFlags: 0x10, QuestionId: 0x530, VarStoreId: 0xE, VarOffset: 0x9, Flags: 0x12, Size: 32, Min: 0x2580, Max: 0x5B8D80, Step: 0x0 { 05 9A B8 1F B9 1F 30 05 0E 00 09 00 10 12 80 25 00 00 80 8D 5B 00 00 00 00 00 }
0x3D840: 				OneOfOption Option: "9600" Value: 9600 { 09 0A A8 1F 02 02 80 25 00 00 }
0x3D84A: 				OneOfOption Option: "19200" Value: 19200 { 09 0A A9 1F 02 02 00 4B 00 00 }
0x3D854: 				OneOfOption Option: "57600" Value: 57600 { 09 0A AA 1F 02 02 00 E1 00 00 }
0x3D85E: 				OneOfOption Option: "115200" Value: 115200, Default, MfgDefault { 09 0A AB 1F 32 02 00 C2 01 00 }
0x3D868: 				OneOfOption Option: "460800" Value: 460800 { 09 0A BA 1F 02 02 00 08 07 00 }
0x3D872: 				OneOfOption Option: "921600" Value: 921600 { 09 0A BB 1F 02 02 00 10 0E 00 }
0x3D87C: 				OneOfOption Option: "1500000" Value: 1500000 { 09 0A BC 1F 02 02 60 E3 16 00 }
0x3D886: 				OneOfOption Option: "1843200" Value: 1843200 { 09 0A BD 1F 02 02 00 20 1C 00 }
0x3D890: 				OneOfOption Option: "3000000" Value: 3000000 { 09 0A BE 1F 02 02 C0 C6 2D 00 }
0x3D89A: 				OneOfOption Option: "3686400" Value: 3686400 { 09 0A BF 1F 02 02 00 40 38 00 }
0x3D8A4: 				OneOfOption Option: "6000000" Value: 6000000 { 09 0A C0 1F 02 02 80 8D 5B 00 }
0x3D8AE: 			End  { 29 02 }
0x3D8B0: 			OneOf Prompt: "Stop Bits", Help: "Number of stop bits. This is used to select the number of stop bits per character that the peripheral transmits and receives.", QuestionFlags: 0x10, QuestionId: 0x531, VarStoreId: 0xE, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 C1 1F C2 1F 31 05 0E 00 0D 00 10 10 00 03 00 }
0x3D8C1: 				OneOfOption Option: "Default" Value: 0 { 09 07 C3 1F 00 00 00 }
0x3D8C8: 				OneOfOption Option: "1" Value: 1, Default, MfgDefault { 09 07 C4 1F 30 00 01 }
0x3D8CF: 				OneOfOption Option: "1.5" Value: 2 { 09 07 C5 1F 00 00 02 }
0x3D8D6: 				OneOfOption Option: "2" Value: 3 { 09 07 C6 1F 00 00 03 }
0x3D8DD: 			End  { 29 02 }
0x3D8DF: 			OneOf Prompt: "Parity Bits", Help: "Enable and disable parity generation and detection in transmitted and received serial character", QuestionFlags: 0x10, QuestionId: 0x532, VarStoreId: 0xE, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 C7 1F C8 1F 32 05 0E 00 0E 00 10 10 00 03 00 }
0x3D8F0: 				OneOfOption Option: "Default" Value: 0 { 09 07 C9 1F 00 00 00 }
0x3D8F7: 				OneOfOption Option: "None" Value: 1, Default, MfgDefault { 09 07 CA 1F 30 00 01 }
0x3D8FE: 				OneOfOption Option: "Even" Value: 2 { 09 07 CB 1F 00 00 02 }
0x3D905: 				OneOfOption Option: "Odd" Value: 3 { 09 07 CC 1F 00 00 03 }
0x3D90C: 			End  { 29 02 }
0x3D90E: 			CheckBox Prompt: "Flow Control", Help: "Auto or None. Used to help for flow control using external IO pins with the pairing device.", QuestionFlags: 0x10, QuestionId: 0x533, VarStoreId: 0xE, VarOffset: 0xF, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CD 1F CE 1F 33 05 0E 00 0F 00 10 00 }
0x3D91C: 			End  { 29 02 }
0x3D91E: 			OneOf Prompt: "Word Length", Help: "Select the number of data bits per character that the peripheral transmits and receives", QuestionFlags: 0x10, QuestionId: 0x534, VarStoreId: 0xE, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x5, Max: 0x8, Step: 0x0 { 05 91 CF 1F D0 1F 34 05 0E 00 10 00 10 10 05 08 00 }
0x3D92F: 				OneOfOption Option: "5 BITS" Value: 5 { 09 07 D1 1F 00 00 05 }
0x3D936: 				OneOfOption Option: "6 BITS" Value: 6 { 09 07 D2 1F 00 00 06 }
0x3D93D: 				OneOfOption Option: "7 BITS" Value: 7 { 09 07 D3 1F 00 00 07 }
0x3D944: 				OneOfOption Option: "8 BITS" Value: 8, Default, MfgDefault { 09 07 D4 1F 30 00 08 }
0x3D94B: 			End  { 29 02 }
0x3D94D: 		End  { 29 02 }
0x3D94F: 		SuppressIf  { 0A 82 }
0x3D951: 			EqIdVal QuestionId: 0x52A, Value: 0x1 { 12 06 2A 05 01 00 }
0x3D957: 			Subtitle Prompt: "Serial IO Debug Interface Disabled", Help: "", Flags: 0x0 { 02 87 B7 1F 00 00 00 }
0x3D95E: 			End  { 29 02 }
0x3D960: 		End  { 29 02 }
0x3D962: 	End  { 29 02 }
0x3D964: 	Form FormId: 0x28C1, Title: "Trusted Computing" { 01 86 C1 28 87 22 }
0x3D96A: 		Subtitle Prompt: "Configuration", Help: "", Flags: 0x0 { 02 87 98 22 00 00 00 }
0x3D971: 		End  { 29 02 }
0x3D973: 		OneOf Prompt: "  Security Device Support", Help: "Enables or Disables BIOS support for security device. O.S. will not show Security Device. TCG EFI protocol and INT1A interface will not be available.", QuestionFlags: 0x10, QuestionId: 0x535, VarStoreId: 0xF101, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 22 AD 22 35 05 01 F1 13 00 10 10 00 01 00 }
0x3D984: 			OneOfOption Option: "Disable" Value: 0 { 09 07 93 22 00 00 00 }
0x3D98B: 			OneOfOption Option: "Enable" Value: 1, Default, MfgDefault { 09 07 92 22 30 00 01 }
0x3D992: 		End  { 29 02 }
0x3D994: 		Text Prompt: "  NO Security Device Found", Help: "", Text: "" { 03 08 AE 22 02 00 02 00 }
0x3D99C: 	End  { 29 02 }
0x3D99E: 	Form FormId: 0x28C2, Title: "Trusted Computing" { 01 86 C2 28 87 22 }
0x3D9A4: 		Subtitle Prompt: "Configuration", Help: "", Flags: 0x0 { 02 87 98 22 00 00 00 }
0x3D9AB: 		End  { 29 02 }
0x3D9AD: 		SuppressIf  { 0A 82 }
0x3D9AF: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 06 C5 11 00 00 }
0x3D9B5: 			GrayOutIf  { 19 82 }
0x3D9B7: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3D9BD: 				OneOf Prompt: "  Security Device Support", Help: "Enables or Disables BIOS support for security device. O.S. will not show Security Device. TCG EFI protocol and INT1A interface will not be available.", QuestionFlags: 0x10, QuestionId: 0x536, VarStoreId: 0xF101, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 22 AD 22 36 05 01 F1 13 00 10 10 00 01 00 }
0x3D9CE: 					OneOfOption Option: "Disable" Value: 0 { 09 07 93 22 00 00 00 }
0x3D9D5: 					OneOfOption Option: "Enable" Value: 1, Default, MfgDefault { 09 07 92 22 30 00 01 }
0x3D9DC: 				End  { 29 02 }
0x3D9DE: 			End  { 29 02 }
0x3D9E0: 		End  { 29 02 }
0x3D9E2: 		SuppressIf  { 0A 82 }
0x3D9E4: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 86 C5 11 00 00 }
0x3D9EA: 				EqIdVal QuestionId: 0x536, Value: 0x0 { 12 06 36 05 00 00 }
0x3D9F0: 				Or  { 16 02 }
0x3D9F2: 			End  { 29 02 }
0x3D9F4: 			GrayOutIf  { 19 82 }
0x3D9F6: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3D9FC: 				OneOf Prompt: "  TPM State", Help: "Enable/Disable Security Device. NOTE: Your Computer will reboot during restart in order to change State of the Device.", QuestionFlags: 0x10, QuestionId: 0x537, VarStoreId: 0xF101, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 22 8E 22 37 05 01 F1 0E 00 10 10 00 01 00 }
0x3DA0D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 95 22 00 00 00 }
0x3DA14: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 94 22 30 00 01 }
0x3DA1B: 				End  { 29 02 }
0x3DA1D: 			End  { 29 02 }
0x3DA1F: 		End  { 29 02 }
0x3DA21: 		SuppressIf  { 0A 82 }
0x3DA23: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 86 C5 11 00 00 }
0x3DA29: 				EqIdVal QuestionId: 0x536, Value: 0x0 { 12 06 36 05 00 00 }
0x3DA2F: 				Or  { 16 02 }
0x3DA31: 			End  { 29 02 }
0x3DA33: 			GrayOutIf  { 19 82 }
0x3DA35: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3DA3B: 					EqIdVal QuestionId: 0x11C6, Value: 0x1 { 12 06 C6 11 01 00 }
0x3DA41: 					Or  { 16 02 }
0x3DA43: 					EqIdVal QuestionId: 0x537, Value: 0x0 { 12 06 37 05 00 00 }
0x3DA49: 					Or  { 16 02 }
0x3DA4B: 				End  { 29 02 }
0x3DA4D: 				OneOf Prompt: "Pending operation", Help: "Schedule an Operation for the Security Device. NOTE: Your Computer will reboot during restart in order to change State of Security Device.", QuestionFlags: 0x10, QuestionId: 0x538, VarStoreId: 0xF101, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 96 22 AC 22 38 05 01 F1 0F 00 10 10 00 05 00 }
0x3DA5E: 					OneOfOption Option: "None" Value: 0, Default, MfgDefault { 09 07 91 22 30 00 00 }
0x3DA65: 					OneOfOption Option: "TPM Clear" Value: 5 { 09 07 8F 22 00 00 05 }
0x3DA6C: 				End  { 29 02 }
0x3DA6E: 			End  { 29 02 }
0x3DA70: 		End  { 29 02 }
0x3DA72: 		SuppressIf  { 0A 82 }
0x3DA74: 			EqIdVal QuestionId: 0x11C4, Value: 0x0 { 12 06 C4 11 00 00 }
0x3DA7A: 			GrayOutIf  { 19 82 }
0x3DA7C: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3DA82: 				OneOf Prompt: "  Security Device Support", Help: "Enables or Disables BIOS support for security device. O.S. will not show Security Device. TCG EFI protocol and INT1A interface will not be available.", QuestionFlags: 0x10, QuestionId: 0x539, VarStoreId: 0xF101, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 22 AD 22 39 05 01 F1 13 00 10 10 00 01 00 }
0x3DA93: 					OneOfOption Option: "Disable" Value: 0 { 09 07 93 22 00 00 00 }
0x3DA9A: 					OneOfOption Option: "Enable" Value: 1, Default, MfgDefault { 09 07 92 22 30 00 01 }
0x3DAA1: 				End  { 29 02 }
0x3DAA3: 			End  { 29 02 }
0x3DAA5: 		End  { 29 02 }
0x3DAA7: 		SuppressIf  { 0A 82 }
0x3DAA9: 			EqIdVal QuestionId: 0x11C4, Value: 0x0 { 12 86 C4 11 00 00 }
0x3DAAF: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DAB5: 				Or  { 16 02 }
0x3DAB7: 			End  { 29 02 }
0x3DAB9: 			GrayOutIf  { 19 82 }
0x3DABB: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3DAC1: 				OneOf Prompt: "  TCM State", Help: "Enable/Disable Security Device. NOTE: Your Computer will reboot during restart in order to change State of the Device.", QuestionFlags: 0x10, QuestionId: 0x53A, VarStoreId: 0xF101, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 22 8E 22 3A 05 01 F1 0E 00 10 10 00 01 00 }
0x3DAD2: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 95 22 00 00 00 }
0x3DAD9: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 94 22 30 00 01 }
0x3DAE0: 				End  { 29 02 }
0x3DAE2: 			End  { 29 02 }
0x3DAE4: 		End  { 29 02 }
0x3DAE6: 		SuppressIf  { 0A 82 }
0x3DAE8: 			EqIdVal QuestionId: 0x11C4, Value: 0x0 { 12 86 C4 11 00 00 }
0x3DAEE: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DAF4: 				Or  { 16 02 }
0x3DAF6: 			End  { 29 02 }
0x3DAF8: 			GrayOutIf  { 19 82 }
0x3DAFA: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3DB00: 					EqIdVal QuestionId: 0x11C6, Value: 0x1 { 12 06 C6 11 01 00 }
0x3DB06: 					Or  { 16 02 }
0x3DB08: 					EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 06 3A 05 00 00 }
0x3DB0E: 					Or  { 16 02 }
0x3DB10: 				End  { 29 02 }
0x3DB12: 				OneOf Prompt: "Pending operation", Help: "Schedule an Operation for the Security Device. NOTE: Your Computer will reboot during restart in order to change State of Security Device.", QuestionFlags: 0x10, QuestionId: 0x53B, VarStoreId: 0xF101, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 96 22 AC 22 3B 05 01 F1 0F 00 10 10 00 05 00 }
0x3DB23: 					OneOfOption Option: "None" Value: 0, Default, MfgDefault { 09 07 91 22 30 00 00 }
0x3DB2A: 					OneOfOption Option: "TPM Clear" Value: 5 { 09 07 8F 22 00 00 05 }
0x3DB31: 				End  { 29 02 }
0x3DB33: 			End  { 29 02 }
0x3DB35: 		End  { 29 02 }
0x3DB37: 		SuppressIf  { 0A 82 }
0x3DB39: 			EqIdVal QuestionId: 0x539, Value: 0x0 { 12 86 39 05 00 00 }
0x3DB3F: 				EqIdVal QuestionId: 0x11C4, Value: 0x1 { 12 06 C4 11 01 00 }
0x3DB45: 				Or  { 16 02 }
0x3DB47: 			End  { 29 02 }
0x3DB49: 			OneOf Prompt: "  Device Select", Help: "TPM 1.2 will restrict support to TPM 1.2 devices, TPM 2.0 will restrict support to TPM 2.0 devices, Auto will support both with the default set to TPM 2.0 devices if not found, TPM 1.2 devices will be enumerated ", QuestionFlags: 0x10, QuestionId: 0x53C, VarStoreId: 0xF101, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C4 22 C8 22 3C 05 01 F1 20 00 10 10 00 02 00 }
0x3DB5A: 				OneOfOption Option: "TPM 1.2" Value: 0 { 09 07 C5 22 00 00 00 }
0x3DB61: 				OneOfOption Option: "TPM 2.0" Value: 1 { 09 07 C6 22 00 00 01 }
0x3DB68: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 C7 22 30 00 02 }
0x3DB6F: 			End  { 29 02 }
0x3DB71: 		End  { 29 02 }
0x3DB73: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3DB7A: 		End  { 29 02 }
0x3DB7C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3DB83: 		End  { 29 02 }
0x3DB85: 		Subtitle Prompt: "Current Status Information", Help: "", Flags: 0x0 { 02 87 9A 22 00 00 00 }
0x3DB8C: 		End  { 29 02 }
0x3DB8E: 		SuppressIf  { 0A 82 }
0x3DB90: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 86 C5 11 00 00 }
0x3DB96: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DB9C: 				Or  { 16 02 }
0x3DB9E: 			End  { 29 02 }
0x3DBA0: 			GrayOutIf  { 19 82 }
0x3DBA2: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DBA8: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DBAE: 					Or  { 16 02 }
0x3DBB0: 				End  { 29 02 }
0x3DBB2: 				Text Prompt: "  Firmware Version:", Help: "", Text: "" { 03 08 DF 22 02 00 DE 22 }
0x3DBBA: 				Text Prompt: "  Vendor:", Help: "", Text: "" { 03 08 E0 22 02 00 DD 22 }
0x3DBC2: 			End  { 29 02 }
0x3DBC4: 		End  { 29 02 }
0x3DBC6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3DBCD: 		End  { 29 02 }
0x3DBCF: 		SuppressIf  { 0A 82 }
0x3DBD1: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 86 C5 11 00 00 }
0x3DBD7: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DBDD: 				Or  { 16 02 }
0x3DBDF: 			End  { 29 02 }
0x3DBE1: 			GrayOutIf  { 19 82 }
0x3DBE3: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DBE9: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DBEF: 					Or  { 16 02 }
0x3DBF1: 				End  { 29 02 }
0x3DBF3: 				Text Prompt: "  TPM Enabled Status:", Help: "None", Text: "N/A, reset required" { 03 08 9B 22 91 22 9F 22 }
0x3DBFB: 			End  { 29 02 }
0x3DBFD: 		End  { 29 02 }
0x3DBFF: 		SuppressIf  { 0A 82 }
0x3DC01: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 86 C5 11 00 00 }
0x3DC07: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DC0D: 				Or  { 16 02 }
0x3DC0F: 			End  { 29 02 }
0x3DC11: 			GrayOutIf  { 19 82 }
0x3DC13: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DC19: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DC1F: 					Or  { 16 02 }
0x3DC21: 				End  { 29 02 }
0x3DC23: 				Text Prompt: "  TPM Active Status:", Help: "None", Text: "N/A, reset required" { 03 08 9D 22 91 22 A0 22 }
0x3DC2B: 			End  { 29 02 }
0x3DC2D: 		End  { 29 02 }
0x3DC2F: 		SuppressIf  { 0A 82 }
0x3DC31: 			EqIdVal QuestionId: 0x11C5, Value: 0x0 { 12 86 C5 11 00 00 }
0x3DC37: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DC3D: 				Or  { 16 02 }
0x3DC3F: 			End  { 29 02 }
0x3DC41: 			GrayOutIf  { 19 82 }
0x3DC43: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DC49: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DC4F: 					Or  { 16 02 }
0x3DC51: 				End  { 29 02 }
0x3DC53: 				Text Prompt: "  TPM Owner Status:", Help: "None", Text: "N/A, reset required" { 03 08 A7 22 91 22 A1 22 }
0x3DC5B: 			End  { 29 02 }
0x3DC5D: 		End  { 29 02 }
0x3DC5F: 		SuppressIf  { 0A 82 }
0x3DC61: 			EqIdVal QuestionId: 0x11C4, Value: 0x0 { 12 86 C4 11 00 00 }
0x3DC67: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DC6D: 				Or  { 16 02 }
0x3DC6F: 			End  { 29 02 }
0x3DC71: 			GrayOutIf  { 19 82 }
0x3DC73: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DC79: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DC7F: 					Or  { 16 02 }
0x3DC81: 				End  { 29 02 }
0x3DC83: 				Text Prompt: "  TCM Enabled Status:", Help: "None", Text: "N/A, reset required" { 03 08 9C 22 91 22 9F 22 }
0x3DC8B: 			End  { 29 02 }
0x3DC8D: 		End  { 29 02 }
0x3DC8F: 		SuppressIf  { 0A 82 }
0x3DC91: 			EqIdVal QuestionId: 0x11C4, Value: 0x0 { 12 86 C4 11 00 00 }
0x3DC97: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DC9D: 				Or  { 16 02 }
0x3DC9F: 			End  { 29 02 }
0x3DCA1: 			GrayOutIf  { 19 82 }
0x3DCA3: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DCA9: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DCAF: 					Or  { 16 02 }
0x3DCB1: 				End  { 29 02 }
0x3DCB3: 				Text Prompt: "  TCM Active Status:", Help: "None", Text: "N/A, reset required" { 03 08 9E 22 91 22 A0 22 }
0x3DCBB: 			End  { 29 02 }
0x3DCBD: 		End  { 29 02 }
0x3DCBF: 		SuppressIf  { 0A 82 }
0x3DCC1: 			EqIdVal QuestionId: 0x11C4, Value: 0x0 { 12 86 C4 11 00 00 }
0x3DCC7: 				EqIdVal QuestionId: 0x539, Value: 0x0 { 12 06 39 05 00 00 }
0x3DCCD: 				Or  { 16 02 }
0x3DCCF: 			End  { 29 02 }
0x3DCD1: 			GrayOutIf  { 19 82 }
0x3DCD3: 				EqIdVal QuestionId: 0x53A, Value: 0x0 { 12 86 3A 05 00 00 }
0x3DCD9: 					EqIdVal QuestionId: 0x53A, Value: 0x1 { 12 06 3A 05 01 00 }
0x3DCDF: 					Or  { 16 02 }
0x3DCE1: 				End  { 29 02 }
0x3DCE3: 				Text Prompt: "  TCM Owner Status:", Help: "None", Text: "N/A, reset required" { 03 08 A8 22 91 22 A1 22 }
0x3DCEB: 			End  { 29 02 }
0x3DCED: 		End  { 29 02 }
0x3DCEF: 	End  { 29 02 }
0x3DCF1: 	Form FormId: 0x28C3, Title: "Trusted Computing" { 01 86 C3 28 87 22 }
0x3DCF7: 		Subtitle Prompt: "  TPM 2.0 Device Found", Help: "", Flags: 0x0 { 02 87 B5 22 00 00 00 }
0x3DCFE: 		End  { 29 02 }
0x3DD00: 		Text Prompt: "  Firmware Version:", Help: "", Text: "" { 03 08 DF 22 02 00 DE 22 }
0x3DD08: 		Text Prompt: "  Vendor:", Help: "", Text: "" { 03 08 E0 22 02 00 DD 22 }
0x3DD10: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3DD17: 		End  { 29 02 }
0x3DD19: 		OneOf Prompt: "  Security Device Support", Help: "Enables or Disables BIOS support for security device. O.S. will not show Security Device. TCG EFI protocol and INT1A interface will not be available.", QuestionFlags: 0x10, QuestionId: 0x53D, VarStoreId: 0xF101, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 22 AD 22 3D 05 01 F1 13 00 10 10 00 01 00 }
0x3DD2A: 			OneOfOption Option: "Disable" Value: 0 { 09 07 93 22 00 00 00 }
0x3DD31: 			OneOfOption Option: "Enable" Value: 1, Default, MfgDefault { 09 07 92 22 30 00 01 }
0x3DD38: 		End  { 29 02 }
0x3DD3A: 		SuppressIf  { 0A 82 }
0x3DD3C: 			EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 06 3D 05 00 00 }
0x3DD42: 			Text Prompt: "  Active PCR banks", Help: "", Text: "N/A, reset required" { 03 08 C9 22 CA 22 CB 22 }
0x3DD4A: 		End  { 29 02 }
0x3DD4C: 		SuppressIf  { 0A 82 }
0x3DD4E: 			EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 06 3D 05 00 00 }
0x3DD54: 			Text Prompt: "  Available PCR banks", Help: "", Text: "N/A, reset required" { 03 08 CC 22 CD 22 CE 22 }
0x3DD5C: 		End  { 29 02 }
0x3DD5E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3DD65: 		End  { 29 02 }
0x3DD67: 		GrayOutIf  { 19 82 }
0x3DD69: 			EqIdVal QuestionId: 0x548, Value: 0x1 { 12 06 48 05 01 00 }
0x3DD6F: 			SuppressIf  { 0A 82 }
0x3DD71: 				EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 86 3D 05 00 00 }
0x3DD77: 					EqIdVal QuestionId: 0x11BF, Value: 0x0 { 12 06 BF 11 00 00 }
0x3DD7D: 					Or  { 16 02 }
0x3DD7F: 				End  { 29 02 }
0x3DD81: 				OneOf Prompt: "  SHA-1 PCR Bank", Help: "Enable or Disable SHA-1 PCR Bank", QuestionFlags: 0x10, QuestionId: 0x53E, VarStoreId: 0xF101, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 22 D0 22 3E 05 01 F1 27 00 10 10 00 01 00 }
0x3DD92: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3DD98: 					Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3DD9E: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DDA5: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 A6 22 00 00 01 }
0x3DDAC: 				End  { 29 02 }
0x3DDAE: 			End  { 29 02 }
0x3DDB0: 			SuppressIf  { 0A 82 }
0x3DDB2: 				EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 86 3D 05 00 00 }
0x3DDB8: 					EqIdVal QuestionId: 0x11C3, Value: 0x0 { 12 06 C3 11 00 00 }
0x3DDBE: 					Or  { 16 02 }
0x3DDC0: 				End  { 29 02 }
0x3DDC2: 				OneOf Prompt: "  SHA256 PCR Bank", Help: "Enable or Disable SHA256 PCR Bank", QuestionFlags: 0x10, QuestionId: 0x53F, VarStoreId: 0xF101, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D1 22 D2 22 3F 05 01 F1 28 00 10 10 00 02 00 }
0x3DDD3: 					Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x3DDD9: 					Default DefaultId: 0x1 Value: 2 { 5B 06 01 00 00 02 }
0x3DDDF: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DDE6: 					OneOfOption Option: "Enabled" Value: 2 { 09 07 A6 22 00 00 02 }
0x3DDED: 				End  { 29 02 }
0x3DDEF: 			End  { 29 02 }
0x3DDF1: 			SuppressIf  { 0A 82 }
0x3DDF3: 				EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 86 3D 05 00 00 }
0x3DDF9: 					EqIdVal QuestionId: 0x11C2, Value: 0x0 { 12 06 C2 11 00 00 }
0x3DDFF: 					Or  { 16 02 }
0x3DE01: 				End  { 29 02 }
0x3DE03: 				OneOf Prompt: "  SHA384 PCR Bank", Help: "Enable or Disable SHA384 PCR Bank", QuestionFlags: 0x10, QuestionId: 0x540, VarStoreId: 0xF101, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 D3 22 D4 22 40 05 01 F1 29 00 10 10 00 04 00 }
0x3DE14: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3DE1A: 					Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3DE20: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DE27: 					OneOfOption Option: "Enabled" Value: 4 { 09 07 A6 22 00 00 04 }
0x3DE2E: 				End  { 29 02 }
0x3DE30: 			End  { 29 02 }
0x3DE32: 			SuppressIf  { 0A 82 }
0x3DE34: 				EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 86 3D 05 00 00 }
0x3DE3A: 					EqIdVal QuestionId: 0x11C1, Value: 0x0 { 12 06 C1 11 00 00 }
0x3DE40: 					Or  { 16 02 }
0x3DE42: 				End  { 29 02 }
0x3DE44: 				OneOf Prompt: "  SHA512 PCR Bank", Help: "Enable or Disable SHA512 PCR Bank", QuestionFlags: 0x10, QuestionId: 0x541, VarStoreId: 0xF101, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x8, Step: 0x0 { 05 91 D5 22 D6 22 41 05 01 F1 2A 00 10 10 00 08 00 }
0x3DE55: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3DE5B: 					Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3DE61: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DE68: 					OneOfOption Option: "Enabled" Value: 8 { 09 07 A6 22 00 00 08 }
0x3DE6F: 				End  { 29 02 }
0x3DE71: 			End  { 29 02 }
0x3DE73: 			SuppressIf  { 0A 82 }
0x3DE75: 				EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 86 3D 05 00 00 }
0x3DE7B: 					EqIdVal QuestionId: 0x11C0, Value: 0x0 { 12 06 C0 11 00 00 }
0x3DE81: 					Or  { 16 02 }
0x3DE83: 				End  { 29 02 }
0x3DE85: 				OneOf Prompt: "  SM3_256 PCR Bank", Help: "Enable or Disable SM3_256 PCR Bank", QuestionFlags: 0x10, QuestionId: 0x542, VarStoreId: 0xF101, VarOffset: 0x2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D7 22 D8 22 42 05 01 F1 2B 00 10 10 00 01 00 }
0x3DE96: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3DE9C: 					Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3DEA2: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DEA9: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 A6 22 00 00 01 }
0x3DEB0: 				End  { 29 02 }
0x3DEB2: 			End  { 29 02 }
0x3DEB4: 		End  { 29 02 }
0x3DEB6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3DEBD: 		End  { 29 02 }
0x3DEBF: 		SuppressIf  { 0A 82 }
0x3DEC1: 			EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 06 3D 05 00 00 }
0x3DEC7: 			OneOf Prompt: "  Pending operation", Help: "Schedule an Operation for the Security Device. NOTE: Your Computer will reboot during restart in order to change State of Security Device.", QuestionFlags: 0x10, QuestionId: 0x543, VarStoreId: 0xF101, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 22 AC 22 43 05 01 F1 0F 00 10 10 00 01 00 }
0x3DED8: 				OneOfOption Option: "None" Value: 0, Default, MfgDefault { 09 07 91 22 30 00 00 }
0x3DEDF: 				OneOfOption Option: "TPM Clear" Value: 1 { 09 07 8F 22 00 00 01 }
0x3DEE6: 			End  { 29 02 }
0x3DEE8: 			OneOf Prompt: "  Platform Hierarchy", Help: "Enable or Disable Platform Hierarchy", QuestionFlags: 0x10, QuestionId: 0x544, VarStoreId: 0xF101, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 22 B7 22 44 05 01 F1 1C 00 10 10 00 01 00 }
0x3DEF9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DF00: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 A6 22 30 00 01 }
0x3DF07: 			End  { 29 02 }
0x3DF09: 			OneOf Prompt: "  Storage Hierarchy", Help: "Enable or Disable Storage Hierarchy", QuestionFlags: 0x10, QuestionId: 0x545, VarStoreId: 0xF101, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 22 B9 22 45 05 01 F1 1D 00 10 10 00 01 00 }
0x3DF1A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DF21: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 A6 22 30 00 01 }
0x3DF28: 			End  { 29 02 }
0x3DF2A: 			OneOf Prompt: "  Endorsement Hierarchy", Help: "Enable or Disable Endorsement Hierarchy", QuestionFlags: 0x10, QuestionId: 0x546, VarStoreId: 0xF101, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 22 BB 22 46 05 01 F1 1E 00 10 10 00 01 00 }
0x3DF3B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 A3 22 00 00 00 }
0x3DF42: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 A6 22 30 00 01 }
0x3DF49: 			End  { 29 02 }
0x3DF4B: 			OneOf Prompt: "  Physical Presence Spec Version", Help: "  Select to Tell O.S. to support PPI Spec Version 1.2 or 1.3. Note some HCK tests might not support 1.3.", QuestionFlags: 0x10, QuestionId: 0x547, VarStoreId: 0xF101, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D9 22 DA 22 47 05 01 F1 2D 00 10 10 00 01 00 }
0x3DF5C: 				OneOfOption Option: "1.2" Value: 0 { 09 07 DB 22 00 00 00 }
0x3DF63: 				OneOfOption Option: "1.3" Value: 1, Default, MfgDefault { 09 07 DC 22 30 00 01 }
0x3DF6A: 			End  { 29 02 }
0x3DF6C: 		End  { 29 02 }
0x3DF6E: 		SuppressIf  { 0A 82 }
0x3DF70: 			EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 86 3D 05 00 00 }
0x3DF76: 				EqIdVal QuestionId: 0x11BF, Value: 0x0 { 12 06 BF 11 00 00 }
0x3DF7C: 				Or  { 16 02 }
0x3DF7E: 			End  { 29 02 }
0x3DF80: 			OneOf Prompt: "  TPM 2.0 UEFI Spec Version", Help: "Select the TCG2 Spec Version Support,


TCG_1_2: the Compatible mode for Win8/Win10,


TCG_2: Support new TCG2 protocol and event format for Win10 or later", QuestionFlags: 0x10, QuestionId: 0x548, VarStoreId: 0xF101, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 05 91 B1 22 B2 22 48 05 01 F1 1B 00 10 10 01 02 00 }
0x3DF91: 				OneOfOption Option: "TCG_1_2" Value: 1 { 09 07 B3 22 00 00 01 }
0x3DF98: 				OneOfOption Option: "TCG_2" Value: 2, Default, MfgDefault { 09 07 B4 22 30 00 02 }
0x3DF9F: 			End  { 29 02 }
0x3DFA1: 		End  { 29 02 }
0x3DFA3: 		SuppressIf  { 0A 82 }
0x3DFA5: 			EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 06 3D 05 00 00 }
0x3DFAB: 			GrayOutIf  { 19 82 }
0x3DFAD: 				True  { 46 02 }
0x3DFAF: 				OneOf Prompt: "  TPM 2.0 InterfaceType", Help: "  Select the Communication Interface to TPM 20 Device.", QuestionFlags: 0x10, QuestionId: 0x549, VarStoreId: 0xF101, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 22 BD 22 49 05 01 F1 1F 00 10 10 00 01 00 }
0x3DFC0: 					OneOfOption Option: "CRB" Value: 0, Default, MfgDefault { 09 07 C2 22 30 00 00 }
0x3DFC7: 					OneOfOption Option: "TIS" Value: 1 { 09 07 C3 22 00 00 01 }
0x3DFCE: 				End  { 29 02 }
0x3DFD0: 			End  { 29 02 }
0x3DFD2: 		End  { 29 02 }
0x3DFD4: 		SuppressIf  { 0A 82 }
0x3DFD6: 			EqIdVal QuestionId: 0x53D, Value: 0x0 { 12 06 3D 05 00 00 }
0x3DFDC: 			OneOf Prompt: "  Device Select", Help: "TPM 1.2 will restrict support to TPM 1.2 devices, TPM 2.0 will restrict support to TPM 2.0 devices, Auto will support both with the default set to TPM 2.0 devices if not found, TPM 1.2 devices will be enumerated ", QuestionFlags: 0x10, QuestionId: 0x54A, VarStoreId: 0xF101, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C4 22 C8 22 4A 05 01 F1 20 00 10 10 00 02 00 }
0x3DFED: 				OneOfOption Option: "TPM 1.2" Value: 0 { 09 07 C5 22 00 00 00 }
0x3DFF4: 				OneOfOption Option: "TPM 2.0" Value: 1 { 09 07 C6 22 00 00 01 }
0x3DFFB: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 C7 22 30 00 02 }
0x3E002: 			End  { 29 02 }
0x3E004: 		End  { 29 02 }
0x3E006: 	End  { 29 02 }
0x3E008: 	Form FormId: 0x28C4, Title: "ACPI Settings" { 01 86 C4 28 1E 20 }
0x3E00E: 		Subtitle Prompt: "ACPI Settings", Help: "", Flags: 0x0 { 02 87 1E 20 00 00 00 }
0x3E015: 		End  { 29 02 }
0x3E017: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E01E: 		End  { 29 02 }
0x3E020: 		GrayOutIf  { 19 82 }
0x3E022: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3E028: 			CheckBox Prompt: "Enable ACPI Auto Configuration", Help: "Enables or Disables BIOS ACPI Auto Configuration.", QuestionFlags: 0x0, QuestionId: 0x54B, VarStoreId: 0xF101, VarOffset: 0xBCD, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 4A 01 4B 01 4B 05 01 F1 CD 0B 00 00 }
0x3E036: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3E03C: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E042: 			End  { 29 02 }
0x3E044: 		End  { 29 02 }
0x3E046: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E04D: 		End  { 29 02 }
0x3E04F: 		SuppressIf  { 0A 82 }
0x3E051: 			EqIdVal QuestionId: 0x54B, Value: 0x1 { 12 06 4B 05 01 00 }
0x3E057: 			GrayOutIf  { 19 82 }
0x3E059: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3E05F: 				CheckBox Prompt: "Enable Hibernation", Help: "Enables or Disables System ability to Hibernate (OS/S4 Sleep State). This option may not be effective with some operating systems.", QuestionFlags: 0x0, QuestionId: 0x54C, VarStoreId: 0xF101, VarOffset: 0xBD0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 48 01 49 01 4C 05 01 F1 D0 0B 00 00 }
0x3E06D: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E073: 					Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E079: 				End  { 29 02 }
0x3E07B: 				OneOf Prompt: "ACPI Sleep State", Help: "Select the highest ACPI sleep state the system will enter when the SUSPEND button is pressed.", QuestionFlags: 0x10, QuestionId: 0x54D, VarStoreId: 0xF101, VarOffset: 0xBCE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x2, Step: 0x0 { 05 94 1F 20 20 20 4D 05 01 F1 CE 0B 10 11 00 00 02 00 00 00 }
0x3E08F: 					OneOfOption Option: "Suspend Disabled" Value: 0 { 09 08 23 20 01 01 00 00 }
0x3E097: 					OneOfOption Option: "S3 (Suspend to RAM)" Value: 2 { 09 08 22 20 01 01 02 00 }
0x3E09F: 					Default DefaultId: 0x0 Value: 2 { 5B 07 00 00 01 02 00 }
0x3E0A6: 					Default DefaultId: 0x1 Value: 2 { 5B 07 01 00 01 02 00 }
0x3E0AD: 				End  { 29 02 }
0x3E0AF: 			End  { 29 02 }
0x3E0B1: 		End  { 29 02 }
0x3E0B3: 	End  { 29 02 }
0x3E0B5: 	Form FormId: 0x28E2, Title: "Demo Board" { 01 86 E2 28 07 23 }
0x3E0BB: 		CheckBox Prompt: "CRB Test", Help: "Help for CRB Test", QuestionFlags: 0x10, QuestionId: 0x54E, VarStoreId: 0xF101, VarOffset: 0xC5F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 09 23 0A 23 4E 05 01 F1 5F 0C 10 00 }
0x3E0C9: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3E0CF: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E0D5: 		End  { 29 02 }
0x3E0D7: 	End  { 29 02 }
0x3E0D9: 	Form FormId: 0x28E3, Title: "SMART Settings" { 01 86 E3 28 EA 21 }
0x3E0DF: 		Subtitle Prompt: "SMART Settings", Help: "", Flags: 0x0 { 02 87 EA 21 00 00 00 }
0x3E0E6: 		End  { 29 02 }
0x3E0E8: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E0EF: 		End  { 29 02 }
0x3E0F1: 		GrayOutIf  { 19 82 }
0x3E0F3: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3E0F9: 			CheckBox Prompt: "SMART Self Test", Help: "Run SMART Self Test on all HDDs during POST.", QuestionFlags: 0x10, QuestionId: 0x54F, VarStoreId: 0xF101, VarOffset: 0xC60, Flags: 0x2, Default: Disabled, MfgDefault: Enabled { 06 8E EC 21 ED 21 4F 05 01 F1 60 0C 10 02 }
0x3E107: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E10C: 					Value  { 5A 82 }
0x3E10E: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E118: 					End  { 29 02 }
0x3E11A: 				End  { 29 02 }
0x3E11C: 			End  { 29 02 }
0x3E11E: 		End  { 29 02 }
0x3E120: 	End  { 29 02 }
0x3E122: 	Form FormId: 0x28E4, Title: "UEFI Variables Protection" { 01 86 E4 28 F0 1F }
0x3E128: 		OneOf Prompt: "Password protection of Runtime Variables", Help: "Control the NVRAM Runtime Variable protection through System Admin Password", QuestionFlags: 0x10, QuestionId: 0x550, VarStoreId: 0xF101, VarOffset: 0xC61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F4 1F F5 1F 50 05 01 F1 61 0C 10 10 00 01 00 }
0x3E139: 			OneOfOption Option: "Enable" Value: 1 { 09 07 F2 1F 00 00 01 }
0x3E140: 			OneOfOption Option: "Disable" Value: 0 { 09 07 F3 1F 00 00 00 }
0x3E147: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E14D: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E153: 		End  { 29 02 }
0x3E155: 	End  { 29 02 }
0x3E157: 	Form FormId: 0x28E5, Title: "Serial Port Console Redirection" { 01 86 E5 28 60 20 }
0x3E15D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E164: 		End  { 29 02 }
0x3E166: 		Subtitle Prompt: "COM0", Help: "", Flags: 0x0 { 02 87 78 20 00 00 00 }
0x3E16D: 		End  { 29 02 }
0x3E16F: 		SuppressIf  { 0A 82 }
0x3E171: 			EqIdVal QuestionId: 0x11BE, Value: 0x1 { 12 06 BE 11 01 00 }
0x3E177: 			Text Prompt: "Console Redirection", Help: "", Text: "Port Is Disabled" { 03 08 63 20 5F 20 76 20 }
0x3E17F: 		End  { 29 02 }
0x3E181: 		SuppressIf  { 0A 82 }
0x3E183: 			EqIdVal QuestionId: 0x11BE, Value: 0x0 { 12 06 BE 11 00 00 }
0x3E189: 			CheckBox Prompt: "Console Redirection", Help: "Console Redirection Enable or Disable.", QuestionFlags: 0x10, QuestionId: 0x551, VarStoreId: 0xF101, VarOffset: 0xC6C, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 64 20 74 20 51 05 01 F1 6C 0C 10 00 }
0x3E197: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E19C: 					Value  { 5A 82 }
0x3E19E: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E1A8: 					End  { 29 02 }
0x3E1AA: 				End  { 29 02 }
0x3E1AC: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E1B2: 			End  { 29 02 }
0x3E1B4: 		End  { 29 02 }
0x3E1B6: 		SuppressIf  { 0A 82 }
0x3E1B8: 			EqIdVal QuestionId: 0x11BE, Value: 0x0 { 12 06 BE 11 00 00 }
0x3E1BE: 			GrayOutIf  { 19 82 }
0x3E1C0: 				EqIdVal QuestionId: 0x551, Value: 0x0 { 12 06 51 05 00 00 }
0x3E1C6: 				Ref Prompt: "Console Redirection Settings", Help: "The settings specify how the host computer and the remote computer (which the user is using) will exchange data. Both computers should have the same or compatible settings.", QuestionFlags: 0x0, QuestionId: 0x552, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28E8 { 0F 0F 61 20 62 20 52 05 00 00 FF FF 00 E8 28 }
0x3E1D5: 			End  { 29 02 }
0x3E1D7: 		End  { 29 02 }
0x3E1D9: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E1E0: 		End  { 29 02 }
0x3E1E2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 82 20 00 00 00 }
0x3E1E9: 		End  { 29 02 }
0x3E1EB: 		SuppressIf  { 0A 82 }
0x3E1ED: 			EqIdVal QuestionId: 0x11BD, Value: 0x1 { 12 06 BD 11 01 00 }
0x3E1F3: 			Text Prompt: "Console Redirection", Help: "", Text: "Port Is Disabled" { 03 08 63 20 5F 20 76 20 }
0x3E1FB: 		End  { 29 02 }
0x3E1FD: 		SuppressIf  { 0A 82 }
0x3E1FF: 			EqIdVal QuestionId: 0x11BD, Value: 0x0 { 12 06 BD 11 00 00 }
0x3E205: 			CheckBox Prompt: "Console Redirection", Help: "Console Redirection Enable or Disable.", QuestionFlags: 0x10, QuestionId: 0x553, VarStoreId: 0xF101, VarOffset: 0xC6D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 65 20 74 20 53 05 01 F1 6D 0C 10 00 }
0x3E213: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E218: 					Value  { 5A 82 }
0x3E21A: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E224: 					End  { 29 02 }
0x3E226: 				End  { 29 02 }
0x3E228: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E22E: 			End  { 29 02 }
0x3E230: 		End  { 29 02 }
0x3E232: 		SuppressIf  { 0A 82 }
0x3E234: 			EqIdVal QuestionId: 0x11BD, Value: 0x0 { 12 06 BD 11 00 00 }
0x3E23A: 			GrayOutIf  { 19 82 }
0x3E23C: 				EqIdVal QuestionId: 0x553, Value: 0x0 { 12 06 53 05 00 00 }
0x3E242: 				Ref Prompt: "Console Redirection Settings", Help: "The settings specify how the host computer and the remote computer (which the user is using) will exchange data. Both computers should have the same or compatible settings.", QuestionFlags: 0x0, QuestionId: 0x554, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F2 { 0F 0F 61 20 62 20 54 05 00 00 FF FF 00 F2 28 }
0x3E251: 			End  { 29 02 }
0x3E253: 		End  { 29 02 }
0x3E255: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E25C: 		End  { 29 02 }
0x3E25E: 		Subtitle Prompt: "Legacy Console Redirection", Help: "", Flags: 0x0 { 02 87 45 21 00 00 00 }
0x3E265: 		End  { 29 02 }
0x3E267: 		Ref Prompt: "Legacy Console Redirection Settings", Help: "Legacy Console Redirection Settings", QuestionFlags: 0x0, QuestionId: 0x555, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28E7 { 0F 0F 46 21 46 21 55 05 00 00 FF FF 00 E7 28 }
0x3E276: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E27D: 		End  { 29 02 }
0x3E27F: 		Subtitle Prompt: "Serial Port for Out-of-Band Management/", Help: "", Flags: 0x0 { 02 87 F1 20 00 00 00 }
0x3E286: 		End  { 29 02 }
0x3E288: 		Subtitle Prompt: "Windows Emergency Management Services (EMS)", Help: "", Flags: 0x0 { 02 87 F3 20 00 00 00 }
0x3E28F: 		End  { 29 02 }
0x3E291: 		CheckBox Prompt: "Console Redirection EMS", Help: "Console Redirection Enable or Disable.", QuestionFlags: 0x10, QuestionId: 0x556, VarStoreId: 0xF101, VarOffset: 0xC7A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 73 20 74 20 56 05 01 F1 7A 0C 10 00 }
0x3E29F: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3E2A5: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E2AB: 		End  { 29 02 }
0x3E2AD: 		GrayOutIf  { 19 82 }
0x3E2AF: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E2B5: 			Ref Prompt: "Console Redirection Settings", Help: "The settings specify how the host computer and the remote computer (which the user is using) will exchange data. Both computers should have the same or compatible settings.", QuestionFlags: 0x0, QuestionId: 0x557, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28E6 { 0F 0F 61 20 62 20 57 05 00 00 FF FF 00 E6 28 }
0x3E2C4: 		End  { 29 02 }
0x3E2C6: 	End  { 29 02 }
0x3E2C8: 	Form FormId: 0x28E6, Title: "Console Redirection Settings" { 01 86 E6 28 61 20 }
0x3E2CE: 		OneOf Prompt: "Out-of-Band Mgmt Port", Help: "Microsoft Windows Emergency Management Services (EMS) allows for remote management of a Windows Server OS through a serial port.", QuestionFlags: 0x10, QuestionId: 0x558, VarStoreId: 0xF101, VarOffset: 0xC7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F4 20 F5 20 58 05 01 F1 7B 0C 10 10 00 01 00 }
0x3E2DF: 			OneOfOption Option: "COM0" Value: 0, Default, MfgDefault { 09 07 78 20 30 00 00 }
0x3E2E6: 			OneOfOption Option: "" Value: 1 { 09 07 82 20 00 00 01 }
0x3E2ED: 		End  { 29 02 }
0x3E2EF: 		GrayOutIf  { 19 82 }
0x3E2F1: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E2F7: 			OneOf Prompt: "Terminal Type EMS", Help: "VT-UTF8 is the preferred terminal type for out-of-band management. The next best choice is VT100+ and then VT100. See above, in Console Redirection Settings page, for more Help with Terminal Type/Emulation.", QuestionFlags: 0x10, QuestionId: 0x559, VarStoreId: 0xF101, VarOffset: 0xC7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 86 20 F6 20 59 05 01 F1 7C 0C 10 10 00 03 00 }
0x3E308: 				OneOfOption Option: "VT100" Value: 0 { 09 07 96 20 00 00 00 }
0x3E30F: 				OneOfOption Option: "VT100Plus" Value: 1 { 09 07 97 20 00 00 01 }
0x3E316: 				OneOfOption Option: "VT-UTF8" Value: 2 { 09 07 98 20 00 00 02 }
0x3E31D: 				OneOfOption Option: "ANSI" Value: 3 { 09 07 99 20 00 00 03 }
0x3E324: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E329: 					Value  { 5A 82 }
0x3E32B: 						Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x3E335: 					End  { 29 02 }
0x3E337: 				End  { 29 02 }
0x3E339: 				Default DefaultId: 0x1 Value: 2 { 5B 06 01 00 00 02 }
0x3E33F: 			End  { 29 02 }
0x3E341: 		End  { 29 02 }
0x3E343: 		GrayOutIf  { 19 82 }
0x3E345: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E34B: 			OneOf Prompt: "Bits per second EMS", Help: "Selects serial port transmission speed. The speed must be matched on the other side. Long or noisy lines may require lower speeds.", QuestionFlags: 0x10, QuestionId: 0x55A, VarStoreId: 0xF101, VarOffset: 0xC7D, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x7, Step: 0x0 { 05 91 9A 20 A9 20 5A 05 01 F1 7D 0C 10 10 03 07 00 }
0x3E35C: 				OneOfOption Option: "9600" Value: 3 { 09 07 A8 1F 00 00 03 }
0x3E363: 				OneOfOption Option: "19200" Value: 4 { 09 07 A9 1F 00 00 04 }
0x3E36A: 				OneOfOption Option: "57600" Value: 6 { 09 07 AA 1F 00 00 06 }
0x3E371: 				OneOfOption Option: "115200" Value: 7 { 09 07 AB 1F 00 00 07 }
0x3E378: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E37D: 					Value  { 5A 82 }
0x3E37F: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x3E389: 					End  { 29 02 }
0x3E38B: 				End  { 29 02 }
0x3E38D: 				Default DefaultId: 0x1 Value: 7 { 5B 06 01 00 00 07 }
0x3E393: 			End  { 29 02 }
0x3E395: 		End  { 29 02 }
0x3E397: 		GrayOutIf  { 19 82 }
0x3E399: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E39F: 			OneOf Prompt: "Flow Control EMS", Help: "Flow control can prevent data loss from buffer overflow. When sending data, if the receiving buffers are full, a 'stop' signal can be sent to stop the data flow. Once the buffers are empty, a 'start' signal can be sent to re-start the flow. Hardware flow control uses two wires to send start/stop signals.", QuestionFlags: 0x10, QuestionId: 0x55B, VarStoreId: 0xF101, VarOffset: 0xC7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DF 20 EE 20 5B 05 01 F1 7E 0C 10 10 00 02 00 }
0x3E3B0: 				OneOfOption Option: "None" Value: 0 { 09 07 05 00 00 00 00 }
0x3E3B7: 				OneOfOption Option: "Hardware RTS/CTS" Value: 1 { 09 07 EF 20 00 00 01 }
0x3E3BE: 				OneOfOption Option: "Software Xon/Xoff" Value: 2 { 09 07 F0 20 00 00 02 }
0x3E3C5: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E3CA: 					Value  { 5A 82 }
0x3E3CC: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E3D6: 					End  { 29 02 }
0x3E3D8: 				End  { 29 02 }
0x3E3DA: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E3E0: 			End  { 29 02 }
0x3E3E2: 		End  { 29 02 }
0x3E3E4: 		GrayOutIf  { 19 82 }
0x3E3E6: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E3EC: 			Text Prompt: "Data Bits EMS", Help: "Data Bits", Text: "8" { 03 08 AB 20 BA 20 AD 04 }
0x3E3F4: 		End  { 29 02 }
0x3E3F6: 		GrayOutIf  { 19 82 }
0x3E3F8: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E3FE: 			Text Prompt: "Parity EMS", Help: "A parity bit can be sent with the data bits to detect some transmission errors. Even: parity bit is 0 if the num of 1's in the data bits is even. Odd: parity bit is 0 if num of 1's in the data bits is odd.  Mark: parity bit is always 1. Space: Parity bit is always 0. Mark and Space Parity do not allow for error detection. They can be used as an additional data bit.", Text: "None" { 03 08 BB 20 CA 20 05 00 }
0x3E406: 		End  { 29 02 }
0x3E408: 		GrayOutIf  { 19 82 }
0x3E40A: 			EqIdVal QuestionId: 0x556, Value: 0x0 { 12 06 56 05 00 00 }
0x3E410: 			Text Prompt: "Stop Bits EMS", Help: "Stop bits indicate the end of a serial data packet. (A start bit indicates the beginning). The standard setting is 1 stop bit. Communication with slow devices may require more than 1 stop bit.", Text: "1" { 03 08 CF 20 DE 20 A6 04 }
0x3E418: 		End  { 29 02 }
0x3E41A: 	End  { 29 02 }
0x3E41C: 	Form FormId: 0x28E7, Title: "Legacy Console Redirection Settings" { 01 86 E7 28 46 21 }
0x3E422: 		Subtitle Prompt: "Legacy Console Redirection Settings", Help: "", Flags: 0x0 { 02 87 46 21 00 00 00 }
0x3E429: 		End  { 29 02 }
0x3E42B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E432: 		End  { 29 02 }
0x3E434: 		OneOf Prompt: "Redirection COM Port", Help: "Select a COM port to display redirection of Legacy OS and Legacy OPROM Messages", QuestionFlags: 0x10, QuestionId: 0x55C, VarStoreId: 0xF101, VarOffset: 0xC82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 47 21 48 21 5C 05 01 F1 82 0C 10 10 00 01 00 }
0x3E445: 			OneOfOption Option: "COM0" Value: 0, Default, MfgDefault { 09 07 78 20 30 00 00 }
0x3E44C: 			OneOfOption Option: "" Value: 1 { 09 07 82 20 00 00 01 }
0x3E453: 		End  { 29 02 }
0x3E455: 		OneOf Prompt: "Resolution", Help: "On Legacy OS, the Number of Rows and Columns supported redirection", QuestionFlags: 0x10, QuestionId: 0x55D, VarStoreId: 0xF101, VarOffset: 0xC76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 06 21 07 21 5D 05 01 F1 76 0C 10 10 00 01 00 }
0x3E466: 			OneOfOption Option: "80x24" Value: 0 { 09 07 08 21 00 00 00 }
0x3E46D: 			OneOfOption Option: "80x25" Value: 1 { 09 07 09 21 00 00 01 }
0x3E474: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3E47A: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E480: 		End  { 29 02 }
0x3E482: 		OneOf Prompt: "Redirect After POST", Help: "When Bootloader is selected, then Legacy Console Redirection is disabled before booting to legacy OS. When Always Enable is selected, then Legacy Console Redirection is enabled for legacy OS. Default setting for this option is set to Always Enable.", QuestionFlags: 0x10, QuestionId: 0x55E, VarStoreId: 0xF101, VarOffset: 0xC79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 41 21 42 21 5E 05 01 F1 79 0C 10 10 00 01 00 }
0x3E493: 			OneOfOption Option: "Always Enable" Value: 0 { 09 07 43 21 00 00 00 }
0x3E49A: 			OneOfOption Option: "BootLoader" Value: 1 { 09 07 44 21 00 00 01 }
0x3E4A1: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E4A6: 				Value  { 5A 82 }
0x3E4A8: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E4B2: 				End  { 29 02 }
0x3E4B4: 			End  { 29 02 }
0x3E4B6: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E4BC: 		End  { 29 02 }
0x3E4BE: 	End  { 29 02 }
0x3E4C0: 	Form FormId: 0x28E8, Title: "COM0" { 01 86 E8 28 78 20 }
0x3E4C6: 		Subtitle Prompt: "COM0", Help: "", Flags: 0x0 { 02 87 78 20 00 00 00 }
0x3E4CD: 		End  { 29 02 }
0x3E4CF: 		Subtitle Prompt: "Console Redirection Settings", Help: "", Flags: 0x0 { 02 87 61 20 00 00 00 }
0x3E4D6: 		End  { 29 02 }
0x3E4D8: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E4DF: 		End  { 29 02 }
0x3E4E1: 		OneOf Prompt: "Terminal Type", Help: "Emulation: ANSI: Extended ASCII char set. VT100: ASCII char set. VT100Plus: Extends VT100 to support color, function keys, etc. VT-UTF8: Uses UTF8 encoding to map Unicode chars onto 1 or more bytes.", QuestionFlags: 0x10, QuestionId: 0x55F, VarStoreId: 0xF101, VarOffset: 0xC6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 87 20 95 20 5F 05 01 F1 6E 0C 10 10 00 03 00 }
0x3E4F2: 			OneOfOption Option: "VT100" Value: 0 { 09 07 96 20 00 00 00 }
0x3E4F9: 			OneOfOption Option: "VT100Plus" Value: 1 { 09 07 97 20 00 00 01 }
0x3E500: 			OneOfOption Option: "VT-UTF8" Value: 2 { 09 07 98 20 00 00 02 }
0x3E507: 			OneOfOption Option: "ANSI" Value: 3 { 09 07 99 20 00 00 03 }
0x3E50E: 			Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x3E514: 			Default DefaultId: 0x1 Value: 3 { 5B 06 01 00 00 03 }
0x3E51A: 		End  { 29 02 }
0x3E51C: 		OneOf Prompt: "Bits per second", Help: "Selects serial port transmission speed. The speed must be matched on the other side. Long or noisy lines may require lower speeds.", QuestionFlags: 0x10, QuestionId: 0x560, VarStoreId: 0xF101, VarOffset: 0xC62, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x7, Step: 0x0 { 05 91 9B 20 A9 20 60 05 01 F1 62 0C 10 10 03 07 00 }
0x3E52D: 			OneOfOption Option: "9600" Value: 3 { 09 07 A8 1F 00 00 03 }
0x3E534: 			OneOfOption Option: "19200" Value: 4 { 09 07 A9 1F 00 00 04 }
0x3E53B: 			OneOfOption Option: "38400" Value: 5 { 09 07 AA 20 00 00 05 }
0x3E542: 			OneOfOption Option: "57600" Value: 6 { 09 07 AA 1F 00 00 06 }
0x3E549: 			OneOfOption Option: "115200" Value: 7 { 09 07 AB 1F 00 00 07 }
0x3E550: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x3E556: 			Default DefaultId: 0x1 Value: 7 { 5B 06 01 00 00 07 }
0x3E55C: 		End  { 29 02 }
0x3E55E: 		OneOf Prompt: "Data Bits", Help: "Data Bits", QuestionFlags: 0x10, QuestionId: 0x561, VarStoreId: 0xF101, VarOffset: 0xC64, Flags: 0x10, Size: 8, Min: 0x7, Max: 0x8, Step: 0x0 { 05 91 AC 20 BA 20 61 05 01 F1 64 0C 10 10 07 08 00 }
0x3E56F: 			OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x3E576: 			OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x3E57D: 			Default DefaultId: 0x0 Value: 8 { 5B 06 00 00 00 08 }
0x3E583: 			Default DefaultId: 0x1 Value: 8 { 5B 06 01 00 00 08 }
0x3E589: 		End  { 29 02 }
0x3E58B: 		OneOf Prompt: "Parity", Help: "A parity bit can be sent with the data bits to detect some transmission errors. Even: parity bit is 0 if the num of 1's in the data bits is even. Odd: parity bit is 0 if num of 1's in the data bits is odd.  Mark: parity bit is always 1. Space: Parity bit is always 0. Mark and Space Parity do not allow for error detection. They can be used as an additional data bit.", QuestionFlags: 0x10, QuestionId: 0x562, VarStoreId: 0xF101, VarOffset: 0xC66, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x5, Step: 0x0 { 05 91 BC 20 CA 20 62 05 01 F1 66 0C 10 10 01 05 00 }
0x3E59C: 			OneOfOption Option: "None" Value: 1 { 09 07 05 00 00 00 01 }
0x3E5A3: 			OneOfOption Option: "Even" Value: 2 { 09 07 CC 20 00 00 02 }
0x3E5AA: 			OneOfOption Option: "Odd" Value: 3 { 09 07 CB 20 00 00 03 }
0x3E5B1: 			OneOfOption Option: "Mark" Value: 4 { 09 07 CD 20 00 00 04 }
0x3E5B8: 			OneOfOption Option: "Space" Value: 5 { 09 07 CE 20 00 00 05 }
0x3E5BF: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E5C5: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E5CB: 		End  { 29 02 }
0x3E5CD: 		OneOf Prompt: "Stop Bits", Help: "Stop bits indicate the end of a serial data packet. (A start bit indicates the beginning). The standard setting is 1 stop bit. Communication with slow devices may require more than 1 stop bit.", QuestionFlags: 0x10, QuestionId: 0x563, VarStoreId: 0xF101, VarOffset: 0xC68, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0 { 05 91 D0 20 DE 20 63 05 01 F1 68 0C 10 10 01 03 00 }
0x3E5DE: 			OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x3E5E5: 			OneOfOption Option: "2" Value: 3 { 09 07 A7 04 00 00 03 }
0x3E5EC: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E5F2: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E5F8: 		End  { 29 02 }
0x3E5FA: 		OneOf Prompt: "Flow Control", Help: "Flow control can prevent data loss from buffer overflow. When sending data, if the receiving buffers are full, a 'stop' signal can be sent to stop the data flow. Once the buffers are empty, a 'start' signal can be sent to re-start the flow. Hardware flow control uses two wires to send start/stop signals.", QuestionFlags: 0x10, QuestionId: 0x564, VarStoreId: 0xF101, VarOffset: 0xC6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 20 EE 20 64 05 01 F1 6A 0C 10 10 00 01 00 }
0x3E60B: 			OneOfOption Option: "None" Value: 0 { 09 07 05 00 00 00 00 }
0x3E612: 			OneOfOption Option: "Hardware RTS/CTS" Value: 1 { 09 07 EF 20 00 00 01 }
0x3E619: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3E61F: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E625: 		End  { 29 02 }
0x3E627: 		CheckBox Prompt: "VT-UTF8 Combo Key Support", Help: "Enable VT-UTF8 Combination Key Support for ANSI/VT100 terminals", QuestionFlags: 0x10, QuestionId: 0x565, VarStoreId: 0xF101, VarOffset: 0xC70, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 0A 21 18 21 65 05 01 F1 70 0C 10 00 }
0x3E635: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E63A: 				Value  { 5A 82 }
0x3E63C: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3E646: 				End  { 29 02 }
0x3E648: 			End  { 29 02 }
0x3E64A: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E650: 		End  { 29 02 }
0x3E652: 		CheckBox Prompt: "Recorder Mode", Help: "With this mode enabled only text will be sent. This is to capture Terminal data.", QuestionFlags: 0x10, QuestionId: 0x566, VarStoreId: 0xF101, VarOffset: 0xC72, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 19 21 27 21 66 05 01 F1 72 0C 10 00 }
0x3E660: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E665: 				Value  { 5A 82 }
0x3E667: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E671: 				End  { 29 02 }
0x3E673: 			End  { 29 02 }
0x3E675: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E67B: 		End  { 29 02 }
0x3E67D: 		CheckBox Prompt: "Resolution 100x31", Help: "Enables or disables extended terminal resolution", QuestionFlags: 0x10, QuestionId: 0x567, VarStoreId: 0xF101, VarOffset: 0xC74, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E F7 20 05 21 67 05 01 F1 74 0C 10 00 }
0x3E68B: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E690: 				Value  { 5A 82 }
0x3E692: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E69C: 				End  { 29 02 }
0x3E69E: 			End  { 29 02 }
0x3E6A0: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E6A6: 		End  { 29 02 }
0x3E6A8: 		OneOf Prompt: "Putty KeyPad", Help: "Select FunctionKey and KeyPad on Putty.", QuestionFlags: 0x10, QuestionId: 0x568, VarStoreId: 0xF101, VarOffset: 0xC77, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x20, Step: 0x0 { 05 91 2B 21 39 21 68 05 01 F1 77 0C 10 10 01 20 00 }
0x3E6B9: 			OneOfOption Option: "VT100" Value: 1 { 09 07 96 20 00 00 01 }
0x3E6C0: 			OneOfOption Option: "LINUX" Value: 2 { 09 07 3A 21 00 00 02 }
0x3E6C7: 			OneOfOption Option: "XTERMR6" Value: 4 { 09 07 3B 21 00 00 04 }
0x3E6CE: 			OneOfOption Option: "SCO" Value: 8 { 09 07 3C 21 00 00 08 }
0x3E6D5: 			OneOfOption Option: "ESCN" Value: 16 { 09 07 3D 21 00 00 10 }
0x3E6DC: 			OneOfOption Option: "VT400" Value: 32 { 09 07 3E 21 00 00 20 }
0x3E6E3: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E6E9: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E6EF: 		End  { 29 02 }
0x3E6F1: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E6F8: 		End  { 29 02 }
0x3E6FA: 	End  { 29 02 }
0x3E6FC: 	Form FormId: 0x28F2, Title: "" { 01 86 F2 28 82 20 }
0x3E702: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 82 20 00 00 00 }
0x3E709: 		End  { 29 02 }
0x3E70B: 		Subtitle Prompt: "Console Redirection Settings", Help: "", Flags: 0x0 { 02 87 61 20 00 00 00 }
0x3E712: 		End  { 29 02 }
0x3E714: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E71B: 		End  { 29 02 }
0x3E71D: 		OneOf Prompt: "Terminal Type", Help: "Emulation: ANSI: Extended ASCII char set. VT100: ASCII char set. VT100Plus: Extends VT100 to support color, function keys, etc. VT-UTF8: Uses UTF8 encoding to map Unicode chars onto 1 or more bytes.", QuestionFlags: 0x10, QuestionId: 0x569, VarStoreId: 0xF101, VarOffset: 0xC6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 88 20 95 20 69 05 01 F1 6F 0C 10 10 00 03 00 }
0x3E72E: 			OneOfOption Option: "VT100" Value: 0 { 09 07 96 20 00 00 00 }
0x3E735: 			OneOfOption Option: "VT100Plus" Value: 1 { 09 07 97 20 00 00 01 }
0x3E73C: 			OneOfOption Option: "VT-UTF8" Value: 2 { 09 07 98 20 00 00 02 }
0x3E743: 			OneOfOption Option: "ANSI" Value: 3 { 09 07 99 20 00 00 03 }
0x3E74A: 			Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x3E750: 			Default DefaultId: 0x1 Value: 3 { 5B 06 01 00 00 03 }
0x3E756: 		End  { 29 02 }
0x3E758: 		OneOf Prompt: "Bits per second", Help: "Selects serial port transmission speed. The speed must be matched on the other side. Long or noisy lines may require lower speeds.", QuestionFlags: 0x10, QuestionId: 0x56A, VarStoreId: 0xF101, VarOffset: 0xC63, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x7, Step: 0x0 { 05 91 9C 20 A9 20 6A 05 01 F1 63 0C 10 10 03 07 00 }
0x3E769: 			OneOfOption Option: "9600" Value: 3 { 09 07 A8 1F 00 00 03 }
0x3E770: 			OneOfOption Option: "19200" Value: 4 { 09 07 A9 1F 00 00 04 }
0x3E777: 			OneOfOption Option: "38400" Value: 5 { 09 07 AA 20 00 00 05 }
0x3E77E: 			OneOfOption Option: "57600" Value: 6 { 09 07 AA 1F 00 00 06 }
0x3E785: 			OneOfOption Option: "115200" Value: 7 { 09 07 AB 1F 00 00 07 }
0x3E78C: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x3E792: 			Default DefaultId: 0x1 Value: 7 { 5B 06 01 00 00 07 }
0x3E798: 		End  { 29 02 }
0x3E79A: 		OneOf Prompt: "Data Bits", Help: "Data Bits", QuestionFlags: 0x10, QuestionId: 0x56B, VarStoreId: 0xF101, VarOffset: 0xC65, Flags: 0x10, Size: 8, Min: 0x7, Max: 0x8, Step: 0x0 { 05 91 AD 20 BA 20 6B 05 01 F1 65 0C 10 10 07 08 00 }
0x3E7AB: 			OneOfOption Option: "7" Value: 7 { 09 07 AC 04 00 00 07 }
0x3E7B2: 			OneOfOption Option: "8" Value: 8 { 09 07 AD 04 00 00 08 }
0x3E7B9: 			Default DefaultId: 0x0 Value: 8 { 5B 06 00 00 00 08 }
0x3E7BF: 			Default DefaultId: 0x1 Value: 8 { 5B 06 01 00 00 08 }
0x3E7C5: 		End  { 29 02 }
0x3E7C7: 		OneOf Prompt: "Parity", Help: "A parity bit can be sent with the data bits to detect some transmission errors. Even: parity bit is 0 if the num of 1's in the data bits is even. Odd: parity bit is 0 if num of 1's in the data bits is odd.  Mark: parity bit is always 1. Space: Parity bit is always 0. Mark and Space Parity do not allow for error detection. They can be used as an additional data bit.", QuestionFlags: 0x10, QuestionId: 0x56C, VarStoreId: 0xF101, VarOffset: 0xC67, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x5, Step: 0x0 { 05 91 BD 20 CA 20 6C 05 01 F1 67 0C 10 10 01 05 00 }
0x3E7D8: 			OneOfOption Option: "None" Value: 1 { 09 07 05 00 00 00 01 }
0x3E7DF: 			OneOfOption Option: "Even" Value: 2 { 09 07 CC 20 00 00 02 }
0x3E7E6: 			OneOfOption Option: "Odd" Value: 3 { 09 07 CB 20 00 00 03 }
0x3E7ED: 			OneOfOption Option: "Mark" Value: 4 { 09 07 CD 20 00 00 04 }
0x3E7F4: 			OneOfOption Option: "Space" Value: 5 { 09 07 CE 20 00 00 05 }
0x3E7FB: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E801: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E807: 		End  { 29 02 }
0x3E809: 		OneOf Prompt: "Stop Bits", Help: "Stop bits indicate the end of a serial data packet. (A start bit indicates the beginning). The standard setting is 1 stop bit. Communication with slow devices may require more than 1 stop bit.", QuestionFlags: 0x10, QuestionId: 0x56D, VarStoreId: 0xF101, VarOffset: 0xC69, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0 { 05 91 D1 20 DE 20 6D 05 01 F1 69 0C 10 10 01 03 00 }
0x3E81A: 			OneOfOption Option: "1" Value: 1 { 09 07 A6 04 00 00 01 }
0x3E821: 			OneOfOption Option: "2" Value: 3 { 09 07 A7 04 00 00 03 }
0x3E828: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E82E: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E834: 		End  { 29 02 }
0x3E836: 		OneOf Prompt: "Flow Control", Help: "Flow control can prevent data loss from buffer overflow. When sending data, if the receiving buffers are full, a 'stop' signal can be sent to stop the data flow. Once the buffers are empty, a 'start' signal can be sent to re-start the flow. Hardware flow control uses two wires to send start/stop signals.", QuestionFlags: 0x10, QuestionId: 0x56E, VarStoreId: 0xF101, VarOffset: 0xC6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 20 EE 20 6E 05 01 F1 6B 0C 10 10 00 01 00 }
0x3E847: 			OneOfOption Option: "None" Value: 0 { 09 07 05 00 00 00 00 }
0x3E84E: 			OneOfOption Option: "Hardware RTS/CTS" Value: 1 { 09 07 EF 20 00 00 01 }
0x3E855: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3E85B: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E861: 		End  { 29 02 }
0x3E863: 		CheckBox Prompt: "VT-UTF8 Combo Key Support", Help: "Enable VT-UTF8 Combination Key Support for ANSI/VT100 terminals", QuestionFlags: 0x10, QuestionId: 0x56F, VarStoreId: 0xF101, VarOffset: 0xC71, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 0B 21 18 21 6F 05 01 F1 71 0C 10 00 }
0x3E871: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E876: 				Value  { 5A 82 }
0x3E878: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x3E882: 				End  { 29 02 }
0x3E884: 			End  { 29 02 }
0x3E886: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E88C: 		End  { 29 02 }
0x3E88E: 		CheckBox Prompt: "Recorder Mode", Help: "With this mode enabled only text will be sent. This is to capture Terminal data.", QuestionFlags: 0x10, QuestionId: 0x570, VarStoreId: 0xF101, VarOffset: 0xC73, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 1A 21 27 21 70 05 01 F1 73 0C 10 00 }
0x3E89C: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E8A1: 				Value  { 5A 82 }
0x3E8A3: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E8AD: 				End  { 29 02 }
0x3E8AF: 			End  { 29 02 }
0x3E8B1: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E8B7: 		End  { 29 02 }
0x3E8B9: 		CheckBox Prompt: "Resolution 100x31", Help: "Enables or disables extended terminal resolution", QuestionFlags: 0x10, QuestionId: 0x571, VarStoreId: 0xF101, VarOffset: 0xC75, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E F8 20 05 21 71 05 01 F1 75 0C 10 00 }
0x3E8C7: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x3E8CC: 				Value  { 5A 82 }
0x3E8CE: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x3E8D8: 				End  { 29 02 }
0x3E8DA: 			End  { 29 02 }
0x3E8DC: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3E8E2: 		End  { 29 02 }
0x3E8E4: 		OneOf Prompt: "Putty KeyPad", Help: "Select FunctionKey and KeyPad on Putty.", QuestionFlags: 0x10, QuestionId: 0x572, VarStoreId: 0xF101, VarOffset: 0xC78, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x20, Step: 0x0 { 05 91 2C 21 39 21 72 05 01 F1 78 0C 10 10 01 20 00 }
0x3E8F5: 			OneOfOption Option: "VT100" Value: 1 { 09 07 96 20 00 00 01 }
0x3E8FC: 			OneOfOption Option: "LINUX" Value: 2 { 09 07 3A 21 00 00 02 }
0x3E903: 			OneOfOption Option: "XTERMR6" Value: 4 { 09 07 3B 21 00 00 04 }
0x3E90A: 			OneOfOption Option: "SCO" Value: 8 { 09 07 3C 21 00 00 08 }
0x3E911: 			OneOfOption Option: "ESCN" Value: 16 { 09 07 3D 21 00 00 10 }
0x3E918: 			OneOfOption Option: "VT400" Value: 32 { 09 07 3E 21 00 00 20 }
0x3E91F: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3E925: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3E92B: 		End  { 29 02 }
0x3E92D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E934: 		End  { 29 02 }
0x3E936: 	End  { 29 02 }
0x3E938: 	Form FormId: 0x28F9, Title: "Intel TXT Information" { 01 86 F9 28 27 01 }
0x3E93E: 		Subtitle Prompt: "Intel TXT Information", Help: "", Flags: 0x0 { 02 87 27 01 00 00 00 }
0x3E945: 		End  { 29 02 }
0x3E947: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3E94E: 		End  { 29 02 }
0x3E950: 		Text Prompt: "Chipset", Help: "Chipset is production or debug Fused", Text: "Debug Fused" { 03 08 29 01 2A 01 2B 01 }
0x3E958: 		Text Prompt: "BiosAcm", Help: "BiosAcm is production or debug Fused", Text: "Debug Fused" { 03 08 2C 01 2D 01 2E 01 }
0x3E960: 		Text Prompt: "Chipset Txt", Help: "Chipset support Txt", Text: "Not Supported" { 03 08 2F 01 30 01 31 01 }
0x3E968: 		Text Prompt: "Cpu Txt", Help: "Cpu support Txt", Text: "Not Supported" { 03 08 32 01 33 01 34 01 }
0x3E970: 		Text Prompt: "Error Code", Help: "This holds the Intel TXT shutdown error code.", Text: "None" { 03 08 35 01 36 01 37 01 }
0x3E978: 		Text Prompt: "  Class Code", Help: "Error code[9:4]", Text: "None" { 03 08 38 01 39 01 3A 01 }
0x3E980: 		Text Prompt: "  Major Code", Help: "Error code[14:10]", Text: "None" { 03 08 3B 01 3C 01 3D 01 }
0x3E988: 		Text Prompt: "  Minor Code", Help: "Error code[24:16]", Text: "None" { 03 08 3E 01 3F 01 40 01 }
0x3E990: 	End  { 29 02 }
0x3E992: 	Form FormId: 0x28FC, Title: "Switchable Graphics" { 01 86 FC 28 09 20 }
0x3E998: 		GrayOutIf  { 19 82 }
0x3E99A: 			EqIdVal QuestionId: 0x676, Value: 0x4 { 12 86 76 06 04 00 }
0x3E9A0: 				Not  { 17 02 }
0x3E9A2: 			End  { 29 02 }
0x3E9A4: 			OneOf Prompt: "SG Mode Select", Help: "MUXed vs. MUX-less          (nVidia-Optimus, ATI-PX4.0/PX5.0) Note!!! Either mode requires PrimaryDisplay set to 'SG'", QuestionFlags: 0x10, QuestionId: 0x573, VarStoreId: 0xF101, VarOffset: 0xC87, Flags: 0x10, Size: 8, Min: 0x2, Max: 0x2, Step: 0x0 { 05 91 0B 20 0C 20 73 05 01 F1 87 0C 10 10 02 02 00 }
0x3E9B5: 				OneOfOption Option: "Muxless" Value: 2, Default, MfgDefault { 09 07 0D 20 30 00 02 }
0x3E9BC: 			End  { 29 02 }
0x3E9BE: 		End  { 29 02 }
0x3E9C0: 		SuppressIf  { 0A 82 }
0x3E9C2: 			EqIdVal QuestionId: 0x676, Value: 0x4 { 12 86 76 06 04 00 }
0x3E9C8: 				Not  { 17 02 }
0x3E9CA: 				EqIdVal QuestionId: 0x11BC, Value: 0x0 { 12 06 BC 11 00 00 }
0x3E9D0: 				Or  { 16 02 }
0x3E9D2: 			End  { 29 02 }
0x3E9D4: 		End  { 29 02 }
0x3E9D6: 		OneOf Prompt: "Display Mode", Help: "NV DDS function", QuestionFlags: 0x14, QuestionId: 0x28FB, VarStoreId: 0xF101, VarOffset: 0xC88, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 16 20 17 20 FB 28 01 F1 88 0C 14 10 01 04 00 }
0x3E9E7: 			OneOfOption Option: "Integrated" Value: 1 { 09 07 18 20 00 00 01 }
0x3E9EE: 			OneOfOption Option: "Discrete" Value: 2 { 09 07 19 20 00 00 02 }
0x3E9F5: 			OneOfOption Option: "MSHybrid" Value: 3 { 09 07 1A 20 00 00 03 }
0x3E9FC: 			OneOfOption Option: "Dynamic" Value: 4, Default, MfgDefault { 09 07 1B 20 30 00 04 }
0x3EA03: 		End  { 29 02 }
0x3EA05: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3EA0C: 		End  { 29 02 }
0x3EA0E: 		Numeric Prompt: "GPU Package Power Limit Value", Help: "ATIF function 22 to get GPU Package Power Limit
Default:0x0
Minimum:0x0
Maximum:0xFF00", QuestionFlags: 0x10, QuestionId: 0x574, VarStoreId: 0xF101, VarOffset: 0xC8B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFF00, Step: 0x1 { 07 94 1C 20 1D 20 74 05 01 F1 8B 0C 10 21 00 00 00 FF 01 00 }
0x3EA22: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x3EA29: 		End  { 29 02 }
0x3EA2B: 	End  { 29 02 }
0x3EA2D: 	Form FormId: 0x28FF, Title: "AMI Graphic Output Protocol Policy" { 01 86 FF 28 26 20 }
0x3EA33: 		Subtitle Prompt: "Unknown Device", Help: "", Flags: 0x0 { 02 87 2E 20 00 00 00 }
0x3EA3A: 		End  { 29 02 }
0x3EA3C: 		Subtitle Prompt: "Unknown Driver", Help: "", Flags: 0x0 { 02 87 32 20 00 00 00 }
0x3EA43: 		End  { 29 02 }
0x3EA45: 		SuppressIf  { 0A 82 }
0x3EA47: 			EqIdVal QuestionId: 0x11BB, Value: 0x1 { 12 86 BB 11 01 00 }
0x3EA4D: 				Not  { 17 02 }
0x3EA4F: 			End  { 29 02 }
0x3EA51: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2900, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x0, Step: 0x0 { 05 91 28 20 29 20 00 29 01 F1 8D 0C 04 10 00 00 00 }
0x3EA62: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EA69: 			End  { 29 02 }
0x3EA6B: 		End  { 29 02 }
0x3EA6D: 		SuppressIf  { 0A 82 }
0x3EA6F: 			EqIdVal QuestionId: 0x11BB, Value: 0x2 { 12 86 BB 11 02 00 }
0x3EA75: 				Not  { 17 02 }
0x3EA77: 			End  { 29 02 }
0x3EA79: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2901, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 20 29 20 01 29 01 F1 8D 0C 04 10 00 01 00 }
0x3EA8A: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EA91: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EA98: 			End  { 29 02 }
0x3EA9A: 		End  { 29 02 }
0x3EA9C: 		SuppressIf  { 0A 82 }
0x3EA9E: 			EqIdVal QuestionId: 0x11BB, Value: 0x3 { 12 86 BB 11 03 00 }
0x3EAA4: 				Not  { 17 02 }
0x3EAA6: 			End  { 29 02 }
0x3EAA8: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2902, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 28 20 29 20 02 29 01 F1 8D 0C 04 10 00 02 00 }
0x3EAB9: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EAC0: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EAC7: 				OneOfOption Option: "Unknown Device" Value: 2 { 09 07 38 20 00 00 02 }
0x3EACE: 			End  { 29 02 }
0x3EAD0: 		End  { 29 02 }
0x3EAD2: 		SuppressIf  { 0A 82 }
0x3EAD4: 			EqIdVal QuestionId: 0x11BB, Value: 0x4 { 12 86 BB 11 04 00 }
0x3EADA: 				Not  { 17 02 }
0x3EADC: 			End  { 29 02 }
0x3EADE: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2903, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 28 20 29 20 03 29 01 F1 8D 0C 04 10 00 03 00 }
0x3EAEF: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EAF6: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EAFD: 				OneOfOption Option: "Unknown Device" Value: 2 { 09 07 38 20 00 00 02 }
0x3EB04: 				OneOfOption Option: "Unknown Device" Value: 3 { 09 07 39 20 00 00 03 }
0x3EB0B: 			End  { 29 02 }
0x3EB0D: 		End  { 29 02 }
0x3EB0F: 		SuppressIf  { 0A 82 }
0x3EB11: 			EqIdVal QuestionId: 0x11BB, Value: 0x5 { 12 86 BB 11 05 00 }
0x3EB17: 				Not  { 17 02 }
0x3EB19: 			End  { 29 02 }
0x3EB1B: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2904, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 28 20 29 20 04 29 01 F1 8D 0C 04 10 00 04 00 }
0x3EB2C: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EB33: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EB3A: 				OneOfOption Option: "Unknown Device" Value: 2 { 09 07 38 20 00 00 02 }
0x3EB41: 				OneOfOption Option: "Unknown Device" Value: 3 { 09 07 39 20 00 00 03 }
0x3EB48: 				OneOfOption Option: "Unknown Device" Value: 4 { 09 07 3A 20 00 00 04 }
0x3EB4F: 			End  { 29 02 }
0x3EB51: 		End  { 29 02 }
0x3EB53: 		SuppressIf  { 0A 82 }
0x3EB55: 			EqIdVal QuestionId: 0x11BB, Value: 0x6 { 12 86 BB 11 06 00 }
0x3EB5B: 				Not  { 17 02 }
0x3EB5D: 			End  { 29 02 }
0x3EB5F: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2905, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 28 20 29 20 05 29 01 F1 8D 0C 04 10 00 05 00 }
0x3EB70: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EB77: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EB7E: 				OneOfOption Option: "Unknown Device" Value: 2 { 09 07 38 20 00 00 02 }
0x3EB85: 				OneOfOption Option: "Unknown Device" Value: 3 { 09 07 39 20 00 00 03 }
0x3EB8C: 				OneOfOption Option: "Unknown Device" Value: 4 { 09 07 3A 20 00 00 04 }
0x3EB93: 				OneOfOption Option: "Unknown Device" Value: 5 { 09 07 3B 20 00 00 05 }
0x3EB9A: 			End  { 29 02 }
0x3EB9C: 		End  { 29 02 }
0x3EB9E: 		SuppressIf  { 0A 82 }
0x3EBA0: 			EqIdVal QuestionId: 0x11BB, Value: 0x7 { 12 86 BB 11 07 00 }
0x3EBA6: 				Not  { 17 02 }
0x3EBA8: 			End  { 29 02 }
0x3EBAA: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2906, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 28 20 29 20 06 29 01 F1 8D 0C 04 10 00 06 00 }
0x3EBBB: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EBC2: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EBC9: 				OneOfOption Option: "Unknown Device" Value: 2 { 09 07 38 20 00 00 02 }
0x3EBD0: 				OneOfOption Option: "Unknown Device" Value: 3 { 09 07 39 20 00 00 03 }
0x3EBD7: 				OneOfOption Option: "Unknown Device" Value: 4 { 09 07 3A 20 00 00 04 }
0x3EBDE: 				OneOfOption Option: "Unknown Device" Value: 5 { 09 07 3B 20 00 00 05 }
0x3EBE5: 				OneOfOption Option: "Unknown Device" Value: 6 { 09 07 3C 20 00 00 06 }
0x3EBEC: 			End  { 29 02 }
0x3EBEE: 		End  { 29 02 }
0x3EBF0: 		SuppressIf  { 0A 82 }
0x3EBF2: 			EqIdVal QuestionId: 0x11BB, Value: 0x8 { 12 86 BB 11 08 00 }
0x3EBF8: 				Not  { 17 02 }
0x3EBFA: 			End  { 29 02 }
0x3EBFC: 			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2907, VarStoreId: 0xF101, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 28 20 29 20 07 29 01 F1 8D 0C 04 10 00 07 00 }
0x3EC0D: 				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault { 09 07 36 20 30 00 00 }
0x3EC14: 				OneOfOption Option: "Unknown Device" Value: 1 { 09 07 37 20 00 00 01 }
0x3EC1B: 				OneOfOption Option: "Unknown Device" Value: 2 { 09 07 38 20 00 00 02 }
0x3EC22: 				OneOfOption Option: "Unknown Device" Value: 3 { 09 07 39 20 00 00 03 }
0x3EC29: 				OneOfOption Option: "Unknown Device" Value: 4 { 09 07 3A 20 00 00 04 }
0x3EC30: 				OneOfOption Option: "Unknown Device" Value: 5 { 09 07 3B 20 00 00 05 }
0x3EC37: 				OneOfOption Option: "Unknown Device" Value: 6 { 09 07 3C 20 00 00 06 }
0x3EC3E: 				OneOfOption Option: "Unknown Device" Value: 7 { 09 07 3D 20 00 00 07 }
0x3EC45: 			End  { 29 02 }
0x3EC47: 		End  { 29 02 }
0x3EC49: 		SuppressIf  { 0A 82 }
0x3EC4B: 			EqIdVal QuestionId: 0x11BA, Value: 0x0 { 12 06 BA 11 00 00 }
0x3EC51: 			Numeric Prompt: "Brightness Setting", Help: "Set Gop Brightness value", QuestionFlags: 0x4, QuestionId: 0x2908, VarStoreId: 0xF101, VarOffset: 0xC8E, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 2A 20 2B 20 08 29 01 F1 8E 0C 04 12 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x3EC6B: 				Default DefaultId: 0x0 Value: 255 { 5B 09 00 00 02 FF 00 00 00 }
0x3EC74: 				OneOfOption Option: "Brightness Setting" Value: 0, MfgDefault { 09 0A 2A 20 22 02 00 00 00 00 }
0x3EC7E: 			End  { 29 02 }
0x3EC80: 		End  { 29 02 }
0x3EC82: 		SuppressIf  { 0A 82 }
0x3EC84: 			EqIdVal QuestionId: 0x11B9, Value: 0x0 { 12 06 B9 11 00 00 }
0x3EC8A: 			OneOf Prompt: "BIST Enable", Help: "Starts or stops the BIST on the integrated display panel.", QuestionFlags: 0x14, QuestionId: 0x2909, VarStoreId: 0xF101, VarOffset: 0xC92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 20 2D 20 09 29 01 F1 92 0C 14 10 00 01 00 }
0x3EC9B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x3ECA2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x3ECA9: 			End  { 29 02 }
0x3ECAB: 		End  { 29 02 }
0x3ECAD: 	End  { 29 02 }
0x3ECAF: 	Form FormId: 0x290B, Title: "SIO Common Setting" { 01 86 0B 29 5A 20 }
0x3ECB5: 		Subtitle Prompt: "SIO Common Setting", Help: "", Flags: 0x0 { 02 87 5A 20 00 00 00 }
0x3ECBC: 		End  { 29 02 }
0x3ECBE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3ECC5: 		End  { 29 02 }
0x3ECC7: 		CheckBox Prompt: "Lock Legacy Resources", Help: "Enables or Disables Lock of Legacy Resources", QuestionFlags: 0x10, QuestionId: 0x575, VarStoreId: 0x290A, VarOffset: 0x0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 5C 20 5D 20 75 05 0A 29 00 00 10 00 }
0x3ECD5: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3ECDB: 		End  { 29 02 }
0x3ECDD: 	End  { 29 02 }
0x3ECDF: 	Form FormId: 0x290C, Title: "USB Configuration" { 01 86 0C 29 49 21 }
0x3ECE5: 		Subtitle Prompt: "USB Configuration", Help: "", Flags: 0x0 { 02 87 49 21 00 00 00 }
0x3ECEC: 		End  { 29 02 }
0x3ECEE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3ECF5: 		End  { 29 02 }
0x3ECF7: 		Text Prompt: "USB Module Version", Help: "", Text: "00.00" { 03 08 7D 21 02 00 7C 21 }
0x3ECFF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3ED06: 		End  { 29 02 }
0x3ED08: 		Text Prompt: "USB Controllers:", Help: "", Text: "" { 03 08 51 21 02 00 00 00 }
0x3ED10: 		Subtitle Prompt: "N/A", Help: "", Flags: 0x0 { 02 87 52 21 00 00 00 }
0x3ED17: 		End  { 29 02 }
0x3ED19: 		Text Prompt: "USB Devices:", Help: "", Text: "" { 03 08 53 21 02 00 00 00 }
0x3ED21: 		Subtitle Prompt: "N/A", Help: "", Flags: 0x0 { 02 87 54 21 00 00 00 }
0x3ED28: 		End  { 29 02 }
0x3ED2A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3ED31: 		End  { 29 02 }
0x3ED33: 		SuppressIf  { 0A 82 }
0x3ED35: 			EqIdId QuestionId: 0x20, OtherQuestionId: 0x20 { 13 06 20 00 20 00 }
0x3ED3B: 			GrayOutIf  { 19 82 }
0x3ED3D: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3ED43: 				OneOf Prompt: "USB Support", Help: "USB Support Parameters", QuestionFlags: 0x10, QuestionId: 0x576, VarStoreId: 0x19, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4B 21 4C 21 76 05 19 00 00 00 10 10 00 01 00 }
0x3ED54: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 4E 21 00 00 00 }
0x3ED5B: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 4D 21 30 00 01 }
0x3ED62: 				End  { 29 02 }
0x3ED64: 			End  { 29 02 }
0x3ED66: 		End  { 29 02 }
0x3ED68: 		SuppressIf  { 0A 82 }
0x3ED6A: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 06 76 05 00 00 }
0x3ED70: 			GrayOutIf  { 19 82 }
0x3ED72: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3ED78: 				OneOf Prompt: "Legacy USB Support", Help: "Enables Legacy USB support. AUTO option disables legacy support if no USB devices are connected. DISABLE option will keep USB devices available only for EFI applications.", QuestionFlags: 0x10, QuestionId: 0x577, VarStoreId: 0x19, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 55 21 56 21 77 05 19 00 01 00 10 10 00 02 00 }
0x3ED89: 					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 4D 21 30 00 00 }
0x3ED90: 					OneOfOption Option: "Disabled" Value: 1 { 09 07 4E 21 00 00 01 }
0x3ED97: 					OneOfOption Option: "Auto" Value: 2 { 09 07 4F 21 00 00 02 }
0x3ED9E: 				End  { 29 02 }
0x3EDA0: 			End  { 29 02 }
0x3EDA2: 		End  { 29 02 }
0x3EDA4: 		SuppressIf  { 0A 82 }
0x3EDA6: 			True  { 46 02 }
0x3EDA8: 			GrayOutIf  { 19 82 }
0x3EDAA: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3EDB0: 				OneOf Prompt: "USB 2.0 Controller Mode", Help: "Configures the USB 2.0 controller in HiSpeed (480Mbps) or FullSpeed (12Mbps).", QuestionFlags: 0x10, QuestionId: 0x578, VarStoreId: 0x19, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 21 77 21 78 05 19 00 2E 00 10 10 00 01 00 }
0x3EDC1: 					OneOfOption Option: "HiSpeed" Value: 1, Default, MfgDefault { 09 07 78 21 30 00 01 }
0x3EDC8: 					OneOfOption Option: "FullSpeed" Value: 0 { 09 07 79 21 00 00 00 }
0x3EDCF: 				End  { 29 02 }
0x3EDD1: 			End  { 29 02 }
0x3EDD3: 		End  { 29 02 }
0x3EDD5: 		SuppressIf  { 0A 82 }
0x3EDD7: 			True  { 46 02 }
0x3EDD9: 			GrayOutIf  { 19 82 }
0x3EDDB: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3EDE1: 				OneOf Prompt: "XHCI Legacy Support", Help: "Enable/Disable XHCI Controller Legacy support.", QuestionFlags: 0x10, QuestionId: 0x579, VarStoreId: 0x19, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 56 16 57 16 79 05 19 00 2A 00 10 10 00 01 00 }
0x3EDF2: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 4D 21 30 00 01 }
0x3EDF9: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 4E 21 00 00 00 }
0x3EE00: 				End  { 29 02 }
0x3EE02: 			End  { 29 02 }
0x3EE04: 		End  { 29 02 }
0x3EE06: 		SuppressIf  { 0A 82 }
0x3EE08: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3EE0E: 				EqIdVal QuestionId: 0x11B5, Value: 0x0 { 12 06 B5 11 00 00 }
0x3EE14: 				Or  { 16 02 }
0x3EE16: 			End  { 29 02 }
0x3EE18: 			GrayOutIf  { 19 82 }
0x3EE1A: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3EE20: 				OneOf Prompt: "XHCI Hand-off", Help: "This is a workaround for OSes without XHCI hand-off support. The XHCI ownership change should be claimed by XHCI driver.", QuestionFlags: 0x10, QuestionId: 0x57A, VarStoreId: 0x19, VarOffset: 0x2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 21 59 21 7A 05 19 00 2B 00 10 10 00 01 00 }
0x3EE31: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 4D 21 00 00 01 }
0x3EE38: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 4E 21 00 00 00 }
0x3EE3F: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3EE45: 					Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3EE4B: 				End  { 29 02 }
0x3EE4D: 			End  { 29 02 }
0x3EE4F: 		End  { 29 02 }
0x3EE51: 		SuppressIf  { 0A 82 }
0x3EE53: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3EE59: 				EqIdVal QuestionId: 0x11B6, Value: 0x0 { 12 06 B6 11 00 00 }
0x3EE5F: 				Or  { 16 02 }
0x3EE61: 			End  { 29 02 }
0x3EE63: 			GrayOutIf  { 19 82 }
0x3EE65: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x3EE6B: 				OneOf Prompt: "EHCI Hand-off", Help: "This is a workaround for OSes without EHCI hand-off support. The EHCI ownership change should be claimed by EHCI driver.", QuestionFlags: 0x10, QuestionId: 0x57B, VarStoreId: 0x19, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5A 21 5B 21 7B 05 19 00 02 00 10 10 00 01 00 }
0x3EE7C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 4E 21 30 00 00 }
0x3EE83: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 4D 21 00 00 01 }
0x3EE8A: 				End  { 29 02 }
0x3EE8C: 			End  { 29 02 }
0x3EE8E: 		End  { 29 02 }
0x3EE90: 		SuppressIf  { 0A 82 }
0x3EE92: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 06 76 05 00 00 }
0x3EE98: 			GrayOutIf  { 19 82 }
0x3EE9A: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3EEA0: 					EqIdVal QuestionId: 0x11B8, Value: 0x0 { 12 06 B8 11 00 00 }
0x3EEA6: 					EqIdVal QuestionId: 0x11B7, Value: 0x0 { 12 06 B7 11 00 00 }
0x3EEAC: 					And  { 15 02 }
0x3EEAE: 					EqIdVal QuestionId: 0x11B6, Value: 0x0 { 12 06 B6 11 00 00 }
0x3EEB4: 					And  { 15 02 }
0x3EEB6: 					EqIdVal QuestionId: 0x11B5, Value: 0x0 { 12 06 B5 11 00 00 }
0x3EEBC: 					And  { 15 02 }
0x3EEBE: 					Or  { 16 02 }
0x3EEC0: 				End  { 29 02 }
0x3EEC2: 				OneOf Prompt: "USB Mass Storage Driver Support", Help: "Enable/Disable USB Mass Storage Driver Support.", QuestionFlags: 0x10, QuestionId: 0x57C, VarStoreId: 0x19, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 21 7B 21 7C 05 19 00 2F 00 10 10 00 01 00 }
0x3EED3: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 4E 21 00 00 00 }
0x3EEDA: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 4D 21 30 00 01 }
0x3EEE1: 				End  { 29 02 }
0x3EEE3: 			End  { 29 02 }
0x3EEE5: 		End  { 29 02 }
0x3EEE7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3EEEE: 		End  { 29 02 }
0x3EEF0: 		Text Prompt: "USB hardware delays and time-outs:", Help: "", Text: "" { 03 08 64 21 02 00 00 00 }
0x3EEF8: 		SuppressIf  { 0A 82 }
0x3EEFA: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 06 76 05 00 00 }
0x3EF00: 			GrayOutIf  { 19 82 }
0x3EF02: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3EF08: 					EqIdVal QuestionId: 0x11B8, Value: 0x0 { 12 06 B8 11 00 00 }
0x3EF0E: 					EqIdVal QuestionId: 0x11B7, Value: 0x0 { 12 06 B7 11 00 00 }
0x3EF14: 					And  { 15 02 }
0x3EF16: 					EqIdVal QuestionId: 0x11B6, Value: 0x0 { 12 06 B6 11 00 00 }
0x3EF1C: 					And  { 15 02 }
0x3EF1E: 					EqIdVal QuestionId: 0x11B5, Value: 0x0 { 12 06 B5 11 00 00 }
0x3EF24: 					And  { 15 02 }
0x3EF26: 					Or  { 16 02 }
0x3EF28: 				End  { 29 02 }
0x3EF2A: 				OneOf Prompt: "USB transfer time-out", Help: "The time-out value for Control, Bulk, and Interrupt transfers.", QuestionFlags: 0x10, QuestionId: 0x57D, VarStoreId: 0x19, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x14, Step: 0x0 { 05 91 67 21 68 21 7D 05 19 00 09 00 10 10 01 14 00 }
0x3EF3B: 					OneOfOption Option: "1 sec" Value: 1 { 09 07 6E 21 00 00 01 }
0x3EF42: 					OneOfOption Option: "5 sec" Value: 5 { 09 07 6F 21 00 00 05 }
0x3EF49: 					OneOfOption Option: "10 sec" Value: 10 { 09 07 70 21 00 00 0A }
0x3EF50: 					OneOfOption Option: "20 sec" Value: 20, Default, MfgDefault { 09 07 71 21 30 00 14 }
0x3EF57: 				End  { 29 02 }
0x3EF59: 			End  { 29 02 }
0x3EF5B: 		End  { 29 02 }
0x3EF5D: 		SuppressIf  { 0A 82 }
0x3EF5F: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 06 76 05 00 00 }
0x3EF65: 			GrayOutIf  { 19 82 }
0x3EF67: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3EF6D: 					EqIdVal QuestionId: 0x11B8, Value: 0x0 { 12 06 B8 11 00 00 }
0x3EF73: 					EqIdVal QuestionId: 0x11B7, Value: 0x0 { 12 06 B7 11 00 00 }
0x3EF79: 					And  { 15 02 }
0x3EF7B: 					EqIdVal QuestionId: 0x11B6, Value: 0x0 { 12 06 B6 11 00 00 }
0x3EF81: 					And  { 15 02 }
0x3EF83: 					EqIdVal QuestionId: 0x11B5, Value: 0x0 { 12 06 B5 11 00 00 }
0x3EF89: 					And  { 15 02 }
0x3EF8B: 					Or  { 16 02 }
0x3EF8D: 				End  { 29 02 }
0x3EF8F: 				OneOf Prompt: "Device reset time-out", Help: "USB mass storage device Start Unit command time-out.", QuestionFlags: 0x10, QuestionId: 0x57E, VarStoreId: 0x19, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 65 21 66 21 7E 05 19 00 08 00 10 10 00 03 00 }
0x3EFA0: 					OneOfOption Option: "10 sec" Value: 0 { 09 07 70 21 00 00 00 }
0x3EFA7: 					OneOfOption Option: "20 sec" Value: 1, Default, MfgDefault { 09 07 71 21 30 00 01 }
0x3EFAE: 					OneOfOption Option: "30 sec" Value: 2 { 09 07 72 21 00 00 02 }
0x3EFB5: 					OneOfOption Option: "40 sec" Value: 3 { 09 07 73 21 00 00 03 }
0x3EFBC: 				End  { 29 02 }
0x3EFBE: 			End  { 29 02 }
0x3EFC0: 		End  { 29 02 }
0x3EFC2: 		GrayOutIf  { 19 82 }
0x3EFC4: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3EFCA: 				EqIdVal QuestionId: 0x11B8, Value: 0x0 { 12 06 B8 11 00 00 }
0x3EFD0: 				EqIdVal QuestionId: 0x11B7, Value: 0x0 { 12 06 B7 11 00 00 }
0x3EFD6: 				And  { 15 02 }
0x3EFD8: 				EqIdVal QuestionId: 0x11B6, Value: 0x0 { 12 06 B6 11 00 00 }
0x3EFDE: 				And  { 15 02 }
0x3EFE0: 				EqIdVal QuestionId: 0x11B5, Value: 0x0 { 12 06 B5 11 00 00 }
0x3EFE6: 				And  { 15 02 }
0x3EFE8: 				Or  { 16 02 }
0x3EFEA: 			End  { 29 02 }
0x3EFEC: 			OneOf Prompt: "Device power-up delay", Help: "Maximum time the device will take before it properly reports itself to the Host Controller. 'Auto' uses default value: for a Root port it is 100 ms, for a Hub port the delay is taken from Hub descriptor.", QuestionFlags: 0x10, QuestionId: 0x57F, VarStoreId: 0x19, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 21 6A 21 7F 05 19 00 2C 00 10 10 00 01 00 }
0x3EFFD: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F004: 				OneOfOption Option: "Manual" Value: 1 { 09 07 6B 21 00 00 01 }
0x3F00B: 			End  { 29 02 }
0x3F00D: 		End  { 29 02 }
0x3F00F: 		SuppressIf  { 0A 82 }
0x3F011: 			EqIdVal QuestionId: 0x57F, Value: 0x0 { 12 06 7F 05 00 00 }
0x3F017: 			GrayOutIf  { 19 82 }
0x3F019: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F01F: 					EqIdVal QuestionId: 0x11B8, Value: 0x0 { 12 06 B8 11 00 00 }
0x3F025: 					EqIdVal QuestionId: 0x11B7, Value: 0x0 { 12 06 B7 11 00 00 }
0x3F02B: 					And  { 15 02 }
0x3F02D: 					EqIdVal QuestionId: 0x11B6, Value: 0x0 { 12 06 B6 11 00 00 }
0x3F033: 					And  { 15 02 }
0x3F035: 					EqIdVal QuestionId: 0x11B5, Value: 0x0 { 12 06 B5 11 00 00 }
0x3F03B: 					And  { 15 02 }
0x3F03D: 					Or  { 16 02 }
0x3F03F: 				End  { 29 02 }
0x3F041: 				Numeric Prompt: "Device power-up delay in seconds", Help: "Delay range is 1..40 seconds, in one second increments", QuestionFlags: 0x10, QuestionId: 0x580, VarStoreId: 0x19, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x28, Step: 0x1 { 07 91 6C 21 6D 21 80 05 19 00 2D 00 10 10 01 28 01 }
0x3F052: 					Default DefaultId: 0x0 Value: 5 { 5B 06 00 00 00 05 }
0x3F058: 					Default DefaultId: 0x1 Value: 5 { 5B 06 01 00 00 05 }
0x3F05E: 				End  { 29 02 }
0x3F060: 			End  { 29 02 }
0x3F062: 		End  { 29 02 }
0x3F064: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3F06B: 		End  { 29 02 }
0x3F06D: 		SuppressIf  { 0A 82 }
0x3F06F: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F075: 				EqIdVal QuestionId: 0x11B4, Value: 0x0 { 12 06 B4 11 00 00 }
0x3F07B: 				Or  { 16 02 }
0x3F07D: 			End  { 29 02 }
0x3F07F: 			Text Prompt: "Mass Storage Devices:", Help: "", Text: "" { 03 08 A2 21 02 00 00 00 }
0x3F087: 		End  { 29 02 }
0x3F089: 		SuppressIf  { 0A 82 }
0x3F08B: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F091: 				EqIdVal QuestionId: 0x11B3, Value: 0x0 { 12 06 B3 11 00 00 }
0x3F097: 				Or  { 16 02 }
0x3F099: 			End  { 29 02 }
0x3F09B: 			GrayOutIf  { 19 82 }
0x3F09D: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F0A3: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F0A9: 					Or  { 16 02 }
0x3F0AB: 				End  { 29 02 }
0x3F0AD: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x581, VarStoreId: 0x19, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 82 21 A8 21 81 05 19 00 0A 00 10 10 00 04 00 }
0x3F0BE: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F0C5: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F0CC: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F0D3: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F0DA: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F0E1: 				End  { 29 02 }
0x3F0E3: 			End  { 29 02 }
0x3F0E5: 		End  { 29 02 }
0x3F0E7: 		SuppressIf  { 0A 82 }
0x3F0E9: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F0EF: 				EqIdVal QuestionId: 0x11B2, Value: 0x0 { 12 06 B2 11 00 00 }
0x3F0F5: 				Or  { 16 02 }
0x3F0F7: 			End  { 29 02 }
0x3F0F9: 			GrayOutIf  { 19 82 }
0x3F0FB: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F101: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F107: 					Or  { 16 02 }
0x3F109: 				End  { 29 02 }
0x3F10B: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x582, VarStoreId: 0x19, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 83 21 A8 21 82 05 19 00 0B 00 10 10 00 04 00 }
0x3F11C: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F123: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F12A: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F131: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F138: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F13F: 				End  { 29 02 }
0x3F141: 			End  { 29 02 }
0x3F143: 		End  { 29 02 }
0x3F145: 		SuppressIf  { 0A 82 }
0x3F147: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F14D: 				EqIdVal QuestionId: 0x11B1, Value: 0x0 { 12 06 B1 11 00 00 }
0x3F153: 				Or  { 16 02 }
0x3F155: 			End  { 29 02 }
0x3F157: 			GrayOutIf  { 19 82 }
0x3F159: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F15F: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F165: 					Or  { 16 02 }
0x3F167: 				End  { 29 02 }
0x3F169: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x583, VarStoreId: 0x19, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 84 21 A8 21 83 05 19 00 0C 00 10 10 00 04 00 }
0x3F17A: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F181: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F188: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F18F: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F196: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F19D: 				End  { 29 02 }
0x3F19F: 			End  { 29 02 }
0x3F1A1: 		End  { 29 02 }
0x3F1A3: 		SuppressIf  { 0A 82 }
0x3F1A5: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F1AB: 				EqIdVal QuestionId: 0x11B0, Value: 0x0 { 12 06 B0 11 00 00 }
0x3F1B1: 				Or  { 16 02 }
0x3F1B3: 			End  { 29 02 }
0x3F1B5: 			GrayOutIf  { 19 82 }
0x3F1B7: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F1BD: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F1C3: 					Or  { 16 02 }
0x3F1C5: 				End  { 29 02 }
0x3F1C7: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x584, VarStoreId: 0x19, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 85 21 A8 21 84 05 19 00 0D 00 10 10 00 04 00 }
0x3F1D8: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F1DF: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F1E6: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F1ED: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F1F4: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F1FB: 				End  { 29 02 }
0x3F1FD: 			End  { 29 02 }
0x3F1FF: 		End  { 29 02 }
0x3F201: 		SuppressIf  { 0A 82 }
0x3F203: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F209: 				EqIdVal QuestionId: 0x11AF, Value: 0x0 { 12 06 AF 11 00 00 }
0x3F20F: 				Or  { 16 02 }
0x3F211: 			End  { 29 02 }
0x3F213: 			GrayOutIf  { 19 82 }
0x3F215: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F21B: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F221: 					Or  { 16 02 }
0x3F223: 				End  { 29 02 }
0x3F225: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x585, VarStoreId: 0x19, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 86 21 A8 21 85 05 19 00 0E 00 10 10 00 04 00 }
0x3F236: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F23D: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F244: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F24B: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F252: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F259: 				End  { 29 02 }
0x3F25B: 			End  { 29 02 }
0x3F25D: 		End  { 29 02 }
0x3F25F: 		SuppressIf  { 0A 82 }
0x3F261: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F267: 				EqIdVal QuestionId: 0x11AE, Value: 0x0 { 12 06 AE 11 00 00 }
0x3F26D: 				Or  { 16 02 }
0x3F26F: 			End  { 29 02 }
0x3F271: 			GrayOutIf  { 19 82 }
0x3F273: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F279: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F27F: 					Or  { 16 02 }
0x3F281: 				End  { 29 02 }
0x3F283: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x586, VarStoreId: 0x19, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 87 21 A8 21 86 05 19 00 0F 00 10 10 00 04 00 }
0x3F294: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F29B: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F2A2: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F2A9: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F2B0: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F2B7: 				End  { 29 02 }
0x3F2B9: 			End  { 29 02 }
0x3F2BB: 		End  { 29 02 }
0x3F2BD: 		SuppressIf  { 0A 82 }
0x3F2BF: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F2C5: 				EqIdVal QuestionId: 0x11AD, Value: 0x0 { 12 06 AD 11 00 00 }
0x3F2CB: 				Or  { 16 02 }
0x3F2CD: 			End  { 29 02 }
0x3F2CF: 			GrayOutIf  { 19 82 }
0x3F2D1: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F2D7: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F2DD: 					Or  { 16 02 }
0x3F2DF: 				End  { 29 02 }
0x3F2E1: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x587, VarStoreId: 0x19, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 88 21 A8 21 87 05 19 00 10 00 10 10 00 04 00 }
0x3F2F2: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F2F9: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F300: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F307: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F30E: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F315: 				End  { 29 02 }
0x3F317: 			End  { 29 02 }
0x3F319: 		End  { 29 02 }
0x3F31B: 		SuppressIf  { 0A 82 }
0x3F31D: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F323: 				EqIdVal QuestionId: 0x11AC, Value: 0x0 { 12 06 AC 11 00 00 }
0x3F329: 				Or  { 16 02 }
0x3F32B: 			End  { 29 02 }
0x3F32D: 			GrayOutIf  { 19 82 }
0x3F32F: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F335: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F33B: 					Or  { 16 02 }
0x3F33D: 				End  { 29 02 }
0x3F33F: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x588, VarStoreId: 0x19, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 89 21 A8 21 88 05 19 00 11 00 10 10 00 04 00 }
0x3F350: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F357: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F35E: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F365: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F36C: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F373: 				End  { 29 02 }
0x3F375: 			End  { 29 02 }
0x3F377: 		End  { 29 02 }
0x3F379: 		SuppressIf  { 0A 82 }
0x3F37B: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F381: 				EqIdVal QuestionId: 0x11AB, Value: 0x0 { 12 06 AB 11 00 00 }
0x3F387: 				Or  { 16 02 }
0x3F389: 			End  { 29 02 }
0x3F38B: 			GrayOutIf  { 19 82 }
0x3F38D: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F393: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F399: 					Or  { 16 02 }
0x3F39B: 				End  { 29 02 }
0x3F39D: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x589, VarStoreId: 0x19, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8A 21 A8 21 89 05 19 00 12 00 10 10 00 04 00 }
0x3F3AE: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F3B5: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F3BC: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F3C3: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F3CA: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F3D1: 				End  { 29 02 }
0x3F3D3: 			End  { 29 02 }
0x3F3D5: 		End  { 29 02 }
0x3F3D7: 		SuppressIf  { 0A 82 }
0x3F3D9: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F3DF: 				EqIdVal QuestionId: 0x11AA, Value: 0x0 { 12 06 AA 11 00 00 }
0x3F3E5: 				Or  { 16 02 }
0x3F3E7: 			End  { 29 02 }
0x3F3E9: 			GrayOutIf  { 19 82 }
0x3F3EB: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F3F1: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F3F7: 					Or  { 16 02 }
0x3F3F9: 				End  { 29 02 }
0x3F3FB: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x58A, VarStoreId: 0x19, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8B 21 A8 21 8A 05 19 00 13 00 10 10 00 04 00 }
0x3F40C: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F413: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F41A: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F421: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F428: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F42F: 				End  { 29 02 }
0x3F431: 			End  { 29 02 }
0x3F433: 		End  { 29 02 }
0x3F435: 		SuppressIf  { 0A 82 }
0x3F437: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F43D: 				EqIdVal QuestionId: 0x11A9, Value: 0x0 { 12 06 A9 11 00 00 }
0x3F443: 				Or  { 16 02 }
0x3F445: 			End  { 29 02 }
0x3F447: 			GrayOutIf  { 19 82 }
0x3F449: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F44F: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F455: 					Or  { 16 02 }
0x3F457: 				End  { 29 02 }
0x3F459: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x58B, VarStoreId: 0x19, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8C 21 A8 21 8B 05 19 00 14 00 10 10 00 04 00 }
0x3F46A: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F471: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F478: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F47F: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F486: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F48D: 				End  { 29 02 }
0x3F48F: 			End  { 29 02 }
0x3F491: 		End  { 29 02 }
0x3F493: 		SuppressIf  { 0A 82 }
0x3F495: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F49B: 				EqIdVal QuestionId: 0x11A8, Value: 0x0 { 12 06 A8 11 00 00 }
0x3F4A1: 				Or  { 16 02 }
0x3F4A3: 			End  { 29 02 }
0x3F4A5: 			GrayOutIf  { 19 82 }
0x3F4A7: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F4AD: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F4B3: 					Or  { 16 02 }
0x3F4B5: 				End  { 29 02 }
0x3F4B7: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x58C, VarStoreId: 0x19, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8D 21 A8 21 8C 05 19 00 15 00 10 10 00 04 00 }
0x3F4C8: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F4CF: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F4D6: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F4DD: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F4E4: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F4EB: 				End  { 29 02 }
0x3F4ED: 			End  { 29 02 }
0x3F4EF: 		End  { 29 02 }
0x3F4F1: 		SuppressIf  { 0A 82 }
0x3F4F3: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F4F9: 				EqIdVal QuestionId: 0x11A7, Value: 0x0 { 12 06 A7 11 00 00 }
0x3F4FF: 				Or  { 16 02 }
0x3F501: 			End  { 29 02 }
0x3F503: 			GrayOutIf  { 19 82 }
0x3F505: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F50B: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F511: 					Or  { 16 02 }
0x3F513: 				End  { 29 02 }
0x3F515: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x58D, VarStoreId: 0x19, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8E 21 A8 21 8D 05 19 00 16 00 10 10 00 04 00 }
0x3F526: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F52D: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F534: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F53B: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F542: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F549: 				End  { 29 02 }
0x3F54B: 			End  { 29 02 }
0x3F54D: 		End  { 29 02 }
0x3F54F: 		SuppressIf  { 0A 82 }
0x3F551: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F557: 				EqIdVal QuestionId: 0x11A6, Value: 0x0 { 12 06 A6 11 00 00 }
0x3F55D: 				Or  { 16 02 }
0x3F55F: 			End  { 29 02 }
0x3F561: 			GrayOutIf  { 19 82 }
0x3F563: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F569: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F56F: 					Or  { 16 02 }
0x3F571: 				End  { 29 02 }
0x3F573: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x58E, VarStoreId: 0x19, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8F 21 A8 21 8E 05 19 00 17 00 10 10 00 04 00 }
0x3F584: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F58B: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F592: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F599: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F5A0: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F5A7: 				End  { 29 02 }
0x3F5A9: 			End  { 29 02 }
0x3F5AB: 		End  { 29 02 }
0x3F5AD: 		SuppressIf  { 0A 82 }
0x3F5AF: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F5B5: 				EqIdVal QuestionId: 0x11A5, Value: 0x0 { 12 06 A5 11 00 00 }
0x3F5BB: 				Or  { 16 02 }
0x3F5BD: 			End  { 29 02 }
0x3F5BF: 			GrayOutIf  { 19 82 }
0x3F5C1: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F5C7: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F5CD: 					Or  { 16 02 }
0x3F5CF: 				End  { 29 02 }
0x3F5D1: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x58F, VarStoreId: 0x19, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 90 21 A8 21 8F 05 19 00 18 00 10 10 00 04 00 }
0x3F5E2: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F5E9: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F5F0: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F5F7: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F5FE: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F605: 				End  { 29 02 }
0x3F607: 			End  { 29 02 }
0x3F609: 		End  { 29 02 }
0x3F60B: 		SuppressIf  { 0A 82 }
0x3F60D: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F613: 				EqIdVal QuestionId: 0x11A4, Value: 0x0 { 12 06 A4 11 00 00 }
0x3F619: 				Or  { 16 02 }
0x3F61B: 			End  { 29 02 }
0x3F61D: 			GrayOutIf  { 19 82 }
0x3F61F: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F625: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F62B: 					Or  { 16 02 }
0x3F62D: 				End  { 29 02 }
0x3F62F: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x590, VarStoreId: 0x19, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 91 21 A8 21 90 05 19 00 19 00 10 10 00 04 00 }
0x3F640: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F647: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F64E: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F655: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F65C: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F663: 				End  { 29 02 }
0x3F665: 			End  { 29 02 }
0x3F667: 		End  { 29 02 }
0x3F669: 		SuppressIf  { 0A 82 }
0x3F66B: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F671: 				EqIdVal QuestionId: 0x11A3, Value: 0x0 { 12 06 A3 11 00 00 }
0x3F677: 				Or  { 16 02 }
0x3F679: 			End  { 29 02 }
0x3F67B: 			GrayOutIf  { 19 82 }
0x3F67D: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F683: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F689: 					Or  { 16 02 }
0x3F68B: 				End  { 29 02 }
0x3F68D: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x591, VarStoreId: 0x19, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 92 21 A8 21 91 05 19 00 1A 00 10 10 00 04 00 }
0x3F69E: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F6A5: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F6AC: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F6B3: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F6BA: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F6C1: 				End  { 29 02 }
0x3F6C3: 			End  { 29 02 }
0x3F6C5: 		End  { 29 02 }
0x3F6C7: 		SuppressIf  { 0A 82 }
0x3F6C9: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F6CF: 				EqIdVal QuestionId: 0x11A2, Value: 0x0 { 12 06 A2 11 00 00 }
0x3F6D5: 				Or  { 16 02 }
0x3F6D7: 			End  { 29 02 }
0x3F6D9: 			GrayOutIf  { 19 82 }
0x3F6DB: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F6E1: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F6E7: 					Or  { 16 02 }
0x3F6E9: 				End  { 29 02 }
0x3F6EB: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x592, VarStoreId: 0x19, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 93 21 A8 21 92 05 19 00 1B 00 10 10 00 04 00 }
0x3F6FC: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F703: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F70A: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F711: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F718: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F71F: 				End  { 29 02 }
0x3F721: 			End  { 29 02 }
0x3F723: 		End  { 29 02 }
0x3F725: 		SuppressIf  { 0A 82 }
0x3F727: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F72D: 				EqIdVal QuestionId: 0x11A1, Value: 0x0 { 12 06 A1 11 00 00 }
0x3F733: 				Or  { 16 02 }
0x3F735: 			End  { 29 02 }
0x3F737: 			GrayOutIf  { 19 82 }
0x3F739: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F73F: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F745: 					Or  { 16 02 }
0x3F747: 				End  { 29 02 }
0x3F749: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x593, VarStoreId: 0x19, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 94 21 A8 21 93 05 19 00 1C 00 10 10 00 04 00 }
0x3F75A: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F761: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F768: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F76F: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F776: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F77D: 				End  { 29 02 }
0x3F77F: 			End  { 29 02 }
0x3F781: 		End  { 29 02 }
0x3F783: 		SuppressIf  { 0A 82 }
0x3F785: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F78B: 				EqIdVal QuestionId: 0x11A0, Value: 0x0 { 12 06 A0 11 00 00 }
0x3F791: 				Or  { 16 02 }
0x3F793: 			End  { 29 02 }
0x3F795: 			GrayOutIf  { 19 82 }
0x3F797: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F79D: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F7A3: 					Or  { 16 02 }
0x3F7A5: 				End  { 29 02 }
0x3F7A7: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x594, VarStoreId: 0x19, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 95 21 A8 21 94 05 19 00 1D 00 10 10 00 04 00 }
0x3F7B8: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F7BF: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F7C6: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F7CD: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F7D4: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F7DB: 				End  { 29 02 }
0x3F7DD: 			End  { 29 02 }
0x3F7DF: 		End  { 29 02 }
0x3F7E1: 		SuppressIf  { 0A 82 }
0x3F7E3: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F7E9: 				EqIdVal QuestionId: 0x119F, Value: 0x0 { 12 06 9F 11 00 00 }
0x3F7EF: 				Or  { 16 02 }
0x3F7F1: 			End  { 29 02 }
0x3F7F3: 			GrayOutIf  { 19 82 }
0x3F7F5: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F7FB: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F801: 					Or  { 16 02 }
0x3F803: 				End  { 29 02 }
0x3F805: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x595, VarStoreId: 0x19, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 96 21 A8 21 95 05 19 00 1E 00 10 10 00 04 00 }
0x3F816: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F81D: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F824: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F82B: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F832: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F839: 				End  { 29 02 }
0x3F83B: 			End  { 29 02 }
0x3F83D: 		End  { 29 02 }
0x3F83F: 		SuppressIf  { 0A 82 }
0x3F841: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F847: 				EqIdVal QuestionId: 0x119E, Value: 0x0 { 12 06 9E 11 00 00 }
0x3F84D: 				Or  { 16 02 }
0x3F84F: 			End  { 29 02 }
0x3F851: 			GrayOutIf  { 19 82 }
0x3F853: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F859: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F85F: 					Or  { 16 02 }
0x3F861: 				End  { 29 02 }
0x3F863: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x596, VarStoreId: 0x19, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 97 21 A8 21 96 05 19 00 1F 00 10 10 00 04 00 }
0x3F874: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F87B: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F882: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F889: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F890: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F897: 				End  { 29 02 }
0x3F899: 			End  { 29 02 }
0x3F89B: 		End  { 29 02 }
0x3F89D: 		SuppressIf  { 0A 82 }
0x3F89F: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F8A5: 				EqIdVal QuestionId: 0x119D, Value: 0x0 { 12 06 9D 11 00 00 }
0x3F8AB: 				Or  { 16 02 }
0x3F8AD: 			End  { 29 02 }
0x3F8AF: 			GrayOutIf  { 19 82 }
0x3F8B1: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F8B7: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F8BD: 					Or  { 16 02 }
0x3F8BF: 				End  { 29 02 }
0x3F8C1: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x597, VarStoreId: 0x19, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 98 21 A8 21 97 05 19 00 20 00 10 10 00 04 00 }
0x3F8D2: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F8D9: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F8E0: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F8E7: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F8EE: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F8F5: 				End  { 29 02 }
0x3F8F7: 			End  { 29 02 }
0x3F8F9: 		End  { 29 02 }
0x3F8FB: 		SuppressIf  { 0A 82 }
0x3F8FD: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F903: 				EqIdVal QuestionId: 0x119C, Value: 0x0 { 12 06 9C 11 00 00 }
0x3F909: 				Or  { 16 02 }
0x3F90B: 			End  { 29 02 }
0x3F90D: 			GrayOutIf  { 19 82 }
0x3F90F: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F915: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F91B: 					Or  { 16 02 }
0x3F91D: 				End  { 29 02 }
0x3F91F: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x598, VarStoreId: 0x19, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 99 21 A8 21 98 05 19 00 21 00 10 10 00 04 00 }
0x3F930: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F937: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F93E: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F945: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F94C: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F953: 				End  { 29 02 }
0x3F955: 			End  { 29 02 }
0x3F957: 		End  { 29 02 }
0x3F959: 		SuppressIf  { 0A 82 }
0x3F95B: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F961: 				EqIdVal QuestionId: 0x119B, Value: 0x0 { 12 06 9B 11 00 00 }
0x3F967: 				Or  { 16 02 }
0x3F969: 			End  { 29 02 }
0x3F96B: 			GrayOutIf  { 19 82 }
0x3F96D: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F973: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F979: 					Or  { 16 02 }
0x3F97B: 				End  { 29 02 }
0x3F97D: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x599, VarStoreId: 0x19, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 9A 21 A8 21 99 05 19 00 22 00 10 10 00 04 00 }
0x3F98E: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F995: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F99C: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3F9A3: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3F9AA: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3F9B1: 				End  { 29 02 }
0x3F9B3: 			End  { 29 02 }
0x3F9B5: 		End  { 29 02 }
0x3F9B7: 		SuppressIf  { 0A 82 }
0x3F9B9: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3F9BF: 				EqIdVal QuestionId: 0x119A, Value: 0x0 { 12 06 9A 11 00 00 }
0x3F9C5: 				Or  { 16 02 }
0x3F9C7: 			End  { 29 02 }
0x3F9C9: 			GrayOutIf  { 19 82 }
0x3F9CB: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3F9D1: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3F9D7: 					Or  { 16 02 }
0x3F9D9: 				End  { 29 02 }
0x3F9DB: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x59A, VarStoreId: 0x19, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 9B 21 A8 21 9A 05 19 00 23 00 10 10 00 04 00 }
0x3F9EC: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3F9F3: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3F9FA: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FA01: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FA08: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FA0F: 				End  { 29 02 }
0x3FA11: 			End  { 29 02 }
0x3FA13: 		End  { 29 02 }
0x3FA15: 		SuppressIf  { 0A 82 }
0x3FA17: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3FA1D: 				EqIdVal QuestionId: 0x1199, Value: 0x0 { 12 06 99 11 00 00 }
0x3FA23: 				Or  { 16 02 }
0x3FA25: 			End  { 29 02 }
0x3FA27: 			GrayOutIf  { 19 82 }
0x3FA29: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3FA2F: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3FA35: 					Or  { 16 02 }
0x3FA37: 				End  { 29 02 }
0x3FA39: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x59B, VarStoreId: 0x19, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 9C 21 A8 21 9B 05 19 00 24 00 10 10 00 04 00 }
0x3FA4A: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3FA51: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3FA58: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FA5F: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FA66: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FA6D: 				End  { 29 02 }
0x3FA6F: 			End  { 29 02 }
0x3FA71: 		End  { 29 02 }
0x3FA73: 		SuppressIf  { 0A 82 }
0x3FA75: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3FA7B: 				EqIdVal QuestionId: 0x1198, Value: 0x0 { 12 06 98 11 00 00 }
0x3FA81: 				Or  { 16 02 }
0x3FA83: 			End  { 29 02 }
0x3FA85: 			GrayOutIf  { 19 82 }
0x3FA87: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3FA8D: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3FA93: 					Or  { 16 02 }
0x3FA95: 				End  { 29 02 }
0x3FA97: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x59C, VarStoreId: 0x19, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 9D 21 A8 21 9C 05 19 00 25 00 10 10 00 04 00 }
0x3FAA8: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3FAAF: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3FAB6: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FABD: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FAC4: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FACB: 				End  { 29 02 }
0x3FACD: 			End  { 29 02 }
0x3FACF: 		End  { 29 02 }
0x3FAD1: 		SuppressIf  { 0A 82 }
0x3FAD3: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3FAD9: 				EqIdVal QuestionId: 0x1197, Value: 0x0 { 12 06 97 11 00 00 }
0x3FADF: 				Or  { 16 02 }
0x3FAE1: 			End  { 29 02 }
0x3FAE3: 			GrayOutIf  { 19 82 }
0x3FAE5: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3FAEB: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3FAF1: 					Or  { 16 02 }
0x3FAF3: 				End  { 29 02 }
0x3FAF5: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x59D, VarStoreId: 0x19, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 9E 21 A8 21 9D 05 19 00 26 00 10 10 00 04 00 }
0x3FB06: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3FB0D: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3FB14: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FB1B: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FB22: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FB29: 				End  { 29 02 }
0x3FB2B: 			End  { 29 02 }
0x3FB2D: 		End  { 29 02 }
0x3FB2F: 		SuppressIf  { 0A 82 }
0x3FB31: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3FB37: 				EqIdVal QuestionId: 0x1196, Value: 0x0 { 12 06 96 11 00 00 }
0x3FB3D: 				Or  { 16 02 }
0x3FB3F: 			End  { 29 02 }
0x3FB41: 			GrayOutIf  { 19 82 }
0x3FB43: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3FB49: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3FB4F: 					Or  { 16 02 }
0x3FB51: 				End  { 29 02 }
0x3FB53: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x59E, VarStoreId: 0x19, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 9F 21 A8 21 9E 05 19 00 27 00 10 10 00 04 00 }
0x3FB64: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3FB6B: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3FB72: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FB79: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FB80: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FB87: 				End  { 29 02 }
0x3FB89: 			End  { 29 02 }
0x3FB8B: 		End  { 29 02 }
0x3FB8D: 		SuppressIf  { 0A 82 }
0x3FB8F: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3FB95: 				EqIdVal QuestionId: 0x1195, Value: 0x0 { 12 06 95 11 00 00 }
0x3FB9B: 				Or  { 16 02 }
0x3FB9D: 			End  { 29 02 }
0x3FB9F: 			GrayOutIf  { 19 82 }
0x3FBA1: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3FBA7: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3FBAD: 					Or  { 16 02 }
0x3FBAF: 				End  { 29 02 }
0x3FBB1: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x59F, VarStoreId: 0x19, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 A0 21 A8 21 9F 05 19 00 28 00 10 10 00 04 00 }
0x3FBC2: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3FBC9: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3FBD0: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FBD7: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FBDE: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FBE5: 				End  { 29 02 }
0x3FBE7: 			End  { 29 02 }
0x3FBE9: 		End  { 29 02 }
0x3FBEB: 		SuppressIf  { 0A 82 }
0x3FBED: 			EqIdVal QuestionId: 0x576, Value: 0x0 { 12 86 76 05 00 00 }
0x3FBF3: 				EqIdVal QuestionId: 0x1194, Value: 0x0 { 12 06 94 11 00 00 }
0x3FBF9: 				Or  { 16 02 }
0x3FBFB: 			End  { 29 02 }
0x3FBFD: 			GrayOutIf  { 19 82 }
0x3FBFF: 				EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x3FC05: 					EqIdVal QuestionId: 0x577, Value: 0x1 { 12 06 77 05 01 00 }
0x3FC0B: 					Or  { 16 02 }
0x3FC0D: 				End  { 29 02 }
0x3FC0F: 				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x5A0, VarStoreId: 0x19, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 A1 21 A8 21 A0 05 19 00 29 00 10 10 00 04 00 }
0x3FC20: 					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 4F 21 30 00 00 }
0x3FC27: 					OneOfOption Option: "Floppy" Value: 1 { 09 07 A3 21 00 00 01 }
0x3FC2E: 					OneOfOption Option: "Forced FDD" Value: 2 { 09 07 A4 21 00 00 02 }
0x3FC35: 					OneOfOption Option: "Hard Disk" Value: 3 { 09 07 A5 21 00 00 03 }
0x3FC3C: 					OneOfOption Option: "CD-ROM" Value: 4 { 09 07 A6 21 00 00 04 }
0x3FC43: 				End  { 29 02 }
0x3FC45: 			End  { 29 02 }
0x3FC47: 		End  { 29 02 }
0x3FC49: 		Text Prompt: "", Help: "", Text: "" { 03 08 02 00 02 00 00 00 }
0x3FC51: 		SuppressIf  { 0A 82 }
0x3FC53: 			True  { 46 02 }
0x3FC55: 			SuppressIf  { 0A 82 }
0x3FC57: 				EqIdVal QuestionId: 0x10FC, Value: 0xB { 12 06 FC 10 0B 00 }
0x3FC5D: 				Action Prompt: "", Help: "", QuestionFlags: 0x4, QuestionId: 0x290D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: "" { 0C 8F 02 00 02 00 0D 29 00 00 FF FF 04 00 00 }
0x3FC6C: 				End  { 29 02 }
0x3FC6E: 			End  { 29 02 }
0x3FC70: 		End  { 29 02 }
0x3FC72: 	End  { 29 02 }
0x3FC74: 	Form FormId: 0x290F, Title: "Network Stack Configuration" { 01 86 0F 29 AB 21 }
0x3FC7A: 		OneOf Prompt: "Network Stack", Help: "Enable/Disable UEFI Network Stack", QuestionFlags: 0x10, QuestionId: 0x5A1, VarStoreId: 0x1A, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 21 AA 21 A1 05 1A 00 00 00 10 10 00 01 00 }
0x3FC8B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3FC92: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3FC99: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FC9F: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FCA5: 		End  { 29 02 }
0x3FCA7: 		SuppressIf  { 0A 82 }
0x3FCA9: 			EqIdVal QuestionId: 0x5A1, Value: 0x0 { 12 06 A1 05 00 00 }
0x3FCAF: 			OneOf Prompt: "IPv4 PXE Support", Help: "Enable/Disable IPv4 PXE boot support. If disabled, IPv4 PXE boot support will not be available.", QuestionFlags: 0x10, QuestionId: 0x5A2, VarStoreId: 0x1A, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 21 AE 21 A2 05 1A 00 01 00 10 10 00 01 00 }
0x3FCC0: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3FCC7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3FCCE: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FCD4: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FCDA: 			End  { 29 02 }
0x3FCDC: 			OneOf Prompt: "IPv4 HTTP Support", Help: "Enable/Disable IPv4 HTTP boot support. If disabled, IPv4 HTTP boot support will not be available.", QuestionFlags: 0x10, QuestionId: 0x5A3, VarStoreId: 0x1A, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 21 B8 21 A3 05 1A 00 06 00 10 10 00 01 00 }
0x3FCED: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3FCF4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3FCFB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FD01: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FD07: 			End  { 29 02 }
0x3FD09: 		End  { 29 02 }
0x3FD0B: 		SuppressIf  { 0A 82 }
0x3FD0D: 			EqIdVal QuestionId: 0x5A1, Value: 0x0 { 12 06 A1 05 00 00 }
0x3FD13: 			OneOf Prompt: "IPv6 PXE Support", Help: "Enable/Disable IPv6 PXE boot support. If disabled, IPv6 PXE boot support will not be available.", QuestionFlags: 0x10, QuestionId: 0x5A4, VarStoreId: 0x1A, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AF 21 B0 21 A4 05 1A 00 02 00 10 10 00 01 00 }
0x3FD24: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3FD2B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3FD32: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FD38: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FD3E: 			End  { 29 02 }
0x3FD40: 			OneOf Prompt: "IPv6 HTTP Support", Help: "Enable/Disable IPv6 HTTP boot support. If disabled, IPv6 HTTP boot support will not be available.", QuestionFlags: 0x10, QuestionId: 0x5A5, VarStoreId: 0x1A, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 21 BA 21 A5 05 1A 00 07 00 10 10 00 01 00 }
0x3FD51: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3FD58: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3FD5F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FD65: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FD6B: 			End  { 29 02 }
0x3FD6D: 		End  { 29 02 }
0x3FD6F: 		SuppressIf  { 0A 82 }
0x3FD71: 			EqIdVal QuestionId: 0x5A1, Value: 0x0 { 12 06 A1 05 00 00 }
0x3FD77: 			Numeric Prompt: "PXE boot wait time", Help: "Wait time in seconds to press ESC key to abort the PXE boot. Use either +/- or numeric keys to set the value.", QuestionFlags: 0x10, QuestionId: 0x5A6, VarStoreId: 0x1A, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x1 { 07 91 B3 21 B4 21 A6 05 1A 00 04 00 10 10 00 05 01 }
0x3FD88: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FD8E: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FD94: 			End  { 29 02 }
0x3FD96: 		End  { 29 02 }
0x3FD98: 		SuppressIf  { 0A 82 }
0x3FD9A: 			EqIdVal QuestionId: 0x5A1, Value: 0x0 { 12 06 A1 05 00 00 }
0x3FDA0: 			Numeric Prompt: "Media detect count", Help: "Number of times the presence of media will be checked. Use either +/- or numeric keys to set the value.", QuestionFlags: 0x10, QuestionId: 0x5A7, VarStoreId: 0x1A, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 B5 21 B6 21 A7 05 1A 00 05 00 10 10 01 32 01 }
0x3FDB1: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3FDB7: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3FDBD: 			End  { 29 02 }
0x3FDBF: 		End  { 29 02 }
0x3FDC1: 	End  { 29 02 }
0x3FDC3: 	Form FormId: 0x2911, Title: "CSM Configuration" { 01 86 11 29 BB 21 }
0x3FDC9: 		Subtitle Prompt: "Compatibility Support Module Configuration", Help: "", Flags: 0x0 { 02 87 BD 21 00 00 00 }
0x3FDD0: 		End  { 29 02 }
0x3FDD2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3FDD9: 		End  { 29 02 }
0x3FDDB: 		SuppressIf  { 0A 82 }
0x3FDDD: 			EqIdVal QuestionId: 0x1108, Value: 0x1 { 12 06 08 11 01 00 }
0x3FDE3: 			OneOf Prompt: "CSM Support", Help: "Enable/Disable CSM Support.", QuestionFlags: 0x14, QuestionId: 0x2910, VarStoreId: 0xF101, VarOffset: 0xC93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 21 D1 21 10 29 01 F1 93 0C 14 10 00 01 00 }
0x3FDF4: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FDFA: 				Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FE00: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x3FE07: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x3FE0E: 			End  { 29 02 }
0x3FE10: 			SuppressIf  { 0A 82 }
0x3FE12: 				EqIdVal QuestionId: 0x2910, Value: 0x0 { 12 06 10 29 00 00 }
0x3FE18: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3FE1F: 				End  { 29 02 }
0x3FE21: 				Text Prompt: "CSM16 Module Version", Help: "CSM16 Module Version", Text: "N/A, reset required" { 03 08 CE 21 CE 21 CF 21 }
0x3FE29: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3FE30: 				End  { 29 02 }
0x3FE32: 				OneOf Prompt: "GateA20 Active", Help: "UPON REQUEST - GA20 can be disabled using BIOS services. ALWAYS - do not allow disabling GA20; this option is useful when any RT code is executed above 1MB.", QuestionFlags: 0x10, QuestionId: 0x5A8, VarStoreId: 0xF101, VarOffset: 0xC98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 21 C9 21 A8 05 01 F1 98 0C 10 10 00 01 00 }
0x3FE43: 					OneOfOption Option: "Upon Request" Value: 0, Default, MfgDefault { 09 07 C7 21 30 00 00 }
0x3FE4A: 					OneOfOption Option: "Always" Value: 1 { 09 07 C8 21 00 00 01 }
0x3FE51: 				End  { 29 02 }
0x3FE53: 				SuppressIf  { 0A 82 }
0x3FE55: 					EqIdVal QuestionId: 0x5AF, Value: 0x2 { 12 86 AF 05 02 00 }
0x3FE5B: 						Not  { 17 02 }
0x3FE5D: 					End  { 29 02 }
0x3FE5F: 					OneOf Prompt: "Option ROM Messages", Help: "Set display mode for Option ROM", QuestionFlags: 0x10, QuestionId: 0x5A9, VarStoreId: 0xF101, VarOffset: 0xC94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 21 BF 21 A9 05 01 F1 94 0C 10 10 00 01 00 }
0x3FE70: 						OneOfOption Option: "Force BIOS" Value: 1, Default, MfgDefault { 09 07 C0 21 30 00 01 }
0x3FE77: 						OneOfOption Option: "Keep Current" Value: 0 { 09 07 C1 21 00 00 00 }
0x3FE7E: 					End  { 29 02 }
0x3FE80: 				End  { 29 02 }
0x3FE82: 				OneOf Prompt: "INT19 Trap Response", Help: "BIOS reaction on INT19 trapping by Option ROM: IMMEDIATE - execute the trap right away; POSTPONED - execute the trap during legacy boot.", QuestionFlags: 0x10, QuestionId: 0x5AA, VarStoreId: 0xF101, VarOffset: 0xC95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 21 C5 21 AA 05 01 F1 95 0C 10 10 00 01 00 }
0x3FE93: 					OneOfOption Option: "Immediate" Value: 1, Default, MfgDefault { 09 07 C3 21 30 00 01 }
0x3FE9A: 					OneOfOption Option: "Postponed" Value: 0 { 09 07 C4 21 00 00 00 }
0x3FEA1: 				End  { 29 02 }
0x3FEA3: 				SuppressIf  { 0A 82 }
0x3FEA5: 					EqIdVal QuestionId: 0x5AC, Value: 0x2 { 12 06 AC 05 02 00 }
0x3FEAB: 					OneOf Prompt: "HDD Connection Order", Help: "Some OS require HDD handles to be adjusted, i.e. OS is installed on drive 80h.", QuestionFlags: 0x10, QuestionId: 0x5AB, VarStoreId: 0xF101, VarOffset: 0xC97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E6 21 E7 21 AB 05 01 F1 97 0C 10 10 00 01 00 }
0x3FEBC: 						OneOfOption Option: "Adjust" Value: 0, Default, MfgDefault { 09 07 E8 21 30 00 00 }
0x3FEC3: 						OneOfOption Option: "Keep" Value: 1 { 09 07 E9 21 00 00 01 }
0x3FECA: 					End  { 29 02 }
0x3FECC: 				End  { 29 02 }
0x3FECE: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3FED5: 				End  { 29 02 }
0x3FED7: 				OneOf Prompt: "Boot option filter", Help: "This option controls Legacy/UEFI ROMs priority", QuestionFlags: 0x10, QuestionId: 0x5AC, VarStoreId: 0xF101, VarOffset: 0xC99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D2 21 D3 21 AC 05 01 F1 99 0C 10 10 00 02 00 }
0x3FEE8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FEEE: 					Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FEF4: 					OneOfOption Option: "UEFI and Legacy" Value: 0 { 09 07 D4 21 00 00 00 }
0x3FEFB: 					OneOfOption Option: "Legacy only" Value: 1 { 09 07 D5 21 00 00 01 }
0x3FF02: 					OneOfOption Option: "UEFI only" Value: 2 { 09 07 D6 21 00 00 02 }
0x3FF09: 				End  { 29 02 }
0x3FF0B: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3FF12: 				End  { 29 02 }
0x3FF14: 				Subtitle Prompt: "Option ROM execution", Help: "", Flags: 0x0 { 02 87 D7 21 00 00 00 }
0x3FF1B: 				End  { 29 02 }
0x3FF1D: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x3FF24: 				End  { 29 02 }
0x3FF26: 				OneOf Prompt: "Network", Help: "Controls the execution of UEFI and Legacy Network OpROM", QuestionFlags: 0x10, QuestionId: 0x5AD, VarStoreId: 0xF101, VarOffset: 0xC9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D8 21 D9 21 AD 05 01 F1 9A 0C 10 10 00 02 00 }
0x3FF37: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x3FF3D: 					Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x3FF43: 					OneOfOption Option: "Do not launch" Value: 0 { 09 07 DE 21 00 00 00 }
0x3FF4A: 					OneOfOption Option: "UEFI" Value: 1 { 09 07 DF 21 00 00 01 }
0x3FF51: 					OneOfOption Option: "Legacy" Value: 2 { 09 07 E0 21 00 00 02 }
0x3FF58: 				End  { 29 02 }
0x3FF5A: 				OneOf Prompt: "Storage", Help: "Controls the execution of UEFI and Legacy Storage OpROM", QuestionFlags: 0x10, QuestionId: 0x5AE, VarStoreId: 0xF101, VarOffset: 0xC9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DA 21 DB 21 AE 05 01 F1 9B 0C 10 10 00 02 00 }
0x3FF6B: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x3FF71: 					Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x3FF77: 					OneOfOption Option: "Do not launch" Value: 0 { 09 07 DE 21 00 00 00 }
0x3FF7E: 					OneOfOption Option: "UEFI" Value: 1 { 09 07 DF 21 00 00 01 }
0x3FF85: 					OneOfOption Option: "Legacy" Value: 2 { 09 07 E0 21 00 00 02 }
0x3FF8C: 				End  { 29 02 }
0x3FF8E: 				OneOf Prompt: "Video", Help: "Controls the execution of UEFI and Legacy Video OpROM", QuestionFlags: 0x10, QuestionId: 0x5AF, VarStoreId: 0xF101, VarOffset: 0xC9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DC 21 DD 21 AF 05 01 F1 9C 0C 10 10 00 02 00 }
0x3FF9F: 					Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x3FFA5: 					Default DefaultId: 0x1 Value: 2 { 5B 06 01 00 00 02 }
0x3FFAB: 					OneOfOption Option: "Do not launch" Value: 0 { 09 07 DE 21 00 00 00 }
0x3FFB2: 					OneOfOption Option: "UEFI" Value: 1 { 09 07 DF 21 00 00 01 }
0x3FFB9: 					OneOfOption Option: "Legacy" Value: 2 { 09 07 E0 21 00 00 02 }
0x3FFC0: 				End  { 29 02 }
0x3FFC2: 				OneOf Prompt: "Other PCI devices", Help: "Determines OpROM execution policy for devices other than Network, Storage, or Video", QuestionFlags: 0x10, QuestionId: 0x5B0, VarStoreId: 0xF101, VarOffset: 0xC9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E1 21 E2 21 B0 05 01 F1 9D 0C 10 10 00 02 00 }
0x3FFD3: 					OneOfOption Option: "Do not launch" Value: 0 { 09 07 DE 21 00 00 00 }
0x3FFDA: 					OneOfOption Option: "UEFI" Value: 1, Default, MfgDefault { 09 07 DF 21 30 00 01 }
0x3FFE1: 					OneOfOption Option: "Legacy" Value: 2 { 09 07 E0 21 00 00 02 }
0x3FFE8: 				End  { 29 02 }
0x3FFEA: 			End  { 29 02 }
0x3FFEC: 		End  { 29 02 }
0x3FFEE: 		SuppressIf  { 0A 82 }
0x3FFF0: 			EqIdVal QuestionId: 0x1108, Value: 0x0 { 12 06 08 11 00 00 }
0x3FFF6: 			Subtitle Prompt: "CSM configuration is disabled.", Help: "", Flags: 0x0 { 02 87 E3 21 00 00 00 }
0x3FFFD: 			End  { 29 02 }
0x3FFFF: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40006: 			End  { 29 02 }
0x40008: 			Subtitle Prompt: "Compatibility Support Module is not loaded", Help: "", Flags: 0x0 { 02 87 E4 21 00 00 00 }
0x4000F: 			End  { 29 02 }
0x40011: 			Subtitle Prompt: "due to active UEFI Secure Boot mode.", Help: "", Flags: 0x0 { 02 87 E5 21 00 00 00 }
0x40018: 			End  { 29 02 }
0x4001A: 		End  { 29 02 }
0x4001C: 	End  { 29 02 }
0x4001E: 	Form FormId: 0x29D4, Title: "SDIO Configuration" { 01 86 D4 29 F0 21 }
0x40024: 		Subtitle Prompt: "SDIO Configuration", Help: "", Flags: 0x0 { 02 87 F0 21 00 00 00 }
0x4002B: 		End  { 29 02 }
0x4002D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40034: 		End  { 29 02 }
0x40036: 		GrayOutIf  { 19 82 }
0x40038: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x4003E: 			OneOf Prompt: "SDIO Access Mode", Help: "Auto Option: Access SD device in DMA mode if controller supports it,otherwise in PIO mode.DMA Option: Access SD device in DMA mode.PIO Option: Access SD device in PIO mode.", QuestionFlags: 0x10, QuestionId: 0x5B1, VarStoreId: 0x29D3, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 0A 22 0B 22 B1 05 D3 29 00 00 10 10 00 03 00 }
0x4004F: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x40056: 				OneOfOption Option: "ADMA" Value: 1 { 09 07 0D 22 00 00 01 }
0x4005D: 				OneOfOption Option: "SDMA" Value: 2 { 09 07 0E 22 00 00 02 }
0x40064: 				OneOfOption Option: "PIO" Value: 3 { 09 07 0F 22 00 00 03 }
0x4006B: 			End  { 29 02 }
0x4006D: 		End  { 29 02 }
0x4006F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40076: 		End  { 29 02 }
0x40078: 		SuppressIf  { 0A 82 }
0x4007A: 			EqIdVal QuestionId: 0x118C, Value: 0x0 { 12 06 8C 11 00 00 }
0x40080: 			Text Prompt: "Mass Storage Devices:", Help: "", Text: "" { 03 08 10 22 02 00 02 00 }
0x40088: 		End  { 29 02 }
0x4008A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40091: 		End  { 29 02 }
0x40093: 		Text Prompt: "", Help: "", Text: "" { 03 08 02 22 02 00 02 00 }
0x4009B: 		Text Prompt: "", Help: "", Text: "" { 03 08 FA 21 02 00 02 00 }
0x400A3: 		SuppressIf  { 0A 82 }
0x400A5: 			EqIdValList QuestionId: 0x118C, Values: [1, 2, 3, 4, 5, 6, 7, 8] { 14 96 8C 11 08 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x400BB: 				Not  { 17 02 }
0x400BD: 			End  { 29 02 }
0x400BF: 			SuppressIf  { 0A 82 }
0x400C1: 				EqIdValList QuestionId: 0x1193, Values: [1] { 14 08 93 11 01 00 01 00 }
0x400C9: 				GrayOutIf  { 19 82 }
0x400CB: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x400D1: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B2, VarStoreId: 0x29D3, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F2 21 11 22 B2 05 D3 29 0A 00 10 10 00 03 00 }
0x400E2: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x400E9: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x400F0: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x400F7: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x400FE: 					End  { 29 02 }
0x40100: 				End  { 29 02 }
0x40102: 			End  { 29 02 }
0x40104: 		End  { 29 02 }
0x40106: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4010D: 		End  { 29 02 }
0x4010F: 		Text Prompt: "", Help: "", Text: "" { 03 08 03 22 02 00 02 00 }
0x40117: 		Text Prompt: "", Help: "", Text: "" { 03 08 FB 21 02 00 02 00 }
0x4011F: 		SuppressIf  { 0A 82 }
0x40121: 			EqIdValList QuestionId: 0x118C, Values: [2, 3, 4, 5, 6, 7, 8] { 14 94 8C 11 07 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x40135: 				Not  { 17 02 }
0x40137: 			End  { 29 02 }
0x40139: 			SuppressIf  { 0A 82 }
0x4013B: 				EqIdValList QuestionId: 0x1192, Values: [1] { 14 08 92 11 01 00 01 00 }
0x40143: 				GrayOutIf  { 19 82 }
0x40145: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x4014B: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B3, VarStoreId: 0x29D3, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F3 21 11 22 B3 05 D3 29 13 00 10 10 00 03 00 }
0x4015C: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x40163: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x4016A: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x40171: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x40178: 					End  { 29 02 }
0x4017A: 				End  { 29 02 }
0x4017C: 			End  { 29 02 }
0x4017E: 		End  { 29 02 }
0x40180: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40187: 		End  { 29 02 }
0x40189: 		Text Prompt: "", Help: "", Text: "" { 03 08 04 22 02 00 02 00 }
0x40191: 		Text Prompt: "", Help: "", Text: "" { 03 08 FC 21 02 00 02 00 }
0x40199: 		SuppressIf  { 0A 82 }
0x4019B: 			EqIdValList QuestionId: 0x118C, Values: [3, 4, 5, 6, 7, 8] { 14 92 8C 11 06 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x401AD: 				Not  { 17 02 }
0x401AF: 			End  { 29 02 }
0x401B1: 			SuppressIf  { 0A 82 }
0x401B3: 				EqIdValList QuestionId: 0x1191, Values: [1] { 14 08 91 11 01 00 01 00 }
0x401BB: 				GrayOutIf  { 19 82 }
0x401BD: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x401C3: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B4, VarStoreId: 0x29D3, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F4 21 11 22 B4 05 D3 29 1C 00 10 10 00 03 00 }
0x401D4: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x401DB: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x401E2: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x401E9: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x401F0: 					End  { 29 02 }
0x401F2: 				End  { 29 02 }
0x401F4: 			End  { 29 02 }
0x401F6: 		End  { 29 02 }
0x401F8: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x401FF: 		End  { 29 02 }
0x40201: 		Text Prompt: "", Help: "", Text: "" { 03 08 05 22 02 00 02 00 }
0x40209: 		Text Prompt: "", Help: "", Text: "" { 03 08 FD 21 02 00 02 00 }
0x40211: 		SuppressIf  { 0A 82 }
0x40213: 			EqIdValList QuestionId: 0x118C, Values: [4, 5, 6, 7, 8] { 14 90 8C 11 05 00 04 00 05 00 06 00 07 00 08 00 }
0x40223: 				Not  { 17 02 }
0x40225: 			End  { 29 02 }
0x40227: 			SuppressIf  { 0A 82 }
0x40229: 				EqIdValList QuestionId: 0x1190, Values: [1] { 14 08 90 11 01 00 01 00 }
0x40231: 				GrayOutIf  { 19 82 }
0x40233: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x40239: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B5, VarStoreId: 0x29D3, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F5 21 11 22 B5 05 D3 29 25 00 10 10 00 03 00 }
0x4024A: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x40251: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x40258: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x4025F: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x40266: 					End  { 29 02 }
0x40268: 				End  { 29 02 }
0x4026A: 			End  { 29 02 }
0x4026C: 		End  { 29 02 }
0x4026E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40275: 		End  { 29 02 }
0x40277: 		Text Prompt: "", Help: "", Text: "" { 03 08 06 22 02 00 02 00 }
0x4027F: 		Text Prompt: "", Help: "", Text: "" { 03 08 FE 21 02 00 02 00 }
0x40287: 		SuppressIf  { 0A 82 }
0x40289: 			EqIdValList QuestionId: 0x118C, Values: [5, 6, 7, 8] { 14 8E 8C 11 04 00 05 00 06 00 07 00 08 00 }
0x40297: 				Not  { 17 02 }
0x40299: 			End  { 29 02 }
0x4029B: 			SuppressIf  { 0A 82 }
0x4029D: 				EqIdValList QuestionId: 0x118F, Values: [1] { 14 08 8F 11 01 00 01 00 }
0x402A5: 				GrayOutIf  { 19 82 }
0x402A7: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x402AD: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B6, VarStoreId: 0x29D3, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F6 21 11 22 B6 05 D3 29 2E 00 10 10 00 03 00 }
0x402BE: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x402C5: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x402CC: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x402D3: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x402DA: 					End  { 29 02 }
0x402DC: 				End  { 29 02 }
0x402DE: 			End  { 29 02 }
0x402E0: 		End  { 29 02 }
0x402E2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x402E9: 		End  { 29 02 }
0x402EB: 		Text Prompt: "", Help: "", Text: "" { 03 08 07 22 02 00 02 00 }
0x402F3: 		Text Prompt: "", Help: "", Text: "" { 03 08 FF 21 02 00 02 00 }
0x402FB: 		SuppressIf  { 0A 82 }
0x402FD: 			EqIdValList QuestionId: 0x118C, Values: [6, 7, 8] { 14 8C 8C 11 03 00 06 00 07 00 08 00 }
0x40309: 				Not  { 17 02 }
0x4030B: 			End  { 29 02 }
0x4030D: 			SuppressIf  { 0A 82 }
0x4030F: 				EqIdValList QuestionId: 0x118E, Values: [1] { 14 08 8E 11 01 00 01 00 }
0x40317: 				GrayOutIf  { 19 82 }
0x40319: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x4031F: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B7, VarStoreId: 0x29D3, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F7 21 11 22 B7 05 D3 29 37 00 10 10 00 03 00 }
0x40330: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x40337: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x4033E: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x40345: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x4034C: 					End  { 29 02 }
0x4034E: 				End  { 29 02 }
0x40350: 			End  { 29 02 }
0x40352: 		End  { 29 02 }
0x40354: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4035B: 		End  { 29 02 }
0x4035D: 		Text Prompt: "", Help: "", Text: "" { 03 08 08 22 02 00 02 00 }
0x40365: 		Text Prompt: "", Help: "", Text: "" { 03 08 00 22 02 00 02 00 }
0x4036D: 		SuppressIf  { 0A 82 }
0x4036F: 			EqIdValList QuestionId: 0x118C, Values: [7, 8] { 14 8A 8C 11 02 00 07 00 08 00 }
0x40379: 				Not  { 17 02 }
0x4037B: 			End  { 29 02 }
0x4037D: 			SuppressIf  { 0A 82 }
0x4037F: 				EqIdValList QuestionId: 0x118D, Values: [1] { 14 08 8D 11 01 00 01 00 }
0x40387: 				GrayOutIf  { 19 82 }
0x40389: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x4038F: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B8, VarStoreId: 0x29D3, VarOffset: 0x40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F8 21 11 22 B8 05 D3 29 40 00 10 10 00 03 00 }
0x403A0: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x403A7: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x403AE: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x403B5: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x403BC: 					End  { 29 02 }
0x403BE: 				End  { 29 02 }
0x403C0: 			End  { 29 02 }
0x403C2: 		End  { 29 02 }
0x403C4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x403CB: 		End  { 29 02 }
0x403CD: 		Text Prompt: "", Help: "", Text: "" { 03 08 09 22 02 00 02 00 }
0x403D5: 		Text Prompt: "", Help: "", Text: "" { 03 08 01 22 02 00 02 00 }
0x403DD: 		SuppressIf  { 0A 82 }
0x403DF: 			EqIdValList QuestionId: 0x118C, Values: [8] { 14 88 8C 11 01 00 08 00 }
0x403E7: 				Not  { 17 02 }
0x403E9: 			End  { 29 02 }
0x403EB: 			SuppressIf  { 0A 82 }
0x403ED: 				EqIdValList QuestionId: 0x118B, Values: [1] { 14 08 8B 11 01 00 01 00 }
0x403F5: 				GrayOutIf  { 19 82 }
0x403F7: 					EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x403FD: 					OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x5B9, VarStoreId: 0x29D3, VarOffset: 0x49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F9 21 11 22 B9 05 D3 29 49 00 10 10 00 03 00 }
0x4040E: 						OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 0C 22 30 00 00 }
0x40415: 						OneOfOption Option: "Floppy" Value: 1 { 09 07 12 22 00 00 01 }
0x4041C: 						OneOfOption Option: "Forced FDD" Value: 2 { 09 07 13 22 00 00 02 }
0x40423: 						OneOfOption Option: "Hard Disk" Value: 3 { 09 07 14 22 00 00 03 }
0x4042A: 					End  { 29 02 }
0x4042C: 				End  { 29 02 }
0x4042E: 			End  { 29 02 }
0x40430: 		End  { 29 02 }
0x40432: 	End  { 29 02 }
0x40434: 	Form FormId: 0x2AE0, Title: "Driver Health" { 01 86 E0 2A 68 00 }
0x4043A: 		SuppressIf  { 0A 82 }
0x4043C: 			EqIdValList QuestionId: 0x118A, Values: [65535] { 14 08 8A 11 01 00 FF FF }
0x40444: 			Ref Prompt: "", Help: "Provides Health Status for the Drivers/Controllers", QuestionFlags: 0x0, QuestionId: 0x5BA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2AE1 { 0F 0F 02 00 69 00 BA 05 00 00 FF FF 00 E1 2A }
0x40453: 		End  { 29 02 }
0x40455: 	End  { 29 02 }
0x40457: 	Form FormId: 0x2AE1, Title: "Driver Health" { 01 86 E1 2A 68 00 }
0x4045D: 		SuppressIf  { 0A 82 }
0x4045F: 			EqIdValList QuestionId: 0x1189, Values: [65535] { 14 08 89 11 01 00 FF FF }
0x40467: 			Ref Prompt: "", Help: "Provides Health Status for the Drivers/Controllers", QuestionFlags: 0x0, QuestionId: 0x5BB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2AE1 { 0F 0F 02 00 69 00 BB 05 00 00 FF FF 00 E1 2A }
0x40476: 		End  { 29 02 }
0x40478: 	End  { 29 02 }
0x4047A: 	Form FormId: 0x2719, Title: "Chipset" { 01 86 19 27 1F 00 }
0x40480: 		Ref Prompt: "System Agent (SA) Configuration", Help: "System Agent (SA) Parameters", QuestionFlags: 0x0, QuestionId: 0x5BC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27AE { 0F 0F CB 07 CC 07 BC 05 00 00 FF FF 00 AE 27 }
0x4048F: 		Ref Prompt: "PCH-IO Configuration", Help: "PCH Parameters", QuestionFlags: 0x0, QuestionId: 0x5BD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x282B { 0F 0F 2B 11 2C 11 BD 05 00 00 FF FF 00 2B 28 }
0x4049E: 	End  { 29 02 }
0x404A0: 	Form FormId: 0x27A9, Title: "PCI Express Root Port 0" { 01 86 A9 27 B4 0F }
0x404A6: 		OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x5BE, VarStoreId: 0x4, VarOffset: 0xC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 0F BD 0F BE 05 04 00 C6 00 10 10 00 01 00 }
0x404B7: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x404BE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x404C5: 		End  { 29 02 }
0x404C7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x404CE: 		End  { 29 02 }
0x404D0: 		Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 BE 0F 00 00 00 }
0x404D7: 		End  { 29 02 }
0x404D9: 		OneOf Prompt: "LTR", Help: "PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x5BF, VarStoreId: 0x4, VarOffset: 0xCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 0F C3 0F BF 05 04 00 CA 00 10 10 00 01 00 }
0x404EA: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x404F1: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x404F8: 		End  { 29 02 }
0x404FA: 		SuppressIf  { 0A 82 }
0x404FC: 			EqIdVal QuestionId: 0x5BF, Value: 0x0 { 12 06 BF 05 00 00 }
0x40502: 			OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5C0, VarStoreId: 0x4, VarOffset: 0xCE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 0F CA 0F C0 05 04 00 CE 00 10 10 00 01 00 }
0x40513: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4051A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40521: 			End  { 29 02 }
0x40523: 			SuppressIf  { 0A 82 }
0x40525: 				EqIdVal QuestionId: 0x5C0, Value: 0x1 { 12 86 C0 05 01 00 }
0x4052B: 					Not  { 17 02 }
0x4052D: 				End  { 29 02 }
0x4052F: 				Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5C1, VarStoreId: 0x4, VarOffset: 0xD6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 C6 0F CD 0F C1 05 04 00 D6 00 10 11 00 00 FF 03 01 00 }
0x40543: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x4054A: 				End  { 29 02 }
0x4054C: 				OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5C2, VarStoreId: 0x4, VarOffset: 0xD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C7 0F CC 0F C2 05 04 00 D2 00 10 10 00 05 00 }
0x4055D: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x40564: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4056B: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x40572: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x40579: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x40580: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x40587: 				End  { 29 02 }
0x40589: 			End  { 29 02 }
0x4058B: 			OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5C3, VarStoreId: 0x4, VarOffset: 0xDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 0F CB 0F C3 05 04 00 DE 00 10 10 00 01 00 }
0x4059C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x405A3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x405AA: 			End  { 29 02 }
0x405AC: 			SuppressIf  { 0A 82 }
0x405AE: 				EqIdVal QuestionId: 0x5C3, Value: 0x1 { 12 86 C3 05 01 00 }
0x405B4: 					Not  { 17 02 }
0x405B6: 				End  { 29 02 }
0x405B8: 				Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x5C4, VarStoreId: 0x4, VarOffset: 0xE6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 C8 0F CE 0F C4 05 04 00 E6 00 10 11 00 00 FF 03 01 00 }
0x405CC: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x405D3: 				End  { 29 02 }
0x405D5: 				OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5C5, VarStoreId: 0x4, VarOffset: 0xE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C9 0F CF 0F C5 05 04 00 E2 00 10 10 00 05 00 }
0x405E6: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x405ED: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x405F4: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x405FB: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x40602: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x40609: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x40610: 				End  { 29 02 }
0x40612: 			End  { 29 02 }
0x40614: 			OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for ITBT PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x5C6, VarStoreId: 0x4, VarOffset: 0xEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 0F E6 0F C6 05 04 00 EE 00 10 10 00 01 00 }
0x40625: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x4062C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x40633: 			End  { 29 02 }
0x40635: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x5C7, VarStoreId: 0x4, VarOffset: 0xF2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E7 0F EB 0F C7 05 04 00 F2 00 10 10 00 01 00 }
0x40646: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4064D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x40654: 			End  { 29 02 }
0x40656: 		End  { 29 02 }
0x40658: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4065F: 		End  { 29 02 }
0x40661: 	End  { 29 02 }
0x40663: 	Form FormId: 0x27AA, Title: "PCI Express Root Port 1" { 01 86 AA 27 B5 0F }
0x40669: 		OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x5C8, VarStoreId: 0x4, VarOffset: 0xC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 0F BD 0F C8 05 04 00 C7 00 10 10 00 01 00 }
0x4067A: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40681: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40688: 		End  { 29 02 }
0x4068A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40691: 		End  { 29 02 }
0x40693: 		Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 BE 0F 00 00 00 }
0x4069A: 		End  { 29 02 }
0x4069C: 		OneOf Prompt: "LTR", Help: "PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x5C9, VarStoreId: 0x4, VarOffset: 0xCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 0F C3 0F C9 05 04 00 CB 00 10 10 00 01 00 }
0x406AD: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x406B4: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x406BB: 		End  { 29 02 }
0x406BD: 		SuppressIf  { 0A 82 }
0x406BF: 			EqIdVal QuestionId: 0x5C9, Value: 0x0 { 12 06 C9 05 00 00 }
0x406C5: 			OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5CA, VarStoreId: 0x4, VarOffset: 0xCF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 0F CA 0F CA 05 04 00 CF 00 10 10 00 01 00 }
0x406D6: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x406DD: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x406E4: 			End  { 29 02 }
0x406E6: 			SuppressIf  { 0A 82 }
0x406E8: 				EqIdVal QuestionId: 0x5CA, Value: 0x1 { 12 86 CA 05 01 00 }
0x406EE: 					Not  { 17 02 }
0x406F0: 				End  { 29 02 }
0x406F2: 				Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5CB, VarStoreId: 0x4, VarOffset: 0xD8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D2 0F CD 0F CB 05 04 00 D8 00 10 11 00 00 FF 03 01 00 }
0x40706: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x4070D: 				End  { 29 02 }
0x4070F: 				OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5CC, VarStoreId: 0x4, VarOffset: 0xD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 D3 0F CC 0F CC 05 04 00 D3 00 10 10 00 05 00 }
0x40720: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x40727: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4072E: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x40735: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x4073C: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x40743: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x4074A: 				End  { 29 02 }
0x4074C: 			End  { 29 02 }
0x4074E: 			OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5CD, VarStoreId: 0x4, VarOffset: 0xDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 0F CB 0F CD 05 04 00 DF 00 10 10 00 01 00 }
0x4075F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40766: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4076D: 			End  { 29 02 }
0x4076F: 			SuppressIf  { 0A 82 }
0x40771: 				EqIdVal QuestionId: 0x5CD, Value: 0x1 { 12 86 CD 05 01 00 }
0x40777: 					Not  { 17 02 }
0x40779: 				End  { 29 02 }
0x4077B: 				Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x5CE, VarStoreId: 0x4, VarOffset: 0xE8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D4 0F CE 0F CE 05 04 00 E8 00 10 11 00 00 FF 03 01 00 }
0x4078F: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x40796: 				End  { 29 02 }
0x40798: 				OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5CF, VarStoreId: 0x4, VarOffset: 0xE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 D5 0F CF 0F CF 05 04 00 E3 00 10 10 00 05 00 }
0x407A9: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x407B0: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x407B7: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x407BE: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x407C5: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x407CC: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x407D3: 				End  { 29 02 }
0x407D5: 			End  { 29 02 }
0x407D7: 			OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for ITBT PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x5D0, VarStoreId: 0x4, VarOffset: 0xEF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 0F E6 0F D0 05 04 00 EF 00 10 10 00 01 00 }
0x407E8: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x407EF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x407F6: 			End  { 29 02 }
0x407F8: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x5D1, VarStoreId: 0x4, VarOffset: 0xF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 0F EB 0F D1 05 04 00 F3 00 10 10 00 01 00 }
0x40809: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x40810: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x40817: 			End  { 29 02 }
0x40819: 		End  { 29 02 }
0x4081B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40822: 		End  { 29 02 }
0x40824: 	End  { 29 02 }
0x40826: 	Form FormId: 0x27AB, Title: "PCI Express Root Port 2" { 01 86 AB 27 B6 0F }
0x4082C: 		OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x5D2, VarStoreId: 0x4, VarOffset: 0xC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 0F BD 0F D2 05 04 00 C8 00 10 10 00 01 00 }
0x4083D: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40844: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4084B: 		End  { 29 02 }
0x4084D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40854: 		End  { 29 02 }
0x40856: 		Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 BE 0F 00 00 00 }
0x4085D: 		End  { 29 02 }
0x4085F: 		OneOf Prompt: "LTR", Help: "PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x5D3, VarStoreId: 0x4, VarOffset: 0xCC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 0F C3 0F D3 05 04 00 CC 00 10 10 00 01 00 }
0x40870: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40877: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4087E: 		End  { 29 02 }
0x40880: 		SuppressIf  { 0A 82 }
0x40882: 			EqIdVal QuestionId: 0x5D3, Value: 0x0 { 12 06 D3 05 00 00 }
0x40888: 			OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5D4, VarStoreId: 0x4, VarOffset: 0xD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 0F CA 0F D4 05 04 00 D0 00 10 10 00 01 00 }
0x40899: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x408A0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x408A7: 			End  { 29 02 }
0x408A9: 			SuppressIf  { 0A 82 }
0x408AB: 				EqIdVal QuestionId: 0x5D4, Value: 0x1 { 12 86 D4 05 01 00 }
0x408B1: 					Not  { 17 02 }
0x408B3: 				End  { 29 02 }
0x408B5: 				Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5D5, VarStoreId: 0x4, VarOffset: 0xDA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D8 0F CD 0F D5 05 04 00 DA 00 10 11 00 00 FF 03 01 00 }
0x408C9: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x408D0: 				End  { 29 02 }
0x408D2: 				OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5D6, VarStoreId: 0x4, VarOffset: 0xD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 D9 0F CC 0F D6 05 04 00 D4 00 10 10 00 05 00 }
0x408E3: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x408EA: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x408F1: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x408F8: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x408FF: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x40906: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x4090D: 				End  { 29 02 }
0x4090F: 			End  { 29 02 }
0x40911: 			OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5D7, VarStoreId: 0x4, VarOffset: 0xE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D7 0F CB 0F D7 05 04 00 E0 00 10 10 00 01 00 }
0x40922: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40929: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40930: 			End  { 29 02 }
0x40932: 			SuppressIf  { 0A 82 }
0x40934: 				EqIdVal QuestionId: 0x5D7, Value: 0x1 { 12 86 D7 05 01 00 }
0x4093A: 					Not  { 17 02 }
0x4093C: 				End  { 29 02 }
0x4093E: 				Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x5D8, VarStoreId: 0x4, VarOffset: 0xEA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 DA 0F CE 0F D8 05 04 00 EA 00 10 11 00 00 FF 03 01 00 }
0x40952: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x40959: 				End  { 29 02 }
0x4095B: 				OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5D9, VarStoreId: 0x4, VarOffset: 0xE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 DB 0F CF 0F D9 05 04 00 E4 00 10 10 00 05 00 }
0x4096C: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x40973: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4097A: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x40981: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x40988: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x4098F: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x40996: 				End  { 29 02 }
0x40998: 			End  { 29 02 }
0x4099A: 			OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for ITBT PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x5DA, VarStoreId: 0x4, VarOffset: 0xF0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 0F E6 0F DA 05 04 00 F0 00 10 10 00 01 00 }
0x409AB: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x409B2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x409B9: 			End  { 29 02 }
0x409BB: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x5DB, VarStoreId: 0x4, VarOffset: 0xF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 0F EB 0F DB 05 04 00 F4 00 10 10 00 01 00 }
0x409CC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x409D3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x409DA: 			End  { 29 02 }
0x409DC: 		End  { 29 02 }
0x409DE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x409E5: 		End  { 29 02 }
0x409E7: 	End  { 29 02 }
0x409E9: 	Form FormId: 0x27AC, Title: "PCI Express Root Port 3" { 01 86 AC 27 B7 0F }
0x409EF: 		OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x5DC, VarStoreId: 0x4, VarOffset: 0xC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 0F BD 0F DC 05 04 00 C9 00 10 10 00 01 00 }
0x40A00: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40A07: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40A0E: 		End  { 29 02 }
0x40A10: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40A17: 		End  { 29 02 }
0x40A19: 		Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 BE 0F 00 00 00 }
0x40A20: 		End  { 29 02 }
0x40A22: 		OneOf Prompt: "LTR", Help: "PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x5DD, VarStoreId: 0x4, VarOffset: 0xCD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 0F C3 0F DD 05 04 00 CD 00 10 10 00 01 00 }
0x40A33: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40A3A: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40A41: 		End  { 29 02 }
0x40A43: 		SuppressIf  { 0A 82 }
0x40A45: 			EqIdVal QuestionId: 0x5DD, Value: 0x0 { 12 06 DD 05 00 00 }
0x40A4B: 			OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5DE, VarStoreId: 0x4, VarOffset: 0xD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 0F CA 0F DE 05 04 00 D1 00 10 10 00 01 00 }
0x40A5C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40A63: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40A6A: 			End  { 29 02 }
0x40A6C: 			SuppressIf  { 0A 82 }
0x40A6E: 				EqIdVal QuestionId: 0x5DE, Value: 0x1 { 12 86 DE 05 01 00 }
0x40A74: 					Not  { 17 02 }
0x40A76: 				End  { 29 02 }
0x40A78: 				Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5DF, VarStoreId: 0x4, VarOffset: 0xDC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 DE 0F CD 0F DF 05 04 00 DC 00 10 11 00 00 FF 03 01 00 }
0x40A8C: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x40A93: 				End  { 29 02 }
0x40A95: 				OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5E0, VarStoreId: 0x4, VarOffset: 0xD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 DF 0F CC 0F E0 05 04 00 D5 00 10 10 00 05 00 }
0x40AA6: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x40AAD: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x40AB4: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x40ABB: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x40AC2: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x40AC9: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x40AD0: 				End  { 29 02 }
0x40AD2: 			End  { 29 02 }
0x40AD4: 			OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x5E1, VarStoreId: 0x4, VarOffset: 0xE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DD 0F CB 0F E1 05 04 00 E1 00 10 10 00 01 00 }
0x40AE5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x40AEC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x40AF3: 			End  { 29 02 }
0x40AF5: 			SuppressIf  { 0A 82 }
0x40AF7: 				EqIdVal QuestionId: 0x5E1, Value: 0x1 { 12 86 E1 05 01 00 }
0x40AFD: 					Not  { 17 02 }
0x40AFF: 				End  { 29 02 }
0x40B01: 				Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x5E2, VarStoreId: 0x4, VarOffset: 0xEC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 E0 0F CE 0F E2 05 04 00 EC 00 10 11 00 00 FF 03 01 00 }
0x40B15: 					Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x40B1C: 				End  { 29 02 }
0x40B1E: 				OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0x5E3, VarStoreId: 0x4, VarOffset: 0xE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 E1 0F CF 0F E3 05 04 00 E5 00 10 10 00 05 00 }
0x40B2F: 					OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x40B36: 					OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x40B3D: 					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x40B44: 					OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x40B4B: 					OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x40B52: 					OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x40B59: 				End  { 29 02 }
0x40B5B: 			End  { 29 02 }
0x40B5D: 			OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for ITBT PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x5E4, VarStoreId: 0x4, VarOffset: 0xF1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E5 0F E6 0F E4 05 04 00 F1 00 10 10 00 01 00 }
0x40B6E: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x40B75: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x40B7C: 			End  { 29 02 }
0x40B7E: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x5E5, VarStoreId: 0x4, VarOffset: 0xF5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 0F EB 0F E5 05 04 00 F5 00 10 10 00 01 00 }
0x40B8F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x40B96: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x40B9D: 			End  { 29 02 }
0x40B9F: 		End  { 29 02 }
0x40BA1: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40BA8: 		End  { 29 02 }
0x40BAA: 	End  { 29 02 }
0x40BAC: 	Form FormId: 0x27AD, Title: "Memory Configuration" { 01 86 AD 27 CD 07 }
0x40BB2: 		Ref Prompt: "Memory Thermal Configuration", Help: "Memory Thermal Configuration Options", QuestionFlags: 0x0, QuestionId: 0x5E6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BC { 0F 0F A6 08 A7 08 E6 05 00 00 FF FF 00 BC 27 }
0x40BC1: 		Ref Prompt: "Memory Training Algorithms", Help: "Enable/Disable Memory Training Algorithms.", QuestionFlags: 0x0, QuestionId: 0x5E7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BA { 0F 0F 65 09 66 09 E7 05 00 00 FF FF 00 BA 27 }
0x40BD0: 		SuppressIf  { 0A 82 }
0x40BD2: 			EqIdVal QuestionId: 0x1188, Value: 0x1 { 12 06 88 11 01 00 }
0x40BD8: 			Ref Prompt: "Memory", Help: "Memory Overclocking Menu", QuestionFlags: 0x0, QuestionId: 0x5E8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27AF { 0F 0F A8 08 A9 08 E8 05 00 00 FF FF 00 AF 27 }
0x40BE7: 		End  { 29 02 }
0x40BE9: 		Subtitle Prompt: "Memory Configuration", Help: "", Flags: 0x0 { 02 87 CD 07 00 00 00 }
0x40BF0: 		End  { 29 02 }
0x40BF2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40BF9: 		End  { 29 02 }
0x40BFB: 		Text Prompt: "Memory RC Version", Help: "Memory RC Version", Text: "N/A" { 03 08 E7 07 E6 07 E8 07 }
0x40C03: 		Text Prompt: "Memory Frequency", Help: "Displays the Frequency of Memory", Text: "N/A" { 03 08 EA 07 E9 07 EB 07 }
0x40C0B: 		Text Prompt: "tCL-tRCD-tRP-tRAS", Help: "Memory Timings", Text: "N/A" { 03 08 ED 07 EC 07 EE 07 }
0x40C13: 		Text Prompt: "MC 0 Ch 0 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F0 07 EF 07 00 08 }
0x40C1B: 		SuppressIf  { 0A 82 }
0x40C1D: 			EqIdVal QuestionId: 0x1187, Value: 0x0 { 12 06 87 11 00 00 }
0x40C23: 			Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 12 08 }
0x40C2B: 			Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 24 08 }
0x40C33: 			Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 36 08 }
0x40C3B: 		End  { 29 02 }
0x40C3D: 		SuppressIf  { 0A 82 }
0x40C3F: 			EqIdValList QuestionId: 0x1177, Values: [2, 3] { 14 0A 77 11 02 00 02 00 03 00 }
0x40C49: 			Text Prompt: "MC 0 Ch 0 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F1 07 EF 07 01 08 }
0x40C51: 			SuppressIf  { 0A 82 }
0x40C53: 				EqIdVal QuestionId: 0x1186, Value: 0x0 { 12 06 86 11 00 00 }
0x40C59: 				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 13 08 }
0x40C61: 				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 25 08 }
0x40C69: 				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 37 08 }
0x40C71: 			End  { 29 02 }
0x40C73: 		End  { 29 02 }
0x40C75: 		SuppressIf  { 0A 82 }
0x40C77: 			EqIdValList QuestionId: 0x1177, Values: [0, 1] { 14 0A 77 11 02 00 00 00 01 00 }
0x40C81: 			Text Prompt: "MC 0 Ch 1 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F2 07 EF 07 02 08 }
0x40C89: 			SuppressIf  { 0A 82 }
0x40C8B: 				EqIdVal QuestionId: 0x1185, Value: 0x0 { 12 06 85 11 00 00 }
0x40C91: 				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 14 08 }
0x40C99: 				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 26 08 }
0x40CA1: 				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 38 08 }
0x40CA9: 			End  { 29 02 }
0x40CAB: 			SuppressIf  { 0A 82 }
0x40CAD: 				EqIdValList QuestionId: 0x1177, Values: [0, 1, 2, 3] { 14 0E 77 11 04 00 00 00 01 00 02 00 03 00 }
0x40CBB: 				Text Prompt: "MC 0 Ch 1 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F3 07 EF 07 03 08 }
0x40CC3: 				SuppressIf  { 0A 82 }
0x40CC5: 					EqIdVal QuestionId: 0x1184, Value: 0x0 { 12 06 84 11 00 00 }
0x40CCB: 					Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 15 08 }
0x40CD3: 					Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 27 08 }
0x40CDB: 					Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 39 08 }
0x40CE3: 				End  { 29 02 }
0x40CE5: 			End  { 29 02 }
0x40CE7: 			SuppressIf  { 0A 82 }
0x40CE9: 				EqIdValList QuestionId: 0x1177, Values: [0, 1] { 14 0A 77 11 02 00 00 00 01 00 }
0x40CF3: 				Text Prompt: "MC 0 Ch 2 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F4 07 EF 07 04 08 }
0x40CFB: 				SuppressIf  { 0A 82 }
0x40CFD: 					EqIdVal QuestionId: 0x1183, Value: 0x0 { 12 06 83 11 00 00 }
0x40D03: 					Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 16 08 }
0x40D0B: 					Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 28 08 }
0x40D13: 					Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 3A 08 }
0x40D1B: 				End  { 29 02 }
0x40D1D: 				SuppressIf  { 0A 82 }
0x40D1F: 					EqIdValList QuestionId: 0x1177, Values: [0, 1, 2, 3] { 14 0E 77 11 04 00 00 00 01 00 02 00 03 00 }
0x40D2D: 					Text Prompt: "MC 0 Ch 2 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F5 07 EF 07 05 08 }
0x40D35: 					SuppressIf  { 0A 82 }
0x40D37: 						EqIdVal QuestionId: 0x1182, Value: 0x0 { 12 06 82 11 00 00 }
0x40D3D: 						Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 17 08 }
0x40D45: 						Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 29 08 }
0x40D4D: 						Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 3B 08 }
0x40D55: 					End  { 29 02 }
0x40D57: 				End  { 29 02 }
0x40D59: 				Text Prompt: "MC 0 Ch 3 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F6 07 EF 07 06 08 }
0x40D61: 				SuppressIf  { 0A 82 }
0x40D63: 					EqIdVal QuestionId: 0x1181, Value: 0x0 { 12 06 81 11 00 00 }
0x40D69: 					Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 18 08 }
0x40D71: 					Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 2A 08 }
0x40D79: 					Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 3C 08 }
0x40D81: 				End  { 29 02 }
0x40D83: 				SuppressIf  { 0A 82 }
0x40D85: 					EqIdValList QuestionId: 0x1177, Values: [0, 1, 2, 3] { 14 0E 77 11 04 00 00 00 01 00 02 00 03 00 }
0x40D93: 					Text Prompt: "MC 0 Ch 3 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F7 07 EF 07 07 08 }
0x40D9B: 					SuppressIf  { 0A 82 }
0x40D9D: 						EqIdVal QuestionId: 0x1180, Value: 0x0 { 12 06 80 11 00 00 }
0x40DA3: 						Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 19 08 }
0x40DAB: 						Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 2B 08 }
0x40DB3: 						Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 3D 08 }
0x40DBB: 					End  { 29 02 }
0x40DBD: 				End  { 29 02 }
0x40DBF: 			End  { 29 02 }
0x40DC1: 		End  { 29 02 }
0x40DC3: 		Text Prompt: "MC 1 Ch 0 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F8 07 EF 07 08 08 }
0x40DCB: 		SuppressIf  { 0A 82 }
0x40DCD: 			EqIdVal QuestionId: 0x117F, Value: 0x0 { 12 06 7F 11 00 00 }
0x40DD3: 			Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 1A 08 }
0x40DDB: 			Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 2C 08 }
0x40DE3: 			Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 3E 08 }
0x40DEB: 		End  { 29 02 }
0x40DED: 		SuppressIf  { 0A 82 }
0x40DEF: 			EqIdValList QuestionId: 0x1177, Values: [2, 3] { 14 0A 77 11 02 00 02 00 03 00 }
0x40DF9: 			Text Prompt: "MC 1 Ch 0 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 F9 07 EF 07 09 08 }
0x40E01: 			SuppressIf  { 0A 82 }
0x40E03: 				EqIdVal QuestionId: 0x117E, Value: 0x0 { 12 06 7E 11 00 00 }
0x40E09: 				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 1B 08 }
0x40E11: 				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 2D 08 }
0x40E19: 				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 3F 08 }
0x40E21: 			End  { 29 02 }
0x40E23: 		End  { 29 02 }
0x40E25: 		SuppressIf  { 0A 82 }
0x40E27: 			EqIdValList QuestionId: 0x1177, Values: [0, 1] { 14 0A 77 11 02 00 00 00 01 00 }
0x40E31: 			Text Prompt: "MC 1 Ch 1 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 FA 07 EF 07 0A 08 }
0x40E39: 			SuppressIf  { 0A 82 }
0x40E3B: 				EqIdVal QuestionId: 0x117D, Value: 0x0 { 12 06 7D 11 00 00 }
0x40E41: 				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 1C 08 }
0x40E49: 				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 2E 08 }
0x40E51: 				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 40 08 }
0x40E59: 			End  { 29 02 }
0x40E5B: 			SuppressIf  { 0A 82 }
0x40E5D: 				EqIdValList QuestionId: 0x1177, Values: [0, 1, 2, 3] { 14 0E 77 11 04 00 00 00 01 00 02 00 03 00 }
0x40E6B: 				Text Prompt: "MC 1 Ch 1 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 FB 07 EF 07 0B 08 }
0x40E73: 				SuppressIf  { 0A 82 }
0x40E75: 					EqIdVal QuestionId: 0x117C, Value: 0x0 { 12 06 7C 11 00 00 }
0x40E7B: 					Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 1D 08 }
0x40E83: 					Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 2F 08 }
0x40E8B: 					Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 41 08 }
0x40E93: 				End  { 29 02 }
0x40E95: 			End  { 29 02 }
0x40E97: 			SuppressIf  { 0A 82 }
0x40E99: 				EqIdValList QuestionId: 0x1177, Values: [0, 1] { 14 0A 77 11 02 00 00 00 01 00 }
0x40EA3: 				Text Prompt: "MC 1 Ch 2 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 FC 07 EF 07 0C 08 }
0x40EAB: 				SuppressIf  { 0A 82 }
0x40EAD: 					EqIdVal QuestionId: 0x117B, Value: 0x0 { 12 06 7B 11 00 00 }
0x40EB3: 					Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 1E 08 }
0x40EBB: 					Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 30 08 }
0x40EC3: 					Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 42 08 }
0x40ECB: 				End  { 29 02 }
0x40ECD: 				SuppressIf  { 0A 82 }
0x40ECF: 					EqIdValList QuestionId: 0x1177, Values: [0, 1, 2, 3] { 14 0E 77 11 04 00 00 00 01 00 02 00 03 00 }
0x40EDD: 					Text Prompt: "MC 1 Ch 2 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 FD 07 EF 07 0D 08 }
0x40EE5: 					SuppressIf  { 0A 82 }
0x40EE7: 						EqIdVal QuestionId: 0x117A, Value: 0x0 { 12 06 7A 11 00 00 }
0x40EED: 						Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 1F 08 }
0x40EF5: 						Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 31 08 }
0x40EFD: 						Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 43 08 }
0x40F05: 					End  { 29 02 }
0x40F07: 				End  { 29 02 }
0x40F09: 				Text Prompt: "MC 1 Ch 3 DIMM 0", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 FE 07 EF 07 0E 08 }
0x40F11: 				SuppressIf  { 0A 82 }
0x40F13: 					EqIdVal QuestionId: 0x1179, Value: 0x0 { 12 06 79 11 00 00 }
0x40F19: 					Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 20 08 }
0x40F21: 					Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 32 08 }
0x40F29: 					Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 44 08 }
0x40F31: 				End  { 29 02 }
0x40F33: 				SuppressIf  { 0A 82 }
0x40F35: 					EqIdValList QuestionId: 0x1177, Values: [0, 1, 2, 3] { 14 0E 77 11 04 00 00 00 01 00 02 00 03 00 }
0x40F43: 					Text Prompt: "MC 1 Ch 3 DIMM 1", Help: "Controller Channel Slot Subtitle", Text: "N/A" { 03 08 FF 07 EF 07 0F 08 }
0x40F4B: 					SuppressIf  { 0A 82 }
0x40F4D: 						EqIdVal QuestionId: 0x1178, Value: 0x0 { 12 06 78 11 00 00 }
0x40F53: 						Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A" { 03 08 11 08 10 08 21 08 }
0x40F5B: 						Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A" { 03 08 23 08 22 08 33 08 }
0x40F63: 						Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown" { 03 08 35 08 34 08 45 08 }
0x40F6B: 					End  { 29 02 }
0x40F6D: 				End  { 29 02 }
0x40F6F: 			End  { 29 02 }
0x40F71: 		End  { 29 02 }
0x40F73: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x40F7A: 		End  { 29 02 }
0x40F7C: 		Numeric Prompt: "Debug Value", Help: "Debug Value", QuestionFlags: 0x10, QuestionId: 0x5E9, VarStoreId: 0x4, VarOffset: 0x427, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A D4 07 D5 07 E9 05 04 00 27 04 10 12 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x40F96: 			Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x40F9F: 		End  { 29 02 }
0x40FA1: 		OneOf Prompt: "MRC ULT Safe Config", Help: "MRC ULT Safe Config for PO", QuestionFlags: 0x10, QuestionId: 0x5EA, VarStoreId: 0x4, VarOffset: 0x23C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 0A 7B 0A EA 05 04 00 3C 02 10 10 00 01 00 }
0x40FB2: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x40FB9: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x40FC0: 		End  { 29 02 }
0x40FC2: 		OneOf Prompt: "LPDDR DqDqs Re-Training", Help: "Disable/Enable LPDDR DqDqs Re Training", QuestionFlags: 0x10, QuestionId: 0x5EB, VarStoreId: 0x4, VarOffset: 0x23D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7C 0A 7D 0A EB 05 04 00 3D 02 10 10 00 01 00 }
0x40FD3: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x40FDA: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x40FE1: 		End  { 29 02 }
0x40FE3: 		OneOf Prompt: "Safe Mode Support", Help: "Safe Mode enable support. Option will be used for changes/WAs that may affect an stable MRC", QuestionFlags: 0x10, QuestionId: 0x5EC, VarStoreId: 0x4, VarOffset: 0x19E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8D 08 8E 08 EC 05 04 00 9E 01 10 10 00 01 00 }
0x40FF4: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x40FFB: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41002: 		End  { 29 02 }
0x41004: 		OneOf Prompt: "Memory Test on Warm Boot", Help: "Enable Or Disable Base Memory Test Run on Warm Boot", QuestionFlags: 0x10, QuestionId: 0x5ED, VarStoreId: 0x4, VarOffset: 0x1A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 08 90 08 ED 05 04 00 A1 01 10 10 00 01 00 }
0x41015: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x4101C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x41023: 		End  { 29 02 }
0x41025: 		OneOf Prompt: "Maximum Memory Frequency", Help: "Maximum Memory Frequency Selections in Mhz.", QuestionFlags: 0x10, QuestionId: 0x5EE, VarStoreId: 0x4, VarOffset: 0x18B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3200, Step: 0x0 { 05 94 8C 0A 8D 0A EE 05 04 00 8B 01 10 11 00 00 00 32 00 00 }
0x41039: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x41040: 			OneOfOption Option: "Auto" Value: 0 { 09 08 90 00 01 01 00 00 }
0x41048: 			OneOfOption Option: "1067" Value: 1067 { 09 08 8E 0A 01 01 2B 04 }
0x41050: 			OneOfOption Option: "1333" Value: 1333 { 09 08 8F 0A 01 01 35 05 }
0x41058: 			OneOfOption Option: "1400" Value: 1400 { 09 08 90 0A 01 01 78 05 }
0x41060: 			OneOfOption Option: "1600" Value: 1600 { 09 08 91 0A 01 01 40 06 }
0x41068: 			OneOfOption Option: "1800" Value: 1800 { 09 08 92 0A 01 01 08 07 }
0x41070: 			OneOfOption Option: "1867" Value: 1867 { 09 08 93 0A 01 01 4B 07 }
0x41078: 			OneOfOption Option: "2000" Value: 2000 { 09 08 94 0A 01 01 D0 07 }
0x41080: 			OneOfOption Option: "2133" Value: 2133 { 09 08 95 0A 01 01 55 08 }
0x41088: 			OneOfOption Option: "2200" Value: 2200 { 09 08 96 0A 01 01 98 08 }
0x41090: 			OneOfOption Option: "2400" Value: 2400 { 09 08 97 0A 01 01 60 09 }
0x41098: 			OneOfOption Option: "2600" Value: 2600 { 09 08 98 0A 01 01 28 0A }
0x410A0: 			OneOfOption Option: "2667" Value: 2667 { 09 08 99 0A 01 01 6B 0A }
0x410A8: 			OneOfOption Option: "2800" Value: 2800 { 09 08 9A 0A 01 01 F0 0A }
0x410B0: 			OneOfOption Option: "2933" Value: 2933 { 09 08 9B 0A 01 01 75 0B }
0x410B8: 			OneOfOption Option: "3000" Value: 3000 { 09 08 9C 0A 01 01 B8 0B }
0x410C0: 			OneOfOption Option: "3200" Value: 3200 { 09 08 9D 0A 01 01 80 0C }
0x410C8: 			OneOfOption Option: "3467" Value: 3467 { 09 08 9E 0A 01 01 8B 0D }
0x410D0: 			OneOfOption Option: "3600" Value: 3600 { 09 08 9F 0A 01 01 10 0E }
0x410D8: 			OneOfOption Option: "3733" Value: 3733 { 09 08 A0 0A 01 01 95 0E }
0x410E0: 			OneOfOption Option: "4000" Value: 4000 { 09 08 A1 0A 01 01 A0 0F }
0x410E8: 			OneOfOption Option: "4200" Value: 4200 { 09 08 A2 0A 01 01 68 10 }
0x410F0: 			OneOfOption Option: "4267" Value: 4267 { 09 08 A3 0A 01 01 AB 10 }
0x410F8: 			OneOfOption Option: "4400" Value: 4400 { 09 08 A4 0A 01 01 30 11 }
0x41100: 			OneOfOption Option: "4600" Value: 4600 { 09 08 A5 0A 01 01 F8 11 }
0x41108: 			OneOfOption Option: "4800" Value: 4800 { 09 08 A6 0A 01 01 C0 12 }
0x41110: 			OneOfOption Option: "5000" Value: 5000 { 09 08 A7 0A 01 01 88 13 }
0x41118: 			OneOfOption Option: "5200" Value: 5200 { 09 08 A8 0A 01 01 50 14 }
0x41120: 			OneOfOption Option: "5400" Value: 5400 { 09 08 A9 0A 01 01 18 15 }
0x41128: 			OneOfOption Option: "5600" Value: 5600 { 09 08 AA 0A 01 01 E0 15 }
0x41130: 			OneOfOption Option: "5800" Value: 5800 { 09 08 AB 0A 01 01 A8 16 }
0x41138: 			OneOfOption Option: "6000" Value: 6000 { 09 08 AC 0A 01 01 70 17 }
0x41140: 			OneOfOption Option: "6200" Value: 6200 { 09 08 AD 0A 01 01 38 18 }
0x41148: 			OneOfOption Option: "6400" Value: 6400 { 09 08 AE 0A 01 01 00 19 }
0x41150: 			OneOfOption Option: "6600" Value: 6600 { 09 08 AF 0A 01 01 C8 19 }
0x41158: 			OneOfOption Option: "6800" Value: 6800 { 09 08 B0 0A 01 01 90 1A }
0x41160: 			OneOfOption Option: "7000" Value: 7000 { 09 08 B1 0A 01 01 58 1B }
0x41168: 			OneOfOption Option: "7200" Value: 7200 { 09 08 B2 0A 01 01 20 1C }
0x41170: 			OneOfOption Option: "7400" Value: 7400 { 09 08 B3 0A 01 01 E8 1C }
0x41178: 			OneOfOption Option: "7600" Value: 7600 { 09 08 B4 0A 01 01 B0 1D }
0x41180: 			OneOfOption Option: "7800" Value: 7800 { 09 08 B5 0A 01 01 78 1E }
0x41188: 			OneOfOption Option: "8000" Value: 8000 { 09 08 B6 0A 01 01 40 1F }
0x41190: 			OneOfOption Option: "8200" Value: 8200 { 09 08 B7 0A 01 01 08 20 }
0x41198: 			OneOfOption Option: "8400" Value: 8400 { 09 08 B8 0A 01 01 D0 20 }
0x411A0: 			OneOfOption Option: "8600" Value: 8600 { 09 08 B9 0A 01 01 98 21 }
0x411A8: 			OneOfOption Option: "8800" Value: 8800 { 09 08 BA 0A 01 01 60 22 }
0x411B0: 			OneOfOption Option: "9000" Value: 9000 { 09 08 BB 0A 01 01 28 23 }
0x411B8: 			OneOfOption Option: "9200" Value: 9200 { 09 08 BC 0A 01 01 F0 23 }
0x411C0: 			OneOfOption Option: "9400" Value: 9400 { 09 08 BD 0A 01 01 B8 24 }
0x411C8: 			OneOfOption Option: "9600" Value: 9600 { 09 08 BE 0A 01 01 80 25 }
0x411D0: 			OneOfOption Option: "9800" Value: 9800 { 09 08 BF 0A 01 01 48 26 }
0x411D8: 			OneOfOption Option: "10000" Value: 10000 { 09 08 C0 0A 01 01 10 27 }
0x411E0: 			OneOfOption Option: "12800" Value: 12800 { 09 08 C1 0A 01 01 00 32 }
0x411E8: 		End  { 29 02 }
0x411EA: 		OneOf Prompt: "LP5 Bank Mode", Help: "LP5 Bank Mode", QuestionFlags: 0x10, QuestionId: 0x5EF, VarStoreId: 0x4, VarOffset: 0x474, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 7E 0A 7F 0A EF 05 04 00 74 04 10 10 00 03 00 }
0x411FB: 			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 90 00 30 00 00 }
0x41202: 			OneOfOption Option: "LP5 8 Bank Mode" Value: 1 { 09 07 80 0A 00 00 01 }
0x41209: 			OneOfOption Option: "LP5 16 Bank Mode" Value: 2 { 09 07 81 0A 00 00 02 }
0x41210: 			OneOfOption Option: "LP5 BG Mode" Value: 3 { 09 07 82 0A 00 00 03 }
0x41217: 		End  { 29 02 }
0x41219: 		SuppressIf  { 0A 82 }
0x4121B: 			EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x41221: 			OneOf Prompt: "DDR5 DFE Gain", Help: "DDR5 DFE Gain", QuestionFlags: 0x10, QuestionId: 0x5F0, VarStoreId: 0x4, VarOffset: 0x47A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xB, Step: 0x0 { 05 91 83 0A 84 0A F0 05 04 00 7A 04 10 10 00 0B 00 }
0x41232: 				OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 85 0A 30 00 00 }
0x41239: 				OneOfOption Option: "1" Value: 1 { 09 07 86 0A 00 00 01 }
0x41240: 				OneOfOption Option: "2" Value: 2 { 09 07 87 0A 00 00 02 }
0x41247: 				OneOfOption Option: "3" Value: 3 { 09 07 88 0A 00 00 03 }
0x4124E: 				OneOfOption Option: "-1" Value: 9 { 09 07 89 0A 00 00 09 }
0x41255: 				OneOfOption Option: "-2" Value: 10 { 09 07 8A 0A 00 00 0A }
0x4125C: 				OneOfOption Option: "-3" Value: 11 { 09 07 8B 0A 00 00 0B }
0x41263: 			End  { 29 02 }
0x41265: 		End  { 29 02 }
0x41267: 		Numeric Prompt: "Frequency Limit for Mixed 2DPC DDR4", Help: "Override the reduced speed in mixed 2DPC config or non-POR 2DPC config. 0=Auto, otherwise speed in MT/s", QuestionFlags: 0x10, QuestionId: 0x5F1, VarStoreId: 0x4, VarOffset: 0x45E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 C2 0A C3 0A F1 05 04 00 5E 04 10 11 00 00 FF FF 01 00 }
0x4127B: 			Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x41282: 		End  { 29 02 }
0x41284: 		Numeric Prompt: "Frequency Limit for Mixed 2DPC DDR5 1 Rank 8GB and 8GB", Help: "Override the reduced speed in mixed 2DPC config or non-POR 2DPC config. 0=Auto, otherwise speed in MT/s", QuestionFlags: 0x10, QuestionId: 0x5F2, VarStoreId: 0x4, VarOffset: 0x469, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 C4 0A C5 0A F2 05 04 00 69 04 10 11 00 00 FF FF 01 00 }
0x41298: 			Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x4129F: 		End  { 29 02 }
0x412A1: 		Numeric Prompt: "Frequency Limit for Mixed 2DPC DDR5 1 Rank 16GB and 16GB", Help: "Override the reduced speed in mixed 2DPC config or non-POR 2DPC config. 0=Auto, otherwise speed in MT/s", QuestionFlags: 0x10, QuestionId: 0x5F3, VarStoreId: 0x4, VarOffset: 0x46B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 C6 0A C7 0A F3 05 04 00 6B 04 10 11 00 00 FF FF 01 00 }
0x412B5: 			Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x412BC: 		End  { 29 02 }
0x412BE: 		Numeric Prompt: "Frequency Limit for Mixed 2DPC DDR5 1 Rank 8GB and 16GB", Help: "Override the reduced speed in mixed 2DPC config or non-POR 2DPC config. 0=Auto, otherwise speed in MT/s", QuestionFlags: 0x10, QuestionId: 0x5F4, VarStoreId: 0x4, VarOffset: 0x46D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 C8 0A C9 0A F4 05 04 00 6D 04 10 11 00 00 FF FF 01 00 }
0x412D2: 			Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x412D9: 		End  { 29 02 }
0x412DB: 		Numeric Prompt: "Frequency Limit for Mixed 2DPC DDR5 2 Rank", Help: "Override the reduced speed in mixed 2DPC config or non-POR 2DPC config. 0=Auto, otherwise speed in MT/s", QuestionFlags: 0x10, QuestionId: 0x5F5, VarStoreId: 0x4, VarOffset: 0x46F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 CA 0A CB 0A F5 05 04 00 6F 04 10 11 00 00 FF FF 01 00 }
0x412EF: 			Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x412F6: 		End  { 29 02 }
0x412F8: 		Numeric Prompt: "LCT Cmd Eye Width", Help: "LCT Cmd Eye Width 0= Auto ", QuestionFlags: 0x10, QuestionId: 0x5F6, VarStoreId: 0x4, VarOffset: 0x471, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 CC 0A CD 0A F6 05 04 00 71 04 10 11 00 00 FF FF 01 00 }
0x4130C: 			Default DefaultId: 0x0 Value: 96 { 5B 07 00 00 01 60 00 }
0x41313: 		End  { 29 02 }
0x41315: 		OneOf Prompt: "HOB Buffer Size", Help: "Size to set HOB Buffer", QuestionFlags: 0x10, QuestionId: 0x5F7, VarStoreId: 0x4, VarOffset: 0x188, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 CF 07 D0 07 F7 05 04 00 88 01 10 10 00 03 00 }
0x41326: 			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 90 00 30 00 00 }
0x4132D: 			OneOfOption Option: "1B" Value: 1 { 09 07 D1 07 00 00 01 }
0x41334: 			OneOfOption Option: "1KB" Value: 2 { 09 07 D2 07 00 00 02 }
0x4133B: 			OneOfOption Option: "Max (assuming 63KB total HOB size)" Value: 3 { 09 07 D3 07 00 00 03 }
0x41342: 		End  { 29 02 }
0x41344: 		SuppressIf  { 0A 82 }
0x41346: 			EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 86 42 11 02 00 }
0x4134C: 				Not  { 17 02 }
0x4134E: 				EqIdVal QuestionId: 0x1142, Value: 0x5 { 12 06 42 11 05 00 }
0x41354: 				Not  { 17 02 }
0x41356: 				And  { 15 02 }
0x41358: 				EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x4135E: 				Not  { 17 02 }
0x41360: 				And  { 15 02 }
0x41362: 				EqIdVal QuestionId: 0x1142, Value: 0x3 { 12 06 42 11 03 00 }
0x41368: 				Not  { 17 02 }
0x4136A: 				And  { 15 02 }
0x4136C: 			End  { 29 02 }
0x4136E: 			OneOf Prompt: "ECC Support", Help: "Enable/disable DDR Ecc Support", QuestionFlags: 0x10, QuestionId: 0x5F8, VarStoreId: 0x4, VarOffset: 0x189, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 07 D7 07 F8 05 04 00 89 01 10 10 00 01 00 }
0x4137F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x41386: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x4138D: 			End  { 29 02 }
0x4138F: 			Numeric Prompt: "Error Injection Address Match", Help: "Address to match against for ECC error injection", QuestionFlags: 0x10, QuestionId: 0x5F9, VarStoreId: 0x4, VarOffset: 0x44A, Flags: 0x13, Size: 64, Min: 0x0, Max: 0x1FFFFFFFF, Step: 0x40 { 07 A6 21 0A 22 0A F9 05 04 00 4A 04 10 13 00 00 00 00 00 00 00 00 FF FF FF FF 01 00 00 00 40 00 00 00 00 00 00 00 }
0x413B5: 				Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x413C2: 			End  { 29 02 }
0x413C4: 			Numeric Prompt: "Error Injection Mask", Help: "Mask to match against for ECC error injection", QuestionFlags: 0x10, QuestionId: 0x5FA, VarStoreId: 0x4, VarOffset: 0x452, Flags: 0x13, Size: 64, Min: 0x0, Max: 0x1FFFFFFFF, Step: 0x0 { 07 A6 23 0A 24 0A FA 05 04 00 52 04 10 13 00 00 00 00 00 00 00 00 FF FF FF FF 01 00 00 00 00 00 00 00 00 00 00 00 }
0x413EA: 				Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x413F7: 			End  { 29 02 }
0x413F9: 			Numeric Prompt: "Error Injection Insertion Count", Help: "Number of transactions between ECC error injection", QuestionFlags: 0x10, QuestionId: 0x5FB, VarStoreId: 0x4, VarOffset: 0x45A, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 25 0A 26 0A FB 05 04 00 5A 04 10 12 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x41413: 				Default DefaultId: 0x0 Value: 15 { 5B 09 00 00 02 0F 00 00 00 }
0x4141C: 			End  { 29 02 }
0x4141E: 		End  { 29 02 }
0x41420: 		OneOf Prompt: "Max TOLUD", Help: "Maximum Value of TOLUD. Dynamic assignment would adjust TOLUD automatically based on largest MMIO length of installed graphic controller", QuestionFlags: 0x10, QuestionId: 0x276F, VarStoreId: 0x4, VarOffset: 0x18A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xB, Step: 0x0 { 05 91 D8 07 D9 07 6F 27 04 00 8A 01 10 10 00 0B 00 }
0x41431: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x41437: 			OneOfOption Option: "Dynamic" Value: 0 { 09 07 DA 07 00 00 00 }
0x4143E: 			OneOfOption Option: "1 GB" Value: 1 { 09 07 E5 07 00 00 01 }
0x41445: 			OneOfOption Option: "1.25 GB" Value: 2 { 09 07 E4 07 00 00 02 }
0x4144C: 			OneOfOption Option: "1.5 GB" Value: 3 { 09 07 E3 07 00 00 03 }
0x41453: 			OneOfOption Option: "1.75 GB" Value: 4 { 09 07 E2 07 00 00 04 }
0x4145A: 			OneOfOption Option: "2 GB" Value: 5 { 09 07 E1 07 00 00 05 }
0x41461: 			OneOfOption Option: "2.25 GB" Value: 6 { 09 07 E0 07 00 00 06 }
0x41468: 			OneOfOption Option: "2.5 GB" Value: 7 { 09 07 DF 07 00 00 07 }
0x4146F: 			OneOfOption Option: "2.75 GB" Value: 8 { 09 07 DE 07 00 00 08 }
0x41476: 			OneOfOption Option: "3 GB" Value: 9 { 09 07 DD 07 00 00 09 }
0x4147D: 			OneOfOption Option: "3.25 GB" Value: 10 { 09 07 DC 07 00 00 0A }
0x41484: 			OneOfOption Option: "3.5 GB" Value: 11 { 09 07 DB 07 00 00 0B }
0x4148B: 		End  { 29 02 }
0x4148D: 		OneOf Prompt: "SA GV", Help: "System Agent Geyserville. Can disable, fix to a specific point, or enable frequency switching.", QuestionFlags: 0x10, QuestionId: 0x2770, VarStoreId: 0x4, VarOffset: 0x1F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 53 09 54 09 70 27 04 00 F1 01 10 10 00 05 00 }
0x4149E: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x414A5: 			OneOfOption Option: "Enabled" Value: 5 { 09 07 91 00 00 00 05 }
0x414AC: 			OneOfOption Option: "Fixed to 1st Point" Value: 1 { 09 07 55 09 00 00 01 }
0x414B3: 			OneOfOption Option: "Fixed to 2nd Point" Value: 2 { 09 07 56 09 00 00 02 }
0x414BA: 			OneOfOption Option: "Fixed to 3rd Point" Value: 3 { 09 07 57 09 00 00 03 }
0x414C1: 			OneOfOption Option: "Fixed to 4th Point" Value: 4 { 09 07 58 09 00 00 04 }
0x414C8: 		End  { 29 02 }
0x414CA: 		SuppressIf  { 0A 82 }
0x414CC: 			EqIdVal QuestionId: 0x2770, Value: 0x0 { 12 86 70 27 00 00 }
0x414D2: 				Not  { 17 02 }
0x414D4: 			End  { 29 02 }
0x414D6: 			Numeric Prompt: "Gear Ratio", Help: "Gear ratio when SAGV is disabled. 0-Auto, 1-G1, 2-G2, 4-G4", QuestionFlags: 0x10, QuestionId: 0x5FC, VarStoreId: 0x4, VarOffset: 0x1FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1 { 07 91 63 09 64 09 FC 05 04 00 FE 01 10 10 00 04 01 }
0x414E7: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x414ED: 			End  { 29 02 }
0x414EF: 		End  { 29 02 }
0x414F1: 		SuppressIf  { 0A 82 }
0x414F3: 			EqIdVal QuestionId: 0x2770, Value: 0x0 { 12 06 70 27 00 00 }
0x414F9: 			Numeric Prompt: "First Point Frequency", Help: "Specify the frequency for the given point.  0 - MRC auto, Else a specific frequency as an integer: 1333", QuestionFlags: 0x10, QuestionId: 0x5FD, VarStoreId: 0x4, VarOffset: 0x1F2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 59 09 61 09 FD 05 04 00 F2 01 10 11 00 00 FF FF 01 00 }
0x4150D: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x41514: 			End  { 29 02 }
0x41516: 			Numeric Prompt: "First Point Gear", Help: "Gear ratio for this SAGV point. 0-Auto, 1-G1, 2-G2, 4-G4", QuestionFlags: 0x10, QuestionId: 0x5FE, VarStoreId: 0x4, VarOffset: 0x1FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1 { 07 91 5A 09 62 09 FE 05 04 00 FA 01 10 10 00 04 01 }
0x41527: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4152D: 			End  { 29 02 }
0x4152F: 			Numeric Prompt: "Second Point Frequency", Help: "Specify the frequency for the given point.  0 - MRC auto, Else a specific frequency as an integer: 1333", QuestionFlags: 0x10, QuestionId: 0x5FF, VarStoreId: 0x4, VarOffset: 0x1F4, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 5B 09 61 09 FF 05 04 00 F4 01 10 11 00 00 FF FF 01 00 }
0x41543: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x4154A: 			End  { 29 02 }
0x4154C: 			Numeric Prompt: "Second Point Gear", Help: "Gear ratio for this SAGV point. 0-Auto, 1-G1, 2-G2, 4-G4", QuestionFlags: 0x10, QuestionId: 0x600, VarStoreId: 0x4, VarOffset: 0x1FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1 { 07 91 5C 09 62 09 00 06 04 00 FB 01 10 10 00 04 01 }
0x4155D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x41563: 			End  { 29 02 }
0x41565: 			Numeric Prompt: "Third Point Frequency", Help: "Specify the frequency for the given point.  0 - MRC auto, Else a specific frequency as an integer: 1333", QuestionFlags: 0x10, QuestionId: 0x601, VarStoreId: 0x4, VarOffset: 0x1F6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 5D 09 61 09 01 06 04 00 F6 01 10 11 00 00 FF FF 01 00 }
0x41579: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x41580: 			End  { 29 02 }
0x41582: 			Numeric Prompt: "Third Point Gear", Help: "Gear ratio for this SAGV point. 0-Auto, 1-G1, 2-G2, 4-G4", QuestionFlags: 0x10, QuestionId: 0x602, VarStoreId: 0x4, VarOffset: 0x1FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1 { 07 91 5E 09 62 09 02 06 04 00 FC 01 10 10 00 04 01 }
0x41593: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x41599: 			End  { 29 02 }
0x4159B: 			Numeric Prompt: "Fourth Point Frequency", Help: "Specify the frequency for the given point.  0 - MRC auto, Else a specific frequency as an integer: 1333", QuestionFlags: 0x10, QuestionId: 0x603, VarStoreId: 0x4, VarOffset: 0x1F8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 5F 09 61 09 03 06 04 00 F8 01 10 11 00 00 FF FF 01 00 }
0x415AF: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x415B6: 			End  { 29 02 }
0x415B8: 			Numeric Prompt: "Fourth Point Gear", Help: "Gear ratio for this SAGV point. 0-Auto, 1-G1, 2-G2, 4-G4", QuestionFlags: 0x10, QuestionId: 0x604, VarStoreId: 0x4, VarOffset: 0x1FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1 { 07 91 60 09 62 09 04 06 04 00 FD 01 10 10 00 04 01 }
0x415C9: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x415CF: 			End  { 29 02 }
0x415D1: 		End  { 29 02 }
0x415D3: 		Numeric Prompt: "SAGV Switch Factor IA", Help: "SAGV Switch Factor of IA Load Percentage To Trigger Switching Up And Down", QuestionFlags: 0x10, QuestionId: 0x605, VarStoreId: 0x4, VarOffset: 0x461, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 EC 08 ED 08 05 06 04 00 61 04 10 10 01 32 01 }
0x415E4: 			Default DefaultId: 0x0 Value: 30 { 5B 06 00 00 00 1E }
0x415EA: 		End  { 29 02 }
0x415EC: 		Numeric Prompt: "SAGV Switch Factor GT", Help: "SAGV Switch Factor of GT Load Percentage To Trigger Switching Up And Down", QuestionFlags: 0x10, QuestionId: 0x606, VarStoreId: 0x4, VarOffset: 0x462, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 EE 08 EF 08 06 06 04 00 62 04 10 10 01 32 01 }
0x415FD: 			Default DefaultId: 0x0 Value: 30 { 5B 06 00 00 00 1E }
0x41603: 		End  { 29 02 }
0x41605: 		Numeric Prompt: "SAGV Switch Factor IO", Help: "SAGV Switch Factor of IO Load Percentage To Trigger Switching Up And Down", QuestionFlags: 0x10, QuestionId: 0x607, VarStoreId: 0x4, VarOffset: 0x463, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 F0 08 F1 08 07 06 04 00 63 04 10 10 01 32 01 }
0x41616: 			Default DefaultId: 0x0 Value: 30 { 5B 06 00 00 00 1E }
0x4161C: 		End  { 29 02 }
0x4161E: 		Numeric Prompt: "SAGV Switch Factor Stall", Help: "SAGV Switch Factor of IA/GT Stall Percentage To Trigger Switching Up And Down", QuestionFlags: 0x10, QuestionId: 0x608, VarStoreId: 0x4, VarOffset: 0x464, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 F2 08 F3 08 08 06 04 00 64 04 10 10 01 32 01 }
0x4162F: 			Default DefaultId: 0x0 Value: 30 { 5B 06 00 00 00 1E }
0x41635: 		End  { 29 02 }
0x41637: 		Numeric Prompt: "Threshold For Switch Up", Help: "Duration In MS Of High Activity After Which SAGV Will Switch Up", QuestionFlags: 0x10, QuestionId: 0x609, VarStoreId: 0x4, VarOffset: 0x465, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 F6 08 F7 08 09 06 04 00 65 04 10 10 01 32 01 }
0x41648: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4164E: 		End  { 29 02 }
0x41650: 		Numeric Prompt: "Threshold For Switch Down", Help: "Duration In MS Of Low Activity After Which SAGV Will Switch Down", QuestionFlags: 0x10, QuestionId: 0x60A, VarStoreId: 0x4, VarOffset: 0x466, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1 { 07 91 F4 08 F5 08 0A 06 04 00 66 04 10 10 01 32 01 }
0x41661: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x41667: 		End  { 29 02 }
0x41669: 		OneOf Prompt: "Retrain on Fast Fail", Help: "Restart MRC in Cold mode if SW MemTest fails during Fast flow. Default = Enabled", QuestionFlags: 0x10, QuestionId: 0x60B, VarStoreId: 0x4, VarOffset: 0x19C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 08 96 08 0B 06 04 00 9C 01 10 10 00 01 00 }
0x4167A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x41681: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x41688: 		End  { 29 02 }
0x4168A: 		OneOf Prompt: "DDR4_1DPC", Help: "DDR4 1DPC performance feature for 2R DIMMs. Can be enabled on DIMM0 or DIMM1 only, or on both", QuestionFlags: 0x10, QuestionId: 0x60C, VarStoreId: 0x4, VarOffset: 0x19D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 97 08 98 08 0C 06 04 00 9D 01 10 10 00 03 00 }
0x4169B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x416A2: 			OneOfOption Option: "Enabled on DIMM0 only" Value: 1 { 09 07 99 08 00 00 01 }
0x416A9: 			OneOfOption Option: "Enabled on DIMM1 only" Value: 2 { 09 07 9A 08 00 00 02 }
0x416B0: 			OneOfOption Option: "Enabled" Value: 3, Default, MfgDefault { 09 07 91 00 30 00 03 }
0x416B7: 		End  { 29 02 }
0x416B9: 		OneOf Prompt: "Row Hammer Mode", Help: "Row Hammer Prevention Mode. RFM will fall back to pTRR if not available", QuestionFlags: 0x10, QuestionId: 0x60D, VarStoreId: 0x4, VarOffset: 0x23E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 5E 08 5F 08 0D 06 04 00 3E 02 10 10 00 02 00 }
0x416CA: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x416D1: 			OneOfOption Option: "RFM" Value: 1, Default, MfgDefault { 09 07 60 08 30 00 01 }
0x416D8: 			OneOfOption Option: "pTRR" Value: 2 { 09 07 61 08 00 00 02 }
0x416DF: 		End  { 29 02 }
0x416E1: 		SuppressIf  { 0A 82 }
0x416E3: 			EqIdVal QuestionId: 0x60D, Value: 0x0 { 12 06 0D 06 00 00 }
0x416E9: 			OneOf Prompt: "RH LFSR0 Mask", Help: "LFSR0 mask for RH pTRR", QuestionFlags: 0x10, QuestionId: 0x60E, VarStoreId: 0x4, VarOffset: 0x23F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xF, Step: 0x0 { 05 91 6C 08 6D 08 0E 06 04 00 3F 02 10 10 01 0F 00 }
0x416FA: 				OneOfOption Option: "1/2^1" Value: 1 { 09 07 82 08 00 00 01 }
0x41701: 				OneOfOption Option: "1/2^2" Value: 2 { 09 07 81 08 00 00 02 }
0x41708: 				OneOfOption Option: "1/2^3" Value: 3 { 09 07 80 08 00 00 03 }
0x4170F: 				OneOfOption Option: "1/2^4" Value: 4 { 09 07 7F 08 00 00 04 }
0x41716: 				OneOfOption Option: "1/2^5" Value: 5 { 09 07 7E 08 00 00 05 }
0x4171D: 				OneOfOption Option: "1/2^6" Value: 6 { 09 07 7D 08 00 00 06 }
0x41724: 				OneOfOption Option: "1/2^7" Value: 7 { 09 07 7C 08 00 00 07 }
0x4172B: 				OneOfOption Option: "1/2^8" Value: 8 { 09 07 7B 08 00 00 08 }
0x41732: 				OneOfOption Option: "1/2^9" Value: 9 { 09 07 7A 08 00 00 09 }
0x41739: 				OneOfOption Option: "1/2^10" Value: 10 { 09 07 79 08 00 00 0A }
0x41740: 				OneOfOption Option: "1/2^11" Value: 11, Default, MfgDefault { 09 07 78 08 30 00 0B }
0x41747: 				OneOfOption Option: "1/2^12" Value: 12 { 09 07 77 08 00 00 0C }
0x4174E: 				OneOfOption Option: "1/2^13" Value: 13 { 09 07 76 08 00 00 0D }
0x41755: 				OneOfOption Option: "1/2^14" Value: 14 { 09 07 75 08 00 00 0E }
0x4175C: 				OneOfOption Option: "1/2^15" Value: 15 { 09 07 74 08 00 00 0F }
0x41763: 			End  { 29 02 }
0x41765: 			OneOf Prompt: "RH LFSR1 Mask", Help: "LFSR1 mask for RH pTRR", QuestionFlags: 0x10, QuestionId: 0x60F, VarStoreId: 0x4, VarOffset: 0x240, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xF, Step: 0x0 { 05 91 6E 08 6F 08 0F 06 04 00 40 02 10 10 01 0F 00 }
0x41776: 				OneOfOption Option: "1/2^1" Value: 1 { 09 07 82 08 00 00 01 }
0x4177D: 				OneOfOption Option: "1/2^2" Value: 2 { 09 07 81 08 00 00 02 }
0x41784: 				OneOfOption Option: "1/2^3" Value: 3 { 09 07 80 08 00 00 03 }
0x4178B: 				OneOfOption Option: "1/2^4" Value: 4 { 09 07 7F 08 00 00 04 }
0x41792: 				OneOfOption Option: "1/2^5" Value: 5 { 09 07 7E 08 00 00 05 }
0x41799: 				OneOfOption Option: "1/2^6" Value: 6 { 09 07 7D 08 00 00 06 }
0x417A0: 				OneOfOption Option: "1/2^7" Value: 7 { 09 07 7C 08 00 00 07 }
0x417A7: 				OneOfOption Option: "1/2^8" Value: 8 { 09 07 7B 08 00 00 08 }
0x417AE: 				OneOfOption Option: "1/2^9" Value: 9 { 09 07 7A 08 00 00 09 }
0x417B5: 				OneOfOption Option: "1/2^10" Value: 10 { 09 07 79 08 00 00 0A }
0x417BC: 				OneOfOption Option: "1/2^11" Value: 11, Default, MfgDefault { 09 07 78 08 30 00 0B }
0x417C3: 				OneOfOption Option: "1/2^12" Value: 12 { 09 07 77 08 00 00 0C }
0x417CA: 				OneOfOption Option: "1/2^13" Value: 13 { 09 07 76 08 00 00 0D }
0x417D1: 				OneOfOption Option: "1/2^14" Value: 14 { 09 07 75 08 00 00 0E }
0x417D8: 				OneOfOption Option: "1/2^15" Value: 15 { 09 07 74 08 00 00 0F }
0x417DF: 			End  { 29 02 }
0x417E1: 		End  { 29 02 }
0x417E3: 		OneOf Prompt: "MC Refresh Rate", Help: "Select refresh rate on the MC", QuestionFlags: 0x10, QuestionId: 0x610, VarStoreId: 0x4, VarOffset: 0x42C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 62 08 63 08 10 06 04 00 2C 04 10 10 00 03 00 }
0x417F4: 			OneOfOption Option: "NORMAL Refresh" Value: 0, Default, MfgDefault { 09 07 64 08 30 00 00 }
0x417FB: 			SuppressIf  { 0A 82 }
0x417FD: 				EqIdValList QuestionId: 0x1177, Values: [0, 1] { 14 0A 77 11 02 00 00 00 01 00 }
0x41807: 				OneOfOption Option: "1x Refresh" Value: 1 { 09 07 65 08 00 00 01 }
0x4180E: 			End  { 29 02 }
0x41810: 			OneOfOption Option: "2x Refresh" Value: 2 { 09 07 66 08 00 00 02 }
0x41817: 			OneOfOption Option: "4x Refresh" Value: 3 { 09 07 67 08 00 00 03 }
0x4181E: 		End  { 29 02 }
0x41820: 		OneOf Prompt: "Refresh Watermarks", Help: "Sets Refresh Panic Watermark and Refresh High-Priority Watermark to HIGH or LOW values", QuestionFlags: 0x10, QuestionId: 0x611, VarStoreId: 0x4, VarOffset: 0x422, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 08 69 08 11 06 04 00 22 04 10 10 00 01 00 }
0x41831: 			OneOfOption Option: "Low" Value: 0 { 09 07 6B 08 00 00 00 }
0x41838: 			OneOfOption Option: "High" Value: 1, Default, MfgDefault { 09 07 6A 08 30 00 01 }
0x4183F: 		End  { 29 02 }
0x41841: 		Numeric Prompt: "LPDDR ODT RttWr", Help: "Initial RttWr ODT override for LP4/5 in Ohms. Range 0x01 - 0xFF, default 0 = AUTO", QuestionFlags: 0x10, QuestionId: 0x612, VarStoreId: 0x4, VarOffset: 0x3F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 70 08 71 08 12 06 04 00 F3 03 10 10 00 FF 01 }
0x41852: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x41858: 		End  { 29 02 }
0x4185A: 		Numeric Prompt: "LPDDR ODT RttCa", Help: "Initial RttCa ODT override for LP4/5 in Ohms. Range 0x01 - 0xFF, default 0 = AUTO", QuestionFlags: 0x10, QuestionId: 0x613, VarStoreId: 0x4, VarOffset: 0x3F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 72 08 73 08 13 06 04 00 F4 03 10 10 00 FF 01 }
0x4186B: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x41871: 		End  { 29 02 }
0x41873: 		OneOf Prompt: "Exit On Failure (MRC)", Help: "Exit On Failure for MRC training steps", QuestionFlags: 0x10, QuestionId: 0x614, VarStoreId: 0x4, VarOffset: 0x245, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 83 08 84 08 14 06 04 00 45 02 10 10 00 01 00 }
0x41884: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x4188B: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x41892: 		End  { 29 02 }
0x41894: 		OneOf Prompt: "New Features 1 - MRC", Help: "Enabling/Disabling Generic New Features 1", QuestionFlags: 0x10, QuestionId: 0x615, VarStoreId: 0x4, VarOffset: 0x246, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 85 08 86 08 15 06 04 00 46 02 10 10 00 01 00 }
0x418A5: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x418AC: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x418B3: 		End  { 29 02 }
0x418B5: 		OneOf Prompt: "New Features 2 - MRC", Help: "Enabling/Disabling Generic New Features 2", QuestionFlags: 0x10, QuestionId: 0x616, VarStoreId: 0x4, VarOffset: 0x247, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 08 88 08 16 06 04 00 47 02 10 10 00 01 00 }
0x418C6: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x418CD: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x418D4: 		End  { 29 02 }
0x418D6: 		OneOf Prompt: "Ch Hash Override", Help: "Override Channel Hash settings", QuestionFlags: 0x10, QuestionId: 0x617, VarStoreId: 0x4, VarOffset: 0x192, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 08 47 08 17 06 04 00 92 01 10 10 00 01 00 }
0x418E7: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x418EE: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x418F5: 		End  { 29 02 }
0x418F7: 		GrayOutIf  { 19 82 }
0x418F9: 			EqIdVal QuestionId: 0x617, Value: 0x0 { 12 06 17 06 00 00 }
0x418FF: 			OneOf Prompt: "Ch Hash Support", Help: "Enable/Disable Channel Hash Support. NOTE: ONLY if Memory interleaved Mode", QuestionFlags: 0x10, QuestionId: 0x618, VarStoreId: 0x4, VarOffset: 0x193, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 08 49 08 18 06 04 00 93 01 10 10 00 01 00 }
0x41910: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x41917: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x4191E: 			End  { 29 02 }
0x41920: 			Numeric Prompt: "Ch Hash Mask", Help: "Set the BIT(s) to be included in the XOR function. NOTE BIT mask corresponds to BITS [19:6}", QuestionFlags: 0x10, QuestionId: 0x619, VarStoreId: 0x4, VarOffset: 0x194, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x3FFF, Step: 0x1 { 07 94 4A 08 4B 08 19 06 04 00 94 01 10 11 01 00 FF 3F 01 00 }
0x41934: 				Default DefaultId: 0x0 Value: 2096 { 5B 07 00 00 01 30 08 }
0x4193B: 			End  { 29 02 }
0x4193D: 			OneOf Prompt: "Ch Hash Interleaved Bit", Help: "Select the BIT to be used for Channel Interleaved mode. NOTE: BIT7 will interlave the channels at a 2 cacheline granularity, BIT8 at 4 and BIT9 at 8", QuestionFlags: 0x10, QuestionId: 0x61A, VarStoreId: 0x4, VarOffset: 0x196, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 50 08 51 08 1A 06 04 00 96 01 10 10 00 07 00 }
0x4194E: 				OneOfOption Option: "BIT6" Value: 0 { 09 07 52 08 00 00 00 }
0x41955: 				OneOfOption Option: "BIT7" Value: 1 { 09 07 53 08 00 00 01 }
0x4195C: 				OneOfOption Option: "BIT8" Value: 2, Default, MfgDefault { 09 07 54 08 30 00 02 }
0x41963: 				OneOfOption Option: "BIT9" Value: 3 { 09 07 55 08 00 00 03 }
0x4196A: 				OneOfOption Option: "BIT10" Value: 4 { 09 07 56 08 00 00 04 }
0x41971: 				OneOfOption Option: "BIT11" Value: 5 { 09 07 57 08 00 00 05 }
0x41978: 				OneOfOption Option: "BIT12" Value: 6 { 09 07 58 08 00 00 06 }
0x4197F: 				OneOfOption Option: "BIT13" Value: 7 { 09 07 59 08 00 00 07 }
0x41986: 			End  { 29 02 }
0x41988: 		End  { 29 02 }
0x4198A: 		OneOf Prompt: "Extended Bank Hashing", Help: "Enable/disable Extended Bank Hashing.", QuestionFlags: 0x10, QuestionId: 0x61B, VarStoreId: 0x4, VarOffset: 0x404, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4C 08 4D 08 1B 06 04 00 04 04 10 10 00 01 00 }
0x4199B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x419A2: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x419A9: 		End  { 29 02 }
0x419AB: 		OneOf Prompt: "Per Bank Refresh", Help: "Enables and Disables the per bank refresh.  This only impacts memory technologies that support PBR: LPDDR4, LPDDR5 and DDR5", QuestionFlags: 0x10, QuestionId: 0x61C, VarStoreId: 0x4, VarOffset: 0x197, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 08 4F 08 1C 06 04 00 97 01 10 10 00 01 00 }
0x419BC: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x419C3: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x419CA: 		End  { 29 02 }
0x419CC: 		OneOf Prompt: "VC1 Read Metering", Help: "Enable/Disable VC1 Read Metering Feature (RdMeter)", QuestionFlags: 0x10, QuestionId: 0x61D, VarStoreId: 0x4, VarOffset: 0x198, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5A 08 5B 08 1D 06 04 00 98 01 10 10 00 01 00 }
0x419DD: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x419E4: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x419EB: 		End  { 29 02 }
0x419ED: 		Numeric Prompt: "Strong Weak Leaker", Help: "Value for StrongWkLeaker", QuestionFlags: 0x10, QuestionId: 0x61E, VarStoreId: 0x4, VarOffset: 0x199, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x7, Step: 0x1 { 07 91 5C 08 5D 08 1E 06 04 00 99 01 10 10 01 07 01 }
0x419FE: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x41A04: 		End  { 29 02 }
0x41A06: 		OneOf Prompt: "Power Down Mode", Help: "CKE Power Down Mode Control", QuestionFlags: 0x10, QuestionId: 0x2771, VarStoreId: 0x4, VarOffset: 0x1A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9D 08 9E 08 71 27 04 00 A2 01 10 10 00 FF 00 }
0x41A17: 			OneOfOption Option: "Auto" Value: 255, Default, MfgDefault { 09 07 90 00 30 00 FF }
0x41A1E: 			OneOfOption Option: "No Power Down" Value: 0 { 09 07 9F 08 00 00 00 }
0x41A25: 			OneOfOption Option: "APD" Value: 1 { 09 07 A0 08 00 00 01 }
0x41A2C: 			OneOfOption Option: "PPD-DLLoff" Value: 6 { 09 07 A1 08 00 00 06 }
0x41A33: 		End  { 29 02 }
0x41A35: 		Numeric Prompt: "Pwr Down Idle Timer", Help: "The minimum value should = to the worst case Roundtrip delay + Burst_Length. 0 means AUTO: 64 for ULX/ULT, 128 for DT/Halo", QuestionFlags: 0x10, QuestionId: 0x61F, VarStoreId: 0x4, VarOffset: 0x1A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 A2 08 A3 08 1F 06 04 00 A3 01 10 10 00 FF 01 }
0x41A46: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x41A4C: 		End  { 29 02 }
0x41A4E: 		OneOf Prompt: "Page Close Idle Timeout", Help: "Page Close Idle Timeout Control", QuestionFlags: 0x10, QuestionId: 0x2772, VarStoreId: 0x4, VarOffset: 0x1A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 08 A5 08 72 27 04 00 A4 01 10 10 00 01 00 }
0x41A5F: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41A66: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41A6D: 		End  { 29 02 }
0x41A6F: 		OneOf Prompt: "Memory Scrambler", Help: "Enable/Disable Memory Scrambler support.", QuestionFlags: 0x10, QuestionId: 0x620, VarStoreId: 0x4, VarOffset: 0x231, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 09 C7 09 20 06 04 00 31 02 10 10 00 01 00 }
0x41A80: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x41A87: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x41A8E: 		End  { 29 02 }
0x41A90: 		OneOf Prompt: "Force ColdReset", Help: "Force ColdReset OR Choose MrcColdBoot mode, when Coldboot is required during MRC execution. Note: If ME 5.0MB is present, ForceColdReset is required!", QuestionFlags: 0x10, QuestionId: 0x621, VarStoreId: 0x4, VarOffset: 0x232, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 09 C9 09 21 06 04 00 32 02 10 10 00 01 00 }
0x41AA1: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41AA8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41AAF: 		End  { 29 02 }
0x41AB1: 		OneOf Prompt: "Controller 0, Channel 0 Control", Help: "Controller 0, Channel 0 Control - Enable or Disable Controller 0, Channel 0.", QuestionFlags: 0x10, QuestionId: 0x622, VarStoreId: 0x4, VarOffset: 0x233, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 09 CB 09 22 06 04 00 33 02 10 10 00 01 00 }
0x41AC2: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41AC9: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41AD0: 		End  { 29 02 }
0x41AD2: 		OneOf Prompt: "Controller 0, Channel 1 Control", Help: "Controller 0, Channel 1 Control - Enable or Disable Controller 0, Channel 1.", QuestionFlags: 0x10, QuestionId: 0x623, VarStoreId: 0x4, VarOffset: 0x234, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CC 09 CD 09 23 06 04 00 34 02 10 10 00 01 00 }
0x41AE3: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41AEA: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41AF1: 		End  { 29 02 }
0x41AF3: 		OneOf Prompt: "Controller 0, Channel 2 Control", Help: "Controller 0, Channel 2 Control - Enable or Disable Controller 0, Channel 2.", QuestionFlags: 0x10, QuestionId: 0x624, VarStoreId: 0x4, VarOffset: 0x235, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CE 09 CF 09 24 06 04 00 35 02 10 10 00 01 00 }
0x41B04: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41B0B: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41B12: 		End  { 29 02 }
0x41B14: 		OneOf Prompt: "Controller 0, Channel 3 Control", Help: "Controller 0, Channel 3 Control - Enable or Disable Controller 0, Channel 3.", QuestionFlags: 0x10, QuestionId: 0x625, VarStoreId: 0x4, VarOffset: 0x236, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 09 D1 09 25 06 04 00 36 02 10 10 00 01 00 }
0x41B25: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41B2C: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41B33: 		End  { 29 02 }
0x41B35: 		OneOf Prompt: "Controller 1, Channel 0 Control", Help: "Controller 1, Channel 0 Control - Enable or Disable Controller 1, Channel 0.", QuestionFlags: 0x10, QuestionId: 0x626, VarStoreId: 0x4, VarOffset: 0x237, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D2 09 D3 09 26 06 04 00 37 02 10 10 00 01 00 }
0x41B46: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41B4D: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41B54: 		End  { 29 02 }
0x41B56: 		OneOf Prompt: "Controller 1, Channel 1 Control", Help: "Controller 1, Channel 1 Control - Enable or Disable Controller 1, Channel 1.", QuestionFlags: 0x10, QuestionId: 0x627, VarStoreId: 0x4, VarOffset: 0x238, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D4 09 D5 09 27 06 04 00 38 02 10 10 00 01 00 }
0x41B67: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41B6E: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41B75: 		End  { 29 02 }
0x41B77: 		OneOf Prompt: "Controller 1, Channel 2 Control", Help: "Controller 1, Channel 2 Control - Enable or Disable Controller 1, Channel 2.", QuestionFlags: 0x10, QuestionId: 0x628, VarStoreId: 0x4, VarOffset: 0x239, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 09 D7 09 28 06 04 00 39 02 10 10 00 01 00 }
0x41B88: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41B8F: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41B96: 		End  { 29 02 }
0x41B98: 		OneOf Prompt: "Controller 1, Channel 3 Control", Help: "Controller 1, Channel 3 Control - Enable or Disable Controller 1, Channel 3.", QuestionFlags: 0x10, QuestionId: 0x629, VarStoreId: 0x4, VarOffset: 0x23A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D8 09 D9 09 29 06 04 00 3A 02 10 10 00 01 00 }
0x41BA9: 			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault { 09 07 91 00 30 00 00 }
0x41BB0: 			OneOfOption Option: "Disabled" Value: 1 { 09 07 92 00 00 00 01 }
0x41BB7: 		End  { 29 02 }
0x41BB9: 		OneOf Prompt: "Force Single Rank", Help: "When enabled, only Rank 0 will be used in each DIMM", QuestionFlags: 0x10, QuestionId: 0x62A, VarStoreId: 0x4, VarOffset: 0x19A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DA 09 DB 09 2A 06 04 00 9A 01 10 10 00 01 00 }
0x41BCA: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41BD1: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41BD8: 		End  { 29 02 }
0x41BDA: 		OneOf Prompt: "In-Band ECC Support", Help: "Enable/Disable In-Band ECC. Will be enabled if memory has symmetric configuration", QuestionFlags: 0x10, QuestionId: 0x62B, VarStoreId: 0x4, VarOffset: 0x1A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 09 DD 09 2B 06 04 00 A5 01 10 10 00 01 00 }
0x41BEB: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41BF2: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41BF9: 		End  { 29 02 }
0x41BFB: 		SuppressIf  { 0A 82 }
0x41BFD: 			EqIdVal QuestionId: 0x62B, Value: 0x0 { 12 06 2B 06 00 00 }
0x41C03: 			OneOf Prompt: "In-Band ECC Operation Mode", Help: "0: Functional Mode protects requests based on the address range, 1: Makes all requests non protected and ignore range checks, 2:Makes all requests protected and ignore range checks", QuestionFlags: 0x10, QuestionId: 0x62C, VarStoreId: 0x4, VarOffset: 0x1A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DE 09 DF 09 2C 06 04 00 A6 01 10 10 00 02 00 }
0x41C14: 				OneOfOption Option: "0" Value: 0 { 09 07 E0 09 00 00 00 }
0x41C1B: 				OneOfOption Option: "1" Value: 1 { 09 07 E1 09 00 00 01 }
0x41C22: 				OneOfOption Option: "2" Value: 2, Default, MfgDefault { 09 07 E2 09 30 00 02 }
0x41C29: 			End  { 29 02 }
0x41C2B: 			SuppressIf  { 0A 82 }
0x41C2D: 				EqIdVal QuestionId: 0x62C, Value: 0x0 { 12 86 2C 06 00 00 }
0x41C33: 					Not  { 17 02 }
0x41C35: 				End  { 29 02 }
0x41C37: 				OneOf Prompt: "IBECC Protect Region 0", Help: "Enable/Disable In-Band ECC for Region 0", QuestionFlags: 0x10, QuestionId: 0x62D, VarStoreId: 0x4, VarOffset: 0x1A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 09 E4 09 2D 06 04 00 A7 01 10 10 00 01 00 }
0x41C48: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41C4F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41C56: 				End  { 29 02 }
0x41C58: 				SuppressIf  { 0A 82 }
0x41C5A: 					EqIdVal QuestionId: 0x62D, Value: 0x0 { 12 06 2D 06 00 00 }
0x41C60: 					Numeric Prompt: "Protected Region 0 BASE", Help: "Set the base address for protected region 0 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x62E, VarStoreId: 0x4, VarOffset: 0x1AF, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A E5 09 E6 09 2E 06 04 00 AF 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41C7A: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41C83: 					End  { 29 02 }
0x41C85: 					Numeric Prompt: "Protected Region 0 MASK", Help: "Set the mask for protected region 0", QuestionFlags: 0x10, QuestionId: 0x62F, VarStoreId: 0x4, VarOffset: 0x1CF, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A E7 09 E8 09 2F 06 04 00 CF 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41C9F: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41CA8: 					End  { 29 02 }
0x41CAA: 				End  { 29 02 }
0x41CAC: 				OneOf Prompt: "IBECC Protect Region 1", Help: "Enable/Disable In-Band ECC for Region 1", QuestionFlags: 0x10, QuestionId: 0x630, VarStoreId: 0x4, VarOffset: 0x1A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 09 EA 09 30 06 04 00 A8 01 10 10 00 01 00 }
0x41CBD: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41CC4: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41CCB: 				End  { 29 02 }
0x41CCD: 				SuppressIf  { 0A 82 }
0x41CCF: 					EqIdVal QuestionId: 0x630, Value: 0x0 { 12 06 30 06 00 00 }
0x41CD5: 					Numeric Prompt: "Protected Region 1 BASE", Help: "Set the base address for protected region 1 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x631, VarStoreId: 0x4, VarOffset: 0x1B3, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A EB 09 EC 09 31 06 04 00 B3 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41CEF: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41CF8: 					End  { 29 02 }
0x41CFA: 					Numeric Prompt: "Protected Region 1 MASK", Help: "Set the mask for protected region 1", QuestionFlags: 0x10, QuestionId: 0x632, VarStoreId: 0x4, VarOffset: 0x1D3, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A ED 09 EE 09 32 06 04 00 D3 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41D14: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41D1D: 					End  { 29 02 }
0x41D1F: 				End  { 29 02 }
0x41D21: 				OneOf Prompt: "IBECC Protect Region 2", Help: "Enable/Disable In-Band ECC for Region 2", QuestionFlags: 0x10, QuestionId: 0x633, VarStoreId: 0x4, VarOffset: 0x1A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EF 09 F0 09 33 06 04 00 A9 01 10 10 00 01 00 }
0x41D32: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41D39: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41D40: 				End  { 29 02 }
0x41D42: 				SuppressIf  { 0A 82 }
0x41D44: 					EqIdVal QuestionId: 0x633, Value: 0x0 { 12 06 33 06 00 00 }
0x41D4A: 					Numeric Prompt: "Protected Region 2 BASE", Help: "Set the base address for protected region 2 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x634, VarStoreId: 0x4, VarOffset: 0x1B7, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A F1 09 F2 09 34 06 04 00 B7 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41D64: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41D6D: 					End  { 29 02 }
0x41D6F: 					Numeric Prompt: "Protected Region 2 MASK", Help: "Set the mask for protected region 2", QuestionFlags: 0x10, QuestionId: 0x635, VarStoreId: 0x4, VarOffset: 0x1D7, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A F3 09 F4 09 35 06 04 00 D7 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41D89: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41D92: 					End  { 29 02 }
0x41D94: 				End  { 29 02 }
0x41D96: 				OneOf Prompt: "IBECC Protect Region 3", Help: "Enable/Disable In-Band ECC for Region 3", QuestionFlags: 0x10, QuestionId: 0x636, VarStoreId: 0x4, VarOffset: 0x1AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 09 F6 09 36 06 04 00 AA 01 10 10 00 01 00 }
0x41DA7: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41DAE: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41DB5: 				End  { 29 02 }
0x41DB7: 				SuppressIf  { 0A 82 }
0x41DB9: 					EqIdVal QuestionId: 0x636, Value: 0x0 { 12 06 36 06 00 00 }
0x41DBF: 					Numeric Prompt: "Protected Region 3 BASE", Help: "Set the base address for protected region 3 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x637, VarStoreId: 0x4, VarOffset: 0x1BB, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A F7 09 F8 09 37 06 04 00 BB 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41DD9: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41DE2: 					End  { 29 02 }
0x41DE4: 					Numeric Prompt: "Protected Region 3 MASK", Help: "Set the mask for protected region 3", QuestionFlags: 0x10, QuestionId: 0x638, VarStoreId: 0x4, VarOffset: 0x1DB, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A F9 09 FA 09 38 06 04 00 DB 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41DFE: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41E07: 					End  { 29 02 }
0x41E09: 				End  { 29 02 }
0x41E0B: 				OneOf Prompt: "IBECC Protect Region 4", Help: "Enable/Disable In-Band ECC for Region 4", QuestionFlags: 0x10, QuestionId: 0x639, VarStoreId: 0x4, VarOffset: 0x1AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FB 09 FC 09 39 06 04 00 AB 01 10 10 00 01 00 }
0x41E1C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41E23: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41E2A: 				End  { 29 02 }
0x41E2C: 				SuppressIf  { 0A 82 }
0x41E2E: 					EqIdVal QuestionId: 0x639, Value: 0x0 { 12 06 39 06 00 00 }
0x41E34: 					Numeric Prompt: "Protected Region 4 BASE", Help: "Set the base address for protected region 4 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x63A, VarStoreId: 0x4, VarOffset: 0x1BF, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A FD 09 FE 09 3A 06 04 00 BF 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41E4E: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41E57: 					End  { 29 02 }
0x41E59: 					Numeric Prompt: "Protected Region 4 MASK", Help: "Set the mask for protected region 4", QuestionFlags: 0x10, QuestionId: 0x63B, VarStoreId: 0x4, VarOffset: 0x1DF, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A FF 09 00 0A 3B 06 04 00 DF 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41E73: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41E7C: 					End  { 29 02 }
0x41E7E: 				End  { 29 02 }
0x41E80: 				OneOf Prompt: "IBECC Protect Region 5", Help: "Enable/Disable In-Band ECC for Region 5", QuestionFlags: 0x10, QuestionId: 0x63C, VarStoreId: 0x4, VarOffset: 0x1AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 0A 02 0A 3C 06 04 00 AC 01 10 10 00 01 00 }
0x41E91: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41E98: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41E9F: 				End  { 29 02 }
0x41EA1: 				SuppressIf  { 0A 82 }
0x41EA3: 					EqIdVal QuestionId: 0x63C, Value: 0x0 { 12 06 3C 06 00 00 }
0x41EA9: 					Numeric Prompt: "Protected Region 5 BASE", Help: "Set the base address for protected region 5 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x63D, VarStoreId: 0x4, VarOffset: 0x1C3, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A 03 0A 04 0A 3D 06 04 00 C3 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41EC3: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41ECC: 					End  { 29 02 }
0x41ECE: 					Numeric Prompt: "Protected Region 5 MASK", Help: "Set the mask for protected region 5", QuestionFlags: 0x10, QuestionId: 0x63E, VarStoreId: 0x4, VarOffset: 0x1E3, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A 05 0A 06 0A 3E 06 04 00 E3 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41EE8: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41EF1: 					End  { 29 02 }
0x41EF3: 				End  { 29 02 }
0x41EF5: 				OneOf Prompt: "IBECC Protect Region 6", Help: "Enable/Disable In-Band ECC for Region 6", QuestionFlags: 0x10, QuestionId: 0x63F, VarStoreId: 0x4, VarOffset: 0x1AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 0A 08 0A 3F 06 04 00 AD 01 10 10 00 01 00 }
0x41F06: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41F0D: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41F14: 				End  { 29 02 }
0x41F16: 				SuppressIf  { 0A 82 }
0x41F18: 					EqIdVal QuestionId: 0x63F, Value: 0x0 { 12 06 3F 06 00 00 }
0x41F1E: 					Numeric Prompt: "Protected Region 6 BASE", Help: "Set the base address for protected region 6 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x640, VarStoreId: 0x4, VarOffset: 0x1C7, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A 09 0A 0A 0A 40 06 04 00 C7 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41F38: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41F41: 					End  { 29 02 }
0x41F43: 					Numeric Prompt: "Protected Region 6 MASK", Help: "Set the mask for protected region 6", QuestionFlags: 0x10, QuestionId: 0x641, VarStoreId: 0x4, VarOffset: 0x1E7, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A 0B 0A 0C 0A 41 06 04 00 E7 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41F5D: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41F66: 					End  { 29 02 }
0x41F68: 				End  { 29 02 }
0x41F6A: 				OneOf Prompt: "IBECC Protect Region 7", Help: "Enable/Disable In-Band ECC for Region 7", QuestionFlags: 0x10, QuestionId: 0x642, VarStoreId: 0x4, VarOffset: 0x1AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0D 0A 0E 0A 42 06 04 00 AE 01 10 10 00 01 00 }
0x41F7B: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x41F82: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x41F89: 				End  { 29 02 }
0x41F8B: 				SuppressIf  { 0A 82 }
0x41F8D: 					EqIdVal QuestionId: 0x642, Value: 0x0 { 12 06 42 06 00 00 }
0x41F93: 					Numeric Prompt: "Protected Region 7 BASE", Help: "Set the base address for protected region 7 (Per IBECC instance)", QuestionFlags: 0x10, QuestionId: 0x643, VarStoreId: 0x4, VarOffset: 0x1CB, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3FFFFFF, Step: 0x1 { 07 9A 0F 0A 10 0A 43 06 04 00 CB 01 10 12 00 00 00 00 FF FF FF 03 01 00 00 00 }
0x41FAD: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x41FB6: 					End  { 29 02 }
0x41FB8: 					Numeric Prompt: "Protected Region 7 MASK", Help: "Set the mask for protected region 7", QuestionFlags: 0x10, QuestionId: 0x644, VarStoreId: 0x4, VarOffset: 0x1EB, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FFFFFF, Step: 0x1 { 07 9A 11 0A 12 0A 44 06 04 00 EB 01 10 12 01 00 00 00 FF FF FF 03 01 00 00 00 }
0x41FD2: 						Default DefaultId: 0x0 Value: 67108832 { 5B 09 00 00 02 E0 FF FF 03 }
0x41FDB: 					End  { 29 02 }
0x41FDD: 				End  { 29 02 }
0x41FDF: 			End  { 29 02 }
0x41FE1: 			OneOf Prompt: "IBECC Error Injection Control", Help: "Enables IBECC Error Injection", QuestionFlags: 0x10, QuestionId: 0x645, VarStoreId: 0x4, VarOffset: 0x405, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 13 0A 14 0A 45 06 04 00 05 04 10 10 00 07 00 }
0x41FF2: 				OneOfOption Option: "No Error Injection" Value: 0, Default, MfgDefault { 09 07 16 0A 30 00 00 }
0x41FF9: 				OneOfOption Option: "Inject Correctable Error Address match" Value: 1 { 09 07 17 0A 00 00 01 }
0x42000: 				OneOfOption Option: "Inject Correctable Error on insertion counter" Value: 3 { 09 07 18 0A 00 00 03 }
0x42007: 				OneOfOption Option: "Inject Uncorrectable Error Address match" Value: 5 { 09 07 19 0A 00 00 05 }
0x4200E: 				OneOfOption Option: "Inject Uncorrectable Error on insertion counter" Value: 7 { 09 07 1A 0A 00 00 07 }
0x42015: 				WarningIf Timeout: 0x0, Warning: "Do not enable in production BIOS" { 63 85 15 0A 00 }
0x4201A: 					QuestionRef1 QuestionId: 0x645 { 40 84 45 06 }
0x4201E: 						Uint8 Value: 0x1 { 42 03 01 }
0x42021: 						GreaterEqual  { 32 02 }
0x42023: 					End  { 29 02 }
0x42025: 				End  { 29 02 }
0x42027: 			End  { 29 02 }
0x42029: 			SuppressIf  { 0A 82 }
0x4202B: 				EqIdVal QuestionId: 0x645, Value: 0x0 { 12 86 45 06 00 00 }
0x42031: 					EqIdVal QuestionId: 0x645, Value: 0x3 { 12 06 45 06 03 00 }
0x42037: 					Or  { 16 02 }
0x42039: 					EqIdVal QuestionId: 0x645, Value: 0x7 { 12 06 45 06 07 00 }
0x4203F: 					Or  { 16 02 }
0x42041: 				End  { 29 02 }
0x42043: 				Numeric Prompt: "Error Injection Address Match", Help: "Address to match against for ECC error injection", QuestionFlags: 0x10, QuestionId: 0x646, VarStoreId: 0x4, VarOffset: 0x406, Flags: 0x13, Size: 64, Min: 0x0, Max: 0x3FFFFFFFFFC0, Step: 0x40 { 07 A6 1B 0A 1C 0A 46 06 04 00 06 04 10 13 00 00 00 00 00 00 00 00 C0 FF FF FF FF 3F 00 00 40 00 00 00 00 00 00 00 }
0x42069: 					Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x42076: 				End  { 29 02 }
0x42078: 				Numeric Prompt: "Error Injection Mask", Help: "Mask to match against for ECC error injection", QuestionFlags: 0x10, QuestionId: 0x647, VarStoreId: 0x4, VarOffset: 0x40E, Flags: 0x13, Size: 64, Min: 0x0, Max: 0x3FFFFFFFFFC0, Step: 0x40 { 07 A6 1D 0A 1E 0A 47 06 04 00 0E 04 10 13 00 00 00 00 00 00 00 00 C0 FF FF FF FF 3F 00 00 40 00 00 00 00 00 00 00 }
0x4209E: 					Default DefaultId: 0x0 Value: 0 { 5B 0D 00 00 03 00 00 00 00 00 00 00 00 }
0x420AB: 				End  { 29 02 }
0x420AD: 			End  { 29 02 }
0x420AF: 			SuppressIf  { 0A 82 }
0x420B1: 				EqIdVal QuestionId: 0x645, Value: 0x0 { 12 86 45 06 00 00 }
0x420B7: 					EqIdVal QuestionId: 0x645, Value: 0x1 { 12 06 45 06 01 00 }
0x420BD: 					Or  { 16 02 }
0x420BF: 					EqIdVal QuestionId: 0x645, Value: 0x5 { 12 06 45 06 05 00 }
0x420C5: 					Or  { 16 02 }
0x420C7: 				End  { 29 02 }
0x420C9: 				Numeric Prompt: "Error Injection Insertion Count", Help: "Number of transactions between ECC error injection", QuestionFlags: 0x10, QuestionId: 0x648, VarStoreId: 0x4, VarOffset: 0x416, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 1F 0A 20 0A 48 06 04 00 16 04 10 12 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x420E3: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x420EC: 				End  { 29 02 }
0x420EE: 			End  { 29 02 }
0x420F0: 		End  { 29 02 }
0x420F2: 		OneOf Prompt: "Memory Remap", Help: "Enable/Disable Memory Remap above 4GB", QuestionFlags: 0x10, QuestionId: 0x649, VarStoreId: 0x4, VarOffset: 0x23B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 0A 28 0A 49 06 04 00 3B 02 10 10 00 01 00 }
0x42103: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x4210A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42111: 		End  { 29 02 }
0x42113: 		OneOf Prompt: "Time Measure", Help: "Enable/Disable printing of the time it takes to execute MRC.", QuestionFlags: 0x10, QuestionId: 0x64A, VarStoreId: 0x4, VarOffset: 0x18E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 29 0A 2A 0A 4A 06 04 00 8E 01 10 10 00 01 00 }
0x42124: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x4212B: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42132: 		End  { 29 02 }
0x42134: 		OneOf Prompt: "CsPiStartHighinEct", Help: "Cs Pi Start With High Value in Ect.", QuestionFlags: 0x10, QuestionId: 0x64B, VarStoreId: 0x4, VarOffset: 0x47C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2B 0A 2C 0A 4B 06 04 00 7C 04 10 10 00 01 00 }
0x42145: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x4214C: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42153: 		End  { 29 02 }
0x42155: 		OneOf Prompt: "DisableFGRAndPBRWA", Help: "Disable FGR And PBR WA.", QuestionFlags: 0x10, QuestionId: 0x64C, VarStoreId: 0x4, VarOffset: 0x47D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 0A 2E 0A 4C 06 04 00 7D 04 10 10 00 01 00 }
0x42166: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x4216D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42174: 		End  { 29 02 }
0x42176: 		OneOf Prompt: "Fast Boot", Help: "Enable/Disable fast path thru the MRC", QuestionFlags: 0x10, QuestionId: 0x64D, VarStoreId: 0x4, VarOffset: 0x18F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 0A 30 0A 4D 06 04 00 8F 01 10 10 00 01 00 }
0x42187: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4218D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42194: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4219B: 		End  { 29 02 }
0x4219D: 		OneOf Prompt: "Rank Margin Tool Per Task", Help: "Enables/Disables RMT running at every major training step", QuestionFlags: 0x10, QuestionId: 0x64E, VarStoreId: 0x4, VarOffset: 0x190, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 09 C5 09 4E 06 04 00 90 01 10 10 00 01 00 }
0x421AE: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x421B5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x421BC: 		End  { 29 02 }
0x421BE: 		OneOf Prompt: "Training Tracing", Help: "Enables/Disables printing of the current trained state at every major training step.", QuestionFlags: 0x10, QuestionId: 0x64F, VarStoreId: 0x4, VarOffset: 0x191, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 09 C3 09 4F 06 04 00 91 01 10 10 00 01 00 }
0x421CF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x421D6: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x421DD: 		End  { 29 02 }
0x421DF: 		OneOf Prompt: "Lpddr Mem WL Set", Help: "Only applicable to LPDDR, Memory Write Latency Set selection (A is default, B will be used if memory devices support it)", QuestionFlags: 0x10, QuestionId: 0x650, VarStoreId: 0x4, VarOffset: 0x19B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 09 BF 09 50 06 04 00 9B 01 10 10 00 01 00 }
0x421F0: 			OneOfOption Option: "Set A" Value: 0 { 09 07 C0 09 00 00 00 }
0x421F7: 			OneOfOption Option: "Set B" Value: 1, Default, MfgDefault { 09 07 C1 09 30 00 01 }
0x421FE: 		End  { 29 02 }
0x42200: 		GrayOutIf  { 19 82 }
0x42202: 			EqIdVal QuestionId: 0x53, Value: 0x0 { 12 06 53 00 00 00 }
0x42208: 			OneOf Prompt: "BDAT Memory Test Type", Help: "Indicates the type of Memory Training data to populate into the BDAT ACPI table.", QuestionFlags: 0x10, QuestionId: 0x651, VarStoreId: 0x4, VarOffset: 0x19F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 69 0E 6A 0E 51 06 04 00 9F 01 10 10 00 02 00 }
0x42219: 				OneOfOption Option: "Rank Margin Tool Rank" Value: 0, Default, MfgDefault { 09 07 6B 0E 30 00 00 }
0x42220: 				OneOfOption Option: "Rank Margin Tool Bit" Value: 1 { 09 07 6C 0E 00 00 01 }
0x42227: 				OneOfOption Option: "Margin 2D" Value: 2 { 09 07 6D 0E 00 00 02 }
0x4222E: 			End  { 29 02 }
0x42230: 		End  { 29 02 }
0x42232: 		Numeric Prompt: "Rank Margin Tool Loop Count", Help: "Specifies the Loop Count to be used during Rank Margin Tool Testing. 0 - AUTO", QuestionFlags: 0x10, QuestionId: 0x652, VarStoreId: 0x4, VarOffset: 0x1A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x20, Step: 0x1 { 07 91 6E 0E 6F 0E 52 06 04 00 A0 01 10 10 00 20 01 }
0x42243: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42249: 		End  { 29 02 }
0x4224B: 		OneOf Prompt: "ECC DFT", Help: "Enable/Disable ECC DFT feature", QuestionFlags: 0x10, QuestionId: 0x653, VarStoreId: 0x4, VarOffset: 0x1EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 0A 32 0A 53 06 04 00 EF 01 10 10 00 01 00 }
0x4225C: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42263: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4226A: 		End  { 29 02 }
0x4226C: 		OneOf Prompt: "Write0", Help: "Write0 feature for LP5/DDR5", QuestionFlags: 0x10, QuestionId: 0x654, VarStoreId: 0x4, VarOffset: 0x1F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 0A 34 0A 54 06 04 00 F0 01 10 10 00 01 00 }
0x4227D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x42284: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4228B: 		End  { 29 02 }
0x4228D: 		OneOf Prompt: "Periodic DCC", Help: "Enable / Disable Periodic DCC", QuestionFlags: 0x10, QuestionId: 0x655, VarStoreId: 0x4, VarOffset: 0x42E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 35 0A 36 0A 55 06 04 00 2E 04 10 10 00 01 00 }
0x4229E: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x422A5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x422AC: 		End  { 29 02 }
0x422AE: 		OneOf Prompt: "LPMode", Help: "Control LPMode feature", QuestionFlags: 0x10, QuestionId: 0x656, VarStoreId: 0x4, VarOffset: 0x42F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 37 0A 38 0A 56 06 04 00 2F 04 10 10 00 02 00 }
0x422BF: 			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x422C6: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x422CD: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x422D4: 		End  { 29 02 }
0x422D6: 		OneOf Prompt: "PPR Enable", Help: "PPR permanently repairs failed rows (if possible).", QuestionFlags: 0x10, QuestionId: 0x657, VarStoreId: 0x4, VarOffset: 0x3EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 EF 0F F0 0F 57 06 04 00 EF 03 10 10 00 02 00 }
0x422E7: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x422EE: 			OneOfOption Option: "Hard PPR" Value: 2 { 09 07 F1 0F 00 00 02 }
0x422F5: 		End  { 29 02 }
0x422F7: 		OneOf Prompt: "SAM Overlaoding", Help: "Enable: copy the sagv frequency point. Disable: not copy.", QuestionFlags: 0x10, QuestionId: 0x2773, VarStoreId: 0x4, VarOffset: 0x477, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 0F 8F 0F 73 27 04 00 77 04 10 10 00 01 00 }
0x42308: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4230F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x42316: 		End  { 29 02 }
0x42318: 	End  { 29 02 }
0x4231A: 	Form FormId: 0x27AE, Title: "System Agent (SA) Configuration" { 01 86 AE 27 CB 07 }
0x42320: 		Subtitle Prompt: "System Agent (SA) Configuration", Help: "", Flags: 0x0 { 02 87 CB 07 00 00 00 }
0x42327: 		End  { 29 02 }
0x42329: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x42330: 		End  { 29 02 }
0x42332: 		Text Prompt: "VT-d", Help: "VT-d capability", Text: "N/A" { 03 08 47 0E 51 0A 48 0E }
0x4233A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x42341: 		End  { 29 02 }
0x42343: 		Ref Prompt: "Memory Configuration", Help: "Memory Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x658, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27AD { 0F 0F CD 07 CE 07 58 06 00 00 FF FF 00 AD 27 }
0x42352: 		Ref Prompt: "Graphics Configuration", Help: "Graphics Configuration", QuestionFlags: 0x0, QuestionId: 0x659, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B0 { 0F 0F 65 0A 65 0A 59 06 00 00 FF FF 00 B0 27 }
0x42361: 		Ref Prompt: "DMI/OPI Configuration", Help: "Control various DMI functions.", QuestionFlags: 0x0, QuestionId: 0x65A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B1 { 0F 0F 3E 0B 3F 0B 5A 06 00 00 FF FF 00 B1 27 }
0x42370: 		SuppressIf  { 0A 82 }
0x42372: 			EqIdVal QuestionId: 0x1176, Value: 0x0 { 12 06 76 11 00 00 }
0x42378: 			Ref Prompt: "VMD setup menu", Help: "VMD Configuration settings", QuestionFlags: 0x0, QuestionId: 0x65B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C6 { 0F 0F 90 0F 92 0F 5B 06 00 00 FF FF 00 C6 27 }
0x42387: 		End  { 29 02 }
0x42389: 		Ref Prompt: "Display setup menu", Help: "Display Configuration settings", QuestionFlags: 0x0, QuestionId: 0x65C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C7 { 0F 0F EC 0F EE 0F 5C 06 00 00 FF FF 00 C7 27 }
0x42398: 		Ref Prompt: "PCI Express Configuration", Help: "PCI Express Configuration settings", QuestionFlags: 0x0, QuestionId: 0x65D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C8 { 0F 0F 7C 0E 7D 0E 5D 06 00 00 FF FF 00 C8 27 }
0x423A7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x423AE: 		End  { 29 02 }
0x423B0: 		OneOf Prompt: "Stop Grant Configuration", Help: "Automatic/Manual stop grant configuration", QuestionFlags: 0x10, QuestionId: 0x65E, VarStoreId: 0x4, VarOffset: 0xAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 0D F2 0D 5E 06 04 00 AF 00 10 10 00 01 00 }
0x423C1: 			OneOfOption Option: "Auto" Value: 1, Default, MfgDefault { 09 07 90 00 30 00 01 }
0x423C8: 			OneOfOption Option: "Manual" Value: 0 { 09 07 CA 07 00 00 00 }
0x423CF: 		End  { 29 02 }
0x423D1: 		SuppressIf  { 0A 82 }
0x423D3: 			EqIdVal QuestionId: 0x65E, Value: 0x1 { 12 06 5E 06 01 00 }
0x423D9: 			Numeric Prompt: "Number of Stop Grant Cycles", Help: "Selects number of Stop-Grant cycles.", QuestionFlags: 0x10, QuestionId: 0x65F, VarStoreId: 0x4, VarOffset: 0xB0, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3F, Step: 0x0 { 07 91 F3 0D F4 0D 5F 06 04 00 B0 00 10 10 01 3F 00 }
0x423EA: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x423F0: 			End  { 29 02 }
0x423F2: 		End  { 29 02 }
0x423F4: 		SuppressIf  { 0A 82 }
0x423F6: 			EqIdVal QuestionId: 0x1174, Value: 0x0 { 12 06 74 11 00 00 }
0x423FC: 			GrayOutIf  { 19 82 }
0x423FE: 				EqIdVal QuestionId: 0x1175, Value: 0x1 { 12 06 75 11 01 00 }
0x42404: 				OneOf Prompt: "VT-d", Help: "VT-d capability", QuestionFlags: 0x10, QuestionId: 0x2774, VarStoreId: 0x4, VarOffset: 0x7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 50 0A 51 0A 74 27 04 00 7D 00 10 10 00 01 00 }
0x42415: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x4241C: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42423: 				End  { 29 02 }
0x42425: 			End  { 29 02 }
0x42427: 		End  { 29 02 }
0x42429: 		GrayOutIf  { 19 82 }
0x4242B: 			EqIdVal QuestionId: 0x1174, Value: 0x0 { 12 86 74 11 00 00 }
0x42431: 				EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x42437: 				Or  { 16 02 }
0x42439: 			End  { 29 02 }
0x4243B: 			OneOf Prompt: "Control Iommu Pre-boot Behavior", Help: "Enable IOMMU in Pre-boot environment (If DMAR table is installed in DXE and If VTD_INFO_PPI is installed in PEI.)", QuestionFlags: 0x14, QuestionId: 0x660, VarStoreId: 0xF101, VarOffset: 0x995, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 53 1C 54 1C 60 06 01 F1 95 09 14 10 00 01 00 }
0x4244C: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x42452: 				OneOfOption Option: "Disable IOMMU" Value: 0 { 09 07 55 1C 00 00 00 }
0x42459: 				OneOfOption Option: "Enable IOMMU during boot" Value: 1 { 09 07 56 1C 00 00 01 }
0x42460: 			End  { 29 02 }
0x42462: 		End  { 29 02 }
0x42464: 		GrayOutIf  { 19 82 }
0x42466: 			EqIdVal QuestionId: 0x1174, Value: 0x0 { 12 86 74 11 00 00 }
0x4246C: 				EqIdVal QuestionId: 0x2774, Value: 0x0 { 12 06 74 27 00 00 }
0x42472: 				Or  { 16 02 }
0x42474: 			End  { 29 02 }
0x42476: 			SuppressIf  { 0A 82 }
0x42478: 				EqIdVal QuestionId: 0x1173, Value: 0x0 { 12 06 73 11 00 00 }
0x4247E: 				OneOf Prompt: "X2APIC Opt Out", Help: "Enable/Disable X2APIC_OPT_OUT bit", QuestionFlags: 0x10, QuestionId: 0x661, VarStoreId: 0x4, VarOffset: 0x86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 0D B6 0D 61 06 04 00 86 00 10 10 00 01 00 }
0x4248F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42496: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x4249D: 				End  { 29 02 }
0x4249F: 			End  { 29 02 }
0x424A1: 			OneOf Prompt: "DMA Control Guarantee", Help: "Enable/Disable DMA_CONTROL_GUARANTEE bit", QuestionFlags: 0x10, QuestionId: 0x662, VarStoreId: 0x4, VarOffset: 0x87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 0D B8 0D 62 06 04 00 87 00 10 10 00 01 00 }
0x424B2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x424B9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x424C0: 			End  { 29 02 }
0x424C2: 		End  { 29 02 }
0x424C4: 		OneOf Prompt: "Thermal Device (B0:D4:F0)", Help: "Enable/Disable SA Thermal Device. Always enabled for ICL A0 stepping.", QuestionFlags: 0x10, QuestionId: 0x663, VarStoreId: 0x4, VarOffset: 0x7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 0B 41 0B 63 06 04 00 7C 00 10 10 00 01 00 }
0x424D5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x424DC: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x424E3: 		End  { 29 02 }
0x424E5: 		OneOf Prompt: "Cpu CrashLog (Device 10)", Help: "Enable/Disable Cpu CrashLog Device.", QuestionFlags: 0x10, QuestionId: 0x664, VarStoreId: 0x4, VarOffset: 0xF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 0B 43 0B 64 06 04 00 F6 00 10 10 00 01 00 }
0x424F6: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x424FD: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42504: 		End  { 29 02 }
0x42506: 		OneOf Prompt: "GNA Device (B0:D8:F0)", Help: "Enable/Disable SA GNA Device.", QuestionFlags: 0x10, QuestionId: 0x665, VarStoreId: 0x4, VarOffset: 0x7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 0B 45 0B 65 06 04 00 7F 00 10 10 00 01 00 }
0x42517: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4251E: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42525: 		End  { 29 02 }
0x42527: 		OneOf Prompt: "CRID Support", Help: "Enable/Disable SA CRID and TCSS CRID control for Intel SIPP", QuestionFlags: 0x14, QuestionId: 0x2775, VarStoreId: 0x4, VarOffset: 0x257, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 0D AE 0D 75 27 04 00 57 02 14 10 00 01 00 }
0x42538: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4253F: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42546: 		End  { 29 02 }
0x42548: 		OneOf Prompt: "WRC Feature", Help: "Enable/Disable SA WRC(Write Cache) Feature of IOP. When enabled, supports IO devices allocating onto the ring and into LLC.", QuestionFlags: 0x10, QuestionId: 0x2776, VarStoreId: 0x4, VarOffset: 0x277, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AF 0D B0 0D 76 27 04 00 77 02 10 10 00 01 00 }
0x42559: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42560: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42567: 		End  { 29 02 }
0x42569: 		SuppressIf  { 0A 82 }
0x4256B: 			EqIdVal QuestionId: 0x278C, Value: 0xF { 12 06 8C 27 0F 00 }
0x42571: 			OneOf Prompt: "Above 4GB MMIO BIOS assignment", Help: "Enable/Disable above 4GB MemoryMappedIO BIOS assignment

This is enabled automatically when Aperture Size is set to 2048MB.", QuestionFlags: 0x10, QuestionId: 0x666, VarStoreId: 0x4, VarOffset: 0x7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 0D B2 0D 66 06 04 00 7E 00 10 10 00 01 00 }
0x42582: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x42589: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42590: 			End  { 29 02 }
0x42592: 		End  { 29 02 }
0x42594: 		OneOf Prompt: "Program Grant Count", Help: "Enable/Disable Programming Of Grant Count", QuestionFlags: 0x10, QuestionId: 0x667, VarStoreId: 0x4, VarOffset: 0x47B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 0D B4 0D 67 06 04 00 7B 04 10 10 00 01 00 }
0x425A5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x425AC: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x425B3: 		End  { 29 02 }
0x425B5: 		SuppressIf  { 0A 82 }
0x425B7: 			EqIdVal QuestionId: 0x1172, Value: 0x0 { 12 06 72 11 00 00 }
0x425BD: 			OneOf Prompt: "IPU Device (B0:D5:F0)", Help: "Enable/Disable SA IPU Device.", QuestionFlags: 0x10, QuestionId: 0x668, VarStoreId: 0x4, VarOffset: 0x80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 0B 47 0B 68 06 04 00 80 00 10 10 00 01 00 }
0x425CE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x425D5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x425DC: 			End  { 29 02 }
0x425DE: 		End  { 29 02 }
0x425E0: 		Ref Prompt: "MIPI Camera Configuration", Help: "MIPI Camera Configuration", QuestionFlags: 0x0, QuestionId: 0x669, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BE { 0F 0F 48 0B 48 0B 69 06 00 00 FF FF 00 BE 27 }
0x425EF: 		SuppressIf  { 0A 82 }
0x425F1: 			EqIdVal QuestionId: 0x1171, Value: 0x1 { 12 86 71 11 01 00 }
0x425F7: 				Not  { 17 02 }
0x425F9: 			End  { 29 02 }
0x425FB: 			OneOf Prompt: "eDRAM Mode", Help: "SW Mode eDRAM On or eDRAM Off", QuestionFlags: 0x10, QuestionId: 0x66A, VarStoreId: 0x4, VarOffset: 0x82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 64 0E 65 0E 6A 06 04 00 82 00 10 10 00 02 00 }
0x4260C: 				OneOfOption Option: "SW Mode eDRAM Off" Value: 0 { 09 07 66 0E 00 00 00 }
0x42613: 				OneOfOption Option: "SW Mode eDRAM On" Value: 1 { 09 07 67 0E 00 00 01 }
0x4261A: 				OneOfOption Option: "eDRAM HW Mode" Value: 2, Default { 09 07 68 0E 10 00 02 }
0x42621: 			End  { 29 02 }
0x42623: 		End  { 29 02 }
0x42625: 	End  { 29 02 }
0x42627: 	Form FormId: 0x27AF, Title: "Memory Overclocking Menu" { 01 86 AF 27 A9 08 }
0x4262D: 		SuppressIf  { 0A 82 }
0x4262F: 			EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x42635: 			Text Prompt: "Memory Profile:", Help: "", Text: "Default  Custom    XMP1    XMP2    XMP3    USER4    USER5" { 03 08 AA 08 C9 07 AB 08 }
0x4263D: 			Text Prompt: "  tCK [MHz]", Help: "", Text: "0000000 0000000 0000000 0000000 0000000 0000000 0000000" { 03 08 AC 08 C9 07 AD 08 }
0x42645: 			Text Prompt: "  tCL", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 AE 08 C9 07 AF 08 }
0x4264D: 			Text Prompt: "  tRCD/tRP", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 B0 08 C9 07 B1 08 }
0x42655: 			Text Prompt: "  tRAS", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 B2 08 C9 07 B3 08 }
0x4265D: 			Text Prompt: "  tCWL", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 B4 08 C9 07 B5 08 }
0x42665: 			Text Prompt: "  tFAW", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 B6 08 C9 07 B7 08 }
0x4266D: 			Text Prompt: "  tREFI", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 B8 08 C9 07 B9 08 }
0x42675: 			Text Prompt: "  tRFC", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 BA 08 C9 07 BB 08 }
0x4267D: 			Text Prompt: "  tRRD", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 BC 08 C9 07 BD 08 }
0x42685: 			Text Prompt: "  tRTP", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 BE 08 C9 07 BF 08 }
0x4268D: 			Text Prompt: "  tWR", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 C0 08 C9 07 C1 08 }
0x42695: 			Text Prompt: "  tWTR", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 C2 08 C9 07 C3 08 }
0x4269D: 			Text Prompt: "  tRFCpb", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 C4 08 C9 07 C5 08 }
0x426A5: 			Text Prompt: "  tRFC2", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 C6 08 C9 07 C7 08 }
0x426AD: 			Text Prompt: "  tRFC4", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 C8 08 C9 07 C9 08 }
0x426B5: 			Text Prompt: "  tRRD_L", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 CA 08 C9 07 CB 08 }
0x426BD: 			Text Prompt: "  tRRD_S", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 CC 08 C9 07 CD 08 }
0x426C5: 			Text Prompt: "  tWTR_L", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 CE 08 C9 07 CF 08 }
0x426CD: 			Text Prompt: "  tWTR_S", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 D0 08 C9 07 D1 08 }
0x426D5: 			Text Prompt: "  tCCD_L", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 D2 08 C9 07 D3 08 }
0x426DD: 			Text Prompt: "  NMode", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 D4 08 C9 07 D5 08 }
0x426E5: 			Text Prompt: "  VDD [mV]", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 D6 08 C9 07 D7 08 }
0x426ED: 			Text Prompt: "  VDDQ [mV]", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 D8 08 C9 07 D9 08 }
0x426F5: 			Text Prompt: "  VPP [mV]", Help: "", Text: "  00000   00000   00000   00000   00000   00000   00000" { 03 08 DA 08 C9 07 DB 08 }
0x426FD: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x42704: 			End  { 29 02 }
0x42706: 			OneOf Prompt: "Realtime Memory Timing", Help: "Enable/Disable realtime memory timings. When enabled, the system will allow performing realtime memory timing changes after MRC_DONE.", QuestionFlags: 0x10, QuestionId: 0x66B, VarStoreId: 0x4, VarOffset: 0x274, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 08 DD 08 6B 06 04 00 74 02 10 10 00 01 00 }
0x42717: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4271E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x42725: 			End  { 29 02 }
0x42727: 			OneOf Prompt: "Memory profile", Help: "Select DIMM timing profile. The below values start with the currently running values and don't auto populate.", QuestionFlags: 0x14, QuestionId: 0x2777, VarStoreId: 0x4, VarOffset: 0x18D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 DE 08 DF 08 77 27 04 00 8D 01 14 10 00 06 00 }
0x42738: 				OneOfOption Option: "Default SPD Profile" Value: 0, Default, MfgDefault { 09 07 E0 08 30 00 00 }
0x4273F: 				OneOfOption Option: "Custom Profile" Value: 1 { 09 07 E4 08 00 00 01 }
0x42746: 				SuppressIf  { 0A 82 }
0x42748: 					Get VarStoreId: 0x4, VarStoreInfo: 0x2, VarStoreType: 0x0 { 2B 87 04 00 02 00 00 }
0x4274F: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x42759: 						BitwiseAnd  { 35 02 }
0x4275B: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x42765: 						Equal  { 2F 02 }
0x42767: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x42771: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4277B: 						Conditional  { 50 02 }
0x4277D: 					End  { 29 02 }
0x4277F: 					OneOfOption Option: "XMP Profile 1" Value: 2 { 09 07 E1 08 00 00 02 }
0x42786: 				End  { 29 02 }
0x42788: 				SuppressIf  { 0A 82 }
0x4278A: 					Get VarStoreId: 0x4, VarStoreInfo: 0x2, VarStoreType: 0x0 { 2B 87 04 00 02 00 00 }
0x42791: 						Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x4279B: 						BitwiseAnd  { 35 02 }
0x4279D: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x427A7: 						Equal  { 2F 02 }
0x427A9: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x427B3: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x427BD: 						Conditional  { 50 02 }
0x427BF: 					End  { 29 02 }
0x427C1: 					OneOfOption Option: "XMP Profile 2" Value: 3 { 09 07 E2 08 00 00 03 }
0x427C8: 				End  { 29 02 }
0x427CA: 				SuppressIf  { 0A 82 }
0x427CC: 					Get VarStoreId: 0x4, VarStoreInfo: 0x2, VarStoreType: 0x0 { 2B 87 04 00 02 00 00 }
0x427D3: 						Uint64 Value: 0x4 { 45 0A 04 00 00 00 00 00 00 00 }
0x427DD: 						BitwiseAnd  { 35 02 }
0x427DF: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x427E9: 						Equal  { 2F 02 }
0x427EB: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x427F5: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x427FF: 						Conditional  { 50 02 }
0x42801: 					End  { 29 02 }
0x42803: 					OneOfOption Option: "XMP Profile 3" Value: 4 { 09 07 E3 08 00 00 04 }
0x4280A: 				End  { 29 02 }
0x4280C: 				SuppressIf  { 0A 82 }
0x4280E: 					Get VarStoreId: 0x4, VarStoreInfo: 0x2, VarStoreType: 0x0 { 2B 87 04 00 02 00 00 }
0x42815: 						Uint64 Value: 0x8 { 45 0A 08 00 00 00 00 00 00 00 }
0x4281F: 						BitwiseAnd  { 35 02 }
0x42821: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4282B: 						Equal  { 2F 02 }
0x4282D: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x42837: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x42841: 						Conditional  { 50 02 }
0x42843: 					End  { 29 02 }
0x42845: 					OneOfOption Option: "XMP User Profile 4" Value: 5 { 09 07 E5 08 00 00 05 }
0x4284C: 				End  { 29 02 }
0x4284E: 				SuppressIf  { 0A 82 }
0x42850: 					Get VarStoreId: 0x4, VarStoreInfo: 0x2, VarStoreType: 0x0 { 2B 87 04 00 02 00 00 }
0x42857: 						Uint64 Value: 0x10 { 45 0A 10 00 00 00 00 00 00 00 }
0x42861: 						BitwiseAnd  { 35 02 }
0x42863: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4286D: 						Equal  { 2F 02 }
0x4286F: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x42879: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x42883: 						Conditional  { 50 02 }
0x42885: 					End  { 29 02 }
0x42887: 					OneOfOption Option: "XMP User Profile 5" Value: 6 { 09 07 E6 08 00 00 06 }
0x4288E: 				End  { 29 02 }
0x42890: 			End  { 29 02 }
0x42892: 			SuppressIf  { 0A 82 }
0x42894: 				EqIdVal QuestionId: 0x1170, Value: 0x0 { 12 06 70 11 00 00 }
0x4289A: 				Text Prompt: "***DMB FAILED*** - Forced to Standard Profile, DMB disabled", Help: "", Text: "" { 03 08 E9 08 C9 07 C9 07 }
0x428A2: 			End  { 29 02 }
0x428A4: 			GrayOutIf  { 19 82 }
0x428A6: 				EqIdValList QuestionId: 0x2777, Values: [0, 1, 5, 6] { 14 8E 77 27 04 00 00 00 01 00 05 00 06 00 }
0x428B4: 					EqIdVal QuestionId: 0x66D, Value: 0x1 { 12 06 6D 06 01 00 }
0x428BA: 					Or  { 16 02 }
0x428BC: 				End  { 29 02 }
0x428BE: 				OneOf Prompt: "Dynamic Memory Boost", Help: "Enable/Disable Dynamic Memory Boost feature, Allows automatic switching between default SPD Profile frequency and selected XMP profile frequency. Only valid if an XMP Profile is selected.", QuestionFlags: 0x10, QuestionId: 0x66C, VarStoreId: 0x4, VarOffset: 0x41A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E7 08 E8 08 6C 06 04 00 1A 04 10 10 00 01 00 }
0x428CF: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x428D6: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x428DD: 				End  { 29 02 }
0x428DF: 			End  { 29 02 }
0x428E1: 			GrayOutIf  { 19 82 }
0x428E3: 				EqIdValList QuestionId: 0x2777, Values: [0, 1, 5, 6] { 14 8E 77 27 04 00 00 00 01 00 05 00 06 00 }
0x428F1: 					EqIdVal QuestionId: 0x66C, Value: 0x1 { 12 06 6C 06 01 00 }
0x428F7: 					Or  { 16 02 }
0x428F9: 				End  { 29 02 }
0x428FB: 				OneOf Prompt: "Realtime Memory Frequency", Help: "Enable/Disable Realtime Memory Frequency feature, Allows manual switching in runtime between default SPD Profile frequency and selected XMP profile frequency. Only valid if an XMP Profile is selected.", QuestionFlags: 0x10, QuestionId: 0x66D, VarStoreId: 0x4, VarOffset: 0x42D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 08 EB 08 6D 06 04 00 2D 04 10 10 00 01 00 }
0x4290C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x42913: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4291A: 				End  { 29 02 }
0x4291C: 			End  { 29 02 }
0x4291E: 		End  { 29 02 }
0x42920: 		GrayOutIf  { 19 82 }
0x42922: 			EqIdVal QuestionId: 0x2777, Value: 0x0 { 12 06 77 27 00 00 }
0x42928: 			OneOf Prompt: "OCSafeMode", Help: "OverClocking Safe Mode: When enabled, memory training uses less aggressive timing and algoes", QuestionFlags: 0x10, QuestionId: 0x66E, VarStoreId: 0x4, VarOffset: 0x478, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F8 08 F9 08 6E 06 04 00 78 04 10 10 00 01 00 }
0x42939: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x42940: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x42947: 			End  { 29 02 }
0x42949: 		End  { 29 02 }
0x4294B: 		GrayOutIf  { 19 82 }
0x4294D: 			EqIdVal QuestionId: 0x2777, Value: 0x1 { 12 86 77 27 01 00 }
0x42953: 				Not  { 17 02 }
0x42955: 			End  { 29 02 }
0x42957: 			OneOf Prompt: "Memory Reference Clock", Help: "100MHz, 133MHz.", QuestionFlags: 0x10, QuestionId: 0x66F, VarStoreId: 0x4, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 08 FB 08 6F 06 04 00 05 00 10 10 00 01 00 }
0x42968: 				OneOfOption Option: "133" Value: 0, Default, MfgDefault { 09 07 FD 08 30 00 00 }
0x4296F: 				OneOfOption Option: "100" Value: 1 { 09 07 FC 08 00 00 01 }
0x42976: 			End  { 29 02 }
0x42978: 			Numeric Prompt: "Memory Ratio", Help: "0 = Auto, or the frequency will equal ratio times reference clock. Set to 0 (Auto) to recalculate memory timings listed below.", QuestionFlags: 0x10, QuestionId: 0x670, VarStoreId: 0x4, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1 { 07 91 FE 08 FF 08 70 06 04 00 06 00 10 10 00 64 01 }
0x42989: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4298F: 			End  { 29 02 }
0x42991: 			Numeric Prompt: "  tCL", Help: "CAS Latency, 0: AUTO, max: 31", QuestionFlags: 0x14, QuestionId: 0x2778, VarStoreId: 0x4, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 00 09 01 09 78 27 04 00 08 00 14 10 00 FF 01 }
0x429A2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x429A8: 			End  { 29 02 }
0x429AA: 			Numeric Prompt: "  tRCD/tRP", Help: "RAS to CAS delay time and Row Precharge delay time, 0: AUTO, max: 63", QuestionFlags: 0x14, QuestionId: 0x2779, VarStoreId: 0x4, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 02 09 03 09 79 27 04 00 0E 00 14 10 00 FF 01 }
0x429BB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x429C1: 			End  { 29 02 }
0x429C3: 			Numeric Prompt: "  tRAS", Help: "RAS Active Time, 0: AUTO, max: 64", QuestionFlags: 0x14, QuestionId: 0x277A, VarStoreId: 0x4, VarOffset: 0xC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 04 09 05 09 7A 27 04 00 0C 00 14 11 00 00 FF FF 01 00 }
0x429D7: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x429DE: 			End  { 29 02 }
0x429E0: 			Numeric Prompt: "  tCWL", Help: "Min CAS Write Latency Delay Time, 0: AUTO, max: 20", QuestionFlags: 0x14, QuestionId: 0x277B, VarStoreId: 0x4, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 06 09 07 09 7B 27 04 00 09 00 14 10 00 FF 01 }
0x429F1: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x429F7: 			End  { 29 02 }
0x429F9: 			Numeric Prompt: "  tFAW", Help: "Min Four Activate Window Delay Time, 0: AUTO, max: 63", QuestionFlags: 0x14, QuestionId: 0x277C, VarStoreId: 0x4, VarOffset: 0xA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 08 09 09 09 7C 27 04 00 0A 00 14 11 00 00 FF FF 01 00 }
0x42A0D: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42A14: 			End  { 29 02 }
0x42A16: 			Numeric Prompt: "  tREFI", Help: "Refresh Interval, 0: AUTO, max: 65535", QuestionFlags: 0x14, QuestionId: 0x277D, VarStoreId: 0x4, VarOffset: 0xF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 0A 09 0B 09 7D 27 04 00 0F 00 14 11 00 00 FF FF 01 00 }
0x42A2A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42A31: 			End  { 29 02 }
0x42A33: 			Numeric Prompt: "  tRFC", Help: "Min Refresh Recovery Delay Time, 0: AUTO, max: 1023", QuestionFlags: 0x14, QuestionId: 0x277E, VarStoreId: 0x4, VarOffset: 0x11, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 0C 09 0D 09 7E 27 04 00 11 00 14 11 00 00 FF FF 01 00 }
0x42A47: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42A4E: 			End  { 29 02 }
0x42A50: 			Numeric Prompt: "  tRRD", Help: "Min Row Active to Row Active Delay Time, 0: AUTO, max: 31", QuestionFlags: 0x14, QuestionId: 0x277F, VarStoreId: 0x4, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 0E 09 0F 09 7F 27 04 00 13 00 14 10 00 FF 01 }
0x42A61: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42A67: 			End  { 29 02 }
0x42A69: 			Numeric Prompt: "  tRTP", Help: "Min Internal Read to Precharge Command Delay Time, 0: AUTO, max: 15. DDR4 legal values: 5, 6, 7, 8, 9, 10, 12", QuestionFlags: 0x14, QuestionId: 0x2780, VarStoreId: 0x4, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 10 09 11 09 80 27 04 00 14 00 14 10 00 FF 01 }
0x42A7A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42A80: 			End  { 29 02 }
0x42A82: 			Numeric Prompt: "  tWR", Help: "Min Write Recovery Time, 0: AUTO", QuestionFlags: 0x14, QuestionId: 0x2781, VarStoreId: 0x4, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 12 09 13 09 81 27 04 00 15 00 14 10 00 FF 01 }
0x42A93: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42A99: 			End  { 29 02 }
0x42A9B: 			Numeric Prompt: "  tWTR", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 28", QuestionFlags: 0x14, QuestionId: 0x2782, VarStoreId: 0x4, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 14 09 15 09 82 27 04 00 16 00 14 10 00 FF 01 }
0x42AAC: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42AB2: 			End  { 29 02 }
0x42AB4: 			Numeric Prompt: "  tRFCpb", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 15000", QuestionFlags: 0x14, QuestionId: 0x2783, VarStoreId: 0x4, VarOffset: 0x434, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3A98, Step: 0x1 { 07 94 16 09 17 09 83 27 04 00 34 04 14 11 00 00 98 3A 01 00 }
0x42AC8: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42ACF: 			End  { 29 02 }
0x42AD1: 			Numeric Prompt: "  tRFC2", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 15000", QuestionFlags: 0x14, QuestionId: 0x2784, VarStoreId: 0x4, VarOffset: 0x436, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3A98, Step: 0x1 { 07 94 18 09 19 09 84 27 04 00 36 04 14 11 00 00 98 3A 01 00 }
0x42AE5: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42AEC: 			End  { 29 02 }
0x42AEE: 			Numeric Prompt: "  tRFC4", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 15000", QuestionFlags: 0x14, QuestionId: 0x2785, VarStoreId: 0x4, VarOffset: 0x438, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3A98, Step: 0x1 { 07 94 1A 09 1B 09 85 27 04 00 38 04 14 11 00 00 98 3A 01 00 }
0x42B02: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42B09: 			End  { 29 02 }
0x42B0B: 			Numeric Prompt: "  tRRD_L", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max:80 ", QuestionFlags: 0x14, QuestionId: 0x2786, VarStoreId: 0x4, VarOffset: 0x43A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1C 09 1D 09 86 27 04 00 3A 04 14 10 00 FF 01 }
0x42B1C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42B22: 			End  { 29 02 }
0x42B24: 			Numeric Prompt: "  tRRD_S", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 80", QuestionFlags: 0x14, QuestionId: 0x2787, VarStoreId: 0x4, VarOffset: 0x43B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 1E 09 1F 09 87 27 04 00 3B 04 14 10 00 FF 01 }
0x42B35: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42B3B: 			End  { 29 02 }
0x42B3D: 			Numeric Prompt: "  tWTR_L", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 127", QuestionFlags: 0x14, QuestionId: 0x2788, VarStoreId: 0x4, VarOffset: 0x43C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 20 09 21 09 88 27 04 00 3C 04 14 10 00 FF 01 }
0x42B4E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42B54: 			End  { 29 02 }
0x42B56: 			Numeric Prompt: "  tCCD_L", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 80", QuestionFlags: 0x14, QuestionId: 0x2789, VarStoreId: 0x4, VarOffset: 0x43D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 22 09 23 09 89 27 04 00 3D 04 14 10 00 FF 01 }
0x42B67: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42B6D: 			End  { 29 02 }
0x42B6F: 			Numeric Prompt: "  tWTR_S", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 50", QuestionFlags: 0x14, QuestionId: 0x278A, VarStoreId: 0x4, VarOffset: 0x43E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 24 09 25 09 8A 27 04 00 3E 04 14 10 00 FF 01 }
0x42B80: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42B86: 			End  { 29 02 }
0x42B88: 			Numeric Prompt: "  NMode", Help: "System command rate, range 0-2, 0 means auto, 1 = 1N, 2 = 2N", QuestionFlags: 0x14, QuestionId: 0x278B, VarStoreId: 0x4, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x1 { 07 91 26 09 27 09 8B 27 04 00 17 00 14 10 00 02 01 }
0x42B99: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42B9F: 			End  { 29 02 }
0x42BA1: 		End  { 29 02 }
0x42BA3: 		GrayOutIf  { 19 82 }
0x42BA5: 			EqIdValList QuestionId: 0x2777, Values: [2, 3, 4, 5, 6] { 14 10 77 27 05 00 02 00 03 00 04 00 05 00 06 00 }
0x42BB5: 			Numeric Prompt: "Memory Voltage", Help: "Memory Voltage Override (Vdd) at DRAM Side. 0 = no override", QuestionFlags: 0x10, QuestionId: 0x671, VarStoreId: 0x4, VarOffset: 0x3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x5 { 07 94 28 09 29 09 71 06 04 00 03 00 10 11 00 00 D0 07 05 00 }
0x42BC9: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42BD0: 			End  { 29 02 }
0x42BD2: 			Numeric Prompt: "Memory Voltage VDDQ", Help: "Memory Voltage Override (Vddq) at DRAM Side. 0 = no override", QuestionFlags: 0x10, QuestionId: 0x672, VarStoreId: 0x4, VarOffset: 0x3F5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x5 { 07 94 2A 09 2B 09 72 06 04 00 F5 03 10 11 00 00 D0 07 05 00 }
0x42BE6: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42BED: 			End  { 29 02 }
0x42BEF: 			Numeric Prompt: "Memory Voltage VPP", Help: "Memory Voltage Override (Vpp) at DRAM Side. 0 = no override", QuestionFlags: 0x10, QuestionId: 0x673, VarStoreId: 0x4, VarOffset: 0x3F7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x8FC, Step: 0x5 { 07 94 2C 09 2D 09 73 06 04 00 F7 03 10 11 00 00 FC 08 05 00 }
0x42C03: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x42C0A: 			End  { 29 02 }
0x42C0C: 		End  { 29 02 }
0x42C0E: 		Text Prompt: "VDD", Help: "", Text: "N/A" { 03 08 2E 09 C9 07 2F 09 }
0x42C16: 	End  { 29 02 }
0x42C18: 	Form FormId: 0x27B0, Title: "Graphics Configuration" { 01 86 B0 27 65 0A }
0x42C1E: 		Subtitle Prompt: "Graphics Configuration", Help: "", Flags: 0x0 { 02 87 65 0A 00 00 00 }
0x42C25: 		End  { 29 02 }
0x42C27: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x42C2E: 		End  { 29 02 }
0x42C30: 		SuppressIf  { 0A 82 }
0x42C32: 			EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x42C38: 			Numeric Prompt: "Graphics Turbo IMON Current", Help: "Graphics turbo IMON current values supported (14-31)", QuestionFlags: 0x10, QuestionId: 0x674, VarStoreId: 0x4, VarOffset: 0xB8, Flags: 0x10, Size: 8, Min: 0xE, Max: 0x1F, Step: 0x1 { 07 91 66 0A 67 0A 74 06 04 00 B8 00 10 10 0E 1F 01 }
0x42C49: 				Default DefaultId: 0x0 Value: 31 { 5B 06 00 00 00 1F }
0x42C4F: 			End  { 29 02 }
0x42C51: 		End  { 29 02 }
0x42C53: 		OneOf Prompt: "Skip Scaning of External Gfx Card", Help: "If Enable, it will not scan for External Gfx Card on PEG and PCH PCIE Ports", QuestionFlags: 0x10, QuestionId: 0x675, VarStoreId: 0x4, VarOffset: 0x256, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 0A 69 0A 75 06 04 00 56 02 10 10 00 01 00 }
0x42C64: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42C6B: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42C72: 		End  { 29 02 }
0x42C74: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x42C7B: 		End  { 29 02 }
0x42C7D: 		SuppressIf  { 0A 82 }
0x42C7F: 			EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x42C85: 				Not  { 17 02 }
0x42C87: 				EqIdVal QuestionId: 0x1142, Value: 0x5 { 12 06 42 11 05 00 }
0x42C8D: 				Not  { 17 02 }
0x42C8F: 				And  { 15 02 }
0x42C91: 				EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x42C97: 				Not  { 17 02 }
0x42C99: 				And  { 15 02 }
0x42C9B: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x42CA1: 				Not  { 17 02 }
0x42CA3: 				And  { 15 02 }
0x42CA5: 				EqIdVal QuestionId: 0x1142, Value: 0x3 { 12 06 42 11 03 00 }
0x42CAB: 				Not  { 17 02 }
0x42CAD: 				And  { 15 02 }
0x42CAF: 			End  { 29 02 }
0x42CB1: 			OneOf Prompt: "Primary Display", Help: "Select which of IGFX/PEG/PCI Graphics device should be Primary Display Or select HG for Hybrid Gfx.", QuestionFlags: 0x10, QuestionId: 0x676, VarStoreId: 0x4, VarOffset: 0xB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5F 0A 60 0A 76 06 04 00 B1 00 10 10 00 04 00 }
0x42CC2: 				OneOfOption Option: "Auto" Value: 3 { 09 07 90 00 00 00 03 }
0x42CC9: 				OneOfOption Option: "IGFX" Value: 0 { 09 07 61 0A 00 00 00 }
0x42CD0: 				OneOfOption Option: "PEG Slot" Value: 1 { 09 07 62 0A 00 00 01 }
0x42CD7: 				OneOfOption Option: "PCH PCI" Value: 2 { 09 07 63 0A 00 00 02 }
0x42CDE: 				OneOfOption Option: "HG" Value: 4, Default, MfgDefault { 09 07 64 0A 30 00 04 }
0x42CE5: 			End  { 29 02 }
0x42CE7: 		End  { 29 02 }
0x42CE9: 		SuppressIf  { 0A 82 }
0x42CEB: 			EqIdVal QuestionId: 0x676, Value: 0x4 { 12 86 76 06 04 00 }
0x42CF1: 				Not  { 17 02 }
0x42CF3: 			End  { 29 02 }
0x42CF5: 			OneOf Prompt: "HG Support", Help: "HG Support on PEG Port", QuestionFlags: 0x10, QuestionId: 0x677, VarStoreId: 0x4, VarOffset: 0x41B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 6E 0A 6F 0A 77 06 04 00 1B 04 10 10 00 02 00 }
0x42D06: 				OneOfOption Option: "PEG10" Value: 0, Default, MfgDefault { 09 07 70 0A 30 00 00 }
0x42D0D: 				OneOfOption Option: "PEG60" Value: 1 { 09 07 71 0A 00 00 01 }
0x42D14: 				OneOfOption Option: "PEG62" Value: 2 { 09 07 72 0A 00 00 02 }
0x42D1B: 			End  { 29 02 }
0x42D1D: 			OneOf Prompt: "Select PCIE Card", Help: "Select the card used on the platform
Auto       : Skip GPIO based Power Enable to dGPU
Elk Creek 4: DGPU Power Enable = ActiveLow
PEG Eval   : DGPU Power Enable = ActiveHigh", QuestionFlags: 0x10, QuestionId: 0x678, VarStoreId: 0x4, VarOffset: 0xB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 6A 0A 6B 0A 78 06 04 00 B2 00 10 10 00 02 00 }
0x42D2E: 				OneOfOption Option: "Auto" Value: 2 { 09 07 90 00 00 00 02 }
0x42D35: 				OneOfOption Option: "Elk Creek 4" Value: 0 { 09 07 6C 0A 00 00 00 }
0x42D3C: 				OneOfOption Option: "PEG Eval" Value: 1, Default, MfgDefault { 09 07 6D 0A 30 00 01 }
0x42D43: 			End  { 29 02 }
0x42D45: 			Numeric Prompt: "HG Delay After Power Enable", Help: "Delay in milli-seconds after power enable", QuestionFlags: 0x0, QuestionId: 0x679, VarStoreId: 0x4, VarOffset: 0xB3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x0 { 07 94 73 0A 74 0A 79 06 04 00 B3 00 00 11 00 00 E8 03 00 00 }
0x42D59: 				Default DefaultId: 0x0 Value: 300 { 5B 07 00 00 01 2C 01 }
0x42D60: 			End  { 29 02 }
0x42D62: 			Numeric Prompt: "HG Delay After Hold Reset", Help: "Delay in milli-seconds after hold reset", QuestionFlags: 0x0, QuestionId: 0x67A, VarStoreId: 0x4, VarOffset: 0xB5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x0 { 07 94 75 0A 76 0A 7A 06 04 00 B5 00 00 11 00 00 E8 03 00 00 }
0x42D76: 				Default DefaultId: 0x0 Value: 100 { 5B 07 00 00 01 64 00 }
0x42D7D: 			End  { 29 02 }
0x42D7F: 		End  { 29 02 }
0x42D81: 		Ref Prompt: "External Gfx Card Primary Display Configuration", Help: "External Gfx Card Primary Display Configuration", QuestionFlags: 0x0, QuestionId: 0x67B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F8 { 0F 0F 6C 00 6C 00 7B 06 00 00 FF FF 00 F8 28 }
0x42D90: 		OneOf Prompt: "Internal Graphics", Help: "Keep IGFX enabled based on the setup options.", QuestionFlags: 0x10, QuestionId: 0x67C, VarStoreId: 0x4, VarOffset: 0xB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 78 0A 79 0A 7C 06 04 00 B7 00 10 10 00 02 00 }
0x42DA1: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x42DA7: 			OneOfOption Option: "Auto" Value: 2 { 09 07 90 00 00 00 02 }
0x42DAE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42DB5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42DBC: 		End  { 29 02 }
0x42DBE: 		OneOf Prompt: "GTT Size", Help: "Select the GTT Size ", QuestionFlags: 0x10, QuestionId: 0x67D, VarStoreId: 0x4, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0 { 05 91 F2 0A F3 0A 7D 06 04 00 33 00 10 10 01 03 00 }
0x42DCF: 			OneOfOption Option: "2MB" Value: 1 { 09 07 F4 0A 00 00 01 }
0x42DD6: 			OneOfOption Option: "4MB" Value: 2 { 09 07 F5 0A 00 00 02 }
0x42DDD: 			OneOfOption Option: "8MB" Value: 3, Default, MfgDefault { 09 07 F6 0A 30 00 03 }
0x42DE4: 		End  { 29 02 }
0x42DE6: 		OneOf Prompt: "Aperture Size", Help: "Select the Aperture Size

Note : Above 4GB MMIO BIOS assignment is automatically enabled when selecting 2048MB aperture. To use this feature, please disable CSM Support.", QuestionFlags: 0x10, QuestionId: 0x278C, VarStoreId: 0x4, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 F7 0A F8 0A 8C 27 04 00 34 00 10 10 00 07 00 }
0x42DF7: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x42DFC: 				Value  { 5A 82 }
0x42DFE: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x42E08: 				End  { 29 02 }
0x42E0A: 			End  { 29 02 }
0x42E0C: 			OneOfOption Option: "128MB" Value: 0 { 09 07 F9 0A 00 00 00 }
0x42E13: 			OneOfOption Option: "256MB" Value: 1 { 09 07 FA 0A 00 00 01 }
0x42E1A: 			OneOfOption Option: "512MB" Value: 3 { 09 07 FB 0A 00 00 03 }
0x42E21: 			OneOfOption Option: "1024MB" Value: 7 { 09 07 FC 0A 00 00 07 }
0x42E28: 		End  { 29 02 }
0x42E2A: 		SuppressIf  { 0A 82 }
0x42E2C: 			True  { 46 02 }
0x42E2E: 			OneOf Prompt: "PSMI SUPPORT", Help: "PSMI Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x67E, VarStoreId: 0x4, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 0A FE 0A 7E 06 04 00 35 00 10 10 00 01 00 }
0x42E3F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42E46: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x42E4D: 			End  { 29 02 }
0x42E4F: 			SuppressIf  { 0A 82 }
0x42E51: 				EqIdVal QuestionId: 0x67E, Value: 0x0 { 12 06 7E 06 00 00 }
0x42E57: 				OneOf Prompt: "PSMI Region Size", Help: "Select the PSMI Region Size : Range from 32MB to 1024MB", QuestionFlags: 0x10, QuestionId: 0x67F, VarStoreId: 0x4, VarOffset: 0x36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 FF 0A 00 0B 7F 06 04 00 36 00 10 10 00 04 00 }
0x42E68: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x42E6D: 						Value  { 5A 82 }
0x42E6F: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x42E79: 						End  { 29 02 }
0x42E7B: 					End  { 29 02 }
0x42E7D: 					OneOfOption Option: "32MB" Value: 0 { 09 07 01 0B 00 00 00 }
0x42E84: 					OneOfOption Option: "288MB" Value: 1 { 09 07 02 0B 00 00 01 }
0x42E8B: 					OneOfOption Option: "544MB" Value: 2 { 09 07 03 0B 00 00 02 }
0x42E92: 					OneOfOption Option: "800MB" Value: 3 { 09 07 04 0B 00 00 03 }
0x42E99: 					OneOfOption Option: "1024MB" Value: 4 { 09 07 05 0B 00 00 04 }
0x42EA0: 				End  { 29 02 }
0x42EA2: 			End  { 29 02 }
0x42EA4: 		End  { 29 02 }
0x42EA6: 		OneOf Prompt: "DVMT Pre-Allocated", Help: "Select DVMT 5.0 Pre-Allocated (Fixed) Graphics Memory size used by the Internal Graphics Device.", QuestionFlags: 0x10, QuestionId: 0x278D, VarStoreId: 0x4, VarOffset: 0x7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFE, Step: 0x0 { 05 91 39 0A 4F 0A 8D 27 04 00 7A 00 10 10 00 FE 00 }
0x42EB7: 			Default DefaultId: 0x0 Value: 254 { 5B 06 00 00 00 FE }
0x42EBD: 			OneOfOption Option: "0M" Value: 0 { 09 07 3A 0A 00 00 00 }
0x42EC4: 			OneOfOption Option: "32M" Value: 1 { 09 07 3B 0A 00 00 01 }
0x42ECB: 			OneOfOption Option: "64M" Value: 2 { 09 07 3C 0A 00 00 02 }
0x42ED2: 			OneOfOption Option: "96M" Value: 3 { 09 07 3D 0A 00 00 03 }
0x42ED9: 			OneOfOption Option: "128M" Value: 4 { 09 07 3E 0A 00 00 04 }
0x42EE0: 			OneOfOption Option: "160M" Value: 5 { 09 07 3F 0A 00 00 05 }
0x42EE7: 			OneOfOption Option: "4M" Value: 240 { 09 07 40 0A 00 00 F0 }
0x42EEE: 			OneOfOption Option: "8M" Value: 241 { 09 07 41 0A 00 00 F1 }
0x42EF5: 			OneOfOption Option: "12M" Value: 242 { 09 07 42 0A 00 00 F2 }
0x42EFC: 			OneOfOption Option: "16M" Value: 243 { 09 07 43 0A 00 00 F3 }
0x42F03: 			OneOfOption Option: "20M" Value: 244 { 09 07 44 0A 00 00 F4 }
0x42F0A: 			OneOfOption Option: "24M" Value: 245 { 09 07 45 0A 00 00 F5 }
0x42F11: 			OneOfOption Option: "28M" Value: 246 { 09 07 46 0A 00 00 F6 }
0x42F18: 			OneOfOption Option: "32M/F7" Value: 247 { 09 07 47 0A 00 00 F7 }
0x42F1F: 			OneOfOption Option: "36M" Value: 248 { 09 07 48 0A 00 00 F8 }
0x42F26: 			OneOfOption Option: "40M" Value: 249 { 09 07 49 0A 00 00 F9 }
0x42F2D: 			OneOfOption Option: "44M" Value: 250 { 09 07 4A 0A 00 00 FA }
0x42F34: 			OneOfOption Option: "48M" Value: 251 { 09 07 4B 0A 00 00 FB }
0x42F3B: 			OneOfOption Option: "52M" Value: 252 { 09 07 4C 0A 00 00 FC }
0x42F42: 			OneOfOption Option: "56M" Value: 253 { 09 07 4D 0A 00 00 FD }
0x42F49: 			OneOfOption Option: "60M" Value: 254 { 09 07 4E 0A 00 00 FE }
0x42F50: 		End  { 29 02 }
0x42F52: 		OneOf Prompt: "Intel Graphics Pei Display Peim", Help: "Enable/Disable Pei (Early) Display", QuestionFlags: 0x10, QuestionId: 0x680, VarStoreId: 0x4, VarOffset: 0x39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 0B 23 0B 80 06 04 00 39 00 10 10 00 01 00 }
0x42F63: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x42F69: 			OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 91 00 20 00 01 }
0x42F70: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42F77: 		End  { 29 02 }
0x42F79: 		SuppressIf  { 0A 82 }
0x42F7B: 			True  { 46 02 }
0x42F7D: 			OneOf Prompt: "ALS Support", Help: "Valid only for ACPI.

Legacy = ALS Support through the IGFX INT10 function.

ACPI = ALS support through an ACPI ALS driver.", QuestionFlags: 0x10, QuestionId: 0x681, VarStoreId: 0x4, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 3A 0B 3B 0B 81 06 04 00 30 00 10 10 00 02 00 }
0x42F8E: 				OneOfOption Option: "Enabled" Value: 2 { 09 07 91 00 00 00 02 }
0x42F95: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x42F9C: 			End  { 29 02 }
0x42F9E: 		End  { 29 02 }
0x42FA0: 		SuppressIf  { 0A 82 }
0x42FA2: 			EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x42FA8: 			OneOf Prompt: "VDD Enable", Help: "Enable/Disable forcing of VDD in the BIOS", QuestionFlags: 0x10, QuestionId: 0x682, VarStoreId: 0x4, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 0B 3D 0B 82 06 04 00 37 00 10 10 00 01 00 }
0x42FB9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42FC0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x42FC7: 			End  { 29 02 }
0x42FC9: 		End  { 29 02 }
0x42FCB: 		OneOf Prompt: "Configure GT for use", Help: "Enable/Disable GT configuration in BIOS", QuestionFlags: 0x10, QuestionId: 0x278E, VarStoreId: 0x4, VarOffset: 0x38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 0B 25 0B 8E 27 04 00 38 00 10 10 00 01 00 }
0x42FDC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x42FE3: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x42FEA: 		End  { 29 02 }
0x42FEC: 		SuppressIf  { 0A 82 }
0x42FEE: 			EqIdVal QuestionId: 0x278E, Value: 0x0 { 12 06 8E 27 00 00 }
0x42FF4: 			OneOf Prompt: "RC1p Support", Help: "Enable/Disable RC1p support. If RC1p is enabled, send a RC1p frequency request to PMA based other conditions being met", QuestionFlags: 0x10, QuestionId: 0x683, VarStoreId: 0x4, VarOffset: 0x42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 0B 27 0B 83 06 04 00 42 00 10 10 00 01 00 }
0x43005: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4300C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x43013: 			End  { 29 02 }
0x43015: 		End  { 29 02 }
0x43017: 		OneOf Prompt: "PAVP Enable", Help: "Enable/Disable PAVP", QuestionFlags: 0x10, QuestionId: 0x684, VarStoreId: 0x4, VarOffset: 0x3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 0B 29 0B 84 06 04 00 3A 00 10 10 00 01 00 }
0x43028: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x4302F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x43036: 		End  { 29 02 }
0x43038: 		OneOf Prompt: "Cdynmax Clamping Enable", Help: "Enable/Disable Cdynmax Clamping", QuestionFlags: 0x10, QuestionId: 0x685, VarStoreId: 0x4, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 0B 2B 0B 85 06 04 00 3D 00 10 10 00 01 00 }
0x43049: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x43050: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x43057: 		End  { 29 02 }
0x43059: 		OneOf Prompt: "Cd Clock Frequency", Help: "Select the highest Cd Clock frequency supported by the platform", QuestionFlags: 0x10, QuestionId: 0x686, VarStoreId: 0x4, VarOffset: 0x3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 2C 0B 2D 0B 86 06 04 00 3E 00 10 10 00 FF 00 }
0x4306A: 			SuppressIf  { 0A 82 }
0x4306C: 				EqIdVal QuestionId: 0x116F, Value: 0x1 { 12 86 6F 11 01 00 }
0x43072: 					EqIdVal QuestionId: 0x116F, Value: 0x0 { 12 06 6F 11 00 00 }
0x43078: 					Or  { 16 02 }
0x4307A: 				End  { 29 02 }
0x4307C: 				OneOfOption Option: "192 Mhz" Value: 0 { 09 07 2E 0B 00 00 00 }
0x43083: 				OneOfOption Option: "312 Mhz" Value: 2 { 09 07 30 0B 00 00 02 }
0x4308A: 				OneOfOption Option: "324 Mhz" Value: 3 { 09 07 31 0B 00 00 03 }
0x43091: 				OneOfOption Option: "552 Mhz" Value: 5 { 09 07 33 0B 00 00 05 }
0x43098: 				OneOfOption Option: "648 Mhz" Value: 7 { 09 07 35 0B 00 00 07 }
0x4309F: 			End  { 29 02 }
0x430A1: 			SuppressIf  { 0A 82 }
0x430A3: 				EqIdVal QuestionId: 0x116F, Value: 0x2 { 12 06 6F 11 02 00 }
0x430A9: 				OneOfOption Option: "192 Mhz" Value: 0 { 09 07 2E 0B 00 00 00 }
0x430B0: 				OneOfOption Option: "307.2 Mhz" Value: 1 { 09 07 2F 0B 00 00 01 }
0x430B7: 				OneOfOption Option: "326.4 Mhz" Value: 4 { 09 07 32 0B 00 00 04 }
0x430BE: 				OneOfOption Option: "556.8 Mhz" Value: 6 { 09 07 34 0B 00 00 06 }
0x430C5: 				OneOfOption Option: "652.8 Mhz" Value: 8 { 09 07 36 0B 00 00 08 }
0x430CC: 			End  { 29 02 }
0x430CE: 			OneOfOption Option: "Max CdClock freq based on Reference Clk" Value: 255, Default, MfgDefault { 09 07 37 0B 30 00 FF }
0x430D5: 		End  { 29 02 }
0x430D7: 		OneOf Prompt: "Skip Full CD Clock Init", Help: "Enabled: Skip Full CD clock initializaton.
Disabled: Initialize the full CD clock if not initialized by Gfx PEIM", QuestionFlags: 0x10, QuestionId: 0x687, VarStoreId: 0x4, VarOffset: 0x41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 0B 39 0B 87 06 04 00 41 00 10 10 00 01 00 }
0x430E8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x430EF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x430F6: 		End  { 29 02 }
0x430F8: 		OneOf Prompt: "VBT Select", Help: "Select VBT for GOP Driver
Select Vbt to MIPI if any of the Display has MIPI", QuestionFlags: 0x10, QuestionId: 0x688, VarStoreId: 0x4, VarOffset: 0x3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 49 0E 4A 0E 88 06 04 00 3B 00 10 10 00 01 00 }
0x43109: 			OneOfOption Option: "eDP" Value: 0, Default { 09 07 4B 0E 10 00 00 }
0x43110: 			OneOfOption Option: "MIPI" Value: 1 { 09 07 4C 0E 00 00 01 }
0x43117: 		End  { 29 02 }
0x43119: 		OneOf Prompt: "Enable Display Audio Link in Pre-OS", Help: "Enable : Display Audio Link will be enabled in Pre-OS.
Disabled : Display Audio Link will be disabled in Pre-OS.", QuestionFlags: 0x10, QuestionId: 0x689, VarStoreId: 0x4, VarOffset: 0x3EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4D 0E 4E 0E 89 06 04 00 EE 03 10 10 00 01 00 }
0x4312A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x43131: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x43138: 		End  { 29 02 }
0x4313A: 		OneOf Prompt: "IUER Button Enable", Help: "Enable/Disable IUER Button Functionality", QuestionFlags: 0x10, QuestionId: 0x68A, VarStoreId: 0x4, VarOffset: 0x25C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 62 0E 63 0E 8A 06 04 00 5C 02 10 10 00 01 00 }
0x4314B: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43151: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x43158: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4315F: 		End  { 29 02 }
0x43161: 		SuppressIf  { 0A 82 }
0x43163: 			EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x43169: 			Ref Prompt: "LCD Control", Help: "LCD Control", QuestionFlags: 0x0, QuestionId: 0x68B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B7 { 0F 0F 77 0A 77 0A 8B 06 00 00 FF FF 00 B7 27 }
0x43178: 		End  { 29 02 }
0x4317A: 		SuppressIf  { 0A 82 }
0x4317C: 			EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x43182: 				Not  { 17 02 }
0x43184: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x4318A: 				Not  { 17 02 }
0x4318C: 				And  { 15 02 }
0x4318E: 			End  { 29 02 }
0x43190: 			Ref Prompt: "Intel(R) Ultrabook Event Support", Help: "Intel(R) Ultrabook Event Support", QuestionFlags: 0x0, QuestionId: 0x68C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B8 { 0F 0F 4F 0E 4F 0E 8C 06 00 00 FF FF 00 B8 27 }
0x4319F: 		End  { 29 02 }
0x431A1: 	End  { 29 02 }
0x431A3: 	Form FormId: 0x27B1, Title: "DMI/OPI Configuration" { 01 86 B1 27 3E 0B }
0x431A9: 		Subtitle Prompt: "DMI/OPI Configuration", Help: "", Flags: 0x0 { 02 87 3E 0B 00 00 00 }
0x431B0: 		End  { 29 02 }
0x431B2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x431B9: 		End  { 29 02 }
0x431BB: 		SuppressIf  { 0A 82 }
0x431BD: 			EqIdVal QuestionId: 0x1112, Value: 0x1 { 12 86 12 11 01 00 }
0x431C3: 				Not  { 17 02 }
0x431C5: 			End  { 29 02 }
0x431C7: 			Text Prompt: "DMI", Help: "DMI Link and Speed Information", Text: "N/A" { 03 08 C0 0D BF 0D C1 0D }
0x431CF: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x431D6: 			End  { 29 02 }
0x431D8: 			OneOf Prompt: "DMI Max Link Speed", Help: "Set DMI Speed Gen1/Gen2/Gen3", QuestionFlags: 0x10, QuestionId: 0x68D, VarStoreId: 0x4, VarOffset: 0x8B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 C8 0D C9 0D 8D 06 04 00 8B 00 10 10 01 04 00 }
0x431E9: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x431F0: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x431F7: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x431FE: 				OneOfOption Option: "Gen4" Value: 4, Default, MfgDefault { 09 07 D7 0E 30 00 04 }
0x43205: 			End  { 29 02 }
0x43207: 		End  { 29 02 }
0x43209: 		OneOf Prompt: "CDR Relock for CPU DMI", Help: "Enable/Disable CDR Relock", QuestionFlags: 0x10, QuestionId: 0x68E, VarStoreId: 0x4, VarOffset: 0x3FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 0E F2 0E 8E 06 04 00 FE 03 10 10 00 01 00 }
0x4321A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x43221: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x43228: 		End  { 29 02 }
0x4322A: 		SuppressIf  { 0A 82 }
0x4322C: 			EqIdVal QuestionId: 0x1112, Value: 0x1 { 12 06 12 11 01 00 }
0x43232: 			OneOf Prompt: "DMI Gen3 Eq Phase 2", Help: "Perform Gen3 Equalization Phase 2", QuestionFlags: 0x10, QuestionId: 0x68F, VarStoreId: 0x4, VarOffset: 0x8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 04 0E 05 0E 8F 06 04 00 8D 00 10 10 00 02 00 }
0x43243: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x4324A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x43251: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x43258: 				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled" { 11 84 06 0E }
0x4325C: 					EqIdVal QuestionId: 0x68F, Value: 0x0 { 12 86 8F 06 00 00 }
0x43262: 						EqIdVal QuestionId: 0x690, Value: 0x1 { 12 06 90 06 01 00 }
0x43268: 						And  { 15 02 }
0x4326A: 					End  { 29 02 }
0x4326C: 				End  { 29 02 }
0x4326E: 			End  { 29 02 }
0x43270: 			OneOf Prompt: "DMI Gen3 Eq Phase 3 Method", Help: "Select Method for Gen3 Equalization Phase 3", QuestionFlags: 0x10, QuestionId: 0x690, VarStoreId: 0x4, VarOffset: 0x8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 FF 0D 00 0E 90 06 04 00 8E 00 10 10 00 04 00 }
0x43281: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 90 00 30 00 00 }
0x43288: 				OneOfOption Option: "Adaptive Hardware Equalization" Value: 1 { 09 07 01 0E 00 00 01 }
0x4328F: 				OneOfOption Option: "Adaptive Software Equalization" Value: 2 { 09 07 02 0E 00 00 02 }
0x43296: 				OneOfOption Option: "Static Equalization" Value: 3 { 09 07 03 0E 00 00 03 }
0x4329D: 				OneOfOption Option: "Disabled" Value: 4 { 09 07 92 00 00 00 04 }
0x432A4: 				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled" { 11 84 E8 10 }
0x432A8: 					EqIdVal QuestionId: 0x68F, Value: 0x0 { 12 86 8F 06 00 00 }
0x432AE: 						EqIdVal QuestionId: 0x690, Value: 0x1 { 12 06 90 06 01 00 }
0x432B4: 						And  { 15 02 }
0x432B6: 					End  { 29 02 }
0x432B8: 				End  { 29 02 }
0x432BA: 			End  { 29 02 }
0x432BC: 			SuppressIf  { 0A 82 }
0x432BE: 				EqIdVal QuestionId: 0x1112, Value: 0x1 { 12 86 12 11 01 00 }
0x432C4: 					Not  { 17 02 }
0x432C6: 				End  { 29 02 }
0x432C8: 				OneOf Prompt: "Program Static Phase1 Eq", Help: "Program Phase1 Presets/CTLEp", QuestionFlags: 0x10, QuestionId: 0x691, VarStoreId: 0x4, VarOffset: 0x8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 0D FE 0D 91 06 04 00 8F 00 10 10 00 01 00 }
0x432D9: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x432E0: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 91 00 30 00 01 }
0x432E7: 				End  { 29 02 }
0x432E9: 				SuppressIf  { 0A 82 }
0x432EB: 					EqIdVal QuestionId: 0x691, Value: 0x0 { 12 06 91 06 00 00 }
0x432F1: 					Ref Prompt: " Gen3 Root Port Preset value for each Lane", Help: "Root Port preset value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x692, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B2 { 0F 0F 11 0E 12 0E 92 06 00 00 FF FF 00 B2 27 }
0x43300: 					Ref Prompt: " Gen3 Endpoint Preset value for each Lane", Help: "Endpoint preset value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x693, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B3 { 0F 0F 13 0E 14 0E 93 06 00 00 FF FF 00 B3 27 }
0x4330F: 					Ref Prompt: " Gen3 Endpoint Hint value for each Lane", Help: "Endpoint Hint value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x694, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B4 { 0F 0F 15 0E 16 0E 94 06 00 00 FF FF 00 B4 27 }
0x4331E: 				End  { 29 02 }
0x43320: 				Ref Prompt: "Gen3 RxCTLE Control", Help: "Gen3 RxCTLE Control per Bundle", QuestionFlags: 0x0, QuestionId: 0x695, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B5 { 0F 0F 07 0E 08 0E 95 06 00 00 FF FF 00 B5 27 }
0x4332F: 				OneOf Prompt: "DMI De-emphasis Control", Help: "Configure the De-emphasis control on DMI", QuestionFlags: 0x10, QuestionId: 0x696, VarStoreId: 0x4, VarOffset: 0x8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 0D FA 0D 96 06 04 00 8C 00 10 10 00 01 00 }
0x43340: 					OneOfOption Option: "-6 dB" Value: 0 { 09 07 FB 0D 00 00 00 }
0x43347: 					OneOfOption Option: "-3.5 dB" Value: 1, Default, MfgDefault { 09 07 FC 0D 30 00 01 }
0x4334E: 				End  { 29 02 }
0x43350: 			End  { 29 02 }
0x43352: 			OneOf Prompt: "DMI Gen3 ASPM", Help: "DMI Gen3 ASPM Support", QuestionFlags: 0x10, QuestionId: 0x697, VarStoreId: 0x4, VarOffset: 0xAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 C2 0D C3 0D 97 06 04 00 AC 00 10 10 00 04 00 }
0x43363: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x4336A: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x43371: 				OneOfOption Option: "ASPM L0s" Value: 1 { 09 07 F6 0D 00 00 01 }
0x43378: 				OneOfOption Option: "ASPM L1" Value: 2, Default, MfgDefault { 09 07 F8 0D 30 00 02 }
0x4337F: 				OneOfOption Option: "ASPM L0sL1" Value: 3 { 09 07 F7 0D 00 00 03 }
0x43386: 			End  { 29 02 }
0x43388: 		End  { 29 02 }
0x4338A: 		OneOf Prompt: "DMI ASPM", Help: "DMI ASPM Support", QuestionFlags: 0x10, QuestionId: 0x698, VarStoreId: 0x4, VarOffset: 0xAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 C4 0D C5 0D 98 06 04 00 AD 00 10 10 00 04 00 }
0x4339B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x433A2: 			OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x433A9: 			OneOfOption Option: "ASPM L0s" Value: 1 { 09 07 F6 0D 00 00 01 }
0x433B0: 			OneOfOption Option: "ASPM L1" Value: 2, Default, MfgDefault { 09 07 F8 0D 30 00 02 }
0x433B7: 			OneOfOption Option: "ASPM L0sL1" Value: 3 { 09 07 F7 0D 00 00 03 }
0x433BE: 		End  { 29 02 }
0x433C0: 		Numeric Prompt: "DMI Gen3 L1 Exit Latency", Help: "DMI Gen3 L1 Exit Latency", QuestionFlags: 0x10, QuestionId: 0x699, VarStoreId: 0x4, VarOffset: 0xAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 C6 0D C7 0D 99 06 04 00 AE 00 10 10 00 07 01 }
0x433D1: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x433D7: 		End  { 29 02 }
0x433D9: 		OneOf Prompt: "New FOM for CPU DMI", Help: "Enable/Disable New FOM", QuestionFlags: 0x10, QuestionId: 0x69A, VarStoreId: 0x4, VarOffset: 0x3FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EE 0E EF 0E 9A 06 04 00 FD 03 10 10 00 01 00 }
0x433EA: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x433F1: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x433F8: 		End  { 29 02 }
0x433FA: 		Ref Prompt: "DMI Advanced Menu", Help: "DMI Advanced Menu", QuestionFlags: 0x0, QuestionId: 0x69B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B6 { 0F 0F CE 0D CE 0D 9B 06 00 00 FF FF 00 B6 27 }
0x43409: 	End  { 29 02 }
0x4340B: 	Form FormId: 0x27B2, Title: " Gen3 Root Port Preset value for each Lane" { 01 86 B2 27 11 0E }
0x43411: 		Subtitle Prompt: " Gen3 Root Port Preset value for each Lane", Help: "", Flags: 0x0 { 02 87 11 0E 00 00 00 }
0x43418: 		End  { 29 02 }
0x4341A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x43421: 		End  { 29 02 }
0x43423: 		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x69C, VarStoreId: 0x4, VarOffset: 0x90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 17 0E 18 0E 9C 06 04 00 90 00 10 10 00 09 01 }
0x43434: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x4343A: 		End  { 29 02 }
0x4343C: 		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x69D, VarStoreId: 0x4, VarOffset: 0x91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 19 0E 1A 0E 9D 06 04 00 91 00 10 10 00 09 01 }
0x4344D: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x43453: 		End  { 29 02 }
0x43455: 		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x69E, VarStoreId: 0x4, VarOffset: 0x92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 1B 0E 1C 0E 9E 06 04 00 92 00 10 10 00 09 01 }
0x43466: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x4346C: 		End  { 29 02 }
0x4346E: 		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x69F, VarStoreId: 0x4, VarOffset: 0x93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 1D 0E 1E 0E 9F 06 04 00 93 00 10 10 00 09 01 }
0x4347F: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x43485: 		End  { 29 02 }
0x43487: 		Numeric Prompt: " Lane 4", Help: " Value for Lane 4", QuestionFlags: 0x10, QuestionId: 0x6A0, VarStoreId: 0x4, VarOffset: 0x94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 1F 0E 20 0E A0 06 04 00 94 00 10 10 00 09 01 }
0x43498: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x4349E: 		End  { 29 02 }
0x434A0: 		Numeric Prompt: " Lane 5", Help: " Value for Lane 5", QuestionFlags: 0x10, QuestionId: 0x6A1, VarStoreId: 0x4, VarOffset: 0x95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 21 0E 22 0E A1 06 04 00 95 00 10 10 00 09 01 }
0x434B1: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x434B7: 		End  { 29 02 }
0x434B9: 		Numeric Prompt: " Lane 6", Help: " Value for Lane 6", QuestionFlags: 0x10, QuestionId: 0x6A2, VarStoreId: 0x4, VarOffset: 0x96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 23 0E 24 0E A2 06 04 00 96 00 10 10 00 09 01 }
0x434CA: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x434D0: 		End  { 29 02 }
0x434D2: 		Numeric Prompt: " Lane 7", Help: " Value for Lane 7", QuestionFlags: 0x10, QuestionId: 0x6A3, VarStoreId: 0x4, VarOffset: 0x97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 25 0E 26 0E A3 06 04 00 97 00 10 10 00 09 01 }
0x434E3: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x434E9: 		End  { 29 02 }
0x434EB: 	End  { 29 02 }
0x434ED: 	Form FormId: 0x27B3, Title: " Gen3 Endpoint Preset value for each Lane" { 01 86 B3 27 13 0E }
0x434F3: 		Subtitle Prompt: " Gen3 Endpoint Preset value for each Lane", Help: "", Flags: 0x0 { 02 87 13 0E 00 00 00 }
0x434FA: 		End  { 29 02 }
0x434FC: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x43503: 		End  { 29 02 }
0x43505: 		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x6A4, VarStoreId: 0x4, VarOffset: 0x98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 27 0E 28 0E A4 06 04 00 98 00 10 10 00 09 01 }
0x43516: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4351C: 		End  { 29 02 }
0x4351E: 		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x6A5, VarStoreId: 0x4, VarOffset: 0x99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 29 0E 2A 0E A5 06 04 00 99 00 10 10 00 09 01 }
0x4352F: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x43535: 		End  { 29 02 }
0x43537: 		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x6A6, VarStoreId: 0x4, VarOffset: 0x9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 2B 0E 2C 0E A6 06 04 00 9A 00 10 10 00 09 01 }
0x43548: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4354E: 		End  { 29 02 }
0x43550: 		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x6A7, VarStoreId: 0x4, VarOffset: 0x9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 2D 0E 2E 0E A7 06 04 00 9B 00 10 10 00 09 01 }
0x43561: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x43567: 		End  { 29 02 }
0x43569: 		Numeric Prompt: " Lane 4", Help: " Value for Lane 4", QuestionFlags: 0x10, QuestionId: 0x6A8, VarStoreId: 0x4, VarOffset: 0x9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 2F 0E 30 0E A8 06 04 00 9C 00 10 10 00 09 01 }
0x4357A: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x43580: 		End  { 29 02 }
0x43582: 		Numeric Prompt: " Lane 5", Help: " Value for Lane 5", QuestionFlags: 0x10, QuestionId: 0x6A9, VarStoreId: 0x4, VarOffset: 0x9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 31 0E 32 0E A9 06 04 00 9D 00 10 10 00 09 01 }
0x43593: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x43599: 		End  { 29 02 }
0x4359B: 		Numeric Prompt: " Lane 6", Help: " Value for Lane 6", QuestionFlags: 0x10, QuestionId: 0x6AA, VarStoreId: 0x4, VarOffset: 0x9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 33 0E 34 0E AA 06 04 00 9E 00 10 10 00 09 01 }
0x435AC: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x435B2: 		End  { 29 02 }
0x435B4: 		Numeric Prompt: " Lane 7", Help: " Value for Lane 7", QuestionFlags: 0x10, QuestionId: 0x6AB, VarStoreId: 0x4, VarOffset: 0x9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1 { 07 91 35 0E 36 0E AB 06 04 00 9F 00 10 10 00 09 01 }
0x435C5: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x435CB: 		End  { 29 02 }
0x435CD: 	End  { 29 02 }
0x435CF: 	Form FormId: 0x27B4, Title: " Gen3 Endpoint Hint value for each Lane" { 01 86 B4 27 15 0E }
0x435D5: 		Subtitle Prompt: " Gen3 Endpoint Hint value for each Lane", Help: "", Flags: 0x0 { 02 87 15 0E 00 00 00 }
0x435DC: 		End  { 29 02 }
0x435DE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x435E5: 		End  { 29 02 }
0x435E7: 		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x6AC, VarStoreId: 0x4, VarOffset: 0xA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 37 0E 38 0E AC 06 04 00 A0 00 10 10 00 06 01 }
0x435F8: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x435FE: 		End  { 29 02 }
0x43600: 		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x6AD, VarStoreId: 0x4, VarOffset: 0xA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 39 0E 3A 0E AD 06 04 00 A1 00 10 10 00 06 01 }
0x43611: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x43617: 		End  { 29 02 }
0x43619: 		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x6AE, VarStoreId: 0x4, VarOffset: 0xA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 3B 0E 3C 0E AE 06 04 00 A2 00 10 10 00 06 01 }
0x4362A: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x43630: 		End  { 29 02 }
0x43632: 		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x6AF, VarStoreId: 0x4, VarOffset: 0xA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 3D 0E 3E 0E AF 06 04 00 A3 00 10 10 00 06 01 }
0x43643: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x43649: 		End  { 29 02 }
0x4364B: 		Numeric Prompt: " Lane 4", Help: " Value for Lane 4", QuestionFlags: 0x10, QuestionId: 0x6B0, VarStoreId: 0x4, VarOffset: 0xA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 3F 0E 40 0E B0 06 04 00 A4 00 10 10 00 06 01 }
0x4365C: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x43662: 		End  { 29 02 }
0x43664: 		Numeric Prompt: " Lane 5", Help: " Value for Lane 5", QuestionFlags: 0x10, QuestionId: 0x6B1, VarStoreId: 0x4, VarOffset: 0xA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 41 0E 42 0E B1 06 04 00 A5 00 10 10 00 06 01 }
0x43675: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x4367B: 		End  { 29 02 }
0x4367D: 		Numeric Prompt: " Lane 6", Help: " Value for Lane 6", QuestionFlags: 0x10, QuestionId: 0x6B2, VarStoreId: 0x4, VarOffset: 0xA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 43 0E 44 0E B2 06 04 00 A6 00 10 10 00 06 01 }
0x4368E: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x43694: 		End  { 29 02 }
0x43696: 		Numeric Prompt: " Lane 7", Help: " Value for Lane 7", QuestionFlags: 0x10, QuestionId: 0x6B3, VarStoreId: 0x4, VarOffset: 0xA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 45 0E 46 0E B3 06 04 00 A7 00 10 10 00 06 01 }
0x436A7: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x436AD: 		End  { 29 02 }
0x436AF: 	End  { 29 02 }
0x436B1: 	Form FormId: 0x27B5, Title: "Gen3 RxCTLE Control" { 01 86 B5 27 07 0E }
0x436B7: 		Subtitle Prompt: "Gen3 RxCTLE Control", Help: "", Flags: 0x0 { 02 87 07 0E 00 00 00 }
0x436BE: 		End  { 29 02 }
0x436C0: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x436C7: 		End  { 29 02 }
0x436C9: 		Numeric Prompt: "Bundle0", Help: "Gen3 RxCTLE setting for Bundle0 (Lane0, Lane1)", QuestionFlags: 0x10, QuestionId: 0x6B4, VarStoreId: 0x4, VarOffset: 0xA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 09 0E 0A 0E B4 06 04 00 A8 00 10 10 00 0F 01 }
0x436DA: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x436E0: 		End  { 29 02 }
0x436E2: 		Numeric Prompt: "Bundle1", Help: "Gen3 RxCTLE setting for Bundle1 (Lane2, Lane3)", QuestionFlags: 0x10, QuestionId: 0x6B5, VarStoreId: 0x4, VarOffset: 0xA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 0B 0E 0C 0E B5 06 04 00 A9 00 10 10 00 0F 01 }
0x436F3: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x436F9: 		End  { 29 02 }
0x436FB: 		Numeric Prompt: "Bundle2", Help: "Gen3 RxCTLE setting for Bundle2 (Lane4, Lane5)", QuestionFlags: 0x10, QuestionId: 0x6B6, VarStoreId: 0x4, VarOffset: 0xAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 0D 0E 0E 0E B6 06 04 00 AA 00 10 10 00 0F 01 }
0x4370C: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43712: 		End  { 29 02 }
0x43714: 		Numeric Prompt: "Bundle3", Help: "Gen3 RxCTLE setting for Bundle3 (Lane6, Lane7)", QuestionFlags: 0x10, QuestionId: 0x6B7, VarStoreId: 0x4, VarOffset: 0xAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 0F 0E 10 0E B7 06 04 00 AB 00 10 10 00 0F 01 }
0x43725: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4372B: 		End  { 29 02 }
0x4372D: 		Ref Prompt: "PEG Port Feature Configuration", Help: "PEG Port Feature Configuration", QuestionFlags: 0x0, QuestionId: 0x6B8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F7 { 0F 0F 87 00 87 00 B8 06 00 00 FF FF 00 F7 28 }
0x4373C: 	End  { 29 02 }
0x4373E: 	Form FormId: 0x27B6, Title: "DMI Advanced Menu" { 01 86 B6 27 CE 0D }
0x43744: 		Subtitle Prompt: "DMI Advanced Menu", Help: "", Flags: 0x0 { 02 87 CE 0D 00 00 00 }
0x4374B: 		End  { 29 02 }
0x4374D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x43754: 		End  { 29 02 }
0x43756: 		OneOf Prompt: "DMI Gen4 EQ Mode", Help: "DMI Gen4 EQ Mode", QuestionFlags: 0x10, QuestionId: 0x6B9, VarStoreId: 0xF101, VarOffset: 0xBAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 CA 0D CB 0D B9 06 01 F1 AE 0B 10 10 00 02 00 }
0x43767: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x4376E: 			OneOfOption Option: "Fixed EQ" Value: 1 { 09 07 CC 0D 00 00 01 }
0x43775: 			OneOfOption Option: "HW EQ" Value: 2, Default, MfgDefault { 09 07 CD 0D 30 00 02 }
0x4377C: 		End  { 29 02 }
0x4377E: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane0", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6BA, VarStoreId: 0xF101, VarOffset: 0xB9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E0 0D F0 0D BA 06 01 F1 9E 0B 10 10 00 3F 01 }
0x4378F: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43795: 		End  { 29 02 }
0x43797: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane0", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6BB, VarStoreId: 0xF101, VarOffset: 0xBA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E1 0D F0 0D BB 06 01 F1 A6 0B 10 10 00 3F 01 }
0x437A8: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x437AE: 		End  { 29 02 }
0x437B0: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane1", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6BC, VarStoreId: 0xF101, VarOffset: 0xB9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E2 0D F0 0D BC 06 01 F1 9F 0B 10 10 00 3F 01 }
0x437C1: 			Default DefaultId: 0x0 Value: 14 { 5B 06 00 00 00 0E }
0x437C7: 		End  { 29 02 }
0x437C9: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane1", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6BD, VarStoreId: 0xF101, VarOffset: 0xBA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E3 0D F0 0D BD 06 01 F1 A7 0B 10 10 00 3F 01 }
0x437DA: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x437E0: 		End  { 29 02 }
0x437E2: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane2", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6BE, VarStoreId: 0xF101, VarOffset: 0xBA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E4 0D F0 0D BE 06 01 F1 A0 0B 10 10 00 3F 01 }
0x437F3: 			Default DefaultId: 0x0 Value: 10 { 5B 06 00 00 00 0A }
0x437F9: 		End  { 29 02 }
0x437FB: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane2", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6BF, VarStoreId: 0xF101, VarOffset: 0xBA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E5 0D F0 0D BF 06 01 F1 A8 0B 10 10 00 3F 01 }
0x4380C: 			Default DefaultId: 0x0 Value: 6 { 5B 06 00 00 00 06 }
0x43812: 		End  { 29 02 }
0x43814: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane3", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C0, VarStoreId: 0xF101, VarOffset: 0xBA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E6 0D F0 0D C0 06 01 F1 A1 0B 10 10 00 3F 01 }
0x43825: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4382B: 		End  { 29 02 }
0x4382D: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane3", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C1, VarStoreId: 0xF101, VarOffset: 0xBA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E7 0D F0 0D C1 06 01 F1 A9 0B 10 10 00 3F 01 }
0x4383E: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x43844: 		End  { 29 02 }
0x43846: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane4", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C2, VarStoreId: 0xF101, VarOffset: 0xBA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E8 0D F0 0D C2 06 01 F1 A2 0B 10 10 00 3F 01 }
0x43857: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4385D: 		End  { 29 02 }
0x4385F: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane4", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C3, VarStoreId: 0xF101, VarOffset: 0xBAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 E9 0D F0 0D C3 06 01 F1 AA 0B 10 10 00 3F 01 }
0x43870: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x43876: 		End  { 29 02 }
0x43878: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane5", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C4, VarStoreId: 0xF101, VarOffset: 0xBA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 EA 0D F0 0D C4 06 01 F1 A3 0B 10 10 00 3F 01 }
0x43889: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4388F: 		End  { 29 02 }
0x43891: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane5", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C5, VarStoreId: 0xF101, VarOffset: 0xBAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 EB 0D F0 0D C5 06 01 F1 AB 0B 10 10 00 3F 01 }
0x438A2: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x438A8: 		End  { 29 02 }
0x438AA: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane6", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C6, VarStoreId: 0xF101, VarOffset: 0xBA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 EC 0D F0 0D C6 06 01 F1 A4 0B 10 10 00 3F 01 }
0x438BB: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x438C1: 		End  { 29 02 }
0x438C3: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane6", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C7, VarStoreId: 0xF101, VarOffset: 0xBAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 ED 0D F0 0D C7 06 01 F1 AC 0B 10 10 00 3F 01 }
0x438D4: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x438DA: 		End  { 29 02 }
0x438DC: 		Numeric Prompt: "DMI Gen4 RTCO Cpost Lane7", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C8, VarStoreId: 0xF101, VarOffset: 0xBA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 EF 0D F0 0D C8 06 01 F1 A5 0B 10 10 00 3F 01 }
0x438ED: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x438F3: 		End  { 29 02 }
0x438F5: 		Numeric Prompt: "DMI Gen4 RTCO Cpre Lane7", Help: "DMI Gen4 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6C9, VarStoreId: 0xF101, VarOffset: 0xBAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 EE 0D F0 0D C9 06 01 F1 AD 0B 10 10 00 3F 01 }
0x43906: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4390C: 		End  { 29 02 }
0x4390E: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane0", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6CA, VarStoreId: 0xF101, VarOffset: 0xB8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 CF 0D DF 0D CA 06 01 F1 8E 0B 10 10 00 3F 01 }
0x4391F: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43925: 		End  { 29 02 }
0x43927: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane0", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6CB, VarStoreId: 0xF101, VarOffset: 0xB96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D0 0D DF 0D CB 06 01 F1 96 0B 10 10 00 3F 01 }
0x43938: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4393E: 		End  { 29 02 }
0x43940: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane1", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6CC, VarStoreId: 0xF101, VarOffset: 0xB8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D1 0D DF 0D CC 06 01 F1 8F 0B 10 10 00 3F 01 }
0x43951: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43957: 		End  { 29 02 }
0x43959: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane1", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6CD, VarStoreId: 0xF101, VarOffset: 0xB97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D2 0D DF 0D CD 06 01 F1 97 0B 10 10 00 3F 01 }
0x4396A: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43970: 		End  { 29 02 }
0x43972: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane2", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6CE, VarStoreId: 0xF101, VarOffset: 0xB90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D3 0D DF 0D CE 06 01 F1 90 0B 10 10 00 3F 01 }
0x43983: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43989: 		End  { 29 02 }
0x4398B: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane2", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6CF, VarStoreId: 0xF101, VarOffset: 0xB98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D4 0D DF 0D CF 06 01 F1 98 0B 10 10 00 3F 01 }
0x4399C: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x439A2: 		End  { 29 02 }
0x439A4: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane3", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D0, VarStoreId: 0xF101, VarOffset: 0xB91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D5 0D DF 0D D0 06 01 F1 91 0B 10 10 00 3F 01 }
0x439B5: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x439BB: 		End  { 29 02 }
0x439BD: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane3", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D1, VarStoreId: 0xF101, VarOffset: 0xB99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D6 0D DF 0D D1 06 01 F1 99 0B 10 10 00 3F 01 }
0x439CE: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x439D4: 		End  { 29 02 }
0x439D6: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane4", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D2, VarStoreId: 0xF101, VarOffset: 0xB92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D7 0D DF 0D D2 06 01 F1 92 0B 10 10 00 3F 01 }
0x439E7: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x439ED: 		End  { 29 02 }
0x439EF: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane4", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D3, VarStoreId: 0xF101, VarOffset: 0xB9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D8 0D DF 0D D3 06 01 F1 9A 0B 10 10 00 3F 01 }
0x43A00: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A06: 		End  { 29 02 }
0x43A08: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane5", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D4, VarStoreId: 0xF101, VarOffset: 0xB93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 D9 0D DF 0D D4 06 01 F1 93 0B 10 10 00 3F 01 }
0x43A19: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A1F: 		End  { 29 02 }
0x43A21: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane5", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D5, VarStoreId: 0xF101, VarOffset: 0xB9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 DA 0D DF 0D D5 06 01 F1 9B 0B 10 10 00 3F 01 }
0x43A32: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A38: 		End  { 29 02 }
0x43A3A: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane6", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D6, VarStoreId: 0xF101, VarOffset: 0xB94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 DB 0D DF 0D D6 06 01 F1 94 0B 10 10 00 3F 01 }
0x43A4B: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A51: 		End  { 29 02 }
0x43A53: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane6", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D7, VarStoreId: 0xF101, VarOffset: 0xB9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 DC 0D DF 0D D7 06 01 F1 9C 0B 10 10 00 3F 01 }
0x43A64: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A6A: 		End  { 29 02 }
0x43A6C: 		Numeric Prompt: "DMI Gen3 RTCO Cpre Lane7", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D8, VarStoreId: 0xF101, VarOffset: 0xB95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 DD 0D DF 0D D8 06 01 F1 95 0B 10 10 00 3F 01 }
0x43A7D: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A83: 		End  { 29 02 }
0x43A85: 		Numeric Prompt: "DMI Gen3 RTCO Cpost Lane7", Help: "DMI Gen3 Lane Transmitter Pre/Post-Cursor Coefficient values.", QuestionFlags: 0x10, QuestionId: 0x6D9, VarStoreId: 0xF101, VarOffset: 0xB9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 DE 0D DF 0D D9 06 01 F1 9D 0B 10 10 00 3F 01 }
0x43A96: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43A9C: 		End  { 29 02 }
0x43A9E: 	End  { 29 02 }
0x43AA0: 	Form FormId: 0x27B7, Title: "LCD Control" { 01 86 B7 27 77 0A }
0x43AA6: 		Subtitle Prompt: "LCD Control", Help: "", Flags: 0x0 { 02 87 77 0A 00 00 00 }
0x43AAD: 		End  { 29 02 }
0x43AAF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x43AB6: 		End  { 29 02 }
0x43AB8: 		OneOf Prompt: "Primary IGFX Boot Display", Help: "Select the Video Device which will be activated during POST.
This has no effect if external graphics present.
Secondary boot display selection will appear based on your selection.
VGA modes will be supported only on primary display
", QuestionFlags: 0x10, QuestionId: 0x6DA, VarStoreId: 0x4, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x0 { 05 91 54 0A 55 0A DA 06 04 00 2A 00 10 10 00 40 00 }
0x43AC9: 			OneOfOption Option: "VBIOS Default" Value: 0, Default, MfgDefault { 09 07 56 0A 30 00 00 }
0x43AD0: 			OneOfOption Option: "EFP" Value: 4 { 09 07 58 0A 00 00 04 }
0x43AD7: 			OneOfOption Option: "LFP" Value: 8 { 09 07 57 0A 00 00 08 }
0x43ADE: 			OneOfOption Option: "EFP3" Value: 32 { 09 07 5A 0A 00 00 20 }
0x43AE5: 			OneOfOption Option: "EFP2" Value: 64 { 09 07 59 0A 00 00 40 }
0x43AEC: 			OneOfOption Option: "EFP4" Value: 16 { 09 07 5B 0A 00 00 10 }
0x43AF3: 		End  { 29 02 }
0x43AF5: 		SuppressIf  { 0A 82 }
0x43AF7: 			EqIdVal QuestionId: 0x6DA, Value: 0x0 { 12 06 DA 06 00 00 }
0x43AFD: 			OneOf Prompt: "Secondary IGFX Boot Display", Help: "Select Secondary Display Device", QuestionFlags: 0x10, QuestionId: 0x6DB, VarStoreId: 0x4, VarOffset: 0x2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x0 { 05 91 5C 0A 5D 0A DB 06 04 00 2B 00 10 10 00 40 00 }
0x43B0E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 5E 0A 30 00 00 }
0x43B15: 				OneOfOption Option: "EFP" Value: 4 { 09 07 58 0A 00 00 04 }
0x43B1C: 				OneOfOption Option: "EFP3" Value: 32 { 09 07 5A 0A 00 00 20 }
0x43B23: 				OneOfOption Option: "EFP2" Value: 64 { 09 07 59 0A 00 00 40 }
0x43B2A: 				OneOfOption Option: "EFP4" Value: 16 { 09 07 5B 0A 00 00 10 }
0x43B31: 			End  { 29 02 }
0x43B33: 		End  { 29 02 }
0x43B35: 		OneOf Prompt: "LCD Panel Type", Help: "Select LCD panel used by Internal Graphics Device by selecting the appropriate setup item.", QuestionFlags: 0x10, QuestionId: 0x6DC, VarStoreId: 0x4, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x11, Step: 0x0 { 05 91 CE 0A CF 0A DC 06 04 00 2C 00 10 10 00 11 00 }
0x43B46: 			OneOfOption Option: "VBIOS Default" Value: 0, Default, MfgDefault { 09 07 56 0A 30 00 00 }
0x43B4D: 			OneOfOption Option: "640x480    LVDS" Value: 1 { 09 07 D0 0A 00 00 01 }
0x43B54: 			OneOfOption Option: "800x600    LVDS" Value: 2 { 09 07 D1 0A 00 00 02 }
0x43B5B: 			OneOfOption Option: "1024x768   LVDS" Value: 3 { 09 07 D2 0A 00 00 03 }
0x43B62: 			OneOfOption Option: "1280x1024  LVDS" Value: 4 { 09 07 D3 0A 00 00 04 }
0x43B69: 			OneOfOption Option: "1400x1050  LVDS1" Value: 5 { 09 07 D4 0A 00 00 05 }
0x43B70: 			OneOfOption Option: "1400x1050  LVDS2" Value: 6 { 09 07 D5 0A 00 00 06 }
0x43B77: 			OneOfOption Option: "1600x1200  LVDS" Value: 7 { 09 07 D6 0A 00 00 07 }
0x43B7E: 			OneOfOption Option: "1280x768   LVDS" Value: 8 { 09 07 D7 0A 00 00 08 }
0x43B85: 			OneOfOption Option: "1680x1050  LVDS" Value: 9 { 09 07 D8 0A 00 00 09 }
0x43B8C: 			OneOfOption Option: "1920x1200  LVDS" Value: 10 { 09 07 D9 0A 00 00 0A }
0x43B93: 			OneOfOption Option: "1600x900   LVDS" Value: 13 { 09 07 DA 0A 00 00 0D }
0x43B9A: 			OneOfOption Option: "1280x800   LVDS" Value: 14 { 09 07 DB 0A 00 00 0E }
0x43BA1: 			OneOfOption Option: "1280x600   LVDS" Value: 15 { 09 07 DC 0A 00 00 0F }
0x43BA8: 			OneOfOption Option: "2048x1536  LVDS" Value: 16 { 09 07 DD 0A 00 00 10 }
0x43BAF: 			OneOfOption Option: "1366x768  LVDS" Value: 17 { 09 07 DE 0A 00 00 11 }
0x43BB6: 		End  { 29 02 }
0x43BB8: 		OneOf Prompt: "Panel Scaling", Help: "Select the LCD panel scaling option used by the Internal Graphics Device.", QuestionFlags: 0x10, QuestionId: 0x6DD, VarStoreId: 0x4, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 DF 0A E0 0A DD 06 04 00 2D 00 10 10 00 06 00 }
0x43BC9: 			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 E1 0A 30 00 00 }
0x43BD0: 			OneOfOption Option: "Off" Value: 1 { 09 07 E3 0A 00 00 01 }
0x43BD7: 			OneOfOption Option: "Force Scaling" Value: 6 { 09 07 E2 0A 00 00 06 }
0x43BDE: 		End  { 29 02 }
0x43BE0: 		OneOf Prompt: "Backlight Control", Help: "Back Light Control Setting", QuestionFlags: 0x10, QuestionId: 0x6DE, VarStoreId: 0x4, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E4 0A E5 0A DE 06 04 00 2F 00 10 10 00 02 00 }
0x43BF1: 			OneOfOption Option: "PWM Inverted" Value: 0 { 09 07 E6 0A 00 00 00 }
0x43BF8: 			OneOfOption Option: "PWM Normal" Value: 2, Default, MfgDefault { 09 07 E7 0A 30 00 02 }
0x43BFF: 		End  { 29 02 }
0x43C01: 		OneOf Prompt: "Active LFP", Help: "Select the Active LFP Configuration.

No LVDS:VBIOS does not enable LVDS.
Int-LVDS:VBIOS enables LVDS driver by Integrated encoder.
SDVO LVDS:VBIOS enables LVDS driver by SDVO encoder.
eDP Port-A:LFP Driven by Int-DisplayPort encoder from Port-A.
eDP Port-D:LFP Driven by Int-DisplayPort encoder from Port-D(through PCH).", QuestionFlags: 0x10, QuestionId: 0x6DF, VarStoreId: 0x4, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 EC 0A ED 0A DF 06 04 00 31 00 10 10 00 03 00 }
0x43C12: 			OneOfOption Option: "No eDP" Value: 0 { 09 07 EE 0A 00 00 00 }
0x43C19: 			OneOfOption Option: "eDP Port-A" Value: 3, Default, MfgDefault { 09 07 EF 0A 30 00 03 }
0x43C20: 		End  { 29 02 }
0x43C22: 		OneOf Prompt: "Panel Color Depth", Help: "Select the LFP Panel Color Depth", QuestionFlags: 0x10, QuestionId: 0x6E0, VarStoreId: 0x4, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 0A E9 0A E0 06 04 00 32 00 10 10 00 01 00 }
0x43C33: 			OneOfOption Option: "18 Bit" Value: 0, Default, MfgDefault { 09 07 EA 0A 30 00 00 }
0x43C3A: 			OneOfOption Option: "24 Bit" Value: 1 { 09 07 EB 0A 00 00 01 }
0x43C41: 		End  { 29 02 }
0x43C43: 		Numeric Prompt: "Backlight Brightness", Help: "Set VBIOS Brightness.
Range : 0-255.", QuestionFlags: 0x0, QuestionId: 0x6E1, VarStoreId: 0x4, VarOffset: 0x3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 F0 0A F1 0A E1 06 04 00 3C 00 00 10 00 FF 00 }
0x43C54: 			Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x43C5A: 		End  { 29 02 }
0x43C5C: 	End  { 29 02 }
0x43C5E: 	Form FormId: 0x27B8, Title: "Intel(R) Ultrabook Event Support" { 01 86 B8 27 4F 0E }
0x43C64: 		Subtitle Prompt: "Intel(R) Ultrabook Event Support", Help: "", Flags: 0x0 { 02 87 4F 0E 00 00 00 }
0x43C6B: 		End  { 29 02 }
0x43C6D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x43C74: 		End  { 29 02 }
0x43C76: 		OneOf Prompt: "IUER Slate Enable", Help: "Enable/Disable IUER Slate Functionality", QuestionFlags: 0x10, QuestionId: 0x6E2, VarStoreId: 0x4, VarOffset: 0x25D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5E 0E 5F 0E E2 06 04 00 5D 02 10 10 00 01 00 }
0x43C87: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43C8D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x43C94: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x43C9B: 		End  { 29 02 }
0x43C9D: 		SuppressIf  { 0A 82 }
0x43C9F: 			EqIdVal QuestionId: 0x6E2, Value: 0x0 { 12 06 E2 06 00 00 }
0x43CA5: 			OneOf Prompt: "  Slate Mode boot value", Help: "Choose Slate or Laptop as boot mode.", QuestionFlags: 0x10, QuestionId: 0x6E3, VarStoreId: 0x4, VarOffset: 0x258, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 50 0E 51 0E E3 06 04 00 58 02 10 10 00 01 00 }
0x43CB6: 				OneOfOption Option: "Slate Mode" Value: 0 { 09 07 58 0E 00 00 00 }
0x43CBD: 				OneOfOption Option: "Laptop Mode" Value: 1, Default, MfgDefault { 09 07 59 0E 30 00 01 }
0x43CC4: 			End  { 29 02 }
0x43CC6: 			OneOf Prompt: "  Slate Mode on S3 and S4 resume", Help: "Keep it the same as Sx entry or toggle it.", QuestionFlags: 0x10, QuestionId: 0x6E4, VarStoreId: 0x4, VarOffset: 0x259, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 54 0E 55 0E E4 06 04 00 59 02 10 10 00 01 00 }
0x43CD7: 				OneOfOption Option: "No change" Value: 0, Default, MfgDefault { 09 07 5C 0E 30 00 00 }
0x43CDE: 				OneOfOption Option: "Toggle" Value: 1 { 09 07 5D 0E 00 00 01 }
0x43CE5: 			End  { 29 02 }
0x43CE7: 		End  { 29 02 }
0x43CE9: 		OneOf Prompt: "IUER Dock Enable", Help: "Enable/Disable IUER Dock Functionality", QuestionFlags: 0x10, QuestionId: 0x6E5, VarStoreId: 0x4, VarOffset: 0x25E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 60 0E 61 0E E5 06 04 00 5E 02 10 10 00 01 00 }
0x43CFA: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x43D00: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x43D07: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x43D0E: 		End  { 29 02 }
0x43D10: 		SuppressIf  { 0A 82 }
0x43D12: 			EqIdVal QuestionId: 0x6E5, Value: 0x0 { 12 06 E5 06 00 00 }
0x43D18: 			OneOf Prompt: "  Dock Mode boot value", Help: "Choose Docked or Undocked as boot mode.", QuestionFlags: 0x10, QuestionId: 0x6E6, VarStoreId: 0x4, VarOffset: 0x25A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 52 0E 53 0E E6 06 04 00 5A 02 10 10 00 01 00 }
0x43D29: 				OneOfOption Option: "Undocked" Value: 0, Default, MfgDefault { 09 07 5B 0E 30 00 00 }
0x43D30: 				OneOfOption Option: "Docked" Value: 1 { 09 07 5A 0E 00 00 01 }
0x43D37: 			End  { 29 02 }
0x43D39: 			OneOf Prompt: "  Dock Mode upon S3 and S4 resume", Help: "Keep it the same as Sx entry or toggle it.", QuestionFlags: 0x10, QuestionId: 0x6E7, VarStoreId: 0x4, VarOffset: 0x25B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 56 0E 57 0E E7 06 04 00 5B 02 10 10 00 01 00 }
0x43D4A: 				OneOfOption Option: "No change" Value: 0, Default, MfgDefault { 09 07 5C 0E 30 00 00 }
0x43D51: 				OneOfOption Option: "Toggle" Value: 1 { 09 07 5D 0E 00 00 01 }
0x43D58: 			End  { 29 02 }
0x43D5A: 		End  { 29 02 }
0x43D5C: 	End  { 29 02 }
0x43D5E: 	Form FormId: 0x27B9, Title: "GT - Power Management Control" { 01 86 B9 27 8E 04 }
0x43D64: 		Subtitle Prompt: "GT - Power Management Control", Help: "", Flags: 0x0 { 02 87 8E 04 00 00 00 }
0x43D6B: 		End  { 29 02 }
0x43D6D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x43D74: 		End  { 29 02 }
0x43D76: 		SuppressIf  { 0A 82 }
0x43D78: 			EqIdVal QuestionId: 0x278E, Value: 0x0 { 12 06 8E 27 00 00 }
0x43D7E: 			OneOf Prompt: "RC6(Render Standby)", Help: "Check to enable render standby support.", QuestionFlags: 0x10, QuestionId: 0x278F, VarStoreId: 0x4, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 52 0A 53 0A 8F 27 04 00 2E 00 10 10 00 01 00 }
0x43D8F: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x43D95: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43D9C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x43DA3: 			End  { 29 02 }
0x43DA5: 		End  { 29 02 }
0x43DA7: 		OneOf Prompt: "Maximum GT frequency", Help: "Auto Updated", QuestionFlags: 0x10, QuestionId: 0x6E8, VarStoreId: 0x4, VarOffset: 0x3F, Flags: 0x10, Size: 8, Min: 0x2, Max: 0xFF, Step: 0x0 { 05 91 06 0B 07 0B E8 06 04 00 3F 00 10 10 02 FF 00 }
0x43DB8: 			Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x43DBE: 			OneOfOption Option: "Default Max Frequency" Value: 255 { 09 07 1F 0B 00 00 FF }
0x43DC5: 			OneOfOption Option: "100Mhz" Value: 2 { 09 07 08 0B 00 00 02 }
0x43DCC: 			OneOfOption Option: "150Mhz" Value: 3 { 09 07 09 0B 00 00 03 }
0x43DD3: 			OneOfOption Option: "200Mhz" Value: 4 { 09 07 0A 0B 00 00 04 }
0x43DDA: 			OneOfOption Option: "250Mhz" Value: 5 { 09 07 0B 0B 00 00 05 }
0x43DE1: 			OneOfOption Option: "300Mhz" Value: 6 { 09 07 0C 0B 00 00 06 }
0x43DE8: 			OneOfOption Option: "350Mhz" Value: 7 { 09 07 0D 0B 00 00 07 }
0x43DEF: 			OneOfOption Option: "400Mhz" Value: 8 { 09 07 0E 0B 00 00 08 }
0x43DF6: 			OneOfOption Option: "450Mhz" Value: 9 { 09 07 0F 0B 00 00 09 }
0x43DFD: 			OneOfOption Option: "500Mhz" Value: 10 { 09 07 10 0B 00 00 0A }
0x43E04: 			OneOfOption Option: "550Mhz" Value: 11 { 09 07 11 0B 00 00 0B }
0x43E0B: 			OneOfOption Option: "600Mhz" Value: 12 { 09 07 12 0B 00 00 0C }
0x43E12: 			OneOfOption Option: "650Mhz" Value: 13 { 09 07 13 0B 00 00 0D }
0x43E19: 			OneOfOption Option: "700Mhz" Value: 14 { 09 07 14 0B 00 00 0E }
0x43E20: 			OneOfOption Option: "750Mhz" Value: 15 { 09 07 15 0B 00 00 0F }
0x43E27: 			OneOfOption Option: "800Mhz" Value: 16 { 09 07 16 0B 00 00 10 }
0x43E2E: 			OneOfOption Option: "850Mhz" Value: 17 { 09 07 17 0B 00 00 11 }
0x43E35: 			OneOfOption Option: "900Mhz" Value: 18 { 09 07 18 0B 00 00 12 }
0x43E3C: 			OneOfOption Option: "950Mhz" Value: 19 { 09 07 19 0B 00 00 13 }
0x43E43: 			OneOfOption Option: "1000Mhz" Value: 20 { 09 07 1A 0B 00 00 14 }
0x43E4A: 			OneOfOption Option: "1050Mhz" Value: 21 { 09 07 1B 0B 00 00 15 }
0x43E51: 			OneOfOption Option: "1100Mhz" Value: 22 { 09 07 1C 0B 00 00 16 }
0x43E58: 			OneOfOption Option: "1150Mhz" Value: 23 { 09 07 1D 0B 00 00 17 }
0x43E5F: 			OneOfOption Option: "1200Mhz" Value: 24 { 09 07 1E 0B 00 00 18 }
0x43E66: 		End  { 29 02 }
0x43E68: 		GrayOutIf  { 19 82 }
0x43E6A: 			EqIdVal QuestionId: 0x6E8, Value: 0xFF { 12 86 E8 06 FF 00 }
0x43E70: 				Not  { 17 02 }
0x43E72: 			End  { 29 02 }
0x43E74: 			OneOf Prompt: "Disable Turbo GT frequency", Help: "Enabled: Disables Turbo GT frequency. Disabled: GT frequency is not limited", QuestionFlags: 0x10, QuestionId: 0x6E9, VarStoreId: 0x4, VarOffset: 0x40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 20 0B 21 0B E9 06 04 00 40 00 10 10 00 01 00 }
0x43E85: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x43E8C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x43E93: 			End  { 29 02 }
0x43E95: 		End  { 29 02 }
0x43E97: 	End  { 29 02 }
0x43E99: 	Form FormId: 0x27BA, Title: "Memory Training Algorithms" { 01 86 BA 27 65 09 }
0x43E9F: 		OneOf Prompt: "Early Command Training", Help: "Early Command Training", QuestionFlags: 0x10, QuestionId: 0x6EA, VarStoreId: 0x4, VarOffset: 0x1FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 09 68 09 EA 06 04 00 FF 01 10 10 00 01 00 }
0x43EB0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43EB7: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43EBE: 		End  { 29 02 }
0x43EC0: 		OneOf Prompt: "SenseAmp Offset Training", Help: "SenseAmp Offset Training", QuestionFlags: 0x10, QuestionId: 0x6EB, VarStoreId: 0x4, VarOffset: 0x200, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 09 6A 09 EB 06 04 00 00 02 10 10 00 01 00 }
0x43ED1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x43ED8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x43EDF: 		End  { 29 02 }
0x43EE1: 		OneOf Prompt: "Early ReadMPR Timing Centering 2D", Help: "", QuestionFlags: 0x10, QuestionId: 0x6EC, VarStoreId: 0x4, VarOffset: 0x201, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 09 C9 07 EC 06 04 00 01 02 10 10 00 01 00 }
0x43EF2: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43EF9: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43F00: 		End  { 29 02 }
0x43F02: 		OneOf Prompt: "Read MPR Training", Help: "Read MPR Training", QuestionFlags: 0x10, QuestionId: 0x6ED, VarStoreId: 0x4, VarOffset: 0x202, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 09 6D 09 ED 06 04 00 02 02 10 10 00 01 00 }
0x43F13: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x43F1A: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x43F21: 		End  { 29 02 }
0x43F23: 		OneOf Prompt: "Receive Enable Training", Help: "Receive Enable Training", QuestionFlags: 0x10, QuestionId: 0x6EE, VarStoreId: 0x4, VarOffset: 0x203, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 09 6F 09 EE 06 04 00 03 02 10 10 00 01 00 }
0x43F34: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43F3B: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43F42: 		End  { 29 02 }
0x43F44: 		OneOf Prompt: "Jedec Write Leveling", Help: "Jedec Write Leveling", QuestionFlags: 0x10, QuestionId: 0x6EF, VarStoreId: 0x4, VarOffset: 0x204, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 09 71 09 EF 06 04 00 04 02 10 10 00 01 00 }
0x43F55: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43F5C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43F63: 		End  { 29 02 }
0x43F65: 		OneOf Prompt: "Early Write Time Centering 2D", Help: "Early Write Time Centering 2D", QuestionFlags: 0x10, QuestionId: 0x6F0, VarStoreId: 0x4, VarOffset: 0x205, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 09 73 09 F0 06 04 00 05 02 10 10 00 01 00 }
0x43F76: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43F7D: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43F84: 		End  { 29 02 }
0x43F86: 		OneOf Prompt: "Early Read Time Centering 2D", Help: "", QuestionFlags: 0x10, QuestionId: 0x6F1, VarStoreId: 0x4, VarOffset: 0x206, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 09 C9 07 F1 06 04 00 06 02 10 10 00 01 00 }
0x43F97: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43F9E: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43FA5: 		End  { 29 02 }
0x43FA7: 		OneOf Prompt: "Write Timing Centering 1D", Help: "Write Timing Centering 1D", QuestionFlags: 0x10, QuestionId: 0x6F2, VarStoreId: 0x4, VarOffset: 0x207, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 75 09 76 09 F2 06 04 00 07 02 10 10 00 01 00 }
0x43FB8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43FBF: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43FC6: 		End  { 29 02 }
0x43FC8: 		OneOf Prompt: "Write Voltage Centering 1D", Help: "", QuestionFlags: 0x10, QuestionId: 0x6F3, VarStoreId: 0x4, VarOffset: 0x208, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 77 09 C9 07 F3 06 04 00 08 02 10 10 00 01 00 }
0x43FD9: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x43FE0: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x43FE7: 		End  { 29 02 }
0x43FE9: 		OneOf Prompt: "Read Timing Centering 1D", Help: "Read Timing Centering 1D", QuestionFlags: 0x10, QuestionId: 0x6F4, VarStoreId: 0x4, VarOffset: 0x209, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 09 79 09 F4 06 04 00 09 02 10 10 00 01 00 }
0x43FFA: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44001: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44008: 		End  { 29 02 }
0x4400A: 		OneOf Prompt: "Dimm ODT Training*", Help: "Dimm On-Die Termination Training", QuestionFlags: 0x10, QuestionId: 0x6F5, VarStoreId: 0x4, VarOffset: 0x20A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 09 7B 09 F5 06 04 00 0A 02 10 10 00 01 00 }
0x4401B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44022: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44029: 		End  { 29 02 }
0x4402B: 		GrayOutIf  { 19 82 }
0x4402D: 			EqIdVal QuestionId: 0x6F5, Value: 0x0 { 12 06 F5 06 00 00 }
0x44033: 			OneOf Prompt: "  Max RTT_WR", Help: "Caps the maximum RTT_WR in power training.", QuestionFlags: 0x10, QuestionId: 0x6F6, VarStoreId: 0x4, VarOffset: 0x244, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 08 8A 08 F6 06 04 00 44 02 10 10 00 01 00 }
0x44044: 				OneOfOption Option: "ODT Off" Value: 0, Default, MfgDefault { 09 07 8B 08 30 00 00 }
0x4404B: 				OneOfOption Option: "120 Ohms" Value: 1 { 09 07 8C 08 00 00 01 }
0x44052: 			End  { 29 02 }
0x44054: 		End  { 29 02 }
0x44056: 		OneOf Prompt: "DIMM RON Training*", Help: "DIMM RON Training", QuestionFlags: 0x10, QuestionId: 0x6F7, VarStoreId: 0x4, VarOffset: 0x20B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7C 09 7D 09 F7 06 04 00 0B 02 10 10 00 01 00 }
0x44067: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4406E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44075: 		End  { 29 02 }
0x44077: 		OneOf Prompt: "Write Drive Strength/Equalization 2D*", Help: "", QuestionFlags: 0x10, QuestionId: 0x6F8, VarStoreId: 0x4, VarOffset: 0x20C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7E 09 C9 07 F8 06 04 00 0C 02 10 10 00 01 00 }
0x44088: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4408F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44096: 		End  { 29 02 }
0x44098: 		OneOf Prompt: "Write Slew Rate Training*", Help: "Write Slew Rate Training", QuestionFlags: 0x10, QuestionId: 0x6F9, VarStoreId: 0x4, VarOffset: 0x20D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7F 09 80 09 F9 06 04 00 0D 02 10 10 00 01 00 }
0x440A9: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x440B0: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x440B7: 		End  { 29 02 }
0x440B9: 		OneOf Prompt: "Read ODT Training*", Help: "Read On-Die Termination Training", QuestionFlags: 0x10, QuestionId: 0x6FA, VarStoreId: 0x4, VarOffset: 0x20E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 81 09 82 09 FA 06 04 00 0E 02 10 10 00 01 00 }
0x440CA: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x440D1: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x440D8: 		End  { 29 02 }
0x440DA: 		OneOf Prompt: "Read Equalization Training*", Help: "Read Equalization Training", QuestionFlags: 0x10, QuestionId: 0x6FB, VarStoreId: 0x4, VarOffset: 0x20F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 83 09 84 09 FB 06 04 00 0F 02 10 10 00 01 00 }
0x440EB: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x440F2: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x440F9: 		End  { 29 02 }
0x440FB: 		OneOf Prompt: "Read Amplifier Training*", Help: "Read Amplifier Training", QuestionFlags: 0x10, QuestionId: 0x6FC, VarStoreId: 0x4, VarOffset: 0x210, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 85 09 86 09 FC 06 04 00 10 02 10 10 00 01 00 }
0x4410C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44113: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4411A: 		End  { 29 02 }
0x4411C: 		OneOf Prompt: "Write Timing Centering 2D", Help: "Write Dq-Dqs Timing Centering 2D", QuestionFlags: 0x10, QuestionId: 0x6FD, VarStoreId: 0x4, VarOffset: 0x211, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 09 88 09 FD 06 04 00 11 02 10 10 00 01 00 }
0x4412D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44134: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4413B: 		End  { 29 02 }
0x4413D: 		OneOf Prompt: "Read Timing Centering 2D", Help: "Read Dq-Dqs Timing Centering 2D", QuestionFlags: 0x10, QuestionId: 0x6FE, VarStoreId: 0x4, VarOffset: 0x212, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 09 8A 09 FE 06 04 00 12 02 10 10 00 01 00 }
0x4414E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44155: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4415C: 		End  { 29 02 }
0x4415E: 		OneOf Prompt: "Command Voltage Centering", Help: "Command Voltage Centering", QuestionFlags: 0x10, QuestionId: 0x6FF, VarStoreId: 0x4, VarOffset: 0x213, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 09 8C 09 FF 06 04 00 13 02 10 10 00 01 00 }
0x4416F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44176: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4417D: 		End  { 29 02 }
0x4417F: 		OneOf Prompt: "Write Voltage Centering 2D", Help: "Write Voltage Centering 2D", QuestionFlags: 0x10, QuestionId: 0x700, VarStoreId: 0x4, VarOffset: 0x214, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8D 09 8E 09 00 07 04 00 14 02 10 10 00 01 00 }
0x44190: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44197: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4419E: 		End  { 29 02 }
0x441A0: 		OneOf Prompt: "Read Voltage Centering 2D", Help: "Read Voltage Centering 2D", QuestionFlags: 0x10, QuestionId: 0x701, VarStoreId: 0x4, VarOffset: 0x215, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 09 90 09 01 07 04 00 15 02 10 10 00 01 00 }
0x441B1: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x441B8: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x441BF: 		End  { 29 02 }
0x441C1: 		OneOf Prompt: "Late Command Training", Help: "Late Command Training", QuestionFlags: 0x10, QuestionId: 0x702, VarStoreId: 0x4, VarOffset: 0x216, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 09 92 09 02 07 04 00 16 02 10 10 00 01 00 }
0x441D2: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x441D9: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x441E0: 		End  { 29 02 }
0x441E2: 		OneOf Prompt: "Round Trip Latency", Help: "Round Trip Latency Training", QuestionFlags: 0x10, QuestionId: 0x703, VarStoreId: 0x4, VarOffset: 0x217, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 09 94 09 03 07 04 00 17 02 10 10 00 01 00 }
0x441F3: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x441FA: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44201: 		End  { 29 02 }
0x44203: 		OneOf Prompt: "Turn Around Timing Training", Help: "Turn Around Timing Training", QuestionFlags: 0x10, QuestionId: 0x704, VarStoreId: 0x4, VarOffset: 0x218, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 09 96 09 04 07 04 00 18 02 10 10 00 01 00 }
0x44214: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4421B: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44222: 		End  { 29 02 }
0x44224: 		OneOf Prompt: "CMD CTL CLK Slew Rate", Help: "CMD CTL CLK Slew Rate", QuestionFlags: 0x10, QuestionId: 0x705, VarStoreId: 0x4, VarOffset: 0x24E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A6 09 A6 09 05 07 04 00 4E 02 10 10 00 01 00 }
0x44235: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4423C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44243: 		End  { 29 02 }
0x44245: 		OneOf Prompt: "CMD/CTL DS & E 2D", Help: "CMD/CTL Drive Strength and Equalization 2D", QuestionFlags: 0x10, QuestionId: 0x706, VarStoreId: 0x4, VarOffset: 0x24D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 09 A5 09 06 07 04 00 4D 02 10 10 00 01 00 }
0x44256: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4425D: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44264: 		End  { 29 02 }
0x44266: 		OneOf Prompt: "Read Voltage Centering 1D", Help: "Read Voltage Centering 1D", QuestionFlags: 0x10, QuestionId: 0x707, VarStoreId: 0x4, VarOffset: 0x248, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 09 9F 09 07 07 04 00 48 02 10 10 00 01 00 }
0x44277: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4427E: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44285: 		End  { 29 02 }
0x44287: 		OneOf Prompt: "TxDqTCO Comp Training*", Help: "TxDqTCO Comp Training*", QuestionFlags: 0x10, QuestionId: 0x708, VarStoreId: 0x4, VarOffset: 0x249, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 09 A0 09 08 07 04 00 49 02 10 10 00 01 00 }
0x44298: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4429F: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x442A6: 		End  { 29 02 }
0x442A8: 		OneOf Prompt: "ClkTCO Comp Training*", Help: "ClkTCO Comp Training*", QuestionFlags: 0x10, QuestionId: 0x709, VarStoreId: 0x4, VarOffset: 0x24C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A3 09 A3 09 09 07 04 00 4C 02 10 10 00 01 00 }
0x442B9: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x442C0: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x442C7: 		End  { 29 02 }
0x442C9: 		OneOf Prompt: "TxDqsTCO Comp Training*", Help: "TxDqsTCO Comp Training*", QuestionFlags: 0x10, QuestionId: 0x70A, VarStoreId: 0x4, VarOffset: 0x24A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 09 A1 09 0A 07 04 00 4A 02 10 10 00 01 00 }
0x442DA: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x442E1: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x442E8: 		End  { 29 02 }
0x442EA: 		OneOf Prompt: "VccDLL Bypass Training", Help: "VccDLL Bypass Training", QuestionFlags: 0x10, QuestionId: 0x70B, VarStoreId: 0x4, VarOffset: 0x24B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 09 A2 09 0B 07 04 00 4B 02 10 10 00 01 00 }
0x442FB: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44302: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44309: 		End  { 29 02 }
0x4430B: 		OneOf Prompt: "CMD/CTL Drive Strength Up/Dn 2D", Help: "CMD/CTL Drive Strength Up/Dn 2D", QuestionFlags: 0x10, QuestionId: 0x70C, VarStoreId: 0x4, VarOffset: 0x24F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A7 09 A7 09 0C 07 04 00 4F 02 10 10 00 01 00 }
0x4431C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44323: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4432A: 		End  { 29 02 }
0x4432C: 		OneOf Prompt: "DIMM CA ODT Training", Help: "DIMM CA ODT Training", QuestionFlags: 0x10, QuestionId: 0x70D, VarStoreId: 0x4, VarOffset: 0x250, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 09 A8 09 0D 07 04 00 50 02 10 10 00 01 00 }
0x4433D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44344: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4434B: 		End  { 29 02 }
0x4434D: 		OneOf Prompt: "PanicVttDnLp Training*", Help: "PanicVttDnLp Training*", QuestionFlags: 0x10, QuestionId: 0x70E, VarStoreId: 0x4, VarOffset: 0x251, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 09 A9 09 0E 07 04 00 51 02 10 10 00 01 00 }
0x4435E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44365: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4436C: 		End  { 29 02 }
0x4436E: 		OneOf Prompt: "Read Vref Decap Training*", Help: "Read Vref Decap Training*", QuestionFlags: 0x10, QuestionId: 0x70F, VarStoreId: 0x4, VarOffset: 0x252, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 09 AA 09 0F 07 04 00 52 02 10 10 00 01 00 }
0x4437F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44386: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4438D: 		End  { 29 02 }
0x4438F: 		OneOf Prompt: "Vddq Training", Help: "Vddq Training", QuestionFlags: 0x10, QuestionId: 0x710, VarStoreId: 0x4, VarOffset: 0x253, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AB 09 AB 09 10 07 04 00 53 02 10 10 00 01 00 }
0x443A0: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x443A7: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x443AE: 		End  { 29 02 }
0x443B0: 		OneOf Prompt: "Duty Cycle Correction Training", Help: "Duty Cycle Correction Training", QuestionFlags: 0x10, QuestionId: 0x711, VarStoreId: 0x4, VarOffset: 0x254, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 09 AC 09 11 07 04 00 54 02 10 10 00 01 00 }
0x443C1: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x443C8: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x443CF: 		End  { 29 02 }
0x443D1: 		OneOf Prompt: "Rank Margin Tool Per Bit", Help: "Rank Margin Tool Per Bit", QuestionFlags: 0x10, QuestionId: 0x712, VarStoreId: 0x4, VarOffset: 0x255, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 09 AD 09 12 07 04 00 55 02 10 10 00 01 00 }
0x443E2: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x443E9: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x443F0: 		End  { 29 02 }
0x443F2: 		OneOf Prompt: "DIMM DFE Training", Help: "DIMM DFE Training", QuestionFlags: 0x10, QuestionId: 0x713, VarStoreId: 0x4, VarOffset: 0x403, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AF 09 AF 09 13 07 04 00 03 04 10 10 00 01 00 }
0x44403: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4440A: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44411: 		End  { 29 02 }
0x44413: 		OneOf Prompt: "EARLY DIMM DFE Training", Help: "EARLY DIMM DFE Training", QuestionFlags: 0x10, QuestionId: 0x2790, VarStoreId: 0x4, VarOffset: 0x476, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 09 B0 09 90 27 04 00 76 04 10 10 00 01 00 }
0x44424: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4442B: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44432: 		End  { 29 02 }
0x44434: 		OneOf Prompt: "Tx Dqs Dcc Training", Help: "Tx Dqs duty cycle Training", QuestionFlags: 0x10, QuestionId: 0x714, VarStoreId: 0x4, VarOffset: 0x433, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 09 B2 09 14 07 04 00 33 04 10 10 00 01 00 }
0x44445: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4444C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44453: 		End  { 29 02 }
0x44455: 		OneOf Prompt: "DRAM DCA Training", Help: "DRAM DCA Training", QuestionFlags: 0x10, QuestionId: 0x715, VarStoreId: 0x4, VarOffset: 0x467, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 09 B3 09 15 07 04 00 67 04 10 10 00 01 00 }
0x44466: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4446D: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44474: 		End  { 29 02 }
0x44476: 		OneOf Prompt: "Write Driver Strength Training", Help: "Write Driver Strength Training", QuestionFlags: 0x10, QuestionId: 0x716, VarStoreId: 0x4, VarOffset: 0x475, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 09 B6 09 16 07 04 00 75 04 10 10 00 01 00 }
0x44487: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4448E: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44495: 		End  { 29 02 }
0x44497: 		OneOf Prompt: "Rank Margin Tool", Help: "Rank Margin Tool Training", QuestionFlags: 0x10, QuestionId: 0x717, VarStoreId: 0x4, VarOffset: 0x219, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 09 98 09 17 07 04 00 19 02 10 10 00 01 00 }
0x444A8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x444AF: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x444B6: 		End  { 29 02 }
0x444B8: 		OneOf Prompt: "Memory Test", Help: "Memory Test Training", QuestionFlags: 0x10, QuestionId: 0x718, VarStoreId: 0x4, VarOffset: 0x21A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 09 9A 09 18 07 04 00 1A 02 10 10 00 01 00 }
0x444C9: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x444D0: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x444D7: 		End  { 29 02 }
0x444D9: 		OneOf Prompt: "DQS OFFSET ADJUST Training", Help: "DQS OFFSET ADJUST Training", QuestionFlags: 0x10, QuestionId: 0x719, VarStoreId: 0x4, VarOffset: 0x479, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 09 B5 09 19 07 04 00 79 04 10 10 00 01 00 }
0x444EA: 			OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 04 00 20 00 00 }
0x444F1: 			OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x444F8: 		End  { 29 02 }
0x444FA: 		OneOf Prompt: "DIMM SPD Alias Test", Help: "Test to determine if the SPD has been corrupted to cause memory aliasing.", QuestionFlags: 0x10, QuestionId: 0x71A, VarStoreId: 0x4, VarOffset: 0x21B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 09 9C 09 1A 07 04 00 1B 02 10 10 00 01 00 }
0x4450B: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x44512: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44519: 		End  { 29 02 }
0x4451B: 		OneOf Prompt: "Receive Enable Centering 1D", Help: "Receive Enable Centering 1D", QuestionFlags: 0x10, QuestionId: 0x71B, VarStoreId: 0x4, VarOffset: 0x21C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 09 9D 09 1B 07 04 00 1C 02 10 10 00 01 00 }
0x4452C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44533: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4453A: 		End  { 29 02 }
0x4453C: 		OneOf Prompt: "Retrain Margin Check", Help: "Retrain Margin Check", QuestionFlags: 0x10, QuestionId: 0x71C, VarStoreId: 0x4, VarOffset: 0x21D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9E 09 9E 09 1C 07 04 00 1D 02 10 10 00 01 00 }
0x4454D: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x44554: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4455B: 		End  { 29 02 }
0x4455D: 		OneOf Prompt: "Write Drive Strength Up/Dn independently", Help: "Write Drive Strength Up/Dn independently", QuestionFlags: 0x10, QuestionId: 0x71D, VarStoreId: 0x4, VarOffset: 0x21E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 09 AE 09 1D 07 04 00 1E 02 10 10 00 01 00 }
0x4456E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44575: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4457C: 		End  { 29 02 }
0x4457E: 		OneOf Prompt: "Margin Check Limit", Help: "Checks Margin to Limit to see if next boot memory needs to be retrain", QuestionFlags: 0x10, QuestionId: 0x71E, VarStoreId: 0x4, VarOffset: 0x3F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 B7 09 B8 09 1E 07 04 00 F0 03 10 10 00 03 00 }
0x4458F: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x44596: 			OneOfOption Option: "L1" Value: 1 { 09 07 B9 09 00 00 01 }
0x4459D: 			OneOfOption Option: "L2" Value: 2 { 09 07 BA 09 00 00 02 }
0x445A4: 			OneOfOption Option: "Both" Value: 3 { 09 07 BB 09 00 00 03 }
0x445AB: 		End  { 29 02 }
0x445AD: 		GrayOutIf  { 19 82 }
0x445AF: 			EqIdVal QuestionId: 0x71E, Value: 0x0 { 12 86 1E 07 00 00 }
0x445B5: 				EqIdVal QuestionId: 0x71E, Value: 0x1 { 12 06 1E 07 01 00 }
0x445BB: 				Or  { 16 02 }
0x445BD: 			End  { 29 02 }
0x445BF: 			Numeric Prompt: "Margin Limit Check L2 ", Help: "L2 check threshold is scale of L1 check. Ex. 200 is 2 x L1 Check", QuestionFlags: 0x10, QuestionId: 0x71F, VarStoreId: 0x4, VarOffset: 0x3F1, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x12C, Step: 0x1 { 07 94 BC 09 BD 09 1F 07 04 00 F1 03 10 11 01 00 2C 01 01 00 }
0x445D3: 				Default DefaultId: 0x0 Value: 100 { 5B 07 00 00 01 64 00 }
0x445DA: 			End  { 29 02 }
0x445DC: 		End  { 29 02 }
0x445DE: 	End  { 29 02 }
0x445E0: 	Form FormId: 0x27BB, Title: "SA TCSS USB Configuration" { 01 86 BB 27 3D 0F }
0x445E6: 		OneOf Prompt: "USB CONNECT OVERRIDE", Help: "Option will allow VCCSTTPC to turn off even when there is a connection for a USB3 port.", QuestionFlags: 0x10, QuestionId: 0x720, VarStoreId: 0x4, VarOffset: 0xC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 52 0F 53 0F 20 07 04 00 C3 00 10 10 00 01 00 }
0x445F7: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x445FE: 			OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x44605: 		End  { 29 02 }
0x44607: 		OneOf Prompt: "TCSS xDCI Support", Help: "Enable/Disable TCSS xDCI", QuestionFlags: 0x10, QuestionId: 0x721, VarStoreId: 0x4, VarOffset: 0xBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 75 0E 76 0E 21 07 04 00 BF 00 10 10 00 01 00 }
0x44618: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4461F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44626: 		End  { 29 02 }
0x44628: 		OneOf Prompt: "TCSS CPU USB PDO Programming", Help: "Select 'Enabled' if Port Disable Override functionality is used.", QuestionFlags: 0x10, QuestionId: 0x722, VarStoreId: 0x4, VarOffset: 0x3E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 0F 41 0F 22 07 04 00 E8 03 10 10 00 01 00 }
0x44639: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44640: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44647: 		End  { 29 02 }
0x44649: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x44650: 		End  { 29 02 }
0x44652: 		SuppressIf  { 0A 82 }
0x44654: 			EqIdVal QuestionId: 0x722, Value: 0x0 { 12 06 22 07 00 00 }
0x4465A: 			OneOf Prompt: "TCSS CPU USB Port Disable Override", Help: "Selectively Enable/Disable the corresponding USB port from reporting a Device Connection to the controller.", QuestionFlags: 0x10, QuestionId: 0x723, VarStoreId: 0x4, VarOffset: 0x3E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 0F 43 0F 23 07 04 00 E9 03 10 10 00 01 00 }
0x4466B: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x44671: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x44678: 				OneOfOption Option: "Select Per-Pin" Value: 1 { 09 07 44 0F 00 00 01 }
0x4467F: 			End  { 29 02 }
0x44681: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x44688: 			End  { 29 02 }
0x4468A: 			SuppressIf  { 0A 82 }
0x4468C: 				EqIdVal QuestionId: 0x723, Value: 0x0 { 12 06 23 07 00 00 }
0x44692: 				SuppressIf  { 0A 82 }
0x44694: 					EqIdVal QuestionId: 0x116E, Value: 0x0 { 12 06 6E 11 00 00 }
0x4469A: 					OneOf Prompt: "TCSS CPU USB SS Physical Connector #0", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x724, VarStoreId: 0x4, VarOffset: 0x3EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 45 0F 73 16 24 07 04 00 EA 03 10 10 00 01 00 }
0x446AB: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x446B2: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x446B9: 					End  { 29 02 }
0x446BB: 				End  { 29 02 }
0x446BD: 				SuppressIf  { 0A 82 }
0x446BF: 					EqIdVal QuestionId: 0x116D, Value: 0x0 { 12 06 6D 11 00 00 }
0x446C5: 					OneOf Prompt: "TCSS CPU USB SS Physical Connector #1", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x725, VarStoreId: 0x4, VarOffset: 0x3EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 0F 73 16 25 07 04 00 EB 03 10 10 00 01 00 }
0x446D6: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x446DD: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x446E4: 					End  { 29 02 }
0x446E6: 				End  { 29 02 }
0x446E8: 				SuppressIf  { 0A 82 }
0x446EA: 					EqIdVal QuestionId: 0x116C, Value: 0x0 { 12 06 6C 11 00 00 }
0x446F0: 					OneOf Prompt: "TCSS CPU USB SS Physical Connector #2", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x726, VarStoreId: 0x4, VarOffset: 0x3EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 47 0F 73 16 26 07 04 00 EC 03 10 10 00 01 00 }
0x44701: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44708: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4470F: 					End  { 29 02 }
0x44711: 				End  { 29 02 }
0x44713: 				SuppressIf  { 0A 82 }
0x44715: 					EqIdVal QuestionId: 0x116B, Value: 0x0 { 12 06 6B 11 00 00 }
0x4471B: 					OneOf Prompt: "TCSS CPU USB SS Physical Connector #3", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x727, VarStoreId: 0x4, VarOffset: 0x3ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 0F 73 16 27 07 04 00 ED 03 10 10 00 01 00 }
0x4472C: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44733: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4473A: 					End  { 29 02 }
0x4473C: 				End  { 29 02 }
0x4473E: 			End  { 29 02 }
0x44740: 		End  { 29 02 }
0x44742: 	End  { 29 02 }
0x44744: 	Form FormId: 0x27BC, Title: "Memory Thermal Configuration" { 01 86 BC 27 48 09 }
0x4474A: 		Subtitle Prompt: "Memory Thermal Configuration", Help: "", Flags: 0x0 { 02 87 48 09 00 00 00 }
0x44751: 		End  { 29 02 }
0x44753: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4475A: 		End  { 29 02 }
0x4475C: 		Ref Prompt: "Memory Power and Thermal Throttling", Help: ".", QuestionFlags: 0x0, QuestionId: 0x728, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BD { 0F 0F 30 09 31 09 28 07 00 00 FF FF 00 BD 27 }
0x4476B: 		OneOf Prompt: "Memory Thermal Management", Help: "Enable/Disable Memory Thermal Management.", QuestionFlags: 0x10, QuestionId: 0x729, VarStoreId: 0x4, VarOffset: 0x22C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 49 09 4A 09 29 07 04 00 2C 02 10 10 00 01 00 }
0x4477C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44783: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4478A: 		End  { 29 02 }
0x4478C: 		SuppressIf  { 0A 82 }
0x4478E: 			EqIdVal QuestionId: 0x729, Value: 0x0 { 12 06 29 07 00 00 }
0x44794: 			OneOf Prompt: "PECI Injected Temperature", Help: "Enable/Disable memory temperatures to be injected to the processor via PECI.", QuestionFlags: 0x10, QuestionId: 0x72A, VarStoreId: 0x4, VarOffset: 0x22D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4B 09 4C 09 2A 07 04 00 2D 02 10 10 00 01 00 }
0x447A5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x447AC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x447B3: 			End  { 29 02 }
0x447B5: 			OneOf Prompt: "EXTTS# via TS-on-Board", Help: "Enable/Disable routing TS-on-Board's ALERT# and THERM# to EXTTS# pins on the PCH.", QuestionFlags: 0x10, QuestionId: 0x72B, VarStoreId: 0x4, VarOffset: 0x22E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4D 09 4E 09 2B 07 04 00 2E 02 10 10 00 01 00 }
0x447C6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x447CD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x447D4: 			End  { 29 02 }
0x447D6: 			OneOf Prompt: "EXTTS# via TS-on-DIMM", Help: "Enable/Disable routing TS-on-DIMM's ALERT# to EXTTS# pin on the PCH.", QuestionFlags: 0x10, QuestionId: 0x72C, VarStoreId: 0x4, VarOffset: 0x22F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4F 09 50 09 2C 07 04 00 2F 02 10 10 00 01 00 }
0x447E7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x447EE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x447F5: 			End  { 29 02 }
0x447F7: 			OneOf Prompt: "Virtual Temperature Sensor (VTS)", Help: "Enable/Disable Virtual Temperature Sensor (VTS).", QuestionFlags: 0x10, QuestionId: 0x72D, VarStoreId: 0x4, VarOffset: 0x230, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 51 09 52 09 2D 07 04 00 30 02 10 10 00 01 00 }
0x44808: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4480F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44816: 			End  { 29 02 }
0x44818: 		End  { 29 02 }
0x4481A: 	End  { 29 02 }
0x4481C: 	Form FormId: 0x27BD, Title: "Memory Power and Thermal Throttling" { 01 86 BD 27 30 09 }
0x44822: 		Subtitle Prompt: "Memory Power and Thermal Throttling", Help: "", Flags: 0x0 { 02 87 30 09 00 00 00 }
0x44829: 		End  { 29 02 }
0x4482B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x44832: 		End  { 29 02 }
0x44834: 		OneOf Prompt: "DDR PowerDown and idle counter", Help: "BIOS: BIOS is in control of DDR CKE mode and idle timer value. PCODE: pcode will manage the modes.", QuestionFlags: 0x10, QuestionId: 0x72E, VarStoreId: 0x4, VarOffset: 0x21F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 09 33 09 2E 07 04 00 1F 02 10 10 00 01 00 }
0x44845: 			OneOfOption Option: "PCODE" Value: 0 { 09 07 37 09 00 00 00 }
0x4484C: 			OneOfOption Option: "BIOS" Value: 1, Default, MfgDefault { 09 07 36 09 30 00 01 }
0x44853: 		End  { 29 02 }
0x44855: 		OneOf Prompt: "For LPDDR Only: DDR PowerDown and idle counter", Help: "For LPDDR Only: BIOS: BIOS is in control of DDR CKE mode and idle timer value. PCODE: pcode will manage the modes.", QuestionFlags: 0x10, QuestionId: 0x72F, VarStoreId: 0x4, VarOffset: 0x220, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 09 35 09 2F 07 04 00 20 02 10 10 00 01 00 }
0x44866: 			OneOfOption Option: "PCODE" Value: 0 { 09 07 37 09 00 00 00 }
0x4486D: 			OneOfOption Option: "BIOS" Value: 1, Default, MfgDefault { 09 07 36 09 30 00 01 }
0x44874: 		End  { 29 02 }
0x44876: 		OneOf Prompt: "REFRESH_2X_MODE", Help: "0- Disabled 1-iMC enables 2xRef when Warm and Hot 2- iMC enables 2xRef when Hot", QuestionFlags: 0x10, QuestionId: 0x730, VarStoreId: 0x4, VarOffset: 0x221, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 38 09 39 09 30 07 04 00 21 02 10 10 00 02 00 }
0x44887: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4488E: 			OneOfOption Option: "1- Enabled for WARM or HOT" Value: 1 { 09 07 3A 09 00 00 01 }
0x44895: 			OneOfOption Option: "2- Enabled HOT only" Value: 2 { 09 07 3B 09 00 00 02 }
0x4489C: 		End  { 29 02 }
0x4489E: 		OneOf Prompt: "SelfRefresh Enable", Help: "Enable, Disable(Enable= Def)", QuestionFlags: 0x10, QuestionId: 0x731, VarStoreId: 0x4, VarOffset: 0x223, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 09 3D 09 31 07 04 00 23 02 10 10 00 01 00 }
0x448AF: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x448B6: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x448BD: 		End  { 29 02 }
0x448BF: 		Numeric Prompt: "SelfRefresh IdleTimer", Help: "range [64K-1;512]in DLCK800s, (512= Def)", QuestionFlags: 0x10, QuestionId: 0x732, VarStoreId: 0x4, VarOffset: 0x224, Flags: 0x11, Size: 16, Min: 0x200, Max: 0xFFFF, Step: 0x1 { 07 94 3E 09 3F 09 32 07 04 00 24 02 10 11 00 02 FF FF 01 00 }
0x448D3: 			Default DefaultId: 0x0 Value: 512 { 5B 07 00 00 01 00 02 }
0x448DA: 		End  { 29 02 }
0x448DC: 		OneOf Prompt: "Throttler CKEMin Defeature", Help: "On, Off", QuestionFlags: 0x10, QuestionId: 0x733, VarStoreId: 0x4, VarOffset: 0x226, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 09 41 09 33 07 04 00 26 02 10 10 00 01 00 }
0x448ED: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x448F4: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x448FB: 		End  { 29 02 }
0x448FD: 		Numeric Prompt: "Throttler CKEMin Timer", Help: "Timer value for CKEMin, range[255;0]. Req'd min of SC_ROUND_T + BYTE_LENGTH (4)", QuestionFlags: 0x10, QuestionId: 0x734, VarStoreId: 0x4, VarOffset: 0x227, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 42 09 43 09 34 07 04 00 27 02 10 10 00 FF 01 }
0x4490E: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x44914: 		End  { 29 02 }
0x44916: 		OneOf Prompt: "Allow Opp Ref Below Write Threhold", Help: "Allow opportunistic refreshes while we don't exit power down.", QuestionFlags: 0x10, QuestionId: 0x735, VarStoreId: 0x4, VarOffset: 0x22A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 08 92 08 35 07 04 00 2A 02 10 10 00 01 00 }
0x44927: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x4492E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x44935: 		End  { 29 02 }
0x44937: 		Numeric Prompt: "Write Threshold", Help: "Number of writes that can be accumulated while CKE is low before CKE is asserted.", QuestionFlags: 0x10, QuestionId: 0x736, VarStoreId: 0x4, VarOffset: 0x22B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 93 08 94 08 36 07 04 00 2B 02 10 10 00 3F 01 }
0x44948: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4494E: 		End  { 29 02 }
0x44950: 		SuppressIf  { 0A 82 }
0x44952: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x44958: 				Not  { 17 02 }
0x4495A: 			End  { 29 02 }
0x4495C: 			OneOf Prompt: "For LPDDR Only: Throttler CKEMin Defeature", Help: "For LPDDR Only: On, Off", QuestionFlags: 0x10, QuestionId: 0x737, VarStoreId: 0x4, VarOffset: 0x228, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 09 45 09 37 07 04 00 28 02 10 10 00 01 00 }
0x4496D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x44974: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4497B: 			End  { 29 02 }
0x4497D: 			Numeric Prompt: "For LPDDR Only: Throttler CKEMin Timer", Help: "For LPDDR Only: Timer value for CKEMin, range[255;0]. Req'd min of SC_ROUND_T + BYTE_LENGTH (4)", QuestionFlags: 0x10, QuestionId: 0x738, VarStoreId: 0x4, VarOffset: 0x229, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 46 09 47 09 38 07 04 00 29 02 10 10 00 FF 01 }
0x4498E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x44994: 			End  { 29 02 }
0x44996: 		End  { 29 02 }
0x44998: 	End  { 29 02 }
0x4499A: 	Form FormId: 0x27BE, Title: "MIPI Camera Configuration" { 01 86 BE 27 48 0B }
0x449A0: 		OneOf Prompt: "CVF Support", Help: "Disables/Enables CVF using either Native IOs or USB IOs Expansion. ", QuestionFlags: 0x10, QuestionId: 0x739, VarStoreId: 0xF101, VarOffset: 0x9D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 49 0B 4A 0B 39 07 01 F1 D9 09 10 10 00 02 00 }
0x449B1: 			OneOfOption Option: "Native IOs" Value: 1 { 09 07 4B 0B 00 00 01 }
0x449B8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x449BF: 			OneOfOption Option: "USB Bridge" Value: 2 { 09 07 4C 0B 00 00 02 }
0x449C6: 		End  { 29 02 }
0x449C8: 		OneOf Prompt: "Control Logic 1", Help: "Control Logic 1", QuestionFlags: 0x10, QuestionId: 0x73A, VarStoreId: 0xF101, VarOffset: 0x6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 0D 22 0D 3A 07 01 F1 6F 00 10 10 00 01 00 }
0x449D9: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x449E0: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x449E7: 		End  { 29 02 }
0x449E9: 		SuppressIf  { 0A 82 }
0x449EB: 			EqIdVal QuestionId: 0x73A, Value: 0x0 { 12 06 3A 07 00 00 }
0x449F1: 			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0x73B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x93 { 0F 0F 21 0D 21 0D 3B 07 00 00 FF FF 00 93 00 }
0x44A00: 		End  { 29 02 }
0x44A02: 		OneOf Prompt: "Control Logic 2", Help: "Control Logic 2", QuestionFlags: 0x10, QuestionId: 0x73C, VarStoreId: 0xF101, VarOffset: 0x70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 23 0D 23 0D 3C 07 01 F1 70 00 10 10 00 01 00 }
0x44A13: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44A1A: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44A21: 		End  { 29 02 }
0x44A23: 		SuppressIf  { 0A 82 }
0x44A25: 			EqIdVal QuestionId: 0x73C, Value: 0x0 { 12 06 3C 07 00 00 }
0x44A2B: 			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0x73D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x94 { 0F 0F A7 10 21 0D 3D 07 00 00 FF FF 00 94 00 }
0x44A3A: 		End  { 29 02 }
0x44A3C: 		OneOf Prompt: "Control Logic 3", Help: "Control Logic 3", QuestionFlags: 0x10, QuestionId: 0x73E, VarStoreId: 0xF101, VarOffset: 0x71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 0D 24 0D 3E 07 01 F1 71 00 10 10 00 01 00 }
0x44A4D: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44A54: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44A5B: 		End  { 29 02 }
0x44A5D: 		SuppressIf  { 0A 82 }
0x44A5F: 			EqIdVal QuestionId: 0x73E, Value: 0x0 { 12 06 3E 07 00 00 }
0x44A65: 			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0x73F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x95 { 0F 0F A8 10 21 0D 3F 07 00 00 FF FF 00 95 00 }
0x44A74: 		End  { 29 02 }
0x44A76: 		OneOf Prompt: "Control Logic 4", Help: "Control Logic 4", QuestionFlags: 0x10, QuestionId: 0x740, VarStoreId: 0xF101, VarOffset: 0x72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 25 0D 25 0D 40 07 01 F1 72 00 10 10 00 01 00 }
0x44A87: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44A8E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44A95: 		End  { 29 02 }
0x44A97: 		SuppressIf  { 0A 82 }
0x44A99: 			EqIdVal QuestionId: 0x740, Value: 0x0 { 12 06 40 07 00 00 }
0x44A9F: 			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0x741, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x96 { 0F 0F A9 10 21 0D 41 07 00 00 FF FF 00 96 00 }
0x44AAE: 		End  { 29 02 }
0x44AB0: 		SuppressIf  { 0A 82 }
0x44AB2: 			EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x44AB8: 				Not  { 17 02 }
0x44ABA: 			End  { 29 02 }
0x44ABC: 			OneOf Prompt: "Control Logic 5", Help: "Control Logic 5", QuestionFlags: 0x10, QuestionId: 0x742, VarStoreId: 0xF101, VarOffset: 0x73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 0D 26 0D 42 07 01 F1 73 00 10 10 00 01 00 }
0x44ACD: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44AD4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44ADB: 			End  { 29 02 }
0x44ADD: 		End  { 29 02 }
0x44ADF: 		SuppressIf  { 0A 82 }
0x44AE1: 			EqIdVal QuestionId: 0x742, Value: 0x0 { 12 06 42 07 00 00 }
0x44AE7: 			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0x743, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x97 { 0F 0F AA 10 21 0D 43 07 00 00 FF FF 00 97 00 }
0x44AF6: 		End  { 29 02 }
0x44AF8: 		SuppressIf  { 0A 82 }
0x44AFA: 			EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x44B00: 				Not  { 17 02 }
0x44B02: 			End  { 29 02 }
0x44B04: 			OneOf Prompt: "Control Logic 6", Help: "Control Logic 6", QuestionFlags: 0x10, QuestionId: 0x744, VarStoreId: 0xF101, VarOffset: 0x74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 0D 27 0D 44 07 01 F1 74 00 10 10 00 01 00 }
0x44B15: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44B1C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44B23: 			End  { 29 02 }
0x44B25: 		End  { 29 02 }
0x44B27: 		SuppressIf  { 0A 82 }
0x44B29: 			EqIdVal QuestionId: 0x744, Value: 0x0 { 12 06 44 07 00 00 }
0x44B2F: 			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0x745, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x98 { 0F 0F AB 10 21 0D 45 07 00 00 FF FF 00 98 00 }
0x44B3E: 		End  { 29 02 }
0x44B40: 		OneOf Prompt: "Camera1", Help: "Camera1", QuestionFlags: 0x10, QuestionId: 0x746, VarStoreId: 0xF101, VarOffset: 0x75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4D 0B 4D 0B 46 07 01 F1 75 00 10 10 00 01 00 }
0x44B51: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44B58: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44B5F: 		End  { 29 02 }
0x44B61: 		SuppressIf  { 0A 82 }
0x44B63: 			EqIdVal QuestionId: 0x746, Value: 0x0 { 12 06 46 07 00 00 }
0x44B69: 			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0x747, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x8D { 0F 0F 5E 0B 5E 0B 47 07 00 00 FF FF 00 8D 00 }
0x44B78: 			SuppressIf  { 0A 82 }
0x44B7A: 				EqIdVal QuestionId: 0x784, Value: 0x0 { 12 06 84 07 00 00 }
0x44B80: 				Ref Prompt: "Flash Options", Help: "Flash Options", QuestionFlags: 0x0, QuestionId: 0x748, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BF { 0F 0F A0 0D A0 0D 48 07 00 00 FF FF 00 BF 27 }
0x44B8F: 			End  { 29 02 }
0x44B91: 		End  { 29 02 }
0x44B93: 		OneOf Prompt: "Camera2", Help: "Camera2", QuestionFlags: 0x10, QuestionId: 0x749, VarStoreId: 0xF101, VarOffset: 0x76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 0B 4E 0B 49 07 01 F1 76 00 10 10 00 01 00 }
0x44BA4: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44BAB: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44BB2: 		End  { 29 02 }
0x44BB4: 		SuppressIf  { 0A 82 }
0x44BB6: 			EqIdVal QuestionId: 0x749, Value: 0x0 { 12 06 49 07 00 00 }
0x44BBC: 			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0x74A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x8E { 0F 0F F7 0F 5E 0B 4A 07 00 00 FF FF 00 8E 00 }
0x44BCB: 			SuppressIf  { 0A 82 }
0x44BCD: 				EqIdVal QuestionId: 0x7B2, Value: 0x0 { 12 06 B2 07 00 00 }
0x44BD3: 				Ref Prompt: "Flash Options", Help: "Flash Options", QuestionFlags: 0x0, QuestionId: 0x74B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C0 { 0F 0F B4 10 A0 0D 4B 07 00 00 FF FF 00 C0 27 }
0x44BE2: 			End  { 29 02 }
0x44BE4: 		End  { 29 02 }
0x44BE6: 		OneOf Prompt: "Camera3", Help: "Camera3", QuestionFlags: 0x10, QuestionId: 0x74C, VarStoreId: 0xF101, VarOffset: 0x77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4F 0B 4F 0B 4C 07 01 F1 77 00 10 10 00 01 00 }
0x44BF7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x44BFE: 			OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x44C05: 		End  { 29 02 }
0x44C07: 		SuppressIf  { 0A 82 }
0x44C09: 			EqIdVal QuestionId: 0x74C, Value: 0x0 { 12 06 4C 07 00 00 }
0x44C0F: 			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0x74D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x8F { 0F 0F F8 0F 5E 0B 4D 07 00 00 FF FF 00 8F 00 }
0x44C1E: 			SuppressIf  { 0A 82 }
0x44C20: 				EqIdVal QuestionId: 0x7E0, Value: 0x0 { 12 06 E0 07 00 00 }
0x44C26: 				Ref Prompt: "Flash Options", Help: "Flash Options", QuestionFlags: 0x0, QuestionId: 0x74E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C1 { 0F 0F B5 10 A0 0D 4E 07 00 00 FF FF 00 C1 27 }
0x44C35: 			End  { 29 02 }
0x44C37: 		End  { 29 02 }
0x44C39: 		OneOf Prompt: "Camera4", Help: "Camera4", QuestionFlags: 0x10, QuestionId: 0x74F, VarStoreId: 0xF101, VarOffset: 0x78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 50 0B 50 0B 4F 07 01 F1 78 00 10 10 00 01 00 }
0x44C4A: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44C51: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44C58: 		End  { 29 02 }
0x44C5A: 		SuppressIf  { 0A 82 }
0x44C5C: 			EqIdVal QuestionId: 0x74F, Value: 0x0 { 12 06 4F 07 00 00 }
0x44C62: 			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0x750, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x90 { 0F 0F F9 0F 5E 0B 50 07 00 00 FF FF 00 90 00 }
0x44C71: 			SuppressIf  { 0A 82 }
0x44C73: 				EqIdVal QuestionId: 0x80E, Value: 0x0 { 12 06 0E 08 00 00 }
0x44C79: 				Ref Prompt: "Flash Options", Help: "Flash Options", QuestionFlags: 0x0, QuestionId: 0x751, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C2 { 0F 0F B6 10 A0 0D 51 07 00 00 FF FF 00 C2 27 }
0x44C88: 			End  { 29 02 }
0x44C8A: 		End  { 29 02 }
0x44C8C: 		SuppressIf  { 0A 82 }
0x44C8E: 			EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x44C94: 				Not  { 17 02 }
0x44C96: 			End  { 29 02 }
0x44C98: 			OneOf Prompt: "Camera5", Help: "Camera5", QuestionFlags: 0x10, QuestionId: 0x752, VarStoreId: 0xF101, VarOffset: 0x79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 51 0B 51 0B 52 07 01 F1 79 00 10 10 00 01 00 }
0x44CA9: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44CB0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44CB7: 			End  { 29 02 }
0x44CB9: 		End  { 29 02 }
0x44CBB: 		SuppressIf  { 0A 82 }
0x44CBD: 			EqIdVal QuestionId: 0x752, Value: 0x0 { 12 06 52 07 00 00 }
0x44CC3: 			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0x753, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x91 { 0F 0F FA 0F 5E 0B 53 07 00 00 FF FF 00 91 00 }
0x44CD2: 			SuppressIf  { 0A 82 }
0x44CD4: 				EqIdVal QuestionId: 0x83C, Value: 0x0 { 12 06 3C 08 00 00 }
0x44CDA: 				Ref Prompt: "Flash Options", Help: "Flash Options", QuestionFlags: 0x0, QuestionId: 0x754, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C3 { 0F 0F B7 10 A0 0D 54 07 00 00 FF FF 00 C3 27 }
0x44CE9: 			End  { 29 02 }
0x44CEB: 		End  { 29 02 }
0x44CED: 		SuppressIf  { 0A 82 }
0x44CEF: 			EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x44CF5: 				Not  { 17 02 }
0x44CF7: 			End  { 29 02 }
0x44CF9: 			OneOf Prompt: "Camera6", Help: "Camera6", QuestionFlags: 0x10, QuestionId: 0x755, VarStoreId: 0xF101, VarOffset: 0x7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 52 0B 52 0B 55 07 01 F1 7A 00 10 10 00 01 00 }
0x44D0A: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x44D11: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x44D18: 			End  { 29 02 }
0x44D1A: 		End  { 29 02 }
0x44D1C: 		SuppressIf  { 0A 82 }
0x44D1E: 			EqIdVal QuestionId: 0x755, Value: 0x0 { 12 06 55 07 00 00 }
0x44D24: 			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0x756, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x92 { 0F 0F FB 0F 5E 0B 56 07 00 00 FF FF 00 92 00 }
0x44D33: 			SuppressIf  { 0A 82 }
0x44D35: 				EqIdVal QuestionId: 0x86A, Value: 0x0 { 12 06 6A 08 00 00 }
0x44D3B: 				Ref Prompt: "Flash Options", Help: "Flash Options", QuestionFlags: 0x0, QuestionId: 0x757, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C4 { 0F 0F B8 10 A0 0D 57 07 00 00 FF FF 00 C4 27 }
0x44D4A: 			End  { 29 02 }
0x44D4C: 		End  { 29 02 }
0x44D4E: 	End  { 29 02 }
0x44D50: 	Form FormId: 0x8D, Title: "Link0 options" { 01 86 8D 00 5F 0B }
0x44D56: 		Subtitle Prompt: "Camera1", Help: "", Flags: 0x0 { 02 87 4D 0B 00 00 00 }
0x44D5D: 		End  { 29 02 }
0x44D5F: 		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0x758, VarStoreId: 0xF101, VarOffset: 0x1A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 66 0B 65 0B 58 07 01 F1 A4 01 10 10 00 FF 00 }
0x44D70: 			OneOfOption Option: "IMX135" Value: 0 { 09 07 FF 0C 00 00 00 }
0x44D77: 			OneOfOption Option: "OV5693" Value: 1 { 09 07 00 0D 00 00 01 }
0x44D7E: 			OneOfOption Option: "IMX179" Value: 2 { 09 07 01 0D 00 00 02 }
0x44D85: 			OneOfOption Option: "OV8858" Value: 3 { 09 07 02 0D 00 00 03 }
0x44D8C: 			OneOfOption Option: "OV2740-IVCAM" Value: 4 { 09 07 03 0D 00 00 04 }
0x44D93: 			OneOfOption Option: "OV9728" Value: 5 { 09 07 04 0D 00 00 05 }
0x44D9A: 			OneOfOption Option: "IMX188" Value: 6 { 09 07 05 0D 00 00 06 }
0x44DA1: 			OneOfOption Option: "IMX208" Value: 7 { 09 07 06 0D 00 00 07 }
0x44DA8: 			OneOfOption Option: "OV5670" Value: 8 { 09 07 07 0D 00 00 08 }
0x44DAF: 			OneOfOption Option: "OV8865" Value: 9 { 09 07 08 0D 00 00 09 }
0x44DB6: 			OneOfOption Option: "HM2051" Value: 10 { 09 07 09 0D 00 00 0A }
0x44DBD: 			OneOfOption Option: "OV2742" Value: 11 { 09 07 0A 0D 00 00 0B }
0x44DC4: 			OneOfOption Option: "OV9234" Value: 12 { 09 07 0B 0D 00 00 0C }
0x44DCB: 			OneOfOption Option: "OV8856" Value: 13 { 09 07 0C 0D 00 00 0D }
0x44DD2: 			OneOfOption Option: "OV16860" Value: 14 { 09 07 0D 0D 00 00 0E }
0x44DD9: 			OneOfOption Option: "IMX362" Value: 15, Default { 09 07 0E 0D 10 00 0F }
0x44DE0: 			OneOfOption Option: "IMX488" Value: 16 { 09 07 0F 0D 00 00 10 }
0x44DE7: 			OneOfOption Option: "OVTI01AS" Value: 17 { 09 07 11 0D 00 00 11 }
0x44DEE: 			OneOfOption Option: "OVTI01A0" Value: 18 { 09 07 12 0D 00 00 12 }
0x44DF5: 			OneOfOption Option: "OVTI5678" Value: 19 { 09 07 13 0D 00 00 13 }
0x44DFC: 			OneOfOption Option: "OVTI9738" Value: 20 { 09 07 14 0D 00 00 14 }
0x44E03: 			OneOfOption Option: "HIMAX11B1" Value: 21 { 09 07 16 0D 00 00 15 }
0x44E0A: 			OneOfOption Option: "User Custom" Value: 255 { 09 07 17 0D 00 00 FF }
0x44E11: 		End  { 29 02 }
0x44E13: 		SuppressIf  { 0A 82 }
0x44E15: 			EqIdVal QuestionId: 0x758, Value: 0xFF { 12 86 58 07 FF 00 }
0x44E1B: 				Not  { 17 02 }
0x44E1D: 			End  { 29 02 }
0x44E1F: 			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0x759, VarStoreId: 0xF101, VarStoreInfo: 0x1A5, MinSize: 0x6, MaxSize: 0x14, Flags: 0x0 { 1C 90 18 0D 18 0D 59 07 01 F1 A5 01 00 06 14 00 }
0x44E2F: 			End  { 29 02 }
0x44E31: 		End  { 29 02 }
0x44E33: 		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0x75A, VarStoreId: 0xF101, VarOffset: 0xA92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 77 0B 76 0B 5A 07 01 F1 92 0A 10 10 00 07 00 }
0x44E44: 			OneOfOption Option: "4 4 2 2" Value: 0, Default { 09 07 7D 0B 10 00 00 }
0x44E4B: 			OneOfOption Option: "4 4 3 1" Value: 2 { 09 07 7E 0B 00 00 02 }
0x44E52: 			OneOfOption Option: "4 4 4 0" Value: 3 { 09 07 7F 0B 00 00 03 }
0x44E59: 			OneOfOption Option: "8 0 2 2" Value: 4 { 09 07 80 0B 00 00 04 }
0x44E60: 			OneOfOption Option: "8 0 3 1" Value: 6 { 09 07 81 0B 00 00 06 }
0x44E67: 			OneOfOption Option: "8 0 4 0" Value: 7 { 09 07 82 0B 00 00 07 }
0x44E6E: 		End  { 29 02 }
0x44E70: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x75B, VarStoreId: 0xF101, VarOffset: 0x215, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 AA 0C A9 0C 5B 07 01 F1 15 02 10 10 10 50 00 }
0x44E81: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x44E88: 			OneOfOption Option: "CRD-G" Value: 48 { 09 07 B4 0C 00 00 30 }
0x44E8F: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x44E96: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x44E9D: 			OneOfOption Option: "CRD-G2" Value: 80, Default { 09 07 B6 0C 10 00 50 }
0x44EA4: 		End  { 29 02 }
0x44EA6: 		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0x75C, VarStoreId: 0xF101, VarOffset: 0x223, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 7F 0D 7E 0D 5C 07 01 F1 23 02 10 10 00 FF 00 }
0x44EB7: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x44EBD: 			OneOfOption Option: "No Control Logic" Value: 255 { 09 07 28 0D 00 00 FF }
0x44EC4: 			OneOfOption Option: "Control Logic 1" Value: 0 { 09 07 22 0D 00 00 00 }
0x44ECB: 			OneOfOption Option: "Control Logic 2" Value: 1 { 09 07 23 0D 00 00 01 }
0x44ED2: 			OneOfOption Option: "Control Logic 3" Value: 2 { 09 07 24 0D 00 00 02 }
0x44ED9: 			OneOfOption Option: "Control Logic 4" Value: 3 { 09 07 25 0D 00 00 03 }
0x44EE0: 			SuppressIf  { 0A 82 }
0x44EE2: 				EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x44EE8: 					Not  { 17 02 }
0x44EEA: 				End  { 29 02 }
0x44EEC: 				OneOfOption Option: "Control Logic 5" Value: 3 { 09 07 26 0D 00 00 03 }
0x44EF3: 			End  { 29 02 }
0x44EF5: 			SuppressIf  { 0A 82 }
0x44EF7: 				EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x44EFD: 					Not  { 17 02 }
0x44EFF: 				End  { 29 02 }
0x44F01: 				OneOfOption Option: "Control Logic 6" Value: 3 { 09 07 27 0D 00 00 03 }
0x44F08: 			End  { 29 02 }
0x44F0A: 		End  { 29 02 }
0x44F0C: 		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0x75D, VarStoreId: 0xF101, VarOffset: 0x1CD, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0 { 05 91 60 0C 5F 0C 5D 07 01 F1 CD 01 10 10 61 69 00 }
0x44F1D: 			OneOfOption Option: "Front" Value: 97 { 09 07 6C 0C 00 00 61 }
0x44F24: 			OneOfOption Option: "Back" Value: 105, Default { 09 07 6D 0C 10 00 69 }
0x44F2B: 		End  { 29 02 }
0x44F2D: 		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0x75E, VarStoreId: 0xF101, VarOffset: 0x224, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 72 0C 71 0C 5E 07 01 F1 24 02 10 10 00 03 00 }
0x44F3E: 			OneOfOption Option: "Driver default" Value: 0 { 09 07 78 0C 00 00 00 }
0x44F45: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x44F4C: 			OneOfOption Option: "Enabled" Value: 3, Default { 09 07 03 00 10 00 03 }
0x44F53: 		End  { 29 02 }
0x44F55: 		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0x75F, VarStoreId: 0xF101, VarOffset: 0x225, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7A 0C 79 0C 5F 07 01 F1 25 02 10 10 00 05 00 }
0x44F66: 			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault { 09 07 80 0C 30 00 00 }
0x44F6D: 			OneOfOption Option: "ILEDA, 16mA" Value: 1 { 09 07 81 0C 00 00 01 }
0x44F74: 			OneOfOption Option: "ILEDB, 2mA" Value: 2 { 09 07 82 0C 00 00 02 }
0x44F7B: 			OneOfOption Option: "ILEDB, 4mA" Value: 3 { 09 07 83 0C 00 00 03 }
0x44F82: 			OneOfOption Option: "ILEDB, 8mA" Value: 4 { 09 07 84 0C 00 00 04 }
0x44F89: 			OneOfOption Option: "ILEDB, 16mA" Value: 5 { 09 07 85 0C 00 00 05 }
0x44F90: 		End  { 29 02 }
0x44F92: 		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0x760, VarStoreId: 0xF101, VarOffset: 0x226, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 87 0C 86 0C 60 07 01 F1 26 02 10 10 00 06 00 }
0x44FA3: 			OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 8D 0C 30 00 00 }
0x44FAA: 			OneOfOption Option: "90" Value: 2 { 09 07 8E 0C 00 00 02 }
0x44FB1: 			OneOfOption Option: "180" Value: 4 { 09 07 8F 0C 00 00 04 }
0x44FB8: 			OneOfOption Option: "270" Value: 6 { 09 07 90 0C 00 00 06 }
0x44FBF: 		End  { 29 02 }
0x44FC1: 		SuppressIf  { 0A 82 }
0x44FC3: 			EqIdVal QuestionId: 0x75B, Value: 0x50 { 12 86 5B 07 50 00 }
0x44FC9: 				Not  { 17 02 }
0x44FCB: 			End  { 29 02 }
0x44FCD: 			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0x761, VarStoreId: 0xF101, VarOffset: 0x227, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 0C 91 0C 61 07 01 F1 27 02 10 10 00 01 00 }
0x44FDE: 				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault { 09 07 97 0C 30 00 00 }
0x44FE5: 				OneOfOption Option: "Position 2" Value: 1 { 09 07 98 0C 00 00 01 }
0x44FEC: 			End  { 29 02 }
0x44FEE: 		End  { 29 02 }
0x44FF0: 		SuppressIf  { 0A 82 }
0x44FF2: 			EqIdVal QuestionId: 0x761, Value: 0x1 { 12 86 61 07 01 00 }
0x44FF8: 				Not  { 17 02 }
0x44FFA: 			End  { 29 02 }
0x44FFC: 			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0x762, VarStoreId: 0xF101, VarOffset: 0x228, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9A 0C 99 0C 62 07 01 F1 28 02 10 10 00 01 00 }
0x4500D: 				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault { 09 07 A0 0C 30 00 00 }
0x45014: 				OneOfOption Option: "2 voltage rail" Value: 1 { 09 07 A1 0C 00 00 01 }
0x4501B: 			End  { 29 02 }
0x4501D: 		End  { 29 02 }
0x4501F: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x763, VarStoreId: 0xF101, VarStoreInfo: 0x1CE, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 66 0C 66 0C 63 07 01 F1 CE 01 00 01 0F 00 }
0x4502F: 			Default DefaultId: 0x0 String: "A12N08B" { 5B 07 00 00 07 67 0C }
0x45036: 		End  { 29 02 }
0x45038: 		Numeric Prompt: "MIPI port", Help: "LinkUsed", QuestionFlags: 0x10, QuestionId: 0x764, VarStoreId: 0xF101, VarOffset: 0x216, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 B8 0C B7 0C 64 07 01 F1 16 02 10 10 00 0A 01 }
0x45049: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4504F: 		End  { 29 02 }
0x45051: 		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0x765, VarStoreId: 0xF101, VarOffset: 0x217, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x8, Step: 0x0 { 05 91 BF 0C BE 0C 65 07 01 F1 17 02 10 10 01 08 00 }
0x45062: 			OneOfOption Option: "x1" Value: 1 { 09 07 F3 0C 00 00 01 }
0x45069: 			OneOfOption Option: "x2" Value: 2 { 09 07 F4 0C 00 00 02 }
0x45070: 			OneOfOption Option: "x3" Value: 3 { 09 07 F5 0C 00 00 03 }
0x45077: 			OneOfOption Option: "x4" Value: 4, Default { 09 07 F6 0C 10 00 04 }
0x4507E: 			OneOfOption Option: "x8" Value: 8 { 09 07 F7 0C 00 00 08 }
0x45085: 		End  { 29 02 }
0x45087: 		OneOf Prompt: "PortSpeed", Help: "PortSpeed: 0:Sensor Default, 1:<416Mbps, 2:<1.5Gbps, 3:<2Gbps, 4:<2.5Gbps, 5:<4Gbps, 6:>4Gbps", QuestionFlags: 0x10, QuestionId: 0x766, VarStoreId: 0xF101, VarOffset: 0x218, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 C5 0C C6 0C 66 07 01 F1 18 02 10 10 00 06 00 }
0x45098: 			OneOfOption Option: "0" Value: 0 { 09 07 F8 0C 00 00 00 }
0x4509F: 			OneOfOption Option: "1" Value: 1 { 09 07 F9 0C 00 00 01 }
0x450A6: 			OneOfOption Option: "2" Value: 2, Default { 09 07 FA 0C 10 00 02 }
0x450AD: 			OneOfOption Option: "3" Value: 3 { 09 07 FB 0C 00 00 03 }
0x450B4: 			OneOfOption Option: "4" Value: 4 { 09 07 FC 0C 00 00 04 }
0x450BB: 			OneOfOption Option: "5" Value: 5 { 09 07 FD 0C 00 00 05 }
0x450C2: 			OneOfOption Option: "6" Value: 6 { 09 07 FE 0C 00 00 06 }
0x450C9: 		End  { 29 02 }
0x450CB: 		Numeric Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0x767, VarStoreId: 0xF101, VarOffset: 0x21F, Flags: 0x12, Size: 32, Min: 0x5B8D80, Max: 0x19BFCC0, Step: 0x186A0 { 07 9A C8 0C C7 0C 67 07 01 F1 1F 02 10 12 80 8D 5B 00 C0 FC 9B 01 A0 86 01 00 }
0x450E5: 			Default DefaultId: 0x0 Value: 19200000 { 5B 09 00 00 02 00 F8 24 01 }
0x450EE: 		End  { 29 02 }
0x450F0: 		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type
0x00: ROM_NONE
0x01: ROM_OTP
0x02: ROM_EEPROM_16K_64
0x03: ROM_EEPROM_16K_16
0x04: ROM_OTP_ACPI_ACPI
0x05: ROM_ACPI
0x06: ROM_EEPROM_BRCA016GWZ
0x07: ROM_EEPROM_24AA32
0x08: ROM_EEPROM_CAT24C08
0x09: ROM_M24C64
0x0A: ROM_DW9806B
0x10: ROM_EEPROM_CAT24C16
0x11: ROM_EEPROM_CAT24C64
0x12: ROM_EEPROM_24AA16", QuestionFlags: 0x10, QuestionId: 0x768, VarStoreId: 0xF101, VarOffset: 0x219, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CA 0C C9 0C 68 07 01 F1 19 02 10 10 00 12 00 }
0x45101: 			OneOfOption Option: "ROM_OTP" Value: 1 { 09 07 D8 0C 00 00 01 }
0x45108: 			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2 { 09 07 D9 0C 00 00 02 }
0x4510F: 			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3 { 09 07 DA 0C 00 00 03 }
0x45116: 			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4 { 09 07 DB 0C 00 00 04 }
0x4511D: 			OneOfOption Option: "ROM_ACPI" Value: 5 { 09 07 DC 0C 00 00 05 }
0x45124: 			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6 { 09 07 DD 0C 00 00 06 }
0x4512B: 			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7 { 09 07 DE 0C 00 00 07 }
0x45132: 			OneOfOption Option: "ROM_EEPROM_M24C64" Value: 9 { 09 07 E0 0C 00 00 09 }
0x45139: 			OneOfOption Option: "ROM_EEPROM_DW9806B" Value: 10 { 09 07 E1 0C 00 00 0A }
0x45140: 			OneOfOption Option: "ROM_EEPROM_CAT24C16" Value: 16 { 09 07 E2 0C 00 00 10 }
0x45147: 			OneOfOption Option: "ROM_EEPROM_CAT24C64" Value: 17 { 09 07 E3 0C 00 00 11 }
0x4514E: 			OneOfOption Option: "ROM_EEPROM_24AA16" Value: 18 { 09 07 E4 0C 00 00 12 }
0x45155: 			OneOfOption Option: "ROM_NONE" Value: 0, Default { 09 07 D7 0C 10 00 00 }
0x4515C: 			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8 { 09 07 DF 0C 00 00 08 }
0x45163: 		End  { 29 02 }
0x45165: 		OneOf Prompt: "VCM Type", Help: "VCM Type
0x00: VCM_NONE
0x01: VCM_AD5823
0x02: VCM_DW9714
0x03: VCM_AD5816
0x04: VCM_DW9719
0x05: VCM_DW9718
0x06: VCM_DW9806B
0x07: VCM_WV517S
0x08: VCM_LC898122XA
0x09: VCM_LC898212AXB
0x0F: VCM_AK7371
0x10: VCM_BU64297GWZ", QuestionFlags: 0x10, QuestionId: 0x769, VarStoreId: 0xF101, VarOffset: 0x21A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0 { 05 91 D1 0C D0 0C 69 07 01 F1 1A 02 10 10 00 10 00 }
0x45176: 			OneOfOption Option: "VCM_NONE" Value: 0 { 09 07 E5 0C 00 00 00 }
0x4517D: 			OneOfOption Option: "VCM_AD5823" Value: 1 { 09 07 E6 0C 00 00 01 }
0x45184: 			OneOfOption Option: "VCM_AD5816" Value: 3 { 09 07 E8 0C 00 00 03 }
0x4518B: 			OneOfOption Option: "VCM_DW9719" Value: 4 { 09 07 EA 0C 00 00 04 }
0x45192: 			OneOfOption Option: "VCM_DW9718" Value: 5 { 09 07 E9 0C 00 00 05 }
0x45199: 			OneOfOption Option: "VCM_DW9806B" Value: 6 { 09 07 EB 0C 00 00 06 }
0x451A0: 			OneOfOption Option: "VCM_WV517S" Value: 7 { 09 07 EC 0C 00 00 07 }
0x451A7: 			OneOfOption Option: "VCM_LC898122XA" Value: 8 { 09 07 ED 0C 00 00 08 }
0x451AE: 			OneOfOption Option: "VCM_LC898212AXB" Value: 9 { 09 07 EE 0C 00 00 09 }
0x451B5: 			OneOfOption Option: "VCM_RESERVED1" Value: 10 { 09 07 EF 0C 00 00 0A }
0x451BC: 			OneOfOption Option: "VCM_RESERVED2" Value: 11 { 09 07 F0 0C 00 00 0B }
0x451C3: 			OneOfOption Option: "VCM_BU64297GWZ" Value: 16 { 09 07 F2 0C 00 00 10 }
0x451CA: 			OneOfOption Option: "VCM_DW9714" Value: 2 { 09 07 E7 0C 00 00 02 }
0x451D1: 			OneOfOption Option: "VCM_AK7371" Value: 15, Default { 09 07 F1 0C 10 00 0F }
0x451D8: 		End  { 29 02 }
0x451DA: 		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0x76A, VarStoreId: 0xF101, VarOffset: 0x1EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1 { 07 91 6D 0B 6C 0B 6A 07 01 F1 EE 01 10 10 00 0C 01 }
0x451EB: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x451F1: 		End  { 29 02 }
0x451F3: 		SuppressIf  { 0A 82 }
0x451F5: 			EqIdVal QuestionId: 0x76A, Value: 0x0 { 12 06 6A 07 00 00 }
0x451FB: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x76B, VarStoreId: 0xF101, VarOffset: 0x1EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 90 0B 8F 0B 6B 07 01 F1 EF 01 10 10 00 05 00 }
0x4520C: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x45213: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4521A: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x45221: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x45228: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4522F: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x45236: 			End  { 29 02 }
0x45238: 			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0 { 02 87 83 0B 00 00 00 }
0x4523F: 			End  { 29 02 }
0x45241: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x76C, VarStoreId: 0xF101, VarOffset: 0x1F0, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 9B 0B 98 0B 6C 07 01 F1 F0 01 10 21 00 00 7F 00 01 00 }
0x45255: 				Default DefaultId: 0x0 Value: 26 { 5B 07 00 00 01 1A 00 }
0x4525C: 			End  { 29 02 }
0x4525E: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x76D, VarStoreId: 0xF101, VarOffset: 0x208, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 2A 0D 29 0D 6D 07 01 F1 08 02 10 10 00 0C 00 }
0x4526F: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x45276: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4527D: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x45284: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4528B: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x45292: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45299: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x452A0: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x452A7: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x452AE: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x452B5: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x452BC: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x452C3: 			End  { 29 02 }
0x452C5: 		End  { 29 02 }
0x452C7: 		SuppressIf  { 0A 82 }
0x452C9: 			EqIdValList QuestionId: 0x76A, Values: [0, 1] { 14 0A 6A 07 02 00 00 00 01 00 }
0x452D3: 			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0 { 02 87 84 0B 00 00 00 }
0x452DA: 			End  { 29 02 }
0x452DC: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x76E, VarStoreId: 0xF101, VarOffset: 0x1F2, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 9C 0B 98 0B 6E 07 01 F1 F2 01 10 21 00 00 7F 00 01 00 }
0x452F0: 				Default DefaultId: 0x0 Value: 12 { 5B 07 00 00 01 0C 00 }
0x452F7: 			End  { 29 02 }
0x452F9: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x76F, VarStoreId: 0xF101, VarOffset: 0x209, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 2B 0D 29 0D 6F 07 01 F1 09 02 10 10 00 0C 00 }
0x4530A: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x45311: 				OneOfOption Option: "VCM" Value: 1, Default { 09 07 73 0D 10 00 01 }
0x45318: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4531F: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x45326: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4532D: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45334: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x4533B: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x45342: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45349: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x45350: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x45357: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4535E: 			End  { 29 02 }
0x45360: 		End  { 29 02 }
0x45362: 		SuppressIf  { 0A 82 }
0x45364: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2] { 14 0C 6A 07 03 00 00 00 01 00 02 00 }
0x45370: 			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0 { 02 87 85 0B 00 00 00 }
0x45377: 			End  { 29 02 }
0x45379: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x770, VarStoreId: 0xF101, VarOffset: 0x1F4, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 9D 0B 98 0B 70 07 01 F1 F4 01 10 21 00 00 7F 00 01 00 }
0x4538D: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x45394: 			End  { 29 02 }
0x45396: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x771, VarStoreId: 0xF101, VarOffset: 0x20A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 2C 0D 29 0D 71 07 01 F1 0A 02 10 10 00 0C 00 }
0x453A7: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x453AE: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x453B5: 				OneOfOption Option: "EEPROM" Value: 2, Default { 09 07 74 0D 10 00 02 }
0x453BC: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x453C3: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x453CA: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x453D1: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x453D8: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x453DF: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x453E6: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x453ED: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x453F4: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x453FB: 			End  { 29 02 }
0x453FD: 		End  { 29 02 }
0x453FF: 		SuppressIf  { 0A 82 }
0x45401: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3] { 14 0E 6A 07 04 00 00 00 01 00 02 00 03 00 }
0x4540F: 			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0 { 02 87 86 0B 00 00 00 }
0x45416: 			End  { 29 02 }
0x45418: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x772, VarStoreId: 0xF101, VarOffset: 0x1F6, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 9E 0B 98 0B 72 07 01 F1 F6 01 10 21 00 00 7F 00 01 00 }
0x4542C: 				Default DefaultId: 0x0 Value: 81 { 5B 07 00 00 01 51 00 }
0x45433: 			End  { 29 02 }
0x45435: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x773, VarStoreId: 0xF101, VarOffset: 0x20B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 2D 0D 29 0D 73 07 01 F1 0B 02 10 10 00 0C 00 }
0x45446: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4544D: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x45454: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4545B: 				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default { 09 07 75 0D 10 00 03 }
0x45462: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x45469: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45470: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x45477: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4547E: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45485: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4548C: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x45493: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4549A: 			End  { 29 02 }
0x4549C: 		End  { 29 02 }
0x4549E: 		SuppressIf  { 0A 82 }
0x454A0: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4] { 14 10 6A 07 05 00 00 00 01 00 02 00 03 00 04 00 }
0x454B0: 			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0 { 02 87 87 0B 00 00 00 }
0x454B7: 			End  { 29 02 }
0x454B9: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x774, VarStoreId: 0xF101, VarOffset: 0x1F8, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 9F 0B 98 0B 74 07 01 F1 F8 01 10 21 00 00 7F 00 01 00 }
0x454CD: 				Default DefaultId: 0x0 Value: 82 { 5B 07 00 00 01 52 00 }
0x454D4: 			End  { 29 02 }
0x454D6: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x775, VarStoreId: 0xF101, VarOffset: 0x20C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 2E 0D 29 0D 75 07 01 F1 0C 02 10 10 00 0C 00 }
0x454E7: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x454EE: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x454F5: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x454FC: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x45503: 				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default { 09 07 76 0D 10 00 04 }
0x4550A: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45511: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x45518: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4551F: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45526: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4552D: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x45534: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4553B: 			End  { 29 02 }
0x4553D: 		End  { 29 02 }
0x4553F: 		SuppressIf  { 0A 82 }
0x45541: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5] { 14 12 6A 07 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x45553: 			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0 { 02 87 88 0B 00 00 00 }
0x4555A: 			End  { 29 02 }
0x4555C: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x776, VarStoreId: 0xF101, VarOffset: 0x1FA, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A0 0B 98 0B 76 07 01 F1 FA 01 10 21 00 00 7F 00 01 00 }
0x45570: 				Default DefaultId: 0x0 Value: 83 { 5B 07 00 00 01 53 00 }
0x45577: 			End  { 29 02 }
0x45579: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x777, VarStoreId: 0xF101, VarOffset: 0x20D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 2F 0D 29 0D 77 07 01 F1 0D 02 10 10 00 0C 00 }
0x4558A: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x45591: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x45598: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4559F: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x455A6: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x455AD: 				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default { 09 07 77 0D 10 00 05 }
0x455B4: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x455BB: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x455C2: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x455C9: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x455D0: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x455D7: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x455DE: 			End  { 29 02 }
0x455E0: 		End  { 29 02 }
0x455E2: 		SuppressIf  { 0A 82 }
0x455E4: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5, 6] { 14 14 6A 07 07 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 }
0x455F8: 			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0 { 02 87 89 0B 00 00 00 }
0x455FF: 			End  { 29 02 }
0x45601: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x778, VarStoreId: 0xF101, VarOffset: 0x1FC, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A1 0B 98 0B 78 07 01 F1 FC 01 10 21 00 00 7F 00 01 00 }
0x45615: 				Default DefaultId: 0x0 Value: 84 { 5B 07 00 00 01 54 00 }
0x4561C: 			End  { 29 02 }
0x4561E: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x779, VarStoreId: 0xF101, VarOffset: 0x20E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 30 0D 29 0D 79 07 01 F1 0E 02 10 10 00 0C 00 }
0x4562F: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x45636: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4563D: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x45644: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4564B: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x45652: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45659: 				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default { 09 07 78 0D 10 00 06 }
0x45660: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x45667: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4566E: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x45675: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x4567C: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x45683: 			End  { 29 02 }
0x45685: 		End  { 29 02 }
0x45687: 		SuppressIf  { 0A 82 }
0x45689: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5, 6, 7] { 14 16 6A 07 08 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 }
0x4569F: 			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0 { 02 87 8A 0B 00 00 00 }
0x456A6: 			End  { 29 02 }
0x456A8: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x77A, VarStoreId: 0xF101, VarOffset: 0x1FE, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A2 0B 98 0B 7A 07 01 F1 FE 01 10 21 00 00 7F 00 01 00 }
0x456BC: 				Default DefaultId: 0x0 Value: 85 { 5B 07 00 00 01 55 00 }
0x456C3: 			End  { 29 02 }
0x456C5: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x77B, VarStoreId: 0xF101, VarOffset: 0x20F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 31 0D 29 0D 7B 07 01 F1 0F 02 10 10 00 0C 00 }
0x456D6: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x456DD: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x456E4: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x456EB: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x456F2: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x456F9: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45700: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x45707: 				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default { 09 07 79 0D 10 00 07 }
0x4570E: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45715: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4571C: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x45723: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4572A: 			End  { 29 02 }
0x4572C: 		End  { 29 02 }
0x4572E: 		SuppressIf  { 0A 82 }
0x45730: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8] { 14 18 6A 07 09 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x45748: 			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0 { 02 87 8B 0B 00 00 00 }
0x4574F: 			End  { 29 02 }
0x45751: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x77C, VarStoreId: 0xF101, VarOffset: 0x200, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A3 0B 98 0B 7C 07 01 F1 00 02 10 21 00 00 7F 00 01 00 }
0x45765: 				Default DefaultId: 0x0 Value: 86 { 5B 07 00 00 01 56 00 }
0x4576C: 			End  { 29 02 }
0x4576E: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x77D, VarStoreId: 0xF101, VarOffset: 0x210, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 32 0D 29 0D 7D 07 01 F1 10 02 10 10 00 0C 00 }
0x4577F: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x45786: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4578D: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x45794: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4579B: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x457A2: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x457A9: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x457B0: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x457B7: 				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default { 09 07 7A 0D 10 00 08 }
0x457BE: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x457C5: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x457CC: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x457D3: 			End  { 29 02 }
0x457D5: 		End  { 29 02 }
0x457D7: 		SuppressIf  { 0A 82 }
0x457D9: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9] { 14 1A 6A 07 0A 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 }
0x457F3: 			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0 { 02 87 8C 0B 00 00 00 }
0x457FA: 			End  { 29 02 }
0x457FC: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x77E, VarStoreId: 0xF101, VarOffset: 0x202, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A4 0B 98 0B 7E 07 01 F1 02 02 10 21 00 00 7F 00 01 00 }
0x45810: 				Default DefaultId: 0x0 Value: 87 { 5B 07 00 00 01 57 00 }
0x45817: 			End  { 29 02 }
0x45819: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x77F, VarStoreId: 0xF101, VarOffset: 0x211, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 33 0D 29 0D 7F 07 01 F1 11 02 10 10 00 0C 00 }
0x4582A: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x45831: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x45838: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4583F: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x45846: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4584D: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45854: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x4585B: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x45862: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45869: 				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default { 09 07 7B 0D 10 00 09 }
0x45870: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x45877: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4587E: 			End  { 29 02 }
0x45880: 		End  { 29 02 }
0x45882: 		SuppressIf  { 0A 82 }
0x45884: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10] { 14 1C 6A 07 0B 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 }
0x458A0: 			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0 { 02 87 8D 0B 00 00 00 }
0x458A7: 			End  { 29 02 }
0x458A9: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x780, VarStoreId: 0xF101, VarOffset: 0x204, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A5 0B 98 0B 80 07 01 F1 04 02 10 21 00 00 7F 00 01 00 }
0x458BD: 				Default DefaultId: 0x0 Value: 88 { 5B 07 00 00 01 58 00 }
0x458C4: 			End  { 29 02 }
0x458C6: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x781, VarStoreId: 0xF101, VarOffset: 0x212, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 34 0D 29 0D 81 07 01 F1 12 02 10 10 00 0C 00 }
0x458D7: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x458DE: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x458E5: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x458EC: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x458F3: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x458FA: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45901: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x45908: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4590F: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45916: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4591D: 				OneOfOption Option: "IO Expander" Value: 10, Default { 09 07 7C 0D 10 00 0A }
0x45924: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4592B: 			End  { 29 02 }
0x4592D: 		End  { 29 02 }
0x4592F: 		SuppressIf  { 0A 82 }
0x45931: 			EqIdValList QuestionId: 0x76A, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11] { 14 1E 6A 07 0C 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 0B 00 }
0x4594F: 			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0 { 02 87 8E 0B 00 00 00 }
0x45956: 			End  { 29 02 }
0x45958: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x782, VarStoreId: 0xF101, VarOffset: 0x206, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A6 0B 98 0B 82 07 01 F1 06 02 10 21 00 00 7F 00 01 00 }
0x4596C: 				Default DefaultId: 0x0 Value: 89 { 5B 07 00 00 01 59 00 }
0x45973: 			End  { 29 02 }
0x45975: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x783, VarStoreId: 0xF101, VarOffset: 0x213, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 35 0D 29 0D 83 07 01 F1 13 02 10 10 00 0C 00 }
0x45986: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x4598D: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x45994: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4599B: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x459A2: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x459A9: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x459B0: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x459B7: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x459BE: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x459C5: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x459CC: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x459D3: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x459DA: 			End  { 29 02 }
0x459DC: 		End  { 29 02 }
0x459DE: 		OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x784, VarStoreId: 0xF101, VarOffset: 0x22B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A3 0C A2 0C 84 07 01 F1 2B 02 10 10 00 02 00 }
0x459EF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 A4 0C 30 00 00 }
0x459F6: 			OneOfOption Option: "External" Value: 1 { 09 07 A5 0C 00 00 01 }
0x459FD: 			OneOfOption Option: "Internal PMIC" Value: 2 { 09 07 A6 0C 00 00 02 }
0x45A04: 		End  { 29 02 }
0x45A06: 		SuppressIf  { 0A 82 }
0x45A08: 			EqIdVal QuestionId: 0x784, Value: 0x1 { 12 86 84 07 01 00 }
0x45A0E: 				Not  { 17 02 }
0x45A10: 			End  { 29 02 }
0x45A12: 			OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x785, VarStoreId: 0xF101, VarOffset: 0xAF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 A8 0C A7 0C 85 07 01 F1 F6 0A 10 10 00 05 00 }
0x45A23: 				OneOfOption Option: "Flash1" Value: 0, Default, MfgDefault { 09 07 9A 0D 30 00 00 }
0x45A2A: 				OneOfOption Option: "Flash2" Value: 1 { 09 07 9B 0D 00 00 01 }
0x45A31: 				OneOfOption Option: "Flash3" Value: 2 { 09 07 9C 0D 00 00 02 }
0x45A38: 				OneOfOption Option: "Flash4" Value: 3 { 09 07 9D 0D 00 00 03 }
0x45A3F: 				OneOfOption Option: "Flash5" Value: 4 { 09 07 9E 0D 00 00 04 }
0x45A46: 				OneOfOption Option: "Flash6" Value: 5 { 09 07 9F 0D 00 00 05 }
0x45A4D: 			End  { 29 02 }
0x45A4F: 		End  { 29 02 }
0x45A51: 	End  { 29 02 }
0x45A53: 	Form FormId: 0x8E, Title: "Link1 options" { 01 86 8E 00 60 0B }
0x45A59: 		Subtitle Prompt: "Camera2", Help: "", Flags: 0x0 { 02 87 4E 0B 00 00 00 }
0x45A60: 		End  { 29 02 }
0x45A62: 		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0x786, VarStoreId: 0xF101, VarOffset: 0x22C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 67 0B 65 0B 86 07 01 F1 2C 02 10 10 00 FF 00 }
0x45A73: 			OneOfOption Option: "IMX135" Value: 0 { 09 07 FF 0C 00 00 00 }
0x45A7A: 			OneOfOption Option: "OV5693" Value: 1 { 09 07 00 0D 00 00 01 }
0x45A81: 			OneOfOption Option: "IMX179" Value: 2 { 09 07 01 0D 00 00 02 }
0x45A88: 			OneOfOption Option: "OV8858" Value: 3 { 09 07 02 0D 00 00 03 }
0x45A8F: 			OneOfOption Option: "OV2740-IVCAM" Value: 4 { 09 07 03 0D 00 00 04 }
0x45A96: 			OneOfOption Option: "OV9728" Value: 5 { 09 07 04 0D 00 00 05 }
0x45A9D: 			OneOfOption Option: "IMX188" Value: 6 { 09 07 05 0D 00 00 06 }
0x45AA4: 			OneOfOption Option: "IMX208" Value: 7 { 09 07 06 0D 00 00 07 }
0x45AAB: 			OneOfOption Option: "OV5670" Value: 8 { 09 07 07 0D 00 00 08 }
0x45AB2: 			OneOfOption Option: "OV8865" Value: 9 { 09 07 08 0D 00 00 09 }
0x45AB9: 			OneOfOption Option: "HM2051" Value: 10 { 09 07 09 0D 00 00 0A }
0x45AC0: 			OneOfOption Option: "OV2742" Value: 11 { 09 07 0A 0D 00 00 0B }
0x45AC7: 			OneOfOption Option: "OV9234" Value: 12 { 09 07 0B 0D 00 00 0C }
0x45ACE: 			OneOfOption Option: "OV8856" Value: 13 { 09 07 0C 0D 00 00 0D }
0x45AD5: 			OneOfOption Option: "OV16860" Value: 14 { 09 07 0D 0D 00 00 0E }
0x45ADC: 			OneOfOption Option: "IMX362" Value: 15 { 09 07 0E 0D 00 00 0F }
0x45AE3: 			OneOfOption Option: "IMX488" Value: 16, Default { 09 07 0F 0D 10 00 10 }
0x45AEA: 			OneOfOption Option: "OVTI01AS" Value: 17 { 09 07 11 0D 00 00 11 }
0x45AF1: 			OneOfOption Option: "OVTI01A0" Value: 18 { 09 07 12 0D 00 00 12 }
0x45AF8: 			OneOfOption Option: "OVTI5678" Value: 19 { 09 07 13 0D 00 00 13 }
0x45AFF: 			OneOfOption Option: "OVTI9738" Value: 20 { 09 07 14 0D 00 00 14 }
0x45B06: 			OneOfOption Option: "HIMAX11B1" Value: 21 { 09 07 16 0D 00 00 15 }
0x45B0D: 			OneOfOption Option: "OVTID858" Value: 22 { 09 07 15 0D 00 00 16 }
0x45B14: 			OneOfOption Option: "User Custom" Value: 255 { 09 07 17 0D 00 00 FF }
0x45B1B: 		End  { 29 02 }
0x45B1D: 		SuppressIf  { 0A 82 }
0x45B1F: 			EqIdVal QuestionId: 0x786, Value: 0xFF { 12 86 86 07 FF 00 }
0x45B25: 				Not  { 17 02 }
0x45B27: 			End  { 29 02 }
0x45B29: 			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0x787, VarStoreId: 0xF101, VarStoreInfo: 0x22D, MinSize: 0x6, MaxSize: 0x14, Flags: 0x0 { 1C 90 A2 10 18 0D 87 07 01 F1 2D 02 00 06 14 00 }
0x45B39: 			End  { 29 02 }
0x45B3B: 		End  { 29 02 }
0x45B3D: 		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0x788, VarStoreId: 0xF101, VarOffset: 0xA93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 78 0B 76 0B 88 07 01 F1 93 0A 10 10 00 07 00 }
0x45B4E: 			OneOfOption Option: "4 4 2 2" Value: 0, Default { 09 07 7D 0B 10 00 00 }
0x45B55: 			OneOfOption Option: "4 4 3 1" Value: 2 { 09 07 7E 0B 00 00 02 }
0x45B5C: 			OneOfOption Option: "4 4 4 0" Value: 3 { 09 07 7F 0B 00 00 03 }
0x45B63: 			OneOfOption Option: "8 0 2 2" Value: 4 { 09 07 80 0B 00 00 04 }
0x45B6A: 			OneOfOption Option: "8 0 3 1" Value: 6 { 09 07 81 0B 00 00 06 }
0x45B71: 			OneOfOption Option: "8 0 4 0" Value: 7 { 09 07 82 0B 00 00 07 }
0x45B78: 		End  { 29 02 }
0x45B7A: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x789, VarStoreId: 0xF101, VarOffset: 0x29E, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 AB 0C A9 0C 89 07 01 F1 9E 02 10 10 10 50 00 }
0x45B8B: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x45B92: 			OneOfOption Option: "CRD-G" Value: 48 { 09 07 B4 0C 00 00 30 }
0x45B99: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x45BA0: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x45BA7: 			OneOfOption Option: "CRD-G2" Value: 80, Default { 09 07 B6 0C 10 00 50 }
0x45BAE: 		End  { 29 02 }
0x45BB0: 		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0x78A, VarStoreId: 0xF101, VarOffset: 0x2AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 80 0D 7E 0D 8A 07 01 F1 AB 02 10 10 00 FF 00 }
0x45BC1: 			OneOfOption Option: "No Control Logic" Value: 255 { 09 07 28 0D 00 00 FF }
0x45BC8: 			OneOfOption Option: "Control Logic 1" Value: 0, Default { 09 07 22 0D 10 00 00 }
0x45BCF: 			OneOfOption Option: "Control Logic 2" Value: 1 { 09 07 23 0D 00 00 01 }
0x45BD6: 			OneOfOption Option: "Control Logic 3" Value: 2 { 09 07 24 0D 00 00 02 }
0x45BDD: 			OneOfOption Option: "Control Logic 4" Value: 3 { 09 07 25 0D 00 00 03 }
0x45BE4: 			SuppressIf  { 0A 82 }
0x45BE6: 				EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x45BEC: 					Not  { 17 02 }
0x45BEE: 				End  { 29 02 }
0x45BF0: 				OneOfOption Option: "Control Logic 5" Value: 3 { 09 07 26 0D 00 00 03 }
0x45BF7: 			End  { 29 02 }
0x45BF9: 			SuppressIf  { 0A 82 }
0x45BFB: 				EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x45C01: 					Not  { 17 02 }
0x45C03: 				End  { 29 02 }
0x45C05: 				OneOfOption Option: "Control Logic 6" Value: 3 { 09 07 27 0D 00 00 03 }
0x45C0C: 			End  { 29 02 }
0x45C0E: 		End  { 29 02 }
0x45C10: 		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0x78B, VarStoreId: 0xF101, VarOffset: 0x255, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0 { 05 91 61 0C 5F 0C 8B 07 01 F1 55 02 10 10 61 69 00 }
0x45C21: 			OneOfOption Option: "Front" Value: 97, Default { 09 07 6C 0C 10 00 61 }
0x45C28: 			OneOfOption Option: "Back" Value: 105 { 09 07 6D 0C 00 00 69 }
0x45C2F: 		End  { 29 02 }
0x45C31: 		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0x78C, VarStoreId: 0xF101, VarOffset: 0x2AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 73 0C 71 0C 8C 07 01 F1 AC 02 10 10 00 03 00 }
0x45C42: 			OneOfOption Option: "Driver default" Value: 0 { 09 07 78 0C 00 00 00 }
0x45C49: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x45C50: 			OneOfOption Option: "Enabled" Value: 3, Default { 09 07 03 00 10 00 03 }
0x45C57: 		End  { 29 02 }
0x45C59: 		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0x78D, VarStoreId: 0xF101, VarOffset: 0x2AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7B 0C 79 0C 8D 07 01 F1 AD 02 10 10 00 05 00 }
0x45C6A: 			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault { 09 07 80 0C 30 00 00 }
0x45C71: 			OneOfOption Option: "ILEDA, 16mA" Value: 1 { 09 07 81 0C 00 00 01 }
0x45C78: 			OneOfOption Option: "ILEDB, 2mA" Value: 2 { 09 07 82 0C 00 00 02 }
0x45C7F: 			OneOfOption Option: "ILEDB, 4mA" Value: 3 { 09 07 83 0C 00 00 03 }
0x45C86: 			OneOfOption Option: "ILEDB, 8mA" Value: 4 { 09 07 84 0C 00 00 04 }
0x45C8D: 			OneOfOption Option: "ILEDB, 16mA" Value: 5 { 09 07 85 0C 00 00 05 }
0x45C94: 		End  { 29 02 }
0x45C96: 		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0x78E, VarStoreId: 0xF101, VarOffset: 0x2AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 88 0C 86 0C 8E 07 01 F1 AE 02 10 10 00 06 00 }
0x45CA7: 			OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 8D 0C 30 00 00 }
0x45CAE: 			OneOfOption Option: "90" Value: 2 { 09 07 8E 0C 00 00 02 }
0x45CB5: 			OneOfOption Option: "180" Value: 4 { 09 07 8F 0C 00 00 04 }
0x45CBC: 			OneOfOption Option: "270" Value: 6 { 09 07 90 0C 00 00 06 }
0x45CC3: 		End  { 29 02 }
0x45CC5: 		SuppressIf  { 0A 82 }
0x45CC7: 			EqIdVal QuestionId: 0x789, Value: 0x50 { 12 86 89 07 50 00 }
0x45CCD: 				Not  { 17 02 }
0x45CCF: 			End  { 29 02 }
0x45CD1: 			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0x78F, VarStoreId: 0xF101, VarOffset: 0x2AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 0C 91 0C 8F 07 01 F1 AF 02 10 10 00 01 00 }
0x45CE2: 				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault { 09 07 97 0C 30 00 00 }
0x45CE9: 				OneOfOption Option: "Position 2" Value: 1 { 09 07 98 0C 00 00 01 }
0x45CF0: 			End  { 29 02 }
0x45CF2: 		End  { 29 02 }
0x45CF4: 		SuppressIf  { 0A 82 }
0x45CF6: 			EqIdVal QuestionId: 0x78F, Value: 0x1 { 12 86 8F 07 01 00 }
0x45CFC: 				Not  { 17 02 }
0x45CFE: 			End  { 29 02 }
0x45D00: 			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0x790, VarStoreId: 0xF101, VarOffset: 0x2B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 0C 99 0C 90 07 01 F1 B0 02 10 10 00 01 00 }
0x45D11: 				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault { 09 07 A0 0C 30 00 00 }
0x45D18: 				OneOfOption Option: "2 voltage rail" Value: 1 { 09 07 A1 0C 00 00 01 }
0x45D1F: 			End  { 29 02 }
0x45D21: 		End  { 29 02 }
0x45D23: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x791, VarStoreId: 0xF101, VarStoreInfo: 0x256, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 7C 10 66 0C 91 07 01 F1 56 02 00 01 0F 00 }
0x45D33: 			Default DefaultId: 0x0 String: "56B6" { 5B 07 00 00 07 69 0C }
0x45D3A: 		End  { 29 02 }
0x45D3C: 		Numeric Prompt: "MIPI port", Help: "LinkUsed", QuestionFlags: 0x10, QuestionId: 0x792, VarStoreId: 0xF101, VarOffset: 0x29D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 B9 0C B7 0C 92 07 01 F1 9D 02 10 10 00 0A 01 }
0x45D4D: 			Default DefaultId: 0x0 Value: 5 { 5B 06 00 00 00 05 }
0x45D53: 		End  { 29 02 }
0x45D55: 		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0x793, VarStoreId: 0xF101, VarOffset: 0x29F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 C0 0C BE 0C 93 07 01 F1 9F 02 10 10 01 04 00 }
0x45D66: 			OneOfOption Option: "x1" Value: 1, Default { 09 07 F3 0C 10 00 01 }
0x45D6D: 			OneOfOption Option: "x2" Value: 2 { 09 07 F4 0C 00 00 02 }
0x45D74: 			OneOfOption Option: "x3" Value: 3 { 09 07 F5 0C 00 00 03 }
0x45D7B: 			OneOfOption Option: "x4" Value: 4 { 09 07 F6 0C 00 00 04 }
0x45D82: 		End  { 29 02 }
0x45D84: 		OneOf Prompt: "PortSpeed", Help: "PortSpeed: 0:Sensor Default, 1:<416Mbps, 2:<1.5Gbps, 3:<2Gbps, 4:<2.5Gbps, 5:<4Gbps, 6:>4Gbps", QuestionFlags: 0x10, QuestionId: 0x794, VarStoreId: 0xF101, VarOffset: 0x2A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 98 10 C6 0C 94 07 01 F1 A0 02 10 10 00 06 00 }
0x45D95: 			OneOfOption Option: "0" Value: 0 { 09 07 F8 0C 00 00 00 }
0x45D9C: 			OneOfOption Option: "1" Value: 1 { 09 07 F9 0C 00 00 01 }
0x45DA3: 			OneOfOption Option: "2" Value: 2, Default { 09 07 FA 0C 10 00 02 }
0x45DAA: 			OneOfOption Option: "3" Value: 3 { 09 07 FB 0C 00 00 03 }
0x45DB1: 			OneOfOption Option: "4" Value: 4 { 09 07 FC 0C 00 00 04 }
0x45DB8: 			OneOfOption Option: "5" Value: 5 { 09 07 FD 0C 00 00 05 }
0x45DBF: 			OneOfOption Option: "6" Value: 6 { 09 07 FE 0C 00 00 06 }
0x45DC6: 		End  { 29 02 }
0x45DC8: 		Numeric Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0x795, VarStoreId: 0xF101, VarOffset: 0x2A7, Flags: 0x12, Size: 32, Min: 0x5B8D80, Max: 0x19BFCC0, Step: 0x186A0 { 07 9A 9D 10 C7 0C 95 07 01 F1 A7 02 10 12 80 8D 5B 00 C0 FC 9B 01 A0 86 01 00 }
0x45DE2: 			Default DefaultId: 0x0 Value: 19200000 { 5B 09 00 00 02 00 F8 24 01 }
0x45DEB: 		End  { 29 02 }
0x45DED: 		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type
0x00: ROM_NONE
0x01: ROM_OTP
0x02: ROM_EEPROM_16K_64
0x03: ROM_EEPROM_16K_16
0x04: ROM_OTP_ACPI_ACPI
0x05: ROM_ACPI
0x06: ROM_EEPROM_BRCA016GWZ
0x07: ROM_EEPROM_24AA32
0x08: ROM_EEPROM_CAT24C08
0x09: ROM_M24C64
0x0A: ROM_DW9806B
0x10: ROM_EEPROM_CAT24C16
0x11: ROM_EEPROM_CAT24C64
0x12: ROM_EEPROM_24AA16", QuestionFlags: 0x10, QuestionId: 0x796, VarStoreId: 0xF101, VarOffset: 0x2A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CB 0C C9 0C 96 07 01 F1 A1 02 10 10 00 12 00 }
0x45DFE: 			OneOfOption Option: "ROM_NONE" Value: 0, Default { 09 07 D7 0C 10 00 00 }
0x45E05: 			OneOfOption Option: "ROM_OTP" Value: 1 { 09 07 D8 0C 00 00 01 }
0x45E0C: 			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2 { 09 07 D9 0C 00 00 02 }
0x45E13: 			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3 { 09 07 DA 0C 00 00 03 }
0x45E1A: 			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4 { 09 07 DB 0C 00 00 04 }
0x45E21: 			OneOfOption Option: "ROM_ACPI" Value: 5 { 09 07 DC 0C 00 00 05 }
0x45E28: 			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6 { 09 07 DD 0C 00 00 06 }
0x45E2F: 			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7 { 09 07 DE 0C 00 00 07 }
0x45E36: 			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8 { 09 07 DF 0C 00 00 08 }
0x45E3D: 			OneOfOption Option: "ROM_EEPROM_M24C64" Value: 9 { 09 07 E0 0C 00 00 09 }
0x45E44: 			OneOfOption Option: "ROM_EEPROM_DW9806B" Value: 10 { 09 07 E1 0C 00 00 0A }
0x45E4B: 			OneOfOption Option: "ROM_EEPROM_CAT24C16" Value: 16 { 09 07 E2 0C 00 00 10 }
0x45E52: 			OneOfOption Option: "ROM_EEPROM_CAT24C64" Value: 17 { 09 07 E3 0C 00 00 11 }
0x45E59: 			OneOfOption Option: "ROM_EEPROM_24AA16" Value: 18 { 09 07 E4 0C 00 00 12 }
0x45E60: 		End  { 29 02 }
0x45E62: 		OneOf Prompt: "VCM Type", Help: "VCM Type
0x00: VCM_NONE
0x01: VCM_AD5823
0x02: VCM_DW9714
0x03: VCM_AD5816
0x04: VCM_DW9719
0x05: VCM_DW9718
0x06: VCM_DW9806B
0x07: VCM_WV517S
0x08: VCM_LC898122XA
0x09: VCM_LC898212AXB
0x0F: VCM_AK7371
0x10: VCM_BU64297GWZ", QuestionFlags: 0x10, QuestionId: 0x797, VarStoreId: 0xF101, VarOffset: 0x2A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0 { 05 91 D2 0C D0 0C 97 07 01 F1 A2 02 10 10 00 10 00 }
0x45E73: 			OneOfOption Option: "VCM_NONE" Value: 0, Default { 09 07 E5 0C 10 00 00 }
0x45E7A: 			OneOfOption Option: "VCM_AD5823" Value: 1 { 09 07 E6 0C 00 00 01 }
0x45E81: 			OneOfOption Option: "VCM_DW9714" Value: 2 { 09 07 E7 0C 00 00 02 }
0x45E88: 			OneOfOption Option: "VCM_AD5816" Value: 3 { 09 07 E8 0C 00 00 03 }
0x45E8F: 			OneOfOption Option: "VCM_DW9719" Value: 4 { 09 07 EA 0C 00 00 04 }
0x45E96: 			OneOfOption Option: "VCM_DW9718" Value: 5 { 09 07 E9 0C 00 00 05 }
0x45E9D: 			OneOfOption Option: "VCM_DW9806B" Value: 6 { 09 07 EB 0C 00 00 06 }
0x45EA4: 			OneOfOption Option: "VCM_WV517S" Value: 7 { 09 07 EC 0C 00 00 07 }
0x45EAB: 			OneOfOption Option: "VCM_LC898122XA" Value: 8 { 09 07 ED 0C 00 00 08 }
0x45EB2: 			OneOfOption Option: "VCM_LC898212AXB" Value: 9 { 09 07 EE 0C 00 00 09 }
0x45EB9: 			OneOfOption Option: "VCM_RESERVED1" Value: 10 { 09 07 EF 0C 00 00 0A }
0x45EC0: 			OneOfOption Option: "VCM_RESERVED2" Value: 11 { 09 07 F0 0C 00 00 0B }
0x45EC7: 			OneOfOption Option: "VCM_AK7371" Value: 15 { 09 07 F1 0C 00 00 0F }
0x45ECE: 			OneOfOption Option: "VCM_BU64297GWZ" Value: 16 { 09 07 F2 0C 00 00 10 }
0x45ED5: 		End  { 29 02 }
0x45ED7: 		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0x798, VarStoreId: 0xF101, VarOffset: 0x276, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1 { 07 91 6E 0B 6C 0B 98 07 01 F1 76 02 10 10 00 0C 01 }
0x45EE8: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x45EEE: 		End  { 29 02 }
0x45EF0: 		SuppressIf  { 0A 82 }
0x45EF2: 			EqIdVal QuestionId: 0x798, Value: 0x0 { 12 06 98 07 00 00 }
0x45EF8: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x799, VarStoreId: 0xF101, VarOffset: 0x277, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 91 0B 8F 0B 99 07 01 F1 77 02 10 10 00 05 00 }
0x45F09: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x45F10: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x45F17: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x45F1E: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x45F25: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x45F2C: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x45F33: 			End  { 29 02 }
0x45F35: 			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0 { 02 87 83 0B 00 00 00 }
0x45F3C: 			End  { 29 02 }
0x45F3E: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x79A, VarStoreId: 0xF101, VarOffset: 0x278, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A7 0B 98 0B 9A 07 01 F1 78 02 10 21 00 00 7F 00 01 00 }
0x45F52: 				Default DefaultId: 0x0 Value: 55 { 5B 07 00 00 01 37 00 }
0x45F59: 			End  { 29 02 }
0x45F5B: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x79B, VarStoreId: 0xF101, VarOffset: 0x290, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 36 0D 29 0D 9B 07 01 F1 90 02 10 10 00 0C 00 }
0x45F6C: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x45F73: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x45F7A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x45F81: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x45F88: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x45F8F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x45F96: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x45F9D: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x45FA4: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x45FAB: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x45FB2: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x45FB9: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x45FC0: 			End  { 29 02 }
0x45FC2: 		End  { 29 02 }
0x45FC4: 		SuppressIf  { 0A 82 }
0x45FC6: 			EqIdValList QuestionId: 0x798, Values: [0, 1] { 14 0A 98 07 02 00 00 00 01 00 }
0x45FD0: 			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0 { 02 87 84 0B 00 00 00 }
0x45FD7: 			End  { 29 02 }
0x45FD9: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x79C, VarStoreId: 0xF101, VarOffset: 0x27A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A8 0B 98 0B 9C 07 01 F1 7A 02 10 21 00 00 7F 00 01 00 }
0x45FED: 				Default DefaultId: 0x0 Value: 12 { 5B 07 00 00 01 0C 00 }
0x45FF4: 			End  { 29 02 }
0x45FF6: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x79D, VarStoreId: 0xF101, VarOffset: 0x291, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 37 0D 29 0D 9D 07 01 F1 91 02 10 10 00 0C 00 }
0x46007: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4600E: 				OneOfOption Option: "VCM" Value: 1, Default { 09 07 73 0D 10 00 01 }
0x46015: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4601C: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46023: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4602A: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46031: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46038: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4603F: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46046: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4604D: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46054: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4605B: 			End  { 29 02 }
0x4605D: 		End  { 29 02 }
0x4605F: 		SuppressIf  { 0A 82 }
0x46061: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2] { 14 0C 98 07 03 00 00 00 01 00 02 00 }
0x4606D: 			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0 { 02 87 85 0B 00 00 00 }
0x46074: 			End  { 29 02 }
0x46076: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x79E, VarStoreId: 0xF101, VarOffset: 0x27C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 A9 0B 98 0B 9E 07 01 F1 7C 02 10 21 00 00 7F 00 01 00 }
0x4608A: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x46091: 			End  { 29 02 }
0x46093: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x79F, VarStoreId: 0xF101, VarOffset: 0x292, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 38 0D 29 0D 9F 07 01 F1 92 02 10 10 00 0C 00 }
0x460A4: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x460AB: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x460B2: 				OneOfOption Option: "EEPROM" Value: 2, Default { 09 07 74 0D 10 00 02 }
0x460B9: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x460C0: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x460C7: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x460CE: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x460D5: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x460DC: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x460E3: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x460EA: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x460F1: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x460F8: 			End  { 29 02 }
0x460FA: 		End  { 29 02 }
0x460FC: 		SuppressIf  { 0A 82 }
0x460FE: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3] { 14 0E 98 07 04 00 00 00 01 00 02 00 03 00 }
0x4610C: 			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0 { 02 87 86 0B 00 00 00 }
0x46113: 			End  { 29 02 }
0x46115: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7A0, VarStoreId: 0xF101, VarOffset: 0x27E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 AA 0B 98 0B A0 07 01 F1 7E 02 10 21 00 00 7F 00 01 00 }
0x46129: 				Default DefaultId: 0x0 Value: 81 { 5B 07 00 00 01 51 00 }
0x46130: 			End  { 29 02 }
0x46132: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7A1, VarStoreId: 0xF101, VarOffset: 0x293, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 39 0D 29 0D A1 07 01 F1 93 02 10 10 00 0C 00 }
0x46143: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4614A: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46151: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46158: 				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default { 09 07 75 0D 10 00 03 }
0x4615F: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x46166: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4616D: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46174: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4617B: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46182: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46189: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46190: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46197: 			End  { 29 02 }
0x46199: 		End  { 29 02 }
0x4619B: 		SuppressIf  { 0A 82 }
0x4619D: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4] { 14 10 98 07 05 00 00 00 01 00 02 00 03 00 04 00 }
0x461AD: 			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0 { 02 87 87 0B 00 00 00 }
0x461B4: 			End  { 29 02 }
0x461B6: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7A2, VarStoreId: 0xF101, VarOffset: 0x280, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 AB 0B 98 0B A2 07 01 F1 80 02 10 21 00 00 7F 00 01 00 }
0x461CA: 				Default DefaultId: 0x0 Value: 82 { 5B 07 00 00 01 52 00 }
0x461D1: 			End  { 29 02 }
0x461D3: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7A3, VarStoreId: 0xF101, VarOffset: 0x294, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 3A 0D 29 0D A3 07 01 F1 94 02 10 10 00 0C 00 }
0x461E4: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x461EB: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x461F2: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x461F9: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46200: 				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default { 09 07 76 0D 10 00 04 }
0x46207: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4620E: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46215: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4621C: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46223: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4622A: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46231: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46238: 			End  { 29 02 }
0x4623A: 		End  { 29 02 }
0x4623C: 		SuppressIf  { 0A 82 }
0x4623E: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5] { 14 12 98 07 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x46250: 			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0 { 02 87 88 0B 00 00 00 }
0x46257: 			End  { 29 02 }
0x46259: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7A4, VarStoreId: 0xF101, VarOffset: 0x282, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 AC 0B 98 0B A4 07 01 F1 82 02 10 21 00 00 7F 00 01 00 }
0x4626D: 				Default DefaultId: 0x0 Value: 83 { 5B 07 00 00 01 53 00 }
0x46274: 			End  { 29 02 }
0x46276: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7A5, VarStoreId: 0xF101, VarOffset: 0x295, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 3B 0D 29 0D A5 07 01 F1 95 02 10 10 00 0C 00 }
0x46287: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4628E: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46295: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4629C: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x462A3: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x462AA: 				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default { 09 07 77 0D 10 00 05 }
0x462B1: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x462B8: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x462BF: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x462C6: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x462CD: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x462D4: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x462DB: 			End  { 29 02 }
0x462DD: 		End  { 29 02 }
0x462DF: 		SuppressIf  { 0A 82 }
0x462E1: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5, 6] { 14 14 98 07 07 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 }
0x462F5: 			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0 { 02 87 89 0B 00 00 00 }
0x462FC: 			End  { 29 02 }
0x462FE: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7A6, VarStoreId: 0xF101, VarOffset: 0x284, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 AD 0B 98 0B A6 07 01 F1 84 02 10 21 00 00 7F 00 01 00 }
0x46312: 				Default DefaultId: 0x0 Value: 84 { 5B 07 00 00 01 54 00 }
0x46319: 			End  { 29 02 }
0x4631B: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7A7, VarStoreId: 0xF101, VarOffset: 0x296, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 3C 0D 29 0D A7 07 01 F1 96 02 10 10 00 0C 00 }
0x4632C: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46333: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4633A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46341: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46348: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4634F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46356: 				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default { 09 07 78 0D 10 00 06 }
0x4635D: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46364: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4636B: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46372: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46379: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46380: 			End  { 29 02 }
0x46382: 		End  { 29 02 }
0x46384: 		SuppressIf  { 0A 82 }
0x46386: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5, 6, 7] { 14 16 98 07 08 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 }
0x4639C: 			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0 { 02 87 8A 0B 00 00 00 }
0x463A3: 			End  { 29 02 }
0x463A5: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7A8, VarStoreId: 0xF101, VarOffset: 0x286, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 AE 0B 98 0B A8 07 01 F1 86 02 10 21 00 00 7F 00 01 00 }
0x463B9: 				Default DefaultId: 0x0 Value: 85 { 5B 07 00 00 01 55 00 }
0x463C0: 			End  { 29 02 }
0x463C2: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7A9, VarStoreId: 0xF101, VarOffset: 0x297, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 3D 0D 29 0D A9 07 01 F1 97 02 10 10 00 0C 00 }
0x463D3: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x463DA: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x463E1: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x463E8: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x463EF: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x463F6: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x463FD: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46404: 				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default { 09 07 79 0D 10 00 07 }
0x4640B: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46412: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46419: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46420: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46427: 			End  { 29 02 }
0x46429: 		End  { 29 02 }
0x4642B: 		SuppressIf  { 0A 82 }
0x4642D: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8] { 14 18 98 07 09 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x46445: 			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0 { 02 87 8B 0B 00 00 00 }
0x4644C: 			End  { 29 02 }
0x4644E: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7AA, VarStoreId: 0xF101, VarOffset: 0x288, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 AF 0B 98 0B AA 07 01 F1 88 02 10 21 00 00 7F 00 01 00 }
0x46462: 				Default DefaultId: 0x0 Value: 86 { 5B 07 00 00 01 56 00 }
0x46469: 			End  { 29 02 }
0x4646B: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7AB, VarStoreId: 0xF101, VarOffset: 0x298, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 3E 0D 29 0D AB 07 01 F1 98 02 10 10 00 0C 00 }
0x4647C: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46483: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4648A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46491: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46498: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4649F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x464A6: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x464AD: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x464B4: 				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default { 09 07 7A 0D 10 00 08 }
0x464BB: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x464C2: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x464C9: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x464D0: 			End  { 29 02 }
0x464D2: 		End  { 29 02 }
0x464D4: 		SuppressIf  { 0A 82 }
0x464D6: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9] { 14 1A 98 07 0A 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 }
0x464F0: 			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0 { 02 87 8C 0B 00 00 00 }
0x464F7: 			End  { 29 02 }
0x464F9: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7AC, VarStoreId: 0xF101, VarOffset: 0x28A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B0 0B 98 0B AC 07 01 F1 8A 02 10 21 00 00 7F 00 01 00 }
0x4650D: 				Default DefaultId: 0x0 Value: 87 { 5B 07 00 00 01 57 00 }
0x46514: 			End  { 29 02 }
0x46516: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7AD, VarStoreId: 0xF101, VarOffset: 0x299, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 3F 0D 29 0D AD 07 01 F1 99 02 10 10 00 0C 00 }
0x46527: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4652E: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46535: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4653C: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46543: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4654A: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46551: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46558: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4655F: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46566: 				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default { 09 07 7B 0D 10 00 09 }
0x4656D: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46574: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4657B: 			End  { 29 02 }
0x4657D: 		End  { 29 02 }
0x4657F: 		SuppressIf  { 0A 82 }
0x46581: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10] { 14 1C 98 07 0B 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 }
0x4659D: 			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0 { 02 87 8D 0B 00 00 00 }
0x465A4: 			End  { 29 02 }
0x465A6: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7AE, VarStoreId: 0xF101, VarOffset: 0x28C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B1 0B 98 0B AE 07 01 F1 8C 02 10 21 00 00 7F 00 01 00 }
0x465BA: 				Default DefaultId: 0x0 Value: 88 { 5B 07 00 00 01 58 00 }
0x465C1: 			End  { 29 02 }
0x465C3: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7AF, VarStoreId: 0xF101, VarOffset: 0x29A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 40 0D 29 0D AF 07 01 F1 9A 02 10 10 00 0C 00 }
0x465D4: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x465DB: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x465E2: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x465E9: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x465F0: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x465F7: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x465FE: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46605: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4660C: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46613: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4661A: 				OneOfOption Option: "IO Expander" Value: 10, Default { 09 07 7C 0D 10 00 0A }
0x46621: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46628: 			End  { 29 02 }
0x4662A: 		End  { 29 02 }
0x4662C: 		SuppressIf  { 0A 82 }
0x4662E: 			EqIdValList QuestionId: 0x798, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11] { 14 1E 98 07 0C 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 0B 00 }
0x4664C: 			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0 { 02 87 8E 0B 00 00 00 }
0x46653: 			End  { 29 02 }
0x46655: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7B0, VarStoreId: 0xF101, VarOffset: 0x28E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B2 0B 98 0B B0 07 01 F1 8E 02 10 21 00 00 7F 00 01 00 }
0x46669: 				Default DefaultId: 0x0 Value: 89 { 5B 07 00 00 01 59 00 }
0x46670: 			End  { 29 02 }
0x46672: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7B1, VarStoreId: 0xF101, VarOffset: 0x29B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 41 0D 29 0D B1 07 01 F1 9B 02 10 10 00 0C 00 }
0x46683: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4668A: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46691: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46698: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4669F: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x466A6: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x466AD: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x466B4: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x466BB: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x466C2: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x466C9: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x466D0: 				OneOfOption Option: "Flash" Value: 12, Default { 09 07 7D 0D 10 00 0C }
0x466D7: 			End  { 29 02 }
0x466D9: 		End  { 29 02 }
0x466DB: 		OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x7B2, VarStoreId: 0xF101, VarOffset: 0x2B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8B 10 A2 0C B2 07 01 F1 B3 02 10 10 00 02 00 }
0x466EC: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 A4 0C 30 00 00 }
0x466F3: 			OneOfOption Option: "External" Value: 1 { 09 07 A5 0C 00 00 01 }
0x466FA: 			OneOfOption Option: "Internal PMIC" Value: 2 { 09 07 A6 0C 00 00 02 }
0x46701: 		End  { 29 02 }
0x46703: 		SuppressIf  { 0A 82 }
0x46705: 			EqIdVal QuestionId: 0x7B2, Value: 0x1 { 12 86 B2 07 01 00 }
0x4670B: 				Not  { 17 02 }
0x4670D: 			End  { 29 02 }
0x4670F: 			OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x7B3, VarStoreId: 0xF101, VarOffset: 0xAF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 8C 10 A7 0C B3 07 01 F1 F7 0A 10 10 00 05 00 }
0x46720: 				OneOfOption Option: "Flash1" Value: 0 { 09 07 9A 0D 00 00 00 }
0x46727: 				OneOfOption Option: "Flash2" Value: 1, Default, MfgDefault { 09 07 9B 0D 30 00 01 }
0x4672E: 				OneOfOption Option: "Flash3" Value: 2 { 09 07 9C 0D 00 00 02 }
0x46735: 				OneOfOption Option: "Flash4" Value: 3 { 09 07 9D 0D 00 00 03 }
0x4673C: 				OneOfOption Option: "Flash5" Value: 4 { 09 07 9E 0D 00 00 04 }
0x46743: 				OneOfOption Option: "Flash6" Value: 5 { 09 07 9F 0D 00 00 05 }
0x4674A: 			End  { 29 02 }
0x4674C: 		End  { 29 02 }
0x4674E: 	End  { 29 02 }
0x46750: 	Form FormId: 0x8F, Title: "Link2 options" { 01 86 8F 00 61 0B }
0x46756: 		Subtitle Prompt: "Camera3", Help: "", Flags: 0x0 { 02 87 4F 0B 00 00 00 }
0x4675D: 		End  { 29 02 }
0x4675F: 		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0x7B4, VarStoreId: 0xF101, VarOffset: 0x2B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 68 0B 65 0B B4 07 01 F1 B4 02 10 10 00 FF 00 }
0x46770: 			OneOfOption Option: "IMX135" Value: 0 { 09 07 FF 0C 00 00 00 }
0x46777: 			OneOfOption Option: "OV5693" Value: 1 { 09 07 00 0D 00 00 01 }
0x4677E: 			OneOfOption Option: "IMX179" Value: 2 { 09 07 01 0D 00 00 02 }
0x46785: 			OneOfOption Option: "OV8858" Value: 3 { 09 07 02 0D 00 00 03 }
0x4678C: 			OneOfOption Option: "OV2740-IVCAM" Value: 4 { 09 07 03 0D 00 00 04 }
0x46793: 			OneOfOption Option: "OV9728" Value: 5 { 09 07 04 0D 00 00 05 }
0x4679A: 			OneOfOption Option: "IMX188" Value: 6 { 09 07 05 0D 00 00 06 }
0x467A1: 			OneOfOption Option: "IMX208" Value: 7 { 09 07 06 0D 00 00 07 }
0x467A8: 			OneOfOption Option: "OV5670" Value: 8 { 09 07 07 0D 00 00 08 }
0x467AF: 			OneOfOption Option: "OV8865" Value: 9 { 09 07 08 0D 00 00 09 }
0x467B6: 			OneOfOption Option: "HM2051" Value: 10 { 09 07 09 0D 00 00 0A }
0x467BD: 			OneOfOption Option: "OV2742" Value: 11 { 09 07 0A 0D 00 00 0B }
0x467C4: 			OneOfOption Option: "OV9234" Value: 12 { 09 07 0B 0D 00 00 0C }
0x467CB: 			OneOfOption Option: "OV8856" Value: 13 { 09 07 0C 0D 00 00 0D }
0x467D2: 			OneOfOption Option: "OV16860" Value: 14 { 09 07 0D 0D 00 00 0E }
0x467D9: 			OneOfOption Option: "IMX362" Value: 15 { 09 07 0E 0D 00 00 0F }
0x467E0: 			OneOfOption Option: "IMX488" Value: 16 { 09 07 0F 0D 00 00 10 }
0x467E7: 			OneOfOption Option: "OVTI01AS" Value: 17, Default { 09 07 11 0D 10 00 11 }
0x467EE: 			OneOfOption Option: "OVTI01A0" Value: 18 { 09 07 12 0D 00 00 12 }
0x467F5: 			OneOfOption Option: "OVTI5678" Value: 19 { 09 07 13 0D 00 00 13 }
0x467FC: 			OneOfOption Option: "OVTI9738" Value: 20 { 09 07 14 0D 00 00 14 }
0x46803: 			OneOfOption Option: "HIMAX11B1" Value: 21 { 09 07 16 0D 00 00 15 }
0x4680A: 			OneOfOption Option: "OVTID858" Value: 22 { 09 07 15 0D 00 00 16 }
0x46811: 			OneOfOption Option: "User Custom" Value: 255 { 09 07 17 0D 00 00 FF }
0x46818: 		End  { 29 02 }
0x4681A: 		SuppressIf  { 0A 82 }
0x4681C: 			EqIdVal QuestionId: 0x7B4, Value: 0xFF { 12 86 B4 07 FF 00 }
0x46822: 				Not  { 17 02 }
0x46824: 			End  { 29 02 }
0x46826: 			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0x7B5, VarStoreId: 0xF101, VarStoreInfo: 0x2B5, MinSize: 0x6, MaxSize: 0x14, Flags: 0x0 { 1C 90 A3 10 18 0D B5 07 01 F1 B5 02 00 06 14 00 }
0x46836: 			End  { 29 02 }
0x46838: 		End  { 29 02 }
0x4683A: 		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0x7B6, VarStoreId: 0xF101, VarOffset: 0xA94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 79 0B 76 0B B6 07 01 F1 94 0A 10 10 00 07 00 }
0x4684B: 			OneOfOption Option: "4 4 2 2" Value: 0, Default { 09 07 7D 0B 10 00 00 }
0x46852: 			OneOfOption Option: "4 4 3 1" Value: 2 { 09 07 7E 0B 00 00 02 }
0x46859: 			OneOfOption Option: "4 4 4 0" Value: 3 { 09 07 7F 0B 00 00 03 }
0x46860: 			OneOfOption Option: "8 0 2 2" Value: 4 { 09 07 80 0B 00 00 04 }
0x46867: 			OneOfOption Option: "8 0 3 1" Value: 6 { 09 07 81 0B 00 00 06 }
0x4686E: 			OneOfOption Option: "8 0 4 0" Value: 7 { 09 07 82 0B 00 00 07 }
0x46875: 		End  { 29 02 }
0x46877: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x7B7, VarStoreId: 0xF101, VarOffset: 0x325, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 AC 0C A9 0C B7 07 01 F1 25 03 10 10 10 50 00 }
0x46888: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x4688F: 			OneOfOption Option: "CRD-D" Value: 32, Default { 09 07 B3 0C 10 00 20 }
0x46896: 			OneOfOption Option: "CRD-G" Value: 48 { 09 07 B4 0C 00 00 30 }
0x4689D: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x468A4: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x468AB: 		End  { 29 02 }
0x468AD: 		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0x7B8, VarStoreId: 0xF101, VarOffset: 0x333, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 81 0D 7E 0D B8 07 01 F1 33 03 10 10 00 FF 00 }
0x468BE: 			OneOfOption Option: "No Control Logic" Value: 255 { 09 07 28 0D 00 00 FF }
0x468C5: 			OneOfOption Option: "Control Logic 1" Value: 0 { 09 07 22 0D 00 00 00 }
0x468CC: 			OneOfOption Option: "Control Logic 2" Value: 1, Default { 09 07 23 0D 10 00 01 }
0x468D3: 			OneOfOption Option: "Control Logic 3" Value: 2 { 09 07 24 0D 00 00 02 }
0x468DA: 			OneOfOption Option: "Control Logic 4" Value: 3 { 09 07 25 0D 00 00 03 }
0x468E1: 			SuppressIf  { 0A 82 }
0x468E3: 				EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x468E9: 					Not  { 17 02 }
0x468EB: 				End  { 29 02 }
0x468ED: 				OneOfOption Option: "Control Logic 5" Value: 3 { 09 07 26 0D 00 00 03 }
0x468F4: 			End  { 29 02 }
0x468F6: 			SuppressIf  { 0A 82 }
0x468F8: 				EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x468FE: 					Not  { 17 02 }
0x46900: 				End  { 29 02 }
0x46902: 				OneOfOption Option: "Control Logic 6" Value: 3 { 09 07 27 0D 00 00 03 }
0x46909: 			End  { 29 02 }
0x4690B: 		End  { 29 02 }
0x4690D: 		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0x7B9, VarStoreId: 0xF101, VarOffset: 0x2DD, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0 { 05 91 62 0C 5F 0C B9 07 01 F1 DD 02 10 10 61 69 00 }
0x4691E: 			OneOfOption Option: "Front" Value: 97, Default { 09 07 6C 0C 10 00 61 }
0x46925: 			OneOfOption Option: "Back" Value: 105 { 09 07 6D 0C 00 00 69 }
0x4692C: 		End  { 29 02 }
0x4692E: 		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0x7BA, VarStoreId: 0xF101, VarOffset: 0x334, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 74 0C 71 0C BA 07 01 F1 34 03 10 10 00 03 00 }
0x4693F: 			OneOfOption Option: "Driver default" Value: 0 { 09 07 78 0C 00 00 00 }
0x46946: 			OneOfOption Option: "Disabled" Value: 2, Default { 09 07 04 00 10 00 02 }
0x4694D: 			OneOfOption Option: "Enabled" Value: 3 { 09 07 03 00 00 00 03 }
0x46954: 		End  { 29 02 }
0x46956: 		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0x7BB, VarStoreId: 0xF101, VarOffset: 0x335, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7C 0C 79 0C BB 07 01 F1 35 03 10 10 00 05 00 }
0x46967: 			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault { 09 07 80 0C 30 00 00 }
0x4696E: 			OneOfOption Option: "ILEDA, 16mA" Value: 1 { 09 07 81 0C 00 00 01 }
0x46975: 			OneOfOption Option: "ILEDB, 2mA" Value: 2 { 09 07 82 0C 00 00 02 }
0x4697C: 			OneOfOption Option: "ILEDB, 4mA" Value: 3 { 09 07 83 0C 00 00 03 }
0x46983: 			OneOfOption Option: "ILEDB, 8mA" Value: 4 { 09 07 84 0C 00 00 04 }
0x4698A: 			OneOfOption Option: "ILEDB, 16mA" Value: 5 { 09 07 85 0C 00 00 05 }
0x46991: 		End  { 29 02 }
0x46993: 		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0x7BC, VarStoreId: 0xF101, VarOffset: 0x336, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 89 0C 86 0C BC 07 01 F1 36 03 10 10 00 06 00 }
0x469A4: 			OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 8D 0C 30 00 00 }
0x469AB: 			OneOfOption Option: "90" Value: 2 { 09 07 8E 0C 00 00 02 }
0x469B2: 			OneOfOption Option: "180" Value: 4 { 09 07 8F 0C 00 00 04 }
0x469B9: 			OneOfOption Option: "270" Value: 6 { 09 07 90 0C 00 00 06 }
0x469C0: 		End  { 29 02 }
0x469C2: 		SuppressIf  { 0A 82 }
0x469C4: 			EqIdVal QuestionId: 0x7B7, Value: 0x50 { 12 86 B7 07 50 00 }
0x469CA: 				Not  { 17 02 }
0x469CC: 			End  { 29 02 }
0x469CE: 			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0x7BD, VarStoreId: 0xF101, VarOffset: 0x337, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 0C 91 0C BD 07 01 F1 37 03 10 10 00 01 00 }
0x469DF: 				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault { 09 07 97 0C 30 00 00 }
0x469E6: 				OneOfOption Option: "Position 2" Value: 1 { 09 07 98 0C 00 00 01 }
0x469ED: 			End  { 29 02 }
0x469EF: 		End  { 29 02 }
0x469F1: 		SuppressIf  { 0A 82 }
0x469F3: 			EqIdVal QuestionId: 0x7BD, Value: 0x1 { 12 86 BD 07 01 00 }
0x469F9: 				Not  { 17 02 }
0x469FB: 			End  { 29 02 }
0x469FD: 			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0x7BE, VarStoreId: 0xF101, VarOffset: 0x338, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9C 0C 99 0C BE 07 01 F1 38 03 10 10 00 01 00 }
0x46A0E: 				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault { 09 07 A0 0C 30 00 00 }
0x46A15: 				OneOfOption Option: "2 voltage rail" Value: 1 { 09 07 A1 0C 00 00 01 }
0x46A1C: 			End  { 29 02 }
0x46A1E: 		End  { 29 02 }
0x46A20: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x7BF, VarStoreId: 0xF101, VarStoreInfo: 0x2DE, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 7D 10 66 0C BF 07 01 F1 DE 02 00 01 0F 00 }
0x46A30: 			Default DefaultId: 0x0 String: "A12N08BU" { 5B 07 00 00 07 68 0C }
0x46A37: 		End  { 29 02 }
0x46A39: 		Numeric Prompt: "MIPI port", Help: "LinkUsed", QuestionFlags: 0x10, QuestionId: 0x7C0, VarStoreId: 0xF101, VarOffset: 0x326, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 BA 0C B7 0C C0 07 01 F1 26 03 10 10 00 0A 01 }
0x46A4A: 			Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x46A50: 		End  { 29 02 }
0x46A52: 		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0x7C1, VarStoreId: 0xF101, VarOffset: 0x327, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 C1 0C BE 0C C1 07 01 F1 27 03 10 10 01 04 00 }
0x46A63: 			OneOfOption Option: "x1" Value: 1 { 09 07 F3 0C 00 00 01 }
0x46A6A: 			OneOfOption Option: "x2" Value: 2, Default { 09 07 F4 0C 10 00 02 }
0x46A71: 			OneOfOption Option: "x3" Value: 3 { 09 07 F5 0C 00 00 03 }
0x46A78: 			OneOfOption Option: "x4" Value: 4 { 09 07 F6 0C 00 00 04 }
0x46A7F: 		End  { 29 02 }
0x46A81: 		OneOf Prompt: "PortSpeed", Help: "PortSpeed: 0:Sensor Default, 1:<416Mbps, 2:<1.5Gbps, 3:<2Gbps, 4:<2.5Gbps, 5:<4Gbps, 6:>4Gbps", QuestionFlags: 0x10, QuestionId: 0x7C2, VarStoreId: 0xF101, VarOffset: 0x328, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 99 10 C6 0C C2 07 01 F1 28 03 10 10 00 06 00 }
0x46A92: 			OneOfOption Option: "0" Value: 0 { 09 07 F8 0C 00 00 00 }
0x46A99: 			OneOfOption Option: "1" Value: 1 { 09 07 F9 0C 00 00 01 }
0x46AA0: 			OneOfOption Option: "2" Value: 2, Default { 09 07 FA 0C 10 00 02 }
0x46AA7: 			OneOfOption Option: "3" Value: 3 { 09 07 FB 0C 00 00 03 }
0x46AAE: 			OneOfOption Option: "4" Value: 4 { 09 07 FC 0C 00 00 04 }
0x46AB5: 			OneOfOption Option: "5" Value: 5 { 09 07 FD 0C 00 00 05 }
0x46ABC: 			OneOfOption Option: "6" Value: 6 { 09 07 FE 0C 00 00 06 }
0x46AC3: 		End  { 29 02 }
0x46AC5: 		Numeric Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0x7C3, VarStoreId: 0xF101, VarOffset: 0x32F, Flags: 0x12, Size: 32, Min: 0x5B8D80, Max: 0x19BFCC0, Step: 0x186A0 { 07 9A 9E 10 C7 0C C3 07 01 F1 2F 03 10 12 80 8D 5B 00 C0 FC 9B 01 A0 86 01 00 }
0x46ADF: 			Default DefaultId: 0x0 Value: 19200000 { 5B 09 00 00 02 00 F8 24 01 }
0x46AE8: 		End  { 29 02 }
0x46AEA: 		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type
0x00: ROM_NONE
0x01: ROM_OTP
0x02: ROM_EEPROM_16K_64
0x03: ROM_EEPROM_16K_16
0x04: ROM_OTP_ACPI_ACPI
0x05: ROM_ACPI
0x06: ROM_EEPROM_BRCA016GWZ
0x07: ROM_EEPROM_24AA32
0x08: ROM_EEPROM_CAT24C08
0x09: ROM_M24C64
0x0A: ROM_DW9806B
0x10: ROM_EEPROM_CAT24C16
0x11: ROM_EEPROM_CAT24C64
0x12: ROM_EEPROM_24AA16", QuestionFlags: 0x10, QuestionId: 0x7C4, VarStoreId: 0xF101, VarOffset: 0x329, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CC 0C C9 0C C4 07 01 F1 29 03 10 10 00 12 00 }
0x46AFB: 			OneOfOption Option: "ROM_NONE" Value: 0, Default { 09 07 D7 0C 10 00 00 }
0x46B02: 			OneOfOption Option: "ROM_OTP" Value: 1 { 09 07 D8 0C 00 00 01 }
0x46B09: 			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2 { 09 07 D9 0C 00 00 02 }
0x46B10: 			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3 { 09 07 DA 0C 00 00 03 }
0x46B17: 			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4 { 09 07 DB 0C 00 00 04 }
0x46B1E: 			OneOfOption Option: "ROM_ACPI" Value: 5 { 09 07 DC 0C 00 00 05 }
0x46B25: 			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6 { 09 07 DD 0C 00 00 06 }
0x46B2C: 			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7 { 09 07 DE 0C 00 00 07 }
0x46B33: 			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8 { 09 07 DF 0C 00 00 08 }
0x46B3A: 			OneOfOption Option: "ROM_EEPROM_M24C64" Value: 9 { 09 07 E0 0C 00 00 09 }
0x46B41: 			OneOfOption Option: "ROM_EEPROM_DW9806B" Value: 10 { 09 07 E1 0C 00 00 0A }
0x46B48: 			OneOfOption Option: "ROM_EEPROM_CAT24C16" Value: 16 { 09 07 E2 0C 00 00 10 }
0x46B4F: 			OneOfOption Option: "ROM_EEPROM_CAT24C64" Value: 17 { 09 07 E3 0C 00 00 11 }
0x46B56: 			OneOfOption Option: "ROM_EEPROM_24AA16" Value: 18 { 09 07 E4 0C 00 00 12 }
0x46B5D: 		End  { 29 02 }
0x46B5F: 		OneOf Prompt: "VCM Type", Help: "VCM Type
0x00: VCM_NONE
0x01: VCM_AD5823
0x02: VCM_DW9714
0x03: VCM_AD5816
0x04: VCM_DW9719
0x05: VCM_DW9718
0x06: VCM_DW9806B
0x07: VCM_WV517S
0x08: VCM_LC898122XA
0x09: VCM_LC898212AXB
0x0F: VCM_AK7371
0x10: VCM_BU64297GWZ", QuestionFlags: 0x10, QuestionId: 0x7C5, VarStoreId: 0xF101, VarOffset: 0x32A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0 { 05 91 D3 0C D0 0C C5 07 01 F1 2A 03 10 10 00 10 00 }
0x46B70: 			OneOfOption Option: "VCM_NONE" Value: 0, Default { 09 07 E5 0C 10 00 00 }
0x46B77: 			OneOfOption Option: "VCM_AD5823" Value: 1 { 09 07 E6 0C 00 00 01 }
0x46B7E: 			OneOfOption Option: "VCM_DW9714" Value: 2 { 09 07 E7 0C 00 00 02 }
0x46B85: 			OneOfOption Option: "VCM_AD5816" Value: 3 { 09 07 E8 0C 00 00 03 }
0x46B8C: 			OneOfOption Option: "VCM_DW9719" Value: 4 { 09 07 EA 0C 00 00 04 }
0x46B93: 			OneOfOption Option: "VCM_DW9718" Value: 5 { 09 07 E9 0C 00 00 05 }
0x46B9A: 			OneOfOption Option: "VCM_DW9806B" Value: 6 { 09 07 EB 0C 00 00 06 }
0x46BA1: 			OneOfOption Option: "VCM_WV517S" Value: 7 { 09 07 EC 0C 00 00 07 }
0x46BA8: 			OneOfOption Option: "VCM_LC898122XA" Value: 8 { 09 07 ED 0C 00 00 08 }
0x46BAF: 			OneOfOption Option: "VCM_LC898212AXB" Value: 9 { 09 07 EE 0C 00 00 09 }
0x46BB6: 			OneOfOption Option: "VCM_RESERVED1" Value: 10 { 09 07 EF 0C 00 00 0A }
0x46BBD: 			OneOfOption Option: "VCM_RESERVED2" Value: 11 { 09 07 F0 0C 00 00 0B }
0x46BC4: 			OneOfOption Option: "VCM_AK7371" Value: 15 { 09 07 F1 0C 00 00 0F }
0x46BCB: 			OneOfOption Option: "VCM_BU64297GWZ" Value: 16 { 09 07 F2 0C 00 00 10 }
0x46BD2: 		End  { 29 02 }
0x46BD4: 		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0x7C6, VarStoreId: 0xF101, VarOffset: 0x2FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1 { 07 91 6F 0B 6C 0B C6 07 01 F1 FE 02 10 10 00 0C 01 }
0x46BE5: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x46BEB: 		End  { 29 02 }
0x46BED: 		SuppressIf  { 0A 82 }
0x46BEF: 			EqIdVal QuestionId: 0x7C6, Value: 0x0 { 12 06 C6 07 00 00 }
0x46BF5: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x7C7, VarStoreId: 0xF101, VarOffset: 0x2FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 92 0B 8F 0B C7 07 01 F1 FF 02 10 10 00 05 00 }
0x46C06: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x46C0D: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x46C14: 				OneOfOption Option: "I2C2" Value: 2, Default { 09 07 1B 0D 10 00 02 }
0x46C1B: 				OneOfOption Option: "I2C3" Value: 3 { 09 07 1C 0D 00 00 03 }
0x46C22: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x46C29: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x46C30: 			End  { 29 02 }
0x46C32: 			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0 { 02 87 83 0B 00 00 00 }
0x46C39: 			End  { 29 02 }
0x46C3B: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7C8, VarStoreId: 0xF101, VarOffset: 0x300, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B3 0B 98 0B C8 07 01 F1 00 03 10 21 00 00 7F 00 01 00 }
0x46C4F: 				Default DefaultId: 0x0 Value: 26 { 5B 07 00 00 01 1A 00 }
0x46C56: 			End  { 29 02 }
0x46C58: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7C9, VarStoreId: 0xF101, VarOffset: 0x318, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 42 0D 29 0D C9 07 01 F1 18 03 10 10 00 0C 00 }
0x46C69: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x46C70: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46C77: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46C7E: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46C85: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x46C8C: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46C93: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46C9A: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46CA1: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46CA8: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46CAF: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46CB6: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46CBD: 			End  { 29 02 }
0x46CBF: 		End  { 29 02 }
0x46CC1: 		SuppressIf  { 0A 82 }
0x46CC3: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1] { 14 0A C6 07 02 00 00 00 01 00 }
0x46CCD: 			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0 { 02 87 84 0B 00 00 00 }
0x46CD4: 			End  { 29 02 }
0x46CD6: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7CA, VarStoreId: 0xF101, VarOffset: 0x302, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B4 0B 98 0B CA 07 01 F1 02 03 10 21 00 00 7F 00 01 00 }
0x46CEA: 				Default DefaultId: 0x0 Value: 14 { 5B 07 00 00 01 0E 00 }
0x46CF1: 			End  { 29 02 }
0x46CF3: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7CB, VarStoreId: 0xF101, VarOffset: 0x319, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 43 0D 29 0D CB 07 01 F1 19 03 10 10 00 0C 00 }
0x46D04: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46D0B: 				OneOfOption Option: "VCM" Value: 1, Default { 09 07 73 0D 10 00 01 }
0x46D12: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46D19: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46D20: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x46D27: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46D2E: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46D35: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46D3C: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46D43: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46D4A: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46D51: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46D58: 			End  { 29 02 }
0x46D5A: 		End  { 29 02 }
0x46D5C: 		SuppressIf  { 0A 82 }
0x46D5E: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2] { 14 0C C6 07 03 00 00 00 01 00 02 00 }
0x46D6A: 			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0 { 02 87 85 0B 00 00 00 }
0x46D71: 			End  { 29 02 }
0x46D73: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7CC, VarStoreId: 0xF101, VarOffset: 0x304, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B5 0B 98 0B CC 07 01 F1 04 03 10 21 00 00 7F 00 01 00 }
0x46D87: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x46D8E: 			End  { 29 02 }
0x46D90: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7CD, VarStoreId: 0xF101, VarOffset: 0x31A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 44 0D 29 0D CD 07 01 F1 1A 03 10 10 00 0C 00 }
0x46DA1: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46DA8: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46DAF: 				OneOfOption Option: "EEPROM" Value: 2, Default { 09 07 74 0D 10 00 02 }
0x46DB6: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46DBD: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x46DC4: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46DCB: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46DD2: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46DD9: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46DE0: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46DE7: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46DEE: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46DF5: 			End  { 29 02 }
0x46DF7: 		End  { 29 02 }
0x46DF9: 		SuppressIf  { 0A 82 }
0x46DFB: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3] { 14 0E C6 07 04 00 00 00 01 00 02 00 03 00 }
0x46E09: 			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0 { 02 87 86 0B 00 00 00 }
0x46E10: 			End  { 29 02 }
0x46E12: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7CE, VarStoreId: 0xF101, VarOffset: 0x306, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B6 0B 98 0B CE 07 01 F1 06 03 10 21 00 00 7F 00 01 00 }
0x46E26: 				Default DefaultId: 0x0 Value: 81 { 5B 07 00 00 01 51 00 }
0x46E2D: 			End  { 29 02 }
0x46E2F: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7CF, VarStoreId: 0xF101, VarOffset: 0x31B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 45 0D 29 0D CF 07 01 F1 1B 03 10 10 00 0C 00 }
0x46E40: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46E47: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46E4E: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46E55: 				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default { 09 07 75 0D 10 00 03 }
0x46E5C: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x46E63: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46E6A: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46E71: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46E78: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46E7F: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46E86: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46E8D: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46E94: 			End  { 29 02 }
0x46E96: 		End  { 29 02 }
0x46E98: 		SuppressIf  { 0A 82 }
0x46E9A: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4] { 14 10 C6 07 05 00 00 00 01 00 02 00 03 00 04 00 }
0x46EAA: 			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0 { 02 87 87 0B 00 00 00 }
0x46EB1: 			End  { 29 02 }
0x46EB3: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7D0, VarStoreId: 0xF101, VarOffset: 0x308, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B7 0B 98 0B D0 07 01 F1 08 03 10 21 00 00 7F 00 01 00 }
0x46EC7: 				Default DefaultId: 0x0 Value: 82 { 5B 07 00 00 01 52 00 }
0x46ECE: 			End  { 29 02 }
0x46ED0: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7D1, VarStoreId: 0xF101, VarOffset: 0x31C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 46 0D 29 0D D1 07 01 F1 1C 03 10 10 00 0C 00 }
0x46EE1: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46EE8: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46EEF: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46EF6: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46EFD: 				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default { 09 07 76 0D 10 00 04 }
0x46F04: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x46F0B: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46F12: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46F19: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46F20: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46F27: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46F2E: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46F35: 			End  { 29 02 }
0x46F37: 		End  { 29 02 }
0x46F39: 		SuppressIf  { 0A 82 }
0x46F3B: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5] { 14 12 C6 07 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x46F4D: 			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0 { 02 87 88 0B 00 00 00 }
0x46F54: 			End  { 29 02 }
0x46F56: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7D2, VarStoreId: 0xF101, VarOffset: 0x30A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B8 0B 98 0B D2 07 01 F1 0A 03 10 21 00 00 7F 00 01 00 }
0x46F6A: 				Default DefaultId: 0x0 Value: 83 { 5B 07 00 00 01 53 00 }
0x46F71: 			End  { 29 02 }
0x46F73: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7D3, VarStoreId: 0xF101, VarOffset: 0x31D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 47 0D 29 0D D3 07 01 F1 1D 03 10 10 00 0C 00 }
0x46F84: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x46F8B: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x46F92: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x46F99: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x46FA0: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x46FA7: 				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default { 09 07 77 0D 10 00 05 }
0x46FAE: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x46FB5: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x46FBC: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x46FC3: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x46FCA: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x46FD1: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x46FD8: 			End  { 29 02 }
0x46FDA: 		End  { 29 02 }
0x46FDC: 		SuppressIf  { 0A 82 }
0x46FDE: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5, 6] { 14 14 C6 07 07 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 }
0x46FF2: 			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0 { 02 87 89 0B 00 00 00 }
0x46FF9: 			End  { 29 02 }
0x46FFB: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7D4, VarStoreId: 0xF101, VarOffset: 0x30C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 B9 0B 98 0B D4 07 01 F1 0C 03 10 21 00 00 7F 00 01 00 }
0x4700F: 				Default DefaultId: 0x0 Value: 84 { 5B 07 00 00 01 54 00 }
0x47016: 			End  { 29 02 }
0x47018: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7D5, VarStoreId: 0xF101, VarOffset: 0x31E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 48 0D 29 0D D5 07 01 F1 1E 03 10 10 00 0C 00 }
0x47029: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47030: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47037: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4703E: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47045: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4704C: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47053: 				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default { 09 07 78 0D 10 00 06 }
0x4705A: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47061: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47068: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4706F: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47076: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4707D: 			End  { 29 02 }
0x4707F: 		End  { 29 02 }
0x47081: 		SuppressIf  { 0A 82 }
0x47083: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5, 6, 7] { 14 16 C6 07 08 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 }
0x47099: 			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0 { 02 87 8A 0B 00 00 00 }
0x470A0: 			End  { 29 02 }
0x470A2: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7D6, VarStoreId: 0xF101, VarOffset: 0x30E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 BA 0B 98 0B D6 07 01 F1 0E 03 10 21 00 00 7F 00 01 00 }
0x470B6: 				Default DefaultId: 0x0 Value: 85 { 5B 07 00 00 01 55 00 }
0x470BD: 			End  { 29 02 }
0x470BF: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7D7, VarStoreId: 0xF101, VarOffset: 0x31F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 49 0D 29 0D D7 07 01 F1 1F 03 10 10 00 0C 00 }
0x470D0: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x470D7: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x470DE: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x470E5: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x470EC: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x470F3: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x470FA: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47101: 				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default { 09 07 79 0D 10 00 07 }
0x47108: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4710F: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47116: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x4711D: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47124: 			End  { 29 02 }
0x47126: 		End  { 29 02 }
0x47128: 		SuppressIf  { 0A 82 }
0x4712A: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8] { 14 18 C6 07 09 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x47142: 			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0 { 02 87 8B 0B 00 00 00 }
0x47149: 			End  { 29 02 }
0x4714B: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7D8, VarStoreId: 0xF101, VarOffset: 0x310, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 BB 0B 98 0B D8 07 01 F1 10 03 10 21 00 00 7F 00 01 00 }
0x4715F: 				Default DefaultId: 0x0 Value: 86 { 5B 07 00 00 01 56 00 }
0x47166: 			End  { 29 02 }
0x47168: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7D9, VarStoreId: 0xF101, VarOffset: 0x320, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 4A 0D 29 0D D9 07 01 F1 20 03 10 10 00 0C 00 }
0x47179: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x47180: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47187: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4718E: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47195: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4719C: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x471A3: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x471AA: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x471B1: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x471B8: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x471BF: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x471C6: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x471CD: 			End  { 29 02 }
0x471CF: 		End  { 29 02 }
0x471D1: 		SuppressIf  { 0A 82 }
0x471D3: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9] { 14 1A C6 07 0A 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 }
0x471ED: 			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0 { 02 87 8C 0B 00 00 00 }
0x471F4: 			End  { 29 02 }
0x471F6: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7DA, VarStoreId: 0xF101, VarOffset: 0x312, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 BC 0B 98 0B DA 07 01 F1 12 03 10 21 00 00 7F 00 01 00 }
0x4720A: 				Default DefaultId: 0x0 Value: 87 { 5B 07 00 00 01 57 00 }
0x47211: 			End  { 29 02 }
0x47213: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7DB, VarStoreId: 0xF101, VarOffset: 0x321, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 4B 0D 29 0D DB 07 01 F1 21 03 10 10 00 0C 00 }
0x47224: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x4722B: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47232: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47239: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47240: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47247: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4724E: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47255: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4725C: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47263: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4726A: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47271: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47278: 			End  { 29 02 }
0x4727A: 		End  { 29 02 }
0x4727C: 		SuppressIf  { 0A 82 }
0x4727E: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10] { 14 1C C6 07 0B 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 }
0x4729A: 			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0 { 02 87 8D 0B 00 00 00 }
0x472A1: 			End  { 29 02 }
0x472A3: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7DC, VarStoreId: 0xF101, VarOffset: 0x314, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 BD 0B 98 0B DC 07 01 F1 14 03 10 21 00 00 7F 00 01 00 }
0x472B7: 				Default DefaultId: 0x0 Value: 88 { 5B 07 00 00 01 58 00 }
0x472BE: 			End  { 29 02 }
0x472C0: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7DD, VarStoreId: 0xF101, VarOffset: 0x322, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 4C 0D 29 0D DD 07 01 F1 22 03 10 10 00 0C 00 }
0x472D1: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x472D8: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x472DF: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x472E6: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x472ED: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x472F4: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x472FB: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47302: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47309: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47310: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47317: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x4731E: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47325: 			End  { 29 02 }
0x47327: 		End  { 29 02 }
0x47329: 		SuppressIf  { 0A 82 }
0x4732B: 			EqIdValList QuestionId: 0x7C6, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11] { 14 1E C6 07 0C 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 0B 00 }
0x47349: 			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0 { 02 87 8E 0B 00 00 00 }
0x47350: 			End  { 29 02 }
0x47352: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7DE, VarStoreId: 0xF101, VarOffset: 0x316, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 BE 0B 98 0B DE 07 01 F1 16 03 10 21 00 00 7F 00 01 00 }
0x47366: 				Default DefaultId: 0x0 Value: 89 { 5B 07 00 00 01 59 00 }
0x4736D: 			End  { 29 02 }
0x4736F: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7DF, VarStoreId: 0xF101, VarOffset: 0x323, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 4D 0D 29 0D DF 07 01 F1 23 03 10 10 00 0C 00 }
0x47380: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x47387: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4738E: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47395: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4739C: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x473A3: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x473AA: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x473B1: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x473B8: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x473BF: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x473C6: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x473CD: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x473D4: 			End  { 29 02 }
0x473D6: 		End  { 29 02 }
0x473D8: 		OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x7E0, VarStoreId: 0xF101, VarOffset: 0x33B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8D 10 A2 0C E0 07 01 F1 3B 03 10 10 00 02 00 }
0x473E9: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x473EF: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 A4 0C 00 00 00 }
0x473F6: 			OneOfOption Option: "External" Value: 1 { 09 07 A5 0C 00 00 01 }
0x473FD: 			OneOfOption Option: "Internal PMIC" Value: 2 { 09 07 A6 0C 00 00 02 }
0x47404: 		End  { 29 02 }
0x47406: 		SuppressIf  { 0A 82 }
0x47408: 			EqIdVal QuestionId: 0x7E0, Value: 0x1 { 12 86 E0 07 01 00 }
0x4740E: 				Not  { 17 02 }
0x47410: 			End  { 29 02 }
0x47412: 			OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x7E1, VarStoreId: 0xF101, VarOffset: 0xAF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 8E 10 A7 0C E1 07 01 F1 F8 0A 10 10 00 05 00 }
0x47423: 				OneOfOption Option: "Flash1" Value: 0, Default, MfgDefault { 09 07 9A 0D 30 00 00 }
0x4742A: 				OneOfOption Option: "Flash2" Value: 1 { 09 07 9B 0D 00 00 01 }
0x47431: 				OneOfOption Option: "Flash3" Value: 2 { 09 07 9C 0D 00 00 02 }
0x47438: 				OneOfOption Option: "Flash4" Value: 3 { 09 07 9D 0D 00 00 03 }
0x4743F: 				OneOfOption Option: "Flash5" Value: 4 { 09 07 9E 0D 00 00 04 }
0x47446: 				OneOfOption Option: "Flash6" Value: 5 { 09 07 9F 0D 00 00 05 }
0x4744D: 			End  { 29 02 }
0x4744F: 		End  { 29 02 }
0x47451: 	End  { 29 02 }
0x47453: 	Form FormId: 0x90, Title: "Link3 options" { 01 86 90 00 62 0B }
0x47459: 		Subtitle Prompt: "Camera4", Help: "", Flags: 0x0 { 02 87 50 0B 00 00 00 }
0x47460: 		End  { 29 02 }
0x47462: 		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0x7E2, VarStoreId: 0xF101, VarOffset: 0x33C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 69 0B 65 0B E2 07 01 F1 3C 03 10 10 00 FF 00 }
0x47473: 			OneOfOption Option: "IMX135" Value: 0 { 09 07 FF 0C 00 00 00 }
0x4747A: 			OneOfOption Option: "OV5693" Value: 1, Default { 09 07 00 0D 10 00 01 }
0x47481: 			OneOfOption Option: "IMX179" Value: 2 { 09 07 01 0D 00 00 02 }
0x47488: 			OneOfOption Option: "OV8858" Value: 3 { 09 07 02 0D 00 00 03 }
0x4748F: 			OneOfOption Option: "OV2740-IVCAM" Value: 4 { 09 07 03 0D 00 00 04 }
0x47496: 			OneOfOption Option: "OV9728" Value: 5 { 09 07 04 0D 00 00 05 }
0x4749D: 			OneOfOption Option: "IMX188" Value: 6 { 09 07 05 0D 00 00 06 }
0x474A4: 			OneOfOption Option: "IMX208" Value: 7 { 09 07 06 0D 00 00 07 }
0x474AB: 			OneOfOption Option: "OV5670" Value: 8 { 09 07 07 0D 00 00 08 }
0x474B2: 			OneOfOption Option: "OV8865" Value: 9 { 09 07 08 0D 00 00 09 }
0x474B9: 			OneOfOption Option: "HM2051" Value: 10 { 09 07 09 0D 00 00 0A }
0x474C0: 			OneOfOption Option: "OV2742" Value: 11 { 09 07 0A 0D 00 00 0B }
0x474C7: 			OneOfOption Option: "OV9234" Value: 12 { 09 07 0B 0D 00 00 0C }
0x474CE: 			OneOfOption Option: "OV8856" Value: 13 { 09 07 0C 0D 00 00 0D }
0x474D5: 			OneOfOption Option: "OV16860" Value: 14 { 09 07 0D 0D 00 00 0E }
0x474DC: 			OneOfOption Option: "IMX362" Value: 15 { 09 07 0E 0D 00 00 0F }
0x474E3: 			OneOfOption Option: "IMX488" Value: 16 { 09 07 0F 0D 00 00 10 }
0x474EA: 			OneOfOption Option: "OVTI01AS" Value: 17 { 09 07 11 0D 00 00 11 }
0x474F1: 			OneOfOption Option: "OVTI01A0" Value: 18 { 09 07 12 0D 00 00 12 }
0x474F8: 			OneOfOption Option: "OVTI5678" Value: 19 { 09 07 13 0D 00 00 13 }
0x474FF: 			OneOfOption Option: "OVTI9738" Value: 20 { 09 07 14 0D 00 00 14 }
0x47506: 			OneOfOption Option: "HIMAX11B1" Value: 21 { 09 07 16 0D 00 00 15 }
0x4750D: 			OneOfOption Option: "OVTID858" Value: 22 { 09 07 15 0D 00 00 16 }
0x47514: 			OneOfOption Option: "User Custom" Value: 255 { 09 07 17 0D 00 00 FF }
0x4751B: 		End  { 29 02 }
0x4751D: 		SuppressIf  { 0A 82 }
0x4751F: 			EqIdVal QuestionId: 0x7E2, Value: 0xFF { 12 86 E2 07 FF 00 }
0x47525: 				Not  { 17 02 }
0x47527: 			End  { 29 02 }
0x47529: 			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0x7E3, VarStoreId: 0xF101, VarStoreInfo: 0x33D, MinSize: 0x6, MaxSize: 0x14, Flags: 0x0 { 1C 90 A4 10 18 0D E3 07 01 F1 3D 03 00 06 14 00 }
0x47539: 			End  { 29 02 }
0x4753B: 		End  { 29 02 }
0x4753D: 		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0x7E4, VarStoreId: 0xF101, VarOffset: 0xA95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 7A 0B 76 0B E4 07 01 F1 95 0A 10 10 00 07 00 }
0x4754E: 			OneOfOption Option: "4 4 2 2" Value: 0, Default { 09 07 7D 0B 10 00 00 }
0x47555: 			OneOfOption Option: "4 4 3 1" Value: 2 { 09 07 7E 0B 00 00 02 }
0x4755C: 			OneOfOption Option: "4 4 4 0" Value: 3 { 09 07 7F 0B 00 00 03 }
0x47563: 			OneOfOption Option: "8 0 2 2" Value: 4 { 09 07 80 0B 00 00 04 }
0x4756A: 			OneOfOption Option: "8 0 3 1" Value: 6 { 09 07 81 0B 00 00 06 }
0x47571: 			OneOfOption Option: "8 0 4 0" Value: 7 { 09 07 82 0B 00 00 07 }
0x47578: 		End  { 29 02 }
0x4757A: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x7E5, VarStoreId: 0xF101, VarOffset: 0x3AD, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 AD 0C A9 0C E5 07 01 F1 AD 03 10 10 10 50 00 }
0x4758B: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x47592: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x47599: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x475A0: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x475A7: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x475AE: 		End  { 29 02 }
0x475B0: 		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0x7E6, VarStoreId: 0xF101, VarOffset: 0x3BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 82 0D 7E 0D E6 07 01 F1 BB 03 10 10 00 FF 00 }
0x475C1: 			OneOfOption Option: "No Control Logic" Value: 255, Default { 09 07 28 0D 10 00 FF }
0x475C8: 			OneOfOption Option: "Control Logic 1" Value: 0 { 09 07 22 0D 00 00 00 }
0x475CF: 			OneOfOption Option: "Control Logic 2" Value: 1 { 09 07 23 0D 00 00 01 }
0x475D6: 			OneOfOption Option: "Control Logic 3" Value: 2 { 09 07 24 0D 00 00 02 }
0x475DD: 			OneOfOption Option: "Control Logic 4" Value: 3 { 09 07 25 0D 00 00 03 }
0x475E4: 			SuppressIf  { 0A 82 }
0x475E6: 				EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x475EC: 					Not  { 17 02 }
0x475EE: 				End  { 29 02 }
0x475F0: 				OneOfOption Option: "Control Logic 5" Value: 3 { 09 07 26 0D 00 00 03 }
0x475F7: 			End  { 29 02 }
0x475F9: 			SuppressIf  { 0A 82 }
0x475FB: 				EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x47601: 					Not  { 17 02 }
0x47603: 				End  { 29 02 }
0x47605: 				OneOfOption Option: "Control Logic 6" Value: 3 { 09 07 27 0D 00 00 03 }
0x4760C: 			End  { 29 02 }
0x4760E: 		End  { 29 02 }
0x47610: 		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0x7E7, VarStoreId: 0xF101, VarOffset: 0x365, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0 { 05 91 63 0C 5F 0C E7 07 01 F1 65 03 10 10 61 69 00 }
0x47621: 			OneOfOption Option: "Front" Value: 97 { 09 07 6C 0C 00 00 61 }
0x47628: 			OneOfOption Option: "Back" Value: 105, Default { 09 07 6D 0C 10 00 69 }
0x4762F: 		End  { 29 02 }
0x47631: 		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0x7E8, VarStoreId: 0xF101, VarOffset: 0x3BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 75 0C 71 0C E8 07 01 F1 BC 03 10 10 00 03 00 }
0x47642: 			OneOfOption Option: "Driver default" Value: 0, Default { 09 07 78 0C 10 00 00 }
0x47649: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x47650: 			OneOfOption Option: "Enabled" Value: 3 { 09 07 03 00 00 00 03 }
0x47657: 		End  { 29 02 }
0x47659: 		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0x7E9, VarStoreId: 0xF101, VarOffset: 0x3BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7D 0C 79 0C E9 07 01 F1 BD 03 10 10 00 05 00 }
0x4766A: 			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault { 09 07 80 0C 30 00 00 }
0x47671: 			OneOfOption Option: "ILEDA, 16mA" Value: 1 { 09 07 81 0C 00 00 01 }
0x47678: 			OneOfOption Option: "ILEDB, 2mA" Value: 2 { 09 07 82 0C 00 00 02 }
0x4767F: 			OneOfOption Option: "ILEDB, 4mA" Value: 3 { 09 07 83 0C 00 00 03 }
0x47686: 			OneOfOption Option: "ILEDB, 8mA" Value: 4 { 09 07 84 0C 00 00 04 }
0x4768D: 			OneOfOption Option: "ILEDB, 16mA" Value: 5 { 09 07 85 0C 00 00 05 }
0x47694: 		End  { 29 02 }
0x47696: 		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0x7EA, VarStoreId: 0xF101, VarOffset: 0x3BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 8A 0C 86 0C EA 07 01 F1 BE 03 10 10 00 06 00 }
0x476A7: 			OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 8D 0C 30 00 00 }
0x476AE: 			OneOfOption Option: "90" Value: 2 { 09 07 8E 0C 00 00 02 }
0x476B5: 			OneOfOption Option: "180" Value: 4 { 09 07 8F 0C 00 00 04 }
0x476BC: 			OneOfOption Option: "270" Value: 6 { 09 07 90 0C 00 00 06 }
0x476C3: 		End  { 29 02 }
0x476C5: 		SuppressIf  { 0A 82 }
0x476C7: 			EqIdVal QuestionId: 0x7E5, Value: 0x50 { 12 86 E5 07 50 00 }
0x476CD: 				Not  { 17 02 }
0x476CF: 			End  { 29 02 }
0x476D1: 			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0x7EB, VarStoreId: 0xF101, VarOffset: 0x3BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 0C 91 0C EB 07 01 F1 BF 03 10 10 00 01 00 }
0x476E2: 				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault { 09 07 97 0C 30 00 00 }
0x476E9: 				OneOfOption Option: "Position 2" Value: 1 { 09 07 98 0C 00 00 01 }
0x476F0: 			End  { 29 02 }
0x476F2: 		End  { 29 02 }
0x476F4: 		SuppressIf  { 0A 82 }
0x476F6: 			EqIdVal QuestionId: 0x7EB, Value: 0x1 { 12 86 EB 07 01 00 }
0x476FC: 				Not  { 17 02 }
0x476FE: 			End  { 29 02 }
0x47700: 			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0x7EC, VarStoreId: 0xF101, VarOffset: 0x3C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 0C 99 0C EC 07 01 F1 C0 03 10 10 00 01 00 }
0x47711: 				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault { 09 07 A0 0C 30 00 00 }
0x47718: 				OneOfOption Option: "2 voltage rail" Value: 1 { 09 07 A1 0C 00 00 01 }
0x4771F: 			End  { 29 02 }
0x47721: 		End  { 29 02 }
0x47723: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x7ED, VarStoreId: 0xF101, VarStoreInfo: 0x366, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 7E 10 66 0C ED 07 01 F1 66 03 00 01 0F 00 }
0x47733: 		End  { 29 02 }
0x47735: 		Numeric Prompt: "MIPI port", Help: "LinkUsed", QuestionFlags: 0x10, QuestionId: 0x7EE, VarStoreId: 0xF101, VarOffset: 0x3AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 BB 0C B7 0C EE 07 01 F1 AE 03 10 10 00 0A 01 }
0x47746: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4774C: 		End  { 29 02 }
0x4774E: 		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0x7EF, VarStoreId: 0xF101, VarOffset: 0x3AF, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 C2 0C BE 0C EF 07 01 F1 AF 03 10 10 01 04 00 }
0x4775F: 			OneOfOption Option: "x1" Value: 1 { 09 07 F3 0C 00 00 01 }
0x47766: 			OneOfOption Option: "x2" Value: 2 { 09 07 F4 0C 00 00 02 }
0x4776D: 			OneOfOption Option: "x3" Value: 3 { 09 07 F5 0C 00 00 03 }
0x47774: 			OneOfOption Option: "x4" Value: 4, Default { 09 07 F6 0C 10 00 04 }
0x4777B: 		End  { 29 02 }
0x4777D: 		OneOf Prompt: "PortSpeed", Help: "PortSpeed: 0:Sensor Default, 1:<416Mbps, 2:<1.5Gbps, 3:<2Gbps, 4:<2.5Gbps, 5:<4Gbps, 6:>4Gbps", QuestionFlags: 0x10, QuestionId: 0x7F0, VarStoreId: 0xF101, VarOffset: 0x3B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 9A 10 C6 0C F0 07 01 F1 B0 03 10 10 00 06 00 }
0x4778E: 			OneOfOption Option: "0" Value: 0 { 09 07 F8 0C 00 00 00 }
0x47795: 			OneOfOption Option: "1" Value: 1 { 09 07 F9 0C 00 00 01 }
0x4779C: 			OneOfOption Option: "2" Value: 2, Default { 09 07 FA 0C 10 00 02 }
0x477A3: 			OneOfOption Option: "3" Value: 3 { 09 07 FB 0C 00 00 03 }
0x477AA: 			OneOfOption Option: "4" Value: 4 { 09 07 FC 0C 00 00 04 }
0x477B1: 			OneOfOption Option: "5" Value: 5 { 09 07 FD 0C 00 00 05 }
0x477B8: 			OneOfOption Option: "6" Value: 6 { 09 07 FE 0C 00 00 06 }
0x477BF: 		End  { 29 02 }
0x477C1: 		Numeric Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0x7F1, VarStoreId: 0xF101, VarOffset: 0x3B7, Flags: 0x12, Size: 32, Min: 0x5B8D80, Max: 0x19BFCC0, Step: 0x186A0 { 07 9A 9F 10 C7 0C F1 07 01 F1 B7 03 10 12 80 8D 5B 00 C0 FC 9B 01 A0 86 01 00 }
0x477DB: 			Default DefaultId: 0x0 Value: 19200000 { 5B 09 00 00 02 00 F8 24 01 }
0x477E4: 		End  { 29 02 }
0x477E6: 		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type
0x00: ROM_NONE
0x01: ROM_OTP
0x02: ROM_EEPROM_16K_64
0x03: ROM_EEPROM_16K_16
0x04: ROM_OTP_ACPI_ACPI
0x05: ROM_ACPI
0x06: ROM_EEPROM_BRCA016GWZ
0x07: ROM_EEPROM_24AA32
0x08: ROM_EEPROM_CAT24C08
0x09: ROM_M24C64
0x0A: ROM_DW9806B
0x10: ROM_EEPROM_CAT24C16
0x11: ROM_EEPROM_CAT24C64
0x12: ROM_EEPROM_24AA16", QuestionFlags: 0x10, QuestionId: 0x7F2, VarStoreId: 0xF101, VarOffset: 0x3B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CD 0C C9 0C F2 07 01 F1 B1 03 10 10 00 12 00 }
0x477F7: 			OneOfOption Option: "ROM_NONE" Value: 0, Default { 09 07 D7 0C 10 00 00 }
0x477FE: 			OneOfOption Option: "ROM_OTP" Value: 1 { 09 07 D8 0C 00 00 01 }
0x47805: 			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2 { 09 07 D9 0C 00 00 02 }
0x4780C: 			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3 { 09 07 DA 0C 00 00 03 }
0x47813: 			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4 { 09 07 DB 0C 00 00 04 }
0x4781A: 			OneOfOption Option: "ROM_ACPI" Value: 5 { 09 07 DC 0C 00 00 05 }
0x47821: 			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6 { 09 07 DD 0C 00 00 06 }
0x47828: 			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7 { 09 07 DE 0C 00 00 07 }
0x4782F: 			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8 { 09 07 DF 0C 00 00 08 }
0x47836: 			OneOfOption Option: "ROM_EEPROM_M24C64" Value: 9 { 09 07 E0 0C 00 00 09 }
0x4783D: 			OneOfOption Option: "ROM_EEPROM_DW9806B" Value: 10 { 09 07 E1 0C 00 00 0A }
0x47844: 			OneOfOption Option: "ROM_EEPROM_CAT24C16" Value: 16 { 09 07 E2 0C 00 00 10 }
0x4784B: 			OneOfOption Option: "ROM_EEPROM_CAT24C64" Value: 17 { 09 07 E3 0C 00 00 11 }
0x47852: 			OneOfOption Option: "ROM_EEPROM_24AA16" Value: 18 { 09 07 E4 0C 00 00 12 }
0x47859: 		End  { 29 02 }
0x4785B: 		OneOf Prompt: "VCM Type", Help: "VCM Type
0x00: VCM_NONE
0x01: VCM_AD5823
0x02: VCM_DW9714
0x03: VCM_AD5816
0x04: VCM_DW9719
0x05: VCM_DW9718
0x06: VCM_DW9806B
0x07: VCM_WV517S
0x08: VCM_LC898122XA
0x09: VCM_LC898212AXB
0x0F: VCM_AK7371
0x10: VCM_BU64297GWZ", QuestionFlags: 0x10, QuestionId: 0x7F3, VarStoreId: 0xF101, VarOffset: 0x3B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0 { 05 91 D4 0C D0 0C F3 07 01 F1 B2 03 10 10 00 10 00 }
0x4786C: 			OneOfOption Option: "VCM_NONE" Value: 0, Default { 09 07 E5 0C 10 00 00 }
0x47873: 			OneOfOption Option: "VCM_AD5823" Value: 1 { 09 07 E6 0C 00 00 01 }
0x4787A: 			OneOfOption Option: "VCM_DW9714" Value: 2 { 09 07 E7 0C 00 00 02 }
0x47881: 			OneOfOption Option: "VCM_AD5816" Value: 3 { 09 07 E8 0C 00 00 03 }
0x47888: 			OneOfOption Option: "VCM_DW9719" Value: 4 { 09 07 EA 0C 00 00 04 }
0x4788F: 			OneOfOption Option: "VCM_DW9718" Value: 5 { 09 07 E9 0C 00 00 05 }
0x47896: 			OneOfOption Option: "VCM_DW9806B" Value: 6 { 09 07 EB 0C 00 00 06 }
0x4789D: 			OneOfOption Option: "VCM_WV517S" Value: 7 { 09 07 EC 0C 00 00 07 }
0x478A4: 			OneOfOption Option: "VCM_LC898122XA" Value: 8 { 09 07 ED 0C 00 00 08 }
0x478AB: 			OneOfOption Option: "VCM_LC898212AXB" Value: 9 { 09 07 EE 0C 00 00 09 }
0x478B2: 			OneOfOption Option: "VCM_RESERVED1" Value: 10 { 09 07 EF 0C 00 00 0A }
0x478B9: 			OneOfOption Option: "VCM_RESERVED2" Value: 11 { 09 07 F0 0C 00 00 0B }
0x478C0: 			OneOfOption Option: "VCM_AK7371" Value: 15 { 09 07 F1 0C 00 00 0F }
0x478C7: 			OneOfOption Option: "VCM_BU64297GWZ" Value: 16 { 09 07 F2 0C 00 00 10 }
0x478CE: 		End  { 29 02 }
0x478D0: 		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0x7F4, VarStoreId: 0xF101, VarOffset: 0x386, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1 { 07 91 70 0B 6C 0B F4 07 01 F1 86 03 10 10 00 0C 01 }
0x478E1: 			Default DefaultId: 0x0 Value: 6 { 5B 06 00 00 00 06 }
0x478E7: 		End  { 29 02 }
0x478E9: 		SuppressIf  { 0A 82 }
0x478EB: 			EqIdVal QuestionId: 0x7F4, Value: 0x0 { 12 06 F4 07 00 00 }
0x478F1: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x7F5, VarStoreId: 0xF101, VarOffset: 0x387, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 93 0B 8F 0B F5 07 01 F1 87 03 10 10 00 05 00 }
0x47902: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x47909: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x47910: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x47917: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4791E: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x47925: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4792C: 			End  { 29 02 }
0x4792E: 			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0 { 02 87 83 0B 00 00 00 }
0x47935: 			End  { 29 02 }
0x47937: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7F6, VarStoreId: 0xF101, VarOffset: 0x388, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 BF 0B 98 0B F6 07 01 F1 88 03 10 21 00 00 7F 00 01 00 }
0x4794B: 				Default DefaultId: 0x0 Value: 16 { 5B 07 00 00 01 10 00 }
0x47952: 			End  { 29 02 }
0x47954: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7F7, VarStoreId: 0xF101, VarOffset: 0x3A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 4E 0D 29 0D F7 07 01 F1 A0 03 10 10 00 0C 00 }
0x47965: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x4796C: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47973: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4797A: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47981: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47988: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4798F: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47996: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4799D: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x479A4: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x479AB: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x479B2: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x479B9: 			End  { 29 02 }
0x479BB: 		End  { 29 02 }
0x479BD: 		SuppressIf  { 0A 82 }
0x479BF: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1] { 14 0A F4 07 02 00 00 00 01 00 }
0x479C9: 			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0 { 02 87 84 0B 00 00 00 }
0x479D0: 			End  { 29 02 }
0x479D2: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7F8, VarStoreId: 0xF101, VarOffset: 0x38A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C0 0B 98 0B F8 07 01 F1 8A 03 10 21 00 00 7F 00 01 00 }
0x479E6: 				Default DefaultId: 0x0 Value: 12 { 5B 07 00 00 01 0C 00 }
0x479ED: 			End  { 29 02 }
0x479EF: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7F9, VarStoreId: 0xF101, VarOffset: 0x3A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 4F 0D 29 0D F9 07 01 F1 A1 03 10 10 00 0C 00 }
0x47A00: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47A07: 				OneOfOption Option: "VCM" Value: 1, Default { 09 07 73 0D 10 00 01 }
0x47A0E: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47A15: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47A1C: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47A23: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47A2A: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47A31: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47A38: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47A3F: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47A46: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47A4D: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47A54: 			End  { 29 02 }
0x47A56: 		End  { 29 02 }
0x47A58: 		SuppressIf  { 0A 82 }
0x47A5A: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2] { 14 0C F4 07 03 00 00 00 01 00 02 00 }
0x47A66: 			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0 { 02 87 85 0B 00 00 00 }
0x47A6D: 			End  { 29 02 }
0x47A6F: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7FA, VarStoreId: 0xF101, VarOffset: 0x38C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C1 0B 98 0B FA 07 01 F1 8C 03 10 21 00 00 7F 00 01 00 }
0x47A83: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x47A8A: 			End  { 29 02 }
0x47A8C: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7FB, VarStoreId: 0xF101, VarOffset: 0x3A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 50 0D 29 0D FB 07 01 F1 A2 03 10 10 00 0C 00 }
0x47A9D: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47AA4: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47AAB: 				OneOfOption Option: "EEPROM" Value: 2, Default { 09 07 74 0D 10 00 02 }
0x47AB2: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47AB9: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47AC0: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47AC7: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47ACE: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47AD5: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47ADC: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47AE3: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47AEA: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47AF1: 			End  { 29 02 }
0x47AF3: 		End  { 29 02 }
0x47AF5: 		SuppressIf  { 0A 82 }
0x47AF7: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3] { 14 0E F4 07 04 00 00 00 01 00 02 00 03 00 }
0x47B05: 			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0 { 02 87 86 0B 00 00 00 }
0x47B0C: 			End  { 29 02 }
0x47B0E: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7FC, VarStoreId: 0xF101, VarOffset: 0x38E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C2 0B 98 0B FC 07 01 F1 8E 03 10 21 00 00 7F 00 01 00 }
0x47B22: 				Default DefaultId: 0x0 Value: 81 { 5B 07 00 00 01 51 00 }
0x47B29: 			End  { 29 02 }
0x47B2B: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7FD, VarStoreId: 0xF101, VarOffset: 0x3A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 51 0D 29 0D FD 07 01 F1 A3 03 10 10 00 0C 00 }
0x47B3C: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47B43: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47B4A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47B51: 				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default { 09 07 75 0D 10 00 03 }
0x47B58: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47B5F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47B66: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47B6D: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47B74: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47B7B: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47B82: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47B89: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47B90: 			End  { 29 02 }
0x47B92: 		End  { 29 02 }
0x47B94: 		SuppressIf  { 0A 82 }
0x47B96: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4] { 14 10 F4 07 05 00 00 00 01 00 02 00 03 00 04 00 }
0x47BA6: 			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0 { 02 87 87 0B 00 00 00 }
0x47BAD: 			End  { 29 02 }
0x47BAF: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x7FE, VarStoreId: 0xF101, VarOffset: 0x390, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C3 0B 98 0B FE 07 01 F1 90 03 10 21 00 00 7F 00 01 00 }
0x47BC3: 				Default DefaultId: 0x0 Value: 82 { 5B 07 00 00 01 52 00 }
0x47BCA: 			End  { 29 02 }
0x47BCC: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x7FF, VarStoreId: 0xF101, VarOffset: 0x3A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 52 0D 29 0D FF 07 01 F1 A4 03 10 10 00 0C 00 }
0x47BDD: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47BE4: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47BEB: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47BF2: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47BF9: 				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default { 09 07 76 0D 10 00 04 }
0x47C00: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47C07: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47C0E: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47C15: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47C1C: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47C23: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47C2A: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47C31: 			End  { 29 02 }
0x47C33: 		End  { 29 02 }
0x47C35: 		SuppressIf  { 0A 82 }
0x47C37: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5] { 14 12 F4 07 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x47C49: 			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0 { 02 87 88 0B 00 00 00 }
0x47C50: 			End  { 29 02 }
0x47C52: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x800, VarStoreId: 0xF101, VarOffset: 0x392, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C4 0B 98 0B 00 08 01 F1 92 03 10 21 00 00 7F 00 01 00 }
0x47C66: 				Default DefaultId: 0x0 Value: 83 { 5B 07 00 00 01 53 00 }
0x47C6D: 			End  { 29 02 }
0x47C6F: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x801, VarStoreId: 0xF101, VarOffset: 0x3A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 53 0D 29 0D 01 08 01 F1 A5 03 10 10 00 0C 00 }
0x47C80: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47C87: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47C8E: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47C95: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47C9C: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47CA3: 				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default { 09 07 77 0D 10 00 05 }
0x47CAA: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47CB1: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47CB8: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47CBF: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47CC6: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47CCD: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47CD4: 			End  { 29 02 }
0x47CD6: 		End  { 29 02 }
0x47CD8: 		SuppressIf  { 0A 82 }
0x47CDA: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5, 6] { 14 14 F4 07 07 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 }
0x47CEE: 			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0 { 02 87 89 0B 00 00 00 }
0x47CF5: 			End  { 29 02 }
0x47CF7: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x802, VarStoreId: 0xF101, VarOffset: 0x394, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C5 0B 98 0B 02 08 01 F1 94 03 10 21 00 00 7F 00 01 00 }
0x47D0B: 				Default DefaultId: 0x0 Value: 84 { 5B 07 00 00 01 54 00 }
0x47D12: 			End  { 29 02 }
0x47D14: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x803, VarStoreId: 0xF101, VarOffset: 0x3A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 54 0D 29 0D 03 08 01 F1 A6 03 10 10 00 0C 00 }
0x47D25: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47D2C: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47D33: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47D3A: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47D41: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47D48: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47D4F: 				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default { 09 07 78 0D 10 00 06 }
0x47D56: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47D5D: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47D64: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47D6B: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47D72: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47D79: 			End  { 29 02 }
0x47D7B: 		End  { 29 02 }
0x47D7D: 		SuppressIf  { 0A 82 }
0x47D7F: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5, 6, 7] { 14 16 F4 07 08 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 }
0x47D95: 			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0 { 02 87 8A 0B 00 00 00 }
0x47D9C: 			End  { 29 02 }
0x47D9E: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x804, VarStoreId: 0xF101, VarOffset: 0x396, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C6 0B 98 0B 04 08 01 F1 96 03 10 21 00 00 7F 00 01 00 }
0x47DB2: 				Default DefaultId: 0x0 Value: 85 { 5B 07 00 00 01 55 00 }
0x47DB9: 			End  { 29 02 }
0x47DBB: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x805, VarStoreId: 0xF101, VarOffset: 0x3A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 55 0D 29 0D 05 08 01 F1 A7 03 10 10 00 0C 00 }
0x47DCC: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47DD3: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47DDA: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47DE1: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47DE8: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47DEF: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47DF6: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47DFD: 				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default { 09 07 79 0D 10 00 07 }
0x47E04: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47E0B: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47E12: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47E19: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47E20: 			End  { 29 02 }
0x47E22: 		End  { 29 02 }
0x47E24: 		SuppressIf  { 0A 82 }
0x47E26: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8] { 14 18 F4 07 09 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x47E3E: 			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0 { 02 87 8B 0B 00 00 00 }
0x47E45: 			End  { 29 02 }
0x47E47: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x806, VarStoreId: 0xF101, VarOffset: 0x398, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C7 0B 98 0B 06 08 01 F1 98 03 10 21 00 00 7F 00 01 00 }
0x47E5B: 				Default DefaultId: 0x0 Value: 86 { 5B 07 00 00 01 56 00 }
0x47E62: 			End  { 29 02 }
0x47E64: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x807, VarStoreId: 0xF101, VarOffset: 0x3A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 56 0D 29 0D 07 08 01 F1 A8 03 10 10 00 0C 00 }
0x47E75: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47E7C: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47E83: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47E8A: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47E91: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47E98: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47E9F: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47EA6: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47EAD: 				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default { 09 07 7A 0D 10 00 08 }
0x47EB4: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x47EBB: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47EC2: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47EC9: 			End  { 29 02 }
0x47ECB: 		End  { 29 02 }
0x47ECD: 		SuppressIf  { 0A 82 }
0x47ECF: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9] { 14 1A F4 07 0A 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 }
0x47EE9: 			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0 { 02 87 8C 0B 00 00 00 }
0x47EF0: 			End  { 29 02 }
0x47EF2: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x808, VarStoreId: 0xF101, VarOffset: 0x39A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C8 0B 98 0B 08 08 01 F1 9A 03 10 21 00 00 7F 00 01 00 }
0x47F06: 				Default DefaultId: 0x0 Value: 87 { 5B 07 00 00 01 57 00 }
0x47F0D: 			End  { 29 02 }
0x47F0F: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x809, VarStoreId: 0xF101, VarOffset: 0x3A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 57 0D 29 0D 09 08 01 F1 A9 03 10 10 00 0C 00 }
0x47F20: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47F27: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47F2E: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47F35: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47F3C: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47F43: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47F4A: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47F51: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x47F58: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x47F5F: 				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default { 09 07 7B 0D 10 00 09 }
0x47F66: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x47F6D: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x47F74: 			End  { 29 02 }
0x47F76: 		End  { 29 02 }
0x47F78: 		SuppressIf  { 0A 82 }
0x47F7A: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10] { 14 1C F4 07 0B 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 }
0x47F96: 			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0 { 02 87 8D 0B 00 00 00 }
0x47F9D: 			End  { 29 02 }
0x47F9F: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x80A, VarStoreId: 0xF101, VarOffset: 0x39C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 C9 0B 98 0B 0A 08 01 F1 9C 03 10 21 00 00 7F 00 01 00 }
0x47FB3: 				Default DefaultId: 0x0 Value: 88 { 5B 07 00 00 01 58 00 }
0x47FBA: 			End  { 29 02 }
0x47FBC: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x80B, VarStoreId: 0xF101, VarOffset: 0x3AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 58 0D 29 0D 0B 08 01 F1 AA 03 10 10 00 0C 00 }
0x47FCD: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x47FD4: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x47FDB: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x47FE2: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x47FE9: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x47FF0: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x47FF7: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x47FFE: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48005: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4800C: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48013: 				OneOfOption Option: "IO Expander" Value: 10, Default { 09 07 7C 0D 10 00 0A }
0x4801A: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48021: 			End  { 29 02 }
0x48023: 		End  { 29 02 }
0x48025: 		SuppressIf  { 0A 82 }
0x48027: 			EqIdValList QuestionId: 0x7F4, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11] { 14 1E F4 07 0C 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 0B 00 }
0x48045: 			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0 { 02 87 8E 0B 00 00 00 }
0x4804C: 			End  { 29 02 }
0x4804E: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x80C, VarStoreId: 0xF101, VarOffset: 0x39E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 CA 0B 98 0B 0C 08 01 F1 9E 03 10 21 00 00 7F 00 01 00 }
0x48062: 				Default DefaultId: 0x0 Value: 89 { 5B 07 00 00 01 59 00 }
0x48069: 			End  { 29 02 }
0x4806B: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x80D, VarStoreId: 0xF101, VarOffset: 0x3AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 59 0D 29 0D 0D 08 01 F1 AB 03 10 10 00 0C 00 }
0x4807C: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48083: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4808A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48091: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48098: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4809F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x480A6: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x480AD: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x480B4: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x480BB: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x480C2: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x480C9: 				OneOfOption Option: "Flash" Value: 12, Default { 09 07 7D 0D 10 00 0C }
0x480D0: 			End  { 29 02 }
0x480D2: 		End  { 29 02 }
0x480D4: 		OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x80E, VarStoreId: 0xF101, VarOffset: 0x3C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8F 10 A2 0C 0E 08 01 F1 C3 03 10 10 00 02 00 }
0x480E5: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 A4 0C 30 00 00 }
0x480EC: 			OneOfOption Option: "External" Value: 1 { 09 07 A5 0C 00 00 01 }
0x480F3: 			OneOfOption Option: "Internal PMIC" Value: 2 { 09 07 A6 0C 00 00 02 }
0x480FA: 		End  { 29 02 }
0x480FC: 		SuppressIf  { 0A 82 }
0x480FE: 			EqIdVal QuestionId: 0x80E, Value: 0x1 { 12 86 0E 08 01 00 }
0x48104: 				Not  { 17 02 }
0x48106: 			End  { 29 02 }
0x48108: 			OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x80F, VarStoreId: 0xF101, VarOffset: 0xAF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 90 10 A7 0C 0F 08 01 F1 F9 0A 10 10 00 05 00 }
0x48119: 				OneOfOption Option: "Flash1" Value: 0, Default, MfgDefault { 09 07 9A 0D 30 00 00 }
0x48120: 				OneOfOption Option: "Flash2" Value: 1 { 09 07 9B 0D 00 00 01 }
0x48127: 				OneOfOption Option: "Flash3" Value: 2 { 09 07 9C 0D 00 00 02 }
0x4812E: 				OneOfOption Option: "Flash4" Value: 3 { 09 07 9D 0D 00 00 03 }
0x48135: 				OneOfOption Option: "Flash5" Value: 4 { 09 07 9E 0D 00 00 04 }
0x4813C: 				OneOfOption Option: "Flash6" Value: 5 { 09 07 9F 0D 00 00 05 }
0x48143: 			End  { 29 02 }
0x48145: 		End  { 29 02 }
0x48147: 	End  { 29 02 }
0x48149: 	Form FormId: 0x91, Title: "Link4 options" { 01 86 91 00 63 0B }
0x4814F: 		Subtitle Prompt: "Camera5", Help: "", Flags: 0x0 { 02 87 51 0B 00 00 00 }
0x48156: 		End  { 29 02 }
0x48158: 		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0x810, VarStoreId: 0xF101, VarOffset: 0x3C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 6A 0B 65 0B 10 08 01 F1 C4 03 10 10 00 FF 00 }
0x48169: 			OneOfOption Option: "IMX135" Value: 0 { 09 07 FF 0C 00 00 00 }
0x48170: 			OneOfOption Option: "OV5693" Value: 1, Default { 09 07 00 0D 10 00 01 }
0x48177: 			OneOfOption Option: "IMX179" Value: 2 { 09 07 01 0D 00 00 02 }
0x4817E: 			OneOfOption Option: "OV8858" Value: 3 { 09 07 02 0D 00 00 03 }
0x48185: 			OneOfOption Option: "OV2740-IVCAM" Value: 4 { 09 07 03 0D 00 00 04 }
0x4818C: 			OneOfOption Option: "OV9728" Value: 5 { 09 07 04 0D 00 00 05 }
0x48193: 			OneOfOption Option: "IMX188" Value: 6 { 09 07 05 0D 00 00 06 }
0x4819A: 			OneOfOption Option: "IMX208" Value: 7 { 09 07 06 0D 00 00 07 }
0x481A1: 			OneOfOption Option: "OV5670" Value: 8 { 09 07 07 0D 00 00 08 }
0x481A8: 			OneOfOption Option: "OV8865" Value: 9 { 09 07 08 0D 00 00 09 }
0x481AF: 			OneOfOption Option: "HM2051" Value: 10 { 09 07 09 0D 00 00 0A }
0x481B6: 			OneOfOption Option: "OV2742" Value: 11 { 09 07 0A 0D 00 00 0B }
0x481BD: 			OneOfOption Option: "OV9234" Value: 12 { 09 07 0B 0D 00 00 0C }
0x481C4: 			OneOfOption Option: "OV8856" Value: 13 { 09 07 0C 0D 00 00 0D }
0x481CB: 			OneOfOption Option: "OV16860" Value: 14 { 09 07 0D 0D 00 00 0E }
0x481D2: 			OneOfOption Option: "IMX362" Value: 15 { 09 07 0E 0D 00 00 0F }
0x481D9: 			OneOfOption Option: "IMX488" Value: 16 { 09 07 0F 0D 00 00 10 }
0x481E0: 			OneOfOption Option: "OVTI01AS" Value: 17 { 09 07 11 0D 00 00 11 }
0x481E7: 			OneOfOption Option: "OVTI01A0" Value: 18 { 09 07 12 0D 00 00 12 }
0x481EE: 			OneOfOption Option: "OVTI5678" Value: 19 { 09 07 13 0D 00 00 13 }
0x481F5: 			OneOfOption Option: "OVTI9738" Value: 20 { 09 07 14 0D 00 00 14 }
0x481FC: 			OneOfOption Option: "HIMAX11B1" Value: 21 { 09 07 16 0D 00 00 15 }
0x48203: 			OneOfOption Option: "OVTID858" Value: 22 { 09 07 15 0D 00 00 16 }
0x4820A: 			OneOfOption Option: "User Custom" Value: 255 { 09 07 17 0D 00 00 FF }
0x48211: 		End  { 29 02 }
0x48213: 		SuppressIf  { 0A 82 }
0x48215: 			EqIdVal QuestionId: 0x810, Value: 0xFF { 12 86 10 08 FF 00 }
0x4821B: 				Not  { 17 02 }
0x4821D: 			End  { 29 02 }
0x4821F: 			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0x811, VarStoreId: 0xF101, VarStoreInfo: 0x3C5, MinSize: 0x6, MaxSize: 0x14, Flags: 0x0 { 1C 90 A5 10 18 0D 11 08 01 F1 C5 03 00 06 14 00 }
0x4822F: 			End  { 29 02 }
0x48231: 		End  { 29 02 }
0x48233: 		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0x812, VarStoreId: 0xF101, VarOffset: 0xA96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 7B 0B 76 0B 12 08 01 F1 96 0A 10 10 00 07 00 }
0x48244: 			OneOfOption Option: "4 4 2 2" Value: 0, Default { 09 07 7D 0B 10 00 00 }
0x4824B: 			OneOfOption Option: "4 4 3 1" Value: 2 { 09 07 7E 0B 00 00 02 }
0x48252: 			OneOfOption Option: "4 4 4 0" Value: 3 { 09 07 7F 0B 00 00 03 }
0x48259: 			OneOfOption Option: "8 0 2 2" Value: 4 { 09 07 80 0B 00 00 04 }
0x48260: 			OneOfOption Option: "8 0 3 1" Value: 6 { 09 07 81 0B 00 00 06 }
0x48267: 			OneOfOption Option: "8 0 4 0" Value: 7 { 09 07 82 0B 00 00 07 }
0x4826E: 		End  { 29 02 }
0x48270: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x813, VarStoreId: 0xF101, VarOffset: 0x435, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 AE 0C A9 0C 13 08 01 F1 35 04 10 10 10 50 00 }
0x48281: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x48288: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x4828F: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x48296: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x4829D: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x482A4: 		End  { 29 02 }
0x482A6: 		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0x814, VarStoreId: 0xF101, VarOffset: 0x443, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 83 0D 7E 0D 14 08 01 F1 43 04 10 10 00 FF 00 }
0x482B7: 			OneOfOption Option: "No Control Logic" Value: 255, Default { 09 07 28 0D 10 00 FF }
0x482BE: 			OneOfOption Option: "Control Logic 1" Value: 0 { 09 07 22 0D 00 00 00 }
0x482C5: 			OneOfOption Option: "Control Logic 2" Value: 1 { 09 07 23 0D 00 00 01 }
0x482CC: 			OneOfOption Option: "Control Logic 3" Value: 2 { 09 07 24 0D 00 00 02 }
0x482D3: 			OneOfOption Option: "Control Logic 4" Value: 3 { 09 07 25 0D 00 00 03 }
0x482DA: 			SuppressIf  { 0A 82 }
0x482DC: 				EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x482E2: 					Not  { 17 02 }
0x482E4: 				End  { 29 02 }
0x482E6: 				OneOfOption Option: "Control Logic 5" Value: 3 { 09 07 26 0D 00 00 03 }
0x482ED: 			End  { 29 02 }
0x482EF: 			SuppressIf  { 0A 82 }
0x482F1: 				EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x482F7: 					Not  { 17 02 }
0x482F9: 				End  { 29 02 }
0x482FB: 				OneOfOption Option: "Control Logic 6" Value: 3 { 09 07 27 0D 00 00 03 }
0x48302: 			End  { 29 02 }
0x48304: 		End  { 29 02 }
0x48306: 		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0x815, VarStoreId: 0xF101, VarOffset: 0x3ED, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0 { 05 91 64 0C 5F 0C 15 08 01 F1 ED 03 10 10 61 69 00 }
0x48317: 			OneOfOption Option: "Front" Value: 97 { 09 07 6C 0C 00 00 61 }
0x4831E: 			OneOfOption Option: "Back" Value: 105, Default { 09 07 6D 0C 10 00 69 }
0x48325: 		End  { 29 02 }
0x48327: 		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0x816, VarStoreId: 0xF101, VarOffset: 0x444, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 76 0C 71 0C 16 08 01 F1 44 04 10 10 00 03 00 }
0x48338: 			OneOfOption Option: "Driver default" Value: 0, Default { 09 07 78 0C 10 00 00 }
0x4833F: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x48346: 			OneOfOption Option: "Enabled" Value: 3 { 09 07 03 00 00 00 03 }
0x4834D: 		End  { 29 02 }
0x4834F: 		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0x817, VarStoreId: 0xF101, VarOffset: 0x445, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7E 0C 79 0C 17 08 01 F1 45 04 10 10 00 05 00 }
0x48360: 			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault { 09 07 80 0C 30 00 00 }
0x48367: 			OneOfOption Option: "ILEDA, 16mA" Value: 1 { 09 07 81 0C 00 00 01 }
0x4836E: 			OneOfOption Option: "ILEDB, 2mA" Value: 2 { 09 07 82 0C 00 00 02 }
0x48375: 			OneOfOption Option: "ILEDB, 4mA" Value: 3 { 09 07 83 0C 00 00 03 }
0x4837C: 			OneOfOption Option: "ILEDB, 8mA" Value: 4 { 09 07 84 0C 00 00 04 }
0x48383: 			OneOfOption Option: "ILEDB, 16mA" Value: 5 { 09 07 85 0C 00 00 05 }
0x4838A: 		End  { 29 02 }
0x4838C: 		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0x818, VarStoreId: 0xF101, VarOffset: 0x446, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 8B 0C 86 0C 18 08 01 F1 46 04 10 10 00 06 00 }
0x4839D: 			OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 8D 0C 30 00 00 }
0x483A4: 			OneOfOption Option: "90" Value: 2 { 09 07 8E 0C 00 00 02 }
0x483AB: 			OneOfOption Option: "180" Value: 4 { 09 07 8F 0C 00 00 04 }
0x483B2: 			OneOfOption Option: "270" Value: 6 { 09 07 90 0C 00 00 06 }
0x483B9: 		End  { 29 02 }
0x483BB: 		SuppressIf  { 0A 82 }
0x483BD: 			EqIdVal QuestionId: 0x813, Value: 0x50 { 12 86 13 08 50 00 }
0x483C3: 				Not  { 17 02 }
0x483C5: 			End  { 29 02 }
0x483C7: 			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0x819, VarStoreId: 0xF101, VarOffset: 0x447, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 96 0C 91 0C 19 08 01 F1 47 04 10 10 00 01 00 }
0x483D8: 				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault { 09 07 97 0C 30 00 00 }
0x483DF: 				OneOfOption Option: "Position 2" Value: 1 { 09 07 98 0C 00 00 01 }
0x483E6: 			End  { 29 02 }
0x483E8: 		End  { 29 02 }
0x483EA: 		SuppressIf  { 0A 82 }
0x483EC: 			EqIdVal QuestionId: 0x819, Value: 0x1 { 12 86 19 08 01 00 }
0x483F2: 				Not  { 17 02 }
0x483F4: 			End  { 29 02 }
0x483F6: 			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0x81A, VarStoreId: 0xF101, VarOffset: 0x448, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9E 0C 99 0C 1A 08 01 F1 48 04 10 10 00 01 00 }
0x48407: 				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault { 09 07 A0 0C 30 00 00 }
0x4840E: 				OneOfOption Option: "2 voltage rail" Value: 1 { 09 07 A1 0C 00 00 01 }
0x48415: 			End  { 29 02 }
0x48417: 		End  { 29 02 }
0x48419: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x81B, VarStoreId: 0xF101, VarStoreInfo: 0x3EE, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 7F 10 66 0C 1B 08 01 F1 EE 03 00 01 0F 00 }
0x48429: 		End  { 29 02 }
0x4842B: 		Numeric Prompt: "MIPI port", Help: "LinkUsed", QuestionFlags: 0x10, QuestionId: 0x81C, VarStoreId: 0xF101, VarOffset: 0x436, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 BC 0C B7 0C 1C 08 01 F1 36 04 10 10 00 0A 01 }
0x4843C: 			Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x48442: 		End  { 29 02 }
0x48444: 		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0x81D, VarStoreId: 0xF101, VarOffset: 0x437, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 C3 0C BE 0C 1D 08 01 F1 37 04 10 10 01 04 00 }
0x48455: 			OneOfOption Option: "x1" Value: 1 { 09 07 F3 0C 00 00 01 }
0x4845C: 			OneOfOption Option: "x2" Value: 2 { 09 07 F4 0C 00 00 02 }
0x48463: 			OneOfOption Option: "x3" Value: 3 { 09 07 F5 0C 00 00 03 }
0x4846A: 			OneOfOption Option: "x4" Value: 4, Default { 09 07 F6 0C 10 00 04 }
0x48471: 		End  { 29 02 }
0x48473: 		OneOf Prompt: "PortSpeed", Help: "PortSpeed: 0:Sensor Default, 1:<416Mbps, 2:<1.5Gbps, 3:<2Gbps, 4:<2.5Gbps, 5:<4Gbps, 6:>4Gbps", QuestionFlags: 0x10, QuestionId: 0x81E, VarStoreId: 0xF101, VarOffset: 0x438, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 9B 10 C6 0C 1E 08 01 F1 38 04 10 10 00 06 00 }
0x48484: 			OneOfOption Option: "0" Value: 0 { 09 07 F8 0C 00 00 00 }
0x4848B: 			OneOfOption Option: "1" Value: 1 { 09 07 F9 0C 00 00 01 }
0x48492: 			OneOfOption Option: "2" Value: 2, Default { 09 07 FA 0C 10 00 02 }
0x48499: 			OneOfOption Option: "3" Value: 3 { 09 07 FB 0C 00 00 03 }
0x484A0: 			OneOfOption Option: "4" Value: 4 { 09 07 FC 0C 00 00 04 }
0x484A7: 			OneOfOption Option: "5" Value: 5 { 09 07 FD 0C 00 00 05 }
0x484AE: 			OneOfOption Option: "6" Value: 6 { 09 07 FE 0C 00 00 06 }
0x484B5: 		End  { 29 02 }
0x484B7: 		Numeric Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0x81F, VarStoreId: 0xF101, VarOffset: 0x43F, Flags: 0x12, Size: 32, Min: 0x5B8D80, Max: 0x19BFCC0, Step: 0x186A0 { 07 9A A0 10 C7 0C 1F 08 01 F1 3F 04 10 12 80 8D 5B 00 C0 FC 9B 01 A0 86 01 00 }
0x484D1: 			Default DefaultId: 0x0 Value: 19200000 { 5B 09 00 00 02 00 F8 24 01 }
0x484DA: 		End  { 29 02 }
0x484DC: 		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type
0x00: ROM_NONE
0x01: ROM_OTP
0x02: ROM_EEPROM_16K_64
0x03: ROM_EEPROM_16K_16
0x04: ROM_OTP_ACPI_ACPI
0x05: ROM_ACPI
0x06: ROM_EEPROM_BRCA016GWZ
0x07: ROM_EEPROM_24AA32
0x08: ROM_EEPROM_CAT24C08
0x09: ROM_M24C64
0x0A: ROM_DW9806B
0x10: ROM_EEPROM_CAT24C16
0x11: ROM_EEPROM_CAT24C64
0x12: ROM_EEPROM_24AA16", QuestionFlags: 0x10, QuestionId: 0x820, VarStoreId: 0xF101, VarOffset: 0x439, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CE 0C C9 0C 20 08 01 F1 39 04 10 10 00 12 00 }
0x484ED: 			OneOfOption Option: "ROM_NONE" Value: 0, Default { 09 07 D7 0C 10 00 00 }
0x484F4: 			OneOfOption Option: "ROM_OTP" Value: 1 { 09 07 D8 0C 00 00 01 }
0x484FB: 			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2 { 09 07 D9 0C 00 00 02 }
0x48502: 			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3 { 09 07 DA 0C 00 00 03 }
0x48509: 			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4 { 09 07 DB 0C 00 00 04 }
0x48510: 			OneOfOption Option: "ROM_ACPI" Value: 5 { 09 07 DC 0C 00 00 05 }
0x48517: 			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6 { 09 07 DD 0C 00 00 06 }
0x4851E: 			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7 { 09 07 DE 0C 00 00 07 }
0x48525: 			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8 { 09 07 DF 0C 00 00 08 }
0x4852C: 			OneOfOption Option: "ROM_EEPROM_M24C64" Value: 9 { 09 07 E0 0C 00 00 09 }
0x48533: 			OneOfOption Option: "ROM_EEPROM_DW9806B" Value: 10 { 09 07 E1 0C 00 00 0A }
0x4853A: 			OneOfOption Option: "ROM_EEPROM_CAT24C16" Value: 16 { 09 07 E2 0C 00 00 10 }
0x48541: 			OneOfOption Option: "ROM_EEPROM_CAT24C64" Value: 17 { 09 07 E3 0C 00 00 11 }
0x48548: 			OneOfOption Option: "ROM_EEPROM_24AA16" Value: 18 { 09 07 E4 0C 00 00 12 }
0x4854F: 		End  { 29 02 }
0x48551: 		OneOf Prompt: "VCM Type", Help: "VCM Type
0x00: VCM_NONE
0x01: VCM_AD5823
0x02: VCM_DW9714
0x03: VCM_AD5816
0x04: VCM_DW9719
0x05: VCM_DW9718
0x06: VCM_DW9806B
0x07: VCM_WV517S
0x08: VCM_LC898122XA
0x09: VCM_LC898212AXB
0x0F: VCM_AK7371
0x10: VCM_BU64297GWZ", QuestionFlags: 0x10, QuestionId: 0x821, VarStoreId: 0xF101, VarOffset: 0x43A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0 { 05 91 D5 0C D0 0C 21 08 01 F1 3A 04 10 10 00 10 00 }
0x48562: 			OneOfOption Option: "VCM_NONE" Value: 0, Default { 09 07 E5 0C 10 00 00 }
0x48569: 			OneOfOption Option: "VCM_AD5823" Value: 1 { 09 07 E6 0C 00 00 01 }
0x48570: 			OneOfOption Option: "VCM_DW9714" Value: 2 { 09 07 E7 0C 00 00 02 }
0x48577: 			OneOfOption Option: "VCM_AD5816" Value: 3 { 09 07 E8 0C 00 00 03 }
0x4857E: 			OneOfOption Option: "VCM_DW9719" Value: 4 { 09 07 EA 0C 00 00 04 }
0x48585: 			OneOfOption Option: "VCM_DW9718" Value: 5 { 09 07 E9 0C 00 00 05 }
0x4858C: 			OneOfOption Option: "VCM_DW9806B" Value: 6 { 09 07 EB 0C 00 00 06 }
0x48593: 			OneOfOption Option: "VCM_WV517S" Value: 7 { 09 07 EC 0C 00 00 07 }
0x4859A: 			OneOfOption Option: "VCM_LC898122XA" Value: 8 { 09 07 ED 0C 00 00 08 }
0x485A1: 			OneOfOption Option: "VCM_LC898212AXB" Value: 9 { 09 07 EE 0C 00 00 09 }
0x485A8: 			OneOfOption Option: "VCM_RESERVED1" Value: 10 { 09 07 EF 0C 00 00 0A }
0x485AF: 			OneOfOption Option: "VCM_RESERVED2" Value: 11 { 09 07 F0 0C 00 00 0B }
0x485B6: 			OneOfOption Option: "VCM_AK7371" Value: 15 { 09 07 F1 0C 00 00 0F }
0x485BD: 			OneOfOption Option: "VCM_BU64297GWZ" Value: 16 { 09 07 F2 0C 00 00 10 }
0x485C4: 		End  { 29 02 }
0x485C6: 		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0x822, VarStoreId: 0xF101, VarOffset: 0x40E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1 { 07 91 71 0B 6C 0B 22 08 01 F1 0E 04 10 10 00 0C 01 }
0x485D7: 			Default DefaultId: 0x0 Value: 6 { 5B 06 00 00 00 06 }
0x485DD: 		End  { 29 02 }
0x485DF: 		SuppressIf  { 0A 82 }
0x485E1: 			EqIdVal QuestionId: 0x822, Value: 0x0 { 12 06 22 08 00 00 }
0x485E7: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x823, VarStoreId: 0xF101, VarOffset: 0x40F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 94 0B 8F 0B 23 08 01 F1 0F 04 10 10 00 05 00 }
0x485F8: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x485FF: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x48606: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4860D: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x48614: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4861B: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x48622: 			End  { 29 02 }
0x48624: 			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0 { 02 87 83 0B 00 00 00 }
0x4862B: 			End  { 29 02 }
0x4862D: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x824, VarStoreId: 0xF101, VarOffset: 0x410, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 CB 0B 98 0B 24 08 01 F1 10 04 10 21 00 00 7F 00 01 00 }
0x48641: 				Default DefaultId: 0x0 Value: 16 { 5B 07 00 00 01 10 00 }
0x48648: 			End  { 29 02 }
0x4864A: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x825, VarStoreId: 0xF101, VarOffset: 0x428, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 5A 0D 29 0D 25 08 01 F1 28 04 10 10 00 0C 00 }
0x4865B: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x48662: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48669: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48670: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48677: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4867E: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48685: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x4868C: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48693: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4869A: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x486A1: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x486A8: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x486AF: 			End  { 29 02 }
0x486B1: 		End  { 29 02 }
0x486B3: 		SuppressIf  { 0A 82 }
0x486B5: 			EqIdValList QuestionId: 0x822, Values: [0, 1] { 14 0A 22 08 02 00 00 00 01 00 }
0x486BF: 			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0 { 02 87 84 0B 00 00 00 }
0x486C6: 			End  { 29 02 }
0x486C8: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x826, VarStoreId: 0xF101, VarOffset: 0x412, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 CC 0B 98 0B 26 08 01 F1 12 04 10 21 00 00 7F 00 01 00 }
0x486DC: 				Default DefaultId: 0x0 Value: 12 { 5B 07 00 00 01 0C 00 }
0x486E3: 			End  { 29 02 }
0x486E5: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x827, VarStoreId: 0xF101, VarOffset: 0x429, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 5B 0D 29 0D 27 08 01 F1 29 04 10 10 00 0C 00 }
0x486F6: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x486FD: 				OneOfOption Option: "VCM" Value: 1, Default { 09 07 73 0D 10 00 01 }
0x48704: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4870B: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48712: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48719: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48720: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48727: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4872E: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48735: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4873C: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48743: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4874A: 			End  { 29 02 }
0x4874C: 		End  { 29 02 }
0x4874E: 		SuppressIf  { 0A 82 }
0x48750: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2] { 14 0C 22 08 03 00 00 00 01 00 02 00 }
0x4875C: 			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0 { 02 87 85 0B 00 00 00 }
0x48763: 			End  { 29 02 }
0x48765: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x828, VarStoreId: 0xF101, VarOffset: 0x414, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 CD 0B 98 0B 28 08 01 F1 14 04 10 21 00 00 7F 00 01 00 }
0x48779: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x48780: 			End  { 29 02 }
0x48782: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x829, VarStoreId: 0xF101, VarOffset: 0x42A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 5C 0D 29 0D 29 08 01 F1 2A 04 10 10 00 0C 00 }
0x48793: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4879A: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x487A1: 				OneOfOption Option: "EEPROM" Value: 2, Default { 09 07 74 0D 10 00 02 }
0x487A8: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x487AF: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x487B6: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x487BD: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x487C4: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x487CB: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x487D2: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x487D9: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x487E0: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x487E7: 			End  { 29 02 }
0x487E9: 		End  { 29 02 }
0x487EB: 		SuppressIf  { 0A 82 }
0x487ED: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3] { 14 0E 22 08 04 00 00 00 01 00 02 00 03 00 }
0x487FB: 			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0 { 02 87 86 0B 00 00 00 }
0x48802: 			End  { 29 02 }
0x48804: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x82A, VarStoreId: 0xF101, VarOffset: 0x416, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 CE 0B 98 0B 2A 08 01 F1 16 04 10 21 00 00 7F 00 01 00 }
0x48818: 				Default DefaultId: 0x0 Value: 81 { 5B 07 00 00 01 51 00 }
0x4881F: 			End  { 29 02 }
0x48821: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x82B, VarStoreId: 0xF101, VarOffset: 0x42B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 5D 0D 29 0D 2B 08 01 F1 2B 04 10 10 00 0C 00 }
0x48832: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48839: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48840: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48847: 				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default { 09 07 75 0D 10 00 03 }
0x4884E: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48855: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4885C: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48863: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4886A: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48871: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48878: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x4887F: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48886: 			End  { 29 02 }
0x48888: 		End  { 29 02 }
0x4888A: 		SuppressIf  { 0A 82 }
0x4888C: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4] { 14 10 22 08 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4889C: 			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0 { 02 87 87 0B 00 00 00 }
0x488A3: 			End  { 29 02 }
0x488A5: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x82C, VarStoreId: 0xF101, VarOffset: 0x418, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 CF 0B 98 0B 2C 08 01 F1 18 04 10 21 00 00 7F 00 01 00 }
0x488B9: 				Default DefaultId: 0x0 Value: 82 { 5B 07 00 00 01 52 00 }
0x488C0: 			End  { 29 02 }
0x488C2: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x82D, VarStoreId: 0xF101, VarOffset: 0x42C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 5E 0D 29 0D 2D 08 01 F1 2C 04 10 10 00 0C 00 }
0x488D3: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x488DA: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x488E1: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x488E8: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x488EF: 				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default { 09 07 76 0D 10 00 04 }
0x488F6: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x488FD: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48904: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x4890B: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48912: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48919: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48920: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48927: 			End  { 29 02 }
0x48929: 		End  { 29 02 }
0x4892B: 		SuppressIf  { 0A 82 }
0x4892D: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5] { 14 12 22 08 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4893F: 			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0 { 02 87 88 0B 00 00 00 }
0x48946: 			End  { 29 02 }
0x48948: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x82E, VarStoreId: 0xF101, VarOffset: 0x41A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D0 0B 98 0B 2E 08 01 F1 1A 04 10 21 00 00 7F 00 01 00 }
0x4895C: 				Default DefaultId: 0x0 Value: 83 { 5B 07 00 00 01 53 00 }
0x48963: 			End  { 29 02 }
0x48965: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x82F, VarStoreId: 0xF101, VarOffset: 0x42D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 5F 0D 29 0D 2F 08 01 F1 2D 04 10 10 00 0C 00 }
0x48976: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4897D: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48984: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4898B: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48992: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48999: 				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default { 09 07 77 0D 10 00 05 }
0x489A0: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x489A7: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x489AE: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x489B5: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x489BC: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x489C3: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x489CA: 			End  { 29 02 }
0x489CC: 		End  { 29 02 }
0x489CE: 		SuppressIf  { 0A 82 }
0x489D0: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5, 6] { 14 14 22 08 07 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 }
0x489E4: 			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0 { 02 87 89 0B 00 00 00 }
0x489EB: 			End  { 29 02 }
0x489ED: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x830, VarStoreId: 0xF101, VarOffset: 0x41C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D1 0B 98 0B 30 08 01 F1 1C 04 10 21 00 00 7F 00 01 00 }
0x48A01: 				Default DefaultId: 0x0 Value: 84 { 5B 07 00 00 01 54 00 }
0x48A08: 			End  { 29 02 }
0x48A0A: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x831, VarStoreId: 0xF101, VarOffset: 0x42E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 60 0D 29 0D 31 08 01 F1 2E 04 10 10 00 0C 00 }
0x48A1B: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48A22: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48A29: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48A30: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48A37: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48A3E: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48A45: 				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default { 09 07 78 0D 10 00 06 }
0x48A4C: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48A53: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48A5A: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48A61: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48A68: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48A6F: 			End  { 29 02 }
0x48A71: 		End  { 29 02 }
0x48A73: 		SuppressIf  { 0A 82 }
0x48A75: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5, 6, 7] { 14 16 22 08 08 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 }
0x48A8B: 			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0 { 02 87 8A 0B 00 00 00 }
0x48A92: 			End  { 29 02 }
0x48A94: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x832, VarStoreId: 0xF101, VarOffset: 0x41E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D2 0B 98 0B 32 08 01 F1 1E 04 10 21 00 00 7F 00 01 00 }
0x48AA8: 				Default DefaultId: 0x0 Value: 85 { 5B 07 00 00 01 55 00 }
0x48AAF: 			End  { 29 02 }
0x48AB1: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x833, VarStoreId: 0xF101, VarOffset: 0x42F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 61 0D 29 0D 33 08 01 F1 2F 04 10 10 00 0C 00 }
0x48AC2: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48AC9: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48AD0: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48AD7: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48ADE: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48AE5: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48AEC: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48AF3: 				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default { 09 07 79 0D 10 00 07 }
0x48AFA: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48B01: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48B08: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48B0F: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48B16: 			End  { 29 02 }
0x48B18: 		End  { 29 02 }
0x48B1A: 		SuppressIf  { 0A 82 }
0x48B1C: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8] { 14 18 22 08 09 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x48B34: 			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0 { 02 87 8B 0B 00 00 00 }
0x48B3B: 			End  { 29 02 }
0x48B3D: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x834, VarStoreId: 0xF101, VarOffset: 0x420, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D3 0B 98 0B 34 08 01 F1 20 04 10 21 00 00 7F 00 01 00 }
0x48B51: 				Default DefaultId: 0x0 Value: 86 { 5B 07 00 00 01 56 00 }
0x48B58: 			End  { 29 02 }
0x48B5A: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x835, VarStoreId: 0xF101, VarOffset: 0x430, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 62 0D 29 0D 35 08 01 F1 30 04 10 10 00 0C 00 }
0x48B6B: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48B72: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48B79: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48B80: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48B87: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48B8E: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48B95: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48B9C: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48BA3: 				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default { 09 07 7A 0D 10 00 08 }
0x48BAA: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48BB1: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48BB8: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48BBF: 			End  { 29 02 }
0x48BC1: 		End  { 29 02 }
0x48BC3: 		SuppressIf  { 0A 82 }
0x48BC5: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9] { 14 1A 22 08 0A 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 }
0x48BDF: 			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0 { 02 87 8C 0B 00 00 00 }
0x48BE6: 			End  { 29 02 }
0x48BE8: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x836, VarStoreId: 0xF101, VarOffset: 0x422, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D4 0B 98 0B 36 08 01 F1 22 04 10 21 00 00 7F 00 01 00 }
0x48BFC: 				Default DefaultId: 0x0 Value: 87 { 5B 07 00 00 01 57 00 }
0x48C03: 			End  { 29 02 }
0x48C05: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x837, VarStoreId: 0xF101, VarOffset: 0x431, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 63 0D 29 0D 37 08 01 F1 31 04 10 10 00 0C 00 }
0x48C16: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48C1D: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48C24: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48C2B: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48C32: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48C39: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48C40: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48C47: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48C4E: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48C55: 				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default { 09 07 7B 0D 10 00 09 }
0x48C5C: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48C63: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48C6A: 			End  { 29 02 }
0x48C6C: 		End  { 29 02 }
0x48C6E: 		SuppressIf  { 0A 82 }
0x48C70: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10] { 14 1C 22 08 0B 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 }
0x48C8C: 			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0 { 02 87 8D 0B 00 00 00 }
0x48C93: 			End  { 29 02 }
0x48C95: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x838, VarStoreId: 0xF101, VarOffset: 0x424, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D5 0B 98 0B 38 08 01 F1 24 04 10 21 00 00 7F 00 01 00 }
0x48CA9: 				Default DefaultId: 0x0 Value: 88 { 5B 07 00 00 01 58 00 }
0x48CB0: 			End  { 29 02 }
0x48CB2: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x839, VarStoreId: 0xF101, VarOffset: 0x432, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 64 0D 29 0D 39 08 01 F1 32 04 10 10 00 0C 00 }
0x48CC3: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48CCA: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48CD1: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48CD8: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48CDF: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48CE6: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48CED: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48CF4: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48CFB: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48D02: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48D09: 				OneOfOption Option: "IO Expander" Value: 10, Default { 09 07 7C 0D 10 00 0A }
0x48D10: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x48D17: 			End  { 29 02 }
0x48D19: 		End  { 29 02 }
0x48D1B: 		SuppressIf  { 0A 82 }
0x48D1D: 			EqIdValList QuestionId: 0x822, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11] { 14 1E 22 08 0C 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 0B 00 }
0x48D3B: 			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0 { 02 87 8E 0B 00 00 00 }
0x48D42: 			End  { 29 02 }
0x48D44: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x83A, VarStoreId: 0xF101, VarOffset: 0x426, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D6 0B 98 0B 3A 08 01 F1 26 04 10 21 00 00 7F 00 01 00 }
0x48D58: 				Default DefaultId: 0x0 Value: 89 { 5B 07 00 00 01 59 00 }
0x48D5F: 			End  { 29 02 }
0x48D61: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x83B, VarStoreId: 0xF101, VarOffset: 0x433, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 65 0D 29 0D 3B 08 01 F1 33 04 10 10 00 0C 00 }
0x48D72: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x48D79: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x48D80: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x48D87: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x48D8E: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x48D95: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x48D9C: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x48DA3: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x48DAA: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x48DB1: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x48DB8: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x48DBF: 				OneOfOption Option: "Flash" Value: 12, Default { 09 07 7D 0D 10 00 0C }
0x48DC6: 			End  { 29 02 }
0x48DC8: 		End  { 29 02 }
0x48DCA: 		OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x83C, VarStoreId: 0xF101, VarOffset: 0x44B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 91 10 A2 0C 3C 08 01 F1 4B 04 10 10 00 02 00 }
0x48DDB: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 A4 0C 30 00 00 }
0x48DE2: 			OneOfOption Option: "External" Value: 1 { 09 07 A5 0C 00 00 01 }
0x48DE9: 			OneOfOption Option: "Internal PMIC" Value: 2 { 09 07 A6 0C 00 00 02 }
0x48DF0: 		End  { 29 02 }
0x48DF2: 		SuppressIf  { 0A 82 }
0x48DF4: 			EqIdVal QuestionId: 0x83C, Value: 0x1 { 12 86 3C 08 01 00 }
0x48DFA: 				Not  { 17 02 }
0x48DFC: 			End  { 29 02 }
0x48DFE: 			OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x83D, VarStoreId: 0xF101, VarOffset: 0xAFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 92 10 A7 0C 3D 08 01 F1 FA 0A 10 10 00 05 00 }
0x48E0F: 				OneOfOption Option: "Flash1" Value: 0, Default, MfgDefault { 09 07 9A 0D 30 00 00 }
0x48E16: 				OneOfOption Option: "Flash2" Value: 1 { 09 07 9B 0D 00 00 01 }
0x48E1D: 				OneOfOption Option: "Flash3" Value: 2 { 09 07 9C 0D 00 00 02 }
0x48E24: 				OneOfOption Option: "Flash4" Value: 3 { 09 07 9D 0D 00 00 03 }
0x48E2B: 				OneOfOption Option: "Flash5" Value: 4 { 09 07 9E 0D 00 00 04 }
0x48E32: 				OneOfOption Option: "Flash6" Value: 5 { 09 07 9F 0D 00 00 05 }
0x48E39: 			End  { 29 02 }
0x48E3B: 		End  { 29 02 }
0x48E3D: 	End  { 29 02 }
0x48E3F: 	Form FormId: 0x92, Title: "Link5 options" { 01 86 92 00 64 0B }
0x48E45: 		Subtitle Prompt: "Camera6", Help: "", Flags: 0x0 { 02 87 52 0B 00 00 00 }
0x48E4C: 		End  { 29 02 }
0x48E4E: 		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0x83E, VarStoreId: 0xF101, VarOffset: 0x44C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 6B 0B 65 0B 3E 08 01 F1 4C 04 10 10 00 FF 00 }
0x48E5F: 			OneOfOption Option: "IMX135" Value: 0 { 09 07 FF 0C 00 00 00 }
0x48E66: 			OneOfOption Option: "OV5693" Value: 1, Default { 09 07 00 0D 10 00 01 }
0x48E6D: 			OneOfOption Option: "IMX179" Value: 2 { 09 07 01 0D 00 00 02 }
0x48E74: 			OneOfOption Option: "OV8858" Value: 3 { 09 07 02 0D 00 00 03 }
0x48E7B: 			OneOfOption Option: "OV2740-IVCAM" Value: 4 { 09 07 03 0D 00 00 04 }
0x48E82: 			OneOfOption Option: "OV9728" Value: 5 { 09 07 04 0D 00 00 05 }
0x48E89: 			OneOfOption Option: "IMX188" Value: 6 { 09 07 05 0D 00 00 06 }
0x48E90: 			OneOfOption Option: "IMX208" Value: 7 { 09 07 06 0D 00 00 07 }
0x48E97: 			OneOfOption Option: "OV5670" Value: 8 { 09 07 07 0D 00 00 08 }
0x48E9E: 			OneOfOption Option: "OV8865" Value: 9 { 09 07 08 0D 00 00 09 }
0x48EA5: 			OneOfOption Option: "HM2051" Value: 10 { 09 07 09 0D 00 00 0A }
0x48EAC: 			OneOfOption Option: "OV2742" Value: 11 { 09 07 0A 0D 00 00 0B }
0x48EB3: 			OneOfOption Option: "OV9234" Value: 12 { 09 07 0B 0D 00 00 0C }
0x48EBA: 			OneOfOption Option: "OV8856" Value: 13 { 09 07 0C 0D 00 00 0D }
0x48EC1: 			OneOfOption Option: "OV16860" Value: 14 { 09 07 0D 0D 00 00 0E }
0x48EC8: 			OneOfOption Option: "IMX362" Value: 15 { 09 07 0E 0D 00 00 0F }
0x48ECF: 			OneOfOption Option: "IMX488" Value: 16 { 09 07 0F 0D 00 00 10 }
0x48ED6: 			OneOfOption Option: "OVTI01AS" Value: 17 { 09 07 11 0D 00 00 11 }
0x48EDD: 			OneOfOption Option: "OVTI01A0" Value: 18 { 09 07 12 0D 00 00 12 }
0x48EE4: 			OneOfOption Option: "OVTI5678" Value: 19 { 09 07 13 0D 00 00 13 }
0x48EEB: 			OneOfOption Option: "OVTI9738" Value: 20 { 09 07 14 0D 00 00 14 }
0x48EF2: 			OneOfOption Option: "HIMAX11B1" Value: 21 { 09 07 16 0D 00 00 15 }
0x48EF9: 			OneOfOption Option: "OVTID858" Value: 22 { 09 07 15 0D 00 00 16 }
0x48F00: 			OneOfOption Option: "User Custom" Value: 255 { 09 07 17 0D 00 00 FF }
0x48F07: 		End  { 29 02 }
0x48F09: 		SuppressIf  { 0A 82 }
0x48F0B: 			EqIdVal QuestionId: 0x83E, Value: 0xFF { 12 86 3E 08 FF 00 }
0x48F11: 				Not  { 17 02 }
0x48F13: 			End  { 29 02 }
0x48F15: 			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0x83F, VarStoreId: 0xF101, VarStoreInfo: 0x44D, MinSize: 0x6, MaxSize: 0x14, Flags: 0x0 { 1C 90 A6 10 18 0D 3F 08 01 F1 4D 04 00 06 14 00 }
0x48F25: 			End  { 29 02 }
0x48F27: 		End  { 29 02 }
0x48F29: 		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0x840, VarStoreId: 0xF101, VarOffset: 0xA97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 7C 0B 76 0B 40 08 01 F1 97 0A 10 10 00 07 00 }
0x48F3A: 			OneOfOption Option: "4 4 2 2" Value: 0, Default { 09 07 7D 0B 10 00 00 }
0x48F41: 			OneOfOption Option: "4 4 3 1" Value: 2 { 09 07 7E 0B 00 00 02 }
0x48F48: 			OneOfOption Option: "4 4 4 0" Value: 3 { 09 07 7F 0B 00 00 03 }
0x48F4F: 			OneOfOption Option: "8 0 2 2" Value: 4 { 09 07 80 0B 00 00 04 }
0x48F56: 			OneOfOption Option: "8 0 3 1" Value: 6 { 09 07 81 0B 00 00 06 }
0x48F5D: 			OneOfOption Option: "8 0 4 0" Value: 7 { 09 07 82 0B 00 00 07 }
0x48F64: 		End  { 29 02 }
0x48F66: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x841, VarStoreId: 0xF101, VarOffset: 0x4BD, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 AF 0C A9 0C 41 08 01 F1 BD 04 10 10 10 50 00 }
0x48F77: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x48F7E: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x48F85: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x48F8C: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x48F93: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x48F9A: 		End  { 29 02 }
0x48F9C: 		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0x842, VarStoreId: 0xF101, VarOffset: 0x4CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 84 0D 7E 0D 42 08 01 F1 CB 04 10 10 00 FF 00 }
0x48FAD: 			OneOfOption Option: "No Control Logic" Value: 255, Default { 09 07 28 0D 10 00 FF }
0x48FB4: 			OneOfOption Option: "Control Logic 1" Value: 0 { 09 07 22 0D 00 00 00 }
0x48FBB: 			OneOfOption Option: "Control Logic 2" Value: 1 { 09 07 23 0D 00 00 01 }
0x48FC2: 			OneOfOption Option: "Control Logic 3" Value: 2 { 09 07 24 0D 00 00 02 }
0x48FC9: 			OneOfOption Option: "Control Logic 4" Value: 3 { 09 07 25 0D 00 00 03 }
0x48FD0: 			SuppressIf  { 0A 82 }
0x48FD2: 				EqIdVal QuestionId: 0x116A, Value: 0x1 { 12 86 6A 11 01 00 }
0x48FD8: 					Not  { 17 02 }
0x48FDA: 				End  { 29 02 }
0x48FDC: 				OneOfOption Option: "Control Logic 5" Value: 3 { 09 07 26 0D 00 00 03 }
0x48FE3: 			End  { 29 02 }
0x48FE5: 			SuppressIf  { 0A 82 }
0x48FE7: 				EqIdVal QuestionId: 0x1169, Value: 0x1 { 12 86 69 11 01 00 }
0x48FED: 					Not  { 17 02 }
0x48FEF: 				End  { 29 02 }
0x48FF1: 				OneOfOption Option: "Control Logic 6" Value: 3 { 09 07 27 0D 00 00 03 }
0x48FF8: 			End  { 29 02 }
0x48FFA: 		End  { 29 02 }
0x48FFC: 		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0x843, VarStoreId: 0xF101, VarOffset: 0x475, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0 { 05 91 65 0C 5F 0C 43 08 01 F1 75 04 10 10 61 69 00 }
0x4900D: 			OneOfOption Option: "Front" Value: 97 { 09 07 6C 0C 00 00 61 }
0x49014: 			OneOfOption Option: "Back" Value: 105, Default { 09 07 6D 0C 10 00 69 }
0x4901B: 		End  { 29 02 }
0x4901D: 		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0x844, VarStoreId: 0xF101, VarOffset: 0x4CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 77 0C 71 0C 44 08 01 F1 CC 04 10 10 00 03 00 }
0x4902E: 			OneOfOption Option: "Driver default" Value: 0, Default { 09 07 78 0C 10 00 00 }
0x49035: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x4903C: 			OneOfOption Option: "Enabled" Value: 3 { 09 07 03 00 00 00 03 }
0x49043: 		End  { 29 02 }
0x49045: 		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0x845, VarStoreId: 0xF101, VarOffset: 0x4CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7F 0C 79 0C 45 08 01 F1 CD 04 10 10 00 05 00 }
0x49056: 			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault { 09 07 80 0C 30 00 00 }
0x4905D: 			OneOfOption Option: "ILEDA, 16mA" Value: 1 { 09 07 81 0C 00 00 01 }
0x49064: 			OneOfOption Option: "ILEDB, 2mA" Value: 2 { 09 07 82 0C 00 00 02 }
0x4906B: 			OneOfOption Option: "ILEDB, 4mA" Value: 3 { 09 07 83 0C 00 00 03 }
0x49072: 			OneOfOption Option: "ILEDB, 8mA" Value: 4 { 09 07 84 0C 00 00 04 }
0x49079: 			OneOfOption Option: "ILEDB, 16mA" Value: 5 { 09 07 85 0C 00 00 05 }
0x49080: 		End  { 29 02 }
0x49082: 		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0x846, VarStoreId: 0xF101, VarOffset: 0x4CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 8C 0C 86 0C 46 08 01 F1 CE 04 10 10 00 06 00 }
0x49093: 			OneOfOption Option: "0" Value: 0, Default, MfgDefault { 09 07 8D 0C 30 00 00 }
0x4909A: 			OneOfOption Option: "90" Value: 2 { 09 07 8E 0C 00 00 02 }
0x490A1: 			OneOfOption Option: "180" Value: 4 { 09 07 8F 0C 00 00 04 }
0x490A8: 			OneOfOption Option: "270" Value: 6 { 09 07 90 0C 00 00 06 }
0x490AF: 		End  { 29 02 }
0x490B1: 		SuppressIf  { 0A 82 }
0x490B3: 			EqIdVal QuestionId: 0x841, Value: 0x50 { 12 86 41 08 50 00 }
0x490B9: 				Not  { 17 02 }
0x490BB: 			End  { 29 02 }
0x490BD: 			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0x847, VarStoreId: 0xF101, VarOffset: 0x4CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 10 91 0C 47 08 01 F1 CF 04 10 10 00 01 00 }
0x490CE: 				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault { 09 07 97 0C 30 00 00 }
0x490D5: 				OneOfOption Option: "Position 2" Value: 1 { 09 07 98 0C 00 00 01 }
0x490DC: 			End  { 29 02 }
0x490DE: 		End  { 29 02 }
0x490E0: 		SuppressIf  { 0A 82 }
0x490E2: 			EqIdVal QuestionId: 0x847, Value: 0x1 { 12 86 47 08 01 00 }
0x490E8: 				Not  { 17 02 }
0x490EA: 			End  { 29 02 }
0x490EC: 			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0x848, VarStoreId: 0xF101, VarOffset: 0x4D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 0C 99 0C 48 08 01 F1 D0 04 10 10 00 01 00 }
0x490FD: 				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault { 09 07 A0 0C 30 00 00 }
0x49104: 				OneOfOption Option: "2 voltage rail" Value: 1 { 09 07 A1 0C 00 00 01 }
0x4910B: 			End  { 29 02 }
0x4910D: 		End  { 29 02 }
0x4910F: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x849, VarStoreId: 0xF101, VarStoreInfo: 0x476, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 80 10 66 0C 49 08 01 F1 76 04 00 01 0F 00 }
0x4911F: 		End  { 29 02 }
0x49121: 		Numeric Prompt: "MIPI port", Help: "LinkUsed", QuestionFlags: 0x10, QuestionId: 0x84A, VarStoreId: 0xF101, VarOffset: 0x4BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 BD 0C B7 0C 4A 08 01 F1 BE 04 10 10 00 0A 01 }
0x49132: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x49138: 		End  { 29 02 }
0x4913A: 		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0x84B, VarStoreId: 0xF101, VarOffset: 0x4BF, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 C4 0C BE 0C 4B 08 01 F1 BF 04 10 10 01 04 00 }
0x4914B: 			OneOfOption Option: "x1" Value: 1 { 09 07 F3 0C 00 00 01 }
0x49152: 			OneOfOption Option: "x2" Value: 2 { 09 07 F4 0C 00 00 02 }
0x49159: 			OneOfOption Option: "x3" Value: 3 { 09 07 F5 0C 00 00 03 }
0x49160: 			OneOfOption Option: "x4" Value: 4, Default { 09 07 F6 0C 10 00 04 }
0x49167: 		End  { 29 02 }
0x49169: 		OneOf Prompt: "PortSpeed", Help: "PortSpeed: 0:Sensor Default, 1:<416Mbps, 2:<1.5Gbps, 3:<2Gbps, 4:<2.5Gbps, 5:<4Gbps, 6:>4Gbps", QuestionFlags: 0x10, QuestionId: 0x84C, VarStoreId: 0xF101, VarOffset: 0x4C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 9C 10 C6 0C 4C 08 01 F1 C0 04 10 10 00 06 00 }
0x4917A: 			OneOfOption Option: "0" Value: 0 { 09 07 F8 0C 00 00 00 }
0x49181: 			OneOfOption Option: "1" Value: 1 { 09 07 F9 0C 00 00 01 }
0x49188: 			OneOfOption Option: "2" Value: 2, Default { 09 07 FA 0C 10 00 02 }
0x4918F: 			OneOfOption Option: "3" Value: 3 { 09 07 FB 0C 00 00 03 }
0x49196: 			OneOfOption Option: "4" Value: 4 { 09 07 FC 0C 00 00 04 }
0x4919D: 			OneOfOption Option: "5" Value: 5 { 09 07 FD 0C 00 00 05 }
0x491A4: 			OneOfOption Option: "6" Value: 6 { 09 07 FE 0C 00 00 06 }
0x491AB: 		End  { 29 02 }
0x491AD: 		Numeric Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0x84D, VarStoreId: 0xF101, VarOffset: 0x4C7, Flags: 0x12, Size: 32, Min: 0x5B8D80, Max: 0x19BFCC0, Step: 0x186A0 { 07 9A A1 10 C7 0C 4D 08 01 F1 C7 04 10 12 80 8D 5B 00 C0 FC 9B 01 A0 86 01 00 }
0x491C7: 			Default DefaultId: 0x0 Value: 19200000 { 5B 09 00 00 02 00 F8 24 01 }
0x491D0: 		End  { 29 02 }
0x491D2: 		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type
0x00: ROM_NONE
0x01: ROM_OTP
0x02: ROM_EEPROM_16K_64
0x03: ROM_EEPROM_16K_16
0x04: ROM_OTP_ACPI_ACPI
0x05: ROM_ACPI
0x06: ROM_EEPROM_BRCA016GWZ
0x07: ROM_EEPROM_24AA32
0x08: ROM_EEPROM_CAT24C08
0x09: ROM_M24C64
0x0A: ROM_DW9806B
0x10: ROM_EEPROM_CAT24C16
0x11: ROM_EEPROM_CAT24C64
0x12: ROM_EEPROM_24AA16", QuestionFlags: 0x10, QuestionId: 0x84E, VarStoreId: 0xF101, VarOffset: 0x4C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CF 0C C9 0C 4E 08 01 F1 C1 04 10 10 00 12 00 }
0x491E3: 			OneOfOption Option: "ROM_NONE" Value: 0, Default { 09 07 D7 0C 10 00 00 }
0x491EA: 			OneOfOption Option: "ROM_OTP" Value: 1 { 09 07 D8 0C 00 00 01 }
0x491F1: 			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2 { 09 07 D9 0C 00 00 02 }
0x491F8: 			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3 { 09 07 DA 0C 00 00 03 }
0x491FF: 			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4 { 09 07 DB 0C 00 00 04 }
0x49206: 			OneOfOption Option: "ROM_ACPI" Value: 5 { 09 07 DC 0C 00 00 05 }
0x4920D: 			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6 { 09 07 DD 0C 00 00 06 }
0x49214: 			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7 { 09 07 DE 0C 00 00 07 }
0x4921B: 			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8 { 09 07 DF 0C 00 00 08 }
0x49222: 			OneOfOption Option: "ROM_EEPROM_M24C64" Value: 9 { 09 07 E0 0C 00 00 09 }
0x49229: 			OneOfOption Option: "ROM_EEPROM_DW9806B" Value: 10 { 09 07 E1 0C 00 00 0A }
0x49230: 			OneOfOption Option: "ROM_EEPROM_CAT24C16" Value: 16 { 09 07 E2 0C 00 00 10 }
0x49237: 			OneOfOption Option: "ROM_EEPROM_CAT24C64" Value: 17 { 09 07 E3 0C 00 00 11 }
0x4923E: 			OneOfOption Option: "ROM_EEPROM_24AA16" Value: 18 { 09 07 E4 0C 00 00 12 }
0x49245: 		End  { 29 02 }
0x49247: 		OneOf Prompt: "VCM Type", Help: "VCM Type
0x00: VCM_NONE
0x01: VCM_AD5823
0x02: VCM_DW9714
0x03: VCM_AD5816
0x04: VCM_DW9719
0x05: VCM_DW9718
0x06: VCM_DW9806B
0x07: VCM_WV517S
0x08: VCM_LC898122XA
0x09: VCM_LC898212AXB
0x0F: VCM_AK7371
0x10: VCM_BU64297GWZ", QuestionFlags: 0x10, QuestionId: 0x84F, VarStoreId: 0xF101, VarOffset: 0x4C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0 { 05 91 D6 0C D0 0C 4F 08 01 F1 C2 04 10 10 00 10 00 }
0x49258: 			OneOfOption Option: "VCM_NONE" Value: 0, Default { 09 07 E5 0C 10 00 00 }
0x4925F: 			OneOfOption Option: "VCM_AD5823" Value: 1 { 09 07 E6 0C 00 00 01 }
0x49266: 			OneOfOption Option: "VCM_DW9714" Value: 2 { 09 07 E7 0C 00 00 02 }
0x4926D: 			OneOfOption Option: "VCM_AD5816" Value: 3 { 09 07 E8 0C 00 00 03 }
0x49274: 			OneOfOption Option: "VCM_DW9719" Value: 4 { 09 07 EA 0C 00 00 04 }
0x4927B: 			OneOfOption Option: "VCM_DW9718" Value: 5 { 09 07 E9 0C 00 00 05 }
0x49282: 			OneOfOption Option: "VCM_DW9806B" Value: 6 { 09 07 EB 0C 00 00 06 }
0x49289: 			OneOfOption Option: "VCM_WV517S" Value: 7 { 09 07 EC 0C 00 00 07 }
0x49290: 			OneOfOption Option: "VCM_LC898122XA" Value: 8 { 09 07 ED 0C 00 00 08 }
0x49297: 			OneOfOption Option: "VCM_LC898212AXB" Value: 9 { 09 07 EE 0C 00 00 09 }
0x4929E: 			OneOfOption Option: "VCM_RESERVED1" Value: 10 { 09 07 EF 0C 00 00 0A }
0x492A5: 			OneOfOption Option: "VCM_RESERVED2" Value: 11 { 09 07 F0 0C 00 00 0B }
0x492AC: 			OneOfOption Option: "VCM_AK7371" Value: 15 { 09 07 F1 0C 00 00 0F }
0x492B3: 			OneOfOption Option: "VCM_BU64297GWZ" Value: 16 { 09 07 F2 0C 00 00 10 }
0x492BA: 		End  { 29 02 }
0x492BC: 		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0x850, VarStoreId: 0xF101, VarOffset: 0x496, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1 { 07 91 72 0B 6C 0B 50 08 01 F1 96 04 10 10 00 0C 01 }
0x492CD: 			Default DefaultId: 0x0 Value: 6 { 5B 06 00 00 00 06 }
0x492D3: 		End  { 29 02 }
0x492D5: 		SuppressIf  { 0A 82 }
0x492D7: 			EqIdVal QuestionId: 0x850, Value: 0x0 { 12 06 50 08 00 00 }
0x492DD: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x851, VarStoreId: 0xF101, VarOffset: 0x497, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 95 0B 8F 0B 51 08 01 F1 97 04 10 10 00 05 00 }
0x492EE: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x492F5: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x492FC: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x49303: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4930A: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x49311: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x49318: 			End  { 29 02 }
0x4931A: 			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0 { 02 87 83 0B 00 00 00 }
0x49321: 			End  { 29 02 }
0x49323: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x852, VarStoreId: 0xF101, VarOffset: 0x498, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D7 0B 98 0B 52 08 01 F1 98 04 10 21 00 00 7F 00 01 00 }
0x49337: 				Default DefaultId: 0x0 Value: 16 { 5B 07 00 00 01 10 00 }
0x4933E: 			End  { 29 02 }
0x49340: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x853, VarStoreId: 0xF101, VarOffset: 0x4B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 66 0D 29 0D 53 08 01 F1 B0 04 10 10 00 0C 00 }
0x49351: 				OneOfOption Option: "Sensor" Value: 0, Default { 09 07 72 0D 10 00 00 }
0x49358: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4935F: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49366: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4936D: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x49374: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4937B: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x49382: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49389: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x49390: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x49397: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x4939E: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x493A5: 			End  { 29 02 }
0x493A7: 		End  { 29 02 }
0x493A9: 		SuppressIf  { 0A 82 }
0x493AB: 			EqIdValList QuestionId: 0x850, Values: [0, 1] { 14 0A 50 08 02 00 00 00 01 00 }
0x493B5: 			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0 { 02 87 84 0B 00 00 00 }
0x493BC: 			End  { 29 02 }
0x493BE: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x854, VarStoreId: 0xF101, VarOffset: 0x49A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D8 0B 98 0B 54 08 01 F1 9A 04 10 21 00 00 7F 00 01 00 }
0x493D2: 				Default DefaultId: 0x0 Value: 12 { 5B 07 00 00 01 0C 00 }
0x493D9: 			End  { 29 02 }
0x493DB: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x855, VarStoreId: 0xF101, VarOffset: 0x4B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 67 0D 29 0D 55 08 01 F1 B1 04 10 10 00 0C 00 }
0x493EC: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x493F3: 				OneOfOption Option: "VCM" Value: 1, Default { 09 07 73 0D 10 00 01 }
0x493FA: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49401: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x49408: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4940F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x49416: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x4941D: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49424: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4942B: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x49432: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x49439: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x49440: 			End  { 29 02 }
0x49442: 		End  { 29 02 }
0x49444: 		SuppressIf  { 0A 82 }
0x49446: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2] { 14 0C 50 08 03 00 00 00 01 00 02 00 }
0x49452: 			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0 { 02 87 85 0B 00 00 00 }
0x49459: 			End  { 29 02 }
0x4945B: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x856, VarStoreId: 0xF101, VarOffset: 0x49C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 D9 0B 98 0B 56 08 01 F1 9C 04 10 21 00 00 7F 00 01 00 }
0x4946F: 				Default DefaultId: 0x0 Value: 80 { 5B 07 00 00 01 50 00 }
0x49476: 			End  { 29 02 }
0x49478: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x857, VarStoreId: 0xF101, VarOffset: 0x4B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 68 0D 29 0D 57 08 01 F1 B2 04 10 10 00 0C 00 }
0x49489: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x49490: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x49497: 				OneOfOption Option: "EEPROM" Value: 2, Default { 09 07 74 0D 10 00 02 }
0x4949E: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x494A5: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x494AC: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x494B3: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x494BA: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x494C1: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x494C8: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x494CF: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x494D6: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x494DD: 			End  { 29 02 }
0x494DF: 		End  { 29 02 }
0x494E1: 		SuppressIf  { 0A 82 }
0x494E3: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3] { 14 0E 50 08 04 00 00 00 01 00 02 00 03 00 }
0x494F1: 			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0 { 02 87 86 0B 00 00 00 }
0x494F8: 			End  { 29 02 }
0x494FA: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x858, VarStoreId: 0xF101, VarOffset: 0x49E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 DA 0B 98 0B 58 08 01 F1 9E 04 10 21 00 00 7F 00 01 00 }
0x4950E: 				Default DefaultId: 0x0 Value: 81 { 5B 07 00 00 01 51 00 }
0x49515: 			End  { 29 02 }
0x49517: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x859, VarStoreId: 0xF101, VarOffset: 0x4B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 69 0D 29 0D 59 08 01 F1 B3 04 10 10 00 0C 00 }
0x49528: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x4952F: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x49536: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x4953D: 				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default { 09 07 75 0D 10 00 03 }
0x49544: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4954B: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x49552: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x49559: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49560: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x49567: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4956E: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x49575: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4957C: 			End  { 29 02 }
0x4957E: 		End  { 29 02 }
0x49580: 		SuppressIf  { 0A 82 }
0x49582: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4] { 14 10 50 08 05 00 00 00 01 00 02 00 03 00 04 00 }
0x49592: 			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0 { 02 87 87 0B 00 00 00 }
0x49599: 			End  { 29 02 }
0x4959B: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x85A, VarStoreId: 0xF101, VarOffset: 0x4A0, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 DB 0B 98 0B 5A 08 01 F1 A0 04 10 21 00 00 7F 00 01 00 }
0x495AF: 				Default DefaultId: 0x0 Value: 82 { 5B 07 00 00 01 52 00 }
0x495B6: 			End  { 29 02 }
0x495B8: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x85B, VarStoreId: 0xF101, VarOffset: 0x4B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 6A 0D 29 0D 5B 08 01 F1 B4 04 10 10 00 0C 00 }
0x495C9: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x495D0: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x495D7: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x495DE: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x495E5: 				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default { 09 07 76 0D 10 00 04 }
0x495EC: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x495F3: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x495FA: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49601: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x49608: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x4960F: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x49616: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4961D: 			End  { 29 02 }
0x4961F: 		End  { 29 02 }
0x49621: 		SuppressIf  { 0A 82 }
0x49623: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5] { 14 12 50 08 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x49635: 			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0 { 02 87 88 0B 00 00 00 }
0x4963C: 			End  { 29 02 }
0x4963E: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x85C, VarStoreId: 0xF101, VarOffset: 0x4A2, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 DC 0B 98 0B 5C 08 01 F1 A2 04 10 21 00 00 7F 00 01 00 }
0x49652: 				Default DefaultId: 0x0 Value: 83 { 5B 07 00 00 01 53 00 }
0x49659: 			End  { 29 02 }
0x4965B: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x85D, VarStoreId: 0xF101, VarOffset: 0x4B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 6B 0D 29 0D 5D 08 01 F1 B5 04 10 10 00 0C 00 }
0x4966C: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x49673: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4967A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49681: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x49688: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4968F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default { 09 07 77 0D 10 00 05 }
0x49696: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x4969D: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x496A4: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x496AB: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x496B2: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x496B9: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x496C0: 			End  { 29 02 }
0x496C2: 		End  { 29 02 }
0x496C4: 		SuppressIf  { 0A 82 }
0x496C6: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5, 6] { 14 14 50 08 07 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 }
0x496DA: 			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0 { 02 87 89 0B 00 00 00 }
0x496E1: 			End  { 29 02 }
0x496E3: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x85E, VarStoreId: 0xF101, VarOffset: 0x4A4, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 DD 0B 98 0B 5E 08 01 F1 A4 04 10 21 00 00 7F 00 01 00 }
0x496F7: 				Default DefaultId: 0x0 Value: 84 { 5B 07 00 00 01 54 00 }
0x496FE: 			End  { 29 02 }
0x49700: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x85F, VarStoreId: 0xF101, VarOffset: 0x4B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 6C 0D 29 0D 5F 08 01 F1 B6 04 10 10 00 0C 00 }
0x49711: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x49718: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4971F: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49726: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4972D: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x49734: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4973B: 				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default { 09 07 78 0D 10 00 06 }
0x49742: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49749: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x49750: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x49757: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x4975E: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x49765: 			End  { 29 02 }
0x49767: 		End  { 29 02 }
0x49769: 		SuppressIf  { 0A 82 }
0x4976B: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5, 6, 7] { 14 16 50 08 08 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 }
0x49781: 			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0 { 02 87 8A 0B 00 00 00 }
0x49788: 			End  { 29 02 }
0x4978A: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x860, VarStoreId: 0xF101, VarOffset: 0x4A6, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 DE 0B 98 0B 60 08 01 F1 A6 04 10 21 00 00 7F 00 01 00 }
0x4979E: 				Default DefaultId: 0x0 Value: 85 { 5B 07 00 00 01 55 00 }
0x497A5: 			End  { 29 02 }
0x497A7: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x861, VarStoreId: 0xF101, VarOffset: 0x4B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 6D 0D 29 0D 61 08 01 F1 B7 04 10 10 00 0C 00 }
0x497B8: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x497BF: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x497C6: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x497CD: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x497D4: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x497DB: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x497E2: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x497E9: 				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default { 09 07 79 0D 10 00 07 }
0x497F0: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x497F7: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x497FE: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x49805: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x4980C: 			End  { 29 02 }
0x4980E: 		End  { 29 02 }
0x49810: 		SuppressIf  { 0A 82 }
0x49812: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8] { 14 18 50 08 09 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 }
0x4982A: 			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0 { 02 87 8B 0B 00 00 00 }
0x49831: 			End  { 29 02 }
0x49833: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x862, VarStoreId: 0xF101, VarOffset: 0x4A8, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 DF 0B 98 0B 62 08 01 F1 A8 04 10 21 00 00 7F 00 01 00 }
0x49847: 				Default DefaultId: 0x0 Value: 86 { 5B 07 00 00 01 56 00 }
0x4984E: 			End  { 29 02 }
0x49850: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x863, VarStoreId: 0xF101, VarOffset: 0x4B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 6E 0D 29 0D 63 08 01 F1 B8 04 10 10 00 0C 00 }
0x49861: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x49868: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4986F: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49876: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x4987D: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x49884: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x4988B: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x49892: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49899: 				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default { 09 07 7A 0D 10 00 08 }
0x498A0: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x498A7: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x498AE: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x498B5: 			End  { 29 02 }
0x498B7: 		End  { 29 02 }
0x498B9: 		SuppressIf  { 0A 82 }
0x498BB: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9] { 14 1A 50 08 0A 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 }
0x498D5: 			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0 { 02 87 8C 0B 00 00 00 }
0x498DC: 			End  { 29 02 }
0x498DE: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x864, VarStoreId: 0xF101, VarOffset: 0x4AA, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 E0 0B 98 0B 64 08 01 F1 AA 04 10 21 00 00 7F 00 01 00 }
0x498F2: 				Default DefaultId: 0x0 Value: 87 { 5B 07 00 00 01 57 00 }
0x498F9: 			End  { 29 02 }
0x498FB: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x865, VarStoreId: 0xF101, VarOffset: 0x4B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 6F 0D 29 0D 65 08 01 F1 B9 04 10 10 00 0C 00 }
0x4990C: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x49913: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x4991A: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49921: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x49928: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x4992F: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x49936: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x4993D: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49944: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x4994B: 				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default { 09 07 7B 0D 10 00 09 }
0x49952: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x49959: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x49960: 			End  { 29 02 }
0x49962: 		End  { 29 02 }
0x49964: 		SuppressIf  { 0A 82 }
0x49966: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10] { 14 1C 50 08 0B 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 }
0x49982: 			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0 { 02 87 8D 0B 00 00 00 }
0x49989: 			End  { 29 02 }
0x4998B: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x866, VarStoreId: 0xF101, VarOffset: 0x4AC, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 E1 0B 98 0B 66 08 01 F1 AC 04 10 21 00 00 7F 00 01 00 }
0x4999F: 				Default DefaultId: 0x0 Value: 88 { 5B 07 00 00 01 58 00 }
0x499A6: 			End  { 29 02 }
0x499A8: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x867, VarStoreId: 0xF101, VarOffset: 0x4BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 70 0D 29 0D 67 08 01 F1 BA 04 10 10 00 0C 00 }
0x499B9: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x499C0: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x499C7: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x499CE: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x499D5: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x499DC: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x499E3: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x499EA: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x499F1: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x499F8: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x499FF: 				OneOfOption Option: "IO Expander" Value: 10, Default { 09 07 7C 0D 10 00 0A }
0x49A06: 				OneOfOption Option: "Flash" Value: 12 { 09 07 7D 0D 00 00 0C }
0x49A0D: 			End  { 29 02 }
0x49A0F: 		End  { 29 02 }
0x49A11: 		SuppressIf  { 0A 82 }
0x49A13: 			EqIdValList QuestionId: 0x850, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11] { 14 1E 50 08 0C 00 00 00 01 00 02 00 03 00 04 00 05 00 06 00 07 00 08 00 09 00 0A 00 0B 00 }
0x49A31: 			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0 { 02 87 8E 0B 00 00 00 }
0x49A38: 			End  { 29 02 }
0x49A3A: 			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x868, VarStoreId: 0xF101, VarOffset: 0x4AE, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 E2 0B 98 0B 68 08 01 F1 AE 04 10 21 00 00 7F 00 01 00 }
0x49A4E: 				Default DefaultId: 0x0 Value: 89 { 5B 07 00 00 01 59 00 }
0x49A55: 			End  { 29 02 }
0x49A57: 			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0x869, VarStoreId: 0xF101, VarOffset: 0x4BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0 { 05 91 71 0D 29 0D 69 08 01 F1 BB 04 10 10 00 0C 00 }
0x49A68: 				OneOfOption Option: "Sensor" Value: 0 { 09 07 72 0D 00 00 00 }
0x49A6F: 				OneOfOption Option: "VCM" Value: 1 { 09 07 73 0D 00 00 01 }
0x49A76: 				OneOfOption Option: "EEPROM" Value: 2 { 09 07 74 0D 00 00 02 }
0x49A7D: 				OneOfOption Option: "EEPROM_EXT1" Value: 3 { 09 07 75 0D 00 00 03 }
0x49A84: 				OneOfOption Option: "EEPROM_EXT2" Value: 4 { 09 07 76 0D 00 00 04 }
0x49A8B: 				OneOfOption Option: "EEPROM_EXT3" Value: 5 { 09 07 77 0D 00 00 05 }
0x49A92: 				OneOfOption Option: "EEPROM_EXT4" Value: 6 { 09 07 78 0D 00 00 06 }
0x49A99: 				OneOfOption Option: "EEPROM_EXT5" Value: 7 { 09 07 79 0D 00 00 07 }
0x49AA0: 				OneOfOption Option: "EEPROM_EXT6" Value: 8 { 09 07 7A 0D 00 00 08 }
0x49AA7: 				OneOfOption Option: "EEPROM_EXT7" Value: 9 { 09 07 7B 0D 00 00 09 }
0x49AAE: 				OneOfOption Option: "IO Expander" Value: 10 { 09 07 7C 0D 00 00 0A }
0x49AB5: 				OneOfOption Option: "Flash" Value: 12, Default { 09 07 7D 0D 10 00 0C }
0x49ABC: 			End  { 29 02 }
0x49ABE: 		End  { 29 02 }
0x49AC0: 		OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x86A, VarStoreId: 0xF101, VarOffset: 0x4D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 93 10 A2 0C 6A 08 01 F1 D3 04 10 10 00 02 00 }
0x49AD1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 A4 0C 30 00 00 }
0x49AD8: 			OneOfOption Option: "External" Value: 1 { 09 07 A5 0C 00 00 01 }
0x49ADF: 			OneOfOption Option: "Internal PMIC" Value: 2 { 09 07 A6 0C 00 00 02 }
0x49AE6: 		End  { 29 02 }
0x49AE8: 		SuppressIf  { 0A 82 }
0x49AEA: 			EqIdVal QuestionId: 0x86A, Value: 0x1 { 12 86 6A 08 01 00 }
0x49AF0: 				Not  { 17 02 }
0x49AF2: 			End  { 29 02 }
0x49AF4: 			OneOf Prompt: "Flash Driver Selection", Help: "Select the Flash Driver as External or Internal PMIC ", QuestionFlags: 0x10, QuestionId: 0x86B, VarStoreId: 0xF101, VarOffset: 0xAFB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 94 10 A7 0C 6B 08 01 F1 FB 0A 10 10 00 05 00 }
0x49B05: 				OneOfOption Option: "Flash1" Value: 0, Default, MfgDefault { 09 07 9A 0D 30 00 00 }
0x49B0C: 				OneOfOption Option: "Flash2" Value: 1 { 09 07 9B 0D 00 00 01 }
0x49B13: 				OneOfOption Option: "Flash3" Value: 2 { 09 07 9C 0D 00 00 02 }
0x49B1A: 				OneOfOption Option: "Flash4" Value: 3 { 09 07 9D 0D 00 00 03 }
0x49B21: 				OneOfOption Option: "Flash5" Value: 4 { 09 07 9E 0D 00 00 04 }
0x49B28: 				OneOfOption Option: "Flash6" Value: 5 { 09 07 9F 0D 00 00 05 }
0x49B2F: 			End  { 29 02 }
0x49B31: 		End  { 29 02 }
0x49B33: 	End  { 29 02 }
0x49B35: 	Form FormId: 0x93, Title: "Control Logic options" { 01 86 93 00 21 0D }
0x49B3B: 		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0 { 02 87 21 0D 00 00 00 }
0x49B42: 		End  { 29 02 }
0x49B44: 		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0x86C, VarStoreId: 0xF101, VarOffset: 0x7E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0 { 05 91 86 0D 85 0D 6C 08 01 F1 7E 00 10 10 01 FE 00 }
0x49B55: 			OneOfOption Option: "Discrete" Value: 1 { 09 07 88 0D 00 00 01 }
0x49B5C: 			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default { 09 07 89 0D 10 00 02 }
0x49B63: 			OneOfOption Option: "PMIC_UP6641" Value: 3 { 09 07 8A 0D 00 00 03 }
0x49B6A: 			OneOfOption Option: "PMIC_USER0" Value: 253 { 09 07 8B 0D 00 00 FD }
0x49B71: 			OneOfOption Option: "PMIC_USER1" Value: 254 { 09 07 8C 0D 00 00 FE }
0x49B78: 		End  { 29 02 }
0x49B7A: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x86D, VarStoreId: 0xF101, VarOffset: 0x7F, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 B0 0C A9 0C 6D 08 01 F1 7F 00 10 10 10 50 00 }
0x49B8B: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x49B92: 			OneOfOption Option: "CRD-G" Value: 48 { 09 07 B4 0C 00 00 30 }
0x49B99: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x49BA0: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x49BA7: 			OneOfOption Option: "CRD-G2" Value: 80, Default { 09 07 B6 0C 10 00 50 }
0x49BAE: 		End  { 29 02 }
0x49BB0: 		OneOf Prompt: "Input Clock", Help: "Input Clock", QuestionFlags: 0x10, QuestionId: 0x86E, VarStoreId: 0xF101, VarOffset: 0x80, Flags: 0x12, Size: 32, Min: 0x10, Max: 0x40, Step: 0x0 { 05 9A 53 0B 53 0B 6E 08 01 F1 80 00 10 12 10 00 00 00 40 00 00 00 00 00 00 00 }
0x49BCA: 			OneOfOption Option: "24 MHz" Value: 32 { 09 0A 55 0B 02 02 20 00 00 00 }
0x49BD4: 			OneOfOption Option: "26 MHz" Value: 48 { 09 0A 56 0B 02 02 30 00 00 00 }
0x49BDE: 			OneOfOption Option: "20 MHz" Value: 16, Default { 09 0A 54 0B 12 02 10 00 00 00 }
0x49BE8: 			OneOfOption Option: "19.2 MHz" Value: 64 { 09 0A 57 0B 02 02 40 00 00 00 }
0x49BF2: 		End  { 29 02 }
0x49BF4: 		OneOf Prompt: "PCH Clock Source", Help: "This option specifies which IMGCLKOUT is chosen", QuestionFlags: 0x10, QuestionId: 0x86F, VarStoreId: 0xF101, VarOffset: 0x84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 93 0D 94 0D 6F 08 01 F1 84 00 10 10 00 04 00 }
0x49C05: 			OneOfOption Option: "IMGCLKOUT_0" Value: 0, Default { 09 07 95 0D 10 00 00 }
0x49C0C: 			OneOfOption Option: "IMGCLKOUT_1" Value: 1 { 09 07 96 0D 00 00 01 }
0x49C13: 			OneOfOption Option: "IMGCLKOUT_2" Value: 2 { 09 07 97 0D 00 00 02 }
0x49C1A: 			OneOfOption Option: "IMGCLKOUT_3" Value: 3 { 09 07 98 0D 00 00 03 }
0x49C21: 			OneOfOption Option: "IMGCLKOUT_4" Value: 4 { 09 07 99 0D 00 00 04 }
0x49C28: 		End  { 29 02 }
0x49C2A: 		SuppressIf  { 0A 82 }
0x49C2C: 			EqIdValList QuestionId: 0x86D, Values: [48, 80] { 14 8A 6D 08 02 00 30 00 50 00 }
0x49C36: 				Not  { 17 02 }
0x49C38: 			End  { 29 02 }
0x49C3A: 			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0x870, VarStoreId: 0xF101, VarOffset: 0x89, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0 { 05 91 6F 0C 6E 0C 70 08 01 F1 89 00 10 10 21 29 00 }
0x49C4B: 				OneOfOption Option: "Front" Value: 33 { 09 07 6C 0C 00 00 21 }
0x49C52: 				OneOfOption Option: "Back" Value: 41, Default { 09 07 6D 0C 10 00 29 }
0x49C59: 			End  { 29 02 }
0x49C5B: 		End  { 29 02 }
0x49C5D: 		SuppressIf  { 0A 82 }
0x49C5F: 			EqIdVal QuestionId: 0x86C, Value: 0x1 { 12 06 6C 08 01 00 }
0x49C65: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x871, VarStoreId: 0xF101, VarOffset: 0x86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 96 0B 8F 0B 71 08 01 F1 86 00 10 10 00 05 00 }
0x49C76: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x49C7D: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x49C84: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x49C8B: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x49C92: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x49C99: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x49CA0: 			End  { 29 02 }
0x49CA2: 			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x872, VarStoreId: 0xF101, VarOffset: 0x87, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 99 0B 98 0B 72 08 01 F1 87 00 10 21 00 00 7F 00 01 00 }
0x49CB6: 				Default DefaultId: 0x0 Value: 77 { 5B 07 00 00 01 4D 00 }
0x49CBD: 			End  { 29 02 }
0x49CBF: 			SuppressIf  { 0A 82 }
0x49CC1: 				EqIdValList QuestionId: 0x86C, Values: [2, 3] { 14 8A 6C 08 02 00 02 00 03 00 }
0x49CCB: 					Not  { 17 02 }
0x49CCD: 				End  { 29 02 }
0x49CCF: 				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x873, VarStoreId: 0xF101, VarOffset: 0x8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 FE 0B FD 0B 73 08 01 F1 8F 00 10 10 00 04 00 }
0x49CE0: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x49CE7: 					OneOfOption Option: "White Led" Value: 1, Default, MfgDefault { 09 07 09 0C 30 00 01 }
0x49CEE: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x49CF5: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x49CFC: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x49D03: 				End  { 29 02 }
0x49D05: 				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x874, VarStoreId: 0xF101, VarOffset: 0x8A, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 E4 0B E3 0B 74 08 01 F1 8A 00 10 20 00 1F 01 }
0x49D16: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49D1C: 				End  { 29 02 }
0x49D1E: 				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x875, VarStoreId: 0xF101, VarOffset: 0x8B, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F1 0B F0 0B 75 08 01 F1 8B 00 10 20 00 07 01 }
0x49D2F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49D35: 				End  { 29 02 }
0x49D37: 				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x876, VarStoreId: 0xF101, VarOffset: 0x90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 03 0C FD 0B 76 08 01 F1 90 00 10 10 00 04 00 }
0x49D48: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x49D4F: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x49D56: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x49D5D: 					OneOfOption Option: "IR Led" Value: 3, Default, MfgDefault { 09 07 0B 0C 30 00 03 }
0x49D64: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x49D6B: 				End  { 29 02 }
0x49D6D: 				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x877, VarStoreId: 0xF101, VarOffset: 0x8C, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 EA 0B E3 0B 77 08 01 F1 8C 00 10 20 00 1F 01 }
0x49D7E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49D84: 				End  { 29 02 }
0x49D86: 				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x878, VarStoreId: 0xF101, VarOffset: 0x8D, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F7 0B F0 0B 78 08 01 F1 8D 00 10 20 00 07 01 }
0x49D97: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49D9D: 				End  { 29 02 }
0x49D9F: 				Numeric Prompt: "SubPlatformId", Help: "SubPlatformId", QuestionFlags: 0x10, QuestionId: 0x879, VarStoreId: 0xF101, VarOffset: 0x8E, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 58 0B 58 0B 79 08 01 F1 8E 00 10 20 00 0F 01 }
0x49DB0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49DB6: 				End  { 29 02 }
0x49DB8: 			End  { 29 02 }
0x49DBA: 		End  { 29 02 }
0x49DBC: 		SuppressIf  { 0A 82 }
0x49DBE: 			EqIdValList QuestionId: 0x86C, Values: [253, 254] { 14 0A 6C 08 02 00 FD 00 FE 00 }
0x49DC8: 			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0x87A, VarStoreId: 0xF101, VarOffset: 0x85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 74 0B 73 0B 7A 08 01 F1 85 00 10 10 00 06 01 }
0x49DD9: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49DDF: 			End  { 29 02 }
0x49DE1: 			SuppressIf  { 0A 82 }
0x49DE3: 				EqIdVal QuestionId: 0x87A, Value: 0x0 { 12 06 7A 08 00 00 }
0x49DE9: 				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0 { 02 87 8D 0D 00 00 00 }
0x49DF0: 				End  { 29 02 }
0x49DF2: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x87B, VarStoreId: 0xF101, VarOffset: 0x91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 1B 0C 1A 0C 7B 08 01 F1 91 00 10 10 00 17 01 }
0x49E03: 					Default DefaultId: 0x0 Value: 22 { 5B 06 00 00 00 16 }
0x49E09: 				End  { 29 02 }
0x49E0B: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x87C, VarStoreId: 0xF101, VarOffset: 0x97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 28 0C 27 0C 7C 08 01 F1 97 00 10 10 00 0E 00 }
0x49E1C: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x49E23: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x49E2A: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x49E31: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x49E38: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x49E3F: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x49E46: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x49E4D: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x49E54: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x49E5B: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x49E62: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x49E69: 				End  { 29 02 }
0x49E6B: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x87D, VarStoreId: 0xF101, VarOffset: 0x9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 0E 0C 0D 0C 7D 08 01 F1 9D 00 10 10 00 12 00 }
0x49E7C: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x49E83: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x49E8A: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x49E91: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x49E98: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x49E9F: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x49EA6: 				End  { 29 02 }
0x49EA8: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x87E, VarStoreId: 0xF101, VarOffset: 0xA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 35 0C 34 0C 7E 08 01 F1 A3 00 10 10 00 01 01 }
0x49EB9: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x49EBF: 				End  { 29 02 }
0x49EC1: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x87F, VarStoreId: 0xF101, VarOffset: 0xA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 42 0C 41 0C 7F 08 01 F1 A9 00 10 10 00 01 01 }
0x49ED2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49ED8: 				End  { 29 02 }
0x49EDA: 			End  { 29 02 }
0x49EDC: 			SuppressIf  { 0A 82 }
0x49EDE: 				EqIdValList QuestionId: 0x87A, Values: [0, 1] { 14 0A 7A 08 02 00 00 00 01 00 }
0x49EE8: 				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0 { 02 87 8E 0D 00 00 00 }
0x49EEF: 				End  { 29 02 }
0x49EF1: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x880, VarStoreId: 0xF101, VarOffset: 0x92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 1C 0C 1A 0C 80 08 01 F1 92 00 10 10 00 17 01 }
0x49F02: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x49F08: 				End  { 29 02 }
0x49F0A: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x881, VarStoreId: 0xF101, VarOffset: 0x98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 29 0C 27 0C 81 08 01 F1 98 00 10 10 00 0E 00 }
0x49F1B: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x49F22: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x49F29: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x49F30: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x49F37: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x49F3E: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x49F45: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x49F4C: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x49F53: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x49F5A: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x49F61: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x49F68: 				End  { 29 02 }
0x49F6A: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x882, VarStoreId: 0xF101, VarOffset: 0x9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 0F 0C 0D 0C 82 08 01 F1 9E 00 10 10 00 12 00 }
0x49F7B: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x49F82: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x49F89: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x49F90: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x49F97: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x49F9E: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x49FA5: 				End  { 29 02 }
0x49FA7: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x883, VarStoreId: 0xF101, VarOffset: 0xA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 36 0C 34 0C 83 08 01 F1 A4 00 10 10 00 01 01 }
0x49FB8: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x49FBE: 				End  { 29 02 }
0x49FC0: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x884, VarStoreId: 0xF101, VarOffset: 0xAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 43 0C 41 0C 84 08 01 F1 AA 00 10 10 00 01 01 }
0x49FD1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x49FD7: 				End  { 29 02 }
0x49FD9: 			End  { 29 02 }
0x49FDB: 			SuppressIf  { 0A 82 }
0x49FDD: 				EqIdValList QuestionId: 0x87A, Values: [0, 1, 2] { 14 0C 7A 08 03 00 00 00 01 00 02 00 }
0x49FE9: 				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0 { 02 87 8F 0D 00 00 00 }
0x49FF0: 				End  { 29 02 }
0x49FF2: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x885, VarStoreId: 0xF101, VarOffset: 0x93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 1D 0C 1A 0C 85 08 01 F1 93 00 10 10 00 17 01 }
0x4A003: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4A009: 				End  { 29 02 }
0x4A00B: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x886, VarStoreId: 0xF101, VarOffset: 0x99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 2A 0C 27 0C 86 08 01 F1 99 00 10 10 00 0E 00 }
0x4A01C: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A023: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A02A: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A031: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4A038: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A03F: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A046: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4A04D: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A054: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A05B: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A062: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A069: 				End  { 29 02 }
0x4A06B: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x887, VarStoreId: 0xF101, VarOffset: 0x9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 10 0C 0D 0C 87 08 01 F1 9F 00 10 10 00 12 00 }
0x4A07C: 					OneOfOption Option: "Reset" Value: 0 { 09 07 4E 0C 00 00 00 }
0x4A083: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4A08A: 					OneOfOption Option: "Clock_En" Value: 12, Default { 09 07 50 0C 10 00 0C }
0x4A091: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A098: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A09F: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A0A6: 				End  { 29 02 }
0x4A0A8: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x888, VarStoreId: 0xF101, VarOffset: 0xA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 37 0C 34 0C 88 08 01 F1 A5 00 10 10 00 01 01 }
0x4A0B9: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A0BF: 				End  { 29 02 }
0x4A0C1: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x889, VarStoreId: 0xF101, VarOffset: 0xAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 44 0C 41 0C 89 08 01 F1 AB 00 10 10 00 01 01 }
0x4A0D2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A0D8: 				End  { 29 02 }
0x4A0DA: 			End  { 29 02 }
0x4A0DC: 			SuppressIf  { 0A 82 }
0x4A0DE: 				EqIdValList QuestionId: 0x87A, Values: [0, 1, 2, 3] { 14 0E 7A 08 04 00 00 00 01 00 02 00 03 00 }
0x4A0EC: 				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0 { 02 87 90 0D 00 00 00 }
0x4A0F3: 				End  { 29 02 }
0x4A0F5: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x88A, VarStoreId: 0xF101, VarOffset: 0x94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 1E 0C 1A 0C 8A 08 01 F1 94 00 10 10 00 17 01 }
0x4A106: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4A10C: 				End  { 29 02 }
0x4A10E: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x88B, VarStoreId: 0xF101, VarOffset: 0x9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 2B 0C 27 0C 8B 08 01 F1 9A 00 10 10 00 0E 00 }
0x4A11F: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A126: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A12D: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A134: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4A13B: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A142: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A149: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4A150: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A157: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A15E: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A165: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A16C: 				End  { 29 02 }
0x4A16E: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x88C, VarStoreId: 0xF101, VarOffset: 0xA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 11 0C 0D 0C 8C 08 01 F1 A0 00 10 10 00 12 00 }
0x4A17F: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4A186: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4A18D: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4A194: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A19B: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A1A2: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A1A9: 				End  { 29 02 }
0x4A1AB: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x88D, VarStoreId: 0xF101, VarOffset: 0xA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 38 0C 34 0C 8D 08 01 F1 A6 00 10 10 00 01 01 }
0x4A1BC: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A1C2: 				End  { 29 02 }
0x4A1C4: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x88E, VarStoreId: 0xF101, VarOffset: 0xAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 45 0C 41 0C 8E 08 01 F1 AC 00 10 10 00 01 01 }
0x4A1D5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A1DB: 				End  { 29 02 }
0x4A1DD: 			End  { 29 02 }
0x4A1DF: 			SuppressIf  { 0A 82 }
0x4A1E1: 				EqIdValList QuestionId: 0x87A, Values: [0, 1, 2, 3, 4] { 14 10 7A 08 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4A1F1: 				Subtitle Prompt: "GPIO 4", Help: "", Flags: 0x0 { 02 87 91 0D 00 00 00 }
0x4A1F8: 				End  { 29 02 }
0x4A1FA: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x88F, VarStoreId: 0xF101, VarOffset: 0x95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 1F 0C 1A 0C 8F 08 01 F1 95 00 10 10 00 17 01 }
0x4A20B: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4A211: 				End  { 29 02 }
0x4A213: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x890, VarStoreId: 0xF101, VarOffset: 0x9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 2C 0C 27 0C 90 08 01 F1 9B 00 10 10 00 0E 00 }
0x4A224: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A22B: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A232: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A239: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4A240: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A247: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A24E: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4A255: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A25C: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A263: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A26A: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A271: 				End  { 29 02 }
0x4A273: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x891, VarStoreId: 0xF101, VarOffset: 0xA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 12 0C 0D 0C 91 08 01 F1 A1 00 10 10 00 12 00 }
0x4A284: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4A28B: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4A292: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4A299: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A2A0: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A2A7: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A2AE: 				End  { 29 02 }
0x4A2B0: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x892, VarStoreId: 0xF101, VarOffset: 0xA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 39 0C 34 0C 92 08 01 F1 A7 00 10 10 00 01 01 }
0x4A2C1: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A2C7: 				End  { 29 02 }
0x4A2C9: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x893, VarStoreId: 0xF101, VarOffset: 0xAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 46 0C 41 0C 93 08 01 F1 AD 00 10 10 00 01 01 }
0x4A2DA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A2E0: 				End  { 29 02 }
0x4A2E2: 			End  { 29 02 }
0x4A2E4: 			SuppressIf  { 0A 82 }
0x4A2E6: 				EqIdValList QuestionId: 0x87A, Values: [0, 1, 2, 3, 4, 5] { 14 12 7A 08 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4A2F8: 				Subtitle Prompt: "GPIO 5", Help: "", Flags: 0x0 { 02 87 92 0D 00 00 00 }
0x4A2FF: 				End  { 29 02 }
0x4A301: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x894, VarStoreId: 0xF101, VarOffset: 0x96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 20 0C 1A 0C 94 08 01 F1 96 00 10 10 00 17 01 }
0x4A312: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4A318: 				End  { 29 02 }
0x4A31A: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x895, VarStoreId: 0xF101, VarOffset: 0x9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 2D 0C 27 0C 95 08 01 F1 9C 00 10 10 00 0E 00 }
0x4A32B: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A332: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A339: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A340: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4A347: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A34E: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A355: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4A35C: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A363: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A36A: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A371: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A378: 				End  { 29 02 }
0x4A37A: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x896, VarStoreId: 0xF101, VarOffset: 0xA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 13 0C 0D 0C 96 08 01 F1 A2 00 10 10 00 12 00 }
0x4A38B: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4A392: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4A399: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4A3A0: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A3A7: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A3AE: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A3B5: 				End  { 29 02 }
0x4A3B7: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x897, VarStoreId: 0xF101, VarOffset: 0xA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 3A 0C 34 0C 97 08 01 F1 A8 00 10 10 00 01 01 }
0x4A3C8: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A3CE: 				End  { 29 02 }
0x4A3D0: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x898, VarStoreId: 0xF101, VarOffset: 0xAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 47 0C 41 0C 98 08 01 F1 AE 00 10 10 00 01 01 }
0x4A3E1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A3E7: 				End  { 29 02 }
0x4A3E9: 			End  { 29 02 }
0x4A3EB: 		End  { 29 02 }
0x4A3ED: 	End  { 29 02 }
0x4A3EF: 	Form FormId: 0x94, Title: "Control Logic options" { 01 86 94 00 21 0D }
0x4A3F5: 		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0 { 02 87 21 0D 00 00 00 }
0x4A3FC: 		End  { 29 02 }
0x4A3FE: 		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0x899, VarStoreId: 0xF101, VarOffset: 0xAF, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0 { 05 91 87 0D 85 0D 99 08 01 F1 AF 00 10 10 01 FE 00 }
0x4A40F: 			OneOfOption Option: "Discrete" Value: 1, Default { 09 07 88 0D 10 00 01 }
0x4A416: 			OneOfOption Option: "PMIC_TPS68470" Value: 2 { 09 07 89 0D 00 00 02 }
0x4A41D: 			OneOfOption Option: "PMIC_UP6641" Value: 3 { 09 07 8A 0D 00 00 03 }
0x4A424: 			OneOfOption Option: "PMIC_USER0" Value: 253 { 09 07 8B 0D 00 00 FD }
0x4A42B: 			OneOfOption Option: "PMIC_USER1" Value: 254 { 09 07 8C 0D 00 00 FE }
0x4A432: 		End  { 29 02 }
0x4A434: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x89A, VarStoreId: 0xF101, VarOffset: 0xB0, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 B1 0C A9 0C 9A 08 01 F1 B0 00 10 10 10 50 00 }
0x4A445: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x4A44C: 			OneOfOption Option: "CRD-D" Value: 32, Default { 09 07 B3 0C 10 00 20 }
0x4A453: 			OneOfOption Option: "CRD-G" Value: 48 { 09 07 B4 0C 00 00 30 }
0x4A45A: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x4A461: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x4A468: 		End  { 29 02 }
0x4A46A: 		OneOf Prompt: "Input Clock", Help: "Input Clock", QuestionFlags: 0x10, QuestionId: 0x89B, VarStoreId: 0xF101, VarOffset: 0xB1, Flags: 0x12, Size: 32, Min: 0x10, Max: 0x40, Step: 0x0 { 05 9A F2 0F 53 0B 9B 08 01 F1 B1 00 10 12 10 00 00 00 40 00 00 00 00 00 00 00 }
0x4A484: 			OneOfOption Option: "24 MHz" Value: 32 { 09 0A 55 0B 02 02 20 00 00 00 }
0x4A48E: 			OneOfOption Option: "26 MHz" Value: 48 { 09 0A 56 0B 02 02 30 00 00 00 }
0x4A498: 			OneOfOption Option: "20 MHz" Value: 16, Default { 09 0A 54 0B 12 02 10 00 00 00 }
0x4A4A2: 			OneOfOption Option: "19.2 MHz" Value: 64 { 09 0A 57 0B 02 02 40 00 00 00 }
0x4A4AC: 		End  { 29 02 }
0x4A4AE: 		OneOf Prompt: "PCH Clock Source", Help: "This option specifies which IMGCLKOUT is chosen", QuestionFlags: 0x10, QuestionId: 0x89C, VarStoreId: 0xF101, VarOffset: 0xB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 AF 10 94 0D 9C 08 01 F1 B5 00 10 10 00 04 00 }
0x4A4BF: 			OneOfOption Option: "IMGCLKOUT_0" Value: 0 { 09 07 95 0D 00 00 00 }
0x4A4C6: 			OneOfOption Option: "IMGCLKOUT_1" Value: 1 { 09 07 96 0D 00 00 01 }
0x4A4CD: 			OneOfOption Option: "IMGCLKOUT_2" Value: 2, Default { 09 07 97 0D 10 00 02 }
0x4A4D4: 			OneOfOption Option: "IMGCLKOUT_3" Value: 3 { 09 07 98 0D 00 00 03 }
0x4A4DB: 			OneOfOption Option: "IMGCLKOUT_4" Value: 4 { 09 07 99 0D 00 00 04 }
0x4A4E2: 		End  { 29 02 }
0x4A4E4: 		SuppressIf  { 0A 82 }
0x4A4E6: 			EqIdValList QuestionId: 0x89A, Values: [48, 80] { 14 8A 9A 08 02 00 30 00 50 00 }
0x4A4F0: 				Not  { 17 02 }
0x4A4F2: 			End  { 29 02 }
0x4A4F4: 			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0x89D, VarStoreId: 0xF101, VarOffset: 0xBA, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0 { 05 91 70 0C 6E 0C 9D 08 01 F1 BA 00 10 10 21 29 00 }
0x4A505: 				OneOfOption Option: "Front" Value: 33 { 09 07 6C 0C 00 00 21 }
0x4A50C: 				OneOfOption Option: "Back" Value: 41, Default { 09 07 6D 0C 10 00 29 }
0x4A513: 			End  { 29 02 }
0x4A515: 		End  { 29 02 }
0x4A517: 		SuppressIf  { 0A 82 }
0x4A519: 			EqIdVal QuestionId: 0x899, Value: 0x1 { 12 06 99 08 01 00 }
0x4A51F: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x89E, VarStoreId: 0xF101, VarOffset: 0xB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 97 0B 8F 0B 9E 08 01 F1 B7 00 10 10 00 05 00 }
0x4A530: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4A537: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4A53E: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4A545: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4A54C: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4A553: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4A55A: 			End  { 29 02 }
0x4A55C: 			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x89F, VarStoreId: 0xF101, VarOffset: 0xB8, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 9A 0B 98 0B 9F 08 01 F1 B8 00 10 21 00 00 7F 00 01 00 }
0x4A570: 				Default DefaultId: 0x0 Value: 73 { 5B 07 00 00 01 49 00 }
0x4A577: 			End  { 29 02 }
0x4A579: 			SuppressIf  { 0A 82 }
0x4A57B: 				EqIdValList QuestionId: 0x899, Values: [2, 3] { 14 8A 99 08 02 00 02 00 03 00 }
0x4A585: 					Not  { 17 02 }
0x4A587: 				End  { 29 02 }
0x4A589: 				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x8A0, VarStoreId: 0xF101, VarOffset: 0xC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 FF 0B FD 0B A0 08 01 F1 C0 00 10 10 00 04 00 }
0x4A59A: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4A5A1: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4A5A8: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4A5AF: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4A5B6: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4A5BD: 				End  { 29 02 }
0x4A5BF: 				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8A1, VarStoreId: 0xF101, VarOffset: 0xBB, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 E5 0B E3 0B A1 08 01 F1 BB 00 10 20 00 1F 01 }
0x4A5D0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A5D6: 				End  { 29 02 }
0x4A5D8: 				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8A2, VarStoreId: 0xF101, VarOffset: 0xBC, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F2 0B F0 0B A2 08 01 F1 BC 00 10 20 00 07 01 }
0x4A5E9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A5EF: 				End  { 29 02 }
0x4A5F1: 				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x8A3, VarStoreId: 0xF101, VarOffset: 0xC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 04 0C FD 0B A3 08 01 F1 C1 00 10 10 00 04 00 }
0x4A602: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4A609: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4A610: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4A617: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4A61E: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4A625: 				End  { 29 02 }
0x4A627: 				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8A4, VarStoreId: 0xF101, VarOffset: 0xBD, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 EB 0B E3 0B A4 08 01 F1 BD 00 10 20 00 1F 01 }
0x4A638: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A63E: 				End  { 29 02 }
0x4A640: 				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8A5, VarStoreId: 0xF101, VarOffset: 0xBE, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F8 0B F0 0B A5 08 01 F1 BE 00 10 20 00 07 01 }
0x4A651: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A657: 				End  { 29 02 }
0x4A659: 				Numeric Prompt: "SubPlatformId", Help: "SubPlatformId", QuestionFlags: 0x10, QuestionId: 0x8A6, VarStoreId: 0xF101, VarOffset: 0xBF, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 59 0B 59 0B A6 08 01 F1 BF 00 10 20 00 0F 01 }
0x4A66A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A670: 				End  { 29 02 }
0x4A672: 			End  { 29 02 }
0x4A674: 		End  { 29 02 }
0x4A676: 		SuppressIf  { 0A 82 }
0x4A678: 			EqIdValList QuestionId: 0x899, Values: [253, 254] { 14 0A 99 08 02 00 FD 00 FE 00 }
0x4A682: 			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0x8A7, VarStoreId: 0xF101, VarOffset: 0xB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 75 0B 73 0B A7 08 01 F1 B6 00 10 10 00 06 01 }
0x4A693: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x4A699: 			End  { 29 02 }
0x4A69B: 			SuppressIf  { 0A 82 }
0x4A69D: 				EqIdVal QuestionId: 0x8A7, Value: 0x0 { 12 06 A7 08 00 00 }
0x4A6A3: 				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0 { 02 87 8D 0D 00 00 00 }
0x4A6AA: 				End  { 29 02 }
0x4A6AC: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8A8, VarStoreId: 0xF101, VarOffset: 0xC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 21 0C 1A 0C A8 08 01 F1 C2 00 10 10 00 17 01 }
0x4A6BD: 					Default DefaultId: 0x0 Value: 13 { 5B 06 00 00 00 0D }
0x4A6C3: 				End  { 29 02 }
0x4A6C5: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8A9, VarStoreId: 0xF101, VarOffset: 0xC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 2E 0C 27 0C A9 08 01 F1 C8 00 10 10 00 0E 00 }
0x4A6D6: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A6DD: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A6E4: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A6EB: 					OneOfOption Option: "D" Value: 8 { 09 07 57 0C 00 00 08 }
0x4A6F2: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A6F9: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A700: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A707: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A70E: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A715: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A71C: 					OneOfOption Option: "H" Value: 7, Default { 09 07 5A 0C 10 00 07 }
0x4A723: 				End  { 29 02 }
0x4A725: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8AA, VarStoreId: 0xF101, VarOffset: 0xCE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 14 0C 0D 0C AA 08 01 F1 CE 00 10 10 00 12 00 }
0x4A736: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4A73D: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4A744: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4A74B: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A752: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A759: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A760: 				End  { 29 02 }
0x4A762: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8AB, VarStoreId: 0xF101, VarOffset: 0xD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 3B 0C 34 0C AB 08 01 F1 D4 00 10 10 00 01 01 }
0x4A773: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A779: 				End  { 29 02 }
0x4A77B: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8AC, VarStoreId: 0xF101, VarOffset: 0xDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 48 0C 41 0C AC 08 01 F1 DA 00 10 10 00 01 01 }
0x4A78C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A792: 				End  { 29 02 }
0x4A794: 			End  { 29 02 }
0x4A796: 			SuppressIf  { 0A 82 }
0x4A798: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1] { 14 0A A7 08 02 00 00 00 01 00 }
0x4A7A2: 				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0 { 02 87 8E 0D 00 00 00 }
0x4A7A9: 				End  { 29 02 }
0x4A7AB: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8AD, VarStoreId: 0xF101, VarOffset: 0xC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 22 0C 1A 0C AD 08 01 F1 C3 00 10 10 00 17 01 }
0x4A7BC: 					Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x4A7C2: 				End  { 29 02 }
0x4A7C4: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8AE, VarStoreId: 0xF101, VarOffset: 0xC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 2F 0C 27 0C AE 08 01 F1 C9 00 10 10 00 0E 00 }
0x4A7D5: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A7DC: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A7E3: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A7EA: 					OneOfOption Option: "D" Value: 8 { 09 07 57 0C 00 00 08 }
0x4A7F1: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A7F8: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A7FF: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A806: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A80D: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A814: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A81B: 					OneOfOption Option: "H" Value: 7, Default { 09 07 5A 0C 10 00 07 }
0x4A822: 				End  { 29 02 }
0x4A824: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8AF, VarStoreId: 0xF101, VarOffset: 0xCF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 15 0C 0D 0C AF 08 01 F1 CF 00 10 10 00 12 00 }
0x4A835: 					OneOfOption Option: "Reset" Value: 0 { 09 07 4E 0C 00 00 00 }
0x4A83C: 					OneOfOption Option: "Power_En" Value: 11, Default { 09 07 4F 0C 10 00 0B }
0x4A843: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4A84A: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A851: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A858: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A85F: 				End  { 29 02 }
0x4A861: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8B0, VarStoreId: 0xF101, VarOffset: 0xD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 3C 0C 34 0C B0 08 01 F1 D5 00 10 10 00 01 01 }
0x4A872: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A878: 				End  { 29 02 }
0x4A87A: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8B1, VarStoreId: 0xF101, VarOffset: 0xDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 49 0C 41 0C B1 08 01 F1 DB 00 10 10 00 01 01 }
0x4A88B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A891: 				End  { 29 02 }
0x4A893: 			End  { 29 02 }
0x4A895: 			SuppressIf  { 0A 82 }
0x4A897: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2] { 14 0C A7 08 03 00 00 00 01 00 02 00 }
0x4A8A3: 				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0 { 02 87 8F 0D 00 00 00 }
0x4A8AA: 				End  { 29 02 }
0x4A8AC: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8B2, VarStoreId: 0xF101, VarOffset: 0xC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 23 0C 1A 0C B2 08 01 F1 C4 00 10 10 00 17 01 }
0x4A8BD: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4A8C3: 				End  { 29 02 }
0x4A8C5: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8B3, VarStoreId: 0xF101, VarOffset: 0xCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 30 0C 27 0C B3 08 01 F1 CA 00 10 10 00 0E 00 }
0x4A8D6: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A8DD: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A8E4: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A8EB: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4A8F2: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A8F9: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4A900: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4A907: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4A90E: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4A915: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4A91C: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4A923: 				End  { 29 02 }
0x4A925: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8B4, VarStoreId: 0xF101, VarOffset: 0xD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 16 0C 0D 0C B4 08 01 F1 D0 00 10 10 00 12 00 }
0x4A936: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4A93D: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4A944: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4A94B: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4A952: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4A959: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4A960: 				End  { 29 02 }
0x4A962: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8B5, VarStoreId: 0xF101, VarOffset: 0xD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 3D 0C 34 0C B5 08 01 F1 D6 00 10 10 00 01 01 }
0x4A973: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4A979: 				End  { 29 02 }
0x4A97B: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8B6, VarStoreId: 0xF101, VarOffset: 0xDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4A 0C 41 0C B6 08 01 F1 DC 00 10 10 00 01 01 }
0x4A98C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4A992: 				End  { 29 02 }
0x4A994: 			End  { 29 02 }
0x4A996: 			SuppressIf  { 0A 82 }
0x4A998: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3] { 14 0E A7 08 04 00 00 00 01 00 02 00 03 00 }
0x4A9A6: 				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0 { 02 87 90 0D 00 00 00 }
0x4A9AD: 				End  { 29 02 }
0x4A9AF: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8B7, VarStoreId: 0xF101, VarOffset: 0xC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 24 0C 1A 0C B7 08 01 F1 C5 00 10 10 00 17 01 }
0x4A9C0: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4A9C6: 				End  { 29 02 }
0x4A9C8: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8B8, VarStoreId: 0xF101, VarOffset: 0xCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 31 0C 27 0C B8 08 01 F1 CB 00 10 10 00 0E 00 }
0x4A9D9: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4A9E0: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4A9E7: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4A9EE: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4A9F5: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4A9FC: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4AA03: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4AA0A: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4AA11: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4AA18: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4AA1F: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4AA26: 				End  { 29 02 }
0x4AA28: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8B9, VarStoreId: 0xF101, VarOffset: 0xD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 17 0C 0D 0C B9 08 01 F1 D1 00 10 10 00 12 00 }
0x4AA39: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4AA40: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4AA47: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4AA4E: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4AA55: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4AA5C: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4AA63: 				End  { 29 02 }
0x4AA65: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8BA, VarStoreId: 0xF101, VarOffset: 0xD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 3E 0C 34 0C BA 08 01 F1 D7 00 10 10 00 01 01 }
0x4AA76: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4AA7C: 				End  { 29 02 }
0x4AA7E: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8BB, VarStoreId: 0xF101, VarOffset: 0xDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4B 0C 41 0C BB 08 01 F1 DD 00 10 10 00 01 01 }
0x4AA8F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AA95: 				End  { 29 02 }
0x4AA97: 			End  { 29 02 }
0x4AA99: 			SuppressIf  { 0A 82 }
0x4AA9B: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3, 4] { 14 10 A7 08 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4AAAB: 				Subtitle Prompt: "GPIO 4", Help: "", Flags: 0x0 { 02 87 91 0D 00 00 00 }
0x4AAB2: 				End  { 29 02 }
0x4AAB4: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8BC, VarStoreId: 0xF101, VarOffset: 0xC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 25 0C 1A 0C BC 08 01 F1 C6 00 10 10 00 17 01 }
0x4AAC5: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4AACB: 				End  { 29 02 }
0x4AACD: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8BD, VarStoreId: 0xF101, VarOffset: 0xCC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 32 0C 27 0C BD 08 01 F1 CC 00 10 10 00 0E 00 }
0x4AADE: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4AAE5: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4AAEC: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4AAF3: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4AAFA: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4AB01: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4AB08: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4AB0F: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4AB16: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4AB1D: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4AB24: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4AB2B: 				End  { 29 02 }
0x4AB2D: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8BE, VarStoreId: 0xF101, VarOffset: 0xD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 18 0C 0D 0C BE 08 01 F1 D2 00 10 10 00 12 00 }
0x4AB3E: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4AB45: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4AB4C: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4AB53: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4AB5A: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4AB61: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4AB68: 				End  { 29 02 }
0x4AB6A: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8BF, VarStoreId: 0xF101, VarOffset: 0xD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 3F 0C 34 0C BF 08 01 F1 D8 00 10 10 00 01 01 }
0x4AB7B: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4AB81: 				End  { 29 02 }
0x4AB83: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8C0, VarStoreId: 0xF101, VarOffset: 0xDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4C 0C 41 0C C0 08 01 F1 DE 00 10 10 00 01 01 }
0x4AB94: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AB9A: 				End  { 29 02 }
0x4AB9C: 			End  { 29 02 }
0x4AB9E: 			SuppressIf  { 0A 82 }
0x4ABA0: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3, 4, 5] { 14 12 A7 08 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4ABB2: 				Subtitle Prompt: "GPIO 5", Help: "", Flags: 0x0 { 02 87 92 0D 00 00 00 }
0x4ABB9: 				End  { 29 02 }
0x4ABBB: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8C1, VarStoreId: 0xF101, VarOffset: 0xC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 26 0C 1A 0C C1 08 01 F1 C7 00 10 10 00 17 01 }
0x4ABCC: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4ABD2: 				End  { 29 02 }
0x4ABD4: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8C2, VarStoreId: 0xF101, VarOffset: 0xCD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 33 0C 27 0C C2 08 01 F1 CD 00 10 10 00 0E 00 }
0x4ABE5: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4ABEC: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4ABF3: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4ABFA: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4AC01: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4AC08: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4AC0F: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4AC16: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4AC1D: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4AC24: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4AC2B: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4AC32: 				End  { 29 02 }
0x4AC34: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8C3, VarStoreId: 0xF101, VarOffset: 0xD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 19 0C 0D 0C C3 08 01 F1 D3 00 10 10 00 12 00 }
0x4AC45: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4AC4C: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4AC53: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4AC5A: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4AC61: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4AC68: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4AC6F: 				End  { 29 02 }
0x4AC71: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8C4, VarStoreId: 0xF101, VarOffset: 0xD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 40 0C 34 0C C4 08 01 F1 D9 00 10 10 00 01 01 }
0x4AC82: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4AC88: 				End  { 29 02 }
0x4AC8A: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8C5, VarStoreId: 0xF101, VarOffset: 0xDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4D 0C 41 0C C5 08 01 F1 DF 00 10 10 00 01 01 }
0x4AC9B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4ACA1: 				End  { 29 02 }
0x4ACA3: 			End  { 29 02 }
0x4ACA5: 		End  { 29 02 }
0x4ACA7: 	End  { 29 02 }
0x4ACA9: 	Form FormId: 0x95, Title: "Control Logic options" { 01 86 95 00 21 0D }
0x4ACAF: 		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0 { 02 87 21 0D 00 00 00 }
0x4ACB6: 		End  { 29 02 }
0x4ACB8: 		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0x8C6, VarStoreId: 0xF101, VarOffset: 0xE0, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0 { 05 91 85 0D 85 0D C6 08 01 F1 E0 00 10 10 01 FE 00 }
0x4ACC9: 			OneOfOption Option: "Discrete" Value: 1 { 09 07 88 0D 00 00 01 }
0x4ACD0: 			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default { 09 07 89 0D 10 00 02 }
0x4ACD7: 			OneOfOption Option: "PMIC_UP6641" Value: 3 { 09 07 8A 0D 00 00 03 }
0x4ACDE: 			OneOfOption Option: "PMIC_USER0" Value: 253 { 09 07 8B 0D 00 00 FD }
0x4ACE5: 			OneOfOption Option: "PMIC_USER1" Value: 254 { 09 07 8C 0D 00 00 FE }
0x4ACEC: 		End  { 29 02 }
0x4ACEE: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x8C7, VarStoreId: 0xF101, VarOffset: 0xE1, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 A9 0C A9 0C C7 08 01 F1 E1 00 10 10 10 50 00 }
0x4ACFF: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x4AD06: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x4AD0D: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x4AD14: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x4AD1B: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x4AD22: 		End  { 29 02 }
0x4AD24: 		OneOf Prompt: "Input Clock", Help: "Input Clock", QuestionFlags: 0x10, QuestionId: 0x8C8, VarStoreId: 0xF101, VarOffset: 0xE2, Flags: 0x12, Size: 32, Min: 0x10, Max: 0x40, Step: 0x0 { 05 9A F3 0F 53 0B C8 08 01 F1 E2 00 10 12 10 00 00 00 40 00 00 00 00 00 00 00 }
0x4AD3E: 			OneOfOption Option: "20 MHz" Value: 16, Default { 09 0A 54 0B 12 02 10 00 00 00 }
0x4AD48: 			OneOfOption Option: "24 MHz" Value: 32 { 09 0A 55 0B 02 02 20 00 00 00 }
0x4AD52: 			OneOfOption Option: "26 MHz" Value: 48 { 09 0A 56 0B 02 02 30 00 00 00 }
0x4AD5C: 			OneOfOption Option: "19.2 MHz" Value: 64 { 09 0A 57 0B 02 02 40 00 00 00 }
0x4AD66: 		End  { 29 02 }
0x4AD68: 		OneOf Prompt: "PCH Clock Source", Help: "This option specifies which IMGCLKOUT is chosen", QuestionFlags: 0x10, QuestionId: 0x8C9, VarStoreId: 0xF101, VarOffset: 0xE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 B0 10 94 0D C9 08 01 F1 E6 00 10 10 00 04 00 }
0x4AD79: 			OneOfOption Option: "IMGCLKOUT_0" Value: 0, Default { 09 07 95 0D 10 00 00 }
0x4AD80: 			OneOfOption Option: "IMGCLKOUT_1" Value: 1 { 09 07 96 0D 00 00 01 }
0x4AD87: 			OneOfOption Option: "IMGCLKOUT_2" Value: 2 { 09 07 97 0D 00 00 02 }
0x4AD8E: 			OneOfOption Option: "IMGCLKOUT_3" Value: 3 { 09 07 98 0D 00 00 03 }
0x4AD95: 			OneOfOption Option: "IMGCLKOUT_4" Value: 4 { 09 07 99 0D 00 00 04 }
0x4AD9C: 		End  { 29 02 }
0x4AD9E: 		SuppressIf  { 0A 82 }
0x4ADA0: 			EqIdValList QuestionId: 0x8C7, Values: [48, 80] { 14 8A C7 08 02 00 30 00 50 00 }
0x4ADAA: 				Not  { 17 02 }
0x4ADAC: 			End  { 29 02 }
0x4ADAE: 			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0x8CA, VarStoreId: 0xF101, VarOffset: 0xEB, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0 { 05 91 6E 0C 6E 0C CA 08 01 F1 EB 00 10 10 21 29 00 }
0x4ADBF: 				OneOfOption Option: "Front" Value: 33 { 09 07 6C 0C 00 00 21 }
0x4ADC6: 				OneOfOption Option: "Back" Value: 41, Default { 09 07 6D 0C 10 00 29 }
0x4ADCD: 			End  { 29 02 }
0x4ADCF: 		End  { 29 02 }
0x4ADD1: 		SuppressIf  { 0A 82 }
0x4ADD3: 			EqIdVal QuestionId: 0x8C6, Value: 0x1 { 12 06 C6 08 01 00 }
0x4ADD9: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x8CB, VarStoreId: 0xF101, VarOffset: 0xE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 8F 0B 8F 0B CB 08 01 F1 E8 00 10 10 00 05 00 }
0x4ADEA: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4ADF1: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4ADF8: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4ADFF: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4AE06: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4AE0D: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4AE14: 			End  { 29 02 }
0x4AE16: 			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x8CC, VarStoreId: 0xF101, VarOffset: 0xE9, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 98 0B 98 0B CC 08 01 F1 E9 00 10 21 00 00 7F 00 01 00 }
0x4AE2A: 				Default DefaultId: 0x0 Value: 73 { 5B 07 00 00 01 49 00 }
0x4AE31: 			End  { 29 02 }
0x4AE33: 			SuppressIf  { 0A 82 }
0x4AE35: 				EqIdValList QuestionId: 0x8C6, Values: [2, 3] { 14 8A C6 08 02 00 02 00 03 00 }
0x4AE3F: 					Not  { 17 02 }
0x4AE41: 				End  { 29 02 }
0x4AE43: 				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x8CD, VarStoreId: 0xF101, VarOffset: 0xF1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 00 0C FD 0B CD 08 01 F1 F1 00 10 10 00 04 00 }
0x4AE54: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4AE5B: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4AE62: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4AE69: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4AE70: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4AE77: 				End  { 29 02 }
0x4AE79: 				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8CE, VarStoreId: 0xF101, VarOffset: 0xEC, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 E6 0B E3 0B CE 08 01 F1 EC 00 10 20 00 1F 01 }
0x4AE8A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AE90: 				End  { 29 02 }
0x4AE92: 				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8CF, VarStoreId: 0xF101, VarOffset: 0xED, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F3 0B F0 0B CF 08 01 F1 ED 00 10 20 00 07 01 }
0x4AEA3: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AEA9: 				End  { 29 02 }
0x4AEAB: 				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x8D0, VarStoreId: 0xF101, VarOffset: 0xF2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 05 0C FD 0B D0 08 01 F1 F2 00 10 10 00 04 00 }
0x4AEBC: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4AEC3: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4AECA: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4AED1: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4AED8: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4AEDF: 				End  { 29 02 }
0x4AEE1: 				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8D1, VarStoreId: 0xF101, VarOffset: 0xEE, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 EC 0B E3 0B D1 08 01 F1 EE 00 10 20 00 1F 01 }
0x4AEF2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AEF8: 				End  { 29 02 }
0x4AEFA: 				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8D2, VarStoreId: 0xF101, VarOffset: 0xEF, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F9 0B F0 0B D2 08 01 F1 EF 00 10 20 00 07 01 }
0x4AF0B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AF11: 				End  { 29 02 }
0x4AF13: 				Numeric Prompt: "SubPlatformId", Help: "SubPlatformId", QuestionFlags: 0x10, QuestionId: 0x8D3, VarStoreId: 0xF101, VarOffset: 0xF0, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 5A 0B 5A 0B D3 08 01 F1 F0 00 10 20 00 0F 01 }
0x4AF24: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4AF2A: 				End  { 29 02 }
0x4AF2C: 			End  { 29 02 }
0x4AF2E: 		End  { 29 02 }
0x4AF30: 		SuppressIf  { 0A 82 }
0x4AF32: 			EqIdValList QuestionId: 0x8C6, Values: [253, 254] { 14 0A C6 08 02 00 FD 00 FE 00 }
0x4AF3C: 			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0x8D4, VarStoreId: 0xF101, VarOffset: 0xE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 73 0B 73 0B D4 08 01 F1 E7 00 10 10 00 06 01 }
0x4AF4D: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x4AF53: 			End  { 29 02 }
0x4AF55: 			SuppressIf  { 0A 82 }
0x4AF57: 				EqIdVal QuestionId: 0x8D4, Value: 0x0 { 12 06 D4 08 00 00 }
0x4AF5D: 				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0 { 02 87 8D 0D 00 00 00 }
0x4AF64: 				End  { 29 02 }
0x4AF66: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8D5, VarStoreId: 0xF101, VarOffset: 0xF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 1A 0C 1A 0C D5 08 01 F1 F3 00 10 10 00 17 01 }
0x4AF77: 					Default DefaultId: 0x0 Value: 22 { 5B 06 00 00 00 16 }
0x4AF7D: 				End  { 29 02 }
0x4AF7F: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8D6, VarStoreId: 0xF101, VarOffset: 0xF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 27 0C 27 0C D6 08 01 F1 F9 00 10 10 00 0E 00 }
0x4AF90: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4AF97: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4AF9E: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4AFA5: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4AFAC: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4AFB3: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4AFBA: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4AFC1: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4AFC8: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4AFCF: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4AFD6: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4AFDD: 				End  { 29 02 }
0x4AFDF: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8D7, VarStoreId: 0xF101, VarOffset: 0xFF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 0D 0C 0D 0C D7 08 01 F1 FF 00 10 10 00 12 00 }
0x4AFF0: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4AFF7: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4AFFE: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B005: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B00C: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B013: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B01A: 				End  { 29 02 }
0x4B01C: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8D8, VarStoreId: 0xF101, VarOffset: 0x105, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 34 0C 34 0C D8 08 01 F1 05 01 10 10 00 01 01 }
0x4B02D: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B033: 				End  { 29 02 }
0x4B035: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8D9, VarStoreId: 0xF101, VarOffset: 0x10B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 41 0C 41 0C D9 08 01 F1 0B 01 10 10 00 01 01 }
0x4B046: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B04C: 				End  { 29 02 }
0x4B04E: 			End  { 29 02 }
0x4B050: 			SuppressIf  { 0A 82 }
0x4B052: 				EqIdValList QuestionId: 0x8D4, Values: [0, 1] { 14 0A D4 08 02 00 00 00 01 00 }
0x4B05C: 				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0 { 02 87 8E 0D 00 00 00 }
0x4B063: 				End  { 29 02 }
0x4B065: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8DA, VarStoreId: 0xF101, VarOffset: 0xF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 21 10 1A 0C DA 08 01 F1 F4 00 10 10 00 17 01 }
0x4B076: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4B07C: 				End  { 29 02 }
0x4B07E: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8DB, VarStoreId: 0xF101, VarOffset: 0xFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 30 10 27 0C DB 08 01 F1 FA 00 10 10 00 0E 00 }
0x4B08F: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B096: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B09D: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B0A4: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B0AB: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B0B2: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B0B9: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B0C0: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B0C7: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B0CE: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B0D5: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B0DC: 				End  { 29 02 }
0x4B0DE: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8DC, VarStoreId: 0xF101, VarOffset: 0x100, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 12 10 0D 0C DC 08 01 F1 00 01 10 10 00 12 00 }
0x4B0EF: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B0F6: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B0FD: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B104: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B10B: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B112: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B119: 				End  { 29 02 }
0x4B11B: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8DD, VarStoreId: 0xF101, VarOffset: 0x106, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4B 10 34 0C DD 08 01 F1 06 01 10 10 00 01 01 }
0x4B12C: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B132: 				End  { 29 02 }
0x4B134: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8DE, VarStoreId: 0xF101, VarOffset: 0x10C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 60 10 41 0C DE 08 01 F1 0C 01 10 10 00 01 01 }
0x4B145: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B14B: 				End  { 29 02 }
0x4B14D: 			End  { 29 02 }
0x4B14F: 			SuppressIf  { 0A 82 }
0x4B151: 				EqIdValList QuestionId: 0x8D4, Values: [0, 1, 2] { 14 0C D4 08 03 00 00 00 01 00 02 00 }
0x4B15D: 				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0 { 02 87 8F 0D 00 00 00 }
0x4B164: 				End  { 29 02 }
0x4B166: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8DF, VarStoreId: 0xF101, VarOffset: 0xF5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 22 10 1A 0C DF 08 01 F1 F5 00 10 10 00 17 01 }
0x4B177: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4B17D: 				End  { 29 02 }
0x4B17F: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8E0, VarStoreId: 0xF101, VarOffset: 0xFB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 31 10 27 0C E0 08 01 F1 FB 00 10 10 00 0E 00 }
0x4B190: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B197: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B19E: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B1A5: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B1AC: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B1B3: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B1BA: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B1C1: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B1C8: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B1CF: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B1D6: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B1DD: 				End  { 29 02 }
0x4B1DF: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8E1, VarStoreId: 0xF101, VarOffset: 0x101, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 13 10 0D 0C E1 08 01 F1 01 01 10 10 00 12 00 }
0x4B1F0: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B1F7: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B1FE: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B205: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B20C: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B213: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B21A: 				End  { 29 02 }
0x4B21C: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8E2, VarStoreId: 0xF101, VarOffset: 0x107, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4C 10 34 0C E2 08 01 F1 07 01 10 10 00 01 01 }
0x4B22D: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B233: 				End  { 29 02 }
0x4B235: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8E3, VarStoreId: 0xF101, VarOffset: 0x10D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 61 10 41 0C E3 08 01 F1 0D 01 10 10 00 01 01 }
0x4B246: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B24C: 				End  { 29 02 }
0x4B24E: 			End  { 29 02 }
0x4B250: 			SuppressIf  { 0A 82 }
0x4B252: 				EqIdValList QuestionId: 0x8D4, Values: [0, 1, 2, 3] { 14 0E D4 08 04 00 00 00 01 00 02 00 03 00 }
0x4B260: 				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0 { 02 87 90 0D 00 00 00 }
0x4B267: 				End  { 29 02 }
0x4B269: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8E4, VarStoreId: 0xF101, VarOffset: 0xF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 23 10 1A 0C E4 08 01 F1 F6 00 10 10 00 17 01 }
0x4B27A: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4B280: 				End  { 29 02 }
0x4B282: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8E5, VarStoreId: 0xF101, VarOffset: 0xFC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 32 10 27 0C E5 08 01 F1 FC 00 10 10 00 0E 00 }
0x4B293: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B29A: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B2A1: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B2A8: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B2AF: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B2B6: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B2BD: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B2C4: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B2CB: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B2D2: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B2D9: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B2E0: 				End  { 29 02 }
0x4B2E2: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8E6, VarStoreId: 0xF101, VarOffset: 0x102, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 14 10 0D 0C E6 08 01 F1 02 01 10 10 00 12 00 }
0x4B2F3: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B2FA: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B301: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B308: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B30F: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B316: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B31D: 				End  { 29 02 }
0x4B31F: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8E7, VarStoreId: 0xF101, VarOffset: 0x108, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4D 10 34 0C E7 08 01 F1 08 01 10 10 00 01 01 }
0x4B330: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B336: 				End  { 29 02 }
0x4B338: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8E8, VarStoreId: 0xF101, VarOffset: 0x10E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 62 10 41 0C E8 08 01 F1 0E 01 10 10 00 01 01 }
0x4B349: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B34F: 				End  { 29 02 }
0x4B351: 			End  { 29 02 }
0x4B353: 			SuppressIf  { 0A 82 }
0x4B355: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3, 4] { 14 10 A7 08 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4B365: 				Subtitle Prompt: "GPIO 4", Help: "", Flags: 0x0 { 02 87 91 0D 00 00 00 }
0x4B36C: 				End  { 29 02 }
0x4B36E: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8E9, VarStoreId: 0xF101, VarOffset: 0xF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 24 10 1A 0C E9 08 01 F1 F7 00 10 10 00 17 01 }
0x4B37F: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4B385: 				End  { 29 02 }
0x4B387: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8EA, VarStoreId: 0xF101, VarOffset: 0xFD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 33 10 27 0C EA 08 01 F1 FD 00 10 10 00 0E 00 }
0x4B398: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B39F: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B3A6: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B3AD: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B3B4: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B3BB: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B3C2: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B3C9: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B3D0: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B3D7: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B3DE: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B3E5: 				End  { 29 02 }
0x4B3E7: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8EB, VarStoreId: 0xF101, VarOffset: 0x103, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 15 10 0D 0C EB 08 01 F1 03 01 10 10 00 12 00 }
0x4B3F8: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B3FF: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B406: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B40D: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B414: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B41B: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B422: 				End  { 29 02 }
0x4B424: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8EC, VarStoreId: 0xF101, VarOffset: 0x109, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4E 10 34 0C EC 08 01 F1 09 01 10 10 00 01 01 }
0x4B435: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B43B: 				End  { 29 02 }
0x4B43D: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8ED, VarStoreId: 0xF101, VarOffset: 0x10F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 63 10 41 0C ED 08 01 F1 0F 01 10 10 00 01 01 }
0x4B44E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B454: 				End  { 29 02 }
0x4B456: 			End  { 29 02 }
0x4B458: 			SuppressIf  { 0A 82 }
0x4B45A: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3, 4, 5] { 14 12 A7 08 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4B46C: 				Subtitle Prompt: "GPIO 5", Help: "", Flags: 0x0 { 02 87 92 0D 00 00 00 }
0x4B473: 				End  { 29 02 }
0x4B475: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x8EE, VarStoreId: 0xF101, VarOffset: 0xF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 25 10 1A 0C EE 08 01 F1 F8 00 10 10 00 17 01 }
0x4B486: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4B48C: 				End  { 29 02 }
0x4B48E: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x8EF, VarStoreId: 0xF101, VarOffset: 0xFE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 34 10 27 0C EF 08 01 F1 FE 00 10 10 00 0E 00 }
0x4B49F: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B4A6: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B4AD: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B4B4: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B4BB: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B4C2: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B4C9: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B4D0: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B4D7: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B4DE: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B4E5: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B4EC: 				End  { 29 02 }
0x4B4EE: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x8F0, VarStoreId: 0xF101, VarOffset: 0x104, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 16 10 0D 0C F0 08 01 F1 04 01 10 10 00 12 00 }
0x4B4FF: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B506: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B50D: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B514: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B51B: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B522: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B529: 				End  { 29 02 }
0x4B52B: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x8F1, VarStoreId: 0xF101, VarOffset: 0x10A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 4F 10 34 0C F1 08 01 F1 0A 01 10 10 00 01 01 }
0x4B53C: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B542: 				End  { 29 02 }
0x4B544: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x8F2, VarStoreId: 0xF101, VarOffset: 0x110, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 64 10 41 0C F2 08 01 F1 10 01 10 10 00 01 01 }
0x4B555: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B55B: 				End  { 29 02 }
0x4B55D: 			End  { 29 02 }
0x4B55F: 		End  { 29 02 }
0x4B561: 	End  { 29 02 }
0x4B563: 	Form FormId: 0x96, Title: "Control Logic options" { 01 86 96 00 21 0D }
0x4B569: 		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0 { 02 87 21 0D 00 00 00 }
0x4B570: 		End  { 29 02 }
0x4B572: 		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0x8F3, VarStoreId: 0xF101, VarOffset: 0x111, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0 { 05 91 AC 10 85 0D F3 08 01 F1 11 01 10 10 01 FE 00 }
0x4B583: 			OneOfOption Option: "Discrete" Value: 1 { 09 07 88 0D 00 00 01 }
0x4B58A: 			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default { 09 07 89 0D 10 00 02 }
0x4B591: 			OneOfOption Option: "PMIC_UP6641" Value: 3 { 09 07 8A 0D 00 00 03 }
0x4B598: 			OneOfOption Option: "PMIC_USER0" Value: 253 { 09 07 8B 0D 00 00 FD }
0x4B59F: 			OneOfOption Option: "PMIC_USER1" Value: 254 { 09 07 8C 0D 00 00 FE }
0x4B5A6: 		End  { 29 02 }
0x4B5A8: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x8F4, VarStoreId: 0xF101, VarOffset: 0x112, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 95 10 A9 0C F4 08 01 F1 12 01 10 10 10 50 00 }
0x4B5B9: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x4B5C0: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x4B5C7: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x4B5CE: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x4B5D5: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x4B5DC: 		End  { 29 02 }
0x4B5DE: 		OneOf Prompt: "Input Clock", Help: "Input Clock", QuestionFlags: 0x10, QuestionId: 0x8F5, VarStoreId: 0xF101, VarOffset: 0x113, Flags: 0x12, Size: 32, Min: 0x10, Max: 0x40, Step: 0x0 { 05 9A F4 0F 53 0B F5 08 01 F1 13 01 10 12 10 00 00 00 40 00 00 00 00 00 00 00 }
0x4B5F8: 			OneOfOption Option: "20 MHz" Value: 16, Default { 09 0A 54 0B 12 02 10 00 00 00 }
0x4B602: 			OneOfOption Option: "24 MHz" Value: 32 { 09 0A 55 0B 02 02 20 00 00 00 }
0x4B60C: 			OneOfOption Option: "26 MHz" Value: 48 { 09 0A 56 0B 02 02 30 00 00 00 }
0x4B616: 			OneOfOption Option: "19.2 MHz" Value: 64 { 09 0A 57 0B 02 02 40 00 00 00 }
0x4B620: 		End  { 29 02 }
0x4B622: 		OneOf Prompt: "PCH Clock Source", Help: "This option specifies which IMGCLKOUT is chosen", QuestionFlags: 0x10, QuestionId: 0x8F6, VarStoreId: 0xF101, VarOffset: 0x117, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 B1 10 94 0D F6 08 01 F1 17 01 10 10 00 04 00 }
0x4B633: 			OneOfOption Option: "IMGCLKOUT_0" Value: 0, Default { 09 07 95 0D 10 00 00 }
0x4B63A: 			OneOfOption Option: "IMGCLKOUT_1" Value: 1 { 09 07 96 0D 00 00 01 }
0x4B641: 			OneOfOption Option: "IMGCLKOUT_2" Value: 2 { 09 07 97 0D 00 00 02 }
0x4B648: 			OneOfOption Option: "IMGCLKOUT_3" Value: 3 { 09 07 98 0D 00 00 03 }
0x4B64F: 			OneOfOption Option: "IMGCLKOUT_4" Value: 4 { 09 07 99 0D 00 00 04 }
0x4B656: 		End  { 29 02 }
0x4B658: 		SuppressIf  { 0A 82 }
0x4B65A: 			EqIdValList QuestionId: 0x8F4, Values: [48, 80] { 14 8A F4 08 02 00 30 00 50 00 }
0x4B664: 				Not  { 17 02 }
0x4B666: 			End  { 29 02 }
0x4B668: 			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0x8F7, VarStoreId: 0xF101, VarOffset: 0x11C, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0 { 05 91 87 10 6E 0C F7 08 01 F1 1C 01 10 10 21 29 00 }
0x4B679: 				OneOfOption Option: "Front" Value: 33 { 09 07 6C 0C 00 00 21 }
0x4B680: 				OneOfOption Option: "Back" Value: 41, Default { 09 07 6D 0C 10 00 29 }
0x4B687: 			End  { 29 02 }
0x4B689: 		End  { 29 02 }
0x4B68B: 		SuppressIf  { 0A 82 }
0x4B68D: 			EqIdVal QuestionId: 0x8F3, Value: 0x1 { 12 06 F3 08 01 00 }
0x4B693: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x8F8, VarStoreId: 0xF101, VarOffset: 0x119, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 FF 0F 8F 0B F8 08 01 F1 19 01 10 10 00 05 00 }
0x4B6A4: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4B6AB: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4B6B2: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4B6B9: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4B6C0: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4B6C7: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4B6CE: 			End  { 29 02 }
0x4B6D0: 			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x8F9, VarStoreId: 0xF101, VarOffset: 0x11A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 08 10 98 0B F9 08 01 F1 1A 01 10 21 00 00 7F 00 01 00 }
0x4B6E4: 				Default DefaultId: 0x0 Value: 73 { 5B 07 00 00 01 49 00 }
0x4B6EB: 			End  { 29 02 }
0x4B6ED: 			SuppressIf  { 0A 82 }
0x4B6EF: 				EqIdValList QuestionId: 0x8F3, Values: [2, 3] { 14 8A F3 08 02 00 02 00 03 00 }
0x4B6F9: 					Not  { 17 02 }
0x4B6FB: 				End  { 29 02 }
0x4B6FD: 				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x8FA, VarStoreId: 0xF101, VarOffset: 0x122, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 01 0C FD 0B FA 08 01 F1 22 01 10 10 00 04 00 }
0x4B70E: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4B715: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4B71C: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4B723: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4B72A: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4B731: 				End  { 29 02 }
0x4B733: 				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8FB, VarStoreId: 0xF101, VarOffset: 0x11D, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 E7 0B E3 0B FB 08 01 F1 1D 01 10 20 00 1F 01 }
0x4B744: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B74A: 				End  { 29 02 }
0x4B74C: 				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8FC, VarStoreId: 0xF101, VarOffset: 0x11E, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F4 0B F0 0B FC 08 01 F1 1E 01 10 20 00 07 01 }
0x4B75D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B763: 				End  { 29 02 }
0x4B765: 				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x8FD, VarStoreId: 0xF101, VarOffset: 0x123, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 06 0C FD 0B FD 08 01 F1 23 01 10 10 00 04 00 }
0x4B776: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4B77D: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4B784: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4B78B: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4B792: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4B799: 				End  { 29 02 }
0x4B79B: 				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8FE, VarStoreId: 0xF101, VarOffset: 0x11F, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 ED 0B E3 0B FE 08 01 F1 1F 01 10 20 00 1F 01 }
0x4B7AC: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B7B2: 				End  { 29 02 }
0x4B7B4: 				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x8FF, VarStoreId: 0xF101, VarOffset: 0x120, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 FA 0B F0 0B FF 08 01 F1 20 01 10 20 00 07 01 }
0x4B7C5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B7CB: 				End  { 29 02 }
0x4B7CD: 				Numeric Prompt: "SubPlatformId", Help: "SubPlatformId", QuestionFlags: 0x10, QuestionId: 0x900, VarStoreId: 0xF101, VarOffset: 0x121, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 5B 0B 5B 0B 00 09 01 F1 21 01 10 20 00 0F 01 }
0x4B7DE: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B7E4: 				End  { 29 02 }
0x4B7E6: 			End  { 29 02 }
0x4B7E8: 		End  { 29 02 }
0x4B7EA: 		SuppressIf  { 0A 82 }
0x4B7EC: 			EqIdValList QuestionId: 0x8F3, Values: [253, 254] { 14 0A F3 08 02 00 FD 00 FE 00 }
0x4B7F6: 			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0x901, VarStoreId: 0xF101, VarOffset: 0x118, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 FC 0F 73 0B 01 09 01 F1 18 01 10 10 00 06 01 }
0x4B807: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x4B80D: 			End  { 29 02 }
0x4B80F: 			SuppressIf  { 0A 82 }
0x4B811: 				EqIdVal QuestionId: 0x901, Value: 0x0 { 12 06 01 09 00 00 }
0x4B817: 				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0 { 02 87 8D 0D 00 00 00 }
0x4B81E: 				End  { 29 02 }
0x4B820: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x902, VarStoreId: 0xF101, VarOffset: 0x124, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 26 10 1A 0C 02 09 01 F1 24 01 10 10 00 17 01 }
0x4B831: 					Default DefaultId: 0x0 Value: 22 { 5B 06 00 00 00 16 }
0x4B837: 				End  { 29 02 }
0x4B839: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x903, VarStoreId: 0xF101, VarOffset: 0x12A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 35 10 27 0C 03 09 01 F1 2A 01 10 10 00 0E 00 }
0x4B84A: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B851: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B858: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B85F: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B866: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B86D: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B874: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B87B: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B882: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B889: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B890: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B897: 				End  { 29 02 }
0x4B899: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x904, VarStoreId: 0xF101, VarOffset: 0x130, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 17 10 0D 0C 04 09 01 F1 30 01 10 10 00 12 00 }
0x4B8AA: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B8B1: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B8B8: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B8BF: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B8C6: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B8CD: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B8D4: 				End  { 29 02 }
0x4B8D6: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x905, VarStoreId: 0xF101, VarOffset: 0x136, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 50 10 34 0C 05 09 01 F1 36 01 10 10 00 01 01 }
0x4B8E7: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B8ED: 				End  { 29 02 }
0x4B8EF: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x906, VarStoreId: 0xF101, VarOffset: 0x13C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 65 10 41 0C 06 09 01 F1 3C 01 10 10 00 01 01 }
0x4B900: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4B906: 				End  { 29 02 }
0x4B908: 			End  { 29 02 }
0x4B90A: 			SuppressIf  { 0A 82 }
0x4B90C: 				EqIdValList QuestionId: 0x901, Values: [0, 1] { 14 0A 01 09 02 00 00 00 01 00 }
0x4B916: 				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0 { 02 87 8E 0D 00 00 00 }
0x4B91D: 				End  { 29 02 }
0x4B91F: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x907, VarStoreId: 0xF101, VarOffset: 0x125, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 27 10 1A 0C 07 09 01 F1 25 01 10 10 00 17 01 }
0x4B930: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4B936: 				End  { 29 02 }
0x4B938: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x908, VarStoreId: 0xF101, VarOffset: 0x12B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 36 10 27 0C 08 09 01 F1 2B 01 10 10 00 0E 00 }
0x4B949: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4B950: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4B957: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4B95E: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4B965: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4B96C: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4B973: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4B97A: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4B981: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4B988: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4B98F: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4B996: 				End  { 29 02 }
0x4B998: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x909, VarStoreId: 0xF101, VarOffset: 0x131, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 18 10 0D 0C 09 09 01 F1 31 01 10 10 00 12 00 }
0x4B9A9: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4B9B0: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4B9B7: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4B9BE: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4B9C5: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4B9CC: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4B9D3: 				End  { 29 02 }
0x4B9D5: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x90A, VarStoreId: 0xF101, VarOffset: 0x137, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 51 10 34 0C 0A 09 01 F1 37 01 10 10 00 01 01 }
0x4B9E6: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4B9EC: 				End  { 29 02 }
0x4B9EE: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x90B, VarStoreId: 0xF101, VarOffset: 0x13D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 66 10 41 0C 0B 09 01 F1 3D 01 10 10 00 01 01 }
0x4B9FF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4BA05: 				End  { 29 02 }
0x4BA07: 			End  { 29 02 }
0x4BA09: 			SuppressIf  { 0A 82 }
0x4BA0B: 				EqIdValList QuestionId: 0x901, Values: [0, 1, 2] { 14 0C 01 09 03 00 00 00 01 00 02 00 }
0x4BA17: 				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0 { 02 87 8F 0D 00 00 00 }
0x4BA1E: 				End  { 29 02 }
0x4BA20: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x90C, VarStoreId: 0xF101, VarOffset: 0x126, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 28 10 1A 0C 0C 09 01 F1 26 01 10 10 00 17 01 }
0x4BA31: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4BA37: 				End  { 29 02 }
0x4BA39: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x90D, VarStoreId: 0xF101, VarOffset: 0x12C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 37 10 27 0C 0D 09 01 F1 2C 01 10 10 00 0E 00 }
0x4BA4A: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4BA51: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4BA58: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4BA5F: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4BA66: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4BA6D: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4BA74: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4BA7B: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4BA82: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4BA89: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4BA90: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4BA97: 				End  { 29 02 }
0x4BA99: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x90E, VarStoreId: 0xF101, VarOffset: 0x132, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 19 10 0D 0C 0E 09 01 F1 32 01 10 10 00 12 00 }
0x4BAAA: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4BAB1: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4BAB8: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4BABF: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4BAC6: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4BACD: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4BAD4: 				End  { 29 02 }
0x4BAD6: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x90F, VarStoreId: 0xF101, VarOffset: 0x138, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 52 10 34 0C 0F 09 01 F1 38 01 10 10 00 01 01 }
0x4BAE7: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4BAED: 				End  { 29 02 }
0x4BAEF: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x910, VarStoreId: 0xF101, VarOffset: 0x13E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 67 10 41 0C 10 09 01 F1 3E 01 10 10 00 01 01 }
0x4BB00: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4BB06: 				End  { 29 02 }
0x4BB08: 			End  { 29 02 }
0x4BB0A: 			SuppressIf  { 0A 82 }
0x4BB0C: 				EqIdValList QuestionId: 0x901, Values: [0, 1, 2, 3] { 14 0E 01 09 04 00 00 00 01 00 02 00 03 00 }
0x4BB1A: 				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0 { 02 87 90 0D 00 00 00 }
0x4BB21: 				End  { 29 02 }
0x4BB23: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x911, VarStoreId: 0xF101, VarOffset: 0x127, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 29 10 1A 0C 11 09 01 F1 27 01 10 10 00 17 01 }
0x4BB34: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4BB3A: 				End  { 29 02 }
0x4BB3C: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x912, VarStoreId: 0xF101, VarOffset: 0x12D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 38 10 27 0C 12 09 01 F1 2D 01 10 10 00 0E 00 }
0x4BB4D: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4BB54: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4BB5B: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4BB62: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4BB69: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4BB70: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4BB77: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4BB7E: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4BB85: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4BB8C: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4BB93: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4BB9A: 				End  { 29 02 }
0x4BB9C: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x913, VarStoreId: 0xF101, VarOffset: 0x133, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 1A 10 0D 0C 13 09 01 F1 33 01 10 10 00 12 00 }
0x4BBAD: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4BBB4: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4BBBB: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4BBC2: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4BBC9: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4BBD0: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4BBD7: 				End  { 29 02 }
0x4BBD9: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x914, VarStoreId: 0xF101, VarOffset: 0x139, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 53 10 34 0C 14 09 01 F1 39 01 10 10 00 01 01 }
0x4BBEA: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4BBF0: 				End  { 29 02 }
0x4BBF2: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x915, VarStoreId: 0xF101, VarOffset: 0x13F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 68 10 41 0C 15 09 01 F1 3F 01 10 10 00 01 01 }
0x4BC03: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4BC09: 				End  { 29 02 }
0x4BC0B: 			End  { 29 02 }
0x4BC0D: 			SuppressIf  { 0A 82 }
0x4BC0F: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3, 4] { 14 10 A7 08 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4BC1F: 				Subtitle Prompt: "GPIO 4", Help: "", Flags: 0x0 { 02 87 91 0D 00 00 00 }
0x4BC26: 				End  { 29 02 }
0x4BC28: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x916, VarStoreId: 0xF101, VarOffset: 0x128, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 2A 10 1A 0C 16 09 01 F1 28 01 10 10 00 17 01 }
0x4BC39: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4BC3F: 				End  { 29 02 }
0x4BC41: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x917, VarStoreId: 0xF101, VarOffset: 0x12E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 39 10 27 0C 17 09 01 F1 2E 01 10 10 00 0E 00 }
0x4BC52: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4BC59: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4BC60: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4BC67: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4BC6E: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4BC75: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4BC7C: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4BC83: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4BC8A: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4BC91: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4BC98: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4BC9F: 				End  { 29 02 }
0x4BCA1: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x918, VarStoreId: 0xF101, VarOffset: 0x134, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 1B 10 0D 0C 18 09 01 F1 34 01 10 10 00 12 00 }
0x4BCB2: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4BCB9: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4BCC0: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4BCC7: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4BCCE: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4BCD5: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4BCDC: 				End  { 29 02 }
0x4BCDE: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x919, VarStoreId: 0xF101, VarOffset: 0x13A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 54 10 34 0C 19 09 01 F1 3A 01 10 10 00 01 01 }
0x4BCEF: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4BCF5: 				End  { 29 02 }
0x4BCF7: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x91A, VarStoreId: 0xF101, VarOffset: 0x140, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 69 10 41 0C 1A 09 01 F1 40 01 10 10 00 01 01 }
0x4BD08: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4BD0E: 				End  { 29 02 }
0x4BD10: 			End  { 29 02 }
0x4BD12: 			SuppressIf  { 0A 82 }
0x4BD14: 				EqIdValList QuestionId: 0x8A7, Values: [0, 1, 2, 3, 4, 5] { 14 12 A7 08 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4BD26: 				Subtitle Prompt: "GPIO 5", Help: "", Flags: 0x0 { 02 87 92 0D 00 00 00 }
0x4BD2D: 				End  { 29 02 }
0x4BD2F: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x91B, VarStoreId: 0xF101, VarOffset: 0x129, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 2B 10 1A 0C 1B 09 01 F1 29 01 10 10 00 17 01 }
0x4BD40: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4BD46: 				End  { 29 02 }
0x4BD48: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x91C, VarStoreId: 0xF101, VarOffset: 0x12F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 3A 10 27 0C 1C 09 01 F1 2F 01 10 10 00 0E 00 }
0x4BD59: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4BD60: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4BD67: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4BD6E: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4BD75: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4BD7C: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4BD83: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4BD8A: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4BD91: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4BD98: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4BD9F: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4BDA6: 				End  { 29 02 }
0x4BDA8: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x91D, VarStoreId: 0xF101, VarOffset: 0x135, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 1C 10 0D 0C 1D 09 01 F1 35 01 10 10 00 12 00 }
0x4BDB9: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4BDC0: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4BDC7: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4BDCE: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4BDD5: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4BDDC: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4BDE3: 				End  { 29 02 }
0x4BDE5: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x91E, VarStoreId: 0xF101, VarOffset: 0x13B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 55 10 34 0C 1E 09 01 F1 3B 01 10 10 00 01 01 }
0x4BDF6: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4BDFC: 				End  { 29 02 }
0x4BDFE: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x91F, VarStoreId: 0xF101, VarOffset: 0x141, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 6A 10 41 0C 1F 09 01 F1 41 01 10 10 00 01 01 }
0x4BE0F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4BE15: 				End  { 29 02 }
0x4BE17: 			End  { 29 02 }
0x4BE19: 		End  { 29 02 }
0x4BE1B: 	End  { 29 02 }
0x4BE1D: 	Form FormId: 0x97, Title: "Control Logic options" { 01 86 97 00 21 0D }
0x4BE23: 		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0 { 02 87 21 0D 00 00 00 }
0x4BE2A: 		End  { 29 02 }
0x4BE2C: 		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0x920, VarStoreId: 0xF101, VarOffset: 0x142, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0 { 05 91 AD 10 85 0D 20 09 01 F1 42 01 10 10 01 FE 00 }
0x4BE3D: 			OneOfOption Option: "Discrete" Value: 1 { 09 07 88 0D 00 00 01 }
0x4BE44: 			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default { 09 07 89 0D 10 00 02 }
0x4BE4B: 			OneOfOption Option: "PMIC_UP6641" Value: 3 { 09 07 8A 0D 00 00 03 }
0x4BE52: 			OneOfOption Option: "PMIC_USER0" Value: 253 { 09 07 8B 0D 00 00 FD }
0x4BE59: 			OneOfOption Option: "PMIC_USER1" Value: 254 { 09 07 8C 0D 00 00 FE }
0x4BE60: 		End  { 29 02 }
0x4BE62: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x921, VarStoreId: 0xF101, VarOffset: 0x143, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 96 10 A9 0C 21 09 01 F1 43 01 10 10 10 50 00 }
0x4BE73: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x4BE7A: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x4BE81: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x4BE88: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x4BE8F: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x4BE96: 		End  { 29 02 }
0x4BE98: 		OneOf Prompt: "Input Clock", Help: "Input Clock", QuestionFlags: 0x10, QuestionId: 0x922, VarStoreId: 0xF101, VarOffset: 0x144, Flags: 0x12, Size: 32, Min: 0x10, Max: 0x40, Step: 0x0 { 05 9A F5 0F 53 0B 22 09 01 F1 44 01 10 12 10 00 00 00 40 00 00 00 00 00 00 00 }
0x4BEB2: 			OneOfOption Option: "20 MHz" Value: 16, Default { 09 0A 54 0B 12 02 10 00 00 00 }
0x4BEBC: 			OneOfOption Option: "24 MHz" Value: 32 { 09 0A 55 0B 02 02 20 00 00 00 }
0x4BEC6: 			OneOfOption Option: "26 MHz" Value: 48 { 09 0A 56 0B 02 02 30 00 00 00 }
0x4BED0: 			OneOfOption Option: "19.2 MHz" Value: 64 { 09 0A 57 0B 02 02 40 00 00 00 }
0x4BEDA: 		End  { 29 02 }
0x4BEDC: 		OneOf Prompt: "PCH Clock Source", Help: "This option specifies which IMGCLKOUT is chosen", QuestionFlags: 0x10, QuestionId: 0x923, VarStoreId: 0xF101, VarOffset: 0x148, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 B2 10 94 0D 23 09 01 F1 48 01 10 10 00 04 00 }
0x4BEED: 			OneOfOption Option: "IMGCLKOUT_0" Value: 0, Default { 09 07 95 0D 10 00 00 }
0x4BEF4: 			OneOfOption Option: "IMGCLKOUT_1" Value: 1 { 09 07 96 0D 00 00 01 }
0x4BEFB: 			OneOfOption Option: "IMGCLKOUT_2" Value: 2 { 09 07 97 0D 00 00 02 }
0x4BF02: 			OneOfOption Option: "IMGCLKOUT_3" Value: 3 { 09 07 98 0D 00 00 03 }
0x4BF09: 			OneOfOption Option: "IMGCLKOUT_4" Value: 4 { 09 07 99 0D 00 00 04 }
0x4BF10: 		End  { 29 02 }
0x4BF12: 		SuppressIf  { 0A 82 }
0x4BF14: 			EqIdValList QuestionId: 0x921, Values: [48, 80] { 14 8A 21 09 02 00 30 00 50 00 }
0x4BF1E: 				Not  { 17 02 }
0x4BF20: 			End  { 29 02 }
0x4BF22: 			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0x924, VarStoreId: 0xF101, VarOffset: 0x14D, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0 { 05 91 88 10 6E 0C 24 09 01 F1 4D 01 10 10 21 29 00 }
0x4BF33: 				OneOfOption Option: "Front" Value: 33 { 09 07 6C 0C 00 00 21 }
0x4BF3A: 				OneOfOption Option: "Back" Value: 41, Default { 09 07 6D 0C 10 00 29 }
0x4BF41: 			End  { 29 02 }
0x4BF43: 		End  { 29 02 }
0x4BF45: 		SuppressIf  { 0A 82 }
0x4BF47: 			EqIdVal QuestionId: 0x920, Value: 0x1 { 12 06 20 09 01 00 }
0x4BF4D: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x925, VarStoreId: 0xF101, VarOffset: 0x14A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 00 10 8F 0B 25 09 01 F1 4A 01 10 10 00 05 00 }
0x4BF5E: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4BF65: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4BF6C: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4BF73: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4BF7A: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4BF81: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4BF88: 			End  { 29 02 }
0x4BF8A: 			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x926, VarStoreId: 0xF101, VarOffset: 0x14B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 09 10 98 0B 26 09 01 F1 4B 01 10 21 00 00 7F 00 01 00 }
0x4BF9E: 				Default DefaultId: 0x0 Value: 73 { 5B 07 00 00 01 49 00 }
0x4BFA5: 			End  { 29 02 }
0x4BFA7: 			SuppressIf  { 0A 82 }
0x4BFA9: 				EqIdValList QuestionId: 0x920, Values: [2, 3] { 14 8A 20 09 02 00 02 00 03 00 }
0x4BFB3: 					Not  { 17 02 }
0x4BFB5: 				End  { 29 02 }
0x4BFB7: 				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x927, VarStoreId: 0xF101, VarOffset: 0x153, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 02 0C FD 0B 27 09 01 F1 53 01 10 10 00 04 00 }
0x4BFC8: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4BFCF: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4BFD6: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4BFDD: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4BFE4: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4BFEB: 				End  { 29 02 }
0x4BFED: 				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x928, VarStoreId: 0xF101, VarOffset: 0x14E, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 E8 0B E3 0B 28 09 01 F1 4E 01 10 20 00 1F 01 }
0x4BFFE: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C004: 				End  { 29 02 }
0x4C006: 				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x929, VarStoreId: 0xF101, VarOffset: 0x14F, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F5 0B F0 0B 29 09 01 F1 4F 01 10 20 00 07 01 }
0x4C017: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C01D: 				End  { 29 02 }
0x4C01F: 				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x92A, VarStoreId: 0xF101, VarOffset: 0x154, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 07 0C FD 0B 2A 09 01 F1 54 01 10 10 00 04 00 }
0x4C030: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4C037: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4C03E: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4C045: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4C04C: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4C053: 				End  { 29 02 }
0x4C055: 				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x92B, VarStoreId: 0xF101, VarOffset: 0x150, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 EE 0B E3 0B 2B 09 01 F1 50 01 10 20 00 1F 01 }
0x4C066: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C06C: 				End  { 29 02 }
0x4C06E: 				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x92C, VarStoreId: 0xF101, VarOffset: 0x151, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 FB 0B F0 0B 2C 09 01 F1 51 01 10 20 00 07 01 }
0x4C07F: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C085: 				End  { 29 02 }
0x4C087: 				Numeric Prompt: "SubPlatformId", Help: "SubPlatformId", QuestionFlags: 0x10, QuestionId: 0x92D, VarStoreId: 0xF101, VarOffset: 0x152, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 5C 0B 5C 0B 2D 09 01 F1 52 01 10 20 00 0F 01 }
0x4C098: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C09E: 				End  { 29 02 }
0x4C0A0: 			End  { 29 02 }
0x4C0A2: 		End  { 29 02 }
0x4C0A4: 		SuppressIf  { 0A 82 }
0x4C0A6: 			EqIdValList QuestionId: 0x920, Values: [253, 254] { 14 0A 20 09 02 00 FD 00 FE 00 }
0x4C0B0: 			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0x92E, VarStoreId: 0xF101, VarOffset: 0x149, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 FD 0F 73 0B 2E 09 01 F1 49 01 10 10 00 06 01 }
0x4C0C1: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x4C0C7: 			End  { 29 02 }
0x4C0C9: 			SuppressIf  { 0A 82 }
0x4C0CB: 				EqIdVal QuestionId: 0x92E, Value: 0x0 { 12 06 2E 09 00 00 }
0x4C0D1: 				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0 { 02 87 8D 0D 00 00 00 }
0x4C0D8: 				End  { 29 02 }
0x4C0DA: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x92F, VarStoreId: 0xF101, VarOffset: 0x155, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 2C 10 1A 0C 2F 09 01 F1 55 01 10 10 00 17 01 }
0x4C0EB: 					Default DefaultId: 0x0 Value: 22 { 5B 06 00 00 00 16 }
0x4C0F1: 				End  { 29 02 }
0x4C0F3: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x930, VarStoreId: 0xF101, VarOffset: 0x15B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 3B 10 27 0C 30 09 01 F1 5B 01 10 10 00 0E 00 }
0x4C104: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C10B: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C112: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C119: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C120: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C127: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C12E: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C135: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C13C: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C143: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4C14A: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4C151: 				End  { 29 02 }
0x4C153: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x931, VarStoreId: 0xF101, VarOffset: 0x161, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 1D 10 0D 0C 31 09 01 F1 61 01 10 10 00 12 00 }
0x4C164: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4C16B: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4C172: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4C179: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4C180: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4C187: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4C18E: 				End  { 29 02 }
0x4C190: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x932, VarStoreId: 0xF101, VarOffset: 0x167, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 56 10 34 0C 32 09 01 F1 67 01 10 10 00 01 01 }
0x4C1A1: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4C1A7: 				End  { 29 02 }
0x4C1A9: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x933, VarStoreId: 0xF101, VarOffset: 0x16D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 6B 10 41 0C 33 09 01 F1 6D 01 10 10 00 01 01 }
0x4C1BA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C1C0: 				End  { 29 02 }
0x4C1C2: 			End  { 29 02 }
0x4C1C4: 			SuppressIf  { 0A 82 }
0x4C1C6: 				EqIdValList QuestionId: 0x92E, Values: [0, 1] { 14 0A 2E 09 02 00 00 00 01 00 }
0x4C1D0: 				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0 { 02 87 8E 0D 00 00 00 }
0x4C1D7: 				End  { 29 02 }
0x4C1D9: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x934, VarStoreId: 0xF101, VarOffset: 0x156, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 2D 10 1A 0C 34 09 01 F1 56 01 10 10 00 17 01 }
0x4C1EA: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4C1F0: 				End  { 29 02 }
0x4C1F2: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x935, VarStoreId: 0xF101, VarOffset: 0x15C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 3C 10 27 0C 35 09 01 F1 5C 01 10 10 00 0E 00 }
0x4C203: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C20A: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C211: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C218: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C21F: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C226: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C22D: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C234: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C23B: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C242: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4C249: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4C250: 				End  { 29 02 }
0x4C252: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x936, VarStoreId: 0xF101, VarOffset: 0x162, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 1E 10 0D 0C 36 09 01 F1 62 01 10 10 00 12 00 }
0x4C263: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4C26A: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4C271: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4C278: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4C27F: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4C286: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4C28D: 				End  { 29 02 }
0x4C28F: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x937, VarStoreId: 0xF101, VarOffset: 0x168, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 57 10 34 0C 37 09 01 F1 68 01 10 10 00 01 01 }
0x4C2A0: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4C2A6: 				End  { 29 02 }
0x4C2A8: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x938, VarStoreId: 0xF101, VarOffset: 0x16E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 6C 10 41 0C 38 09 01 F1 6E 01 10 10 00 01 01 }
0x4C2B9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C2BF: 				End  { 29 02 }
0x4C2C1: 			End  { 29 02 }
0x4C2C3: 			SuppressIf  { 0A 82 }
0x4C2C5: 				EqIdValList QuestionId: 0x92E, Values: [0, 1, 2] { 14 0C 2E 09 03 00 00 00 01 00 02 00 }
0x4C2D1: 				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0 { 02 87 8F 0D 00 00 00 }
0x4C2D8: 				End  { 29 02 }
0x4C2DA: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x939, VarStoreId: 0xF101, VarOffset: 0x157, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 2E 10 1A 0C 39 09 01 F1 57 01 10 10 00 17 01 }
0x4C2EB: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4C2F1: 				End  { 29 02 }
0x4C2F3: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x93A, VarStoreId: 0xF101, VarOffset: 0x15D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 3D 10 27 0C 3A 09 01 F1 5D 01 10 10 00 0E 00 }
0x4C304: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C30B: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C312: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C319: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C320: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C327: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C32E: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C335: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C33C: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C343: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4C34A: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4C351: 				End  { 29 02 }
0x4C353: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x93B, VarStoreId: 0xF101, VarOffset: 0x163, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 1F 10 0D 0C 3B 09 01 F1 63 01 10 10 00 12 00 }
0x4C364: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4C36B: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4C372: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4C379: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4C380: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4C387: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4C38E: 				End  { 29 02 }
0x4C390: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x93C, VarStoreId: 0xF101, VarOffset: 0x169, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 58 10 34 0C 3C 09 01 F1 69 01 10 10 00 01 01 }
0x4C3A1: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4C3A7: 				End  { 29 02 }
0x4C3A9: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x93D, VarStoreId: 0xF101, VarOffset: 0x16F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 6D 10 41 0C 3D 09 01 F1 6F 01 10 10 00 01 01 }
0x4C3BA: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C3C0: 				End  { 29 02 }
0x4C3C2: 			End  { 29 02 }
0x4C3C4: 			SuppressIf  { 0A 82 }
0x4C3C6: 				EqIdValList QuestionId: 0x92E, Values: [0, 1, 2, 3] { 14 0E 2E 09 04 00 00 00 01 00 02 00 03 00 }
0x4C3D4: 				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0 { 02 87 90 0D 00 00 00 }
0x4C3DB: 				End  { 29 02 }
0x4C3DD: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x93E, VarStoreId: 0xF101, VarOffset: 0x158, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 2F 10 1A 0C 3E 09 01 F1 58 01 10 10 00 17 01 }
0x4C3EE: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4C3F4: 				End  { 29 02 }
0x4C3F6: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x93F, VarStoreId: 0xF101, VarOffset: 0x15E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 3E 10 27 0C 3F 09 01 F1 5E 01 10 10 00 0E 00 }
0x4C407: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C40E: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C415: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C41C: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C423: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C42A: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C431: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C438: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C43F: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C446: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4C44D: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4C454: 				End  { 29 02 }
0x4C456: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x940, VarStoreId: 0xF101, VarOffset: 0x164, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 20 10 0D 0C 40 09 01 F1 64 01 10 10 00 12 00 }
0x4C467: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4C46E: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4C475: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4C47C: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4C483: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4C48A: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4C491: 				End  { 29 02 }
0x4C493: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x941, VarStoreId: 0xF101, VarOffset: 0x16A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 59 10 34 0C 41 09 01 F1 6A 01 10 10 00 01 01 }
0x4C4A4: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4C4AA: 				End  { 29 02 }
0x4C4AC: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x942, VarStoreId: 0xF101, VarOffset: 0x170, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 6E 10 41 0C 42 09 01 F1 70 01 10 10 00 01 01 }
0x4C4BD: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C4C3: 				End  { 29 02 }
0x4C4C5: 			End  { 29 02 }
0x4C4C7: 			SuppressIf  { 0A 82 }
0x4C4C9: 				EqIdValList QuestionId: 0x92E, Values: [0, 1, 2, 3, 4] { 14 10 2E 09 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4C4D9: 				Subtitle Prompt: "GPIO 4", Help: "", Flags: 0x0 { 02 87 91 0D 00 00 00 }
0x4C4E0: 				End  { 29 02 }
0x4C4E2: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x943, VarStoreId: 0xF101, VarOffset: 0x159, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 6F 10 1A 0C 43 09 01 F1 59 01 10 10 00 17 01 }
0x4C4F3: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4C4F9: 				End  { 29 02 }
0x4C4FB: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x944, VarStoreId: 0xF101, VarOffset: 0x15F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 3F 10 27 0C 44 09 01 F1 5F 01 10 10 00 0E 00 }
0x4C50C: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C513: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C51A: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C521: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C528: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C52F: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C536: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C53D: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C544: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C54B: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4C552: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4C559: 				End  { 29 02 }
0x4C55B: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x945, VarStoreId: 0xF101, VarOffset: 0x165, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 40 10 0D 0C 45 09 01 F1 65 01 10 10 00 12 00 }
0x4C56C: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4C573: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4C57A: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4C581: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4C588: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4C58F: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4C596: 				End  { 29 02 }
0x4C598: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x946, VarStoreId: 0xF101, VarOffset: 0x16B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 5A 10 34 0C 46 09 01 F1 6B 01 10 10 00 01 01 }
0x4C5A9: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4C5AF: 				End  { 29 02 }
0x4C5B1: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x947, VarStoreId: 0xF101, VarOffset: 0x171, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 70 10 41 0C 47 09 01 F1 71 01 10 10 00 01 01 }
0x4C5C2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C5C8: 				End  { 29 02 }
0x4C5CA: 			End  { 29 02 }
0x4C5CC: 			SuppressIf  { 0A 82 }
0x4C5CE: 				EqIdValList QuestionId: 0x92E, Values: [0, 1, 2, 3, 4, 5] { 14 12 2E 09 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4C5E0: 				Subtitle Prompt: "GPIO 5", Help: "", Flags: 0x0 { 02 87 92 0D 00 00 00 }
0x4C5E7: 				End  { 29 02 }
0x4C5E9: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x948, VarStoreId: 0xF101, VarOffset: 0x15A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 71 10 1A 0C 48 09 01 F1 5A 01 10 10 00 17 01 }
0x4C5FA: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4C600: 				End  { 29 02 }
0x4C602: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x949, VarStoreId: 0xF101, VarOffset: 0x160, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 41 10 27 0C 49 09 01 F1 60 01 10 10 00 0E 00 }
0x4C613: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C61A: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C621: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C628: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C62F: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C636: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C63D: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C644: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C64B: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C652: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4C659: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4C660: 				End  { 29 02 }
0x4C662: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x94A, VarStoreId: 0xF101, VarOffset: 0x166, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 42 10 0D 0C 4A 09 01 F1 66 01 10 10 00 12 00 }
0x4C673: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4C67A: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4C681: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4C688: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4C68F: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4C696: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4C69D: 				End  { 29 02 }
0x4C69F: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x94B, VarStoreId: 0xF101, VarOffset: 0x16C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 5B 10 34 0C 4B 09 01 F1 6C 01 10 10 00 01 01 }
0x4C6B0: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4C6B6: 				End  { 29 02 }
0x4C6B8: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x94C, VarStoreId: 0xF101, VarOffset: 0x172, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 72 10 41 0C 4C 09 01 F1 72 01 10 10 00 01 01 }
0x4C6C9: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C6CF: 				End  { 29 02 }
0x4C6D1: 			End  { 29 02 }
0x4C6D3: 		End  { 29 02 }
0x4C6D5: 	End  { 29 02 }
0x4C6D7: 	Form FormId: 0x98, Title: "Control Logic options" { 01 86 98 00 21 0D }
0x4C6DD: 		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0 { 02 87 21 0D 00 00 00 }
0x4C6E4: 		End  { 29 02 }
0x4C6E6: 		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0x94D, VarStoreId: 0xF101, VarOffset: 0x173, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0 { 05 91 AE 10 85 0D 4D 09 01 F1 73 01 10 10 01 FE 00 }
0x4C6F7: 			OneOfOption Option: "Discrete" Value: 1 { 09 07 88 0D 00 00 01 }
0x4C6FE: 			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default { 09 07 89 0D 10 00 02 }
0x4C705: 			OneOfOption Option: "PMIC_UP6641" Value: 3 { 09 07 8A 0D 00 00 03 }
0x4C70C: 			OneOfOption Option: "PMIC_USER0" Value: 253 { 09 07 8B 0D 00 00 FD }
0x4C713: 			OneOfOption Option: "PMIC_USER1" Value: 254 { 09 07 8C 0D 00 00 FE }
0x4C71A: 		End  { 29 02 }
0x4C71C: 		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0x94E, VarStoreId: 0xF101, VarOffset: 0x174, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0 { 05 91 97 10 A9 0C 4E 09 01 F1 74 01 10 10 10 50 00 }
0x4C72D: 			OneOfOption Option: "PTC" Value: 16 { 09 07 B2 0C 00 00 10 }
0x4C734: 			OneOfOption Option: "CRD-D" Value: 32 { 09 07 B3 0C 00 00 20 }
0x4C73B: 			OneOfOption Option: "CRD-G" Value: 48, Default { 09 07 B4 0C 10 00 30 }
0x4C742: 			OneOfOption Option: "Kilshon-PPV" Value: 64 { 09 07 B5 0C 00 00 40 }
0x4C749: 			OneOfOption Option: "CRD-G2" Value: 80 { 09 07 B6 0C 00 00 50 }
0x4C750: 		End  { 29 02 }
0x4C752: 		OneOf Prompt: "Input Clock", Help: "Input Clock", QuestionFlags: 0x10, QuestionId: 0x94F, VarStoreId: 0xF101, VarOffset: 0x175, Flags: 0x12, Size: 32, Min: 0x10, Max: 0x40, Step: 0x0 { 05 9A F6 0F 53 0B 4F 09 01 F1 75 01 10 12 10 00 00 00 40 00 00 00 00 00 00 00 }
0x4C76C: 			OneOfOption Option: "20 MHz" Value: 16, Default { 09 0A 54 0B 12 02 10 00 00 00 }
0x4C776: 			OneOfOption Option: "24 MHz" Value: 32 { 09 0A 55 0B 02 02 20 00 00 00 }
0x4C780: 			OneOfOption Option: "26 MHz" Value: 48 { 09 0A 56 0B 02 02 30 00 00 00 }
0x4C78A: 			OneOfOption Option: "19.2 MHz" Value: 64 { 09 0A 57 0B 02 02 40 00 00 00 }
0x4C794: 		End  { 29 02 }
0x4C796: 		OneOf Prompt: "PCH Clock Source", Help: "This option specifies which IMGCLKOUT is chosen", QuestionFlags: 0x10, QuestionId: 0x950, VarStoreId: 0xF101, VarOffset: 0x179, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 B3 10 94 0D 50 09 01 F1 79 01 10 10 00 04 00 }
0x4C7A7: 			OneOfOption Option: "IMGCLKOUT_0" Value: 0, Default { 09 07 95 0D 10 00 00 }
0x4C7AE: 			OneOfOption Option: "IMGCLKOUT_1" Value: 1 { 09 07 96 0D 00 00 01 }
0x4C7B5: 			OneOfOption Option: "IMGCLKOUT_2" Value: 2 { 09 07 97 0D 00 00 02 }
0x4C7BC: 			OneOfOption Option: "IMGCLKOUT_3" Value: 3 { 09 07 98 0D 00 00 03 }
0x4C7C3: 			OneOfOption Option: "IMGCLKOUT_4" Value: 4 { 09 07 99 0D 00 00 04 }
0x4C7CA: 		End  { 29 02 }
0x4C7CC: 		SuppressIf  { 0A 82 }
0x4C7CE: 			EqIdValList QuestionId: 0x94E, Values: [48, 80] { 14 8A 4E 09 02 00 30 00 50 00 }
0x4C7D8: 				Not  { 17 02 }
0x4C7DA: 			End  { 29 02 }
0x4C7DC: 			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0x951, VarStoreId: 0xF101, VarOffset: 0x17E, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0 { 05 91 89 10 6E 0C 51 09 01 F1 7E 01 10 10 21 29 00 }
0x4C7ED: 				OneOfOption Option: "Front" Value: 33 { 09 07 6C 0C 00 00 21 }
0x4C7F4: 				OneOfOption Option: "Back" Value: 41, Default { 09 07 6D 0C 10 00 29 }
0x4C7FB: 			End  { 29 02 }
0x4C7FD: 		End  { 29 02 }
0x4C7FF: 		SuppressIf  { 0A 82 }
0x4C801: 			EqIdVal QuestionId: 0x94D, Value: 0x1 { 12 06 4D 09 01 00 }
0x4C807: 			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x952, VarStoreId: 0xF101, VarOffset: 0x17B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 01 10 8F 0B 52 09 01 F1 7B 01 10 10 00 05 00 }
0x4C818: 				OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4C81F: 				OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4C826: 				OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4C82D: 				OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4C834: 				OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4C83B: 				OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4C842: 			End  { 29 02 }
0x4C844: 			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x953, VarStoreId: 0xF101, VarOffset: 0x17C, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 0A 10 98 0B 53 09 01 F1 7C 01 10 21 00 00 7F 00 01 00 }
0x4C858: 				Default DefaultId: 0x0 Value: 73 { 5B 07 00 00 01 49 00 }
0x4C85F: 			End  { 29 02 }
0x4C861: 			SuppressIf  { 0A 82 }
0x4C863: 				EqIdValList QuestionId: 0x94D, Values: [2, 3] { 14 8A 4D 09 02 00 02 00 03 00 }
0x4C86D: 					Not  { 17 02 }
0x4C86F: 				End  { 29 02 }
0x4C871: 				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x954, VarStoreId: 0xF101, VarOffset: 0x184, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 11 10 FD 0B 54 09 01 F1 84 01 10 10 00 04 00 }
0x4C882: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4C889: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4C890: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4C897: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4C89E: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4C8A5: 				End  { 29 02 }
0x4C8A7: 				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x955, VarStoreId: 0xF101, VarOffset: 0x17F, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 E9 0B E3 0B 55 09 01 F1 7F 01 10 20 00 1F 01 }
0x4C8B8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C8BE: 				End  { 29 02 }
0x4C8C0: 				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x956, VarStoreId: 0xF101, VarOffset: 0x180, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 F6 0B F0 0B 56 09 01 F1 80 01 10 20 00 07 01 }
0x4C8D1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C8D7: 				End  { 29 02 }
0x4C8D9: 				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0x957, VarStoreId: 0xF101, VarOffset: 0x185, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 08 0C FD 0B 57 09 01 F1 85 01 10 10 00 04 00 }
0x4C8EA: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4C8F1: 					OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4C8F8: 					OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4C8FF: 					OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4C906: 					OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4C90D: 				End  { 29 02 }
0x4C90F: 				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x958, VarStoreId: 0xF101, VarOffset: 0x181, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1 { 07 91 EF 0B E3 0B 58 09 01 F1 81 01 10 20 00 1F 01 }
0x4C920: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C926: 				End  { 29 02 }
0x4C928: 				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0x959, VarStoreId: 0xF101, VarOffset: 0x182, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 FC 0B F0 0B 59 09 01 F1 82 01 10 20 00 07 01 }
0x4C939: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C93F: 				End  { 29 02 }
0x4C941: 				Numeric Prompt: "SubPlatformId", Help: "SubPlatformId", QuestionFlags: 0x10, QuestionId: 0x95A, VarStoreId: 0xF101, VarOffset: 0x183, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1 { 07 91 5D 0B 5D 0B 5A 09 01 F1 83 01 10 20 00 0F 01 }
0x4C952: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4C958: 				End  { 29 02 }
0x4C95A: 			End  { 29 02 }
0x4C95C: 		End  { 29 02 }
0x4C95E: 		SuppressIf  { 0A 82 }
0x4C960: 			EqIdValList QuestionId: 0x94D, Values: [253, 254] { 14 0A 4D 09 02 00 FD 00 FE 00 }
0x4C96A: 			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0x95B, VarStoreId: 0xF101, VarOffset: 0x17A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1 { 07 91 FE 0F 73 0B 5B 09 01 F1 7A 01 10 10 00 06 01 }
0x4C97B: 				Default DefaultId: 0x0 Value: 2 { 5B 06 00 00 00 02 }
0x4C981: 			End  { 29 02 }
0x4C983: 			SuppressIf  { 0A 82 }
0x4C985: 				EqIdVal QuestionId: 0x95B, Value: 0x0 { 12 06 5B 09 00 00 }
0x4C98B: 				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0 { 02 87 8D 0D 00 00 00 }
0x4C992: 				End  { 29 02 }
0x4C994: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x95C, VarStoreId: 0xF101, VarOffset: 0x186, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 73 10 1A 0C 5C 09 01 F1 86 01 10 10 00 17 01 }
0x4C9A5: 					Default DefaultId: 0x0 Value: 22 { 5B 06 00 00 00 16 }
0x4C9AB: 				End  { 29 02 }
0x4C9AD: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x95D, VarStoreId: 0xF101, VarOffset: 0x18C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 43 10 27 0C 5D 09 01 F1 8C 01 10 10 00 0E 00 }
0x4C9BE: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4C9C5: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4C9CC: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4C9D3: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4C9DA: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4C9E1: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4C9E8: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4C9EF: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4C9F6: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4C9FD: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4CA04: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4CA0B: 				End  { 29 02 }
0x4CA0D: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x95E, VarStoreId: 0xF101, VarOffset: 0x192, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 44 10 0D 0C 5E 09 01 F1 92 01 10 10 00 12 00 }
0x4CA1E: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4CA25: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4CA2C: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4CA33: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4CA3A: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4CA41: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4CA48: 				End  { 29 02 }
0x4CA4A: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x95F, VarStoreId: 0xF101, VarOffset: 0x198, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 5C 10 34 0C 5F 09 01 F1 98 01 10 10 00 01 01 }
0x4CA5B: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4CA61: 				End  { 29 02 }
0x4CA63: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x960, VarStoreId: 0xF101, VarOffset: 0x19E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 74 10 41 0C 60 09 01 F1 9E 01 10 10 00 01 01 }
0x4CA74: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4CA7A: 				End  { 29 02 }
0x4CA7C: 			End  { 29 02 }
0x4CA7E: 			SuppressIf  { 0A 82 }
0x4CA80: 				EqIdValList QuestionId: 0x95B, Values: [0, 1] { 14 0A 5B 09 02 00 00 00 01 00 }
0x4CA8A: 				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0 { 02 87 8E 0D 00 00 00 }
0x4CA91: 				End  { 29 02 }
0x4CA93: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x961, VarStoreId: 0xF101, VarOffset: 0x187, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 75 10 1A 0C 61 09 01 F1 87 01 10 10 00 17 01 }
0x4CAA4: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4CAAA: 				End  { 29 02 }
0x4CAAC: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x962, VarStoreId: 0xF101, VarOffset: 0x18D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 45 10 27 0C 62 09 01 F1 8D 01 10 10 00 0E 00 }
0x4CABD: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4CAC4: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4CACB: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4CAD2: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4CAD9: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4CAE0: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4CAE7: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4CAEE: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4CAF5: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4CAFC: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4CB03: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4CB0A: 				End  { 29 02 }
0x4CB0C: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x963, VarStoreId: 0xF101, VarOffset: 0x193, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 46 10 0D 0C 63 09 01 F1 93 01 10 10 00 12 00 }
0x4CB1D: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4CB24: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4CB2B: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4CB32: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4CB39: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4CB40: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4CB47: 				End  { 29 02 }
0x4CB49: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x964, VarStoreId: 0xF101, VarOffset: 0x199, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 5D 10 34 0C 64 09 01 F1 99 01 10 10 00 01 01 }
0x4CB5A: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4CB60: 				End  { 29 02 }
0x4CB62: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x965, VarStoreId: 0xF101, VarOffset: 0x19F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 76 10 41 0C 65 09 01 F1 9F 01 10 10 00 01 01 }
0x4CB73: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4CB79: 				End  { 29 02 }
0x4CB7B: 			End  { 29 02 }
0x4CB7D: 			SuppressIf  { 0A 82 }
0x4CB7F: 				EqIdValList QuestionId: 0x95B, Values: [0, 1, 2] { 14 0C 5B 09 03 00 00 00 01 00 02 00 }
0x4CB8B: 				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0 { 02 87 8F 0D 00 00 00 }
0x4CB92: 				End  { 29 02 }
0x4CB94: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x966, VarStoreId: 0xF101, VarOffset: 0x188, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 77 10 1A 0C 66 09 01 F1 88 01 10 10 00 17 01 }
0x4CBA5: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4CBAB: 				End  { 29 02 }
0x4CBAD: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x967, VarStoreId: 0xF101, VarOffset: 0x18E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 47 10 27 0C 67 09 01 F1 8E 01 10 10 00 0E 00 }
0x4CBBE: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4CBC5: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4CBCC: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4CBD3: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4CBDA: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4CBE1: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4CBE8: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4CBEF: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4CBF6: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4CBFD: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4CC04: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4CC0B: 				End  { 29 02 }
0x4CC0D: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x968, VarStoreId: 0xF101, VarOffset: 0x194, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 48 10 0D 0C 68 09 01 F1 94 01 10 10 00 12 00 }
0x4CC1E: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4CC25: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4CC2C: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4CC33: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4CC3A: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4CC41: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4CC48: 				End  { 29 02 }
0x4CC4A: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x969, VarStoreId: 0xF101, VarOffset: 0x19A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 5E 10 34 0C 69 09 01 F1 9A 01 10 10 00 01 01 }
0x4CC5B: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4CC61: 				End  { 29 02 }
0x4CC63: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x96A, VarStoreId: 0xF101, VarOffset: 0x1A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 78 10 41 0C 6A 09 01 F1 A0 01 10 10 00 01 01 }
0x4CC74: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4CC7A: 				End  { 29 02 }
0x4CC7C: 			End  { 29 02 }
0x4CC7E: 			SuppressIf  { 0A 82 }
0x4CC80: 				EqIdValList QuestionId: 0x95B, Values: [0, 1, 2, 3] { 14 0E 5B 09 04 00 00 00 01 00 02 00 03 00 }
0x4CC8E: 				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0 { 02 87 90 0D 00 00 00 }
0x4CC95: 				End  { 29 02 }
0x4CC97: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x96B, VarStoreId: 0xF101, VarOffset: 0x189, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 79 10 1A 0C 6B 09 01 F1 89 01 10 10 00 17 01 }
0x4CCA8: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4CCAE: 				End  { 29 02 }
0x4CCB0: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x96C, VarStoreId: 0xF101, VarOffset: 0x18F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 49 10 27 0C 6C 09 01 F1 8F 01 10 10 00 0E 00 }
0x4CCC1: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4CCC8: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4CCCF: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4CCD6: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4CCDD: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4CCE4: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4CCEB: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4CCF2: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4CCF9: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4CD00: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4CD07: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4CD0E: 				End  { 29 02 }
0x4CD10: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x96D, VarStoreId: 0xF101, VarOffset: 0x195, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 4A 10 0D 0C 6D 09 01 F1 95 01 10 10 00 12 00 }
0x4CD21: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4CD28: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4CD2F: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4CD36: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4CD3D: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4CD44: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4CD4B: 				End  { 29 02 }
0x4CD4D: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x96E, VarStoreId: 0xF101, VarOffset: 0x19B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 5F 10 34 0C 6E 09 01 F1 9B 01 10 10 00 01 01 }
0x4CD5E: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4CD64: 				End  { 29 02 }
0x4CD66: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x96F, VarStoreId: 0xF101, VarOffset: 0x1A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 7A 10 41 0C 6F 09 01 F1 A1 01 10 10 00 01 01 }
0x4CD77: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4CD7D: 				End  { 29 02 }
0x4CD7F: 			End  { 29 02 }
0x4CD81: 			SuppressIf  { 0A 82 }
0x4CD83: 				EqIdValList QuestionId: 0x95B, Values: [0, 1, 2, 3, 4] { 14 10 5B 09 05 00 00 00 01 00 02 00 03 00 04 00 }
0x4CD93: 				Subtitle Prompt: "GPIO 4", Help: "", Flags: 0x0 { 02 87 91 0D 00 00 00 }
0x4CD9A: 				End  { 29 02 }
0x4CD9C: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x970, VarStoreId: 0xF101, VarOffset: 0x18A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 7B 10 1A 0C 70 09 01 F1 8A 01 10 10 00 17 01 }
0x4CDAD: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4CDB3: 				End  { 29 02 }
0x4CDB5: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x971, VarStoreId: 0xF101, VarOffset: 0x190, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 CD 10 27 0C 71 09 01 F1 90 01 10 10 00 0E 00 }
0x4CDC6: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4CDCD: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4CDD4: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4CDDB: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4CDE2: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4CDE9: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4CDF0: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4CDF7: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4CDFE: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4CE05: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4CE0C: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4CE13: 				End  { 29 02 }
0x4CE15: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x972, VarStoreId: 0xF101, VarOffset: 0x196, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 CE 10 0D 0C 72 09 01 F1 96 01 10 10 00 12 00 }
0x4CE26: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4CE2D: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4CE34: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4CE3B: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4CE42: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4CE49: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4CE50: 				End  { 29 02 }
0x4CE52: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x973, VarStoreId: 0xF101, VarOffset: 0x19C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 CF 10 34 0C 73 09 01 F1 9C 01 10 10 00 01 01 }
0x4CE63: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4CE69: 				End  { 29 02 }
0x4CE6B: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x974, VarStoreId: 0xF101, VarOffset: 0x1A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 D0 10 41 0C 74 09 01 F1 A2 01 10 10 00 01 01 }
0x4CE7C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4CE82: 				End  { 29 02 }
0x4CE84: 			End  { 29 02 }
0x4CE86: 			SuppressIf  { 0A 82 }
0x4CE88: 				EqIdValList QuestionId: 0x95B, Values: [0, 1, 2, 3, 4, 5] { 14 12 5B 09 06 00 00 00 01 00 02 00 03 00 04 00 05 00 }
0x4CE9A: 				Subtitle Prompt: "GPIO 5", Help: "", Flags: 0x0 { 02 87 92 0D 00 00 00 }
0x4CEA1: 				End  { 29 02 }
0x4CEA3: 				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x975, VarStoreId: 0xF101, VarOffset: 0x18B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1 { 07 91 D1 10 1A 0C 75 09 01 F1 8B 01 10 10 00 17 01 }
0x4CEB4: 					Default DefaultId: 0x0 Value: 11 { 5B 06 00 00 00 0B }
0x4CEBA: 				End  { 29 02 }
0x4CEBC: 				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x976, VarStoreId: 0xF101, VarOffset: 0x191, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xE, Step: 0x0 { 05 91 D6 10 27 0C 76 09 01 F1 91 01 10 10 00 0E 00 }
0x4CECD: 					OneOfOption Option: "A" Value: 2 { 09 07 54 0C 00 00 02 }
0x4CED4: 					OneOfOption Option: "B" Value: 0 { 09 07 55 0C 00 00 00 }
0x4CEDB: 					OneOfOption Option: "C" Value: 11 { 09 07 56 0C 00 00 0B }
0x4CEE2: 					OneOfOption Option: "D" Value: 8, Default { 09 07 57 0C 10 00 08 }
0x4CEE9: 					OneOfOption Option: "E" Value: 14 { 09 07 58 0C 00 00 0E }
0x4CEF0: 					OneOfOption Option: "F" Value: 12 { 09 07 59 0C 00 00 0C }
0x4CEF7: 					OneOfOption Option: "H" Value: 7 { 09 07 5A 0C 00 00 07 }
0x4CEFE: 					OneOfOption Option: "R" Value: 3 { 09 07 5B 0C 00 00 03 }
0x4CF05: 					OneOfOption Option: "S" Value: 6 { 09 07 5C 0C 00 00 06 }
0x4CF0C: 					OneOfOption Option: "T" Value: 1 { 09 07 5D 0C 00 00 01 }
0x4CF13: 					OneOfOption Option: "U" Value: 9 { 09 07 5E 0C 00 00 09 }
0x4CF1A: 				End  { 29 02 }
0x4CF1C: 				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0x977, VarStoreId: 0xF101, VarOffset: 0x197, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x12, Step: 0x0 { 05 91 D7 10 0D 0C 77 09 01 F1 97 01 10 10 00 12 00 }
0x4CF2D: 					OneOfOption Option: "Reset" Value: 0, Default { 09 07 4E 0C 10 00 00 }
0x4CF34: 					OneOfOption Option: "Power_En" Value: 11 { 09 07 4F 0C 00 00 0B }
0x4CF3B: 					OneOfOption Option: "Clock_En" Value: 12 { 09 07 50 0C 00 00 0C }
0x4CF42: 					OneOfOption Option: "pLED_En" Value: 13 { 09 07 51 0C 00 00 0D }
0x4CF49: 					OneOfOption Option: "Strobe_En" Value: 2 { 09 07 52 0C 00 00 02 }
0x4CF50: 					OneOfOption Option: "Handshake_En" Value: 18 { 09 07 53 0C 00 00 12 }
0x4CF57: 				End  { 29 02 }
0x4CF59: 				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x978, VarStoreId: 0xF101, VarOffset: 0x19D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 D8 10 34 0C 78 09 01 F1 9D 01 10 10 00 01 01 }
0x4CF6A: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4CF70: 				End  { 29 02 }
0x4CF72: 				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x979, VarStoreId: 0xF101, VarOffset: 0x1A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 D9 10 41 0C 79 09 01 F1 A3 01 10 10 00 01 01 }
0x4CF83: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4CF89: 				End  { 29 02 }
0x4CF8B: 			End  { 29 02 }
0x4CF8D: 		End  { 29 02 }
0x4CF8F: 	End  { 29 02 }
0x4CF91: 	Form FormId: 0x27BF, Title: "Flash Options" { 01 86 BF 27 A0 0D }
0x4CF97: 		Subtitle Prompt: "Flash1", Help: "", Flags: 0x0 { 02 87 9A 0D 00 00 00 }
0x4CF9E: 		End  { 29 02 }
0x4CFA0: 		OneOf Prompt: "Flash Model", Help: "Flash Model", QuestionFlags: 0x10, QuestionId: 0x97A, VarStoreId: 0xF101, VarOffset: 0x4D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 0D A1 0D 7A 09 01 F1 D4 04 10 10 00 01 00 }
0x4CFB1: 			OneOfOption Option: "External - LM3643" Value: 0, Default { 09 07 A4 0D 10 00 00 }
0x4CFB8: 			OneOfOption Option: "PMIC - WRC" Value: 1 { 09 07 A5 0D 00 00 01 }
0x4CFBF: 		End  { 29 02 }
0x4CFC1: 		OneOf Prompt: "Flash Mode", Help: "Select Flash Mode White LED/Warm LED/IR LED/Xeon LED", QuestionFlags: 0x10, QuestionId: 0x97B, VarStoreId: 0xF101, VarOffset: 0x9CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 A2 0D A3 0D 7B 09 01 F1 CC 09 10 10 00 04 00 }
0x4CFD2: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4CFD9: 			OneOfOption Option: "White Led" Value: 1, Default, MfgDefault { 09 07 09 0C 30 00 01 }
0x4CFE0: 			OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4CFE7: 			OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4CFEE: 			OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4CFF5: 		End  { 29 02 }
0x4CFF7: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x97C, VarStoreId: 0xF101, VarStoreInfo: 0x4D5, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 81 10 66 0C 7C 09 01 F1 D5 04 00 01 0F 00 }
0x4D007: 			Default DefaultId: 0x0 String: "YHCE" { 5B 07 00 00 07 6B 0C }
0x4D00E: 		End  { 29 02 }
0x4D010: 		OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x97D, VarStoreId: 0xF101, VarOffset: 0x4F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 02 10 8F 0B 7D 09 01 F1 F5 04 10 10 00 05 00 }
0x4D021: 			OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4D028: 			OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4D02F: 			OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4D036: 			OneOfOption Option: "I2C3" Value: 3 { 09 07 1C 0D 00 00 03 }
0x4D03D: 			OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4D044: 			OneOfOption Option: "I2C5" Value: 5, Default { 09 07 1E 0D 10 00 05 }
0x4D04B: 		End  { 29 02 }
0x4D04D: 		Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x97E, VarStoreId: 0xF101, VarOffset: 0x4F6, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 0B 10 98 0B 7E 09 01 F1 F6 04 10 21 00 00 7F 00 01 00 }
0x4D061: 			Default DefaultId: 0x0 Value: 103 { 5B 07 00 00 01 67 00 }
0x4D068: 		End  { 29 02 }
0x4D06A: 		SuppressIf  { 0A 82 }
0x4D06C: 			EqIdValList QuestionId: 0x86C, Values: [253, 254] { 14 0A 6C 08 02 00 FD 00 FE 00 }
0x4D076: 			Subtitle Prompt: "Flash Trigger Gpio", Help: "", Flags: 0x0 { 02 87 A6 0D 00 00 00 }
0x4D07D: 			End  { 29 02 }
0x4D07F: 			Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x97F, VarStoreId: 0xF101, VarOffset: 0x4F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x58, Step: 0x1 { 07 91 A8 0D 1A 0C 7F 09 01 F1 F8 04 10 10 00 58 01 }
0x4D090: 				Default DefaultId: 0x0 Value: 18 { 5B 06 00 00 00 12 }
0x4D096: 			End  { 29 02 }
0x4D098: 			OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x980, VarStoreId: 0xF101, VarOffset: 0x4F9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xE, Step: 0x0 { 05 94 DE 10 27 0C 80 09 01 F1 F9 04 10 11 00 00 0E 00 00 00 }
0x4D0AC: 				OneOfOption Option: "A" Value: 2 { 09 08 54 0C 01 01 02 00 }
0x4D0B4: 				OneOfOption Option: "C" Value: 11 { 09 08 56 0C 01 01 0B 00 }
0x4D0BC: 				OneOfOption Option: "E" Value: 14 { 09 08 58 0C 01 01 0E 00 }
0x4D0C4: 				OneOfOption Option: "F" Value: 12 { 09 08 59 0C 01 01 0C 00 }
0x4D0CC: 				OneOfOption Option: "H" Value: 7 { 09 08 5A 0C 01 01 07 00 }
0x4D0D4: 				OneOfOption Option: "R" Value: 3 { 09 08 5B 0C 01 01 03 00 }
0x4D0DC: 				OneOfOption Option: "S" Value: 6 { 09 08 5C 0C 01 01 06 00 }
0x4D0E4: 				OneOfOption Option: "T" Value: 1 { 09 08 5D 0C 01 01 01 00 }
0x4D0EC: 				OneOfOption Option: "U" Value: 9 { 09 08 5E 0C 01 01 09 00 }
0x4D0F4: 				OneOfOption Option: "B" Value: 0, Default { 09 08 55 0C 11 01 00 00 }
0x4D0FC: 				OneOfOption Option: "D" Value: 8 { 09 08 57 0C 01 01 08 00 }
0x4D104: 			End  { 29 02 }
0x4D106: 			Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x981, VarStoreId: 0xF101, VarOffset: 0x4FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 DF 10 34 0C 81 09 01 F1 FB 04 10 10 00 01 01 }
0x4D117: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4D11D: 			End  { 29 02 }
0x4D11F: 			Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x982, VarStoreId: 0xF101, VarOffset: 0x4FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 E0 10 41 0C 82 09 01 F1 FC 04 10 10 00 01 01 }
0x4D130: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4D136: 			End  { 29 02 }
0x4D138: 		End  { 29 02 }
0x4D13A: 		SuppressIf  { 0A 82 }
0x4D13C: 			EqIdValList QuestionId: 0x784, Values: [0, 1] { 14 0A 84 07 02 00 00 00 01 00 }
0x4D146: 			OneOf Prompt: "Flash Driver Operating Mode", Help: "Select the Flash Driver Operating Mode as Disabled , Torch or Flash", QuestionFlags: 0x10, QuestionId: 0x983, VarStoreId: 0xF101, VarOffset: 0x4FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A7 0D A9 0D 83 09 01 F1 FD 04 10 10 00 02 00 }
0x4D157: 				OneOfOption Option: "Don't flash or light up" Value: 0, Default { 09 07 AA 0D 10 00 00 }
0x4D15E: 				OneOfOption Option: "Light with ITORCH current continuously" Value: 1 { 09 07 AB 0D 00 00 01 }
0x4D165: 				OneOfOption Option: "Flash with IFLASH current when TRIGGERed" Value: 2 { 09 07 AC 0D 00 00 02 }
0x4D16C: 			End  { 29 02 }
0x4D16E: 		End  { 29 02 }
0x4D170: 	End  { 29 02 }
0x4D172: 	Form FormId: 0x27C0, Title: "Flash Options" { 01 86 C0 27 A0 0D }
0x4D178: 		Subtitle Prompt: "Flash2", Help: "", Flags: 0x0 { 02 87 9B 0D 00 00 00 }
0x4D17F: 		End  { 29 02 }
0x4D181: 		OneOf Prompt: "Flash Model", Help: "Flash Model", QuestionFlags: 0x10, QuestionId: 0x984, VarStoreId: 0xF101, VarOffset: 0x4FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 10 A1 0D 84 09 01 F1 FE 04 10 10 00 01 00 }
0x4D192: 			OneOfOption Option: "External - LM3643" Value: 0 { 09 07 A4 0D 00 00 00 }
0x4D199: 			OneOfOption Option: "PMIC - WRC" Value: 1, Default { 09 07 A5 0D 10 00 01 }
0x4D1A0: 		End  { 29 02 }
0x4D1A2: 		OneOf Prompt: "Flash Mode", Help: "Select Flash Mode White LED/Warm LED/IR LED/Xeon LED", QuestionFlags: 0x10, QuestionId: 0x985, VarStoreId: 0xF101, VarOffset: 0x9CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 BE 10 A3 0D 85 09 01 F1 CD 09 10 10 00 04 00 }
0x4D1B3: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4D1BA: 			OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4D1C1: 			OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4D1C8: 			OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4D1CF: 			OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4D1D6: 		End  { 29 02 }
0x4D1D8: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x986, VarStoreId: 0xF101, VarStoreInfo: 0x4FF, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 82 10 66 0C 86 09 01 F1 FF 04 00 01 0F 00 }
0x4D1E8: 			Default DefaultId: 0x0 String: "YHRN" { 5B 07 00 00 07 6A 0C }
0x4D1EF: 		End  { 29 02 }
0x4D1F1: 		OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x987, VarStoreId: 0xF101, VarOffset: 0x51F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 03 10 8F 0B 87 09 01 F1 1F 05 10 10 00 05 00 }
0x4D202: 			OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4D209: 			OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4D210: 			OneOfOption Option: "I2C2" Value: 2, Default { 09 07 1B 0D 10 00 02 }
0x4D217: 			OneOfOption Option: "I2C3" Value: 3 { 09 07 1C 0D 00 00 03 }
0x4D21E: 			OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4D225: 			OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4D22C: 		End  { 29 02 }
0x4D22E: 		Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x988, VarStoreId: 0xF101, VarOffset: 0x520, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 0C 10 98 0B 88 09 01 F1 20 05 10 21 00 00 7F 00 01 00 }
0x4D242: 			Default DefaultId: 0x0 Value: 103 { 5B 07 00 00 01 67 00 }
0x4D249: 		End  { 29 02 }
0x4D24B: 		SuppressIf  { 0A 82 }
0x4D24D: 			EqIdValList QuestionId: 0x899, Values: [253, 254] { 14 0A 99 08 02 00 FD 00 FE 00 }
0x4D257: 			Subtitle Prompt: "Flash Trigger Gpio", Help: "", Flags: 0x0 { 02 87 A6 0D 00 00 00 }
0x4D25E: 			End  { 29 02 }
0x4D260: 			Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x989, VarStoreId: 0xF101, VarOffset: 0x522, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x58, Step: 0x1 { 07 91 C8 10 1A 0C 89 09 01 F1 22 05 10 10 00 58 01 }
0x4D271: 				Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x4D277: 			End  { 29 02 }
0x4D279: 			OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x98A, VarStoreId: 0xF101, VarOffset: 0x523, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xE, Step: 0x0 { 05 94 E5 10 27 0C 8A 09 01 F1 23 05 10 11 00 00 0E 00 00 00 }
0x4D28D: 				OneOfOption Option: "A" Value: 2 { 09 08 54 0C 01 01 02 00 }
0x4D295: 				OneOfOption Option: "C" Value: 11 { 09 08 56 0C 01 01 0B 00 }
0x4D29D: 				OneOfOption Option: "B" Value: 0 { 09 08 55 0C 01 01 00 00 }
0x4D2A5: 				OneOfOption Option: "D" Value: 8, Default { 09 08 57 0C 11 01 08 00 }
0x4D2AD: 				OneOfOption Option: "E" Value: 14 { 09 08 58 0C 01 01 0E 00 }
0x4D2B5: 				OneOfOption Option: "F" Value: 12 { 09 08 59 0C 01 01 0C 00 }
0x4D2BD: 				OneOfOption Option: "H" Value: 7 { 09 08 5A 0C 01 01 07 00 }
0x4D2C5: 				OneOfOption Option: "R" Value: 3 { 09 08 5B 0C 01 01 03 00 }
0x4D2CD: 				OneOfOption Option: "S" Value: 6 { 09 08 5C 0C 01 01 06 00 }
0x4D2D5: 				OneOfOption Option: "T" Value: 1 { 09 08 5D 0C 01 01 01 00 }
0x4D2DD: 				OneOfOption Option: "U" Value: 9 { 09 08 5E 0C 01 01 09 00 }
0x4D2E5: 			End  { 29 02 }
0x4D2E7: 			Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x98B, VarStoreId: 0xF101, VarOffset: 0x525, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 E6 10 34 0C 8B 09 01 F1 25 05 10 10 00 01 01 }
0x4D2F8: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4D2FE: 			End  { 29 02 }
0x4D300: 			Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x98C, VarStoreId: 0xF101, VarOffset: 0x526, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 E7 10 41 0C 8C 09 01 F1 26 05 10 10 00 01 01 }
0x4D311: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4D317: 			End  { 29 02 }
0x4D319: 		End  { 29 02 }
0x4D31B: 		SuppressIf  { 0A 82 }
0x4D31D: 			EqIdValList QuestionId: 0x7B2, Values: [0, 1] { 14 0A B2 07 02 00 00 00 01 00 }
0x4D327: 			OneOf Prompt: "Flash Driver Operating Mode", Help: "Select the Flash Driver Operating Mode as Disabled , Torch or Flash", QuestionFlags: 0x10, QuestionId: 0x98D, VarStoreId: 0xF101, VarOffset: 0x527, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C3 10 A9 0D 8D 09 01 F1 27 05 10 10 00 02 00 }
0x4D338: 				OneOfOption Option: "Don't flash or light up" Value: 0, Default { 09 07 AA 0D 10 00 00 }
0x4D33F: 				OneOfOption Option: "Light with ITORCH current continuously" Value: 1 { 09 07 AB 0D 00 00 01 }
0x4D346: 				OneOfOption Option: "Flash with IFLASH current when TRIGGERed" Value: 2 { 09 07 AC 0D 00 00 02 }
0x4D34D: 			End  { 29 02 }
0x4D34F: 		End  { 29 02 }
0x4D351: 	End  { 29 02 }
0x4D353: 	Form FormId: 0x27C1, Title: "Flash Options" { 01 86 C1 27 A0 0D }
0x4D359: 		Subtitle Prompt: "Flash3", Help: "", Flags: 0x0 { 02 87 9C 0D 00 00 00 }
0x4D360: 		End  { 29 02 }
0x4D362: 		OneOf Prompt: "Flash Model", Help: "Flash Model", QuestionFlags: 0x10, QuestionId: 0x98E, VarStoreId: 0xF101, VarOffset: 0x528, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 10 A1 0D 8E 09 01 F1 28 05 10 10 00 01 00 }
0x4D373: 			OneOfOption Option: "External - LM3643" Value: 0, Default { 09 07 A4 0D 10 00 00 }
0x4D37A: 			OneOfOption Option: "PMIC - WRC" Value: 1 { 09 07 A5 0D 00 00 01 }
0x4D381: 		End  { 29 02 }
0x4D383: 		OneOf Prompt: "Flash Mode", Help: "Select Flash Mode White LED/Warm LED/IR LED/Xeon LED", QuestionFlags: 0x10, QuestionId: 0x98F, VarStoreId: 0xF101, VarOffset: 0x9CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 BF 10 A3 0D 8F 09 01 F1 CE 09 10 10 00 04 00 }
0x4D394: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4D39B: 			OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4D3A2: 			OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4D3A9: 			OneOfOption Option: "IR Led" Value: 3, Default, MfgDefault { 09 07 0B 0C 30 00 03 }
0x4D3B0: 			OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4D3B7: 		End  { 29 02 }
0x4D3B9: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x990, VarStoreId: 0xF101, VarStoreInfo: 0x529, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 83 10 66 0C 90 09 01 F1 29 05 00 01 0F 00 }
0x4D3C9: 		End  { 29 02 }
0x4D3CB: 		OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x991, VarStoreId: 0xF101, VarOffset: 0x549, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 04 10 8F 0B 91 09 01 F1 49 05 10 10 00 05 00 }
0x4D3DC: 			OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4D3E3: 			OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4D3EA: 			OneOfOption Option: "I2C2" Value: 2, Default { 09 07 1B 0D 10 00 02 }
0x4D3F1: 			OneOfOption Option: "I2C3" Value: 3 { 09 07 1C 0D 00 00 03 }
0x4D3F8: 			OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4D3FF: 			OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4D406: 		End  { 29 02 }
0x4D408: 		Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x992, VarStoreId: 0xF101, VarOffset: 0x54A, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 0D 10 98 0B 92 09 01 F1 4A 05 10 21 00 00 7F 00 01 00 }
0x4D41C: 			Default DefaultId: 0x0 Value: 99 { 5B 07 00 00 01 63 00 }
0x4D423: 		End  { 29 02 }
0x4D425: 		SuppressIf  { 0A 82 }
0x4D427: 			EqIdValList QuestionId: 0x8C6, Values: [253, 254] { 14 0A C6 08 02 00 FD 00 FE 00 }
0x4D431: 			Subtitle Prompt: "Flash Trigger Gpio", Help: "", Flags: 0x0 { 02 87 A6 0D 00 00 00 }
0x4D438: 			End  { 29 02 }
0x4D43A: 			Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x993, VarStoreId: 0xF101, VarOffset: 0x54C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x58, Step: 0x1 { 07 91 C9 10 1A 0C 93 09 01 F1 4C 05 10 10 00 58 01 }
0x4D44B: 				Default DefaultId: 0x0 Value: 18 { 5B 06 00 00 00 12 }
0x4D451: 			End  { 29 02 }
0x4D453: 			OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x994, VarStoreId: 0xF101, VarOffset: 0x54D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xE, Step: 0x0 { 05 94 CA 10 27 0C 94 09 01 F1 4D 05 10 11 00 00 0E 00 00 00 }
0x4D467: 				OneOfOption Option: "A" Value: 2 { 09 08 54 0C 01 01 02 00 }
0x4D46F: 				OneOfOption Option: "B" Value: 0, Default { 09 08 55 0C 11 01 00 00 }
0x4D477: 				OneOfOption Option: "C" Value: 11 { 09 08 56 0C 01 01 0B 00 }
0x4D47F: 				OneOfOption Option: "D" Value: 8 { 09 08 57 0C 01 01 08 00 }
0x4D487: 				OneOfOption Option: "E" Value: 14 { 09 08 58 0C 01 01 0E 00 }
0x4D48F: 				OneOfOption Option: "F" Value: 12 { 09 08 59 0C 01 01 0C 00 }
0x4D497: 				OneOfOption Option: "H" Value: 7 { 09 08 5A 0C 01 01 07 00 }
0x4D49F: 				OneOfOption Option: "R" Value: 3 { 09 08 5B 0C 01 01 03 00 }
0x4D4A7: 				OneOfOption Option: "S" Value: 6 { 09 08 5C 0C 01 01 06 00 }
0x4D4AF: 				OneOfOption Option: "T" Value: 1 { 09 08 5D 0C 01 01 01 00 }
0x4D4B7: 				OneOfOption Option: "U" Value: 9 { 09 08 5E 0C 01 01 09 00 }
0x4D4BF: 			End  { 29 02 }
0x4D4C1: 			Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x995, VarStoreId: 0xF101, VarOffset: 0x54F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 CB 10 34 0C 95 09 01 F1 4F 05 10 10 00 01 01 }
0x4D4D2: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4D4D8: 			End  { 29 02 }
0x4D4DA: 			Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x996, VarStoreId: 0xF101, VarOffset: 0x550, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 CC 10 41 0C 96 09 01 F1 50 05 10 10 00 01 01 }
0x4D4EB: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4D4F1: 			End  { 29 02 }
0x4D4F3: 		End  { 29 02 }
0x4D4F5: 		SuppressIf  { 0A 82 }
0x4D4F7: 			EqIdValList QuestionId: 0x7E0, Values: [0, 1] { 14 0A E0 07 02 00 00 00 01 00 }
0x4D501: 			OneOf Prompt: "Flash Driver Operating Mode", Help: "Select the Flash Driver Operating Mode as Disabled , Torch or Flash", QuestionFlags: 0x10, QuestionId: 0x997, VarStoreId: 0xF101, VarOffset: 0x551, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C4 10 A9 0D 97 09 01 F1 51 05 10 10 00 02 00 }
0x4D512: 				OneOfOption Option: "Don't flash or light up" Value: 0, Default { 09 07 AA 0D 10 00 00 }
0x4D519: 				OneOfOption Option: "Light with ITORCH current continuously" Value: 1 { 09 07 AB 0D 00 00 01 }
0x4D520: 				OneOfOption Option: "Flash with IFLASH current when TRIGGERed" Value: 2 { 09 07 AC 0D 00 00 02 }
0x4D527: 			End  { 29 02 }
0x4D529: 		End  { 29 02 }
0x4D52B: 	End  { 29 02 }
0x4D52D: 	Form FormId: 0x27C2, Title: "Flash Options" { 01 86 C2 27 A0 0D }
0x4D533: 		Subtitle Prompt: "Flash4", Help: "", Flags: 0x0 { 02 87 9D 0D 00 00 00 }
0x4D53A: 		End  { 29 02 }
0x4D53C: 		OneOf Prompt: "Flash Model", Help: "Flash Model", QuestionFlags: 0x10, QuestionId: 0x998, VarStoreId: 0xF101, VarOffset: 0x552, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 10 A1 0D 98 09 01 F1 52 05 10 10 00 01 00 }
0x4D54D: 			OneOfOption Option: "External - LM3643" Value: 0 { 09 07 A4 0D 00 00 00 }
0x4D554: 			OneOfOption Option: "PMIC - WRC" Value: 1, Default { 09 07 A5 0D 10 00 01 }
0x4D55B: 		End  { 29 02 }
0x4D55D: 		OneOf Prompt: "Flash Mode", Help: "Select Flash Mode White LED/Warm LED/IR LED/Xeon LED", QuestionFlags: 0x10, QuestionId: 0x999, VarStoreId: 0xF101, VarOffset: 0x9CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 C0 10 A3 0D 99 09 01 F1 CF 09 10 10 00 04 00 }
0x4D56E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4D575: 			OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4D57C: 			OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4D583: 			OneOfOption Option: "IR Led" Value: 3, Default, MfgDefault { 09 07 0B 0C 30 00 03 }
0x4D58A: 			OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4D591: 		End  { 29 02 }
0x4D593: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x99A, VarStoreId: 0xF101, VarStoreInfo: 0x553, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 84 10 66 0C 9A 09 01 F1 53 05 00 01 0F 00 }
0x4D5A3: 		End  { 29 02 }
0x4D5A5: 		OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x99B, VarStoreId: 0xF101, VarOffset: 0x573, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 05 10 8F 0B 9B 09 01 F1 73 05 10 10 00 05 00 }
0x4D5B6: 			OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4D5BD: 			OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4D5C4: 			OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4D5CB: 			OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4D5D2: 			OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4D5D9: 			OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4D5E0: 		End  { 29 02 }
0x4D5E2: 		Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x99C, VarStoreId: 0xF101, VarOffset: 0x574, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 0E 10 98 0B 9C 09 01 F1 74 05 10 21 00 00 7F 00 01 00 }
0x4D5F6: 			Default DefaultId: 0x0 Value: 103 { 5B 07 00 00 01 67 00 }
0x4D5FD: 		End  { 29 02 }
0x4D5FF: 		SuppressIf  { 0A 82 }
0x4D601: 			EqIdValList QuestionId: 0x8F3, Values: [253, 254] { 14 0A F3 08 02 00 FD 00 FE 00 }
0x4D60B: 			Subtitle Prompt: "Flash Trigger Gpio", Help: "", Flags: 0x0 { 02 87 A6 0D 00 00 00 }
0x4D612: 			End  { 29 02 }
0x4D614: 			Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x99D, VarStoreId: 0xF101, VarOffset: 0x576, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x58, Step: 0x1 { 07 91 D2 10 1A 0C 9D 09 01 F1 76 05 10 10 00 58 01 }
0x4D625: 				Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x4D62B: 			End  { 29 02 }
0x4D62D: 			OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x99E, VarStoreId: 0xF101, VarOffset: 0x577, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xE, Step: 0x0 { 05 94 D3 10 27 0C 9E 09 01 F1 77 05 10 11 00 00 0E 00 00 00 }
0x4D641: 				OneOfOption Option: "A" Value: 2 { 09 08 54 0C 01 01 02 00 }
0x4D649: 				OneOfOption Option: "B" Value: 0 { 09 08 55 0C 01 01 00 00 }
0x4D651: 				OneOfOption Option: "C" Value: 11 { 09 08 56 0C 01 01 0B 00 }
0x4D659: 				OneOfOption Option: "D" Value: 8, Default { 09 08 57 0C 11 01 08 00 }
0x4D661: 				OneOfOption Option: "E" Value: 14 { 09 08 58 0C 01 01 0E 00 }
0x4D669: 				OneOfOption Option: "F" Value: 12 { 09 08 59 0C 01 01 0C 00 }
0x4D671: 				OneOfOption Option: "H" Value: 7 { 09 08 5A 0C 01 01 07 00 }
0x4D679: 				OneOfOption Option: "R" Value: 3 { 09 08 5B 0C 01 01 03 00 }
0x4D681: 				OneOfOption Option: "S" Value: 6 { 09 08 5C 0C 01 01 06 00 }
0x4D689: 				OneOfOption Option: "T" Value: 1 { 09 08 5D 0C 01 01 01 00 }
0x4D691: 				OneOfOption Option: "U" Value: 9 { 09 08 5E 0C 01 01 09 00 }
0x4D699: 			End  { 29 02 }
0x4D69B: 			Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x99F, VarStoreId: 0xF101, VarOffset: 0x579, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 D4 10 34 0C 9F 09 01 F1 79 05 10 10 00 01 01 }
0x4D6AC: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4D6B2: 			End  { 29 02 }
0x4D6B4: 			Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x9A0, VarStoreId: 0xF101, VarOffset: 0x57A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 D5 10 41 0C A0 09 01 F1 7A 05 10 10 00 01 01 }
0x4D6C5: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4D6CB: 			End  { 29 02 }
0x4D6CD: 		End  { 29 02 }
0x4D6CF: 		SuppressIf  { 0A 82 }
0x4D6D1: 			EqIdValList QuestionId: 0x80E, Values: [0, 1] { 14 0A 0E 08 02 00 00 00 01 00 }
0x4D6DB: 			OneOf Prompt: "Flash Driver Operating Mode", Help: "Select the Flash Driver Operating Mode as Disabled , Torch or Flash", QuestionFlags: 0x10, QuestionId: 0x9A1, VarStoreId: 0xF101, VarOffset: 0x57B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C5 10 A9 0D A1 09 01 F1 7B 05 10 10 00 02 00 }
0x4D6EC: 				OneOfOption Option: "Don't flash or light up" Value: 0, Default { 09 07 AA 0D 10 00 00 }
0x4D6F3: 				OneOfOption Option: "Light with ITORCH current continuously" Value: 1 { 09 07 AB 0D 00 00 01 }
0x4D6FA: 				OneOfOption Option: "Flash with IFLASH current when TRIGGERed" Value: 2 { 09 07 AC 0D 00 00 02 }
0x4D701: 			End  { 29 02 }
0x4D703: 		End  { 29 02 }
0x4D705: 	End  { 29 02 }
0x4D707: 	Form FormId: 0x27C3, Title: "Flash Options" { 01 86 C3 27 A0 0D }
0x4D70D: 		Subtitle Prompt: "Flash5", Help: "", Flags: 0x0 { 02 87 9E 0D 00 00 00 }
0x4D714: 		End  { 29 02 }
0x4D716: 		OneOf Prompt: "Flash Model", Help: "Flash Model", QuestionFlags: 0x10, QuestionId: 0x9A2, VarStoreId: 0xF101, VarOffset: 0x57C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 10 A1 0D A2 09 01 F1 7C 05 10 10 00 01 00 }
0x4D727: 			OneOfOption Option: "External - LM3643" Value: 0 { 09 07 A4 0D 00 00 00 }
0x4D72E: 			OneOfOption Option: "PMIC - WRC" Value: 1, Default { 09 07 A5 0D 10 00 01 }
0x4D735: 		End  { 29 02 }
0x4D737: 		OneOf Prompt: "Flash Mode", Help: "Select Flash Mode White LED/Warm LED/IR LED/Xeon LED", QuestionFlags: 0x10, QuestionId: 0x9A3, VarStoreId: 0xF101, VarOffset: 0x9D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 C1 10 A3 0D A3 09 01 F1 D0 09 10 10 00 04 00 }
0x4D748: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4D74F: 			OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4D756: 			OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4D75D: 			OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4D764: 			OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4D76B: 		End  { 29 02 }
0x4D76D: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x9A4, VarStoreId: 0xF101, VarStoreInfo: 0x57D, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 85 10 66 0C A4 09 01 F1 7D 05 00 01 0F 00 }
0x4D77D: 		End  { 29 02 }
0x4D77F: 		OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x9A5, VarStoreId: 0xF101, VarOffset: 0x59D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 06 10 8F 0B A5 09 01 F1 9D 05 10 10 00 05 00 }
0x4D790: 			OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4D797: 			OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4D79E: 			OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4D7A5: 			OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4D7AC: 			OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4D7B3: 			OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4D7BA: 		End  { 29 02 }
0x4D7BC: 		Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x9A6, VarStoreId: 0xF101, VarOffset: 0x59E, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 0F 10 98 0B A6 09 01 F1 9E 05 10 21 00 00 7F 00 01 00 }
0x4D7D0: 			Default DefaultId: 0x0 Value: 103 { 5B 07 00 00 01 67 00 }
0x4D7D7: 		End  { 29 02 }
0x4D7D9: 		SuppressIf  { 0A 82 }
0x4D7DB: 			EqIdValList QuestionId: 0x920, Values: [253, 254] { 14 0A 20 09 02 00 FD 00 FE 00 }
0x4D7E5: 			Subtitle Prompt: "Flash Trigger Gpio", Help: "", Flags: 0x0 { 02 87 A6 0D 00 00 00 }
0x4D7EC: 			End  { 29 02 }
0x4D7EE: 			Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x9A7, VarStoreId: 0xF101, VarOffset: 0x5A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x58, Step: 0x1 { 07 91 DA 10 1A 0C A7 09 01 F1 A0 05 10 10 00 58 01 }
0x4D7FF: 				Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x4D805: 			End  { 29 02 }
0x4D807: 			OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x9A8, VarStoreId: 0xF101, VarOffset: 0x5A1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xE, Step: 0x0 { 05 94 DB 10 27 0C A8 09 01 F1 A1 05 10 11 00 00 0E 00 00 00 }
0x4D81B: 				OneOfOption Option: "A" Value: 2 { 09 08 54 0C 01 01 02 00 }
0x4D823: 				OneOfOption Option: "B" Value: 0 { 09 08 55 0C 01 01 00 00 }
0x4D82B: 				OneOfOption Option: "C" Value: 11 { 09 08 56 0C 01 01 0B 00 }
0x4D833: 				OneOfOption Option: "D" Value: 8, Default { 09 08 57 0C 11 01 08 00 }
0x4D83B: 				OneOfOption Option: "E" Value: 14 { 09 08 58 0C 01 01 0E 00 }
0x4D843: 				OneOfOption Option: "F" Value: 12 { 09 08 59 0C 01 01 0C 00 }
0x4D84B: 				OneOfOption Option: "H" Value: 7 { 09 08 5A 0C 01 01 07 00 }
0x4D853: 				OneOfOption Option: "R" Value: 3 { 09 08 5B 0C 01 01 03 00 }
0x4D85B: 				OneOfOption Option: "S" Value: 6 { 09 08 5C 0C 01 01 06 00 }
0x4D863: 				OneOfOption Option: "T" Value: 1 { 09 08 5D 0C 01 01 01 00 }
0x4D86B: 				OneOfOption Option: "U" Value: 9 { 09 08 5E 0C 01 01 09 00 }
0x4D873: 			End  { 29 02 }
0x4D875: 			Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x9A9, VarStoreId: 0xF101, VarOffset: 0x5A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 DC 10 34 0C A9 09 01 F1 A3 05 10 10 00 01 01 }
0x4D886: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4D88C: 			End  { 29 02 }
0x4D88E: 			Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x9AA, VarStoreId: 0xF101, VarOffset: 0x5A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 DD 10 41 0C AA 09 01 F1 A4 05 10 10 00 01 01 }
0x4D89F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4D8A5: 			End  { 29 02 }
0x4D8A7: 		End  { 29 02 }
0x4D8A9: 		SuppressIf  { 0A 82 }
0x4D8AB: 			EqIdValList QuestionId: 0x83C, Values: [0, 1] { 14 0A 3C 08 02 00 00 00 01 00 }
0x4D8B5: 			OneOf Prompt: "Flash Driver Operating Mode", Help: "Select the Flash Driver Operating Mode as Disabled , Torch or Flash", QuestionFlags: 0x10, QuestionId: 0x9AB, VarStoreId: 0xF101, VarOffset: 0x5A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C6 10 A9 0D AB 09 01 F1 A5 05 10 10 00 02 00 }
0x4D8C6: 				OneOfOption Option: "Don't flash or light up" Value: 0, Default { 09 07 AA 0D 10 00 00 }
0x4D8CD: 				OneOfOption Option: "Light with ITORCH current continuously" Value: 1 { 09 07 AB 0D 00 00 01 }
0x4D8D4: 				OneOfOption Option: "Flash with IFLASH current when TRIGGERed" Value: 2 { 09 07 AC 0D 00 00 02 }
0x4D8DB: 			End  { 29 02 }
0x4D8DD: 		End  { 29 02 }
0x4D8DF: 	End  { 29 02 }
0x4D8E1: 	Form FormId: 0x27C4, Title: "Flash Options" { 01 86 C4 27 A0 0D }
0x4D8E7: 		Subtitle Prompt: "Flash6", Help: "", Flags: 0x0 { 02 87 9F 0D 00 00 00 }
0x4D8EE: 		End  { 29 02 }
0x4D8F0: 		OneOf Prompt: "Flash Model", Help: "Flash Model", QuestionFlags: 0x10, QuestionId: 0x9AC, VarStoreId: 0xF101, VarOffset: 0x5A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 10 A1 0D AC 09 01 F1 A6 05 10 10 00 01 00 }
0x4D901: 			OneOfOption Option: "External - LM3643" Value: 0 { 09 07 A4 0D 00 00 00 }
0x4D908: 			OneOfOption Option: "PMIC - WRC" Value: 1, Default { 09 07 A5 0D 10 00 01 }
0x4D90F: 		End  { 29 02 }
0x4D911: 		OneOf Prompt: "Flash Mode", Help: "Select Flash Mode White LED/Warm LED/IR LED/Xeon LED", QuestionFlags: 0x10, QuestionId: 0x9AD, VarStoreId: 0xF101, VarOffset: 0x9D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 C2 10 A3 0D AD 09 01 F1 D1 09 10 10 00 04 00 }
0x4D922: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4D929: 			OneOfOption Option: "White Led" Value: 1 { 09 07 09 0C 00 00 01 }
0x4D930: 			OneOfOption Option: "Warm Led" Value: 2 { 09 07 0A 0C 00 00 02 }
0x4D937: 			OneOfOption Option: "IR Led" Value: 3 { 09 07 0B 0C 00 00 03 }
0x4D93E: 			OneOfOption Option: "Xeon Led" Value: 4 { 09 07 0C 0C 00 00 04 }
0x4D945: 		End  { 29 02 }
0x4D947: 		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0x9AE, VarStoreId: 0xF101, VarStoreInfo: 0x5A7, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0 { 1C 90 86 10 66 0C AE 09 01 F1 A7 05 00 01 0F 00 }
0x4D957: 		End  { 29 02 }
0x4D959: 		OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0x9AF, VarStoreId: 0xF101, VarOffset: 0x5C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 07 10 8F 0B AF 09 01 F1 C7 05 10 10 00 05 00 }
0x4D96A: 			OneOfOption Option: "I2C0" Value: 0 { 09 07 19 0D 00 00 00 }
0x4D971: 			OneOfOption Option: "I2C1" Value: 1 { 09 07 1A 0D 00 00 01 }
0x4D978: 			OneOfOption Option: "I2C2" Value: 2 { 09 07 1B 0D 00 00 02 }
0x4D97F: 			OneOfOption Option: "I2C3" Value: 3, Default { 09 07 1C 0D 10 00 03 }
0x4D986: 			OneOfOption Option: "I2C4" Value: 4 { 09 07 1D 0D 00 00 04 }
0x4D98D: 			OneOfOption Option: "I2C5" Value: 5 { 09 07 1E 0D 00 00 05 }
0x4D994: 		End  { 29 02 }
0x4D996: 		Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0x9B0, VarStoreId: 0xF101, VarOffset: 0x5C8, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 94 10 10 98 0B B0 09 01 F1 C8 05 10 21 00 00 7F 00 01 00 }
0x4D9AA: 			Default DefaultId: 0x0 Value: 103 { 5B 07 00 00 01 67 00 }
0x4D9B1: 		End  { 29 02 }
0x4D9B3: 		SuppressIf  { 0A 82 }
0x4D9B5: 			EqIdValList QuestionId: 0x94D, Values: [253, 254] { 14 0A 4D 09 02 00 FD 00 FE 00 }
0x4D9BF: 			Subtitle Prompt: "Flash Trigger Gpio", Help: "", Flags: 0x0 { 02 87 A6 0D 00 00 00 }
0x4D9C6: 			End  { 29 02 }
0x4D9C8: 			Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0x9B1, VarStoreId: 0xF101, VarOffset: 0x5CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x58, Step: 0x1 { 07 91 E1 10 1A 0C B1 09 01 F1 CA 05 10 10 00 58 01 }
0x4D9D9: 				Default DefaultId: 0x0 Value: 3 { 5B 06 00 00 00 03 }
0x4D9DF: 			End  { 29 02 }
0x4D9E1: 			OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0x9B2, VarStoreId: 0xF101, VarOffset: 0x5CB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xE, Step: 0x0 { 05 94 E2 10 27 0C B2 09 01 F1 CB 05 10 11 00 00 0E 00 00 00 }
0x4D9F5: 				OneOfOption Option: "A" Value: 2 { 09 08 54 0C 01 01 02 00 }
0x4D9FD: 				OneOfOption Option: "B" Value: 0 { 09 08 55 0C 01 01 00 00 }
0x4DA05: 				OneOfOption Option: "C" Value: 11 { 09 08 56 0C 01 01 0B 00 }
0x4DA0D: 				OneOfOption Option: "D" Value: 8, Default { 09 08 57 0C 11 01 08 00 }
0x4DA15: 				OneOfOption Option: "E" Value: 14 { 09 08 58 0C 01 01 0E 00 }
0x4DA1D: 				OneOfOption Option: "F" Value: 12 { 09 08 59 0C 01 01 0C 00 }
0x4DA25: 				OneOfOption Option: "H" Value: 7 { 09 08 5A 0C 01 01 07 00 }
0x4DA2D: 				OneOfOption Option: "R" Value: 3 { 09 08 5B 0C 01 01 03 00 }
0x4DA35: 				OneOfOption Option: "S" Value: 6 { 09 08 5C 0C 01 01 06 00 }
0x4DA3D: 				OneOfOption Option: "T" Value: 1 { 09 08 5D 0C 01 01 01 00 }
0x4DA45: 				OneOfOption Option: "U" Value: 9 { 09 08 5E 0C 01 01 09 00 }
0x4DA4D: 			End  { 29 02 }
0x4DA4F: 			Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0x9B3, VarStoreId: 0xF101, VarOffset: 0x5CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 E3 10 34 0C B3 09 01 F1 CD 05 10 10 00 01 01 }
0x4DA60: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4DA66: 			End  { 29 02 }
0x4DA68: 			Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0x9B4, VarStoreId: 0xF101, VarOffset: 0x5CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1 { 07 91 E4 10 41 0C B4 09 01 F1 CE 05 10 10 00 01 01 }
0x4DA79: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x4DA7F: 			End  { 29 02 }
0x4DA81: 		End  { 29 02 }
0x4DA83: 		SuppressIf  { 0A 82 }
0x4DA85: 			EqIdValList QuestionId: 0x86A, Values: [0, 1] { 14 0A 6A 08 02 00 00 00 01 00 }
0x4DA8F: 			OneOf Prompt: "Flash Driver Operating Mode", Help: "Select the Flash Driver Operating Mode as Disabled , Torch or Flash", QuestionFlags: 0x10, QuestionId: 0x9B5, VarStoreId: 0xF101, VarOffset: 0x5CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C7 10 A9 0D B5 09 01 F1 CF 05 10 10 00 02 00 }
0x4DAA0: 				OneOfOption Option: "Don't flash or light up" Value: 0, Default { 09 07 AA 0D 10 00 00 }
0x4DAA7: 				OneOfOption Option: "Light with ITORCH current continuously" Value: 1 { 09 07 AB 0D 00 00 01 }
0x4DAAE: 				OneOfOption Option: "Flash with IFLASH current when TRIGGERed" Value: 2 { 09 07 AC 0D 00 00 02 }
0x4DAB5: 			End  { 29 02 }
0x4DAB7: 		End  { 29 02 }
0x4DAB9: 	End  { 29 02 }
0x4DABB: 	Form FormId: 0x27C6, Title: "VMD setup menu" { 01 86 C6 27 90 0F }
0x4DAC1: 		Subtitle Prompt: "VMD Configuration", Help: "", Flags: 0x0 { 02 87 91 0F 00 00 00 }
0x4DAC8: 		End  { 29 02 }
0x4DACA: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DAD1: 		End  { 29 02 }
0x4DAD3: 		OneOf Prompt: "Enable VMD controller", Help: "Enable/Disable to VMD controller", QuestionFlags: 0x10, QuestionId: 0x9B6, VarStoreId: 0x4, VarOffset: 0xF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 0F 6A 0F B6 09 04 00 F8 00 10 10 00 01 00 }
0x4DAE4: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4DAEB: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DAF2: 		End  { 29 02 }
0x4DAF4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DAFB: 		End  { 29 02 }
0x4DAFD: 		SuppressIf  { 0A 82 }
0x4DAFF: 			EqIdVal QuestionId: 0x9B6, Value: 0x0 { 12 06 B6 09 00 00 }
0x4DB05: 			OneOf Prompt: "Enable VMD Global Mapping", Help: "Enable/Disable to VMD Global Mapping", QuestionFlags: 0x14, QuestionId: 0x2796, VarStoreId: 0x4, VarOffset: 0x3E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 0F 6C 0F 96 27 04 00 E6 03 14 10 00 01 00 }
0x4DB16: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DB1D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4DB24: 			End  { 29 02 }
0x4DB26: 			GrayOutIf  { 19 82 }
0x4DB28: 				EqIdVal QuestionId: 0x2796, Value: 0x1 { 12 06 96 27 01 00 }
0x4DB2E: 				SuppressIf  { 0A 82 }
0x4DB30: 					EqIdVal QuestionId: 0x1168, Value: 0x0 { 12 06 68 11 00 00 }
0x4DB36: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9B7, VarStoreId: 0x4, VarOffset: 0xF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 0F 6E 0F B7 09 04 00 F9 00 10 10 00 01 00 }
0x4DB47: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DB4C: 							Value  { 5A 82 }
0x4DB4E: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DB55: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DB5F: 									BitwiseAnd  { 35 02 }
0x4DB61: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DB6B: 									Equal  { 2F 02 }
0x4DB6D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DB77: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DB81: 									Conditional  { 50 02 }
0x4DB83: 								End  { 29 02 }
0x4DB85: 							End  { 29 02 }
0x4DB87: 						End  { 29 02 }
0x4DB89: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DB90: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DB97: 					End  { 29 02 }
0x4DB99: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 95 0F }
0x4DBA1: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DBA8: 					End  { 29 02 }
0x4DBAA: 				End  { 29 02 }
0x4DBAC: 				SuppressIf  { 0A 82 }
0x4DBAE: 					EqIdVal QuestionId: 0x1167, Value: 0x0 { 12 06 67 11 00 00 }
0x4DBB4: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9B8, VarStoreId: 0x4, VarOffset: 0xFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 11 6E 0F B8 09 04 00 FA 00 10 10 00 01 00 }
0x4DBC5: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DBCA: 							Value  { 5A 82 }
0x4DBCC: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DBD3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DBDD: 									BitwiseAnd  { 35 02 }
0x4DBDF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DBE9: 									Equal  { 2F 02 }
0x4DBEB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DBF5: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DBFF: 									Conditional  { 50 02 }
0x4DC01: 								End  { 29 02 }
0x4DC03: 							End  { 29 02 }
0x4DC05: 						End  { 29 02 }
0x4DC07: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DC0E: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DC15: 					End  { 29 02 }
0x4DC17: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 96 0F }
0x4DC1F: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DC26: 					End  { 29 02 }
0x4DC28: 				End  { 29 02 }
0x4DC2A: 				SuppressIf  { 0A 82 }
0x4DC2C: 					EqIdVal QuestionId: 0x1166, Value: 0x0 { 12 06 66 11 00 00 }
0x4DC32: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9B9, VarStoreId: 0x4, VarOffset: 0xFB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 11 6E 0F B9 09 04 00 FB 00 10 10 00 01 00 }
0x4DC43: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DC48: 							Value  { 5A 82 }
0x4DC4A: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DC51: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DC5B: 									BitwiseAnd  { 35 02 }
0x4DC5D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DC67: 									Equal  { 2F 02 }
0x4DC69: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DC73: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DC7D: 									Conditional  { 50 02 }
0x4DC7F: 								End  { 29 02 }
0x4DC81: 							End  { 29 02 }
0x4DC83: 						End  { 29 02 }
0x4DC85: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DC8C: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DC93: 					End  { 29 02 }
0x4DC95: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 97 0F }
0x4DC9D: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DCA4: 					End  { 29 02 }
0x4DCA6: 				End  { 29 02 }
0x4DCA8: 				SuppressIf  { 0A 82 }
0x4DCAA: 					EqIdVal QuestionId: 0x1165, Value: 0x0 { 12 06 65 11 00 00 }
0x4DCB0: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9BA, VarStoreId: 0x4, VarOffset: 0xFC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 03 11 6E 0F BA 09 04 00 FC 00 10 10 00 01 00 }
0x4DCC1: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DCC6: 							Value  { 5A 82 }
0x4DCC8: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DCCF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DCD9: 									BitwiseAnd  { 35 02 }
0x4DCDB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DCE5: 									Equal  { 2F 02 }
0x4DCE7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DCF1: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DCFB: 									Conditional  { 50 02 }
0x4DCFD: 								End  { 29 02 }
0x4DCFF: 							End  { 29 02 }
0x4DD01: 						End  { 29 02 }
0x4DD03: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DD0A: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DD11: 					End  { 29 02 }
0x4DD13: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 98 0F }
0x4DD1B: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DD22: 					End  { 29 02 }
0x4DD24: 				End  { 29 02 }
0x4DD26: 				SuppressIf  { 0A 82 }
0x4DD28: 					EqIdVal QuestionId: 0x1164, Value: 0x0 { 12 06 64 11 00 00 }
0x4DD2E: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9BB, VarStoreId: 0x4, VarOffset: 0xFD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 04 11 6E 0F BB 09 04 00 FD 00 10 10 00 01 00 }
0x4DD3F: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DD44: 							Value  { 5A 82 }
0x4DD46: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DD4D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DD57: 									BitwiseAnd  { 35 02 }
0x4DD59: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DD63: 									Equal  { 2F 02 }
0x4DD65: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DD6F: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DD79: 									Conditional  { 50 02 }
0x4DD7B: 								End  { 29 02 }
0x4DD7D: 							End  { 29 02 }
0x4DD7F: 						End  { 29 02 }
0x4DD81: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DD88: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DD8F: 					End  { 29 02 }
0x4DD91: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 99 0F }
0x4DD99: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DDA0: 					End  { 29 02 }
0x4DDA2: 				End  { 29 02 }
0x4DDA4: 				SuppressIf  { 0A 82 }
0x4DDA6: 					EqIdVal QuestionId: 0x1163, Value: 0x0 { 12 06 63 11 00 00 }
0x4DDAC: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9BC, VarStoreId: 0x4, VarOffset: 0xFE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 05 11 6E 0F BC 09 04 00 FE 00 10 10 00 01 00 }
0x4DDBD: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DDC2: 							Value  { 5A 82 }
0x4DDC4: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DDCB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DDD5: 									BitwiseAnd  { 35 02 }
0x4DDD7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DDE1: 									Equal  { 2F 02 }
0x4DDE3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DDED: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DDF7: 									Conditional  { 50 02 }
0x4DDF9: 								End  { 29 02 }
0x4DDFB: 							End  { 29 02 }
0x4DDFD: 						End  { 29 02 }
0x4DDFF: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DE06: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DE0D: 					End  { 29 02 }
0x4DE0F: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 9A 0F }
0x4DE17: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DE1E: 					End  { 29 02 }
0x4DE20: 				End  { 29 02 }
0x4DE22: 				SuppressIf  { 0A 82 }
0x4DE24: 					EqIdVal QuestionId: 0x1162, Value: 0x0 { 12 06 62 11 00 00 }
0x4DE2A: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9BD, VarStoreId: 0x4, VarOffset: 0xFF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 06 11 6E 0F BD 09 04 00 FF 00 10 10 00 01 00 }
0x4DE3B: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DE40: 							Value  { 5A 82 }
0x4DE42: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DE49: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DE53: 									BitwiseAnd  { 35 02 }
0x4DE55: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DE5F: 									Equal  { 2F 02 }
0x4DE61: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DE6B: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DE75: 									Conditional  { 50 02 }
0x4DE77: 								End  { 29 02 }
0x4DE79: 							End  { 29 02 }
0x4DE7B: 						End  { 29 02 }
0x4DE7D: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DE84: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DE8B: 					End  { 29 02 }
0x4DE8D: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 9B 0F }
0x4DE95: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DE9C: 					End  { 29 02 }
0x4DE9E: 				End  { 29 02 }
0x4DEA0: 				SuppressIf  { 0A 82 }
0x4DEA2: 					EqIdVal QuestionId: 0x1161, Value: 0x0 { 12 06 61 11 00 00 }
0x4DEA8: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9BE, VarStoreId: 0x4, VarOffset: 0x100, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 11 6E 0F BE 09 04 00 00 01 10 10 00 01 00 }
0x4DEB9: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DEBE: 							Value  { 5A 82 }
0x4DEC0: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DEC7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DED1: 									BitwiseAnd  { 35 02 }
0x4DED3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DEDD: 									Equal  { 2F 02 }
0x4DEDF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DEE9: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DEF3: 									Conditional  { 50 02 }
0x4DEF5: 								End  { 29 02 }
0x4DEF7: 							End  { 29 02 }
0x4DEF9: 						End  { 29 02 }
0x4DEFB: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DF02: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DF09: 					End  { 29 02 }
0x4DF0B: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 9C 0F }
0x4DF13: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DF1A: 					End  { 29 02 }
0x4DF1C: 				End  { 29 02 }
0x4DF1E: 				SuppressIf  { 0A 82 }
0x4DF20: 					EqIdVal QuestionId: 0x1160, Value: 0x0 { 12 06 60 11 00 00 }
0x4DF26: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9BF, VarStoreId: 0x4, VarOffset: 0x101, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 11 6E 0F BF 09 04 00 01 01 10 10 00 01 00 }
0x4DF37: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DF3C: 							Value  { 5A 82 }
0x4DF3E: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DF45: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DF4F: 									BitwiseAnd  { 35 02 }
0x4DF51: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DF5B: 									Equal  { 2F 02 }
0x4DF5D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DF67: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DF71: 									Conditional  { 50 02 }
0x4DF73: 								End  { 29 02 }
0x4DF75: 							End  { 29 02 }
0x4DF77: 						End  { 29 02 }
0x4DF79: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DF80: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4DF87: 					End  { 29 02 }
0x4DF89: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 9D 0F }
0x4DF91: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4DF98: 					End  { 29 02 }
0x4DF9A: 				End  { 29 02 }
0x4DF9C: 				SuppressIf  { 0A 82 }
0x4DF9E: 					EqIdVal QuestionId: 0x115F, Value: 0x0 { 12 06 5F 11 00 00 }
0x4DFA4: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C0, VarStoreId: 0x4, VarOffset: 0x102, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 11 6E 0F C0 09 04 00 02 01 10 10 00 01 00 }
0x4DFB5: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4DFBA: 							Value  { 5A 82 }
0x4DFBC: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4DFC3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DFCD: 									BitwiseAnd  { 35 02 }
0x4DFCF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DFD9: 									Equal  { 2F 02 }
0x4DFDB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4DFE5: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4DFEF: 									Conditional  { 50 02 }
0x4DFF1: 								End  { 29 02 }
0x4DFF3: 							End  { 29 02 }
0x4DFF5: 						End  { 29 02 }
0x4DFF7: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4DFFE: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E005: 					End  { 29 02 }
0x4E007: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 9E 0F }
0x4E00F: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E016: 					End  { 29 02 }
0x4E018: 				End  { 29 02 }
0x4E01A: 				SuppressIf  { 0A 82 }
0x4E01C: 					EqIdVal QuestionId: 0x115E, Value: 0x0 { 12 06 5E 11 00 00 }
0x4E022: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C1, VarStoreId: 0x4, VarOffset: 0x103, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 11 6E 0F C1 09 04 00 03 01 10 10 00 01 00 }
0x4E033: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E038: 							Value  { 5A 82 }
0x4E03A: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E041: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E04B: 									BitwiseAnd  { 35 02 }
0x4E04D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E057: 									Equal  { 2F 02 }
0x4E059: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E063: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E06D: 									Conditional  { 50 02 }
0x4E06F: 								End  { 29 02 }
0x4E071: 							End  { 29 02 }
0x4E073: 						End  { 29 02 }
0x4E075: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E07C: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E083: 					End  { 29 02 }
0x4E085: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F 9F 0F }
0x4E08D: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E094: 					End  { 29 02 }
0x4E096: 				End  { 29 02 }
0x4E098: 				SuppressIf  { 0A 82 }
0x4E09A: 					EqIdVal QuestionId: 0x115D, Value: 0x0 { 12 06 5D 11 00 00 }
0x4E0A0: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C2, VarStoreId: 0x4, VarOffset: 0x104, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 11 6E 0F C2 09 04 00 04 01 10 10 00 01 00 }
0x4E0B1: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E0B6: 							Value  { 5A 82 }
0x4E0B8: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E0BF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E0C9: 									BitwiseAnd  { 35 02 }
0x4E0CB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E0D5: 									Equal  { 2F 02 }
0x4E0D7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E0E1: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E0EB: 									Conditional  { 50 02 }
0x4E0ED: 								End  { 29 02 }
0x4E0EF: 							End  { 29 02 }
0x4E0F1: 						End  { 29 02 }
0x4E0F3: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E0FA: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E101: 					End  { 29 02 }
0x4E103: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A0 0F }
0x4E10B: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E112: 					End  { 29 02 }
0x4E114: 				End  { 29 02 }
0x4E116: 				SuppressIf  { 0A 82 }
0x4E118: 					EqIdVal QuestionId: 0x115C, Value: 0x0 { 12 06 5C 11 00 00 }
0x4E11E: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C3, VarStoreId: 0x4, VarOffset: 0x105, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0C 11 6E 0F C3 09 04 00 05 01 10 10 00 01 00 }
0x4E12F: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E134: 							Value  { 5A 82 }
0x4E136: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E13D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E147: 									BitwiseAnd  { 35 02 }
0x4E149: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E153: 									Equal  { 2F 02 }
0x4E155: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E15F: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E169: 									Conditional  { 50 02 }
0x4E16B: 								End  { 29 02 }
0x4E16D: 							End  { 29 02 }
0x4E16F: 						End  { 29 02 }
0x4E171: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E178: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E17F: 					End  { 29 02 }
0x4E181: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A1 0F }
0x4E189: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E190: 					End  { 29 02 }
0x4E192: 				End  { 29 02 }
0x4E194: 				SuppressIf  { 0A 82 }
0x4E196: 					EqIdVal QuestionId: 0x115B, Value: 0x0 { 12 06 5B 11 00 00 }
0x4E19C: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C4, VarStoreId: 0x4, VarOffset: 0x106, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0D 11 6E 0F C4 09 04 00 06 01 10 10 00 01 00 }
0x4E1AD: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E1B2: 							Value  { 5A 82 }
0x4E1B4: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E1BB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E1C5: 									BitwiseAnd  { 35 02 }
0x4E1C7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E1D1: 									Equal  { 2F 02 }
0x4E1D3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E1DD: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E1E7: 									Conditional  { 50 02 }
0x4E1E9: 								End  { 29 02 }
0x4E1EB: 							End  { 29 02 }
0x4E1ED: 						End  { 29 02 }
0x4E1EF: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E1F6: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E1FD: 					End  { 29 02 }
0x4E1FF: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A2 0F }
0x4E207: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E20E: 					End  { 29 02 }
0x4E210: 				End  { 29 02 }
0x4E212: 				SuppressIf  { 0A 82 }
0x4E214: 					EqIdVal QuestionId: 0x115A, Value: 0x0 { 12 06 5A 11 00 00 }
0x4E21A: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C5, VarStoreId: 0x4, VarOffset: 0x107, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 11 6E 0F C5 09 04 00 07 01 10 10 00 01 00 }
0x4E22B: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E230: 							Value  { 5A 82 }
0x4E232: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E239: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E243: 									BitwiseAnd  { 35 02 }
0x4E245: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E24F: 									Equal  { 2F 02 }
0x4E251: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E25B: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E265: 									Conditional  { 50 02 }
0x4E267: 								End  { 29 02 }
0x4E269: 							End  { 29 02 }
0x4E26B: 						End  { 29 02 }
0x4E26D: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E274: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E27B: 					End  { 29 02 }
0x4E27D: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A3 0F }
0x4E285: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E28C: 					End  { 29 02 }
0x4E28E: 				End  { 29 02 }
0x4E290: 				SuppressIf  { 0A 82 }
0x4E292: 					EqIdVal QuestionId: 0x1159, Value: 0x0 { 12 06 59 11 00 00 }
0x4E298: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C6, VarStoreId: 0x4, VarOffset: 0x108, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0F 11 6E 0F C6 09 04 00 08 01 10 10 00 01 00 }
0x4E2A9: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E2AE: 							Value  { 5A 82 }
0x4E2B0: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E2B7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E2C1: 									BitwiseAnd  { 35 02 }
0x4E2C3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E2CD: 									Equal  { 2F 02 }
0x4E2CF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E2D9: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E2E3: 									Conditional  { 50 02 }
0x4E2E5: 								End  { 29 02 }
0x4E2E7: 							End  { 29 02 }
0x4E2E9: 						End  { 29 02 }
0x4E2EB: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E2F2: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E2F9: 					End  { 29 02 }
0x4E2FB: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A4 0F }
0x4E303: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E30A: 					End  { 29 02 }
0x4E30C: 				End  { 29 02 }
0x4E30E: 				SuppressIf  { 0A 82 }
0x4E310: 					EqIdVal QuestionId: 0x1158, Value: 0x0 { 12 06 58 11 00 00 }
0x4E316: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C7, VarStoreId: 0x4, VarOffset: 0x109, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 10 11 6E 0F C7 09 04 00 09 01 10 10 00 01 00 }
0x4E327: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E32C: 							Value  { 5A 82 }
0x4E32E: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E335: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E33F: 									BitwiseAnd  { 35 02 }
0x4E341: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E34B: 									Equal  { 2F 02 }
0x4E34D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E357: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E361: 									Conditional  { 50 02 }
0x4E363: 								End  { 29 02 }
0x4E365: 							End  { 29 02 }
0x4E367: 						End  { 29 02 }
0x4E369: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E370: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E377: 					End  { 29 02 }
0x4E379: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A5 0F }
0x4E381: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E388: 					End  { 29 02 }
0x4E38A: 				End  { 29 02 }
0x4E38C: 				SuppressIf  { 0A 82 }
0x4E38E: 					EqIdVal QuestionId: 0x1157, Value: 0x0 { 12 06 57 11 00 00 }
0x4E394: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C8, VarStoreId: 0x4, VarOffset: 0x10A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 11 6E 0F C8 09 04 00 0A 01 10 10 00 01 00 }
0x4E3A5: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E3AA: 							Value  { 5A 82 }
0x4E3AC: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E3B3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E3BD: 									BitwiseAnd  { 35 02 }
0x4E3BF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E3C9: 									Equal  { 2F 02 }
0x4E3CB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E3D5: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E3DF: 									Conditional  { 50 02 }
0x4E3E1: 								End  { 29 02 }
0x4E3E3: 							End  { 29 02 }
0x4E3E5: 						End  { 29 02 }
0x4E3E7: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E3EE: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E3F5: 					End  { 29 02 }
0x4E3F7: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A6 0F }
0x4E3FF: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E406: 					End  { 29 02 }
0x4E408: 				End  { 29 02 }
0x4E40A: 				SuppressIf  { 0A 82 }
0x4E40C: 					EqIdVal QuestionId: 0x1156, Value: 0x0 { 12 06 56 11 00 00 }
0x4E412: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9C9, VarStoreId: 0x4, VarOffset: 0x10B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 12 11 6E 0F C9 09 04 00 0B 01 10 10 00 01 00 }
0x4E423: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E428: 							Value  { 5A 82 }
0x4E42A: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E431: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E43B: 									BitwiseAnd  { 35 02 }
0x4E43D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E447: 									Equal  { 2F 02 }
0x4E449: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E453: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E45D: 									Conditional  { 50 02 }
0x4E45F: 								End  { 29 02 }
0x4E461: 							End  { 29 02 }
0x4E463: 						End  { 29 02 }
0x4E465: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E46C: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E473: 					End  { 29 02 }
0x4E475: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A7 0F }
0x4E47D: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E484: 					End  { 29 02 }
0x4E486: 				End  { 29 02 }
0x4E488: 				SuppressIf  { 0A 82 }
0x4E48A: 					EqIdVal QuestionId: 0x1155, Value: 0x0 { 12 06 55 11 00 00 }
0x4E490: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9CA, VarStoreId: 0x4, VarOffset: 0x10C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 13 11 6E 0F CA 09 04 00 0C 01 10 10 00 01 00 }
0x4E4A1: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E4A6: 							Value  { 5A 82 }
0x4E4A8: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E4AF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E4B9: 									BitwiseAnd  { 35 02 }
0x4E4BB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E4C5: 									Equal  { 2F 02 }
0x4E4C7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E4D1: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E4DB: 									Conditional  { 50 02 }
0x4E4DD: 								End  { 29 02 }
0x4E4DF: 							End  { 29 02 }
0x4E4E1: 						End  { 29 02 }
0x4E4E3: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E4EA: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E4F1: 					End  { 29 02 }
0x4E4F3: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A8 0F }
0x4E4FB: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E502: 					End  { 29 02 }
0x4E504: 				End  { 29 02 }
0x4E506: 				SuppressIf  { 0A 82 }
0x4E508: 					EqIdVal QuestionId: 0x1154, Value: 0x0 { 12 06 54 11 00 00 }
0x4E50E: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9CB, VarStoreId: 0x4, VarOffset: 0x10D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 11 6E 0F CB 09 04 00 0D 01 10 10 00 01 00 }
0x4E51F: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E524: 							Value  { 5A 82 }
0x4E526: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E52D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E537: 									BitwiseAnd  { 35 02 }
0x4E539: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E543: 									Equal  { 2F 02 }
0x4E545: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E54F: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E559: 									Conditional  { 50 02 }
0x4E55B: 								End  { 29 02 }
0x4E55D: 							End  { 29 02 }
0x4E55F: 						End  { 29 02 }
0x4E561: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E568: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E56F: 					End  { 29 02 }
0x4E571: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F A9 0F }
0x4E579: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E580: 					End  { 29 02 }
0x4E582: 				End  { 29 02 }
0x4E584: 				SuppressIf  { 0A 82 }
0x4E586: 					EqIdVal QuestionId: 0x1153, Value: 0x0 { 12 06 53 11 00 00 }
0x4E58C: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9CC, VarStoreId: 0x4, VarOffset: 0x10E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 15 11 6E 0F CC 09 04 00 0E 01 10 10 00 01 00 }
0x4E59D: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E5A2: 							Value  { 5A 82 }
0x4E5A4: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E5AB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E5B5: 									BitwiseAnd  { 35 02 }
0x4E5B7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E5C1: 									Equal  { 2F 02 }
0x4E5C3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E5CD: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E5D7: 									Conditional  { 50 02 }
0x4E5D9: 								End  { 29 02 }
0x4E5DB: 							End  { 29 02 }
0x4E5DD: 						End  { 29 02 }
0x4E5DF: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E5E6: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E5ED: 					End  { 29 02 }
0x4E5EF: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F AA 0F }
0x4E5F7: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E5FE: 					End  { 29 02 }
0x4E600: 				End  { 29 02 }
0x4E602: 				SuppressIf  { 0A 82 }
0x4E604: 					EqIdVal QuestionId: 0x1152, Value: 0x0 { 12 06 52 11 00 00 }
0x4E60A: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9CD, VarStoreId: 0x4, VarOffset: 0x10F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 16 11 6E 0F CD 09 04 00 0F 01 10 10 00 01 00 }
0x4E61B: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E620: 							Value  { 5A 82 }
0x4E622: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E629: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E633: 									BitwiseAnd  { 35 02 }
0x4E635: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E63F: 									Equal  { 2F 02 }
0x4E641: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E64B: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E655: 									Conditional  { 50 02 }
0x4E657: 								End  { 29 02 }
0x4E659: 							End  { 29 02 }
0x4E65B: 						End  { 29 02 }
0x4E65D: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E664: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E66B: 					End  { 29 02 }
0x4E66D: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F AB 0F }
0x4E675: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E67C: 					End  { 29 02 }
0x4E67E: 				End  { 29 02 }
0x4E680: 				SuppressIf  { 0A 82 }
0x4E682: 					EqIdVal QuestionId: 0x1151, Value: 0x0 { 12 06 51 11 00 00 }
0x4E688: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9CE, VarStoreId: 0x4, VarOffset: 0x110, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 17 11 6E 0F CE 09 04 00 10 01 10 10 00 01 00 }
0x4E699: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E69E: 							Value  { 5A 82 }
0x4E6A0: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E6A7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E6B1: 									BitwiseAnd  { 35 02 }
0x4E6B3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E6BD: 									Equal  { 2F 02 }
0x4E6BF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E6C9: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E6D3: 									Conditional  { 50 02 }
0x4E6D5: 								End  { 29 02 }
0x4E6D7: 							End  { 29 02 }
0x4E6D9: 						End  { 29 02 }
0x4E6DB: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E6E2: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E6E9: 					End  { 29 02 }
0x4E6EB: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F AC 0F }
0x4E6F3: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E6FA: 					End  { 29 02 }
0x4E6FC: 				End  { 29 02 }
0x4E6FE: 				SuppressIf  { 0A 82 }
0x4E700: 					EqIdVal QuestionId: 0x1150, Value: 0x0 { 12 06 50 11 00 00 }
0x4E706: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9CF, VarStoreId: 0x4, VarOffset: 0x111, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 18 11 6E 0F CF 09 04 00 11 01 10 10 00 01 00 }
0x4E717: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E71C: 							Value  { 5A 82 }
0x4E71E: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E725: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E72F: 									BitwiseAnd  { 35 02 }
0x4E731: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E73B: 									Equal  { 2F 02 }
0x4E73D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E747: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E751: 									Conditional  { 50 02 }
0x4E753: 								End  { 29 02 }
0x4E755: 							End  { 29 02 }
0x4E757: 						End  { 29 02 }
0x4E759: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E760: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E767: 					End  { 29 02 }
0x4E769: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F AD 0F }
0x4E771: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E778: 					End  { 29 02 }
0x4E77A: 				End  { 29 02 }
0x4E77C: 				SuppressIf  { 0A 82 }
0x4E77E: 					EqIdVal QuestionId: 0x114F, Value: 0x0 { 12 06 4F 11 00 00 }
0x4E784: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9D0, VarStoreId: 0x4, VarOffset: 0x112, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 19 11 6E 0F D0 09 04 00 12 01 10 10 00 01 00 }
0x4E795: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E79A: 							Value  { 5A 82 }
0x4E79C: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E7A3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E7AD: 									BitwiseAnd  { 35 02 }
0x4E7AF: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E7B9: 									Equal  { 2F 02 }
0x4E7BB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E7C5: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E7CF: 									Conditional  { 50 02 }
0x4E7D1: 								End  { 29 02 }
0x4E7D3: 							End  { 29 02 }
0x4E7D5: 						End  { 29 02 }
0x4E7D7: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E7DE: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E7E5: 					End  { 29 02 }
0x4E7E7: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F AE 0F }
0x4E7EF: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E7F6: 					End  { 29 02 }
0x4E7F8: 				End  { 29 02 }
0x4E7FA: 				SuppressIf  { 0A 82 }
0x4E7FC: 					EqIdVal QuestionId: 0x114E, Value: 0x0 { 12 06 4E 11 00 00 }
0x4E802: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9D1, VarStoreId: 0x4, VarOffset: 0x113, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1A 11 6E 0F D1 09 04 00 13 01 10 10 00 01 00 }
0x4E813: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E818: 							Value  { 5A 82 }
0x4E81A: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E821: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E82B: 									BitwiseAnd  { 35 02 }
0x4E82D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E837: 									Equal  { 2F 02 }
0x4E839: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E843: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E84D: 									Conditional  { 50 02 }
0x4E84F: 								End  { 29 02 }
0x4E851: 							End  { 29 02 }
0x4E853: 						End  { 29 02 }
0x4E855: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E85C: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E863: 					End  { 29 02 }
0x4E865: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F AF 0F }
0x4E86D: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E874: 					End  { 29 02 }
0x4E876: 				End  { 29 02 }
0x4E878: 				SuppressIf  { 0A 82 }
0x4E87A: 					EqIdVal QuestionId: 0x114D, Value: 0x0 { 12 06 4D 11 00 00 }
0x4E880: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9D2, VarStoreId: 0x4, VarOffset: 0x114, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1B 11 6E 0F D2 09 04 00 14 01 10 10 00 01 00 }
0x4E891: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E896: 							Value  { 5A 82 }
0x4E898: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E89F: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E8A9: 									BitwiseAnd  { 35 02 }
0x4E8AB: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E8B5: 									Equal  { 2F 02 }
0x4E8B7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E8C1: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E8CB: 									Conditional  { 50 02 }
0x4E8CD: 								End  { 29 02 }
0x4E8CF: 							End  { 29 02 }
0x4E8D1: 						End  { 29 02 }
0x4E8D3: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E8DA: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E8E1: 					End  { 29 02 }
0x4E8E3: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F B0 0F }
0x4E8EB: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E8F2: 					End  { 29 02 }
0x4E8F4: 				End  { 29 02 }
0x4E8F6: 				SuppressIf  { 0A 82 }
0x4E8F8: 					EqIdVal QuestionId: 0x114C, Value: 0x0 { 12 06 4C 11 00 00 }
0x4E8FE: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9D3, VarStoreId: 0x4, VarOffset: 0x115, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1C 11 6E 0F D3 09 04 00 15 01 10 10 00 01 00 }
0x4E90F: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E914: 							Value  { 5A 82 }
0x4E916: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E91D: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E927: 									BitwiseAnd  { 35 02 }
0x4E929: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E933: 									Equal  { 2F 02 }
0x4E935: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E93F: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E949: 									Conditional  { 50 02 }
0x4E94B: 								End  { 29 02 }
0x4E94D: 							End  { 29 02 }
0x4E94F: 						End  { 29 02 }
0x4E951: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E958: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E95F: 					End  { 29 02 }
0x4E961: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F B1 0F }
0x4E969: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E970: 					End  { 29 02 }
0x4E972: 				End  { 29 02 }
0x4E974: 				SuppressIf  { 0A 82 }
0x4E976: 					EqIdVal QuestionId: 0x114B, Value: 0x0 { 12 06 4B 11 00 00 }
0x4E97C: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9D4, VarStoreId: 0x4, VarOffset: 0x116, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1D 11 6E 0F D4 09 04 00 16 01 10 10 00 01 00 }
0x4E98D: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4E992: 							Value  { 5A 82 }
0x4E994: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4E99B: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E9A5: 									BitwiseAnd  { 35 02 }
0x4E9A7: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E9B1: 									Equal  { 2F 02 }
0x4E9B3: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4E9BD: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4E9C7: 									Conditional  { 50 02 }
0x4E9C9: 								End  { 29 02 }
0x4E9CB: 							End  { 29 02 }
0x4E9CD: 						End  { 29 02 }
0x4E9CF: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4E9D6: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4E9DD: 					End  { 29 02 }
0x4E9DF: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F B2 0F }
0x4E9E7: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4E9EE: 					End  { 29 02 }
0x4E9F0: 				End  { 29 02 }
0x4E9F2: 				SuppressIf  { 0A 82 }
0x4E9F4: 					EqIdVal QuestionId: 0x114A, Value: 0x0 { 12 06 4A 11 00 00 }
0x4E9FA: 					OneOf Prompt: "Map this Root Port under VMD", Help: "Map/UnMap this Root Port to VMD", QuestionFlags: 0x10, QuestionId: 0x9D5, VarStoreId: 0x4, VarOffset: 0x117, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1E 11 6E 0F D5 09 04 00 17 01 10 10 00 01 00 }
0x4EA0B: 						Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4EA10: 							Value  { 5A 82 }
0x4EA12: 								Get VarStoreId: 0x4, VarStoreInfo: 0x3E6, VarStoreType: 0x0 { 2B 87 04 00 E6 03 00 }
0x4EA19: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4EA23: 									BitwiseAnd  { 35 02 }
0x4EA25: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4EA2F: 									Equal  { 2F 02 }
0x4EA31: 									Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4EA3B: 									Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4EA45: 									Conditional  { 50 02 }
0x4EA47: 								End  { 29 02 }
0x4EA49: 							End  { 29 02 }
0x4EA4B: 						End  { 29 02 }
0x4EA4D: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EA54: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4EA5B: 					End  { 29 02 }
0x4EA5D: 					Text Prompt: "Root Port BDF details", Help: "Root Port BDF", Text: "N/A" { 03 08 94 0F 93 0F B3 0F }
0x4EA65: 					Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4EA6C: 					End  { 29 02 }
0x4EA6E: 				End  { 29 02 }
0x4EA70: 			End  { 29 02 }
0x4EA72: 			SuppressIf  { 0A 82 }
0x4EA74: 				Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4EA7E: 				Numeric Prompt: "VMD Config Bar Size", Help: "Set The VMD Config Bar Size", QuestionFlags: 0x10, QuestionId: 0x9D6, VarStoreId: 0x4, VarOffset: 0x175, Flags: 0x10, Size: 8, Min: 0x14, Max: 0x1B, Step: 0x1 { 07 91 6F 0F 70 0F D6 09 04 00 75 01 10 10 14 1B 01 }
0x4EA8F: 					Default DefaultId: 0x0 Value: 25 { 5B 06 00 00 00 19 }
0x4EA95: 				End  { 29 02 }
0x4EA97: 				OneOf Prompt: "VMD Config Bar Attributes", Help: "Set The VMD Config Bar Attributes", QuestionFlags: 0x10, QuestionId: 0x9D7, VarStoreId: 0x4, VarOffset: 0x176, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 71 0F 72 0F D7 09 04 00 76 01 10 10 00 02 00 }
0x4EAA8: 					OneOfOption Option: "VMD 64bit prefetch" Value: 2 { 09 07 73 0F 00 00 02 }
0x4EAAF: 					OneOfOption Option: "VMD 32bit non prefetch" Value: 0 { 09 07 74 0F 00 00 00 }
0x4EAB6: 					OneOfOption Option: "VMD 64bit non prefetch" Value: 1, Default, MfgDefault { 09 07 75 0F 30 00 01 }
0x4EABD: 				End  { 29 02 }
0x4EABF: 				Numeric Prompt: "VMD Mem Bar1 Size", Help: "Set The VMD Mem Bar1 Size", QuestionFlags: 0x10, QuestionId: 0x9D8, VarStoreId: 0x4, VarOffset: 0x177, Flags: 0x10, Size: 8, Min: 0x14, Max: 0x27, Step: 0x1 { 07 91 76 0F 77 0F D8 09 04 00 77 01 10 10 14 27 01 }
0x4EAD0: 					Default DefaultId: 0x0 Value: 25 { 5B 06 00 00 00 19 }
0x4EAD6: 				End  { 29 02 }
0x4EAD8: 				OneOf Prompt: "VMD Mem Bar1 Attributes", Help: "Set The VMD Mem Bar1 Attributes", QuestionFlags: 0x10, QuestionId: 0x9D9, VarStoreId: 0x4, VarOffset: 0x178, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 78 0F 79 0F D9 09 04 00 78 01 10 10 00 02 00 }
0x4EAE9: 					OneOfOption Option: "VMD 32bit non prefetch" Value: 0, Default, MfgDefault { 09 07 74 0F 30 00 00 }
0x4EAF0: 					OneOfOption Option: "VMD 64bit non prefetch" Value: 1 { 09 07 75 0F 00 00 01 }
0x4EAF7: 					OneOfOption Option: "VMD 64bit prefetch" Value: 2 { 09 07 73 0F 00 00 02 }
0x4EAFE: 				End  { 29 02 }
0x4EB00: 				Numeric Prompt: "VMD Mem Bar2 Size", Help: "Set The VMD Mem Bar2 Size", QuestionFlags: 0x10, QuestionId: 0x9DA, VarStoreId: 0x4, VarOffset: 0x179, Flags: 0x10, Size: 8, Min: 0x14, Max: 0x27, Step: 0x1 { 07 91 7A 0F 7B 0F DA 09 04 00 79 01 10 10 14 27 01 }
0x4EB11: 					Default DefaultId: 0x0 Value: 20 { 5B 06 00 00 00 14 }
0x4EB17: 				End  { 29 02 }
0x4EB19: 				OneOf Prompt: "VMD Mem Bar2 Attributes", Help: "Set The VMD Mem Bar2 Attributes", QuestionFlags: 0x10, QuestionId: 0x9DB, VarStoreId: 0x4, VarOffset: 0x17A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 7C 0F 7D 0F DB 09 04 00 7A 01 10 10 00 02 00 }
0x4EB2A: 					OneOfOption Option: "VMD 32bit non prefetch" Value: 0 { 09 07 74 0F 00 00 00 }
0x4EB31: 					OneOfOption Option: "VMD 64bit non prefetch" Value: 1, Default, MfgDefault { 09 07 75 0F 30 00 01 }
0x4EB38: 					OneOfOption Option: "VMD 64bit prefetch" Value: 2 { 09 07 73 0F 00 00 02 }
0x4EB3F: 				End  { 29 02 }
0x4EB41: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4EB48: 				End  { 29 02 }
0x4EB4A: 			End  { 29 02 }
0x4EB4C: 			OneOf Prompt: "RAID0", Help: "Enable/Disable RAID0 support", QuestionFlags: 0x10, QuestionId: 0x9DC, VarStoreId: 0x4, VarOffset: 0x17F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7E 0F 7F 0F DC 09 04 00 7F 01 10 10 00 01 00 }
0x4EB5D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EB64: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EB6B: 			End  { 29 02 }
0x4EB6D: 			OneOf Prompt: "RAID1", Help: "Enable/Disable RAID1 support", QuestionFlags: 0x10, QuestionId: 0x9DD, VarStoreId: 0x4, VarOffset: 0x180, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 80 0F 81 0F DD 09 04 00 80 01 10 10 00 01 00 }
0x4EB7E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EB85: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EB8C: 			End  { 29 02 }
0x4EB8E: 			OneOf Prompt: "RAID5", Help: "Enable/Disable RAID5 support", QuestionFlags: 0x10, QuestionId: 0x9DE, VarStoreId: 0x4, VarOffset: 0x182, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 0F 83 0F DE 09 04 00 82 01 10 10 00 01 00 }
0x4EB9F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EBA6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EBAD: 			End  { 29 02 }
0x4EBAF: 			OneOf Prompt: "RAID10", Help: "Enable/Disable RAID10 support", QuestionFlags: 0x10, QuestionId: 0x9DF, VarStoreId: 0x4, VarOffset: 0x181, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 0F 85 0F DF 09 04 00 81 01 10 10 00 01 00 }
0x4EBC0: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EBC7: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EBCE: 			End  { 29 02 }
0x4EBD0: 			OneOf Prompt: "Intel Rapid Recovery Technology", Help: "Enable/Disable Intel Rapid Recovery Technology.", QuestionFlags: 0x10, QuestionId: 0x9E0, VarStoreId: 0x4, VarOffset: 0x183, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 0F 87 0F E0 09 04 00 83 01 10 10 00 01 00 }
0x4EBE1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EBE8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EBEF: 			End  { 29 02 }
0x4EBF1: 			OneOf Prompt: "RRT volumes can span internal and eSATA drives", Help: "Enable/Disable RRT volumes can span internal and eSATA drives.", QuestionFlags: 0x10, QuestionId: 0x9E1, VarStoreId: 0x4, VarOffset: 0x184, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 88 0F 89 0F E1 09 04 00 84 01 10 10 00 01 00 }
0x4EC02: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EC09: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EC10: 			End  { 29 02 }
0x4EC12: 			OneOf Prompt: "Intel(R) Optane(TM) Memory", Help: "Enable/Disable System Acceleration with Intel(R) Optane(TM) Memory feature.", QuestionFlags: 0x10, QuestionId: 0x9E2, VarStoreId: 0x4, VarOffset: 0x185, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 0F 8B 0F E2 09 04 00 85 01 10 10 00 01 00 }
0x4EC23: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EC2A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EC31: 			End  { 29 02 }
0x4EC33: 			SuppressIf  { 0A 82 }
0x4EC35: 				EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x4EC3B: 				OneOf Prompt: "ZPODD", Help: "Enable/Disable ZPODD. 
The option is only needed to be enabled when ZPODD is connected in VMD mode", QuestionFlags: 0x10, QuestionId: 0x2797, VarStoreId: 0xF101, VarOffset: 0xBAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 0F 8D 0F 97 27 01 F1 AF 0B 10 10 00 01 00 }
0x4EC4C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4EC53: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4EC5A: 				End  { 29 02 }
0x4EC5C: 			End  { 29 02 }
0x4EC5E: 		End  { 29 02 }
0x4EC60: 	End  { 29 02 }
0x4EC62: 	Form FormId: 0x27C7, Title: "Display setup menu" { 01 86 C7 27 EC 0F }
0x4EC68: 		Subtitle Prompt: "Display Configuration", Help: "", Flags: 0x0 { 02 87 ED 0F 00 00 00 }
0x4EC6F: 		End  { 29 02 }
0x4EC71: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4EC78: 		End  { 29 02 }
0x4EC7A: 	End  { 29 02 }
0x4EC7C: 	Form FormId: 0x27C8, Title: "PCI Express Configuration" { 01 86 C8 27 7C 0E }
0x4EC82: 		Subtitle Prompt: "PCI Express Configuration", Help: "", Flags: 0x0 { 02 87 7C 0E 00 00 00 }
0x4EC89: 		End  { 29 02 }
0x4EC8B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4EC92: 		End  { 29 02 }
0x4EC94: 		OneOf Prompt: "Fia Programming", Help: "Load Fia Configuration if Enabled for each root port.", QuestionFlags: 0x10, QuestionId: 0x9E3, VarStoreId: 0x4, VarOffset: 0x2A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 0E 85 0E E3 09 04 00 A4 02 10 10 00 01 00 }
0x4ECA5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4ECAC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4ECB3: 		End  { 29 02 }
0x4ECB5: 		OneOf Prompt: "Compliance Test Mode", Help: "Enable when using Compliance Load Board", QuestionFlags: 0x10, QuestionId: 0x9E4, VarStoreId: 0x4, VarOffset: 0x2AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 0E 8D 0E E4 09 04 00 AD 02 10 10 00 01 00 }
0x4ECC6: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4ECCD: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4ECD4: 		End  { 29 02 }
0x4ECD6: 		OneOf Prompt: "CDR Relock", Help: "Enable/Disable CDR Relock", QuestionFlags: 0x10, QuestionId: 0x9E5, VarStoreId: 0x4, VarOffset: 0x3FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F0 0E F2 0E E5 09 04 00 FF 03 10 10 00 01 00 }
0x4ECE7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4ECEE: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4ECF5: 		End  { 29 02 }
0x4ECF7: 		OneOf Prompt: "Assertion on Link Down GPIOs", Help: "GPIO Assertion on Link Down", QuestionFlags: 0x10, QuestionId: 0x9E6, VarStoreId: 0x4, VarOffset: 0x327, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 0E 8F 0E E6 09 04 00 27 03 10 10 00 01 00 }
0x4ED08: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4ED0F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4ED16: 		End  { 29 02 }
0x4ED18: 		OneOf Prompt: "PCI Express Slot Selection", Help: "Select the PCIe M2 or CEMx4 slot", QuestionFlags: 0x10, QuestionId: 0x9E7, VarStoreId: 0x4, VarOffset: 0x32C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 0E 95 0E E7 09 04 00 2C 03 10 10 00 01 00 }
0x4ED29: 			OneOfOption Option: "M2" Value: 1, Default, MfgDefault { 09 07 96 0E 30 00 01 }
0x4ED30: 			OneOfOption Option: "CEMx4 slot" Value: 0 { 09 07 97 0E 00 00 00 }
0x4ED37: 		End  { 29 02 }
0x4ED39: 		SuppressIf  { 0A 82 }
0x4ED3B: 			True  { 46 02 }
0x4ED3D: 			OneOf Prompt: "PCIE Resizable BAR Support", Help: "Enable/Disable PCIE Resizable BAR Support", QuestionFlags: 0x10, QuestionId: 0x9E8, VarStoreId: 0x4, VarOffset: 0x42B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 08 9C 08 E8 09 04 00 2B 04 10 10 00 01 00 }
0x4ED4E: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4ED54: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x4ED5B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 92 00 00 00 00 }
0x4ED62: 			End  { 29 02 }
0x4ED64: 		End  { 29 02 }
0x4ED66: 		SuppressIf  { 0A 82 }
0x4ED68: 			EqIdVal QuestionId: 0x1149, Value: 0x0 { 12 86 49 11 00 00 }
0x4ED6E: 				Not  { 17 02 }
0x4ED70: 			End  { 29 02 }
0x4ED72: 			Ref Prompt: "PCI Express Root Port 1", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0x9E9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C9 { 0F 0F 76 16 92 16 E9 09 00 00 FF FF 00 C9 27 }
0x4ED81: 		End  { 29 02 }
0x4ED83: 		SuppressIf  { 0A 82 }
0x4ED85: 			EqIdVal QuestionId: 0x1149, Value: 0x1 { 12 86 49 11 01 00 }
0x4ED8B: 				Not  { 17 02 }
0x4ED8D: 			End  { 29 02 }
0x4ED8F: 			Text Prompt: "PCI Express Root Port 1", Help: "", Text: "Not present in this SKU" { 03 08 76 16 C9 07 82 0E }
0x4ED97: 		End  { 29 02 }
0x4ED99: 		SuppressIf  { 0A 82 }
0x4ED9B: 			EqIdVal QuestionId: 0x1148, Value: 0x0 { 12 86 48 11 00 00 }
0x4EDA1: 				Not  { 17 02 }
0x4EDA3: 			End  { 29 02 }
0x4EDA5: 			Ref Prompt: "PCI Express Root Port 2", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0x9EA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27CA { 0F 0F 77 16 92 16 EA 09 00 00 FF FF 00 CA 27 }
0x4EDB4: 		End  { 29 02 }
0x4EDB6: 		SuppressIf  { 0A 82 }
0x4EDB8: 			EqIdVal QuestionId: 0x1148, Value: 0x1 { 12 86 48 11 01 00 }
0x4EDBE: 				Not  { 17 02 }
0x4EDC0: 			End  { 29 02 }
0x4EDC2: 			Text Prompt: "PCI Express Root Port 2", Help: "", Text: "Not present in this SKU" { 03 08 77 16 C9 07 82 0E }
0x4EDCA: 		End  { 29 02 }
0x4EDCC: 		SuppressIf  { 0A 82 }
0x4EDCE: 			EqIdVal QuestionId: 0x1147, Value: 0x0 { 12 86 47 11 00 00 }
0x4EDD4: 				Not  { 17 02 }
0x4EDD6: 			End  { 29 02 }
0x4EDD8: 			Ref Prompt: "PCI Express Root Port 3", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0x9EB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27CB { 0F 0F 78 16 92 16 EB 09 00 00 FF FF 00 CB 27 }
0x4EDE7: 		End  { 29 02 }
0x4EDE9: 		SuppressIf  { 0A 82 }
0x4EDEB: 			EqIdVal QuestionId: 0x1147, Value: 0x1 { 12 86 47 11 01 00 }
0x4EDF1: 				Not  { 17 02 }
0x4EDF3: 			End  { 29 02 }
0x4EDF5: 			Text Prompt: "PCI Express Root Port 3", Help: "", Text: "Not present in this SKU" { 03 08 78 16 C9 07 82 0E }
0x4EDFD: 		End  { 29 02 }
0x4EDFF: 	End  { 29 02 }
0x4EE01: 	Form FormId: 0x27C9, Title: "PCI Express Root Port 1" { 01 86 C9 27 7E 0E }
0x4EE07: 		OneOf Prompt: "PCI Express Root Port 1", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x9EC, VarStoreId: 0x4, VarOffset: 0x278, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 0F 81 0E EC 09 04 00 78 02 10 10 00 01 00 }
0x4EE18: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EE1F: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EE26: 		End  { 29 02 }
0x4EE28: 		SuppressIf  { 0A 82 }
0x4EE2A: 			EqIdVal QuestionId: 0x9EC, Value: 0x0 { 12 06 EC 09 00 00 }
0x4EE30: 			GrayOutIf  { 19 82 }
0x4EE32: 				EqIdVal QuestionId: 0x9FE, Value: 0x1 { 12 06 FE 09 01 00 }
0x4EE38: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0x9ED, VarStoreId: 0x4, VarOffset: 0x331, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 0E E5 0E ED 09 04 00 31 03 10 10 00 01 00 }
0x4EE49: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x4EE50: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x4EE57: 				End  { 29 02 }
0x4EE59: 			End  { 29 02 }
0x4EE5B: 			OneOf Prompt: "PCI Express Clock Gating", Help: "PCI Express Clock Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0x2798, VarStoreId: 0x4, VarOffset: 0x2A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 0E 89 0E 98 27 04 00 A5 02 10 10 00 01 00 }
0x4EE6C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EE73: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EE7A: 			End  { 29 02 }
0x4EE7C: 			OneOf Prompt: "PCI Express Power Gating", Help: "PCI Express Power Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0x9EE, VarStoreId: 0x4, VarOffset: 0x2A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 0E 8B 0E EE 09 04 00 A9 02 10 10 00 01 00 }
0x4EE8D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EE94: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EE9B: 			End  { 29 02 }
0x4EE9D: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2799, VarStoreId: 0x4, VarOffset: 0x379, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F8 0E F5 0D 99 27 04 00 79 03 10 10 00 03 00 }
0x4EEAE: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EEB5: 				OneOfOption Option: "L0s" Value: 1 { 09 07 FB 0E 00 00 01 }
0x4EEBC: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x4EEC3: 				OneOfOption Option: "L0sL1" Value: 3 { 09 07 FD 0E 00 00 03 }
0x4EECA: 			End  { 29 02 }
0x4EECC: 			GrayOutIf  { 19 82 }
0x4EECE: 				EqIdVal QuestionId: 0xA01, Value: 0x0 { 12 06 01 0A 00 00 }
0x4EED4: 				OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.L1SS cannot be enabled when CLKREQMSG is disabled", QuestionFlags: 0x10, QuestionId: 0x279A, VarStoreId: 0x4, VarOffset: 0x37D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 FE 0E 01 0F 9A 27 04 00 7D 03 10 10 00 02 00 }
0x4EEE5: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EEEC: 					OneOfOption Option: "L1.1" Value: 1 { 09 07 02 0F 00 00 01 }
0x4EEF3: 					OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 03 0F 30 00 02 }
0x4EEFA: 				End  { 29 02 }
0x4EEFC: 			End  { 29 02 }
0x4EEFE: 			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x9EF, VarStoreId: 0x4, VarOffset: 0x36D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 F3 0E F5 0E EF 09 04 00 6D 03 10 10 01 04 00 }
0x4EF0F: 				OneOfOption Option: "Hardware" Value: 1, Default { 09 07 F6 0E 10 00 01 }
0x4EF16: 				OneOfOption Option: "Static Coeff." Value: 4 { 09 07 F7 0E 00 00 04 }
0x4EF1D: 			End  { 29 02 }
0x4EF1F: 			OneOf Prompt: "Gen4 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x9F0, VarStoreId: 0x4, VarOffset: 0x371, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 F4 0E F5 0E F0 09 04 00 71 03 10 10 01 04 00 }
0x4EF30: 				OneOfOption Option: "Hardware" Value: 1, Default { 09 07 F6 0E 10 00 01 }
0x4EF37: 				OneOfOption Option: "Static Coeff." Value: 4 { 09 07 F7 0E 00 00 04 }
0x4EF3E: 			End  { 29 02 }
0x4EF40: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x9F1, VarStoreId: 0x4, VarOffset: 0x33D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 0E A7 0E F1 09 04 00 3D 03 10 10 00 01 00 }
0x4EF51: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EF58: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EF5F: 			End  { 29 02 }
0x4EF61: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x279B, VarStoreId: 0x4, VarOffset: 0x399, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 0F 17 0F 9B 27 04 00 99 03 10 10 00 01 00 }
0x4EF72: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4EF79: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4EF80: 			End  { 29 02 }
0x4EF82: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0x9F2, VarStoreId: 0x4, VarOffset: 0x361, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 0E CB 0E F2 09 04 00 61 03 10 10 00 01 00 }
0x4EF93: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4EF9A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4EFA1: 			End  { 29 02 }
0x4EFA3: 			OneOf Prompt: "FOM Scoreboard Control Policy", Help: "Select the FOM Scoreboard Control Policy, when set to Auto, speed is based on TLS", QuestionFlags: 0x10, QuestionId: 0x9F3, VarStoreId: 0x4, VarOffset: 0x3DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 DA 0E DD 0E F3 09 04 00 DD 03 10 10 00 04 00 }
0x4EFB4: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x4EFBB: 				OneOfOption Option: "Gen3" Value: 1 { 09 07 D6 0E 00 00 01 }
0x4EFC2: 				OneOfOption Option: "Gen4" Value: 2 { 09 07 D7 0E 00 00 02 }
0x4EFC9: 				OneOfOption Option: "Gen3/Gen4" Value: 3 { 09 07 D8 0E 00 00 03 }
0x4EFD0: 				OneOfOption Option: "Gen5" Value: 4 { 09 07 D9 0E 00 00 04 }
0x4EFD7: 			End  { 29 02 }
0x4EFD9: 			OneOf Prompt: "Multi-VC", Help: "Enable/Disable Multi Virtual Channel", QuestionFlags: 0x10, QuestionId: 0x279C, VarStoreId: 0x4, VarOffset: 0x3A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CC 0E CF 0E 9C 27 04 00 A5 03 10 10 00 01 00 }
0x4EFEA: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4EFEF: 					Value  { 5A 82 }
0x4EFF1: 						Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4EFFB: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F005: 							Equal  { 2F 02 }
0x4F007: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F011: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F01B: 							Conditional  { 50 02 }
0x4F01D: 						End  { 29 02 }
0x4F01F: 					End  { 29 02 }
0x4F021: 				End  { 29 02 }
0x4F023: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F02A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F031: 			End  { 29 02 }
0x4F033: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0x9F4, VarStoreId: 0x4, VarOffset: 0x365, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 0E E1 0E F4 09 04 00 65 03 10 10 00 01 00 }
0x4F044: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F04B: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F052: 			End  { 29 02 }
0x4F054: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9F5, VarStoreId: 0x4, VarOffset: 0x345, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 0E AF 0E F5 09 04 00 45 03 10 10 00 01 00 }
0x4F065: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F06B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F072: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F079: 			End  { 29 02 }
0x4F07B: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9F6, VarStoreId: 0x4, VarOffset: 0x349, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 0E B3 0E F6 09 04 00 49 03 10 10 00 01 00 }
0x4F08C: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F092: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F099: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F0A0: 			End  { 29 02 }
0x4F0A2: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9F7, VarStoreId: 0x4, VarOffset: 0x34D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 0E B7 0E F7 09 04 00 4D 03 10 10 00 01 00 }
0x4F0B3: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F0B9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F0C0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F0C7: 			End  { 29 02 }
0x4F0C9: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9F8, VarStoreId: 0x4, VarOffset: 0x351, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 0E BB 0E F8 09 04 00 51 03 10 10 00 01 00 }
0x4F0DA: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F0E0: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F0E7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F0EE: 			End  { 29 02 }
0x4F0F0: 			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9F9, VarStoreId: 0x6, VarOffset: 0x1A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 13 F4 13 F9 09 06 00 A7 01 10 10 00 01 00 }
0x4F101: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F108: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F10F: 			End  { 29 02 }
0x4F111: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9FA, VarStoreId: 0x4, VarOffset: 0x355, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 0E BF 0E FA 09 04 00 55 03 10 10 00 01 00 }
0x4F122: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F129: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F130: 			End  { 29 02 }
0x4F132: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9FB, VarStoreId: 0x4, VarOffset: 0x359, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 0E C3 0E FB 09 04 00 59 03 10 10 00 01 00 }
0x4F143: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F14A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F151: 			End  { 29 02 }
0x4F153: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9FC, VarStoreId: 0x4, VarOffset: 0x35D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 0E C7 0E FC 09 04 00 5D 03 10 10 00 01 00 }
0x4F164: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F16B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F172: 			End  { 29 02 }
0x4F174: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9FD, VarStoreId: 0x4, VarOffset: 0x335, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9C 0E 9F 0E FD 09 04 00 35 03 10 10 00 01 00 }
0x4F185: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F18C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F193: 			End  { 29 02 }
0x4F195: 			SuppressIf  { 0A 82 }
0x4F197: 				EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x4F19D: 				SuppressIf  { 0A 82 }
0x4F19F: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F1A9: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F1B3: 						Equal  { 2F 02 }
0x4F1B5: 					End  { 29 02 }
0x4F1B7: 					GrayOutIf  { 19 82 }
0x4F1B9: 						EqIdVal QuestionId: 0x9ED, Value: 0x0 { 12 06 ED 09 00 00 }
0x4F1BF: 						OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9FE, VarStoreId: 0x4, VarOffset: 0x32D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 98 0E 9B 0E FE 09 04 00 2D 03 10 10 00 01 00 }
0x4F1D0: 							OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F1D7: 							OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F1DE: 						End  { 29 02 }
0x4F1E0: 					End  { 29 02 }
0x4F1E2: 				End  { 29 02 }
0x4F1E4: 			End  { 29 02 }
0x4F1E6: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9FF, VarStoreId: 0x4, VarOffset: 0x341, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 0E AB 0E FF 09 04 00 41 03 10 10 00 01 00 }
0x4F1F7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F1FE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F205: 			End  { 29 02 }
0x4F207: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xA00, VarStoreId: 0x4, VarOffset: 0x369, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 E8 0E EB 0E 00 0A 04 00 69 03 10 10 00 05 00 }
0x4F218: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x4F21F: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x4F226: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x4F22D: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x4F234: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x4F23B: 				SuppressIf  { 0A 82 }
0x4F23D: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F247: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F251: 						Equal  { 2F 02 }
0x4F253: 					End  { 29 02 }
0x4F255: 					OneOfOption Option: "Gen5" Value: 5 { 09 07 D9 0E 00 00 05 }
0x4F25C: 				End  { 29 02 }
0x4F25E: 			End  { 29 02 }
0x4F260: 			OneOf Prompt: "Enable ClockReq Messaging", Help: "Enable or Disable ClockReq Messaging", QuestionFlags: 0x10, QuestionId: 0xA01, VarStoreId: 0x4, VarOffset: 0x328, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 0E 93 0E 01 0A 04 00 28 03 10 10 00 01 00 }
0x4F271: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F278: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F27F: 			End  { 29 02 }
0x4F281: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA02, VarStoreId: 0x4, VarOffset: 0x339, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 0E A3 0E 02 0A 04 00 39 03 10 10 00 01 00 }
0x4F292: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F299: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F2A0: 			End  { 29 02 }
0x4F2A2: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xA03, VarStoreId: 0x4, VarOffset: 0x39D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 18 0F 1B 0F 03 0A 04 00 9D 03 00 11 00 00 FF FF 01 00 }
0x4F2B6: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x4F2BD: 			End  { 29 02 }
0x4F2BF: 			OneOf Prompt: "P2P Support", Help: "Program P2P Support Registers according to setup option", QuestionFlags: 0x10, QuestionId: 0xA04, VarStoreId: 0x4, VarOffset: 0x3E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 0E D3 0E 04 0A 04 00 E2 03 10 10 00 01 00 }
0x4F2D0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F2D7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F2DE: 			End  { 29 02 }
0x4F2E0: 			SuppressIf  { 0A 82 }
0x4F2E2: 				Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F2EC: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F2F6: 					Equal  { 2F 02 }
0x4F2F8: 					EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x4F2FE: 					And  { 15 02 }
0x4F300: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F30A: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F314: 					Equal  { 2F 02 }
0x4F316: 					EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x4F31C: 					And  { 15 02 }
0x4F31E: 					Or  { 16 02 }
0x4F320: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F32A: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F334: 					Equal  { 2F 02 }
0x4F336: 					EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 06 42 11 01 00 }
0x4F33C: 					And  { 15 02 }
0x4F33E: 					Or  { 16 02 }
0x4F340: 					Not  { 17 02 }
0x4F342: 				End  { 29 02 }
0x4F344: 				OneOf Prompt: "CPU PCIE Func0 Link Disable", Help: "CPU PCIE Func0 Link Disable while Device attached into Port having Func0 and FuncN", QuestionFlags: 0x10, QuestionId: 0xA05, VarStoreId: 0x4, VarOffset: 0x423, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D4 0E D5 0E 05 0A 04 00 23 04 10 10 00 01 00 }
0x4F355: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F35C: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F363: 				End  { 29 02 }
0x4F365: 			End  { 29 02 }
0x4F367: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4F36E: 			End  { 29 02 }
0x4F370: 			Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 04 0F 00 00 00 }
0x4F377: 			End  { 29 02 }
0x4F379: 			OneOf Prompt: "LTR", Help: "SA PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xA06, VarStoreId: 0x4, VarOffset: 0x3AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 05 0F 08 0F 06 0A 04 00 AD 03 10 10 00 01 00 }
0x4F38A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F391: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F398: 			End  { 29 02 }
0x4F39A: 			SuppressIf  { 0A 82 }
0x4F39C: 				EqIdVal QuestionId: 0xA06, Value: 0x0 { 12 06 06 0A 00 00 }
0x4F3A2: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xA07, VarStoreId: 0x4, VarOffset: 0x3B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 1C 0F 31 0F 07 0A 04 00 B5 03 10 10 00 02 00 }
0x4F3B3: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F3BA: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x4F3C1: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x4F3C8: 				End  { 29 02 }
0x4F3CA: 				SuppressIf  { 0A 82 }
0x4F3CC: 					EqIdVal QuestionId: 0xA07, Value: 0x1 { 12 86 07 0A 01 00 }
0x4F3D2: 						Not  { 17 02 }
0x4F3D4: 					End  { 29 02 }
0x4F3D6: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA08, VarStoreId: 0x4, VarOffset: 0x3BD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 1E 0F 34 0F 08 0A 04 00 BD 03 10 11 00 00 FF 03 01 00 }
0x4F3EA: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x4F3F1: 					End  { 29 02 }
0x4F3F3: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA09, VarStoreId: 0x4, VarOffset: 0x3B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 1F 0F 33 0F 09 0A 04 00 B9 03 10 10 00 05 00 }
0x4F404: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x4F40B: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4F412: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x4F419: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x4F420: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x4F427: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x4F42E: 					End  { 29 02 }
0x4F430: 				End  { 29 02 }
0x4F432: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xA0A, VarStoreId: 0x4, VarOffset: 0x3C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 1D 0F 32 0F 0A 0A 04 00 C5 03 10 10 00 02 00 }
0x4F443: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F44A: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x4F451: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x4F458: 				End  { 29 02 }
0x4F45A: 				SuppressIf  { 0A 82 }
0x4F45C: 					EqIdVal QuestionId: 0xA0A, Value: 0x1 { 12 86 0A 0A 01 00 }
0x4F462: 						Not  { 17 02 }
0x4F464: 					End  { 29 02 }
0x4F466: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xA0B, VarStoreId: 0x4, VarOffset: 0x3CD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 20 0F 35 0F 0B 0A 04 00 CD 03 10 11 00 00 FF 03 01 00 }
0x4F47A: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x4F481: 					End  { 29 02 }
0x4F483: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA0C, VarStoreId: 0x4, VarOffset: 0x3C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 21 0F 36 0F 0C 0A 04 00 C9 03 10 10 00 05 00 }
0x4F494: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x4F49B: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4F4A2: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x4F4A9: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x4F4B0: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x4F4B7: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x4F4BE: 					End  { 29 02 }
0x4F4C0: 				End  { 29 02 }
0x4F4C2: 				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for SA PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0xA0D, VarStoreId: 0x4, VarOffset: 0x3D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 0F 37 0F 0D 0A 04 00 D5 03 10 10 00 01 00 }
0x4F4D3: 					OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x4F4DA: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F4E1: 				End  { 29 02 }
0x4F4E3: 			End  { 29 02 }
0x4F4E5: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4F4EC: 			End  { 29 02 }
0x4F4EE: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xA0E, VarStoreId: 0x4, VarOffset: 0x3B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 0F 0C 0F 0E 0A 04 00 B1 03 10 10 00 01 00 }
0x4F4FF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F506: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F50D: 			End  { 29 02 }
0x4F50F: 		End  { 29 02 }
0x4F511: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4F518: 		End  { 29 02 }
0x4F51A: 		Subtitle Prompt: "CPU PCIe Gen3 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0D 0F 00 00 00 }
0x4F521: 		End  { 29 02 }
0x4F523: 		Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA0F, VarStoreId: 0x4, VarOffset: 0x381, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 10 0F 11 0F 0F 0A 04 00 81 03 00 10 00 0A 01 }
0x4F534: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4F539: 				Value  { 5A 82 }
0x4F53B: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F545: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F54F: 						Equal  { 2F 02 }
0x4F551: 						Uint64 Value: 0x5 { 45 0A 05 00 00 00 00 00 00 00 }
0x4F55B: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x4F565: 						Conditional  { 50 02 }
0x4F567: 					End  { 29 02 }
0x4F569: 				End  { 29 02 }
0x4F56B: 			End  { 29 02 }
0x4F56D: 		End  { 29 02 }
0x4F56F: 		Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA10, VarStoreId: 0x4, VarOffset: 0x385, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 12 0F 13 0F 10 0A 04 00 85 03 00 10 00 0A 01 }
0x4F580: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4F586: 		End  { 29 02 }
0x4F588: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4F58F: 		End  { 29 02 }
0x4F591: 		Subtitle Prompt: "CPU PCIe Gen4 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0E 0F 00 00 00 }
0x4F598: 		End  { 29 02 }
0x4F59A: 		Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA11, VarStoreId: 0x4, VarOffset: 0x389, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F1 10 11 0F 11 0A 04 00 89 03 00 10 00 0A 01 }
0x4F5AB: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4F5B0: 				Value  { 5A 82 }
0x4F5B2: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F5BC: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F5C6: 						Equal  { 2F 02 }
0x4F5C8: 						Uint64 Value: 0x8 { 45 0A 08 00 00 00 00 00 00 00 }
0x4F5D2: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x4F5DC: 						Conditional  { 50 02 }
0x4F5DE: 					End  { 29 02 }
0x4F5E0: 				End  { 29 02 }
0x4F5E2: 			End  { 29 02 }
0x4F5E4: 		End  { 29 02 }
0x4F5E6: 		Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA12, VarStoreId: 0x4, VarOffset: 0x38D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F9 10 13 0F 12 0A 04 00 8D 03 00 10 00 0A 01 }
0x4F5F7: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4F5FC: 				Value  { 5A 82 }
0x4F5FE: 					Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F608: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F612: 						Equal  { 2F 02 }
0x4F614: 						Uint64 Value: 0x9 { 45 0A 09 00 00 00 00 00 00 00 }
0x4F61E: 						Uint64 Value: 0x5 { 45 0A 05 00 00 00 00 00 00 00 }
0x4F628: 						Conditional  { 50 02 }
0x4F62A: 					End  { 29 02 }
0x4F62C: 				End  { 29 02 }
0x4F62E: 			End  { 29 02 }
0x4F630: 		End  { 29 02 }
0x4F632: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4F639: 		End  { 29 02 }
0x4F63B: 		SuppressIf  { 0A 82 }
0x4F63D: 			Uint64 Value: 0x0 { 45 8A 00 00 00 00 00 00 00 00 }
0x4F647: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F651: 				Equal  { 2F 02 }
0x4F653: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F65D: 				Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x4F667: 				Equal  { 2F 02 }
0x4F669: 				EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 06 42 11 01 00 }
0x4F66F: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x4F675: 				Or  { 16 02 }
0x4F677: 				And  { 15 02 }
0x4F679: 				Or  { 16 02 }
0x4F67B: 			End  { 29 02 }
0x4F67D: 			Subtitle Prompt: "CPU PCIe Gen5 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0F 0F 00 00 00 }
0x4F684: 			End  { 29 02 }
0x4F686: 			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA13, VarStoreId: 0x4, VarOffset: 0x391, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F2 10 11 0F 13 0A 04 00 91 03 00 10 00 0A 01 }
0x4F697: 				Default DefaultId: 0x0 Value: 5 { 5B 06 00 00 00 05 }
0x4F69D: 			End  { 29 02 }
0x4F69F: 			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA14, VarStoreId: 0x4, VarOffset: 0x395, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 FA 10 13 0F 14 0A 04 00 95 03 00 10 00 0A 01 }
0x4F6B0: 				Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4F6B6: 			End  { 29 02 }
0x4F6B8: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4F6BF: 			End  { 29 02 }
0x4F6C1: 		End  { 29 02 }
0x4F6C3: 	End  { 29 02 }
0x4F6C5: 	Form FormId: 0x27CA, Title: "PCI Express Root Port 2" { 01 86 CA 27 7F 0E }
0x4F6CB: 		OneOf Prompt: "PCI Express Root Port 2", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xA15, VarStoreId: 0x4, VarOffset: 0x279, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 0F 81 0E 15 0A 04 00 79 02 10 10 00 01 00 }
0x4F6DC: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F6E3: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F6EA: 		End  { 29 02 }
0x4F6EC: 		SuppressIf  { 0A 82 }
0x4F6EE: 			EqIdVal QuestionId: 0xA15, Value: 0x0 { 12 06 15 0A 00 00 }
0x4F6F4: 			GrayOutIf  { 19 82 }
0x4F6F6: 				EqIdVal QuestionId: 0xA27, Value: 0x1 { 12 06 27 0A 01 00 }
0x4F6FC: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xA16, VarStoreId: 0x4, VarOffset: 0x332, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 0E E5 0E 16 0A 04 00 32 03 10 10 00 01 00 }
0x4F70D: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x4F714: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x4F71B: 				End  { 29 02 }
0x4F71D: 			End  { 29 02 }
0x4F71F: 			OneOf Prompt: "PCI Express Clock Gating", Help: "PCI Express Clock Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0x279D, VarStoreId: 0x4, VarOffset: 0x2A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 0E 89 0E 9D 27 04 00 A6 02 10 10 00 01 00 }
0x4F730: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F737: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F73E: 			End  { 29 02 }
0x4F740: 			OneOf Prompt: "PCI Express Power Gating", Help: "PCI Express Power Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0xA17, VarStoreId: 0x4, VarOffset: 0x2AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 10 8B 0E 17 0A 04 00 AA 02 10 10 00 01 00 }
0x4F751: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F758: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F75F: 			End  { 29 02 }
0x4F761: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x279E, VarStoreId: 0x4, VarOffset: 0x37A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 F9 0E F5 0D 9E 27 04 00 7A 03 10 10 00 03 00 }
0x4F772: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F779: 				OneOfOption Option: "L0s" Value: 1 { 09 07 FB 0E 00 00 01 }
0x4F780: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x4F787: 				OneOfOption Option: "L0sL1" Value: 3 { 09 07 FD 0E 00 00 03 }
0x4F78E: 			End  { 29 02 }
0x4F790: 			GrayOutIf  { 19 82 }
0x4F792: 				EqIdVal QuestionId: 0xA2A, Value: 0x0 { 12 06 2A 0A 00 00 }
0x4F798: 				OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.L1SS cannot be enabled when CLKREQMSG is disabled", QuestionFlags: 0x10, QuestionId: 0x279F, VarStoreId: 0x4, VarOffset: 0x37E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 FF 0E 01 0F 9F 27 04 00 7E 03 10 10 00 02 00 }
0x4F7A9: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F7B0: 					OneOfOption Option: "L1.1" Value: 1 { 09 07 02 0F 00 00 01 }
0x4F7B7: 					OneOfOption Option: "L1.1 & L1.2" Value: 2 { 09 07 03 0F 00 00 02 }
0x4F7BE: 				End  { 29 02 }
0x4F7C0: 			End  { 29 02 }
0x4F7C2: 			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0xA18, VarStoreId: 0x4, VarOffset: 0x36E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 ED 10 F5 0E 18 0A 04 00 6E 03 10 10 01 04 00 }
0x4F7D3: 				OneOfOption Option: "Hardware" Value: 1, Default { 09 07 F6 0E 10 00 01 }
0x4F7DA: 				OneOfOption Option: "Static Coeff." Value: 4 { 09 07 F7 0E 00 00 04 }
0x4F7E1: 			End  { 29 02 }
0x4F7E3: 			OneOf Prompt: "Gen4 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0xA19, VarStoreId: 0x4, VarOffset: 0x372, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 EF 10 F5 0E 19 0A 04 00 72 03 10 10 01 04 00 }
0x4F7F4: 				OneOfOption Option: "Hardware" Value: 1, Default { 09 07 F6 0E 10 00 01 }
0x4F7FB: 				OneOfOption Option: "Static Coeff." Value: 4 { 09 07 F7 0E 00 00 04 }
0x4F802: 			End  { 29 02 }
0x4F804: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xA1A, VarStoreId: 0x4, VarOffset: 0x33E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A5 0E A7 0E 1A 0A 04 00 3E 03 10 10 00 01 00 }
0x4F815: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F81C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F823: 			End  { 29 02 }
0x4F825: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27A0, VarStoreId: 0x4, VarOffset: 0x39A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 15 0F 17 0F A0 27 04 00 9A 03 10 10 00 01 00 }
0x4F836: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F83D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F844: 			End  { 29 02 }
0x4F846: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xA1B, VarStoreId: 0x4, VarOffset: 0x362, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C9 0E CB 0E 1B 0A 04 00 62 03 10 10 00 01 00 }
0x4F857: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F85E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F865: 			End  { 29 02 }
0x4F867: 			OneOf Prompt: "FOM Scoreboard Control Policy", Help: "Select the FOM Scoreboard Control Policy, when set to Auto, speed is based on TLS", QuestionFlags: 0x10, QuestionId: 0xA1C, VarStoreId: 0x4, VarOffset: 0x3DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 DB 0E DD 0E 1C 0A 04 00 DE 03 10 10 00 04 00 }
0x4F878: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x4F87F: 				OneOfOption Option: "Gen3" Value: 1 { 09 07 D6 0E 00 00 01 }
0x4F886: 				OneOfOption Option: "Gen4" Value: 2 { 09 07 D7 0E 00 00 02 }
0x4F88D: 				OneOfOption Option: "Gen3/Gen4" Value: 3 { 09 07 D8 0E 00 00 03 }
0x4F894: 				OneOfOption Option: "Gen5" Value: 4 { 09 07 D9 0E 00 00 04 }
0x4F89B: 			End  { 29 02 }
0x4F89D: 			OneOf Prompt: "Multi-VC", Help: "Enable/Disable Multi Virtual Channel", QuestionFlags: 0x10, QuestionId: 0x27A1, VarStoreId: 0x4, VarOffset: 0x3A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CD 0E CF 0E A1 27 04 00 A6 03 10 10 00 01 00 }
0x4F8AE: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4F8B3: 					Value  { 5A 82 }
0x4F8B5: 						Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4F8BF: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F8C9: 							Equal  { 2F 02 }
0x4F8CB: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4F8D5: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4F8DF: 							Conditional  { 50 02 }
0x4F8E1: 						End  { 29 02 }
0x4F8E3: 					End  { 29 02 }
0x4F8E5: 				End  { 29 02 }
0x4F8E7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F8EE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F8F5: 			End  { 29 02 }
0x4F8F7: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xA1D, VarStoreId: 0x4, VarOffset: 0x366, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 0E E1 0E 1D 0A 04 00 66 03 10 10 00 01 00 }
0x4F908: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F90F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4F916: 			End  { 29 02 }
0x4F918: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA1E, VarStoreId: 0x4, VarOffset: 0x346, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 0E AF 0E 1E 0A 04 00 46 03 10 10 00 01 00 }
0x4F929: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F92F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F936: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F93D: 			End  { 29 02 }
0x4F93F: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA1F, VarStoreId: 0x4, VarOffset: 0x34A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 0E B3 0E 1F 0A 04 00 4A 03 10 10 00 01 00 }
0x4F950: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F956: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F95D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F964: 			End  { 29 02 }
0x4F966: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA20, VarStoreId: 0x4, VarOffset: 0x34E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 0E B7 0E 20 0A 04 00 4E 03 10 10 00 01 00 }
0x4F977: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F97D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F984: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F98B: 			End  { 29 02 }
0x4F98D: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA21, VarStoreId: 0x4, VarOffset: 0x352, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 0E BB 0E 21 0A 04 00 52 03 10 10 00 01 00 }
0x4F99E: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x4F9A4: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4F9AB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F9B2: 			End  { 29 02 }
0x4F9B4: 			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA22, VarStoreId: 0x6, VarOffset: 0x1A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F2 13 F4 13 22 0A 06 00 A8 01 10 10 00 01 00 }
0x4F9C5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F9CC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F9D3: 			End  { 29 02 }
0x4F9D5: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA23, VarStoreId: 0x4, VarOffset: 0x356, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 0E BF 0E 23 0A 04 00 56 03 10 10 00 01 00 }
0x4F9E6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4F9ED: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4F9F4: 			End  { 29 02 }
0x4F9F6: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA24, VarStoreId: 0x4, VarOffset: 0x35A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 0E C3 0E 24 0A 04 00 5A 03 10 10 00 01 00 }
0x4FA07: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FA0E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FA15: 			End  { 29 02 }
0x4FA17: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA25, VarStoreId: 0x4, VarOffset: 0x35E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 0E C7 0E 25 0A 04 00 5E 03 10 10 00 01 00 }
0x4FA28: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FA2F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FA36: 			End  { 29 02 }
0x4FA38: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA26, VarStoreId: 0x4, VarOffset: 0x336, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 0E 9F 0E 26 0A 04 00 36 03 10 10 00 01 00 }
0x4FA49: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FA50: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4FA57: 			End  { 29 02 }
0x4FA59: 			SuppressIf  { 0A 82 }
0x4FA5B: 				EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x4FA61: 				SuppressIf  { 0A 82 }
0x4FA63: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FA6D: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FA77: 						Equal  { 2F 02 }
0x4FA79: 					End  { 29 02 }
0x4FA7B: 					GrayOutIf  { 19 82 }
0x4FA7D: 						EqIdVal QuestionId: 0xA16, Value: 0x0 { 12 06 16 0A 00 00 }
0x4FA83: 						OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA27, VarStoreId: 0x4, VarOffset: 0x32E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 0E 9B 0E 27 0A 04 00 2E 03 10 10 00 01 00 }
0x4FA94: 							OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FA9B: 							OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FAA2: 						End  { 29 02 }
0x4FAA4: 					End  { 29 02 }
0x4FAA6: 				End  { 29 02 }
0x4FAA8: 			End  { 29 02 }
0x4FAAA: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA28, VarStoreId: 0x4, VarOffset: 0x342, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 0E AB 0E 28 0A 04 00 42 03 10 10 00 01 00 }
0x4FABB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FAC2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4FAC9: 			End  { 29 02 }
0x4FACB: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xA29, VarStoreId: 0x4, VarOffset: 0x36A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 E9 0E EB 0E 29 0A 04 00 6A 03 10 10 00 05 00 }
0x4FADC: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x4FAE3: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x4FAEA: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x4FAF1: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x4FAF8: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x4FAFF: 				SuppressIf  { 0A 82 }
0x4FB01: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FB0B: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4FB15: 						Equal  { 2F 02 }
0x4FB17: 					End  { 29 02 }
0x4FB19: 					OneOfOption Option: "Gen5" Value: 5 { 09 07 D9 0E 00 00 05 }
0x4FB20: 				End  { 29 02 }
0x4FB22: 			End  { 29 02 }
0x4FB24: 			OneOf Prompt: "Enable ClockReq Messaging", Help: "Enable or Disable ClockReq Messaging", QuestionFlags: 0x10, QuestionId: 0xA2A, VarStoreId: 0x4, VarOffset: 0x329, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 0E 93 0E 2A 0A 04 00 29 03 10 10 00 01 00 }
0x4FB35: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4FB3C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FB43: 			End  { 29 02 }
0x4FB45: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA2B, VarStoreId: 0x4, VarOffset: 0x33A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 0E A3 0E 2B 0A 04 00 3A 03 10 10 00 01 00 }
0x4FB56: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FB5D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FB64: 			End  { 29 02 }
0x4FB66: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xA2C, VarStoreId: 0x4, VarOffset: 0x39F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 19 0F 1B 0F 2C 0A 04 00 9F 03 00 11 00 00 FF FF 01 00 }
0x4FB7A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x4FB81: 			End  { 29 02 }
0x4FB83: 			OneOf Prompt: "P2P Support", Help: "Program P2P Support Registers according to setup option", QuestionFlags: 0x10, QuestionId: 0xA2D, VarStoreId: 0x4, VarOffset: 0x3E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 0E D3 0E 2D 0A 04 00 E3 03 10 10 00 01 00 }
0x4FB94: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FB9B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FBA2: 			End  { 29 02 }
0x4FBA4: 			SuppressIf  { 0A 82 }
0x4FBA6: 				Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FBB0: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FBBA: 					Equal  { 2F 02 }
0x4FBBC: 					EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x4FBC2: 					And  { 15 02 }
0x4FBC4: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FBCE: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FBD8: 					Equal  { 2F 02 }
0x4FBDA: 					EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x4FBE0: 					And  { 15 02 }
0x4FBE2: 					Or  { 16 02 }
0x4FBE4: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FBEE: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4FBF8: 					Equal  { 2F 02 }
0x4FBFA: 					EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 06 42 11 01 00 }
0x4FC00: 					And  { 15 02 }
0x4FC02: 					Or  { 16 02 }
0x4FC04: 					Not  { 17 02 }
0x4FC06: 				End  { 29 02 }
0x4FC08: 				OneOf Prompt: "CPU PCIE Func0 Link Disable", Help: "CPU PCIE Func0 Link Disable while Device attached into Port having Func0 and FuncN", QuestionFlags: 0x10, QuestionId: 0xA2E, VarStoreId: 0x4, VarOffset: 0x424, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 10 D5 0E 2E 0A 04 00 24 04 10 10 00 01 00 }
0x4FC19: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FC20: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FC27: 				End  { 29 02 }
0x4FC29: 			End  { 29 02 }
0x4FC2B: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4FC32: 			End  { 29 02 }
0x4FC34: 			Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 04 0F 00 00 00 }
0x4FC3B: 			End  { 29 02 }
0x4FC3D: 			OneOf Prompt: "LTR", Help: "SA PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xA2F, VarStoreId: 0x4, VarOffset: 0x3AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 06 0F 08 0F 2F 0A 04 00 AE 03 10 10 00 01 00 }
0x4FC4E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FC55: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4FC5C: 			End  { 29 02 }
0x4FC5E: 			SuppressIf  { 0A 82 }
0x4FC60: 				EqIdVal QuestionId: 0xA2F, Value: 0x0 { 12 06 2F 0A 00 00 }
0x4FC66: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xA30, VarStoreId: 0x4, VarOffset: 0x3B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 22 0F 31 0F 30 0A 04 00 B6 03 10 10 00 02 00 }
0x4FC77: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FC7E: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x4FC85: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x4FC8C: 				End  { 29 02 }
0x4FC8E: 				SuppressIf  { 0A 82 }
0x4FC90: 					EqIdVal QuestionId: 0xA30, Value: 0x1 { 12 86 30 0A 01 00 }
0x4FC96: 						Not  { 17 02 }
0x4FC98: 					End  { 29 02 }
0x4FC9A: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA31, VarStoreId: 0x4, VarOffset: 0x3BF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 24 0F 34 0F 31 0A 04 00 BF 03 10 11 00 00 FF 03 01 00 }
0x4FCAE: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x4FCB5: 					End  { 29 02 }
0x4FCB7: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA32, VarStoreId: 0x4, VarOffset: 0x3BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 25 0F 33 0F 32 0A 04 00 BA 03 10 10 00 05 00 }
0x4FCC8: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x4FCCF: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4FCD6: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x4FCDD: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x4FCE4: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x4FCEB: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x4FCF2: 					End  { 29 02 }
0x4FCF4: 				End  { 29 02 }
0x4FCF6: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xA33, VarStoreId: 0x4, VarOffset: 0x3C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 23 0F 32 0F 33 0A 04 00 C6 03 10 10 00 02 00 }
0x4FD07: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FD0E: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x4FD15: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x4FD1C: 				End  { 29 02 }
0x4FD1E: 				SuppressIf  { 0A 82 }
0x4FD20: 					EqIdVal QuestionId: 0xA33, Value: 0x1 { 12 86 33 0A 01 00 }
0x4FD26: 						Not  { 17 02 }
0x4FD28: 					End  { 29 02 }
0x4FD2A: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xA34, VarStoreId: 0x4, VarOffset: 0x3CF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 26 0F 35 0F 34 0A 04 00 CF 03 10 11 00 00 FF 03 01 00 }
0x4FD3E: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x4FD45: 					End  { 29 02 }
0x4FD47: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA35, VarStoreId: 0x4, VarOffset: 0x3CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 27 0F 36 0F 35 0A 04 00 CA 03 10 10 00 05 00 }
0x4FD58: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x4FD5F: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x4FD66: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x4FD6D: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x4FD74: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x4FD7B: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x4FD82: 					End  { 29 02 }
0x4FD84: 				End  { 29 02 }
0x4FD86: 				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for SA PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0xA36, VarStoreId: 0x4, VarOffset: 0x3D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 0F 37 0F 36 0A 04 00 D6 03 10 10 00 01 00 }
0x4FD97: 					OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x4FD9E: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FDA5: 				End  { 29 02 }
0x4FDA7: 			End  { 29 02 }
0x4FDA9: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4FDB0: 			End  { 29 02 }
0x4FDB2: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xA37, VarStoreId: 0x4, VarOffset: 0x3B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 0F 0C 0F 37 0A 04 00 B2 03 10 10 00 01 00 }
0x4FDC3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x4FDCA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x4FDD1: 			End  { 29 02 }
0x4FDD3: 		End  { 29 02 }
0x4FDD5: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4FDDC: 		End  { 29 02 }
0x4FDDE: 		Subtitle Prompt: "CPU PCIe Gen3 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0D 0F 00 00 00 }
0x4FDE5: 		End  { 29 02 }
0x4FDE7: 		Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA38, VarStoreId: 0x4, VarOffset: 0x382, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F3 10 11 0F 38 0A 04 00 82 03 00 10 00 0A 01 }
0x4FDF8: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4FDFD: 				Value  { 5A 82 }
0x4FDFF: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FE09: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FE13: 						Equal  { 2F 02 }
0x4FE15: 						Uint64 Value: 0x5 { 45 0A 05 00 00 00 00 00 00 00 }
0x4FE1F: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x4FE29: 						Conditional  { 50 02 }
0x4FE2B: 					End  { 29 02 }
0x4FE2D: 				End  { 29 02 }
0x4FE2F: 			End  { 29 02 }
0x4FE31: 		End  { 29 02 }
0x4FE33: 		Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA39, VarStoreId: 0x4, VarOffset: 0x386, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 FB 10 13 0F 39 0A 04 00 86 03 00 10 00 0A 01 }
0x4FE44: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4FE4A: 		End  { 29 02 }
0x4FE4C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4FE53: 		End  { 29 02 }
0x4FE55: 		Subtitle Prompt: "CPU PCIe Gen4 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0E 0F 00 00 00 }
0x4FE5C: 		End  { 29 02 }
0x4FE5E: 		Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA3A, VarStoreId: 0x4, VarOffset: 0x38A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F4 10 11 0F 3A 0A 04 00 8A 03 00 10 00 0A 01 }
0x4FE6F: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4FE74: 				Value  { 5A 82 }
0x4FE76: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FE80: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FE8A: 						Equal  { 2F 02 }
0x4FE8C: 						Uint64 Value: 0x8 { 45 0A 08 00 00 00 00 00 00 00 }
0x4FE96: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x4FEA0: 						Conditional  { 50 02 }
0x4FEA2: 					End  { 29 02 }
0x4FEA4: 				End  { 29 02 }
0x4FEA6: 			End  { 29 02 }
0x4FEA8: 		End  { 29 02 }
0x4FEAA: 		Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA3B, VarStoreId: 0x4, VarOffset: 0x38E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 FC 10 13 0F 3B 0A 04 00 8E 03 00 10 00 0A 01 }
0x4FEBB: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x4FEC0: 				Value  { 5A 82 }
0x4FEC2: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FECC: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FED6: 						Equal  { 2F 02 }
0x4FED8: 						Uint64 Value: 0x9 { 45 0A 09 00 00 00 00 00 00 00 }
0x4FEE2: 						Uint64 Value: 0x5 { 45 0A 05 00 00 00 00 00 00 00 }
0x4FEEC: 						Conditional  { 50 02 }
0x4FEEE: 					End  { 29 02 }
0x4FEF0: 				End  { 29 02 }
0x4FEF2: 			End  { 29 02 }
0x4FEF4: 		End  { 29 02 }
0x4FEF6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4FEFD: 		End  { 29 02 }
0x4FEFF: 		SuppressIf  { 0A 82 }
0x4FF01: 			Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x4FF0B: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x4FF15: 				Equal  { 2F 02 }
0x4FF17: 				Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x4FF21: 				Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x4FF2B: 				Equal  { 2F 02 }
0x4FF2D: 				EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 06 42 11 01 00 }
0x4FF33: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x4FF39: 				Or  { 16 02 }
0x4FF3B: 				And  { 15 02 }
0x4FF3D: 				Or  { 16 02 }
0x4FF3F: 			End  { 29 02 }
0x4FF41: 			Subtitle Prompt: "CPU PCIe Gen5 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0F 0F 00 00 00 }
0x4FF48: 			End  { 29 02 }
0x4FF4A: 			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA3C, VarStoreId: 0x4, VarOffset: 0x392, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F5 10 11 0F 3C 0A 04 00 92 03 00 10 00 0A 01 }
0x4FF5B: 				Default DefaultId: 0x0 Value: 5 { 5B 06 00 00 00 05 }
0x4FF61: 			End  { 29 02 }
0x4FF63: 			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA3D, VarStoreId: 0x4, VarOffset: 0x396, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 FD 10 13 0F 3D 0A 04 00 96 03 00 10 00 0A 01 }
0x4FF74: 				Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x4FF7A: 			End  { 29 02 }
0x4FF7C: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x4FF83: 			End  { 29 02 }
0x4FF85: 		End  { 29 02 }
0x4FF87: 	End  { 29 02 }
0x4FF89: 	Form FormId: 0x27CB, Title: "PCI Express Root Port 3" { 01 86 CB 27 80 0E }
0x4FF8F: 		OneOf Prompt: "PCI Express Root Port 3", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xA3E, VarStoreId: 0x4, VarOffset: 0x27A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 0F 81 0E 3E 0A 04 00 7A 02 10 10 00 01 00 }
0x4FFA0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FFA7: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x4FFAE: 		End  { 29 02 }
0x4FFB0: 		SuppressIf  { 0A 82 }
0x4FFB2: 			EqIdVal QuestionId: 0xA3E, Value: 0x0 { 12 06 3E 0A 00 00 }
0x4FFB8: 			GrayOutIf  { 19 82 }
0x4FFBA: 				EqIdVal QuestionId: 0xA50, Value: 0x1 { 12 06 50 0A 01 00 }
0x4FFC0: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xA3F, VarStoreId: 0x4, VarOffset: 0x333, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 0E E5 0E 3F 0A 04 00 33 03 10 10 00 01 00 }
0x4FFD1: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x4FFD8: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x4FFDF: 				End  { 29 02 }
0x4FFE1: 			End  { 29 02 }
0x4FFE3: 			OneOf Prompt: "PCI Express Clock Gating", Help: "PCI Express Clock Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0x27A2, VarStoreId: 0x4, VarOffset: 0x2A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 88 0E 89 0E A2 27 04 00 A7 02 10 10 00 01 00 }
0x4FFF4: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x4FFFB: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50002: 			End  { 29 02 }
0x50004: 			OneOf Prompt: "PCI Express Power Gating", Help: "PCI Express Power Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0xA40, VarStoreId: 0x4, VarOffset: 0x2AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EC 10 8B 0E 40 0A 04 00 AB 02 10 10 00 01 00 }
0x50015: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5001C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50023: 			End  { 29 02 }
0x50025: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27A3, VarStoreId: 0x4, VarOffset: 0x37B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 FA 0E F5 0D A3 27 04 00 7B 03 10 10 00 03 00 }
0x50036: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5003D: 				OneOfOption Option: "L0s" Value: 1 { 09 07 FB 0E 00 00 01 }
0x50044: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5004B: 				OneOfOption Option: "L0sL1" Value: 3 { 09 07 FD 0E 00 00 03 }
0x50052: 			End  { 29 02 }
0x50054: 			GrayOutIf  { 19 82 }
0x50056: 				EqIdVal QuestionId: 0xA53, Value: 0x0 { 12 06 53 0A 00 00 }
0x5005C: 				OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.L1SS cannot be enabled when CLKREQMSG is disabled", QuestionFlags: 0x10, QuestionId: 0x27A4, VarStoreId: 0x4, VarOffset: 0x37F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 00 0F 01 0F A4 27 04 00 7F 03 10 10 00 02 00 }
0x5006D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50074: 					OneOfOption Option: "L1.1" Value: 1 { 09 07 02 0F 00 00 01 }
0x5007B: 					OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 03 0F 30 00 02 }
0x50082: 				End  { 29 02 }
0x50084: 			End  { 29 02 }
0x50086: 			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0xA41, VarStoreId: 0x4, VarOffset: 0x36F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 EE 10 F5 0E 41 0A 04 00 6F 03 10 10 01 04 00 }
0x50097: 				OneOfOption Option: "Hardware" Value: 1, Default { 09 07 F6 0E 10 00 01 }
0x5009E: 				OneOfOption Option: "Static Coeff." Value: 4 { 09 07 F7 0E 00 00 04 }
0x500A5: 			End  { 29 02 }
0x500A7: 			OneOf Prompt: "Gen4 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0xA42, VarStoreId: 0x4, VarOffset: 0x373, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0 { 05 91 F0 10 F5 0E 42 0A 04 00 73 03 10 10 01 04 00 }
0x500B8: 				OneOfOption Option: "Hardware" Value: 1, Default { 09 07 F6 0E 10 00 01 }
0x500BF: 				OneOfOption Option: "Static Coeff." Value: 4 { 09 07 F7 0E 00 00 04 }
0x500C6: 			End  { 29 02 }
0x500C8: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xA43, VarStoreId: 0x4, VarOffset: 0x33F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A6 0E A7 0E 43 0A 04 00 3F 03 10 10 00 01 00 }
0x500D9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x500E0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x500E7: 			End  { 29 02 }
0x500E9: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27A5, VarStoreId: 0x4, VarOffset: 0x39B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 16 0F 17 0F A5 27 04 00 9B 03 10 10 00 01 00 }
0x500FA: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50101: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50108: 			End  { 29 02 }
0x5010A: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xA44, VarStoreId: 0x4, VarOffset: 0x363, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 0E CB 0E 44 0A 04 00 63 03 10 10 00 01 00 }
0x5011B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50122: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50129: 			End  { 29 02 }
0x5012B: 			OneOf Prompt: "FOM Scoreboard Control Policy", Help: "Select the FOM Scoreboard Control Policy, when set to Auto, speed is based on TLS", QuestionFlags: 0x10, QuestionId: 0xA45, VarStoreId: 0x4, VarOffset: 0x3DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 DC 0E DD 0E 45 0A 04 00 DF 03 10 10 00 04 00 }
0x5013C: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x50143: 				OneOfOption Option: "Gen3" Value: 1 { 09 07 D6 0E 00 00 01 }
0x5014A: 				OneOfOption Option: "Gen4" Value: 2 { 09 07 D7 0E 00 00 02 }
0x50151: 				OneOfOption Option: "Gen3/Gen4" Value: 3 { 09 07 D8 0E 00 00 03 }
0x50158: 				OneOfOption Option: "Gen5" Value: 4 { 09 07 D9 0E 00 00 04 }
0x5015F: 			End  { 29 02 }
0x50161: 			OneOf Prompt: "Multi-VC", Help: "Enable/Disable Multi Virtual Channel", QuestionFlags: 0x10, QuestionId: 0x27A6, VarStoreId: 0x4, VarOffset: 0x3A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CE 0E CF 0E A6 27 04 00 A7 03 10 10 00 01 00 }
0x50172: 				Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x50177: 					Value  { 5A 82 }
0x50179: 						Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x50183: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x5018D: 							Equal  { 2F 02 }
0x5018F: 							Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x50199: 							Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x501A3: 							Conditional  { 50 02 }
0x501A5: 						End  { 29 02 }
0x501A7: 					End  { 29 02 }
0x501A9: 				End  { 29 02 }
0x501AB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x501B2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x501B9: 			End  { 29 02 }
0x501BB: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xA46, VarStoreId: 0x4, VarOffset: 0x367, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 0E E1 0E 46 0A 04 00 67 03 10 10 00 01 00 }
0x501CC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x501D3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x501DA: 			End  { 29 02 }
0x501DC: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA47, VarStoreId: 0x4, VarOffset: 0x347, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 0E AF 0E 47 0A 04 00 47 03 10 10 00 01 00 }
0x501ED: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x501F3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x501FA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50201: 			End  { 29 02 }
0x50203: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA48, VarStoreId: 0x4, VarOffset: 0x34B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 0E B3 0E 48 0A 04 00 4B 03 10 10 00 01 00 }
0x50214: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x5021A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50221: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50228: 			End  { 29 02 }
0x5022A: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA49, VarStoreId: 0x4, VarOffset: 0x34F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 0E B7 0E 49 0A 04 00 4F 03 10 10 00 01 00 }
0x5023B: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x50241: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50248: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5024F: 			End  { 29 02 }
0x50251: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA4A, VarStoreId: 0x4, VarOffset: 0x353, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 0E BB 0E 4A 0A 04 00 53 03 10 10 00 01 00 }
0x50262: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x50268: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5026F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50276: 			End  { 29 02 }
0x50278: 			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA4B, VarStoreId: 0x6, VarOffset: 0x1A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F3 13 F4 13 4B 0A 06 00 A9 01 10 10 00 01 00 }
0x50289: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50290: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50297: 			End  { 29 02 }
0x50299: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA4C, VarStoreId: 0x4, VarOffset: 0x357, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 0E BF 0E 4C 0A 04 00 57 03 10 10 00 01 00 }
0x502AA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x502B1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x502B8: 			End  { 29 02 }
0x502BA: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA4D, VarStoreId: 0x4, VarOffset: 0x35B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 0E C3 0E 4D 0A 04 00 5B 03 10 10 00 01 00 }
0x502CB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x502D2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x502D9: 			End  { 29 02 }
0x502DB: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA4E, VarStoreId: 0x4, VarOffset: 0x35F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 0E C7 0E 4E 0A 04 00 5F 03 10 10 00 01 00 }
0x502EC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x502F3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x502FA: 			End  { 29 02 }
0x502FC: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA4F, VarStoreId: 0x4, VarOffset: 0x337, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9E 0E 9F 0E 4F 0A 04 00 37 03 10 10 00 01 00 }
0x5030D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50314: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5031B: 			End  { 29 02 }
0x5031D: 			SuppressIf  { 0A 82 }
0x5031F: 				EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x50325: 				SuppressIf  { 0A 82 }
0x50327: 					Uint64 Value: 0x2 { 45 8A 02 00 00 00 00 00 00 00 }
0x50331: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x5033B: 						Equal  { 2F 02 }
0x5033D: 					End  { 29 02 }
0x5033F: 					GrayOutIf  { 19 82 }
0x50341: 						EqIdVal QuestionId: 0xA3F, Value: 0x0 { 12 06 3F 0A 00 00 }
0x50347: 						OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA50, VarStoreId: 0x4, VarOffset: 0x32F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9A 0E 9B 0E 50 0A 04 00 2F 03 10 10 00 01 00 }
0x50358: 							OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5035F: 							OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50366: 						End  { 29 02 }
0x50368: 					End  { 29 02 }
0x5036A: 				End  { 29 02 }
0x5036C: 			End  { 29 02 }
0x5036E: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA51, VarStoreId: 0x4, VarOffset: 0x343, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 0E AB 0E 51 0A 04 00 43 03 10 10 00 01 00 }
0x5037F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50386: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5038D: 			End  { 29 02 }
0x5038F: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xA52, VarStoreId: 0x4, VarOffset: 0x36B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 EA 0E EB 0E 52 0A 04 00 6B 03 10 10 00 05 00 }
0x503A0: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 06 00 30 00 00 }
0x503A7: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x503AE: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x503B5: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x503BC: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x503C3: 				SuppressIf  { 0A 82 }
0x503C5: 					Uint64 Value: 0x2 { 45 8A 02 00 00 00 00 00 00 00 }
0x503CF: 						Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x503D9: 						Equal  { 2F 02 }
0x503DB: 					End  { 29 02 }
0x503DD: 					OneOfOption Option: "Gen5" Value: 5 { 09 07 D9 0E 00 00 05 }
0x503E4: 				End  { 29 02 }
0x503E6: 			End  { 29 02 }
0x503E8: 			OneOf Prompt: "Enable ClockReq Messaging", Help: "Enable or Disable ClockReq Messaging", QuestionFlags: 0x10, QuestionId: 0xA53, VarStoreId: 0x4, VarOffset: 0x32A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 0E 93 0E 53 0A 04 00 2A 03 10 10 00 01 00 }
0x503F9: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50400: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50407: 			End  { 29 02 }
0x50409: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xA54, VarStoreId: 0x4, VarOffset: 0x33B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 0E A3 0E 54 0A 04 00 3B 03 10 10 00 01 00 }
0x5041A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50421: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50428: 			End  { 29 02 }
0x5042A: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xA55, VarStoreId: 0x4, VarOffset: 0x3A1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 1A 0F 1B 0F 55 0A 04 00 A1 03 00 11 00 00 FF FF 01 00 }
0x5043E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x50445: 			End  { 29 02 }
0x50447: 			OneOf Prompt: "P2P Support", Help: "Program P2P Support Registers according to setup option", QuestionFlags: 0x10, QuestionId: 0xA56, VarStoreId: 0x4, VarOffset: 0x3E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D2 0E D3 0E 56 0A 04 00 E4 03 10 10 00 01 00 }
0x50458: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5045F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50466: 			End  { 29 02 }
0x50468: 			SuppressIf  { 0A 82 }
0x5046A: 				Uint64 Value: 0x2 { 45 8A 02 00 00 00 00 00 00 00 }
0x50474: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x5047E: 					Equal  { 2F 02 }
0x50480: 					EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 06 42 11 02 00 }
0x50486: 					And  { 15 02 }
0x50488: 					Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x50492: 					Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x5049C: 					Equal  { 2F 02 }
0x5049E: 					EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x504A4: 					And  { 15 02 }
0x504A6: 					Or  { 16 02 }
0x504A8: 					Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x504B2: 					Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x504BC: 					Equal  { 2F 02 }
0x504BE: 					EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 06 42 11 01 00 }
0x504C4: 					And  { 15 02 }
0x504C6: 					Or  { 16 02 }
0x504C8: 					Not  { 17 02 }
0x504CA: 				End  { 29 02 }
0x504CC: 				OneOf Prompt: "CPU PCIE Func0 Link Disable", Help: "CPU PCIE Func0 Link Disable while Device attached into Port having Func0 and FuncN", QuestionFlags: 0x10, QuestionId: 0xA57, VarStoreId: 0x4, VarOffset: 0x425, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 10 D5 0E 57 0A 04 00 25 04 10 10 00 01 00 }
0x504DD: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x504E4: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x504EB: 				End  { 29 02 }
0x504ED: 			End  { 29 02 }
0x504EF: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x504F6: 			End  { 29 02 }
0x504F8: 			Subtitle Prompt: "SA PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 04 0F 00 00 00 }
0x504FF: 			End  { 29 02 }
0x50501: 			OneOf Prompt: "LTR", Help: "SA PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xA58, VarStoreId: 0x4, VarOffset: 0x3AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 0F 08 0F 58 0A 04 00 AF 03 10 10 00 01 00 }
0x50512: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50519: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50520: 			End  { 29 02 }
0x50522: 			SuppressIf  { 0A 82 }
0x50524: 				EqIdVal QuestionId: 0xA58, Value: 0x0 { 12 06 58 0A 00 00 }
0x5052A: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xA59, VarStoreId: 0x4, VarOffset: 0x3B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 28 0F 31 0F 59 0A 04 00 B7 03 10 10 00 02 00 }
0x5053B: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50542: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x50549: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x50550: 				End  { 29 02 }
0x50552: 				SuppressIf  { 0A 82 }
0x50554: 					EqIdVal QuestionId: 0xA59, Value: 0x1 { 12 86 59 0A 01 00 }
0x5055A: 						Not  { 17 02 }
0x5055C: 					End  { 29 02 }
0x5055E: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA5A, VarStoreId: 0x4, VarOffset: 0x3C1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 2A 0F 34 0F 5A 0A 04 00 C1 03 10 11 00 00 FF 03 01 00 }
0x50572: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x50579: 					End  { 29 02 }
0x5057B: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA5B, VarStoreId: 0x4, VarOffset: 0x3BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 2B 0F 33 0F 5B 0A 04 00 BB 03 10 10 00 05 00 }
0x5058C: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x50593: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5059A: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x505A1: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x505A8: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x505AF: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x505B6: 					End  { 29 02 }
0x505B8: 				End  { 29 02 }
0x505BA: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for SA PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xA5C, VarStoreId: 0x4, VarOffset: 0x3C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 29 0F 32 0F 5C 0A 04 00 C7 03 10 10 00 02 00 }
0x505CB: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x505D2: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x505D9: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x505E0: 				End  { 29 02 }
0x505E2: 				SuppressIf  { 0A 82 }
0x505E4: 					EqIdVal QuestionId: 0xA5C, Value: 0x1 { 12 86 5C 0A 01 00 }
0x505EA: 						Not  { 17 02 }
0x505EC: 					End  { 29 02 }
0x505EE: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xA5D, VarStoreId: 0x4, VarOffset: 0x3D1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 2C 0F 35 0F 5D 0A 04 00 D1 03 10 11 00 00 FF 03 01 00 }
0x50602: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x50609: 					End  { 29 02 }
0x5060B: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of SA PCIE", QuestionFlags: 0x10, QuestionId: 0xA5E, VarStoreId: 0x4, VarOffset: 0x3CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 2D 0F 36 0F 5E 0A 04 00 CB 03 10 10 00 05 00 }
0x5061C: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x50623: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5062A: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x50631: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x50638: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5063F: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x50646: 					End  { 29 02 }
0x50648: 				End  { 29 02 }
0x5064A: 				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for SA PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0xA5F, VarStoreId: 0x4, VarOffset: 0x3D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 0F 37 0F 5F 0A 04 00 D7 03 10 10 00 01 00 }
0x5065B: 					OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x50662: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50669: 				End  { 29 02 }
0x5066B: 			End  { 29 02 }
0x5066D: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x50674: 			End  { 29 02 }
0x50676: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xA60, VarStoreId: 0x4, VarOffset: 0x3B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 0F 0C 0F 60 0A 04 00 B3 03 10 10 00 01 00 }
0x50687: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5068E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50695: 			End  { 29 02 }
0x50697: 		End  { 29 02 }
0x50699: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x506A0: 		End  { 29 02 }
0x506A2: 		Subtitle Prompt: "CPU PCIe Gen3 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0D 0F 00 00 00 }
0x506A9: 		End  { 29 02 }
0x506AB: 		Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA61, VarStoreId: 0x4, VarOffset: 0x383, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F6 10 11 0F 61 0A 04 00 83 03 00 10 00 0A 01 }
0x506BC: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x506C1: 				Value  { 5A 82 }
0x506C3: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x506CD: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x506D7: 						Equal  { 2F 02 }
0x506D9: 						Uint64 Value: 0x5 { 45 0A 05 00 00 00 00 00 00 00 }
0x506E3: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x506ED: 						Conditional  { 50 02 }
0x506EF: 					End  { 29 02 }
0x506F1: 				End  { 29 02 }
0x506F3: 			End  { 29 02 }
0x506F5: 		End  { 29 02 }
0x506F7: 		Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA62, VarStoreId: 0x4, VarOffset: 0x387, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 FE 10 13 0F 62 0A 04 00 87 03 00 10 00 0A 01 }
0x50708: 			Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x5070E: 		End  { 29 02 }
0x50710: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x50717: 		End  { 29 02 }
0x50719: 		Subtitle Prompt: "CPU PCIe Gen4 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0E 0F 00 00 00 }
0x50720: 		End  { 29 02 }
0x50722: 		Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA63, VarStoreId: 0x4, VarOffset: 0x38B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F7 10 11 0F 63 0A 04 00 8B 03 00 10 00 0A 01 }
0x50733: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x50738: 				Value  { 5A 82 }
0x5073A: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x50744: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x5074E: 						Equal  { 2F 02 }
0x50750: 						Uint64 Value: 0x8 { 45 0A 08 00 00 00 00 00 00 00 }
0x5075A: 						Uint64 Value: 0x7 { 45 0A 07 00 00 00 00 00 00 00 }
0x50764: 						Conditional  { 50 02 }
0x50766: 					End  { 29 02 }
0x50768: 				End  { 29 02 }
0x5076A: 			End  { 29 02 }
0x5076C: 		End  { 29 02 }
0x5076E: 		Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA64, VarStoreId: 0x4, VarOffset: 0x38F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 FF 10 13 0F 64 0A 04 00 8F 03 00 10 00 0A 01 }
0x5077F: 			Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x50784: 				Value  { 5A 82 }
0x50786: 					Uint64 Value: 0x1 { 45 8A 01 00 00 00 00 00 00 00 }
0x50790: 						Uint64 Value: 0x1 { 45 0A 01 00 00 00 00 00 00 00 }
0x5079A: 						Equal  { 2F 02 }
0x5079C: 						Uint64 Value: 0x9 { 45 0A 09 00 00 00 00 00 00 00 }
0x507A6: 						Uint64 Value: 0x5 { 45 0A 05 00 00 00 00 00 00 00 }
0x507B0: 						Conditional  { 50 02 }
0x507B2: 					End  { 29 02 }
0x507B4: 				End  { 29 02 }
0x507B6: 			End  { 29 02 }
0x507B8: 		End  { 29 02 }
0x507BA: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x507C1: 		End  { 29 02 }
0x507C3: 		SuppressIf  { 0A 82 }
0x507C5: 			Uint64 Value: 0x2 { 45 8A 02 00 00 00 00 00 00 00 }
0x507CF: 				Uint64 Value: 0x0 { 45 0A 00 00 00 00 00 00 00 00 }
0x507D9: 				Equal  { 2F 02 }
0x507DB: 				Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x507E5: 				Uint64 Value: 0x2 { 45 0A 02 00 00 00 00 00 00 00 }
0x507EF: 				Equal  { 2F 02 }
0x507F1: 				EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 06 42 11 01 00 }
0x507F7: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x507FD: 				Or  { 16 02 }
0x507FF: 				And  { 15 02 }
0x50801: 				Or  { 16 02 }
0x50803: 			End  { 29 02 }
0x50805: 			Subtitle Prompt: "CPU PCIe Gen5 HWEQ Config", Help: "", Flags: 0x0 { 02 87 0F 0F 00 00 00 }
0x5080C: 			End  { 29 02 }
0x5080E: 			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA65, VarStoreId: 0x4, VarOffset: 0x393, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 F8 10 11 0F 65 0A 04 00 93 03 00 10 00 0A 01 }
0x5081F: 				Default DefaultId: 0x0 Value: 5 { 5B 06 00 00 00 05 }
0x50825: 			End  { 29 02 }
0x50827: 			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0xA66, VarStoreId: 0x4, VarOffset: 0x397, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 00 11 13 0F 66 0A 04 00 97 03 00 10 00 0A 01 }
0x50838: 				Default DefaultId: 0x0 Value: 7 { 5B 06 00 00 00 07 }
0x5083E: 			End  { 29 02 }
0x50840: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x50847: 			End  { 29 02 }
0x50849: 		End  { 29 02 }
0x5084B: 	End  { 29 02 }
0x5084D: 	Form FormId: 0x27CD, Title: "PCIE Configuration" { 01 86 CD 27 21 11 }
0x50853: 		Subtitle Prompt: "PCIE Configuration", Help: "", Flags: 0x0 { 02 87 21 11 00 00 00 }
0x5085A: 		End  { 29 02 }
0x5085C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x50863: 		End  { 29 02 }
0x50865: 		Ref Prompt: "IMR Configuration", Help: "IMR Configuration", QuestionFlags: 0x0, QuestionId: 0xA67, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27CE { 0F 0F 22 11 22 11 67 0A 00 00 FF FF 00 CE 27 }
0x50874: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5087B: 		End  { 29 02 }
0x5087D: 	End  { 29 02 }
0x5087F: 	Form FormId: 0x27CE, Title: "IMR Configuration" { 01 86 CE 27 22 11 }
0x50885: 		OneOf Prompt: "PCIe IMR", Help: "Enable/Disable PCIe IMR", QuestionFlags: 0x10, QuestionId: 0xA68, VarStoreId: 0xD, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 23 11 24 11 68 0A 0D 00 02 00 10 10 00 01 00 }
0x50896: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5089D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x508A4: 		End  { 29 02 }
0x508A6: 		SuppressIf  { 0A 82 }
0x508A8: 			EqIdVal QuestionId: 0xA68, Value: 0x0 { 12 06 68 0A 00 00 }
0x508AE: 			Numeric Prompt: "PCIe IMR Size", Help: "PCIe Reserved Memory Size to be requested in MB.
Maximum value of 1024 MB", QuestionFlags: 0x10, QuestionId: 0xA69, VarStoreId: 0xD, VarOffset: 0x3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x400, Step: 0x1 { 07 94 25 11 26 11 69 0A 0D 00 03 00 10 11 00 00 00 04 01 00 }
0x508C2: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x508C9: 			End  { 29 02 }
0x508CB: 			OneOf Prompt: "PCIe RP Location for IMR", Help: "Select SA or PCH roor port associated with IMR", QuestionFlags: 0x10, QuestionId: 0xA6A, VarStoreId: 0xD, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0 { 05 91 27 11 28 11 6A 0A 0D 00 05 00 10 10 01 02 00 }
0x508DC: 				OneOfOption Option: "PCH PCIE" Value: 1 { 09 07 1F 11 00 00 01 }
0x508E3: 				OneOfOption Option: "SA PCIE" Value: 2 { 09 07 20 11 00 00 02 }
0x508EA: 			End  { 29 02 }
0x508EC: 			Numeric Prompt: "RP index for IMR", Help: "Selects which root port will be associated with IMR", QuestionFlags: 0x14, QuestionId: 0x27CC, VarStoreId: 0xD, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1B, Step: 0x1 { 07 91 29 11 2A 11 CC 27 0D 00 06 00 14 10 00 1B 01 }
0x508FD: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x50903: 			End  { 29 02 }
0x50905: 		End  { 29 02 }
0x50907: 	End  { 29 02 }
0x50909: 	Form FormId: 0x282B, Title: "PCH-IO Configuration" { 01 86 2B 28 2B 11 }
0x5090F: 		Subtitle Prompt: "PCH-IO Configuration", Help: "", Flags: 0x0 { 02 87 2B 11 00 00 00 }
0x50916: 		End  { 29 02 }
0x50918: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5091F: 		End  { 29 02 }
0x50921: 		Ref Prompt: "PCI Express Configuration", Help: "PCI Express Configuration settings", QuestionFlags: 0x0, QuestionId: 0xA6B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x282C { 0F 0F 7C 0E 7D 0E 6B 0A 00 00 FF FF 00 2C 28 }
0x50930: 		Ref Prompt: "SATA Configuration", Help: "SATA Device Options Settings", QuestionFlags: 0x0, QuestionId: 0xA6C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x282E { 0F 0F 99 16 9A 16 6C 0A 00 00 FF FF 00 2E 28 }
0x5093F: 		Ref Prompt: "USB Configuration", Help: "USB Configuration settings", QuestionFlags: 0x0, QuestionId: 0xA6D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x282D { 0F 0F 46 16 47 16 6D 0A 00 00 FF FF 00 2D 28 }
0x5094E: 		Ref Prompt: "Security Configuration", Help: "Security Configuration settings", QuestionFlags: 0x0, QuestionId: 0xA6E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2851 { 0F 0F 37 12 38 12 6E 0A 00 00 FF FF 00 51 28 }
0x5095D: 		SuppressIf  { 0A 82 }
0x5095F: 			EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x50965: 			Ref Prompt: "HD Audio Configuration", Help: "HD Audio Subsystem Configuration Settings", QuestionFlags: 0x0, QuestionId: 0xA6F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x284E { 0F 0F 44 11 45 11 6F 0A 00 00 FF FF 00 4E 28 }
0x50974: 		End  { 29 02 }
0x50976: 		GrayOutIf  { 19 82 }
0x50978: 			EqIdVal QuestionId: 0x1146, Value: 0x0 { 12 06 46 11 00 00 }
0x5097E: 			Ref Prompt: "THC Configuration", Help: "Touch Host Controller Configuration Settings", QuestionFlags: 0x0, QuestionId: 0xA70, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x284D { 0F 0F 08 12 09 12 70 0A 00 00 FF FF 00 4D 28 }
0x5098D: 		End  { 29 02 }
0x5098F: 		Ref Prompt: "SerialIo Configuration", Help: "SerialIo Configuration Settings", QuestionFlags: 0x0, QuestionId: 0xA71, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x7A { 0F 0F 7D 17 7E 17 71 0A 00 00 FF FF 00 7A 00 }
0x5099E: 		Ref Prompt: "ISH Configuration", Help: "Integrated Sensor Hub (ISH) Configuration", QuestionFlags: 0x0, QuestionId: 0xA72, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2853 { 0F 0F 65 17 66 17 72 0A 00 00 FF FF 00 53 28 }
0x509AD: 		Ref Prompt: "Pch Thermal Throttling Control", Help: "Pch Thermal Throttling Control", QuestionFlags: 0x0, QuestionId: 0xA73, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2854 { 0F 0F 0A 18 0A 18 73 0A 00 00 FF FF 00 54 28 }
0x509BC: 		OneOf Prompt: "Skip VCCIN_AUX Configuration", Help: "Skips VCCIN_AUX Configuration if enabled", QuestionFlags: 0x10, QuestionId: 0xA74, VarStoreId: 0x6, VarOffset: 0x790, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 18 CB 18 74 0A 06 00 90 07 10 10 00 01 00 }
0x509CD: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x509D4: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x509DB: 		End  { 29 02 }
0x509DD: 		Ref Prompt: "FIVR Configuration", Help: "Menu for changing FIVR configuration parameters", QuestionFlags: 0x0, QuestionId: 0xA75, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2858 { 0F 0F AA 18 AB 18 75 0A 00 00 FF FF 00 58 28 }
0x509EC: 		Ref Prompt: "PMC Configuration", Help: "Power management controller configuration", QuestionFlags: 0x0, QuestionId: 0xA76, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2859 { 0F 0F CC 18 CD 18 76 0A 00 00 FF FF 00 59 28 }
0x509FB: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x50A02: 		End  { 29 02 }
0x50A04: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x50A0B: 		End  { 29 02 }
0x50A0D: 		SuppressIf  { 0A 82 }
0x50A0F: 			EqIdVal QuestionId: 0x1145, Value: 0x0 { 12 06 45 11 00 00 }
0x50A15: 			SuppressIf  { 0A 82 }
0x50A17: 				EqIdVal QuestionId: 0x1144, Value: 0x0 { 12 06 44 11 00 00 }
0x50A1D: 				OneOf Prompt: "PCH LAN Controller", Help: "Enable/Disable onboard NIC.", QuestionFlags: 0x10, QuestionId: 0xA77, VarStoreId: 0x6, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 11 30 11 77 0A 06 00 09 00 10 10 00 01 00 }
0x50A2E: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50A35: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50A3C: 				End  { 29 02 }
0x50A3E: 			End  { 29 02 }
0x50A40: 			SuppressIf  { 0A 82 }
0x50A42: 				EqIdVal QuestionId: 0xA77, Value: 0x0 { 12 86 77 0A 00 00 }
0x50A48: 					EqIdVal QuestionId: 0x1144, Value: 0x0 { 12 06 44 11 00 00 }
0x50A4E: 					Or  { 16 02 }
0x50A50: 				End  { 29 02 }
0x50A52: 				OneOf Prompt: "LAN Wake From DeepSx", Help: "Wake from DeepSx by the assertion of LAN_WAKE# pin", QuestionFlags: 0x10, QuestionId: 0xA78, VarStoreId: 0x6, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 56 17 57 17 78 0A 06 00 05 00 10 10 00 01 00 }
0x50A63: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50A6A: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50A71: 				End  { 29 02 }
0x50A73: 				OneOf Prompt: "Wake on LAN Enable", Help: "Enable/Disable integrated LAN to wake the system.", QuestionFlags: 0x10, QuestionId: 0xA79, VarStoreId: 0x6, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 11 33 11 79 0A 06 00 0C 00 10 10 00 01 00 }
0x50A84: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50A8B: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50A92: 				End  { 29 02 }
0x50A94: 				OneOf Prompt: "  SLP_LAN# Low on DC Power", Help: "Enable/Disable SLP_LAN# Low on DC Power. Please notice this knob only applies to CNVd.", QuestionFlags: 0x10, QuestionId: 0xA7A, VarStoreId: 0x6, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 11 35 11 7A 0A 06 00 0D 00 10 10 00 01 00 }
0x50AA5: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50AAC: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50AB3: 				End  { 29 02 }
0x50AB5: 			End  { 29 02 }
0x50AB7: 			SuppressIf  { 0A 82 }
0x50AB9: 				EqIdVal QuestionId: 0x1144, Value: 0x1 { 12 06 44 11 01 00 }
0x50ABF: 				Text Prompt: "PCH LAN Controller", Help: "", Text: "No GbE Region" { 03 08 2F 11 C9 07 31 11 }
0x50AC7: 			End  { 29 02 }
0x50AC9: 		End  { 29 02 }
0x50ACB: 		OneOf Prompt: "Foxville I225 LAN Controller", Help: "Enable/Disable Foxville I225 LAN Controller.", QuestionFlags: 0x10, QuestionId: 0xA7B, VarStoreId: 0x6, VarOffset: 0x784, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 11 39 11 7B 0A 06 00 84 07 10 10 00 01 00 }
0x50ADC: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50AE3: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50AEA: 		End  { 29 02 }
0x50AEC: 		SuppressIf  { 0A 82 }
0x50AEE: 			EqIdVal QuestionId: 0xA7B, Value: 0x0 { 12 06 7B 0A 00 00 }
0x50AF4: 			OneOf Prompt: "  Foxville I225 Wake on LAN Support", Help: "Enable/Disable Foxville I225 Wake on LAN Support.", QuestionFlags: 0x10, QuestionId: 0xA7C, VarStoreId: 0x6, VarOffset: 0x785, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 11 3B 11 7C 0A 06 00 85 07 10 10 00 01 00 }
0x50B05: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50B0C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50B13: 			End  { 29 02 }
0x50B15: 		End  { 29 02 }
0x50B17: 		SuppressIf  { 0A 82 }
0x50B19: 			EqIdVal QuestionId: 0x1142, Value: 0x1 { 12 86 42 11 01 00 }
0x50B1F: 				Not  { 17 02 }
0x50B21: 				EqIdVal QuestionId: 0x1142, Value: 0x6 { 12 06 42 11 06 00 }
0x50B27: 				Not  { 17 02 }
0x50B29: 				And  { 15 02 }
0x50B2B: 				EqIdVal QuestionId: 0x1142, Value: 0x5 { 12 06 42 11 05 00 }
0x50B31: 				Not  { 17 02 }
0x50B33: 				And  { 15 02 }
0x50B35: 			End  { 29 02 }
0x50B37: 			OneOf Prompt: "Sensor Hub Type", Help: "Choose the Sensor Hub Type, 'None' will Suppress 'I2C Sensor Hub' Setup Option','I2C' Will Suppress 'ALS' Setup Option and 'USB' will Suppress Both I2C and ALS.", QuestionFlags: 0x10, QuestionId: 0xA7D, VarStoreId: 0xF101, VarOffset: 0x66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 4B 17 4C 17 7D 0A 01 F1 66 00 10 10 00 02 00 }
0x50B48: 				OneOfOption Option: "None" Value: 0, Default, MfgDefault { 09 07 4D 17 30 00 00 }
0x50B4F: 				OneOfOption Option: "I2C Sensor Hub" Value: 1 { 09 07 4E 17 00 00 01 }
0x50B56: 				OneOfOption Option: "USB Sensor Hub" Value: 2 { 09 07 4F 17 00 00 02 }
0x50B5D: 			End  { 29 02 }
0x50B5F: 		End  { 29 02 }
0x50B61: 		OneOf Prompt: "DeepSx Power Policies", Help: "configure the DeepSx Mode configuration.", QuestionFlags: 0x10, QuestionId: 0xA7E, VarStoreId: 0x6, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 50 17 51 17 7E 0A 06 00 04 00 10 10 00 04 00 }
0x50B72: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50B79: 			SuppressIf  { 0A 82 }
0x50B7B: 				EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 86 42 11 02 00 }
0x50B81: 					EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x50B87: 					Or  { 16 02 }
0x50B89: 					EqIdVal QuestionId: 0x1142, Value: 0x3 { 12 06 42 11 03 00 }
0x50B8F: 					Or  { 16 02 }
0x50B91: 				End  { 29 02 }
0x50B93: 				OneOfOption Option: "Enabled in S4-S5-Battery" Value: 3 { 09 07 54 17 00 00 03 }
0x50B9A: 				OneOfOption Option: "Enabled in S5-Battery" Value: 1 { 09 07 52 17 00 00 01 }
0x50BA1: 			End  { 29 02 }
0x50BA3: 			OneOfOption Option: "Enabled in S4-S5" Value: 4 { 09 07 55 17 00 00 04 }
0x50BAA: 			OneOfOption Option: "Enabled in S5" Value: 2 { 09 07 53 17 00 00 02 }
0x50BB1: 		End  { 29 02 }
0x50BB3: 		SuppressIf  { 0A 82 }
0x50BB5: 			EqIdVal QuestionId: 0x1142, Value: 0x2 { 12 86 42 11 02 00 }
0x50BBB: 				Not  { 17 02 }
0x50BBD: 			End  { 29 02 }
0x50BBF: 			OneOf Prompt: "PS_ON Enable", Help: "Enable or disable PS_ON ()support a new C10 state from the CPU on desktop SKUs that enables a lower power target that will be required by the California Energy Commission (CEC).", QuestionFlags: 0x10, QuestionId: 0xA7F, VarStoreId: 0x6, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 36 11 37 11 7F 0A 06 00 1E 00 10 10 00 01 00 }
0x50BD0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50BD7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50BDE: 			End  { 29 02 }
0x50BE0: 		End  { 29 02 }
0x50BE2: 		OneOf Prompt: "Wake on WLAN and BT Enable", Help: "Enable/Disable PCI Express Wireless LAN and Bluetooth to wake the system. ", QuestionFlags: 0x10, QuestionId: 0xA80, VarStoreId: 0x6, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 11 3D 11 80 0A 06 00 0E 00 10 10 00 01 00 }
0x50BF3: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50BFA: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50C01: 		End  { 29 02 }
0x50C03: 		SuppressIf  { 0A 82 }
0x50C05: 			EqIdVal QuestionId: 0xA80, Value: 0x0 { 12 06 80 0A 00 00 }
0x50C0B: 			OneOf Prompt: "DeepSx Wake on WLAN and BT Enable", Help: "Enable/Disable PCI Express Wireless LAN and Bluetooth to wake the system from DeepSx. ", QuestionFlags: 0x10, QuestionId: 0xA81, VarStoreId: 0x6, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 11 3F 11 81 0A 06 00 0F 00 10 10 00 01 00 }
0x50C1C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50C23: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50C2A: 			End  { 29 02 }
0x50C2C: 		End  { 29 02 }
0x50C2E: 		OneOf Prompt: "Disable DSX ACPRESENT PullDown", Help: "Disable PCH internal ACPRESENT PullDown when DeepSx or G3 exit.", QuestionFlags: 0x10, QuestionId: 0xA82, VarStoreId: 0x6, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 11 41 11 82 0A 06 00 06 00 10 10 00 01 00 }
0x50C3F: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x50C45: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50C4C: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50C53: 		End  { 29 02 }
0x50C55: 		SuppressIf  { 0A 82 }
0x50C57: 			True  { 46 02 }
0x50C59: 			OneOf Prompt: "High Precision Timer", Help: "Enable or Disable the High Precision Event Timer.", QuestionFlags: 0x10, QuestionId: 0xA83, VarStoreId: 0x6, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 11 43 11 83 0A 06 00 1F 00 10 10 00 01 00 }
0x50C6A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50C71: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50C78: 			End  { 29 02 }
0x50C7A: 		End  { 29 02 }
0x50C7C: 		OneOf Prompt: "State After G3", Help: "Specify what state to go to when power is re-applied after a power failure (G3 state).", QuestionFlags: 0x14, QuestionId: 0x27CF, VarStoreId: 0x6, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 16 96 16 CF 27 06 00 20 00 14 10 00 01 00 }
0x50C8D: 			OneOfOption Option: "S0 State" Value: 0, Default, MfgDefault { 09 07 97 16 30 00 00 }
0x50C94: 			OneOfOption Option: "S5 State" Value: 1 { 09 07 98 16 00 00 01 }
0x50C9B: 		End  { 29 02 }
0x50C9D: 		OneOf Prompt: "Port 80h Redirection", Help: "Control where the Port 80h cycles are sent.", QuestionFlags: 0x10, QuestionId: 0xA84, VarStoreId: 0x6, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 45 17 46 17 84 0A 06 00 21 00 10 10 00 01 00 }
0x50CAE: 			OneOfOption Option: "LPC Bus" Value: 0, Default, MfgDefault { 09 07 47 17 30 00 00 }
0x50CB5: 			OneOfOption Option: "PCIE Bus" Value: 1 { 09 07 48 17 00 00 01 }
0x50CBC: 		End  { 29 02 }
0x50CBE: 		GrayOutIf  { 19 82 }
0x50CC0: 			EqIdVal QuestionId: 0xA84, Value: 0x0 { 12 86 84 0A 00 00 }
0x50CC6: 				Not  { 17 02 }
0x50CC8: 			End  { 29 02 }
0x50CCA: 			OneOf Prompt: "Enhance Port 80h LPC Decoding", Help: "Support the word/dword decoding of port 80h behind LPC", QuestionFlags: 0x10, QuestionId: 0xA85, VarStoreId: 0x6, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 49 17 4A 17 85 0A 06 00 22 00 10 10 00 01 00 }
0x50CDB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50CE2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50CE9: 			End  { 29 02 }
0x50CEB: 		End  { 29 02 }
0x50CED: 		GrayOutIf  { 19 82 }
0x50CEF: 			EqIdVal QuestionId: 0x1143, Value: 0x0 { 12 06 43 11 00 00 }
0x50CF5: 			OneOf Prompt: "Compatible Revision ID", Help: "Enable/Disable the PCH Compatible Revision ID feature", QuestionFlags: 0x14, QuestionId: 0x27D0, VarStoreId: 0x6, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 11 EC 11 D0 27 06 00 12 00 14 10 00 01 00 }
0x50D06: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x50D0C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 CF 00 00 00 00 }
0x50D13: 				OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 CE 00 20 00 01 }
0x50D1A: 			End  { 29 02 }
0x50D1C: 		End  { 29 02 }
0x50D1E: 		OneOf Prompt: "Legacy IO Low Latency", Help: "Set to enable low latency of legacy IO. Some systems require lower IO latency irrespective of power. This is a tradeoff between power and IO latency.", QuestionFlags: 0x10, QuestionId: 0x27D1, VarStoreId: 0x6, VarOffset: 0x76F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 ED 11 EE 11 D1 27 06 00 6F 07 10 10 00 01 00 }
0x50D2F: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x50D36: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50D3D: 		End  { 29 02 }
0x50D3F: 		OneOf Prompt: "PCH Cross Throttling", Help: "Enable/Disable the PCH Cross Throttling feature. Only ULT support this feature.", QuestionFlags: 0x10, QuestionId: 0xA86, VarStoreId: 0x6, VarOffset: 0x6BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EF 11 F0 11 86 0A 06 00 BE 06 10 10 00 01 00 }
0x50D50: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50D57: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50D5E: 		End  { 29 02 }
0x50D60: 		OneOf Prompt: "PCH Energy Reporting", Help: "Enable Energy Report. MUST set it as ENABLED. This is only for test purpose.", QuestionFlags: 0x10, QuestionId: 0xA87, VarStoreId: 0x6, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 11 F2 11 87 0A 06 00 10 00 10 10 00 01 00 }
0x50D71: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50D78: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50D7F: 		End  { 29 02 }
0x50D81: 		OneOf Prompt: "LPM S0i2.0", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA88, VarStoreId: 0x6, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F3 11 FA 11 88 0A 06 00 13 00 10 10 00 01 00 }
0x50D92: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50D99: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50DA0: 		End  { 29 02 }
0x50DA2: 		OneOf Prompt: "LPM S0i2.1", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA89, VarStoreId: 0x6, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F4 11 FA 11 89 0A 06 00 14 00 10 10 00 01 00 }
0x50DB3: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50DBA: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50DC1: 		End  { 29 02 }
0x50DC3: 		SuppressIf  { 0A 82 }
0x50DC5: 			True  { 46 02 }
0x50DC7: 			OneOf Prompt: "LPM S0i3.0", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA8A, VarStoreId: 0x6, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 19 FA 11 8A 0A 06 00 16 00 10 10 00 01 00 }
0x50DD8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50DDF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50DE6: 			End  { 29 02 }
0x50DE8: 			OneOf Prompt: "LPM S0i2.2", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA8B, VarStoreId: 0x6, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 11 FA 11 8B 0A 06 00 15 00 10 10 00 01 00 }
0x50DF9: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50E00: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50E07: 			End  { 29 02 }
0x50E09: 			OneOf Prompt: "LPM S0i3.2", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA8C, VarStoreId: 0x6, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F7 11 FA 11 8C 0A 06 00 18 00 10 10 00 01 00 }
0x50E1A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50E21: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50E28: 			End  { 29 02 }
0x50E2A: 			OneOf Prompt: "LPM S0i3.3", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA8D, VarStoreId: 0x6, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F8 11 FA 11 8D 0A 06 00 19 00 10 10 00 01 00 }
0x50E3B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50E42: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50E49: 			End  { 29 02 }
0x50E4B: 			OneOf Prompt: "LPM S0i3.4", Help: "Enable/Disable S0ix sub-state. This setting is for test purpose. S0ix sub-states should be enabled for production.", QuestionFlags: 0x10, QuestionId: 0xA8E, VarStoreId: 0x6, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 11 FA 11 8E 0A 06 00 1A 00 10 10 00 01 00 }
0x50E5C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50E63: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50E6A: 			End  { 29 02 }
0x50E6C: 		End  { 29 02 }
0x50E6E: 		OneOf Prompt: "C10 Dynamic threshold adjustment", Help: "Enable/Disable C10 dynamic threshold adjustment", QuestionFlags: 0x10, QuestionId: 0xA8F, VarStoreId: 0x6, VarOffset: 0x77D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FB 11 FC 11 8F 0A 06 00 7D 07 10 10 00 01 00 }
0x50E7F: 			OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x50E86: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50E8D: 		End  { 29 02 }
0x50E8F: 		OneOf Prompt: "IEH Mode", Help: "Enable/Bypass IEH Mode", QuestionFlags: 0x10, QuestionId: 0xA90, VarStoreId: 0x6, VarOffset: 0x51E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 11 FE 11 90 0A 06 00 1E 05 10 10 00 01 00 }
0x50EA0: 			OneOfOption Option: "Bypass Mode" Value: 0, Default, MfgDefault { 09 07 FF 11 30 00 00 }
0x50EA7: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50EAE: 		End  { 29 02 }
0x50EB0: 		OneOf Prompt: "Enable TCO Timer", Help: "Enable/Disable TCO timer. When disabled, it disables PCH ACPI timer, stops TCO timer, and ACPI WDAT table will not be published.", QuestionFlags: 0x10, QuestionId: 0xA91, VarStoreId: 0x6, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 12 03 12 91 0A 06 00 11 00 10 10 00 01 00 }
0x50EC1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x50EC8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x50ECF: 		End  { 29 02 }
0x50ED1: 		OneOf Prompt: "Pcie Pll SSC", Help: "Pcie Pll SSC percentage.AUTO - Keep hw default, no BIOS override. Range is 0.0%-2.0%.", QuestionFlags: 0x10, QuestionId: 0xA92, VarStoreId: 0x6, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 5A 18 5B 18 92 0A 06 00 23 00 10 10 00 FF 00 }
0x50EE2: 			OneOfOption Option: "Auto" Value: 255, Default, MfgDefault { 09 07 90 00 30 00 FF }
0x50EE9: 			OneOfOption Option: "0.0%" Value: 0 { 09 07 5C 18 00 00 00 }
0x50EF0: 			OneOfOption Option: "0.1%" Value: 1 { 09 07 5D 18 00 00 01 }
0x50EF7: 			OneOfOption Option: "0.2%" Value: 2 { 09 07 5E 18 00 00 02 }
0x50EFE: 			OneOfOption Option: "0.3%" Value: 3 { 09 07 5F 18 00 00 03 }
0x50F05: 			OneOfOption Option: "0.4%" Value: 4 { 09 07 60 18 00 00 04 }
0x50F0C: 			OneOfOption Option: "0.5%" Value: 5 { 09 07 61 18 00 00 05 }
0x50F13: 			OneOfOption Option: "0.6%" Value: 6 { 09 07 62 18 00 00 06 }
0x50F1A: 			OneOfOption Option: "0.7%" Value: 7 { 09 07 63 18 00 00 07 }
0x50F21: 			OneOfOption Option: "0.8%" Value: 8 { 09 07 64 18 00 00 08 }
0x50F28: 			OneOfOption Option: "0.9%" Value: 9 { 09 07 65 18 00 00 09 }
0x50F2F: 			OneOfOption Option: "1.0%" Value: 10 { 09 07 66 18 00 00 0A }
0x50F36: 			OneOfOption Option: "1.1%" Value: 11 { 09 07 67 18 00 00 0B }
0x50F3D: 			OneOfOption Option: "1.2%" Value: 12 { 09 07 68 18 00 00 0C }
0x50F44: 			OneOfOption Option: "1.3%" Value: 13 { 09 07 69 18 00 00 0D }
0x50F4B: 			OneOfOption Option: "1.4%" Value: 14 { 09 07 6A 18 00 00 0E }
0x50F52: 			OneOfOption Option: "1.5%" Value: 15 { 09 07 6B 18 00 00 0F }
0x50F59: 			OneOfOption Option: "1.6%" Value: 16 { 09 07 6C 18 00 00 10 }
0x50F60: 			OneOfOption Option: "1.7%" Value: 17 { 09 07 6D 18 00 00 11 }
0x50F67: 			OneOfOption Option: "1.8%" Value: 18 { 09 07 6E 18 00 00 12 }
0x50F6E: 			OneOfOption Option: "1.9%" Value: 19 { 09 07 6F 18 00 00 13 }
0x50F75: 			OneOfOption Option: "2.0%" Value: 20 { 09 07 70 18 00 00 14 }
0x50F7C: 			OneOfOption Option: "Disable" Value: 254 { 09 07 71 18 00 00 FE }
0x50F83: 		End  { 29 02 }
0x50F85: 		SuppressIf  { 0A 82 }
0x50F87: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x50F8D: 				Not  { 17 02 }
0x50F8F: 				EqIdVal QuestionId: 0x1142, Value: 0x4 { 12 06 42 11 04 00 }
0x50F95: 				Not  { 17 02 }
0x50F97: 				And  { 15 02 }
0x50F99: 			End  { 29 02 }
0x50F9B: 			OneOf Prompt: "IOAPIC 24-119 Entries", Help: "Enables/Disables IOAPIC 24-119 Entries. IRQ24-119 may be used by PCH devices. Disabling those interrupts may cause certain devices failure.", QuestionFlags: 0x10, QuestionId: 0xA93, VarStoreId: 0x6, VarOffset: 0x6BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 17 59 17 93 0A 06 00 BC 06 10 10 00 01 00 }
0x50FAC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50FB3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50FBA: 			End  { 29 02 }
0x50FBC: 		End  { 29 02 }
0x50FBE: 		OneOf Prompt: "Enable 8254 Clock Gate", Help: "Enables/Disables 8254 clock gate in early phase. Set 8254CGE is necessary for SLP_S0 support. Platform is albe to disable this policy and set 8254CGE in late phase.", QuestionFlags: 0x10, QuestionId: 0xA94, VarStoreId: 0x6, VarOffset: 0x6BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 5A 17 5B 17 94 0A 06 00 BD 06 10 10 00 02 00 }
0x50FCF: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50FD6: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x50FDD: 			OneOfOption Option: "Enabled In Runtime and S3 Resume" Value: 2 { 09 07 5C 17 00 00 02 }
0x50FE4: 		End  { 29 02 }
0x50FE6: 		OneOf Prompt: "Lock PCH Sideband Access", Help: "Lock PCH Sideband access, include SideBand interface lock and SideBand PortID mask for certain end point (e.g. PSFx). The option is invalid if POSTBOOT SAI is set.", QuestionFlags: 0x10, QuestionId: 0xA95, VarStoreId: 0x6, VarOffset: 0x73C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 11 2E 11 95 0A 06 00 3C 07 10 10 00 01 00 }
0x50FF7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x50FFE: 			OneOfOption Option: "Enabled" Value: 1, Default { 09 07 03 00 10 00 01 }
0x51005: 		End  { 29 02 }
0x51007: 		OneOf Prompt: "Flash Protection Range Registers (FPRR)", Help: "Enable Flash Protection Range Registers", QuestionFlags: 0x10, QuestionId: 0xA96, VarStoreId: 0x6, VarOffset: 0x73D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 18 75 18 96 0A 06 00 3D 07 10 10 00 01 00 }
0x51018: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5101F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51026: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x5102C: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x51032: 		End  { 29 02 }
0x51034: 		OneOf Prompt: "SPD Write Disable", Help: "Enable/Disable setting SPD Write Disable. For security recommendations, SPD write disable bit must be set.", QuestionFlags: 0x10, QuestionId: 0xA97, VarStoreId: 0x6, VarOffset: 0x73B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 18 77 18 97 0A 06 00 3B 07 10 10 00 01 00 }
0x51045: 			OneOfOption Option: "TRUE" Value: 1, Default, MfgDefault { 09 07 34 06 30 00 01 }
0x5104C: 			OneOfOption Option: "FALSE" Value: 0 { 09 07 33 06 00 00 00 }
0x51053: 		End  { 29 02 }
0x51055: 		OneOf Prompt: "LGMR", Help: "64KB memory block for LGMR (LPC Memory Range Decode)", QuestionFlags: 0x10, QuestionId: 0xA98, VarStoreId: 0x6, VarOffset: 0x739, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 18 79 18 98 0A 06 00 39 07 10 10 00 01 00 }
0x51066: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5106D: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x51074: 		End  { 29 02 }
0x51076: 		OneOf Prompt: "HOST_C10 reporting to Target", Help: "This option enables HOST_C10 reporting to Target via eSPI Virtual Wire", QuestionFlags: 0x10, QuestionId: 0xA99, VarStoreId: 0x6, VarOffset: 0x73A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 18 7B 18 99 0A 06 00 3A 07 10 10 00 01 00 }
0x51087: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5108E: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51095: 		End  { 29 02 }
0x51097: 		OneOf Prompt: "OS IDLE Mode", Help: "Enable/Disable OS Idle Mode Feature", QuestionFlags: 0x10, QuestionId: 0xA9A, VarStoreId: 0x6, VarOffset: 0x76E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7E 18 7F 18 9A 0A 06 00 6E 07 10 10 00 01 00 }
0x510A8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x510AF: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x510B6: 		End  { 29 02 }
0x510B8: 		OneOf Prompt: "S0ix Auto Demotion", Help: "Enable/Disable Host Low Power Mode S0ix Auto-Demotion", QuestionFlags: 0x10, QuestionId: 0xA9B, VarStoreId: 0x6, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 80 18 81 18 9B 0A 06 00 25 00 10 10 00 01 00 }
0x510C9: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x510D0: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x510D7: 		End  { 29 02 }
0x510D9: 		OneOf Prompt: "Latch Events C10 Exit", Help: "Enable/Disable Latch Events on C10 Exit", QuestionFlags: 0x10, QuestionId: 0xA9C, VarStoreId: 0x6, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 00 12 01 12 9C 0A 06 00 26 00 10 10 00 01 00 }
0x510EA: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x510F1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x510F8: 		End  { 29 02 }
0x510FA: 		OneOf Prompt: "Hybrid Storage Detection and Configuration Mode", Help: "Select Hybrid Storage Detection and Configuration Mode", QuestionFlags: 0x10, QuestionId: 0xA9D, VarStoreId: 0x6, VarOffset: 0x775, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F0 18 F1 18 9D 0A 06 00 75 07 10 10 00 01 00 }
0x5110B: 			OneOfOption Option: "Dynamic Configuration for Hybrid Storage Enable" Value: 1 { 09 07 F2 18 00 00 01 }
0x51112: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x51119: 		End  { 29 02 }
0x5111B: 		SuppressIf  { 0A 82 }
0x5111D: 			EqIdVal QuestionId: 0xA9D, Value: 0x0 { 12 06 9D 0A 00 00 }
0x51123: 			Numeric Prompt: "Cpu Root port used for hybrid storage", Help: "Select cpu root port used for hybrid storage value between 0 to 2", QuestionFlags: 0x10, QuestionId: 0xA9E, VarStoreId: 0x6, VarOffset: 0x787, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F3 18 F4 18 9E 0A 06 00 87 07 10 10 00 FF 01 }
0x51134: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x5113A: 			End  { 29 02 }
0x5113C: 		End  { 29 02 }
0x5113E: 		SuppressIf  { 0A 82 }
0x51140: 			EqIdVal QuestionId: 0xA9E, Value: 0xFF { 12 06 9E 0A FF 00 }
0x51146: 			Numeric Prompt: "Pch root port used for hybrid storage", Help: "Select pch root port used in combination with cpu root port for hybrid storage enter value between 0 to 16", QuestionFlags: 0x10, QuestionId: 0xA9F, VarStoreId: 0x6, VarOffset: 0x788, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1 { 07 91 F5 18 F6 18 9F 0A 06 00 88 07 10 10 00 FF 01 }
0x51157: 				Default DefaultId: 0x0 Value: 255 { 5B 06 00 00 00 FF }
0x5115D: 			End  { 29 02 }
0x5115F: 		End  { 29 02 }
0x51161: 		OneOf Prompt: "Extended BIOS Range Decode", Help: "Enabling this will make memory cycles falling in a specific area to be redirected to SPI flash controller", QuestionFlags: 0x10, QuestionId: 0xAA0, VarStoreId: 0x6, VarOffset: 0x77E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7C 18 7D 18 A0 0A 06 00 7E 07 10 10 00 01 00 }
0x51172: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x51179: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51180: 		End  { 29 02 }
0x51182: 		OneOf Prompt: "ACPI L6D PME Handling", Help: "BIOS through ACPI code can associate specific method to a particular GPE. In this case _L6D for Level-triggered Event, BIOS-ACPI can verify PMEENABLE and PMESTATUS of each device that requires GPE related wake.", QuestionFlags: 0x10, QuestionId: 0xAA1, VarStoreId: 0x6, VarOffset: 0x78A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F7 18 F8 18 A1 0A 06 00 8A 07 10 10 00 01 00 }
0x51193: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5119A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x511A1: 		End  { 29 02 }
0x511A3: 	End  { 29 02 }
0x511A5: 	Form FormId: 0x282C, Title: "PCI Express Configuration" { 01 86 2C 28 7C 0E }
0x511AB: 		Subtitle Prompt: "PCI Express Configuration", Help: "", Flags: 0x0 { 02 87 7C 0E 00 00 00 }
0x511B2: 		End  { 29 02 }
0x511B4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x511BB: 		End  { 29 02 }
0x511BD: 		OneOf Prompt: "DMI Link ASPM Control", Help: "The control of Active State Power Management of the DMI Link.", QuestionFlags: 0x10, QuestionId: 0x27D2, VarStoreId: 0x6, VarOffset: 0x517, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 41 13 42 13 D2 27 06 00 17 05 10 10 00 04 00 }
0x511CE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x511D5: 			OneOfOption Option: "L1" Value: 2, Default, MfgDefault { 09 07 FC 0E 30 00 02 }
0x511DC: 			OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x511E3: 		End  { 29 02 }
0x511E5: 		OneOf Prompt: "Port8xh Decode", Help: "PCI Express Port8xh Decode Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xAA2, VarStoreId: 0x6, VarOffset: 0xBC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A3 14 A4 14 A2 0A 06 00 BC 00 10 10 00 01 00 }
0x511F6: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x511FD: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51204: 		End  { 29 02 }
0x51206: 		SuppressIf  { 0A 82 }
0x51208: 			EqIdVal QuestionId: 0xAA2, Value: 0x0 { 12 06 A2 0A 00 00 }
0x5120E: 			Numeric Prompt: "  Port8xh Decode Port#", Help: "Select PCI Express Port8xh Decode Root Port. User to ensure port availability", QuestionFlags: 0x10, QuestionId: 0xAA3, VarStoreId: 0x6, VarOffset: 0xBD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1B, Step: 0x1 { 07 91 A5 14 A6 14 A3 0A 06 00 BD 00 10 10 00 1B 01 }
0x5121F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x51225: 			End  { 29 02 }
0x51227: 		End  { 29 02 }
0x51229: 		OneOf Prompt: "Compliance Test Mode", Help: "Enable when using Compliance Load Board", QuestionFlags: 0x10, QuestionId: 0xAA4, VarStoreId: 0x6, VarOffset: 0xDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 14 C5 14 A4 0A 06 00 DA 00 10 10 00 01 00 }
0x5123A: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x51241: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51248: 		End  { 29 02 }
0x5124A: 		OneOf Prompt: "PCIe function swap", Help: "When Disabled, prevents PCIE rootport function swap. If any function other than 0th is enabled, 0th will become visible.", QuestionFlags: 0x10, QuestionId: 0xAA5, VarStoreId: 0x6, VarOffset: 0x3BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 18 73 18 A5 0A 06 00 BB 03 10 10 00 01 00 }
0x5125B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51262: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51269: 		End  { 29 02 }
0x5126B: 		Ref Prompt: "PCIe EQ settings", Help: "This form contains options for controlling PCIe EQ process", QuestionFlags: 0x0, QuestionId: 0xAA6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x282F { 0F 0F 3F 12 40 12 A6 0A 00 00 FF FF 00 2F 28 }
0x5127A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x51281: 		End  { 29 02 }
0x51283: 		SuppressIf  { 0A 82 }
0x51285: 			EqIdVal QuestionId: 0x1141, Value: 0x0 { 12 86 41 11 00 00 }
0x5128B: 				Not  { 17 02 }
0x5128D: 			End  { 29 02 }
0x5128F: 			Ref Prompt: "PCI Express Root Port 1", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAA7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2830 { 0F 0F 76 16 92 16 A7 0A 00 00 FF FF 00 30 28 }
0x5129E: 		End  { 29 02 }
0x512A0: 		SuppressIf  { 0A 82 }
0x512A2: 			EqIdVal QuestionId: 0x1141, Value: 0x1 { 12 86 41 11 01 00 }
0x512A8: 				Not  { 17 02 }
0x512AA: 			End  { 29 02 }
0x512AC: 			Text Prompt: "PCI Express Root Port 1", Help: "", Text: "Not present in this SKU" { 03 08 76 16 C9 07 82 0E }
0x512B4: 		End  { 29 02 }
0x512B6: 		SuppressIf  { 0A 82 }
0x512B8: 			EqIdVal QuestionId: 0x1141, Value: 0x2 { 12 86 41 11 02 00 }
0x512BE: 				Not  { 17 02 }
0x512C0: 			End  { 29 02 }
0x512C2: 			Text Prompt: "PCI Express Root Port 1", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 76 16 C9 07 83 0E }
0x512CA: 		End  { 29 02 }
0x512CC: 		SuppressIf  { 0A 82 }
0x512CE: 			EqIdVal QuestionId: 0x1141, Value: 0x3 { 12 86 41 11 03 00 }
0x512D4: 				Not  { 17 02 }
0x512D6: 			End  { 29 02 }
0x512D8: 			Text Prompt: "PCI Express Root Port 1", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 76 16 C9 07 93 16 }
0x512E0: 		End  { 29 02 }
0x512E2: 		SuppressIf  { 0A 82 }
0x512E4: 			EqIdVal QuestionId: 0x1140, Value: 0x0 { 12 86 40 11 00 00 }
0x512EA: 				Not  { 17 02 }
0x512EC: 			End  { 29 02 }
0x512EE: 			Ref Prompt: "PCI Express Root Port 2", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAA8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2831 { 0F 0F 77 16 92 16 A8 0A 00 00 FF FF 00 31 28 }
0x512FD: 		End  { 29 02 }
0x512FF: 		SuppressIf  { 0A 82 }
0x51301: 			EqIdVal QuestionId: 0x1140, Value: 0x1 { 12 86 40 11 01 00 }
0x51307: 				Not  { 17 02 }
0x51309: 			End  { 29 02 }
0x5130B: 			Text Prompt: "PCI Express Root Port 2", Help: "", Text: "Not present in this SKU" { 03 08 77 16 C9 07 82 0E }
0x51313: 		End  { 29 02 }
0x51315: 		SuppressIf  { 0A 82 }
0x51317: 			EqIdVal QuestionId: 0x1140, Value: 0x2 { 12 86 40 11 02 00 }
0x5131D: 				Not  { 17 02 }
0x5131F: 			End  { 29 02 }
0x51321: 			Text Prompt: "PCI Express Root Port 2", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 77 16 C9 07 83 0E }
0x51329: 		End  { 29 02 }
0x5132B: 		SuppressIf  { 0A 82 }
0x5132D: 			EqIdVal QuestionId: 0x1140, Value: 0x3 { 12 86 40 11 03 00 }
0x51333: 				Not  { 17 02 }
0x51335: 			End  { 29 02 }
0x51337: 			Text Prompt: "PCI Express Root Port 2", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 77 16 C9 07 93 16 }
0x5133F: 		End  { 29 02 }
0x51341: 		SuppressIf  { 0A 82 }
0x51343: 			EqIdVal QuestionId: 0x113F, Value: 0x0 { 12 86 3F 11 00 00 }
0x51349: 				Not  { 17 02 }
0x5134B: 			End  { 29 02 }
0x5134D: 			Ref Prompt: "PCI Express Root Port 3", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAA9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2832 { 0F 0F 78 16 92 16 A9 0A 00 00 FF FF 00 32 28 }
0x5135C: 		End  { 29 02 }
0x5135E: 		SuppressIf  { 0A 82 }
0x51360: 			EqIdVal QuestionId: 0x113F, Value: 0x1 { 12 86 3F 11 01 00 }
0x51366: 				Not  { 17 02 }
0x51368: 			End  { 29 02 }
0x5136A: 			Text Prompt: "PCI Express Root Port 3", Help: "", Text: "Not present in this SKU" { 03 08 78 16 C9 07 82 0E }
0x51372: 		End  { 29 02 }
0x51374: 		SuppressIf  { 0A 82 }
0x51376: 			EqIdVal QuestionId: 0x113F, Value: 0x2 { 12 86 3F 11 02 00 }
0x5137C: 				Not  { 17 02 }
0x5137E: 			End  { 29 02 }
0x51380: 			Text Prompt: "PCI Express Root Port 3", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 78 16 C9 07 83 0E }
0x51388: 		End  { 29 02 }
0x5138A: 		SuppressIf  { 0A 82 }
0x5138C: 			EqIdVal QuestionId: 0x113F, Value: 0x3 { 12 86 3F 11 03 00 }
0x51392: 				Not  { 17 02 }
0x51394: 			End  { 29 02 }
0x51396: 			Text Prompt: "PCI Express Root Port 3", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 78 16 C9 07 93 16 }
0x5139E: 		End  { 29 02 }
0x513A0: 		SuppressIf  { 0A 82 }
0x513A2: 			EqIdVal QuestionId: 0x113E, Value: 0x0 { 12 86 3E 11 00 00 }
0x513A8: 				Not  { 17 02 }
0x513AA: 			End  { 29 02 }
0x513AC: 			Ref Prompt: "PCI Express Root Port 4", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAAA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2833 { 0F 0F 79 16 92 16 AA 0A 00 00 FF FF 00 33 28 }
0x513BB: 		End  { 29 02 }
0x513BD: 		SuppressIf  { 0A 82 }
0x513BF: 			EqIdVal QuestionId: 0x113E, Value: 0x1 { 12 86 3E 11 01 00 }
0x513C5: 				Not  { 17 02 }
0x513C7: 			End  { 29 02 }
0x513C9: 			Text Prompt: "PCI Express Root Port 4", Help: "", Text: "Not present in this SKU" { 03 08 79 16 C9 07 82 0E }
0x513D1: 		End  { 29 02 }
0x513D3: 		SuppressIf  { 0A 82 }
0x513D5: 			EqIdVal QuestionId: 0x113E, Value: 0x2 { 12 86 3E 11 02 00 }
0x513DB: 				Not  { 17 02 }
0x513DD: 			End  { 29 02 }
0x513DF: 			Text Prompt: "PCI Express Root Port 4", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 79 16 C9 07 83 0E }
0x513E7: 		End  { 29 02 }
0x513E9: 		SuppressIf  { 0A 82 }
0x513EB: 			EqIdVal QuestionId: 0x113E, Value: 0x3 { 12 86 3E 11 03 00 }
0x513F1: 				Not  { 17 02 }
0x513F3: 			End  { 29 02 }
0x513F5: 			Text Prompt: "PCI Express Root Port 4", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 79 16 C9 07 93 16 }
0x513FD: 		End  { 29 02 }
0x513FF: 		SuppressIf  { 0A 82 }
0x51401: 			EqIdVal QuestionId: 0x113D, Value: 0x0 { 12 86 3D 11 00 00 }
0x51407: 				Not  { 17 02 }
0x51409: 			End  { 29 02 }
0x5140B: 			Ref Prompt: "PCI Express Root Port 5", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAAB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2834 { 0F 0F 7A 16 92 16 AB 0A 00 00 FF FF 00 34 28 }
0x5141A: 		End  { 29 02 }
0x5141C: 		SuppressIf  { 0A 82 }
0x5141E: 			EqIdVal QuestionId: 0x113D, Value: 0x1 { 12 86 3D 11 01 00 }
0x51424: 				Not  { 17 02 }
0x51426: 			End  { 29 02 }
0x51428: 			Text Prompt: "PCI Express Root Port 5", Help: "", Text: "Not present in this SKU" { 03 08 7A 16 C9 07 82 0E }
0x51430: 		End  { 29 02 }
0x51432: 		SuppressIf  { 0A 82 }
0x51434: 			EqIdVal QuestionId: 0x113D, Value: 0x2 { 12 86 3D 11 02 00 }
0x5143A: 				Not  { 17 02 }
0x5143C: 			End  { 29 02 }
0x5143E: 			Text Prompt: "PCI Express Root Port 5", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 7A 16 C9 07 83 0E }
0x51446: 		End  { 29 02 }
0x51448: 		SuppressIf  { 0A 82 }
0x5144A: 			EqIdVal QuestionId: 0x113D, Value: 0x3 { 12 86 3D 11 03 00 }
0x51450: 				Not  { 17 02 }
0x51452: 			End  { 29 02 }
0x51454: 			Text Prompt: "PCI Express Root Port 5", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 7A 16 C9 07 93 16 }
0x5145C: 		End  { 29 02 }
0x5145E: 		SuppressIf  { 0A 82 }
0x51460: 			EqIdVal QuestionId: 0x113C, Value: 0x0 { 12 86 3C 11 00 00 }
0x51466: 				Not  { 17 02 }
0x51468: 			End  { 29 02 }
0x5146A: 			Ref Prompt: "PCI Express Root Port 6", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAAC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2835 { 0F 0F 7B 16 92 16 AC 0A 00 00 FF FF 00 35 28 }
0x51479: 		End  { 29 02 }
0x5147B: 		SuppressIf  { 0A 82 }
0x5147D: 			EqIdVal QuestionId: 0x113C, Value: 0x1 { 12 86 3C 11 01 00 }
0x51483: 				Not  { 17 02 }
0x51485: 			End  { 29 02 }
0x51487: 			Text Prompt: "PCI Express Root Port 6", Help: "", Text: "Not present in this SKU" { 03 08 7B 16 C9 07 82 0E }
0x5148F: 		End  { 29 02 }
0x51491: 		SuppressIf  { 0A 82 }
0x51493: 			EqIdVal QuestionId: 0x113C, Value: 0x2 { 12 86 3C 11 02 00 }
0x51499: 				Not  { 17 02 }
0x5149B: 			End  { 29 02 }
0x5149D: 			Text Prompt: "PCI Express Root Port 6", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 7B 16 C9 07 83 0E }
0x514A5: 		End  { 29 02 }
0x514A7: 		SuppressIf  { 0A 82 }
0x514A9: 			EqIdVal QuestionId: 0x113C, Value: 0x3 { 12 86 3C 11 03 00 }
0x514AF: 				Not  { 17 02 }
0x514B1: 			End  { 29 02 }
0x514B3: 			Text Prompt: "PCI Express Root Port 6", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 7B 16 C9 07 93 16 }
0x514BB: 		End  { 29 02 }
0x514BD: 		SuppressIf  { 0A 82 }
0x514BF: 			EqIdVal QuestionId: 0x113B, Value: 0x0 { 12 86 3B 11 00 00 }
0x514C5: 				Not  { 17 02 }
0x514C7: 			End  { 29 02 }
0x514C9: 			Ref Prompt: "PCI Express Root Port 7", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAAD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2836 { 0F 0F 7C 16 92 16 AD 0A 00 00 FF FF 00 36 28 }
0x514D8: 		End  { 29 02 }
0x514DA: 		SuppressIf  { 0A 82 }
0x514DC: 			EqIdVal QuestionId: 0x113B, Value: 0x1 { 12 86 3B 11 01 00 }
0x514E2: 				Not  { 17 02 }
0x514E4: 			End  { 29 02 }
0x514E6: 			Text Prompt: "PCI Express Root Port 7", Help: "", Text: "Not present in this SKU" { 03 08 7C 16 C9 07 82 0E }
0x514EE: 		End  { 29 02 }
0x514F0: 		SuppressIf  { 0A 82 }
0x514F2: 			EqIdVal QuestionId: 0x113B, Value: 0x2 { 12 86 3B 11 02 00 }
0x514F8: 				Not  { 17 02 }
0x514FA: 			End  { 29 02 }
0x514FC: 			Text Prompt: "PCI Express Root Port 7", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 7C 16 C9 07 83 0E }
0x51504: 		End  { 29 02 }
0x51506: 		SuppressIf  { 0A 82 }
0x51508: 			EqIdVal QuestionId: 0x113B, Value: 0x3 { 12 86 3B 11 03 00 }
0x5150E: 				Not  { 17 02 }
0x51510: 			End  { 29 02 }
0x51512: 			Text Prompt: "PCI Express Root Port 7", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 7C 16 C9 07 93 16 }
0x5151A: 		End  { 29 02 }
0x5151C: 		SuppressIf  { 0A 82 }
0x5151E: 			EqIdVal QuestionId: 0x113A, Value: 0x0 { 12 86 3A 11 00 00 }
0x51524: 				Not  { 17 02 }
0x51526: 			End  { 29 02 }
0x51528: 			Ref Prompt: "PCI Express Root Port 8", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAAE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2837 { 0F 0F 7D 16 92 16 AE 0A 00 00 FF FF 00 37 28 }
0x51537: 		End  { 29 02 }
0x51539: 		SuppressIf  { 0A 82 }
0x5153B: 			EqIdVal QuestionId: 0x113A, Value: 0x1 { 12 86 3A 11 01 00 }
0x51541: 				Not  { 17 02 }
0x51543: 			End  { 29 02 }
0x51545: 			Text Prompt: "PCI Express Root Port 8", Help: "", Text: "Not present in this SKU" { 03 08 7D 16 C9 07 82 0E }
0x5154D: 		End  { 29 02 }
0x5154F: 		SuppressIf  { 0A 82 }
0x51551: 			EqIdVal QuestionId: 0x113A, Value: 0x2 { 12 86 3A 11 02 00 }
0x51557: 				Not  { 17 02 }
0x51559: 			End  { 29 02 }
0x5155B: 			Text Prompt: "PCI Express Root Port 8", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 7D 16 C9 07 83 0E }
0x51563: 		End  { 29 02 }
0x51565: 		SuppressIf  { 0A 82 }
0x51567: 			EqIdVal QuestionId: 0x113A, Value: 0x3 { 12 86 3A 11 03 00 }
0x5156D: 				Not  { 17 02 }
0x5156F: 			End  { 29 02 }
0x51571: 			Text Prompt: "PCI Express Root Port 8", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 7D 16 C9 07 93 16 }
0x51579: 		End  { 29 02 }
0x5157B: 		SuppressIf  { 0A 82 }
0x5157D: 			EqIdVal QuestionId: 0x1139, Value: 0x0 { 12 86 39 11 00 00 }
0x51583: 				Not  { 17 02 }
0x51585: 			End  { 29 02 }
0x51587: 			Ref Prompt: "PCI Express Root Port 9", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAAF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2838 { 0F 0F 7E 16 92 16 AF 0A 00 00 FF FF 00 38 28 }
0x51596: 		End  { 29 02 }
0x51598: 		SuppressIf  { 0A 82 }
0x5159A: 			EqIdVal QuestionId: 0x1139, Value: 0x1 { 12 86 39 11 01 00 }
0x515A0: 				Not  { 17 02 }
0x515A2: 			End  { 29 02 }
0x515A4: 			Text Prompt: "PCI Express Root Port 9", Help: "", Text: "Not present in this SKU" { 03 08 7E 16 C9 07 82 0E }
0x515AC: 		End  { 29 02 }
0x515AE: 		SuppressIf  { 0A 82 }
0x515B0: 			EqIdVal QuestionId: 0x1139, Value: 0x2 { 12 86 39 11 02 00 }
0x515B6: 				Not  { 17 02 }
0x515B8: 			End  { 29 02 }
0x515BA: 			Text Prompt: "PCI Express Root Port 9", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 7E 16 C9 07 83 0E }
0x515C2: 		End  { 29 02 }
0x515C4: 		SuppressIf  { 0A 82 }
0x515C6: 			EqIdVal QuestionId: 0x1139, Value: 0x3 { 12 86 39 11 03 00 }
0x515CC: 				Not  { 17 02 }
0x515CE: 			End  { 29 02 }
0x515D0: 			Text Prompt: "PCI Express Root Port 9", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 7E 16 C9 07 93 16 }
0x515D8: 		End  { 29 02 }
0x515DA: 		SuppressIf  { 0A 82 }
0x515DC: 			EqIdVal QuestionId: 0x1138, Value: 0x0 { 12 86 38 11 00 00 }
0x515E2: 				Not  { 17 02 }
0x515E4: 			End  { 29 02 }
0x515E6: 			Ref Prompt: "PCI Express Root Port 10", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB0, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2839 { 0F 0F 7F 16 92 16 B0 0A 00 00 FF FF 00 39 28 }
0x515F5: 		End  { 29 02 }
0x515F7: 		SuppressIf  { 0A 82 }
0x515F9: 			EqIdVal QuestionId: 0x1138, Value: 0x1 { 12 86 38 11 01 00 }
0x515FF: 				Not  { 17 02 }
0x51601: 			End  { 29 02 }
0x51603: 			Text Prompt: "PCI Express Root Port 10", Help: "", Text: "Not present in this SKU" { 03 08 7F 16 C9 07 82 0E }
0x5160B: 		End  { 29 02 }
0x5160D: 		SuppressIf  { 0A 82 }
0x5160F: 			EqIdVal QuestionId: 0x1138, Value: 0x2 { 12 86 38 11 02 00 }
0x51615: 				Not  { 17 02 }
0x51617: 			End  { 29 02 }
0x51619: 			Text Prompt: "PCI Express Root Port 10", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 7F 16 C9 07 83 0E }
0x51621: 		End  { 29 02 }
0x51623: 		SuppressIf  { 0A 82 }
0x51625: 			EqIdVal QuestionId: 0x1138, Value: 0x3 { 12 86 38 11 03 00 }
0x5162B: 				Not  { 17 02 }
0x5162D: 			End  { 29 02 }
0x5162F: 			Text Prompt: "PCI Express Root Port 10", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 7F 16 C9 07 93 16 }
0x51637: 		End  { 29 02 }
0x51639: 		SuppressIf  { 0A 82 }
0x5163B: 			EqIdVal QuestionId: 0x1137, Value: 0x0 { 12 86 37 11 00 00 }
0x51641: 				Not  { 17 02 }
0x51643: 			End  { 29 02 }
0x51645: 			Ref Prompt: "PCI Express Root Port 11", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x283A { 0F 0F 80 16 92 16 B1 0A 00 00 FF FF 00 3A 28 }
0x51654: 		End  { 29 02 }
0x51656: 		SuppressIf  { 0A 82 }
0x51658: 			EqIdVal QuestionId: 0x1137, Value: 0x1 { 12 86 37 11 01 00 }
0x5165E: 				Not  { 17 02 }
0x51660: 			End  { 29 02 }
0x51662: 			Text Prompt: "PCI Express Root Port 11", Help: "", Text: "Not present in this SKU" { 03 08 80 16 C9 07 82 0E }
0x5166A: 		End  { 29 02 }
0x5166C: 		SuppressIf  { 0A 82 }
0x5166E: 			EqIdVal QuestionId: 0x1137, Value: 0x2 { 12 86 37 11 02 00 }
0x51674: 				Not  { 17 02 }
0x51676: 			End  { 29 02 }
0x51678: 			Text Prompt: "PCI Express Root Port 11", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 80 16 C9 07 83 0E }
0x51680: 		End  { 29 02 }
0x51682: 		SuppressIf  { 0A 82 }
0x51684: 			EqIdVal QuestionId: 0x1137, Value: 0x3 { 12 86 37 11 03 00 }
0x5168A: 				Not  { 17 02 }
0x5168C: 			End  { 29 02 }
0x5168E: 			Text Prompt: "PCI Express Root Port 11", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 80 16 C9 07 93 16 }
0x51696: 		End  { 29 02 }
0x51698: 		SuppressIf  { 0A 82 }
0x5169A: 			EqIdVal QuestionId: 0x1136, Value: 0x0 { 12 86 36 11 00 00 }
0x516A0: 				Not  { 17 02 }
0x516A2: 			End  { 29 02 }
0x516A4: 			Ref Prompt: "PCI Express Root Port 12", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x283B { 0F 0F 81 16 92 16 B2 0A 00 00 FF FF 00 3B 28 }
0x516B3: 		End  { 29 02 }
0x516B5: 		SuppressIf  { 0A 82 }
0x516B7: 			EqIdVal QuestionId: 0x1136, Value: 0x1 { 12 86 36 11 01 00 }
0x516BD: 				Not  { 17 02 }
0x516BF: 			End  { 29 02 }
0x516C1: 			Text Prompt: "PCI Express Root Port 12", Help: "", Text: "Not present in this SKU" { 03 08 81 16 C9 07 82 0E }
0x516C9: 		End  { 29 02 }
0x516CB: 		SuppressIf  { 0A 82 }
0x516CD: 			EqIdVal QuestionId: 0x1136, Value: 0x2 { 12 86 36 11 02 00 }
0x516D3: 				Not  { 17 02 }
0x516D5: 			End  { 29 02 }
0x516D7: 			Text Prompt: "PCI Express Root Port 12", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 81 16 C9 07 83 0E }
0x516DF: 		End  { 29 02 }
0x516E1: 		SuppressIf  { 0A 82 }
0x516E3: 			EqIdVal QuestionId: 0x1136, Value: 0x3 { 12 86 36 11 03 00 }
0x516E9: 				Not  { 17 02 }
0x516EB: 			End  { 29 02 }
0x516ED: 			Text Prompt: "PCI Express Root Port 12", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 81 16 C9 07 93 16 }
0x516F5: 		End  { 29 02 }
0x516F7: 		SuppressIf  { 0A 82 }
0x516F9: 			EqIdVal QuestionId: 0x1135, Value: 0x0 { 12 86 35 11 00 00 }
0x516FF: 				Not  { 17 02 }
0x51701: 			End  { 29 02 }
0x51703: 			Ref Prompt: "PCI Express Root Port 13", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x283C { 0F 0F 82 16 92 16 B3 0A 00 00 FF FF 00 3C 28 }
0x51712: 		End  { 29 02 }
0x51714: 		SuppressIf  { 0A 82 }
0x51716: 			EqIdVal QuestionId: 0x1135, Value: 0x1 { 12 86 35 11 01 00 }
0x5171C: 				Not  { 17 02 }
0x5171E: 			End  { 29 02 }
0x51720: 			Text Prompt: "PCI Express Root Port 13", Help: "", Text: "Not present in this SKU" { 03 08 82 16 C9 07 82 0E }
0x51728: 		End  { 29 02 }
0x5172A: 		SuppressIf  { 0A 82 }
0x5172C: 			EqIdVal QuestionId: 0x1135, Value: 0x2 { 12 86 35 11 02 00 }
0x51732: 				Not  { 17 02 }
0x51734: 			End  { 29 02 }
0x51736: 			Text Prompt: "PCI Express Root Port 13", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 82 16 C9 07 83 0E }
0x5173E: 		End  { 29 02 }
0x51740: 		SuppressIf  { 0A 82 }
0x51742: 			EqIdVal QuestionId: 0x1135, Value: 0x3 { 12 86 35 11 03 00 }
0x51748: 				Not  { 17 02 }
0x5174A: 			End  { 29 02 }
0x5174C: 			Text Prompt: "PCI Express Root Port 13", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 82 16 C9 07 93 16 }
0x51754: 		End  { 29 02 }
0x51756: 		SuppressIf  { 0A 82 }
0x51758: 			EqIdVal QuestionId: 0x1134, Value: 0x0 { 12 86 34 11 00 00 }
0x5175E: 				Not  { 17 02 }
0x51760: 			End  { 29 02 }
0x51762: 			Ref Prompt: "PCI Express Root Port 14", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x283D { 0F 0F 83 16 92 16 B4 0A 00 00 FF FF 00 3D 28 }
0x51771: 		End  { 29 02 }
0x51773: 		SuppressIf  { 0A 82 }
0x51775: 			EqIdVal QuestionId: 0x1134, Value: 0x1 { 12 86 34 11 01 00 }
0x5177B: 				Not  { 17 02 }
0x5177D: 			End  { 29 02 }
0x5177F: 			Text Prompt: "PCI Express Root Port 14", Help: "", Text: "Not present in this SKU" { 03 08 83 16 C9 07 82 0E }
0x51787: 		End  { 29 02 }
0x51789: 		SuppressIf  { 0A 82 }
0x5178B: 			EqIdVal QuestionId: 0x1134, Value: 0x2 { 12 86 34 11 02 00 }
0x51791: 				Not  { 17 02 }
0x51793: 			End  { 29 02 }
0x51795: 			Text Prompt: "PCI Express Root Port 14", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 83 16 C9 07 83 0E }
0x5179D: 		End  { 29 02 }
0x5179F: 		SuppressIf  { 0A 82 }
0x517A1: 			EqIdVal QuestionId: 0x1134, Value: 0x3 { 12 86 34 11 03 00 }
0x517A7: 				Not  { 17 02 }
0x517A9: 			End  { 29 02 }
0x517AB: 			Text Prompt: "PCI Express Root Port 14", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 83 16 C9 07 93 16 }
0x517B3: 		End  { 29 02 }
0x517B5: 		SuppressIf  { 0A 82 }
0x517B7: 			EqIdVal QuestionId: 0x1133, Value: 0x0 { 12 86 33 11 00 00 }
0x517BD: 				Not  { 17 02 }
0x517BF: 			End  { 29 02 }
0x517C1: 			Ref Prompt: "PCI Express Root Port 15", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x283E { 0F 0F 84 16 92 16 B5 0A 00 00 FF FF 00 3E 28 }
0x517D0: 		End  { 29 02 }
0x517D2: 		SuppressIf  { 0A 82 }
0x517D4: 			EqIdVal QuestionId: 0x1133, Value: 0x1 { 12 86 33 11 01 00 }
0x517DA: 				Not  { 17 02 }
0x517DC: 			End  { 29 02 }
0x517DE: 			Text Prompt: "PCI Express Root Port 15", Help: "", Text: "Not present in this SKU" { 03 08 84 16 C9 07 82 0E }
0x517E6: 		End  { 29 02 }
0x517E8: 		SuppressIf  { 0A 82 }
0x517EA: 			EqIdVal QuestionId: 0x1133, Value: 0x2 { 12 86 33 11 02 00 }
0x517F0: 				Not  { 17 02 }
0x517F2: 			End  { 29 02 }
0x517F4: 			Text Prompt: "PCI Express Root Port 15", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 84 16 C9 07 83 0E }
0x517FC: 		End  { 29 02 }
0x517FE: 		SuppressIf  { 0A 82 }
0x51800: 			EqIdVal QuestionId: 0x1133, Value: 0x3 { 12 86 33 11 03 00 }
0x51806: 				Not  { 17 02 }
0x51808: 			End  { 29 02 }
0x5180A: 			Text Prompt: "PCI Express Root Port 15", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 84 16 C9 07 93 16 }
0x51812: 		End  { 29 02 }
0x51814: 		SuppressIf  { 0A 82 }
0x51816: 			EqIdVal QuestionId: 0x1132, Value: 0x0 { 12 86 32 11 00 00 }
0x5181C: 				Not  { 17 02 }
0x5181E: 			End  { 29 02 }
0x51820: 			Ref Prompt: "PCI Express Root Port 16", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x283F { 0F 0F 85 16 92 16 B6 0A 00 00 FF FF 00 3F 28 }
0x5182F: 		End  { 29 02 }
0x51831: 		SuppressIf  { 0A 82 }
0x51833: 			EqIdVal QuestionId: 0x1132, Value: 0x1 { 12 86 32 11 01 00 }
0x51839: 				Not  { 17 02 }
0x5183B: 			End  { 29 02 }
0x5183D: 			Text Prompt: "PCI Express Root Port 16", Help: "", Text: "Not present in this SKU" { 03 08 85 16 C9 07 82 0E }
0x51845: 		End  { 29 02 }
0x51847: 		SuppressIf  { 0A 82 }
0x51849: 			EqIdVal QuestionId: 0x1132, Value: 0x2 { 12 86 32 11 02 00 }
0x5184F: 				Not  { 17 02 }
0x51851: 			End  { 29 02 }
0x51853: 			Text Prompt: "PCI Express Root Port 16", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 85 16 C9 07 83 0E }
0x5185B: 		End  { 29 02 }
0x5185D: 		SuppressIf  { 0A 82 }
0x5185F: 			EqIdVal QuestionId: 0x1132, Value: 0x3 { 12 86 32 11 03 00 }
0x51865: 				Not  { 17 02 }
0x51867: 			End  { 29 02 }
0x51869: 			Text Prompt: "PCI Express Root Port 16", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 85 16 C9 07 93 16 }
0x51871: 		End  { 29 02 }
0x51873: 		SuppressIf  { 0A 82 }
0x51875: 			EqIdVal QuestionId: 0x1131, Value: 0x0 { 12 86 31 11 00 00 }
0x5187B: 				Not  { 17 02 }
0x5187D: 			End  { 29 02 }
0x5187F: 			Ref Prompt: "PCI Express Root Port 17", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2840 { 0F 0F 86 16 92 16 B7 0A 00 00 FF FF 00 40 28 }
0x5188E: 		End  { 29 02 }
0x51890: 		SuppressIf  { 0A 82 }
0x51892: 			EqIdVal QuestionId: 0x1131, Value: 0x1 { 12 86 31 11 01 00 }
0x51898: 				Not  { 17 02 }
0x5189A: 			End  { 29 02 }
0x5189C: 			Text Prompt: "PCI Express Root Port 17", Help: "", Text: "Not present in this SKU" { 03 08 86 16 C9 07 82 0E }
0x518A4: 		End  { 29 02 }
0x518A6: 		SuppressIf  { 0A 82 }
0x518A8: 			EqIdVal QuestionId: 0x1131, Value: 0x2 { 12 86 31 11 02 00 }
0x518AE: 				Not  { 17 02 }
0x518B0: 			End  { 29 02 }
0x518B2: 			Text Prompt: "PCI Express Root Port 17", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 86 16 C9 07 83 0E }
0x518BA: 		End  { 29 02 }
0x518BC: 		SuppressIf  { 0A 82 }
0x518BE: 			EqIdVal QuestionId: 0x1131, Value: 0x3 { 12 86 31 11 03 00 }
0x518C4: 				Not  { 17 02 }
0x518C6: 			End  { 29 02 }
0x518C8: 			Text Prompt: "PCI Express Root Port 17", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 86 16 C9 07 93 16 }
0x518D0: 		End  { 29 02 }
0x518D2: 		SuppressIf  { 0A 82 }
0x518D4: 			EqIdVal QuestionId: 0x1130, Value: 0x0 { 12 86 30 11 00 00 }
0x518DA: 				Not  { 17 02 }
0x518DC: 			End  { 29 02 }
0x518DE: 			Ref Prompt: "PCI Express Root Port 18", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2841 { 0F 0F 87 16 92 16 B8 0A 00 00 FF FF 00 41 28 }
0x518ED: 		End  { 29 02 }
0x518EF: 		SuppressIf  { 0A 82 }
0x518F1: 			EqIdVal QuestionId: 0x1130, Value: 0x1 { 12 86 30 11 01 00 }
0x518F7: 				Not  { 17 02 }
0x518F9: 			End  { 29 02 }
0x518FB: 			Text Prompt: "PCI Express Root Port 18", Help: "", Text: "Not present in this SKU" { 03 08 87 16 C9 07 82 0E }
0x51903: 		End  { 29 02 }
0x51905: 		SuppressIf  { 0A 82 }
0x51907: 			EqIdVal QuestionId: 0x1130, Value: 0x2 { 12 86 30 11 02 00 }
0x5190D: 				Not  { 17 02 }
0x5190F: 			End  { 29 02 }
0x51911: 			Text Prompt: "PCI Express Root Port 18", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 87 16 C9 07 83 0E }
0x51919: 		End  { 29 02 }
0x5191B: 		SuppressIf  { 0A 82 }
0x5191D: 			EqIdVal QuestionId: 0x1130, Value: 0x3 { 12 86 30 11 03 00 }
0x51923: 				Not  { 17 02 }
0x51925: 			End  { 29 02 }
0x51927: 			Text Prompt: "PCI Express Root Port 18", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 87 16 C9 07 93 16 }
0x5192F: 		End  { 29 02 }
0x51931: 		SuppressIf  { 0A 82 }
0x51933: 			EqIdVal QuestionId: 0x112F, Value: 0x0 { 12 86 2F 11 00 00 }
0x51939: 				Not  { 17 02 }
0x5193B: 			End  { 29 02 }
0x5193D: 			Ref Prompt: "PCI Express Root Port 19", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAB9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2842 { 0F 0F 88 16 92 16 B9 0A 00 00 FF FF 00 42 28 }
0x5194C: 		End  { 29 02 }
0x5194E: 		SuppressIf  { 0A 82 }
0x51950: 			EqIdVal QuestionId: 0x112F, Value: 0x1 { 12 86 2F 11 01 00 }
0x51956: 				Not  { 17 02 }
0x51958: 			End  { 29 02 }
0x5195A: 			Text Prompt: "PCI Express Root Port 19", Help: "", Text: "Not present in this SKU" { 03 08 88 16 C9 07 82 0E }
0x51962: 		End  { 29 02 }
0x51964: 		SuppressIf  { 0A 82 }
0x51966: 			EqIdVal QuestionId: 0x112F, Value: 0x2 { 12 86 2F 11 02 00 }
0x5196C: 				Not  { 17 02 }
0x5196E: 			End  { 29 02 }
0x51970: 			Text Prompt: "PCI Express Root Port 19", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 88 16 C9 07 83 0E }
0x51978: 		End  { 29 02 }
0x5197A: 		SuppressIf  { 0A 82 }
0x5197C: 			EqIdVal QuestionId: 0x112F, Value: 0x3 { 12 86 2F 11 03 00 }
0x51982: 				Not  { 17 02 }
0x51984: 			End  { 29 02 }
0x51986: 			Text Prompt: "PCI Express Root Port 19", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 88 16 C9 07 93 16 }
0x5198E: 		End  { 29 02 }
0x51990: 		SuppressIf  { 0A 82 }
0x51992: 			EqIdVal QuestionId: 0x112E, Value: 0x0 { 12 86 2E 11 00 00 }
0x51998: 				Not  { 17 02 }
0x5199A: 			End  { 29 02 }
0x5199C: 			Ref Prompt: "PCI Express Root Port 20", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xABA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2843 { 0F 0F 89 16 92 16 BA 0A 00 00 FF FF 00 43 28 }
0x519AB: 		End  { 29 02 }
0x519AD: 		SuppressIf  { 0A 82 }
0x519AF: 			EqIdVal QuestionId: 0x112E, Value: 0x1 { 12 86 2E 11 01 00 }
0x519B5: 				Not  { 17 02 }
0x519B7: 			End  { 29 02 }
0x519B9: 			Text Prompt: "PCI Express Root Port 20", Help: "", Text: "Not present in this SKU" { 03 08 89 16 C9 07 82 0E }
0x519C1: 		End  { 29 02 }
0x519C3: 		SuppressIf  { 0A 82 }
0x519C5: 			EqIdVal QuestionId: 0x112E, Value: 0x2 { 12 86 2E 11 02 00 }
0x519CB: 				Not  { 17 02 }
0x519CD: 			End  { 29 02 }
0x519CF: 			Text Prompt: "PCI Express Root Port 20", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 89 16 C9 07 83 0E }
0x519D7: 		End  { 29 02 }
0x519D9: 		SuppressIf  { 0A 82 }
0x519DB: 			EqIdVal QuestionId: 0x112E, Value: 0x3 { 12 86 2E 11 03 00 }
0x519E1: 				Not  { 17 02 }
0x519E3: 			End  { 29 02 }
0x519E5: 			Text Prompt: "PCI Express Root Port 20", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 89 16 C9 07 93 16 }
0x519ED: 		End  { 29 02 }
0x519EF: 		SuppressIf  { 0A 82 }
0x519F1: 			EqIdVal QuestionId: 0x112D, Value: 0x0 { 12 86 2D 11 00 00 }
0x519F7: 				Not  { 17 02 }
0x519F9: 			End  { 29 02 }
0x519FB: 			Ref Prompt: "PCI Express Root Port 21", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xABB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2844 { 0F 0F 8A 16 92 16 BB 0A 00 00 FF FF 00 44 28 }
0x51A0A: 		End  { 29 02 }
0x51A0C: 		SuppressIf  { 0A 82 }
0x51A0E: 			EqIdVal QuestionId: 0x112D, Value: 0x1 { 12 86 2D 11 01 00 }
0x51A14: 				Not  { 17 02 }
0x51A16: 			End  { 29 02 }
0x51A18: 			Text Prompt: "PCI Express Root Port 21", Help: "", Text: "Not present in this SKU" { 03 08 8A 16 C9 07 82 0E }
0x51A20: 		End  { 29 02 }
0x51A22: 		SuppressIf  { 0A 82 }
0x51A24: 			EqIdVal QuestionId: 0x112D, Value: 0x2 { 12 86 2D 11 02 00 }
0x51A2A: 				Not  { 17 02 }
0x51A2C: 			End  { 29 02 }
0x51A2E: 			Text Prompt: "PCI Express Root Port 21", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 8A 16 C9 07 83 0E }
0x51A36: 		End  { 29 02 }
0x51A38: 		SuppressIf  { 0A 82 }
0x51A3A: 			EqIdVal QuestionId: 0x112D, Value: 0x3 { 12 86 2D 11 03 00 }
0x51A40: 				Not  { 17 02 }
0x51A42: 			End  { 29 02 }
0x51A44: 			Text Prompt: "PCI Express Root Port 21", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 8A 16 C9 07 93 16 }
0x51A4C: 		End  { 29 02 }
0x51A4E: 		SuppressIf  { 0A 82 }
0x51A50: 			EqIdVal QuestionId: 0x112C, Value: 0x0 { 12 86 2C 11 00 00 }
0x51A56: 				Not  { 17 02 }
0x51A58: 			End  { 29 02 }
0x51A5A: 			Ref Prompt: "PCI Express Root Port 22", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xABC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2845 { 0F 0F 8B 16 92 16 BC 0A 00 00 FF FF 00 45 28 }
0x51A69: 		End  { 29 02 }
0x51A6B: 		SuppressIf  { 0A 82 }
0x51A6D: 			EqIdVal QuestionId: 0x112C, Value: 0x1 { 12 86 2C 11 01 00 }
0x51A73: 				Not  { 17 02 }
0x51A75: 			End  { 29 02 }
0x51A77: 			Text Prompt: "PCI Express Root Port 22", Help: "", Text: "Not present in this SKU" { 03 08 8B 16 C9 07 82 0E }
0x51A7F: 		End  { 29 02 }
0x51A81: 		SuppressIf  { 0A 82 }
0x51A83: 			EqIdVal QuestionId: 0x112C, Value: 0x2 { 12 86 2C 11 02 00 }
0x51A89: 				Not  { 17 02 }
0x51A8B: 			End  { 29 02 }
0x51A8D: 			Text Prompt: "PCI Express Root Port 22", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 8B 16 C9 07 83 0E }
0x51A95: 		End  { 29 02 }
0x51A97: 		SuppressIf  { 0A 82 }
0x51A99: 			EqIdVal QuestionId: 0x112C, Value: 0x3 { 12 86 2C 11 03 00 }
0x51A9F: 				Not  { 17 02 }
0x51AA1: 			End  { 29 02 }
0x51AA3: 			Text Prompt: "PCI Express Root Port 22", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 8B 16 C9 07 93 16 }
0x51AAB: 		End  { 29 02 }
0x51AAD: 		SuppressIf  { 0A 82 }
0x51AAF: 			EqIdVal QuestionId: 0x112B, Value: 0x0 { 12 86 2B 11 00 00 }
0x51AB5: 				Not  { 17 02 }
0x51AB7: 			End  { 29 02 }
0x51AB9: 			Ref Prompt: "PCI Express Root Port 23", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xABD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2846 { 0F 0F 8C 16 92 16 BD 0A 00 00 FF FF 00 46 28 }
0x51AC8: 		End  { 29 02 }
0x51ACA: 		SuppressIf  { 0A 82 }
0x51ACC: 			EqIdVal QuestionId: 0x112B, Value: 0x1 { 12 86 2B 11 01 00 }
0x51AD2: 				Not  { 17 02 }
0x51AD4: 			End  { 29 02 }
0x51AD6: 			Text Prompt: "PCI Express Root Port 23", Help: "", Text: "Not present in this SKU" { 03 08 8C 16 C9 07 82 0E }
0x51ADE: 		End  { 29 02 }
0x51AE0: 		SuppressIf  { 0A 82 }
0x51AE2: 			EqIdVal QuestionId: 0x112B, Value: 0x2 { 12 86 2B 11 02 00 }
0x51AE8: 				Not  { 17 02 }
0x51AEA: 			End  { 29 02 }
0x51AEC: 			Text Prompt: "PCI Express Root Port 23", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 8C 16 C9 07 83 0E }
0x51AF4: 		End  { 29 02 }
0x51AF6: 		SuppressIf  { 0A 82 }
0x51AF8: 			EqIdVal QuestionId: 0x112B, Value: 0x3 { 12 86 2B 11 03 00 }
0x51AFE: 				Not  { 17 02 }
0x51B00: 			End  { 29 02 }
0x51B02: 			Text Prompt: "PCI Express Root Port 23", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 8C 16 C9 07 93 16 }
0x51B0A: 		End  { 29 02 }
0x51B0C: 		SuppressIf  { 0A 82 }
0x51B0E: 			EqIdVal QuestionId: 0x112A, Value: 0x0 { 12 86 2A 11 00 00 }
0x51B14: 				Not  { 17 02 }
0x51B16: 			End  { 29 02 }
0x51B18: 			Ref Prompt: "PCI Express Root Port 24", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xABE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2847 { 0F 0F 8D 16 92 16 BE 0A 00 00 FF FF 00 47 28 }
0x51B27: 		End  { 29 02 }
0x51B29: 		SuppressIf  { 0A 82 }
0x51B2B: 			EqIdVal QuestionId: 0x112A, Value: 0x1 { 12 86 2A 11 01 00 }
0x51B31: 				Not  { 17 02 }
0x51B33: 			End  { 29 02 }
0x51B35: 			Text Prompt: "PCI Express Root Port 24", Help: "", Text: "Not present in this SKU" { 03 08 8D 16 C9 07 82 0E }
0x51B3D: 		End  { 29 02 }
0x51B3F: 		SuppressIf  { 0A 82 }
0x51B41: 			EqIdVal QuestionId: 0x112A, Value: 0x2 { 12 86 2A 11 02 00 }
0x51B47: 				Not  { 17 02 }
0x51B49: 			End  { 29 02 }
0x51B4B: 			Text Prompt: "PCI Express Root Port 24", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 8D 16 C9 07 83 0E }
0x51B53: 		End  { 29 02 }
0x51B55: 		SuppressIf  { 0A 82 }
0x51B57: 			EqIdVal QuestionId: 0x112A, Value: 0x3 { 12 86 2A 11 03 00 }
0x51B5D: 				Not  { 17 02 }
0x51B5F: 			End  { 29 02 }
0x51B61: 			Text Prompt: "PCI Express Root Port 24", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 8D 16 C9 07 93 16 }
0x51B69: 		End  { 29 02 }
0x51B6B: 		SuppressIf  { 0A 82 }
0x51B6D: 			EqIdVal QuestionId: 0x1129, Value: 0x0 { 12 86 29 11 00 00 }
0x51B73: 				Not  { 17 02 }
0x51B75: 			End  { 29 02 }
0x51B77: 			Ref Prompt: "PCI Express Root Port 25", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xABF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2848 { 0F 0F 8E 16 92 16 BF 0A 00 00 FF FF 00 48 28 }
0x51B86: 		End  { 29 02 }
0x51B88: 		SuppressIf  { 0A 82 }
0x51B8A: 			EqIdVal QuestionId: 0x1129, Value: 0x1 { 12 86 29 11 01 00 }
0x51B90: 				Not  { 17 02 }
0x51B92: 			End  { 29 02 }
0x51B94: 			Text Prompt: "PCI Express Root Port 25", Help: "", Text: "Not present in this SKU" { 03 08 8E 16 C9 07 82 0E }
0x51B9C: 		End  { 29 02 }
0x51B9E: 		SuppressIf  { 0A 82 }
0x51BA0: 			EqIdVal QuestionId: 0x1129, Value: 0x2 { 12 86 29 11 02 00 }
0x51BA6: 				Not  { 17 02 }
0x51BA8: 			End  { 29 02 }
0x51BAA: 			Text Prompt: "PCI Express Root Port 25", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 8E 16 C9 07 83 0E }
0x51BB2: 		End  { 29 02 }
0x51BB4: 		SuppressIf  { 0A 82 }
0x51BB6: 			EqIdVal QuestionId: 0x1129, Value: 0x3 { 12 86 29 11 03 00 }
0x51BBC: 				Not  { 17 02 }
0x51BBE: 			End  { 29 02 }
0x51BC0: 			Text Prompt: "PCI Express Root Port 25", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 8E 16 C9 07 93 16 }
0x51BC8: 		End  { 29 02 }
0x51BCA: 		SuppressIf  { 0A 82 }
0x51BCC: 			EqIdVal QuestionId: 0x1128, Value: 0x0 { 12 86 28 11 00 00 }
0x51BD2: 				Not  { 17 02 }
0x51BD4: 			End  { 29 02 }
0x51BD6: 			Ref Prompt: "PCI Express Root Port 26", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAC0, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2849 { 0F 0F 8F 16 92 16 C0 0A 00 00 FF FF 00 49 28 }
0x51BE5: 		End  { 29 02 }
0x51BE7: 		SuppressIf  { 0A 82 }
0x51BE9: 			EqIdVal QuestionId: 0x1128, Value: 0x1 { 12 86 28 11 01 00 }
0x51BEF: 				Not  { 17 02 }
0x51BF1: 			End  { 29 02 }
0x51BF3: 			Text Prompt: "PCI Express Root Port 26", Help: "", Text: "Not present in this SKU" { 03 08 8F 16 C9 07 82 0E }
0x51BFB: 		End  { 29 02 }
0x51BFD: 		SuppressIf  { 0A 82 }
0x51BFF: 			EqIdVal QuestionId: 0x1128, Value: 0x2 { 12 86 28 11 02 00 }
0x51C05: 				Not  { 17 02 }
0x51C07: 			End  { 29 02 }
0x51C09: 			Text Prompt: "PCI Express Root Port 26", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 8F 16 C9 07 83 0E }
0x51C11: 		End  { 29 02 }
0x51C13: 		SuppressIf  { 0A 82 }
0x51C15: 			EqIdVal QuestionId: 0x1128, Value: 0x3 { 12 86 28 11 03 00 }
0x51C1B: 				Not  { 17 02 }
0x51C1D: 			End  { 29 02 }
0x51C1F: 			Text Prompt: "PCI Express Root Port 26", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 8F 16 C9 07 93 16 }
0x51C27: 		End  { 29 02 }
0x51C29: 		SuppressIf  { 0A 82 }
0x51C2B: 			EqIdVal QuestionId: 0x1127, Value: 0x0 { 12 86 27 11 00 00 }
0x51C31: 				Not  { 17 02 }
0x51C33: 			End  { 29 02 }
0x51C35: 			Ref Prompt: "PCI Express Root Port 27", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAC1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x284A { 0F 0F 90 16 92 16 C1 0A 00 00 FF FF 00 4A 28 }
0x51C44: 		End  { 29 02 }
0x51C46: 		SuppressIf  { 0A 82 }
0x51C48: 			EqIdVal QuestionId: 0x1127, Value: 0x1 { 12 86 27 11 01 00 }
0x51C4E: 				Not  { 17 02 }
0x51C50: 			End  { 29 02 }
0x51C52: 			Text Prompt: "PCI Express Root Port 27", Help: "", Text: "Not present in this SKU" { 03 08 90 16 C9 07 82 0E }
0x51C5A: 		End  { 29 02 }
0x51C5C: 		SuppressIf  { 0A 82 }
0x51C5E: 			EqIdVal QuestionId: 0x1127, Value: 0x2 { 12 86 27 11 02 00 }
0x51C64: 				Not  { 17 02 }
0x51C66: 			End  { 29 02 }
0x51C68: 			Text Prompt: "PCI Express Root Port 27", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 90 16 C9 07 83 0E }
0x51C70: 		End  { 29 02 }
0x51C72: 		SuppressIf  { 0A 82 }
0x51C74: 			EqIdVal QuestionId: 0x1127, Value: 0x3 { 12 86 27 11 03 00 }
0x51C7A: 				Not  { 17 02 }
0x51C7C: 			End  { 29 02 }
0x51C7E: 			Text Prompt: "PCI Express Root Port 27", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 90 16 C9 07 93 16 }
0x51C86: 		End  { 29 02 }
0x51C88: 		SuppressIf  { 0A 82 }
0x51C8A: 			EqIdVal QuestionId: 0x1126, Value: 0x0 { 12 86 26 11 00 00 }
0x51C90: 				Not  { 17 02 }
0x51C92: 			End  { 29 02 }
0x51C94: 			Ref Prompt: "PCI Express Root Port 28", Help: "PCI Express Root Port Settings.", QuestionFlags: 0x0, QuestionId: 0xAC2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x284B { 0F 0F 91 16 92 16 C2 0A 00 00 FF FF 00 4B 28 }
0x51CA3: 		End  { 29 02 }
0x51CA5: 		SuppressIf  { 0A 82 }
0x51CA7: 			EqIdVal QuestionId: 0x1126, Value: 0x1 { 12 86 26 11 01 00 }
0x51CAD: 				Not  { 17 02 }
0x51CAF: 			End  { 29 02 }
0x51CB1: 			Text Prompt: "PCI Express Root Port 28", Help: "", Text: "Not present in this SKU" { 03 08 91 16 C9 07 82 0E }
0x51CB9: 		End  { 29 02 }
0x51CBB: 		SuppressIf  { 0A 82 }
0x51CBD: 			EqIdVal QuestionId: 0x1126, Value: 0x2 { 12 86 26 11 02 00 }
0x51CC3: 				Not  { 17 02 }
0x51CC5: 			End  { 29 02 }
0x51CC7: 			Text Prompt: "PCI Express Root Port 28", Help: "", Text: "Shadowed by x2/x4 port" { 03 08 91 16 C9 07 83 0E }
0x51CCF: 		End  { 29 02 }
0x51CD1: 		SuppressIf  { 0A 82 }
0x51CD3: 			EqIdVal QuestionId: 0x1126, Value: 0x3 { 12 86 26 11 03 00 }
0x51CD9: 				Not  { 17 02 }
0x51CDB: 			End  { 29 02 }
0x51CDD: 			Text Prompt: "PCI Express Root Port 28", Help: "", Text: "Lane configured as USB/SATA/UFS" { 03 08 91 16 C9 07 93 16 }
0x51CE5: 		End  { 29 02 }
0x51CE7: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x51CEE: 		End  { 29 02 }
0x51CF0: 		Ref Prompt: "PCIE clocks", Help: "PCIE clocks", QuestionFlags: 0x0, QuestionId: 0xAC3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x284C { 0F 0F 82 18 83 18 C3 0A 00 00 FF FF 00 4C 28 }
0x51CFF: 	End  { 29 02 }
0x51D01: 	Form FormId: 0x282D, Title: "USB Configuration" { 01 86 2D 28 46 16 }
0x51D07: 		Subtitle Prompt: "USB Configuration", Help: "", Flags: 0x0 { 02 87 46 16 00 00 00 }
0x51D0E: 		End  { 29 02 }
0x51D10: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x51D17: 		End  { 29 02 }
0x51D19: 		OneOf Prompt: "xDCI Support", Help: "Enable/Disable xDCI (USB OTG Device).", QuestionFlags: 0x10, QuestionId: 0xAC4, VarStoreId: 0x6, VarOffset: 0x47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 16 75 16 C4 0A 06 00 47 00 10 10 00 01 00 }
0x51D2A: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x51D30: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51D37: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51D3E: 		End  { 29 02 }
0x51D40: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x51D47: 		End  { 29 02 }
0x51D49: 		OneOf Prompt: "USB PDO Programming", Help: "Select 'Enabled' if Port Disable Override functionality is used.", QuestionFlags: 0x10, QuestionId: 0xAC5, VarStoreId: 0x6, VarOffset: 0x42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4A 16 4B 16 C5 0A 06 00 42 00 10 10 00 01 00 }
0x51D5A: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51D61: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51D68: 		End  { 29 02 }
0x51D6A: 		OneOf Prompt: "USB Overcurrent", Help: "Select 'Disabled' for pin-based debug. If pin-based debug is enabled but USB overcurrent is not disabled, USB DbC does not work.", QuestionFlags: 0x10, QuestionId: 0xAC6, VarStoreId: 0x6, VarOffset: 0x43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4C 16 4D 16 C6 0A 06 00 43 00 10 10 00 01 00 }
0x51D7B: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x51D82: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51D89: 		End  { 29 02 }
0x51D8B: 		OneOf Prompt: "USB Overcurrent Lock", Help: "Select 'Enabled' if Overcurrent functionality is used. Enabling this will make xHCI controller consume the Overcurrent mapping data", QuestionFlags: 0x10, QuestionId: 0xAC7, VarStoreId: 0x6, VarOffset: 0x44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 16 4F 16 C7 0A 06 00 44 00 10 10 00 01 00 }
0x51D9C: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x51DA3: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x51DAA: 		End  { 29 02 }
0x51DAC: 		OneOf Prompt: "USB Audio Offload", Help: "Enable/Disable USB Audio Offload functionality", QuestionFlags: 0x10, QuestionId: 0xAC8, VarStoreId: 0x6, VarOffset: 0x783, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 50 16 51 16 C8 0A 06 00 83 07 10 10 00 01 00 }
0x51DBD: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51DC4: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51DCB: 		End  { 29 02 }
0x51DCD: 		OneOf Prompt: "Enable HSII on xHCI", Help: "Enable/Disable HSII feature. It may lead to increased power consumption.", QuestionFlags: 0x10, QuestionId: 0xAC9, VarStoreId: 0x6, VarOffset: 0x7F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 54 16 55 16 C9 0A 06 00 F4 07 10 10 00 01 00 }
0x51DDE: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51DE5: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51DEC: 		End  { 29 02 }
0x51DEE: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x51DF5: 		End  { 29 02 }
0x51DF7: 		OneOf Prompt: "USB Port Disable Override", Help: "Selectively Enable/Disable the corresponding USB port from reporting a Device Connection to the controller.", QuestionFlags: 0x10, QuestionId: 0xACA, VarStoreId: 0x6, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 16 59 16 CA 0A 06 00 27 00 10 10 00 01 00 }
0x51E08: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x51E0E: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x51E15: 			OneOfOption Option: "Select Per-Pin" Value: 1 { 09 07 5A 16 00 00 01 }
0x51E1C: 		End  { 29 02 }
0x51E1E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x51E25: 		End  { 29 02 }
0x51E27: 		SuppressIf  { 0A 82 }
0x51E29: 			EqIdVal QuestionId: 0xACA, Value: 0x0 { 12 06 CA 0A 00 00 }
0x51E2F: 			SuppressIf  { 0A 82 }
0x51E31: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51E35: 					Uint8 Value: 0x0 { 42 03 00 }
0x51E38: 					LessEqual  { 34 02 }
0x51E3A: 				End  { 29 02 }
0x51E3C: 				OneOf Prompt: "USB SS Physical Connector #0", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xACB, VarStoreId: 0x6, VarOffset: 0x38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5B 16 73 16 CB 0A 06 00 38 00 10 10 00 01 00 }
0x51E4D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51E54: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51E5B: 				End  { 29 02 }
0x51E5D: 			End  { 29 02 }
0x51E5F: 			SuppressIf  { 0A 82 }
0x51E61: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51E65: 					Uint8 Value: 0x1 { 42 03 01 }
0x51E68: 					LessEqual  { 34 02 }
0x51E6A: 				End  { 29 02 }
0x51E6C: 				OneOf Prompt: "USB SS Physical Connector #1", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xACC, VarStoreId: 0x6, VarOffset: 0x39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5C 16 73 16 CC 0A 06 00 39 00 10 10 00 01 00 }
0x51E7D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51E84: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51E8B: 				End  { 29 02 }
0x51E8D: 			End  { 29 02 }
0x51E8F: 			SuppressIf  { 0A 82 }
0x51E91: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51E95: 					Uint8 Value: 0x2 { 42 03 02 }
0x51E98: 					LessEqual  { 34 02 }
0x51E9A: 				End  { 29 02 }
0x51E9C: 				OneOf Prompt: "USB SS Physical Connector #2", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xACD, VarStoreId: 0x6, VarOffset: 0x3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5D 16 73 16 CD 0A 06 00 3A 00 10 10 00 01 00 }
0x51EAD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51EB4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51EBB: 				End  { 29 02 }
0x51EBD: 			End  { 29 02 }
0x51EBF: 			SuppressIf  { 0A 82 }
0x51EC1: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51EC5: 					Uint8 Value: 0x3 { 42 03 03 }
0x51EC8: 					LessEqual  { 34 02 }
0x51ECA: 				End  { 29 02 }
0x51ECC: 				OneOf Prompt: "USB SS Physical Connector #3", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xACE, VarStoreId: 0x6, VarOffset: 0x3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5E 16 73 16 CE 0A 06 00 3B 00 10 10 00 01 00 }
0x51EDD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51EE4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51EEB: 				End  { 29 02 }
0x51EED: 			End  { 29 02 }
0x51EEF: 			SuppressIf  { 0A 82 }
0x51EF1: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51EF5: 					Uint8 Value: 0x4 { 42 03 04 }
0x51EF8: 					LessEqual  { 34 02 }
0x51EFA: 				End  { 29 02 }
0x51EFC: 				OneOf Prompt: "USB SS Physical Connector #4", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xACF, VarStoreId: 0x6, VarOffset: 0x3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5F 16 73 16 CF 0A 06 00 3C 00 10 10 00 01 00 }
0x51F0D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51F14: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51F1B: 				End  { 29 02 }
0x51F1D: 			End  { 29 02 }
0x51F1F: 			SuppressIf  { 0A 82 }
0x51F21: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51F25: 					Uint8 Value: 0x5 { 42 03 05 }
0x51F28: 					LessEqual  { 34 02 }
0x51F2A: 				End  { 29 02 }
0x51F2C: 				OneOf Prompt: "USB SS Physical Connector #5", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD0, VarStoreId: 0x6, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 60 16 73 16 D0 0A 06 00 3D 00 10 10 00 01 00 }
0x51F3D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51F44: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51F4B: 				End  { 29 02 }
0x51F4D: 			End  { 29 02 }
0x51F4F: 			SuppressIf  { 0A 82 }
0x51F51: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51F55: 					Uint8 Value: 0x6 { 42 03 06 }
0x51F58: 					LessEqual  { 34 02 }
0x51F5A: 				End  { 29 02 }
0x51F5C: 				OneOf Prompt: "USB SS Physical Connector #6", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD1, VarStoreId: 0x6, VarOffset: 0x3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 16 73 16 D1 0A 06 00 3E 00 10 10 00 01 00 }
0x51F6D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51F74: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51F7B: 				End  { 29 02 }
0x51F7D: 			End  { 29 02 }
0x51F7F: 			SuppressIf  { 0A 82 }
0x51F81: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51F85: 					Uint8 Value: 0x7 { 42 03 07 }
0x51F88: 					LessEqual  { 34 02 }
0x51F8A: 				End  { 29 02 }
0x51F8C: 				OneOf Prompt: "USB SS Physical Connector #7", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD2, VarStoreId: 0x6, VarOffset: 0x3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 62 16 73 16 D2 0A 06 00 3F 00 10 10 00 01 00 }
0x51F9D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51FA4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51FAB: 				End  { 29 02 }
0x51FAD: 			End  { 29 02 }
0x51FAF: 			SuppressIf  { 0A 82 }
0x51FB1: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51FB5: 					Uint8 Value: 0x8 { 42 03 08 }
0x51FB8: 					LessEqual  { 34 02 }
0x51FBA: 				End  { 29 02 }
0x51FBC: 				OneOf Prompt: "USB SS Physical Connector #8", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD3, VarStoreId: 0x6, VarOffset: 0x40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 16 73 16 D3 0A 06 00 40 00 10 10 00 01 00 }
0x51FCD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x51FD4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x51FDB: 				End  { 29 02 }
0x51FDD: 			End  { 29 02 }
0x51FDF: 			SuppressIf  { 0A 82 }
0x51FE1: 				QuestionRef1 QuestionId: 0x1125 { 40 84 25 11 }
0x51FE5: 					Uint8 Value: 0x9 { 42 03 09 }
0x51FE8: 					LessEqual  { 34 02 }
0x51FEA: 				End  { 29 02 }
0x51FEC: 				OneOf Prompt: "USB SS Physical Connector #9", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD4, VarStoreId: 0x6, VarOffset: 0x41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 64 16 73 16 D4 0A 06 00 41 00 10 10 00 01 00 }
0x51FFD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52004: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5200B: 				End  { 29 02 }
0x5200D: 			End  { 29 02 }
0x5200F: 			SuppressIf  { 0A 82 }
0x52011: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52015: 					Uint8 Value: 0x0 { 42 03 00 }
0x52018: 					LessEqual  { 34 02 }
0x5201A: 				End  { 29 02 }
0x5201C: 				OneOf Prompt: "USB HS Physical Connector #0", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD5, VarStoreId: 0x6, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 16 73 16 D5 0A 06 00 28 00 10 10 00 01 00 }
0x5202D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52034: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5203B: 				End  { 29 02 }
0x5203D: 			End  { 29 02 }
0x5203F: 			SuppressIf  { 0A 82 }
0x52041: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52045: 					Uint8 Value: 0x1 { 42 03 01 }
0x52048: 					LessEqual  { 34 02 }
0x5204A: 				End  { 29 02 }
0x5204C: 				OneOf Prompt: "USB HS Physical Connector #1", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD6, VarStoreId: 0x6, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 66 16 73 16 D6 0A 06 00 29 00 10 10 00 01 00 }
0x5205D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52064: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5206B: 				End  { 29 02 }
0x5206D: 			End  { 29 02 }
0x5206F: 			SuppressIf  { 0A 82 }
0x52071: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52075: 					Uint8 Value: 0x2 { 42 03 02 }
0x52078: 					LessEqual  { 34 02 }
0x5207A: 				End  { 29 02 }
0x5207C: 				OneOf Prompt: "USB HS Physical Connector #2", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD7, VarStoreId: 0x6, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 16 73 16 D7 0A 06 00 2A 00 10 10 00 01 00 }
0x5208D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52094: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5209B: 				End  { 29 02 }
0x5209D: 			End  { 29 02 }
0x5209F: 			SuppressIf  { 0A 82 }
0x520A1: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x520A5: 					Uint8 Value: 0x3 { 42 03 03 }
0x520A8: 					LessEqual  { 34 02 }
0x520AA: 				End  { 29 02 }
0x520AC: 				OneOf Prompt: "USB HS Physical Connector #3", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD8, VarStoreId: 0x6, VarOffset: 0x2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 16 73 16 D8 0A 06 00 2B 00 10 10 00 01 00 }
0x520BD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x520C4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x520CB: 				End  { 29 02 }
0x520CD: 			End  { 29 02 }
0x520CF: 			SuppressIf  { 0A 82 }
0x520D1: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x520D5: 					Uint8 Value: 0x4 { 42 03 04 }
0x520D8: 					LessEqual  { 34 02 }
0x520DA: 				End  { 29 02 }
0x520DC: 				OneOf Prompt: "USB HS Physical Connector #4", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAD9, VarStoreId: 0x6, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 16 73 16 D9 0A 06 00 2C 00 10 10 00 01 00 }
0x520ED: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x520F4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x520FB: 				End  { 29 02 }
0x520FD: 			End  { 29 02 }
0x520FF: 			SuppressIf  { 0A 82 }
0x52101: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52105: 					Uint8 Value: 0x5 { 42 03 05 }
0x52108: 					LessEqual  { 34 02 }
0x5210A: 				End  { 29 02 }
0x5210C: 				OneOf Prompt: "USB HS Physical Connector #5", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xADA, VarStoreId: 0x6, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6A 16 73 16 DA 0A 06 00 2D 00 10 10 00 01 00 }
0x5211D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52124: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5212B: 				End  { 29 02 }
0x5212D: 			End  { 29 02 }
0x5212F: 			SuppressIf  { 0A 82 }
0x52131: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52135: 					Uint8 Value: 0x6 { 42 03 06 }
0x52138: 					LessEqual  { 34 02 }
0x5213A: 				End  { 29 02 }
0x5213C: 				OneOf Prompt: "USB HS Physical Connector #6", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xADB, VarStoreId: 0x6, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 16 73 16 DB 0A 06 00 2E 00 10 10 00 01 00 }
0x5214D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52154: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5215B: 				End  { 29 02 }
0x5215D: 			End  { 29 02 }
0x5215F: 			SuppressIf  { 0A 82 }
0x52161: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52165: 					Uint8 Value: 0x7 { 42 03 07 }
0x52168: 					LessEqual  { 34 02 }
0x5216A: 				End  { 29 02 }
0x5216C: 				OneOf Prompt: "USB HS Physical Connector #7", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xADC, VarStoreId: 0x6, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 16 73 16 DC 0A 06 00 2F 00 10 10 00 01 00 }
0x5217D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52184: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5218B: 				End  { 29 02 }
0x5218D: 			End  { 29 02 }
0x5218F: 			SuppressIf  { 0A 82 }
0x52191: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52195: 					Uint8 Value: 0x8 { 42 03 08 }
0x52198: 					LessEqual  { 34 02 }
0x5219A: 				End  { 29 02 }
0x5219C: 				OneOf Prompt: "USB HS Physical Connector #8", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xADD, VarStoreId: 0x6, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 16 73 16 DD 0A 06 00 30 00 10 10 00 01 00 }
0x521AD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x521B4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x521BB: 				End  { 29 02 }
0x521BD: 			End  { 29 02 }
0x521BF: 			SuppressIf  { 0A 82 }
0x521C1: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x521C5: 					Uint8 Value: 0x9 { 42 03 09 }
0x521C8: 					LessEqual  { 34 02 }
0x521CA: 				End  { 29 02 }
0x521CC: 				OneOf Prompt: "USB HS Physical Connector #9", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xADE, VarStoreId: 0x6, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 16 73 16 DE 0A 06 00 31 00 10 10 00 01 00 }
0x521DD: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x521E4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x521EB: 				End  { 29 02 }
0x521ED: 			End  { 29 02 }
0x521EF: 			SuppressIf  { 0A 82 }
0x521F1: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x521F5: 					Uint8 Value: 0xA { 42 03 0A }
0x521F8: 					LessEqual  { 34 02 }
0x521FA: 				End  { 29 02 }
0x521FC: 				OneOf Prompt: "USB HS Physical Connector #10", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xADF, VarStoreId: 0x6, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6F 16 73 16 DF 0A 06 00 32 00 10 10 00 01 00 }
0x5220D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52214: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5221B: 				End  { 29 02 }
0x5221D: 			End  { 29 02 }
0x5221F: 			SuppressIf  { 0A 82 }
0x52221: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52225: 					Uint8 Value: 0xB { 42 03 0B }
0x52228: 					LessEqual  { 34 02 }
0x5222A: 				End  { 29 02 }
0x5222C: 				OneOf Prompt: "USB HS Physical Connector #11", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAE0, VarStoreId: 0x6, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 16 73 16 E0 0A 06 00 33 00 10 10 00 01 00 }
0x5223D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52244: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5224B: 				End  { 29 02 }
0x5224D: 			End  { 29 02 }
0x5224F: 			SuppressIf  { 0A 82 }
0x52251: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52255: 					Uint8 Value: 0xC { 42 03 0C }
0x52258: 					LessEqual  { 34 02 }
0x5225A: 				End  { 29 02 }
0x5225C: 				OneOf Prompt: "USB HS Physical Connector #12", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAE1, VarStoreId: 0x6, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 71 16 73 16 E1 0A 06 00 34 00 10 10 00 01 00 }
0x5226D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52274: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5227B: 				End  { 29 02 }
0x5227D: 			End  { 29 02 }
0x5227F: 			SuppressIf  { 0A 82 }
0x52281: 				QuestionRef1 QuestionId: 0x1124 { 40 84 24 11 }
0x52285: 					Uint8 Value: 0xD { 42 03 0D }
0x52288: 					LessEqual  { 34 02 }
0x5228A: 				End  { 29 02 }
0x5228C: 				OneOf Prompt: "USB HS Physical Connector #13", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0xAE2, VarStoreId: 0x6, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 16 73 16 E2 0A 06 00 35 00 10 10 00 01 00 }
0x5229D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x522A4: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x522AB: 				End  { 29 02 }
0x522AD: 			End  { 29 02 }
0x522AF: 		End  { 29 02 }
0x522B1: 		SuppressIf  { 0A 82 }
0x522B3: 			EqIdVal QuestionId: 0xA7D, Value: 0x2 { 12 86 7D 0A 02 00 }
0x522B9: 				Not  { 17 02 }
0x522BB: 			End  { 29 02 }
0x522BD: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x522C4: 			End  { 29 02 }
0x522C6: 			OneOf Prompt: "USB Sensor Hub", Help: "USB Sensor Hub enable/disable", QuestionFlags: 0x10, QuestionId: 0xAE3, VarStoreId: 0xF101, VarOffset: 0x6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 16 49 16 E3 0A 01 F1 6B 00 10 10 00 01 00 }
0x522D7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x522DE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x522E5: 			End  { 29 02 }
0x522E7: 		End  { 29 02 }
0x522E9: 	End  { 29 02 }
0x522EB: 	Form FormId: 0x282E, Title: "SATA Configuration" { 01 86 2E 28 99 16 }
0x522F1: 		Subtitle Prompt: "SATA Configuration", Help: "", Flags: 0x0 { 02 87 99 16 00 00 00 }
0x522F8: 		End  { 29 02 }
0x522FA: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x52301: 		End  { 29 02 }
0x52303: 		OneOf Prompt: "SATA Controller(s)", Help: "Enable/Disable SATA Device.", QuestionFlags: 0x10, QuestionId: 0xAE4, VarStoreId: 0x6, VarOffset: 0x48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 16 9C 16 E4 0A 06 00 48 00 10 10 00 01 00 }
0x52314: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5231A: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52321: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52328: 		End  { 29 02 }
0x5232A: 		SuppressIf  { 0A 82 }
0x5232C: 			EqIdVal QuestionId: 0xAE4, Value: 0x0 { 12 06 E4 0A 00 00 }
0x52332: 			OneOf Prompt: "SATA Mode Selection", Help: "Determines how SATA controller(s) operate.", QuestionFlags: 0x10, QuestionId: 0xAE5, VarStoreId: 0x6, VarOffset: 0x49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x0, Step: 0x0 { 05 91 9D 16 9E 16 E5 0A 06 00 49 00 10 10 00 00 00 }
0x52343: 				OneOfOption Option: "AHCI" Value: 0, Default, MfgDefault { 09 07 9F 16 30 00 00 }
0x5234A: 			End  { 29 02 }
0x5234C: 			OneOf Prompt: "SATA Test Mode ", Help: "Test Mode Enable/Disable (Loop Back).", QuestionFlags: 0x10, QuestionId: 0xAE6, VarStoreId: 0x6, VarOffset: 0x93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 16 A1 16 E6 0A 06 00 93 00 10 10 00 01 00 }
0x5235D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52364: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5236B: 			End  { 29 02 }
0x5236D: 			SuppressIf  { 0A 82 }
0x5236F: 				EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52377: 				OneOf Prompt: "Aggressive LPM Support", Help: "Enable PCH to aggressively enter link power state.", QuestionFlags: 0x10, QuestionId: 0xAE7, VarStoreId: 0x6, VarOffset: 0x92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 16 FB 16 E7 0A 06 00 92 00 10 10 00 01 00 }
0x52388: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5238F: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x52396: 				End  { 29 02 }
0x52398: 			End  { 29 02 }
0x5239A: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x523A1: 			End  { 29 02 }
0x523A3: 			Text Prompt: "Serial ATA Port 0", Help: "", Text: "Empty" { 03 08 CD 16 C9 07 CE 16 }
0x523AB: 			Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 3D 17 }
0x523B3: 			SuppressIf  { 0A 82 }
0x523B5: 				EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x523BD: 				OneOf Prompt: "  Port 0", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xAE8, VarStoreId: 0x6, VarOffset: 0x4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DD 16 E5 16 E8 0A 06 00 4A 00 10 10 00 01 00 }
0x523CE: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x523D5: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x523DC: 				End  { 29 02 }
0x523DE: 			End  { 29 02 }
0x523E0: 			SuppressIf  { 0A 82 }
0x523E2: 				EqIdVal QuestionId: 0xAEA, Value: 0x1 { 12 06 EA 0A 01 00 }
0x523E8: 				OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xAE9, VarStoreId: 0x6, VarOffset: 0x52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 16 F0 16 E9 0A 06 00 52 00 10 10 00 01 00 }
0x523F9: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52400: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52407: 				End  { 29 02 }
0x52409: 				Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x52411: 			End  { 29 02 }
0x52413: 			OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xAEA, VarStoreId: 0x6, VarOffset: 0x6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E6 16 E7 16 EA 0A 06 00 6A 00 10 10 00 01 00 }
0x52424: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5242B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52432: 			End  { 29 02 }
0x52434: 			SuppressIf  { 0A 82 }
0x52436: 				EqIdVal QuestionId: 0xAE9, Value: 0x0 { 12 06 E9 0A 00 00 }
0x5243C: 				OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xAEB, VarStoreId: 0x6, VarOffset: 0x5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 16 F9 16 EB 0A 06 00 5A 00 10 10 00 01 00 }
0x5244D: 					OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x52454: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x5245B: 				End  { 29 02 }
0x5245D: 			End  { 29 02 }
0x5245F: 			OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xAEC, VarStoreId: 0x6, VarOffset: 0x62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FC 16 04 17 EC 0A 06 00 62 00 10 10 00 01 00 }
0x52470: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52477: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5247E: 			End  { 29 02 }
0x52480: 			OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xAED, VarStoreId: 0x6, VarOffset: 0x72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 17 0F 17 ED 0A 06 00 72 00 10 10 00 01 00 }
0x52491: 				OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x52498: 				OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x5249F: 			End  { 29 02 }
0x524A1: 			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xAEE, VarStoreId: 0x6, VarOffset: 0x7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 12 17 1A 17 EE 0A 06 00 7A 00 10 10 00 04 00 }
0x524B2: 				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault { 09 07 1B 17 30 00 00 }
0x524B9: 				OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x524C0: 				OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x524C7: 				OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x524CE: 				OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x524D5: 			End  { 29 02 }
0x524D7: 			OneOf Prompt: "  SATA Port 0 DevSlp", Help: "Enable/Disable SATA Port 0 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xAEF, VarStoreId: 0x6, VarOffset: 0x94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 16 A3 16 EF 0A 06 00 94 00 10 10 00 01 00 }
0x524E8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x524EE: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x524F5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x524FC: 			End  { 29 02 }
0x524FE: 			OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xAF0, VarStoreId: 0x6, VarOffset: 0x9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 16 BA 16 F0 0A 06 00 9C 00 10 10 00 01 00 }
0x5250F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52516: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5251D: 			End  { 29 02 }
0x5251F: 			GrayOutIf  { 19 82 }
0x52521: 				EqIdVal QuestionId: 0xAF0, Value: 0x0 { 12 06 F0 0A 00 00 }
0x52527: 				Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xAF1, VarStoreId: 0x6, VarOffset: 0xA4, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 BB 16 C3 16 F1 0A 06 00 A4 00 10 11 00 00 FF 03 00 00 }
0x5253B: 					Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x52542: 				End  { 29 02 }
0x52544: 				Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xAF2, VarStoreId: 0x6, VarOffset: 0xB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 C4 16 CC 16 F2 0A 06 00 B4 00 10 10 00 0F 00 }
0x52555: 					Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x5255B: 				End  { 29 02 }
0x5255D: 			End  { 29 02 }
0x5255F: 			Text Prompt: "Serial ATA Port 1", Help: "", Text: "Empty" { 03 08 CF 16 C9 07 D0 16 }
0x52567: 			Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 3E 17 }
0x5256F: 			SuppressIf  { 0A 82 }
0x52571: 				EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52579: 				OneOf Prompt: "  Port 1", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xAF3, VarStoreId: 0x6, VarOffset: 0x4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 16 E5 16 F3 0A 06 00 4B 00 10 10 00 01 00 }
0x5258A: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52591: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x52598: 				End  { 29 02 }
0x5259A: 			End  { 29 02 }
0x5259C: 			SuppressIf  { 0A 82 }
0x5259E: 				EqIdVal QuestionId: 0xAF5, Value: 0x1 { 12 06 F5 0A 01 00 }
0x525A4: 				OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xAF4, VarStoreId: 0x6, VarOffset: 0x53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 16 F0 16 F4 0A 06 00 53 00 10 10 00 01 00 }
0x525B5: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x525BC: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x525C3: 				End  { 29 02 }
0x525C5: 				Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x525CD: 			End  { 29 02 }
0x525CF: 			OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xAF5, VarStoreId: 0x6, VarOffset: 0x6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0D 19 E7 16 F5 0A 06 00 6B 00 10 10 00 01 00 }
0x525E0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x525E7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x525EE: 			End  { 29 02 }
0x525F0: 			SuppressIf  { 0A 82 }
0x525F2: 				EqIdVal QuestionId: 0xAF4, Value: 0x0 { 12 06 F4 0A 00 00 }
0x525F8: 				OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xAF6, VarStoreId: 0x6, VarOffset: 0x5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F2 16 F9 16 F6 0A 06 00 5B 00 10 10 00 01 00 }
0x52609: 					OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x52610: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x52617: 				End  { 29 02 }
0x52619: 			End  { 29 02 }
0x5261B: 			OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xAF7, VarStoreId: 0x6, VarOffset: 0x63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 16 04 17 F7 0A 06 00 63 00 10 10 00 01 00 }
0x5262C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52633: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5263A: 			End  { 29 02 }
0x5263C: 			OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xAF8, VarStoreId: 0x6, VarOffset: 0x73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 17 0F 17 F8 0A 06 00 73 00 10 10 00 01 00 }
0x5264D: 				OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x52654: 				OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x5265B: 			End  { 29 02 }
0x5265D: 			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xAF9, VarStoreId: 0x6, VarOffset: 0x7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 13 17 1A 17 F9 0A 06 00 7B 00 10 10 00 04 00 }
0x5266E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x52674: 				OneOfOption Option: "Unknown" Value: 0 { 09 07 1B 17 00 00 00 }
0x5267B: 				OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x52682: 				OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x52689: 				OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x52690: 				OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x52697: 			End  { 29 02 }
0x52699: 			OneOf Prompt: "  SATA Port 1 DevSlp", Help: "Enable/Disable SATA Port 1 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xAFA, VarStoreId: 0x6, VarOffset: 0x95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 16 A5 16 FA 0A 06 00 95 00 10 10 00 01 00 }
0x526AA: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x526B0: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x526B7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x526BE: 			End  { 29 02 }
0x526C0: 			OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xAFB, VarStoreId: 0x6, VarOffset: 0x9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 16 BA 16 FB 0A 06 00 9D 00 10 10 00 01 00 }
0x526D1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x526D8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x526DF: 			End  { 29 02 }
0x526E1: 			GrayOutIf  { 19 82 }
0x526E3: 				EqIdVal QuestionId: 0xAFB, Value: 0x0 { 12 06 FB 0A 00 00 }
0x526E9: 				Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xAFC, VarStoreId: 0x6, VarOffset: 0xA6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 BC 16 C3 16 FC 0A 06 00 A6 00 10 11 00 00 FF 03 00 00 }
0x526FD: 					Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x52704: 				End  { 29 02 }
0x52706: 				Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xAFD, VarStoreId: 0x6, VarOffset: 0xB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 C5 16 CC 16 FD 0A 06 00 B5 00 10 10 00 0F 00 }
0x52717: 					Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x5271D: 				End  { 29 02 }
0x5271F: 			End  { 29 02 }
0x52721: 			Text Prompt: "Serial ATA Port 2", Help: "", Text: "Empty" { 03 08 D1 16 C9 07 D2 16 }
0x52729: 			Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 3F 17 }
0x52731: 			SuppressIf  { 0A 82 }
0x52733: 				EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x5273B: 				OneOf Prompt: "  Port 2", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xAFE, VarStoreId: 0x6, VarOffset: 0x4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 16 E5 16 FE 0A 06 00 4C 00 10 10 00 01 00 }
0x5274C: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52753: 					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5275A: 				End  { 29 02 }
0x5275C: 			End  { 29 02 }
0x5275E: 			SuppressIf  { 0A 82 }
0x52760: 				EqIdVal QuestionId: 0xB00, Value: 0x1 { 12 06 00 0B 01 00 }
0x52766: 				OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xAFF, VarStoreId: 0x6, VarOffset: 0x54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 16 F0 16 FF 0A 06 00 54 00 10 10 00 01 00 }
0x52777: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5277E: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52785: 				End  { 29 02 }
0x52787: 				Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x5278F: 			End  { 29 02 }
0x52791: 			OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xB00, VarStoreId: 0x6, VarOffset: 0x6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 19 E7 16 00 0B 06 00 6C 00 10 10 00 01 00 }
0x527A2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x527A9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x527B0: 			End  { 29 02 }
0x527B2: 			SuppressIf  { 0A 82 }
0x527B4: 				EqIdVal QuestionId: 0xAFF, Value: 0x0 { 12 06 FF 0A 00 00 }
0x527BA: 				OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xB01, VarStoreId: 0x6, VarOffset: 0x5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F3 16 F9 16 01 0B 06 00 5C 00 10 10 00 01 00 }
0x527CB: 					OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x527D2: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x527D9: 				End  { 29 02 }
0x527DB: 			End  { 29 02 }
0x527DD: 			OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xB02, VarStoreId: 0x6, VarOffset: 0x64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FE 16 04 17 02 0B 06 00 64 00 10 10 00 01 00 }
0x527EE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x527F5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x527FC: 			End  { 29 02 }
0x527FE: 			OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xB03, VarStoreId: 0x6, VarOffset: 0x74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 17 0F 17 03 0B 06 00 74 00 10 10 00 01 00 }
0x5280F: 				OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x52816: 				OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x5281D: 			End  { 29 02 }
0x5281F: 			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xB04, VarStoreId: 0x6, VarOffset: 0x7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 14 17 1A 17 04 0B 06 00 7C 00 10 10 00 04 00 }
0x52830: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x52836: 				OneOfOption Option: "Unknown" Value: 0 { 09 07 1B 17 00 00 00 }
0x5283D: 				OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x52844: 				OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x5284B: 				OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x52852: 				OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x52859: 			End  { 29 02 }
0x5285B: 			OneOf Prompt: "  SATA Port 2 DevSlp", Help: "Enable/Disable SATA Port 2 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xB05, VarStoreId: 0x6, VarOffset: 0x96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A6 16 A7 16 05 0B 06 00 96 00 10 10 00 01 00 }
0x5286C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x52872: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52879: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52880: 			End  { 29 02 }
0x52882: 			OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xB06, VarStoreId: 0x6, VarOffset: 0x9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 16 BA 16 06 0B 06 00 9E 00 10 10 00 01 00 }
0x52893: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5289A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x528A1: 			End  { 29 02 }
0x528A3: 			GrayOutIf  { 19 82 }
0x528A5: 				EqIdVal QuestionId: 0xB06, Value: 0x0 { 12 06 06 0B 00 00 }
0x528AB: 				Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xB07, VarStoreId: 0x6, VarOffset: 0xA8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 BD 16 C3 16 07 0B 06 00 A8 00 10 11 00 00 FF 03 00 00 }
0x528BF: 					Default DefaultId: 0x0 Value: Other { 5B 85 00 00 08 }
0x528C4: 						Value  { 5A 82 }
0x528C6: 							Uint64 Value: 0x271 { 45 0A 71 02 00 00 00 00 00 00 }
0x528D0: 						End  { 29 02 }
0x528D2: 					End  { 29 02 }
0x528D4: 				End  { 29 02 }
0x528D6: 				Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xB08, VarStoreId: 0x6, VarOffset: 0xB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 C6 16 CC 16 08 0B 06 00 B6 00 10 10 00 0F 00 }
0x528E7: 					Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x528ED: 				End  { 29 02 }
0x528EF: 			End  { 29 02 }
0x528F1: 			SuppressIf  { 0A 82 }
0x528F3: 				EqIdVal QuestionId: 0x1112, Value: 0x1 { 12 86 12 11 01 00 }
0x528F9: 					Not  { 17 02 }
0x528FB: 				End  { 29 02 }
0x528FD: 				Text Prompt: "Serial ATA Port 3", Help: "", Text: "Empty" { 03 08 D3 16 C9 07 D4 16 }
0x52905: 				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 40 17 }
0x5290D: 				SuppressIf  { 0A 82 }
0x5290F: 					EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52917: 					OneOf Prompt: "  Port 3", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xB09, VarStoreId: 0x6, VarOffset: 0x4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 16 E5 16 09 0B 06 00 4D 00 10 10 00 01 00 }
0x52928: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5292F: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x52936: 					End  { 29 02 }
0x52938: 				End  { 29 02 }
0x5293A: 				SuppressIf  { 0A 82 }
0x5293C: 					EqIdVal QuestionId: 0xB0B, Value: 0x1 { 12 06 0B 0B 01 00 }
0x52942: 					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xB0A, VarStoreId: 0x6, VarOffset: 0x55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 16 F0 16 0A 0B 06 00 55 00 10 10 00 01 00 }
0x52953: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5295A: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52961: 					End  { 29 02 }
0x52963: 					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x5296B: 				End  { 29 02 }
0x5296D: 				OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xB0B, VarStoreId: 0x6, VarOffset: 0x6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0F 19 E7 16 0B 0B 06 00 6D 00 10 10 00 01 00 }
0x5297E: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52985: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5298C: 				End  { 29 02 }
0x5298E: 				SuppressIf  { 0A 82 }
0x52990: 					EqIdVal QuestionId: 0xB0A, Value: 0x0 { 12 06 0A 0B 00 00 }
0x52996: 					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xB0C, VarStoreId: 0x6, VarOffset: 0x5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F4 16 F9 16 0C 0B 06 00 5D 00 10 10 00 01 00 }
0x529A7: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x529AE: 						OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x529B5: 					End  { 29 02 }
0x529B7: 				End  { 29 02 }
0x529B9: 				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xB0D, VarStoreId: 0x6, VarOffset: 0x65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FF 16 04 17 0D 0B 06 00 65 00 10 10 00 01 00 }
0x529CA: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x529D1: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x529D8: 				End  { 29 02 }
0x529DA: 				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xB0E, VarStoreId: 0x6, VarOffset: 0x75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 17 0F 17 0E 0B 06 00 75 00 10 10 00 01 00 }
0x529EB: 					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x529F2: 					OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x529F9: 				End  { 29 02 }
0x529FB: 				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xB0F, VarStoreId: 0x6, VarOffset: 0x7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 15 17 1A 17 0F 0B 06 00 7D 00 10 10 00 04 00 }
0x52A0C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x52A12: 					OneOfOption Option: "Unknown" Value: 0 { 09 07 1B 17 00 00 00 }
0x52A19: 					OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x52A20: 					OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x52A27: 					OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x52A2E: 					OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x52A35: 				End  { 29 02 }
0x52A37: 				OneOf Prompt: "  SATA Port 3 DevSlp", Help: "Enable/Disable SATA Port 3 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xB10, VarStoreId: 0x6, VarOffset: 0x97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 16 A9 16 10 0B 06 00 97 00 10 10 00 01 00 }
0x52A48: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52A4F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52A56: 				End  { 29 02 }
0x52A58: 				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xB11, VarStoreId: 0x6, VarOffset: 0x9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 16 BA 16 11 0B 06 00 9F 00 10 10 00 01 00 }
0x52A69: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52A70: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52A77: 				End  { 29 02 }
0x52A79: 				GrayOutIf  { 19 82 }
0x52A7B: 					EqIdVal QuestionId: 0xB11, Value: 0x0 { 12 06 11 0B 00 00 }
0x52A81: 					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xB12, VarStoreId: 0x6, VarOffset: 0xAA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 BE 16 C3 16 12 0B 06 00 AA 00 10 11 00 00 FF 03 00 00 }
0x52A95: 						Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x52A9C: 					End  { 29 02 }
0x52A9E: 					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xB13, VarStoreId: 0x6, VarOffset: 0xB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 C7 16 CC 16 13 0B 06 00 B7 00 10 10 00 0F 00 }
0x52AAF: 						Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x52AB5: 					End  { 29 02 }
0x52AB7: 				End  { 29 02 }
0x52AB9: 				Text Prompt: "Serial ATA Port 4", Help: "", Text: "Empty" { 03 08 D5 16 C9 07 D6 16 }
0x52AC1: 				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 41 17 }
0x52AC9: 				SuppressIf  { 0A 82 }
0x52ACB: 					EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52AD3: 					OneOf Prompt: "  Port 4", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xB14, VarStoreId: 0x6, VarOffset: 0x4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 16 E5 16 14 0B 06 00 4E 00 10 10 00 01 00 }
0x52AE4: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52AEB: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x52AF2: 					End  { 29 02 }
0x52AF4: 				End  { 29 02 }
0x52AF6: 				SuppressIf  { 0A 82 }
0x52AF8: 					EqIdVal QuestionId: 0xB16, Value: 0x1 { 12 06 16 0B 01 00 }
0x52AFE: 					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xB15, VarStoreId: 0x6, VarOffset: 0x56, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EC 16 F0 16 15 0B 06 00 56 00 10 10 00 01 00 }
0x52B0F: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52B16: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52B1D: 					End  { 29 02 }
0x52B1F: 					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x52B27: 				End  { 29 02 }
0x52B29: 				OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xB16, VarStoreId: 0x6, VarOffset: 0x6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 10 19 E7 16 16 0B 06 00 6E 00 10 10 00 01 00 }
0x52B3A: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52B41: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52B48: 				End  { 29 02 }
0x52B4A: 				SuppressIf  { 0A 82 }
0x52B4C: 					EqIdVal QuestionId: 0xB15, Value: 0x0 { 12 06 15 0B 00 00 }
0x52B52: 					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xB17, VarStoreId: 0x6, VarOffset: 0x5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 16 F9 16 17 0B 06 00 5E 00 10 10 00 01 00 }
0x52B63: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x52B6A: 						OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x52B71: 					End  { 29 02 }
0x52B73: 				End  { 29 02 }
0x52B75: 				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xB18, VarStoreId: 0x6, VarOffset: 0x66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 00 17 04 17 18 0B 06 00 66 00 10 10 00 01 00 }
0x52B86: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52B8D: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52B94: 				End  { 29 02 }
0x52B96: 				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xB19, VarStoreId: 0x6, VarOffset: 0x76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 17 0F 17 19 0B 06 00 76 00 10 10 00 01 00 }
0x52BA7: 					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x52BAE: 					OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x52BB5: 				End  { 29 02 }
0x52BB7: 				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xB1A, VarStoreId: 0x6, VarOffset: 0x7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 16 17 1A 17 1A 0B 06 00 7E 00 10 10 00 04 00 }
0x52BC8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x52BCE: 					OneOfOption Option: "Unknown" Value: 0 { 09 07 1B 17 00 00 00 }
0x52BD5: 					OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x52BDC: 					OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x52BE3: 					OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x52BEA: 					OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x52BF1: 				End  { 29 02 }
0x52BF3: 				OneOf Prompt: "  SATA Port 4 DevSlp", Help: "Enable/Disable SATA Port 4 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xB1B, VarStoreId: 0x6, VarOffset: 0x98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 16 AB 16 1B 0B 06 00 98 00 10 10 00 01 00 }
0x52C04: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52C0B: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52C12: 				End  { 29 02 }
0x52C14: 				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xB1C, VarStoreId: 0x6, VarOffset: 0xA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 16 BA 16 1C 0B 06 00 A0 00 10 10 00 01 00 }
0x52C25: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52C2C: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52C33: 				End  { 29 02 }
0x52C35: 				GrayOutIf  { 19 82 }
0x52C37: 					EqIdVal QuestionId: 0xB1C, Value: 0x0 { 12 06 1C 0B 00 00 }
0x52C3D: 					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xB1D, VarStoreId: 0x6, VarOffset: 0xAC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 BF 16 C3 16 1D 0B 06 00 AC 00 10 11 00 00 FF 03 00 00 }
0x52C51: 						Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x52C58: 					End  { 29 02 }
0x52C5A: 					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xB1E, VarStoreId: 0x6, VarOffset: 0xB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 C8 16 CC 16 1E 0B 06 00 B8 00 10 10 00 0F 00 }
0x52C6B: 						Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x52C71: 					End  { 29 02 }
0x52C73: 				End  { 29 02 }
0x52C75: 				Text Prompt: "Serial ATA Port 5", Help: "", Text: "Empty" { 03 08 D7 16 C9 07 D8 16 }
0x52C7D: 				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 42 17 }
0x52C85: 				SuppressIf  { 0A 82 }
0x52C87: 					EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52C8F: 					OneOf Prompt: "  Port 5", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xB1F, VarStoreId: 0x6, VarOffset: 0x4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 16 E5 16 1F 0B 06 00 4F 00 10 10 00 01 00 }
0x52CA0: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52CA7: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x52CAE: 					End  { 29 02 }
0x52CB0: 				End  { 29 02 }
0x52CB2: 				SuppressIf  { 0A 82 }
0x52CB4: 					EqIdVal QuestionId: 0xB21, Value: 0x1 { 12 06 21 0B 01 00 }
0x52CBA: 					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xB20, VarStoreId: 0x6, VarOffset: 0x57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 ED 16 F0 16 20 0B 06 00 57 00 10 10 00 01 00 }
0x52CCB: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52CD2: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52CD9: 					End  { 29 02 }
0x52CDB: 					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x52CE3: 				End  { 29 02 }
0x52CE5: 				OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xB21, VarStoreId: 0x6, VarOffset: 0x6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 19 E7 16 21 0B 06 00 6F 00 10 10 00 01 00 }
0x52CF6: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52CFD: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52D04: 				End  { 29 02 }
0x52D06: 				SuppressIf  { 0A 82 }
0x52D08: 					EqIdVal QuestionId: 0xB20, Value: 0x0 { 12 06 20 0B 00 00 }
0x52D0E: 					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xB22, VarStoreId: 0x6, VarOffset: 0x5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F6 16 F9 16 22 0B 06 00 5F 00 10 10 00 01 00 }
0x52D1F: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x52D26: 						OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x52D2D: 					End  { 29 02 }
0x52D2F: 				End  { 29 02 }
0x52D31: 				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xB23, VarStoreId: 0x6, VarOffset: 0x67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 17 04 17 23 0B 06 00 67 00 10 10 00 01 00 }
0x52D42: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52D49: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52D50: 				End  { 29 02 }
0x52D52: 				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xB24, VarStoreId: 0x6, VarOffset: 0x77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0C 17 0F 17 24 0B 06 00 77 00 10 10 00 01 00 }
0x52D63: 					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x52D6A: 					OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x52D71: 				End  { 29 02 }
0x52D73: 				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xB25, VarStoreId: 0x6, VarOffset: 0x7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 17 17 1A 17 25 0B 06 00 7F 00 10 10 00 04 00 }
0x52D84: 					OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault { 09 07 1B 17 30 00 00 }
0x52D8B: 					OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x52D92: 					OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x52D99: 					OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x52DA0: 					OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x52DA7: 				End  { 29 02 }
0x52DA9: 				OneOf Prompt: "  SATA Port 5 DevSlp", Help: "Enable/Disable SATA Port 5 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xB26, VarStoreId: 0x6, VarOffset: 0x99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 16 AD 16 26 0B 06 00 99 00 10 10 00 01 00 }
0x52DBA: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52DC1: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52DC8: 				End  { 29 02 }
0x52DCA: 				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xB27, VarStoreId: 0x6, VarOffset: 0xA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 16 BA 16 27 0B 06 00 A1 00 10 10 00 01 00 }
0x52DDB: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52DE2: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52DE9: 				End  { 29 02 }
0x52DEB: 				GrayOutIf  { 19 82 }
0x52DED: 					EqIdVal QuestionId: 0xB27, Value: 0x0 { 12 06 27 0B 00 00 }
0x52DF3: 					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xB28, VarStoreId: 0x6, VarOffset: 0xAE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 C0 16 C3 16 28 0B 06 00 AE 00 10 11 00 00 FF 03 00 00 }
0x52E07: 						Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x52E0E: 					End  { 29 02 }
0x52E10: 					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xB29, VarStoreId: 0x6, VarOffset: 0xB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 C9 16 CC 16 29 0B 06 00 B9 00 10 10 00 0F 00 }
0x52E21: 						Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x52E27: 					End  { 29 02 }
0x52E29: 				End  { 29 02 }
0x52E2B: 				Text Prompt: "Serial ATA Port 6", Help: "", Text: "Empty" { 03 08 D9 16 C9 07 DA 16 }
0x52E33: 				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 43 17 }
0x52E3B: 				SuppressIf  { 0A 82 }
0x52E3D: 					EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52E45: 					OneOf Prompt: "  Port 6", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xB2A, VarStoreId: 0x6, VarOffset: 0x50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 16 E5 16 2A 0B 06 00 50 00 10 10 00 01 00 }
0x52E56: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x52E5D: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x52E64: 					End  { 29 02 }
0x52E66: 				End  { 29 02 }
0x52E68: 				SuppressIf  { 0A 82 }
0x52E6A: 					EqIdVal QuestionId: 0xB2C, Value: 0x1 { 12 06 2C 0B 01 00 }
0x52E70: 					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xB2B, VarStoreId: 0x6, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EE 16 F0 16 2B 0B 06 00 58 00 10 10 00 01 00 }
0x52E81: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52E88: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52E8F: 					End  { 29 02 }
0x52E91: 					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x52E99: 				End  { 29 02 }
0x52E9B: 				OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xB2C, VarStoreId: 0x6, VarOffset: 0x70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 12 19 E7 16 2C 0B 06 00 70 00 10 10 00 01 00 }
0x52EAC: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52EB3: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52EBA: 				End  { 29 02 }
0x52EBC: 				SuppressIf  { 0A 82 }
0x52EBE: 					EqIdVal QuestionId: 0xB2B, Value: 0x0 { 12 06 2B 0B 00 00 }
0x52EC4: 					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xB2D, VarStoreId: 0x6, VarOffset: 0x60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F7 16 F9 16 2D 0B 06 00 60 00 10 10 00 01 00 }
0x52ED5: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x52EDC: 						OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x52EE3: 					End  { 29 02 }
0x52EE5: 				End  { 29 02 }
0x52EE7: 				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xB2E, VarStoreId: 0x6, VarOffset: 0x68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 17 04 17 2E 0B 06 00 68 00 10 10 00 01 00 }
0x52EF8: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52EFF: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52F06: 				End  { 29 02 }
0x52F08: 				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xB2F, VarStoreId: 0x6, VarOffset: 0x78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0D 17 0F 17 2F 0B 06 00 78 00 10 10 00 01 00 }
0x52F19: 					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x52F20: 					OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x52F27: 				End  { 29 02 }
0x52F29: 				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xB30, VarStoreId: 0x6, VarOffset: 0x80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 18 17 1A 17 30 0B 06 00 80 00 10 10 00 04 00 }
0x52F3A: 					OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault { 09 07 1B 17 30 00 00 }
0x52F41: 					OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x52F48: 					OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x52F4F: 					OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x52F56: 					OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x52F5D: 				End  { 29 02 }
0x52F5F: 				OneOf Prompt: "  SATA Port 6 DevSlp", Help: "Enable/Disable SATA Port 6 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xB31, VarStoreId: 0x6, VarOffset: 0x9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 16 AF 16 31 0B 06 00 9A 00 10 10 00 01 00 }
0x52F70: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52F77: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52F7E: 				End  { 29 02 }
0x52F80: 				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xB32, VarStoreId: 0x6, VarOffset: 0xA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 16 BA 16 32 0B 06 00 A2 00 10 10 00 01 00 }
0x52F91: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x52F98: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x52F9F: 				End  { 29 02 }
0x52FA1: 				GrayOutIf  { 19 82 }
0x52FA3: 					EqIdVal QuestionId: 0xB32, Value: 0x0 { 12 06 32 0B 00 00 }
0x52FA9: 					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xB33, VarStoreId: 0x6, VarOffset: 0xB0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 C1 16 C3 16 33 0B 06 00 B0 00 10 11 00 00 FF 03 00 00 }
0x52FBD: 						Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x52FC4: 					End  { 29 02 }
0x52FC6: 					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xB34, VarStoreId: 0x6, VarOffset: 0xBA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 CA 16 CC 16 34 0B 06 00 BA 00 10 10 00 0F 00 }
0x52FD7: 						Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x52FDD: 					End  { 29 02 }
0x52FDF: 				End  { 29 02 }
0x52FE1: 				Text Prompt: "Serial ATA Port 7", Help: "", Text: "Empty" { 03 08 DB 16 C9 07 DC 16 }
0x52FE9: 				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown" { 03 08 3C 17 C9 07 44 17 }
0x52FF1: 				SuppressIf  { 0A 82 }
0x52FF3: 					EqIdValList QuestionId: 0xAE6, Values: [1] { 14 08 E6 0A 01 00 01 00 }
0x52FFB: 					OneOf Prompt: "  Port 7", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0xB35, VarStoreId: 0x6, VarOffset: 0x51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 16 E5 16 35 0B 06 00 51 00 10 10 00 01 00 }
0x5300C: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53013: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5301A: 					End  { 29 02 }
0x5301C: 				End  { 29 02 }
0x5301E: 				SuppressIf  { 0A 82 }
0x53020: 					EqIdVal QuestionId: 0xB37, Value: 0x1 { 12 06 37 0B 01 00 }
0x53026: 					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0xB36, VarStoreId: 0x6, VarOffset: 0x59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EF 16 F0 16 36 0B 06 00 59 00 10 10 00 01 00 }
0x53037: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5303E: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53045: 					End  { 29 02 }
0x53047: 					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported" { 03 08 05 17 C9 07 06 17 }
0x5304F: 				End  { 29 02 }
0x53051: 				OneOf Prompt: "  External", Help: "Marks this port as external.", QuestionFlags: 0x10, QuestionId: 0xB37, VarStoreId: 0x6, VarOffset: 0x71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 13 19 E7 16 37 0B 06 00 71 00 10 10 00 01 00 }
0x53062: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53069: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53070: 				End  { 29 02 }
0x53072: 				SuppressIf  { 0A 82 }
0x53074: 					EqIdVal QuestionId: 0xB36, Value: 0x0 { 12 06 36 0B 00 00 }
0x5307A: 					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0xB38, VarStoreId: 0x6, VarOffset: 0x61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F8 16 F9 16 38 0B 06 00 61 00 10 10 00 01 00 }
0x5308B: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x53092: 						OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x53099: 					End  { 29 02 }
0x5309B: 				End  { 29 02 }
0x5309D: 				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0xB39, VarStoreId: 0x6, VarOffset: 0x69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 03 17 04 17 39 0B 06 00 69 00 10 10 00 01 00 }
0x530AE: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x530B5: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x530BC: 				End  { 29 02 }
0x530BE: 				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0xB3A, VarStoreId: 0x6, VarOffset: 0x79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 17 0F 17 3A 0B 06 00 79 00 10 10 00 01 00 }
0x530CF: 					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault { 09 07 10 17 30 00 00 }
0x530D6: 					OneOfOption Option: "Solid State Drive" Value: 1 { 09 07 11 17 00 00 01 }
0x530DD: 				End  { 29 02 }
0x530DF: 				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0xB3B, VarStoreId: 0x6, VarOffset: 0x81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 19 17 1A 17 3B 0B 06 00 81 00 10 10 00 04 00 }
0x530F0: 					OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault { 09 07 1B 17 30 00 00 }
0x530F7: 					OneOfOption Option: "ISATA" Value: 1 { 09 07 1C 17 00 00 01 }
0x530FE: 					OneOfOption Option: "Direct Connect" Value: 2 { 09 07 1D 17 00 00 02 }
0x53105: 					OneOfOption Option: "Flex" Value: 3 { 09 07 1E 17 00 00 03 }
0x5310C: 					OneOfOption Option: "M2" Value: 4 { 09 07 1F 17 00 00 04 }
0x53113: 				End  { 29 02 }
0x53115: 				OneOf Prompt: "  SATA Port 7 DevSlp", Help: "Enable/Disable SATA Port 7 DevSlp. For DevSlp to work, both hard drive and SATA port need to support DevSlp function, otherwise an unexpected behavior might happen. Please check board design before enabling it.", QuestionFlags: 0x10, QuestionId: 0xB3C, VarStoreId: 0x6, VarOffset: 0x9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 16 B1 16 3C 0B 06 00 9B 00 10 10 00 01 00 }
0x53126: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5312D: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53134: 				End  { 29 02 }
0x53136: 				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0xB3D, VarStoreId: 0x6, VarOffset: 0xA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 16 BA 16 3D 0B 06 00 A3 00 10 10 00 01 00 }
0x53147: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5314E: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53155: 				End  { 29 02 }
0x53157: 				GrayOutIf  { 19 82 }
0x53159: 					EqIdVal QuestionId: 0xB3D, Value: 0x0 { 12 06 3D 0B 00 00 }
0x5315F: 					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0xB3E, VarStoreId: 0x6, VarOffset: 0xB2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0 { 07 94 C2 16 C3 16 3E 0B 06 00 B2 00 10 11 00 00 FF 03 00 00 }
0x53173: 						Default DefaultId: 0x0 Value: 625 { 5B 07 00 00 01 71 02 }
0x5317A: 					End  { 29 02 }
0x5317C: 					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0xB3F, VarStoreId: 0x6, VarOffset: 0xBB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0 { 07 91 CB 16 CC 16 3F 0B 06 00 BB 00 10 10 00 0F 00 }
0x5318D: 						Default DefaultId: 0x0 Value: 15 { 5B 06 00 00 00 0F }
0x53193: 					End  { 29 02 }
0x53195: 				End  { 29 02 }
0x53197: 			End  { 29 02 }
0x53199: 		End  { 29 02 }
0x5319B: 	End  { 29 02 }
0x5319D: 	Form FormId: 0x282F, Title: "PCIe EQ settings" { 01 86 2F 28 3F 12 }
0x531A3: 		CheckBox Prompt: "PCIe EQ override", Help: "Choose your own PCIe EQ settings, only for users who have a thorough understanding of equalization process", QuestionFlags: 0x0, QuestionId: 0xB40, VarStoreId: 0x6, VarOffset: 0x3BC, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 41 12 42 12 40 0B 06 00 BC 03 00 00 }
0x531B1: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x531B7: 		End  { 29 02 }
0x531B9: 		SuppressIf  { 0A 82 }
0x531BB: 			EqIdVal QuestionId: 0xB40, Value: 0x0 { 12 06 40 0B 00 00 }
0x531C1: 			OneOf Prompt: "PCIe EQ method", Help: "Choose PCIe EQ method", QuestionFlags: 0x10, QuestionId: 0xB41, VarStoreId: 0x6, VarOffset: 0x3BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 43 12 44 12 41 0B 06 00 BD 03 10 10 00 01 00 }
0x531D2: 				OneOfOption Option: "PCIe hardware EQ" Value: 0, Default { 09 07 45 12 10 00 00 }
0x531D9: 				OneOfOption Option: "PCIe fixed EQ" Value: 1 { 09 07 46 12 00 00 01 }
0x531E0: 			End  { 29 02 }
0x531E2: 			OneOf Prompt: "PCIe EQ mode", Help: "Choose EQ mode. Preset mode - root port will use presets during EQ process, Coefficient mode - root port will use coefficients during EQ process", QuestionFlags: 0x10, QuestionId: 0xB42, VarStoreId: 0x6, VarOffset: 0x3BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 47 12 48 12 42 0B 06 00 BE 03 10 10 00 01 00 }
0x531F3: 				OneOfOption Option: "Use presets during EQ" Value: 0, Default { 09 07 49 12 10 00 00 }
0x531FA: 				OneOfOption Option: "Use coefficients during EQ" Value: 1 { 09 07 4A 12 00 00 01 }
0x53201: 			End  { 29 02 }
0x53203: 			Numeric Prompt: "EQ PH1 downstream port transmitter preset", Help: "Choose the value of the preset that will be used during phase 1 of the equalization", QuestionFlags: 0x10, QuestionId: 0xB43, VarStoreId: 0x6, VarOffset: 0x3C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 4B 12 4D 12 43 0B 06 00 C0 03 10 10 00 0A 01 }
0x53214: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5321A: 			End  { 29 02 }
0x5321C: 			Numeric Prompt: "EQ PH1 upstream port transmitter preset", Help: "Choose the value of the preset that will be used during phase 1 of the equalization", QuestionFlags: 0x10, QuestionId: 0xB44, VarStoreId: 0x6, VarOffset: 0x3C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 4C 12 4D 12 44 0B 06 00 C1 03 10 10 00 0A 01 }
0x5322D: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53233: 			End  { 29 02 }
0x53235: 			CheckBox Prompt: "Enable EQ phase 2 local transmitter override", Help: "EQ Phase 2 local transmitter override can be used to debug issues with PCI devices equalization.", QuestionFlags: 0x0, QuestionId: 0xB45, VarStoreId: 0x6, VarOffset: 0x3BF, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 72 12 73 12 45 0B 06 00 BF 03 00 00 }
0x53243: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53249: 			End  { 29 02 }
0x5324B: 			SuppressIf  { 0A 82 }
0x5324D: 				EqIdVal QuestionId: 0xB45, Value: 0x0 { 12 06 45 0B 00 00 }
0x53253: 				Numeric Prompt: "EQ Phase 2 local transmitter override preset", Help: "Select preset which will be used during phase 2 of the PCIe EQ process", QuestionFlags: 0x10, QuestionId: 0xB46, VarStoreId: 0x6, VarOffset: 0x3E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1 { 07 91 74 12 75 12 46 0B 06 00 E2 03 10 10 00 0A 01 }
0x53264: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5326A: 				End  { 29 02 }
0x5326C: 			End  { 29 02 }
0x5326E: 			Numeric Prompt: "Number of presets or coefficients used during phase 3", Help: "Select how many presets or coefficients will be used during phase 3 of EQ. Please not that you have to set all of the list entries to valid values. The interpretation of this field depends on PCIe EQ mode", QuestionFlags: 0x10, QuestionId: 0xB47, VarStoreId: 0x6, VarOffset: 0x3C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xB, Step: 0x1 { 07 91 4E 12 4F 12 47 0B 06 00 C2 03 10 10 00 0B 01 }
0x5327F: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53285: 			End  { 29 02 }
0x53287: 			SuppressIf  { 0A 82 }
0x53289: 				EqIdVal QuestionId: 0xB42, Value: 0x0 { 12 86 42 0B 00 00 }
0x5328F: 					Not  { 17 02 }
0x53291: 				End  { 29 02 }
0x53293: 				Numeric Prompt: "Preset 0", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB48, VarStoreId: 0x6, VarOffset: 0x3D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 50 12 5B 12 48 0B 06 00 D7 03 10 10 00 3F 01 }
0x532A4: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x532AA: 				End  { 29 02 }
0x532AC: 				Numeric Prompt: "Preset 1", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB49, VarStoreId: 0x6, VarOffset: 0x3D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 51 12 5B 12 49 0B 06 00 D8 03 10 10 00 3F 01 }
0x532BD: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x532C3: 				End  { 29 02 }
0x532C5: 				Numeric Prompt: "Preset 2", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB4A, VarStoreId: 0x6, VarOffset: 0x3D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 52 12 5B 12 4A 0B 06 00 D9 03 10 10 00 3F 01 }
0x532D6: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x532DC: 				End  { 29 02 }
0x532DE: 				Numeric Prompt: "Preset 3", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB4B, VarStoreId: 0x6, VarOffset: 0x3DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 53 12 5B 12 4B 0B 06 00 DA 03 10 10 00 3F 01 }
0x532EF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x532F5: 				End  { 29 02 }
0x532F7: 				Numeric Prompt: "Preset 4", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB4C, VarStoreId: 0x6, VarOffset: 0x3DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 54 12 5B 12 4C 0B 06 00 DB 03 10 10 00 3F 01 }
0x53308: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5330E: 				End  { 29 02 }
0x53310: 				Numeric Prompt: "Preset 5", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB4D, VarStoreId: 0x6, VarOffset: 0x3DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 55 12 5B 12 4D 0B 06 00 DC 03 10 10 00 3F 01 }
0x53321: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53327: 				End  { 29 02 }
0x53329: 				Numeric Prompt: "Preset 6", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB4E, VarStoreId: 0x6, VarOffset: 0x3DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 56 12 5B 12 4E 0B 06 00 DD 03 10 10 00 3F 01 }
0x5333A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53340: 				End  { 29 02 }
0x53342: 				Numeric Prompt: "Preset 7", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB4F, VarStoreId: 0x6, VarOffset: 0x3DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 57 12 5B 12 4F 0B 06 00 DE 03 10 10 00 3F 01 }
0x53353: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53359: 				End  { 29 02 }
0x5335B: 				Numeric Prompt: "Preset 8", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB50, VarStoreId: 0x6, VarOffset: 0x3DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 58 12 5B 12 50 0B 06 00 DF 03 10 10 00 3F 01 }
0x5336C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53372: 				End  { 29 02 }
0x53374: 				Numeric Prompt: "Preset 9", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB51, VarStoreId: 0x6, VarOffset: 0x3E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 59 12 5B 12 51 0B 06 00 E0 03 10 10 00 3F 01 }
0x53385: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5338B: 				End  { 29 02 }
0x5338D: 				Numeric Prompt: "Preset 10", Help: "Choose the target preset value", QuestionFlags: 0x10, QuestionId: 0xB52, VarStoreId: 0x6, VarOffset: 0x3E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 5A 12 5B 12 52 0B 06 00 E1 03 10 10 00 3F 01 }
0x5339E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x533A4: 				End  { 29 02 }
0x533A6: 			End  { 29 02 }
0x533A8: 			SuppressIf  { 0A 82 }
0x533AA: 				EqIdVal QuestionId: 0xB42, Value: 0x1 { 12 86 42 0B 01 00 }
0x533B0: 					Not  { 17 02 }
0x533B2: 				End  { 29 02 }
0x533B4: 				Numeric Prompt: "Pre-cursor coefficient 0", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB53, VarStoreId: 0x6, VarOffset: 0x3C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 5C 12 70 12 53 0B 06 00 C3 03 10 10 00 3F 01 }
0x533C5: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x533CB: 				End  { 29 02 }
0x533CD: 				Numeric Prompt: "Post-cursor coefficient 0", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB54, VarStoreId: 0x6, VarOffset: 0x3CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 5D 12 71 12 54 0B 06 00 CD 03 10 10 00 3F 01 }
0x533DE: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x533E4: 				End  { 29 02 }
0x533E6: 				Numeric Prompt: "Pre-cursor coefficient 1", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB55, VarStoreId: 0x6, VarOffset: 0x3C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 5E 12 70 12 55 0B 06 00 C4 03 10 10 00 3F 01 }
0x533F7: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x533FD: 				End  { 29 02 }
0x533FF: 				Numeric Prompt: "Post-cursor coefficient 1", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB56, VarStoreId: 0x6, VarOffset: 0x3CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 5F 12 71 12 56 0B 06 00 CE 03 10 10 00 3F 01 }
0x53410: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53416: 				End  { 29 02 }
0x53418: 				Numeric Prompt: "Pre-cursor coefficient 2", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB57, VarStoreId: 0x6, VarOffset: 0x3C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 60 12 70 12 57 0B 06 00 C5 03 10 10 00 3F 01 }
0x53429: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5342F: 				End  { 29 02 }
0x53431: 				Numeric Prompt: "Post-cursor coefficient 2", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB58, VarStoreId: 0x6, VarOffset: 0x3CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 61 12 71 12 58 0B 06 00 CF 03 10 10 00 3F 01 }
0x53442: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53448: 				End  { 29 02 }
0x5344A: 				Numeric Prompt: "Pre-cursor coefficient 3", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB59, VarStoreId: 0x6, VarOffset: 0x3C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 62 12 70 12 59 0B 06 00 C6 03 10 10 00 3F 01 }
0x5345B: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53461: 				End  { 29 02 }
0x53463: 				Numeric Prompt: "Post-cursor coefficient 3", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB5A, VarStoreId: 0x6, VarOffset: 0x3D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 63 12 71 12 5A 0B 06 00 D0 03 10 10 00 3F 01 }
0x53474: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5347A: 				End  { 29 02 }
0x5347C: 				Numeric Prompt: "Pre-cursor coefficient 4", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB5B, VarStoreId: 0x6, VarOffset: 0x3C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 64 12 70 12 5B 0B 06 00 C7 03 10 10 00 3F 01 }
0x5348D: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53493: 				End  { 29 02 }
0x53495: 				Numeric Prompt: "Post-cursor coefficient 4", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB5C, VarStoreId: 0x6, VarOffset: 0x3D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 65 12 71 12 5C 0B 06 00 D1 03 10 10 00 3F 01 }
0x534A6: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x534AC: 				End  { 29 02 }
0x534AE: 				Numeric Prompt: "Pre-cursor coefficient 5", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB5D, VarStoreId: 0x6, VarOffset: 0x3C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 66 12 70 12 5D 0B 06 00 C8 03 10 10 00 3F 01 }
0x534BF: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x534C5: 				End  { 29 02 }
0x534C7: 				Numeric Prompt: "Post-cursor coefficient 5", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB5E, VarStoreId: 0x6, VarOffset: 0x3D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 67 12 71 12 5E 0B 06 00 D2 03 10 10 00 3F 01 }
0x534D8: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x534DE: 				End  { 29 02 }
0x534E0: 				Numeric Prompt: "Pre-cursor coefficient 6", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB5F, VarStoreId: 0x6, VarOffset: 0x3C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 68 12 70 12 5F 0B 06 00 C9 03 10 10 00 3F 01 }
0x534F1: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x534F7: 				End  { 29 02 }
0x534F9: 				Numeric Prompt: "Post-cursor coefficient 6", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB60, VarStoreId: 0x6, VarOffset: 0x3D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 69 12 71 12 60 0B 06 00 D3 03 10 10 00 3F 01 }
0x5350A: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53510: 				End  { 29 02 }
0x53512: 				Numeric Prompt: "Pre-cursor coefficient 7", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB61, VarStoreId: 0x6, VarOffset: 0x3CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 6A 12 70 12 61 0B 06 00 CA 03 10 10 00 3F 01 }
0x53523: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53529: 				End  { 29 02 }
0x5352B: 				Numeric Prompt: "Post-cursor coefficient 7", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB62, VarStoreId: 0x6, VarOffset: 0x3D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 6B 12 71 12 62 0B 06 00 D4 03 10 10 00 3F 01 }
0x5353C: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53542: 				End  { 29 02 }
0x53544: 				Numeric Prompt: "Pre-cursor coefficient 8", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB63, VarStoreId: 0x6, VarOffset: 0x3CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 6C 12 70 12 63 0B 06 00 CB 03 10 10 00 3F 01 }
0x53555: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5355B: 				End  { 29 02 }
0x5355D: 				Numeric Prompt: "Post-cursor coefficient 8", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB64, VarStoreId: 0x6, VarOffset: 0x3D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 6D 12 71 12 64 0B 06 00 D5 03 10 10 00 3F 01 }
0x5356E: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53574: 				End  { 29 02 }
0x53576: 				Numeric Prompt: "Pre-cursor coefficient 9", Help: "Choose the target pre-cursor coefficient value", QuestionFlags: 0x10, QuestionId: 0xB65, VarStoreId: 0x6, VarOffset: 0x3CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 6E 12 70 12 65 0B 06 00 CC 03 10 10 00 3F 01 }
0x53587: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5358D: 				End  { 29 02 }
0x5358F: 				Numeric Prompt: "Post-cursor coefficient 9", Help: "Choose the target post-curosr coefficient value", QuestionFlags: 0x10, QuestionId: 0xB66, VarStoreId: 0x6, VarOffset: 0x3D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1 { 07 91 6F 12 71 12 66 0B 06 00 D6 03 10 10 00 3F 01 }
0x535A0: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x535A6: 				End  { 29 02 }
0x535A8: 			End  { 29 02 }
0x535AA: 		End  { 29 02 }
0x535AC: 	End  { 29 02 }
0x535AE: 	Form FormId: 0x2830, Title: "PCI Express Root Port 1" { 01 86 30 28 76 16 }
0x535B4: 		OneOf Prompt: "PCI Express Root Port 1", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xB67, VarStoreId: 0x6, VarOffset: 0xFF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 60 13 7C 13 67 0B 06 00 FF 00 10 10 00 01 00 }
0x535C5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x535CC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x535D3: 		End  { 29 02 }
0x535D5: 		SuppressIf  { 0A 82 }
0x535D7: 			EqIdVal QuestionId: 0xB67, Value: 0x0 { 12 06 67 0B 00 00 }
0x535DD: 			GrayOutIf  { 19 82 }
0x535DF: 				EqIdVal QuestionId: 0xB75, Value: 0x1 { 12 06 75 0B 01 00 }
0x535E5: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xB68, VarStoreId: 0x6, VarOffset: 0x367, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 20 17 E5 0E 68 0B 06 00 67 03 10 10 00 01 00 }
0x535F6: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x535FD: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x53604: 				End  { 29 02 }
0x53606: 			End  { 29 02 }
0x53608: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27D3, VarStoreId: 0x6, VarOffset: 0x11B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 76 12 F5 0D D3 27 06 00 1B 01 10 10 00 04 00 }
0x53619: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53620: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x53627: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5362E: 			End  { 29 02 }
0x53630: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27D4, VarStoreId: 0x6, VarOffset: 0x2BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 92 12 AE 12 D4 27 06 00 BF 02 10 10 00 02 00 }
0x53641: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53648: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5364F: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x53656: 			End  { 29 02 }
0x53658: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB69, VarStoreId: 0x6, VarOffset: 0x2DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 12 CD 12 69 0B 06 00 DB 02 10 10 00 01 00 }
0x53669: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53670: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53677: 			End  { 29 02 }
0x53679: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xB6A, VarStoreId: 0x6, VarOffset: 0x2F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CE 12 A7 0E 6A 0B 06 00 F7 02 10 10 00 01 00 }
0x5368A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53691: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53698: 			End  { 29 02 }
0x5369A: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27D5, VarStoreId: 0x6, VarOffset: 0x313, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 12 06 13 D5 27 06 00 13 03 10 10 00 01 00 }
0x536AB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x536B2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x536B9: 			End  { 29 02 }
0x536BB: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xB6B, VarStoreId: 0x6, VarOffset: 0x32F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 13 23 13 6B 0B 06 00 2F 03 10 10 00 01 00 }
0x536CC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x536D3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x536DA: 			End  { 29 02 }
0x536DC: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xB6C, VarStoreId: 0x6, VarOffset: 0x34B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 13 40 13 6C 0B 06 00 4B 03 10 10 00 01 00 }
0x536ED: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x536F4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x536FB: 			End  { 29 02 }
0x536FD: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB6D, VarStoreId: 0x6, VarOffset: 0x137, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7D 13 99 13 6D 0B 06 00 37 01 10 10 00 01 00 }
0x5370E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53715: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5371C: 			End  { 29 02 }
0x5371E: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB6E, VarStoreId: 0x6, VarOffset: 0x153, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9A 13 B6 13 6E 0B 06 00 53 01 10 10 00 01 00 }
0x5372F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53736: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5373D: 			End  { 29 02 }
0x5373F: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB6F, VarStoreId: 0x6, VarOffset: 0x16F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 13 D3 13 6F 0B 06 00 6F 01 10 10 00 01 00 }
0x53750: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53757: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5375E: 			End  { 29 02 }
0x53760: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB70, VarStoreId: 0x6, VarOffset: 0x18B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D4 13 F0 13 70 0B 06 00 8B 01 10 10 00 01 00 }
0x53771: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53778: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5377F: 			End  { 29 02 }
0x53781: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB71, VarStoreId: 0x6, VarOffset: 0x1DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 13 11 14 71 0B 06 00 DF 01 10 10 00 01 00 }
0x53792: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53799: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x537A0: 			End  { 29 02 }
0x537A2: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB72, VarStoreId: 0x6, VarOffset: 0x1FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 12 14 2E 14 72 0B 06 00 FB 01 10 10 00 01 00 }
0x537B3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x537BA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x537C1: 			End  { 29 02 }
0x537C3: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB73, VarStoreId: 0x6, VarOffset: 0x217, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 14 4B 14 73 0B 06 00 17 02 10 10 00 01 00 }
0x537D4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x537DB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x537E2: 			End  { 29 02 }
0x537E4: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB74, VarStoreId: 0x6, VarOffset: 0x233, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4C 14 68 14 74 0B 06 00 33 02 10 10 00 01 00 }
0x537F5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x537FC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53803: 			End  { 29 02 }
0x53805: 			GrayOutIf  { 19 82 }
0x53807: 				EqIdVal QuestionId: 0xB68, Value: 0x0 { 12 06 68 0B 00 00 }
0x5380D: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB75, VarStoreId: 0x6, VarOffset: 0x24F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 14 85 14 75 0B 06 00 4F 02 10 10 00 01 00 }
0x5381E: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53825: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5382C: 				End  { 29 02 }
0x5382E: 			End  { 29 02 }
0x53830: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB76, VarStoreId: 0x6, VarOffset: 0x26B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 14 A2 14 76 0B 06 00 6B 02 10 10 00 01 00 }
0x53841: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53848: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5384F: 			End  { 29 02 }
0x53851: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xB77, VarStoreId: 0x6, VarOffset: 0x287, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 43 13 5F 13 77 0B 06 00 87 02 10 10 00 04 00 }
0x53862: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x53869: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x53870: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x53877: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5387E: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x53885: 			End  { 29 02 }
0x53887: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB78, VarStoreId: 0x6, VarOffset: 0x2A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 14 E2 14 78 0B 06 00 A3 02 10 10 00 01 00 }
0x53898: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5389F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x538A6: 			End  { 29 02 }
0x538A8: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xB79, VarStoreId: 0x6, VarOffset: 0x383, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E3 14 FF 14 79 0B 06 00 83 03 00 11 00 00 FF FF 01 00 }
0x538BC: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x538C3: 			End  { 29 02 }
0x538C5: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xB7A, VarStoreId: 0x6, VarOffset: 0x51F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 00 15 1C 15 7A 0B 06 00 1F 05 00 10 00 07 01 }
0x538D6: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x538DC: 			End  { 29 02 }
0x538DE: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xB7B, VarStoreId: 0x6, VarOffset: 0x53B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 1D 15 39 15 7B 0B 06 00 3B 05 00 11 01 00 14 00 01 00 }
0x538F2: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x538F9: 			End  { 29 02 }
0x538FB: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xB7C, VarStoreId: 0x6, VarOffset: 0x573, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 3A 15 56 15 7C 0B 06 00 73 05 00 10 04 14 04 }
0x5390C: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x53912: 			End  { 29 02 }
0x53914: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5391B: 			End  { 29 02 }
0x5391D: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x53924: 			End  { 29 02 }
0x53926: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xB7D, VarStoreId: 0x6, VarOffset: 0x3E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5E 15 7A 15 7D 0B 06 00 E3 03 10 10 00 01 00 }
0x53937: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5393E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53945: 			End  { 29 02 }
0x53947: 			SuppressIf  { 0A 82 }
0x53949: 				EqIdVal QuestionId: 0xB7D, Value: 0x0 { 12 06 7D 0B 00 00 }
0x5394F: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xB7E, VarStoreId: 0x6, VarOffset: 0x41B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 7B 15 23 16 7E 0B 06 00 1B 04 10 10 00 02 00 }
0x53960: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53967: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5396E: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x53975: 				End  { 29 02 }
0x53977: 				SuppressIf  { 0A 82 }
0x53979: 					EqIdVal QuestionId: 0xB7E, Value: 0x1 { 12 86 7E 0B 01 00 }
0x5397F: 						Not  { 17 02 }
0x53981: 					End  { 29 02 }
0x53983: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xB7F, VarStoreId: 0x6, VarOffset: 0x48B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 7D 15 25 16 7F 0B 06 00 8B 04 10 11 00 00 FF 03 01 00 }
0x53997: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5399E: 					End  { 29 02 }
0x539A0: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xB80, VarStoreId: 0x6, VarOffset: 0x437, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 7E 15 26 16 80 0B 06 00 37 04 10 10 00 05 00 }
0x539B1: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x539B8: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x539BF: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x539C6: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x539CD: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x539D4: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x539DB: 					End  { 29 02 }
0x539DD: 				End  { 29 02 }
0x539DF: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xB81, VarStoreId: 0x6, VarOffset: 0x453, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 7C 15 24 16 81 0B 06 00 53 04 10 10 00 02 00 }
0x539F0: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x539F7: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x539FE: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x53A05: 				End  { 29 02 }
0x53A07: 				SuppressIf  { 0A 82 }
0x53A09: 					EqIdVal QuestionId: 0xB81, Value: 0x1 { 12 86 81 0B 01 00 }
0x53A0F: 						Not  { 17 02 }
0x53A11: 					End  { 29 02 }
0x53A13: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xB82, VarStoreId: 0x6, VarOffset: 0x4C3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 7F 15 27 16 82 0B 06 00 C3 04 10 11 00 00 FF 03 01 00 }
0x53A27: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x53A2E: 					End  { 29 02 }
0x53A30: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xB83, VarStoreId: 0x6, VarOffset: 0x46F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 80 15 28 16 83 0B 06 00 6F 04 10 10 00 05 00 }
0x53A41: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x53A48: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x53A4F: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x53A56: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x53A5D: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x53A64: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x53A6B: 					End  { 29 02 }
0x53A6D: 				End  { 29 02 }
0x53A6F: 			End  { 29 02 }
0x53A71: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x53A78: 			End  { 29 02 }
0x53A7A: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xB84, VarStoreId: 0x6, VarOffset: 0x3FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 29 16 45 16 84 0B 06 00 FF 03 10 10 00 01 00 }
0x53A8B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53A92: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53A99: 			End  { 29 02 }
0x53A9B: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xB85, VarStoreId: 0x6, VarOffset: 0xBE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A7 14 C3 14 85 0B 06 00 BE 00 10 10 00 01 00 }
0x53AAC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53AB3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53ABA: 			End  { 29 02 }
0x53ABC: 		End  { 29 02 }
0x53ABE: 	End  { 29 02 }
0x53AC0: 	Form FormId: 0x2831, Title: "PCI Express Root Port 2" { 01 86 31 28 77 16 }
0x53AC6: 		OneOf Prompt: "PCI Express Root Port 2", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xB86, VarStoreId: 0x6, VarOffset: 0x100, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 13 7C 13 86 0B 06 00 00 01 10 10 00 01 00 }
0x53AD7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53ADE: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53AE5: 		End  { 29 02 }
0x53AE7: 		SuppressIf  { 0A 82 }
0x53AE9: 			EqIdVal QuestionId: 0xB86, Value: 0x0 { 12 06 86 0B 00 00 }
0x53AEF: 			GrayOutIf  { 19 82 }
0x53AF1: 				EqIdVal QuestionId: 0xB94, Value: 0x1 { 12 06 94 0B 01 00 }
0x53AF7: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xB87, VarStoreId: 0x6, VarOffset: 0x368, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 21 17 E5 0E 87 0B 06 00 68 03 10 10 00 01 00 }
0x53B08: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x53B0F: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x53B16: 				End  { 29 02 }
0x53B18: 			End  { 29 02 }
0x53B1A: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27D6, VarStoreId: 0x6, VarOffset: 0x11C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 77 12 F5 0D D6 27 06 00 1C 01 10 10 00 04 00 }
0x53B2B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53B32: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x53B39: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x53B40: 			End  { 29 02 }
0x53B42: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27D7, VarStoreId: 0x6, VarOffset: 0x2C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 93 12 AE 12 D7 27 06 00 C0 02 10 10 00 02 00 }
0x53B53: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53B5A: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x53B61: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x53B68: 			End  { 29 02 }
0x53B6A: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB88, VarStoreId: 0x6, VarOffset: 0x2DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 12 CD 12 88 0B 06 00 DC 02 10 10 00 01 00 }
0x53B7B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53B82: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53B89: 			End  { 29 02 }
0x53B8B: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xB89, VarStoreId: 0x6, VarOffset: 0x2F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 12 A7 0E 89 0B 06 00 F8 02 10 10 00 01 00 }
0x53B9C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53BA3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53BAA: 			End  { 29 02 }
0x53BAC: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27D8, VarStoreId: 0x6, VarOffset: 0x314, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 12 06 13 D8 27 06 00 14 03 10 10 00 01 00 }
0x53BBD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53BC4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53BCB: 			End  { 29 02 }
0x53BCD: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xB8A, VarStoreId: 0x6, VarOffset: 0x330, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 13 23 13 8A 0B 06 00 30 03 10 10 00 01 00 }
0x53BDE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53BE5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53BEC: 			End  { 29 02 }
0x53BEE: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xB8B, VarStoreId: 0x6, VarOffset: 0x34C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 25 13 40 13 8B 0B 06 00 4C 03 10 10 00 01 00 }
0x53BFF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53C06: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53C0D: 			End  { 29 02 }
0x53C0F: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB8C, VarStoreId: 0x6, VarOffset: 0x138, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7E 13 99 13 8C 0B 06 00 38 01 10 10 00 01 00 }
0x53C20: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53C27: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53C2E: 			End  { 29 02 }
0x53C30: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB8D, VarStoreId: 0x6, VarOffset: 0x154, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 13 B6 13 8D 0B 06 00 54 01 10 10 00 01 00 }
0x53C41: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53C48: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53C4F: 			End  { 29 02 }
0x53C51: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB8E, VarStoreId: 0x6, VarOffset: 0x170, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 13 D3 13 8E 0B 06 00 70 01 10 10 00 01 00 }
0x53C62: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53C69: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53C70: 			End  { 29 02 }
0x53C72: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB8F, VarStoreId: 0x6, VarOffset: 0x18C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D5 13 F0 13 8F 0B 06 00 8C 01 10 10 00 01 00 }
0x53C83: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53C8A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53C91: 			End  { 29 02 }
0x53C93: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB90, VarStoreId: 0x6, VarOffset: 0x1E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F6 13 11 14 90 0B 06 00 E0 01 10 10 00 01 00 }
0x53CA4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53CAB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53CB2: 			End  { 29 02 }
0x53CB4: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB91, VarStoreId: 0x6, VarOffset: 0x1FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 13 14 2E 14 91 0B 06 00 FC 01 10 10 00 01 00 }
0x53CC5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53CCC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53CD3: 			End  { 29 02 }
0x53CD5: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB92, VarStoreId: 0x6, VarOffset: 0x218, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 14 4B 14 92 0B 06 00 18 02 10 10 00 01 00 }
0x53CE6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53CED: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53CF4: 			End  { 29 02 }
0x53CF6: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB93, VarStoreId: 0x6, VarOffset: 0x234, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4D 14 68 14 93 0B 06 00 34 02 10 10 00 01 00 }
0x53D07: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53D0E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53D15: 			End  { 29 02 }
0x53D17: 			GrayOutIf  { 19 82 }
0x53D19: 				EqIdVal QuestionId: 0xB87, Value: 0x0 { 12 06 87 0B 00 00 }
0x53D1F: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB94, VarStoreId: 0x6, VarOffset: 0x250, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6A 14 85 14 94 0B 06 00 50 02 10 10 00 01 00 }
0x53D30: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53D37: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53D3E: 				End  { 29 02 }
0x53D40: 			End  { 29 02 }
0x53D42: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB95, VarStoreId: 0x6, VarOffset: 0x26C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 14 A2 14 95 0B 06 00 6C 02 10 10 00 01 00 }
0x53D53: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53D5A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53D61: 			End  { 29 02 }
0x53D63: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xB96, VarStoreId: 0x6, VarOffset: 0x288, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 44 13 5F 13 96 0B 06 00 88 02 10 10 00 04 00 }
0x53D74: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x53D7B: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x53D82: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x53D89: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x53D90: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x53D97: 			End  { 29 02 }
0x53D99: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xB97, VarStoreId: 0x6, VarOffset: 0x2A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C7 14 E2 14 97 0B 06 00 A4 02 10 10 00 01 00 }
0x53DAA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53DB1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53DB8: 			End  { 29 02 }
0x53DBA: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xB98, VarStoreId: 0x6, VarOffset: 0x385, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E4 14 FF 14 98 0B 06 00 85 03 00 11 00 00 FF FF 01 00 }
0x53DCE: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x53DD5: 			End  { 29 02 }
0x53DD7: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xB99, VarStoreId: 0x6, VarOffset: 0x520, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 01 15 1C 15 99 0B 06 00 20 05 00 10 00 07 01 }
0x53DE8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x53DEE: 			End  { 29 02 }
0x53DF0: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xB9A, VarStoreId: 0x6, VarOffset: 0x53D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 1E 15 39 15 9A 0B 06 00 3D 05 00 11 01 00 14 00 01 00 }
0x53E04: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x53E0B: 			End  { 29 02 }
0x53E0D: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xB9B, VarStoreId: 0x6, VarOffset: 0x574, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 3B 15 56 15 9B 0B 06 00 74 05 00 10 04 14 04 }
0x53E1E: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x53E24: 			End  { 29 02 }
0x53E26: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x53E2D: 			End  { 29 02 }
0x53E2F: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x53E36: 			End  { 29 02 }
0x53E38: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xB9C, VarStoreId: 0x6, VarOffset: 0x3E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5F 15 7A 15 9C 0B 06 00 E4 03 10 10 00 01 00 }
0x53E49: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53E50: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53E57: 			End  { 29 02 }
0x53E59: 			SuppressIf  { 0A 82 }
0x53E5B: 				EqIdVal QuestionId: 0xB9C, Value: 0x0 { 12 06 9C 0B 00 00 }
0x53E61: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xB9D, VarStoreId: 0x6, VarOffset: 0x41C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 81 15 23 16 9D 0B 06 00 1C 04 10 10 00 02 00 }
0x53E72: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53E79: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x53E80: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x53E87: 				End  { 29 02 }
0x53E89: 				SuppressIf  { 0A 82 }
0x53E8B: 					EqIdVal QuestionId: 0xB9D, Value: 0x1 { 12 86 9D 0B 01 00 }
0x53E91: 						Not  { 17 02 }
0x53E93: 					End  { 29 02 }
0x53E95: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xB9E, VarStoreId: 0x6, VarOffset: 0x48D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 83 15 25 16 9E 0B 06 00 8D 04 10 11 00 00 FF 03 01 00 }
0x53EA9: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x53EB0: 					End  { 29 02 }
0x53EB2: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xB9F, VarStoreId: 0x6, VarOffset: 0x438, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 84 15 26 16 9F 0B 06 00 38 04 10 10 00 05 00 }
0x53EC3: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x53ECA: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x53ED1: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x53ED8: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x53EDF: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x53EE6: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x53EED: 					End  { 29 02 }
0x53EEF: 				End  { 29 02 }
0x53EF1: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBA0, VarStoreId: 0x6, VarOffset: 0x454, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 82 15 24 16 A0 0B 06 00 54 04 10 10 00 02 00 }
0x53F02: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53F09: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x53F10: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x53F17: 				End  { 29 02 }
0x53F19: 				SuppressIf  { 0A 82 }
0x53F1B: 					EqIdVal QuestionId: 0xBA0, Value: 0x1 { 12 86 A0 0B 01 00 }
0x53F21: 						Not  { 17 02 }
0x53F23: 					End  { 29 02 }
0x53F25: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBA1, VarStoreId: 0x6, VarOffset: 0x4C5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 85 15 27 16 A1 0B 06 00 C5 04 10 11 00 00 FF 03 01 00 }
0x53F39: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x53F40: 					End  { 29 02 }
0x53F42: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBA2, VarStoreId: 0x6, VarOffset: 0x470, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 86 15 28 16 A2 0B 06 00 70 04 10 10 00 05 00 }
0x53F53: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x53F5A: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x53F61: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x53F68: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x53F6F: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x53F76: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x53F7D: 					End  { 29 02 }
0x53F7F: 				End  { 29 02 }
0x53F81: 			End  { 29 02 }
0x53F83: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x53F8A: 			End  { 29 02 }
0x53F8C: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xBA3, VarStoreId: 0x6, VarOffset: 0x400, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 16 45 16 A3 0B 06 00 00 04 10 10 00 01 00 }
0x53F9D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53FA4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53FAB: 			End  { 29 02 }
0x53FAD: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xBA4, VarStoreId: 0x6, VarOffset: 0xBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 14 C3 14 A4 0B 06 00 BF 00 10 10 00 01 00 }
0x53FBE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x53FC5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x53FCC: 			End  { 29 02 }
0x53FCE: 		End  { 29 02 }
0x53FD0: 	End  { 29 02 }
0x53FD2: 	Form FormId: 0x2832, Title: "PCI Express Root Port 3" { 01 86 32 28 78 16 }
0x53FD8: 		OneOf Prompt: "PCI Express Root Port 3", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xBA5, VarStoreId: 0x6, VarOffset: 0x101, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 62 13 7C 13 A5 0B 06 00 01 01 10 10 00 01 00 }
0x53FE9: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x53FF0: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x53FF7: 		End  { 29 02 }
0x53FF9: 		SuppressIf  { 0A 82 }
0x53FFB: 			EqIdVal QuestionId: 0xBA5, Value: 0x0 { 12 06 A5 0B 00 00 }
0x54001: 			GrayOutIf  { 19 82 }
0x54003: 				EqIdVal QuestionId: 0xBB3, Value: 0x1 { 12 06 B3 0B 01 00 }
0x54009: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xBA6, VarStoreId: 0x6, VarOffset: 0x369, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 17 E5 0E A6 0B 06 00 69 03 10 10 00 01 00 }
0x5401A: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x54021: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x54028: 				End  { 29 02 }
0x5402A: 			End  { 29 02 }
0x5402C: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27D9, VarStoreId: 0x6, VarOffset: 0x11D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 78 12 F5 0D D9 27 06 00 1D 01 10 10 00 04 00 }
0x5403D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54044: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5404B: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x54052: 			End  { 29 02 }
0x54054: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27DA, VarStoreId: 0x6, VarOffset: 0x2C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 94 12 AE 12 DA 27 06 00 C1 02 10 10 00 02 00 }
0x54065: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5406C: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x54073: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5407A: 			End  { 29 02 }
0x5407C: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBA7, VarStoreId: 0x6, VarOffset: 0x2DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 12 CD 12 A7 0B 06 00 DD 02 10 10 00 01 00 }
0x5408D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54094: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5409B: 			End  { 29 02 }
0x5409D: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xBA8, VarStoreId: 0x6, VarOffset: 0x2F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 12 A7 0E A8 0B 06 00 F9 02 10 10 00 01 00 }
0x540AE: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x540B5: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x540BC: 			End  { 29 02 }
0x540BE: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27DB, VarStoreId: 0x6, VarOffset: 0x315, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EC 12 06 13 DB 27 06 00 15 03 10 10 00 01 00 }
0x540CF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x540D6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x540DD: 			End  { 29 02 }
0x540DF: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xBA9, VarStoreId: 0x6, VarOffset: 0x331, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 13 23 13 A9 0B 06 00 31 03 10 10 00 01 00 }
0x540F0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x540F7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x540FE: 			End  { 29 02 }
0x54100: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xBAA, VarStoreId: 0x6, VarOffset: 0x34D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 13 40 13 AA 0B 06 00 4D 03 10 10 00 01 00 }
0x54111: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54118: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5411F: 			End  { 29 02 }
0x54121: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBAB, VarStoreId: 0x6, VarOffset: 0x139, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7F 13 99 13 AB 0B 06 00 39 01 10 10 00 01 00 }
0x54132: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54139: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54140: 			End  { 29 02 }
0x54142: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBAC, VarStoreId: 0x6, VarOffset: 0x155, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9C 13 B6 13 AC 0B 06 00 55 01 10 10 00 01 00 }
0x54153: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5415A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54161: 			End  { 29 02 }
0x54163: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBAD, VarStoreId: 0x6, VarOffset: 0x171, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 13 D3 13 AD 0B 06 00 71 01 10 10 00 01 00 }
0x54174: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5417B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54182: 			End  { 29 02 }
0x54184: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBAE, VarStoreId: 0x6, VarOffset: 0x18D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 13 F0 13 AE 0B 06 00 8D 01 10 10 00 01 00 }
0x54195: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5419C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x541A3: 			End  { 29 02 }
0x541A5: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBAF, VarStoreId: 0x6, VarOffset: 0x1E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F7 13 11 14 AF 0B 06 00 E1 01 10 10 00 01 00 }
0x541B6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x541BD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x541C4: 			End  { 29 02 }
0x541C6: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBB0, VarStoreId: 0x6, VarOffset: 0x1FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 14 2E 14 B0 0B 06 00 FD 01 10 10 00 01 00 }
0x541D7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x541DE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x541E5: 			End  { 29 02 }
0x541E7: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBB1, VarStoreId: 0x6, VarOffset: 0x219, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 14 4B 14 B1 0B 06 00 19 02 10 10 00 01 00 }
0x541F8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x541FF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54206: 			End  { 29 02 }
0x54208: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBB2, VarStoreId: 0x6, VarOffset: 0x235, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 14 68 14 B2 0B 06 00 35 02 10 10 00 01 00 }
0x54219: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54220: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54227: 			End  { 29 02 }
0x54229: 			GrayOutIf  { 19 82 }
0x5422B: 				EqIdVal QuestionId: 0xBA6, Value: 0x0 { 12 06 A6 0B 00 00 }
0x54231: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBB3, VarStoreId: 0x6, VarOffset: 0x251, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 14 85 14 B3 0B 06 00 51 02 10 10 00 01 00 }
0x54242: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54249: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54250: 				End  { 29 02 }
0x54252: 			End  { 29 02 }
0x54254: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBB4, VarStoreId: 0x6, VarOffset: 0x26D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 88 14 A2 14 B4 0B 06 00 6D 02 10 10 00 01 00 }
0x54265: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5426C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54273: 			End  { 29 02 }
0x54275: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xBB5, VarStoreId: 0x6, VarOffset: 0x289, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 45 13 5F 13 B5 0B 06 00 89 02 10 10 00 04 00 }
0x54286: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5428D: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x54294: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5429B: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x542A2: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x542A9: 			End  { 29 02 }
0x542AB: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBB6, VarStoreId: 0x6, VarOffset: 0x2A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 14 E2 14 B6 0B 06 00 A5 02 10 10 00 01 00 }
0x542BC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x542C3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x542CA: 			End  { 29 02 }
0x542CC: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xBB7, VarStoreId: 0x6, VarOffset: 0x387, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E5 14 FF 14 B7 0B 06 00 87 03 00 11 00 00 FF FF 01 00 }
0x542E0: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x542E7: 			End  { 29 02 }
0x542E9: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xBB8, VarStoreId: 0x6, VarOffset: 0x521, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 02 15 1C 15 B8 0B 06 00 21 05 00 10 00 07 01 }
0x542FA: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x54300: 			End  { 29 02 }
0x54302: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xBB9, VarStoreId: 0x6, VarOffset: 0x53F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 1F 15 39 15 B9 0B 06 00 3F 05 00 11 01 00 14 00 01 00 }
0x54316: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5431D: 			End  { 29 02 }
0x5431F: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xBBA, VarStoreId: 0x6, VarOffset: 0x575, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 3C 15 56 15 BA 0B 06 00 75 05 00 10 04 14 04 }
0x54330: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x54336: 			End  { 29 02 }
0x54338: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5433F: 			End  { 29 02 }
0x54341: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x54348: 			End  { 29 02 }
0x5434A: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xBBB, VarStoreId: 0x6, VarOffset: 0x3E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 60 15 7A 15 BB 0B 06 00 E5 03 10 10 00 01 00 }
0x5435B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54362: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54369: 			End  { 29 02 }
0x5436B: 			SuppressIf  { 0A 82 }
0x5436D: 				EqIdVal QuestionId: 0xBBB, Value: 0x0 { 12 06 BB 0B 00 00 }
0x54373: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBBC, VarStoreId: 0x6, VarOffset: 0x41D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 87 15 23 16 BC 0B 06 00 1D 04 10 10 00 02 00 }
0x54384: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5438B: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x54392: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x54399: 				End  { 29 02 }
0x5439B: 				SuppressIf  { 0A 82 }
0x5439D: 					EqIdVal QuestionId: 0xBBC, Value: 0x1 { 12 86 BC 0B 01 00 }
0x543A3: 						Not  { 17 02 }
0x543A5: 					End  { 29 02 }
0x543A7: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBBD, VarStoreId: 0x6, VarOffset: 0x48F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 89 15 25 16 BD 0B 06 00 8F 04 10 11 00 00 FF 03 01 00 }
0x543BB: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x543C2: 					End  { 29 02 }
0x543C4: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBBE, VarStoreId: 0x6, VarOffset: 0x439, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 8A 15 26 16 BE 0B 06 00 39 04 10 10 00 05 00 }
0x543D5: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x543DC: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x543E3: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x543EA: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x543F1: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x543F8: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x543FF: 					End  { 29 02 }
0x54401: 				End  { 29 02 }
0x54403: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBBF, VarStoreId: 0x6, VarOffset: 0x455, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 88 15 24 16 BF 0B 06 00 55 04 10 10 00 02 00 }
0x54414: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5441B: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x54422: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x54429: 				End  { 29 02 }
0x5442B: 				SuppressIf  { 0A 82 }
0x5442D: 					EqIdVal QuestionId: 0xBBF, Value: 0x1 { 12 86 BF 0B 01 00 }
0x54433: 						Not  { 17 02 }
0x54435: 					End  { 29 02 }
0x54437: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBC0, VarStoreId: 0x6, VarOffset: 0x4C7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 8B 15 27 16 C0 0B 06 00 C7 04 10 11 00 00 FF 03 01 00 }
0x5444B: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x54452: 					End  { 29 02 }
0x54454: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBC1, VarStoreId: 0x6, VarOffset: 0x471, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 8C 15 28 16 C1 0B 06 00 71 04 10 10 00 05 00 }
0x54465: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5446C: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x54473: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5447A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x54481: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x54488: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5448F: 					End  { 29 02 }
0x54491: 				End  { 29 02 }
0x54493: 			End  { 29 02 }
0x54495: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5449C: 			End  { 29 02 }
0x5449E: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xBC2, VarStoreId: 0x6, VarOffset: 0x401, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2B 16 45 16 C2 0B 06 00 01 04 10 10 00 01 00 }
0x544AF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x544B6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x544BD: 			End  { 29 02 }
0x544BF: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xBC3, VarStoreId: 0x6, VarOffset: 0xC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 14 C3 14 C3 0B 06 00 C0 00 10 10 00 01 00 }
0x544D0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x544D7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x544DE: 			End  { 29 02 }
0x544E0: 		End  { 29 02 }
0x544E2: 	End  { 29 02 }
0x544E4: 	Form FormId: 0x2833, Title: "PCI Express Root Port 4" { 01 86 33 28 79 16 }
0x544EA: 		OneOf Prompt: "PCI Express Root Port 4", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xBC4, VarStoreId: 0x6, VarOffset: 0x102, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 13 7C 13 C4 0B 06 00 02 01 10 10 00 01 00 }
0x544FB: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54502: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54509: 		End  { 29 02 }
0x5450B: 		SuppressIf  { 0A 82 }
0x5450D: 			EqIdVal QuestionId: 0xBC4, Value: 0x0 { 12 06 C4 0B 00 00 }
0x54513: 			GrayOutIf  { 19 82 }
0x54515: 				EqIdVal QuestionId: 0xBD2, Value: 0x1 { 12 06 D2 0B 01 00 }
0x5451B: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xBC5, VarStoreId: 0x6, VarOffset: 0x36A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 23 17 E5 0E C5 0B 06 00 6A 03 10 10 00 01 00 }
0x5452C: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x54533: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5453A: 				End  { 29 02 }
0x5453C: 			End  { 29 02 }
0x5453E: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27DC, VarStoreId: 0x6, VarOffset: 0x11E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 79 12 F5 0D DC 27 06 00 1E 01 10 10 00 04 00 }
0x5454F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54556: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5455D: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x54564: 			End  { 29 02 }
0x54566: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27DD, VarStoreId: 0x6, VarOffset: 0x2C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 95 12 AE 12 DD 27 06 00 C2 02 10 10 00 02 00 }
0x54577: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5457E: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x54585: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5458C: 			End  { 29 02 }
0x5458E: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBC6, VarStoreId: 0x6, VarOffset: 0x2DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 12 CD 12 C6 0B 06 00 DE 02 10 10 00 01 00 }
0x5459F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x545A6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x545AD: 			End  { 29 02 }
0x545AF: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xBC7, VarStoreId: 0x6, VarOffset: 0x2FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 12 A7 0E C7 0B 06 00 FA 02 10 10 00 01 00 }
0x545C0: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x545C7: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x545CE: 			End  { 29 02 }
0x545D0: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27DE, VarStoreId: 0x6, VarOffset: 0x316, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 ED 12 06 13 DE 27 06 00 16 03 10 10 00 01 00 }
0x545E1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x545E8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x545EF: 			End  { 29 02 }
0x545F1: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xBC8, VarStoreId: 0x6, VarOffset: 0x332, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 13 23 13 C8 0B 06 00 32 03 10 10 00 01 00 }
0x54602: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54609: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54610: 			End  { 29 02 }
0x54612: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xBC9, VarStoreId: 0x6, VarOffset: 0x34E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 13 40 13 C9 0B 06 00 4E 03 10 10 00 01 00 }
0x54623: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5462A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54631: 			End  { 29 02 }
0x54633: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBCA, VarStoreId: 0x6, VarOffset: 0x13A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 80 13 99 13 CA 0B 06 00 3A 01 10 10 00 01 00 }
0x54644: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5464B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54652: 			End  { 29 02 }
0x54654: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBCB, VarStoreId: 0x6, VarOffset: 0x156, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 13 B6 13 CB 0B 06 00 56 01 10 10 00 01 00 }
0x54665: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5466C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54673: 			End  { 29 02 }
0x54675: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBCC, VarStoreId: 0x6, VarOffset: 0x172, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 13 D3 13 CC 0B 06 00 72 01 10 10 00 01 00 }
0x54686: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5468D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54694: 			End  { 29 02 }
0x54696: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBCD, VarStoreId: 0x6, VarOffset: 0x18E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D7 13 F0 13 CD 0B 06 00 8E 01 10 10 00 01 00 }
0x546A7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x546AE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x546B5: 			End  { 29 02 }
0x546B7: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBCE, VarStoreId: 0x6, VarOffset: 0x1E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F8 13 11 14 CE 0B 06 00 E2 01 10 10 00 01 00 }
0x546C8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x546CF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x546D6: 			End  { 29 02 }
0x546D8: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBCF, VarStoreId: 0x6, VarOffset: 0x1FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 15 14 2E 14 CF 0B 06 00 FE 01 10 10 00 01 00 }
0x546E9: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x546F0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x546F7: 			End  { 29 02 }
0x546F9: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBD0, VarStoreId: 0x6, VarOffset: 0x21A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 14 4B 14 D0 0B 06 00 1A 02 10 10 00 01 00 }
0x5470A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54711: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54718: 			End  { 29 02 }
0x5471A: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBD1, VarStoreId: 0x6, VarOffset: 0x236, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4F 14 68 14 D1 0B 06 00 36 02 10 10 00 01 00 }
0x5472B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54732: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54739: 			End  { 29 02 }
0x5473B: 			GrayOutIf  { 19 82 }
0x5473D: 				EqIdVal QuestionId: 0xBC5, Value: 0x0 { 12 06 C5 0B 00 00 }
0x54743: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBD2, VarStoreId: 0x6, VarOffset: 0x252, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 14 85 14 D2 0B 06 00 52 02 10 10 00 01 00 }
0x54754: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5475B: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54762: 				End  { 29 02 }
0x54764: 			End  { 29 02 }
0x54766: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBD3, VarStoreId: 0x6, VarOffset: 0x26E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 14 A2 14 D3 0B 06 00 6E 02 10 10 00 01 00 }
0x54777: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5477E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54785: 			End  { 29 02 }
0x54787: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xBD4, VarStoreId: 0x6, VarOffset: 0x28A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 46 13 5F 13 D4 0B 06 00 8A 02 10 10 00 04 00 }
0x54798: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5479F: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x547A6: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x547AD: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x547B4: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x547BB: 			End  { 29 02 }
0x547BD: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBD5, VarStoreId: 0x6, VarOffset: 0x2A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C9 14 E2 14 D5 0B 06 00 A6 02 10 10 00 01 00 }
0x547CE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x547D5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x547DC: 			End  { 29 02 }
0x547DE: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xBD6, VarStoreId: 0x6, VarOffset: 0x389, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E6 14 FF 14 D6 0B 06 00 89 03 00 11 00 00 FF FF 01 00 }
0x547F2: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x547F9: 			End  { 29 02 }
0x547FB: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xBD7, VarStoreId: 0x6, VarOffset: 0x522, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 03 15 1C 15 D7 0B 06 00 22 05 00 10 00 07 01 }
0x5480C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x54812: 			End  { 29 02 }
0x54814: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xBD8, VarStoreId: 0x6, VarOffset: 0x541, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 20 15 39 15 D8 0B 06 00 41 05 00 11 01 00 14 00 01 00 }
0x54828: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5482F: 			End  { 29 02 }
0x54831: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xBD9, VarStoreId: 0x6, VarOffset: 0x576, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 3D 15 56 15 D9 0B 06 00 76 05 00 10 04 14 04 }
0x54842: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x54848: 			End  { 29 02 }
0x5484A: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x54851: 			End  { 29 02 }
0x54853: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5485A: 			End  { 29 02 }
0x5485C: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xBDA, VarStoreId: 0x6, VarOffset: 0x3E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 15 7A 15 DA 0B 06 00 E6 03 10 10 00 01 00 }
0x5486D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54874: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5487B: 			End  { 29 02 }
0x5487D: 			SuppressIf  { 0A 82 }
0x5487F: 				EqIdVal QuestionId: 0xBDA, Value: 0x0 { 12 06 DA 0B 00 00 }
0x54885: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBDB, VarStoreId: 0x6, VarOffset: 0x41E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8D 15 23 16 DB 0B 06 00 1E 04 10 10 00 02 00 }
0x54896: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5489D: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x548A4: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x548AB: 				End  { 29 02 }
0x548AD: 				SuppressIf  { 0A 82 }
0x548AF: 					EqIdVal QuestionId: 0xBDB, Value: 0x1 { 12 86 DB 0B 01 00 }
0x548B5: 						Not  { 17 02 }
0x548B7: 					End  { 29 02 }
0x548B9: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBDC, VarStoreId: 0x6, VarOffset: 0x491, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 8F 15 25 16 DC 0B 06 00 91 04 10 11 00 00 FF 03 01 00 }
0x548CD: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x548D4: 					End  { 29 02 }
0x548D6: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBDD, VarStoreId: 0x6, VarOffset: 0x43A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 90 15 26 16 DD 0B 06 00 3A 04 10 10 00 05 00 }
0x548E7: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x548EE: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x548F5: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x548FC: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x54903: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5490A: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x54911: 					End  { 29 02 }
0x54913: 				End  { 29 02 }
0x54915: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBDE, VarStoreId: 0x6, VarOffset: 0x456, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8E 15 24 16 DE 0B 06 00 56 04 10 10 00 02 00 }
0x54926: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5492D: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x54934: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5493B: 				End  { 29 02 }
0x5493D: 				SuppressIf  { 0A 82 }
0x5493F: 					EqIdVal QuestionId: 0xBDE, Value: 0x1 { 12 86 DE 0B 01 00 }
0x54945: 						Not  { 17 02 }
0x54947: 					End  { 29 02 }
0x54949: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBDF, VarStoreId: 0x6, VarOffset: 0x4C9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 91 15 27 16 DF 0B 06 00 C9 04 10 11 00 00 FF 03 01 00 }
0x5495D: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x54964: 					End  { 29 02 }
0x54966: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBE0, VarStoreId: 0x6, VarOffset: 0x472, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 92 15 28 16 E0 0B 06 00 72 04 10 10 00 05 00 }
0x54977: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5497E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x54985: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5498C: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x54993: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5499A: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x549A1: 					End  { 29 02 }
0x549A3: 				End  { 29 02 }
0x549A5: 			End  { 29 02 }
0x549A7: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x549AE: 			End  { 29 02 }
0x549B0: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xBE1, VarStoreId: 0x6, VarOffset: 0x402, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 16 45 16 E1 0B 06 00 02 04 10 10 00 01 00 }
0x549C1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x549C8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x549CF: 			End  { 29 02 }
0x549D1: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xBE2, VarStoreId: 0x6, VarOffset: 0xC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 14 C3 14 E2 0B 06 00 C1 00 10 10 00 01 00 }
0x549E2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x549E9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x549F0: 			End  { 29 02 }
0x549F2: 		End  { 29 02 }
0x549F4: 	End  { 29 02 }
0x549F6: 	Form FormId: 0x2834, Title: "PCI Express Root Port 5" { 01 86 34 28 7A 16 }
0x549FC: 		OneOf Prompt: "PCI Express Root Port 5", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xBE3, VarStoreId: 0x6, VarOffset: 0x103, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 64 13 7C 13 E3 0B 06 00 03 01 10 10 00 01 00 }
0x54A0D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54A14: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54A1B: 		End  { 29 02 }
0x54A1D: 		SuppressIf  { 0A 82 }
0x54A1F: 			EqIdVal QuestionId: 0xBE3, Value: 0x0 { 12 06 E3 0B 00 00 }
0x54A25: 			GrayOutIf  { 19 82 }
0x54A27: 				EqIdVal QuestionId: 0xBF1, Value: 0x1 { 12 06 F1 0B 01 00 }
0x54A2D: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xBE4, VarStoreId: 0x6, VarOffset: 0x36B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 17 E5 0E E4 0B 06 00 6B 03 10 10 00 01 00 }
0x54A3E: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x54A45: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x54A4C: 				End  { 29 02 }
0x54A4E: 			End  { 29 02 }
0x54A50: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27DF, VarStoreId: 0x6, VarOffset: 0x11F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 7A 12 F5 0D DF 27 06 00 1F 01 10 10 00 04 00 }
0x54A61: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54A68: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x54A6F: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x54A76: 			End  { 29 02 }
0x54A78: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27E0, VarStoreId: 0x6, VarOffset: 0x2C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 96 12 AE 12 E0 27 06 00 C3 02 10 10 00 02 00 }
0x54A89: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54A90: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x54A97: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x54A9E: 			End  { 29 02 }
0x54AA0: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBE5, VarStoreId: 0x6, VarOffset: 0x2DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 12 CD 12 E5 0B 06 00 DF 02 10 10 00 01 00 }
0x54AB1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54AB8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54ABF: 			End  { 29 02 }
0x54AC1: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xBE6, VarStoreId: 0x6, VarOffset: 0x2FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D2 12 A7 0E E6 0B 06 00 FB 02 10 10 00 01 00 }
0x54AD2: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54AD9: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54AE0: 			End  { 29 02 }
0x54AE2: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27E1, VarStoreId: 0x6, VarOffset: 0x317, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EE 12 06 13 E1 27 06 00 17 03 10 10 00 01 00 }
0x54AF3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54AFA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54B01: 			End  { 29 02 }
0x54B03: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xBE7, VarStoreId: 0x6, VarOffset: 0x333, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 13 23 13 E7 0B 06 00 33 03 10 10 00 01 00 }
0x54B14: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54B1B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54B22: 			End  { 29 02 }
0x54B24: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xBE8, VarStoreId: 0x6, VarOffset: 0x34F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 13 40 13 E8 0B 06 00 4F 03 10 10 00 01 00 }
0x54B35: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54B3C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54B43: 			End  { 29 02 }
0x54B45: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBE9, VarStoreId: 0x6, VarOffset: 0x13B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 81 13 99 13 E9 0B 06 00 3B 01 10 10 00 01 00 }
0x54B56: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54B5D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54B64: 			End  { 29 02 }
0x54B66: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBEA, VarStoreId: 0x6, VarOffset: 0x157, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9E 13 B6 13 EA 0B 06 00 57 01 10 10 00 01 00 }
0x54B77: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54B7E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54B85: 			End  { 29 02 }
0x54B87: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBEB, VarStoreId: 0x6, VarOffset: 0x173, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 13 D3 13 EB 0B 06 00 73 01 10 10 00 01 00 }
0x54B98: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54B9F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54BA6: 			End  { 29 02 }
0x54BA8: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBEC, VarStoreId: 0x6, VarOffset: 0x18F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D8 13 F0 13 EC 0B 06 00 8F 01 10 10 00 01 00 }
0x54BB9: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54BC0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54BC7: 			End  { 29 02 }
0x54BC9: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBED, VarStoreId: 0x6, VarOffset: 0x1E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 13 11 14 ED 0B 06 00 E3 01 10 10 00 01 00 }
0x54BDA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54BE1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54BE8: 			End  { 29 02 }
0x54BEA: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBEE, VarStoreId: 0x6, VarOffset: 0x1FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 16 14 2E 14 EE 0B 06 00 FF 01 10 10 00 01 00 }
0x54BFB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54C02: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54C09: 			End  { 29 02 }
0x54C0B: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBEF, VarStoreId: 0x6, VarOffset: 0x21B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 14 4B 14 EF 0B 06 00 1B 02 10 10 00 01 00 }
0x54C1C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54C23: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54C2A: 			End  { 29 02 }
0x54C2C: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBF0, VarStoreId: 0x6, VarOffset: 0x237, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 50 14 68 14 F0 0B 06 00 37 02 10 10 00 01 00 }
0x54C3D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54C44: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54C4B: 			End  { 29 02 }
0x54C4D: 			GrayOutIf  { 19 82 }
0x54C4F: 				EqIdVal QuestionId: 0xBE4, Value: 0x0 { 12 06 E4 0B 00 00 }
0x54C55: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBF1, VarStoreId: 0x6, VarOffset: 0x253, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 14 85 14 F1 0B 06 00 53 02 10 10 00 01 00 }
0x54C66: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54C6D: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54C74: 				End  { 29 02 }
0x54C76: 			End  { 29 02 }
0x54C78: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBF2, VarStoreId: 0x6, VarOffset: 0x26F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 14 A2 14 F2 0B 06 00 6F 02 10 10 00 01 00 }
0x54C89: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54C90: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54C97: 			End  { 29 02 }
0x54C99: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xBF3, VarStoreId: 0x6, VarOffset: 0x28B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 47 13 5F 13 F3 0B 06 00 8B 02 10 10 00 04 00 }
0x54CAA: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x54CB1: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x54CB8: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x54CBF: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x54CC6: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x54CCD: 			End  { 29 02 }
0x54CCF: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xBF4, VarStoreId: 0x6, VarOffset: 0x2A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 14 E2 14 F4 0B 06 00 A7 02 10 10 00 01 00 }
0x54CE0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54CE7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54CEE: 			End  { 29 02 }
0x54CF0: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xBF5, VarStoreId: 0x6, VarOffset: 0x38B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E7 14 FF 14 F5 0B 06 00 8B 03 00 11 00 00 FF FF 01 00 }
0x54D04: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x54D0B: 			End  { 29 02 }
0x54D0D: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xBF6, VarStoreId: 0x6, VarOffset: 0x523, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 04 15 1C 15 F6 0B 06 00 23 05 00 10 00 07 01 }
0x54D1E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x54D24: 			End  { 29 02 }
0x54D26: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xBF7, VarStoreId: 0x6, VarOffset: 0x543, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 21 15 39 15 F7 0B 06 00 43 05 00 11 01 00 14 00 01 00 }
0x54D3A: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x54D41: 			End  { 29 02 }
0x54D43: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xBF8, VarStoreId: 0x6, VarOffset: 0x577, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 3E 15 56 15 F8 0B 06 00 77 05 00 10 04 14 04 }
0x54D54: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x54D5A: 			End  { 29 02 }
0x54D5C: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x54D63: 			End  { 29 02 }
0x54D65: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x54D6C: 			End  { 29 02 }
0x54D6E: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xBF9, VarStoreId: 0x6, VarOffset: 0x3E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 62 15 7A 15 F9 0B 06 00 E7 03 10 10 00 01 00 }
0x54D7F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54D86: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54D8D: 			End  { 29 02 }
0x54D8F: 			SuppressIf  { 0A 82 }
0x54D91: 				EqIdVal QuestionId: 0xBF9, Value: 0x0 { 12 06 F9 0B 00 00 }
0x54D97: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBFA, VarStoreId: 0x6, VarOffset: 0x41F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 93 15 23 16 FA 0B 06 00 1F 04 10 10 00 02 00 }
0x54DA8: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54DAF: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x54DB6: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x54DBD: 				End  { 29 02 }
0x54DBF: 				SuppressIf  { 0A 82 }
0x54DC1: 					EqIdVal QuestionId: 0xBFA, Value: 0x1 { 12 86 FA 0B 01 00 }
0x54DC7: 						Not  { 17 02 }
0x54DC9: 					End  { 29 02 }
0x54DCB: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBFB, VarStoreId: 0x6, VarOffset: 0x493, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 95 15 25 16 FB 0B 06 00 93 04 10 11 00 00 FF 03 01 00 }
0x54DDF: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x54DE6: 					End  { 29 02 }
0x54DE8: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBFC, VarStoreId: 0x6, VarOffset: 0x43B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 96 15 26 16 FC 0B 06 00 3B 04 10 10 00 05 00 }
0x54DF9: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x54E00: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x54E07: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x54E0E: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x54E15: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x54E1C: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x54E23: 					End  { 29 02 }
0x54E25: 				End  { 29 02 }
0x54E27: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xBFD, VarStoreId: 0x6, VarOffset: 0x457, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 94 15 24 16 FD 0B 06 00 57 04 10 10 00 02 00 }
0x54E38: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54E3F: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x54E46: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x54E4D: 				End  { 29 02 }
0x54E4F: 				SuppressIf  { 0A 82 }
0x54E51: 					EqIdVal QuestionId: 0xBFD, Value: 0x1 { 12 86 FD 0B 01 00 }
0x54E57: 						Not  { 17 02 }
0x54E59: 					End  { 29 02 }
0x54E5B: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBFE, VarStoreId: 0x6, VarOffset: 0x4CB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 97 15 27 16 FE 0B 06 00 CB 04 10 11 00 00 FF 03 01 00 }
0x54E6F: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x54E76: 					End  { 29 02 }
0x54E78: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xBFF, VarStoreId: 0x6, VarOffset: 0x473, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 98 15 28 16 FF 0B 06 00 73 04 10 10 00 05 00 }
0x54E89: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x54E90: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x54E97: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x54E9E: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x54EA5: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x54EAC: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x54EB3: 					End  { 29 02 }
0x54EB5: 				End  { 29 02 }
0x54EB7: 			End  { 29 02 }
0x54EB9: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x54EC0: 			End  { 29 02 }
0x54EC2: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xC00, VarStoreId: 0x6, VarOffset: 0x403, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 16 45 16 00 0C 06 00 03 04 10 10 00 01 00 }
0x54ED3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54EDA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54EE1: 			End  { 29 02 }
0x54EE3: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC01, VarStoreId: 0x6, VarOffset: 0xC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AB 14 C3 14 01 0C 06 00 C2 00 10 10 00 01 00 }
0x54EF4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x54EFB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x54F02: 			End  { 29 02 }
0x54F04: 		End  { 29 02 }
0x54F06: 	End  { 29 02 }
0x54F08: 	Form FormId: 0x2835, Title: "PCI Express Root Port 6" { 01 86 35 28 7B 16 }
0x54F0E: 		OneOf Prompt: "PCI Express Root Port 6", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xC02, VarStoreId: 0x6, VarOffset: 0x104, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 13 7C 13 02 0C 06 00 04 01 10 10 00 01 00 }
0x54F1F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54F26: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54F2D: 		End  { 29 02 }
0x54F2F: 		SuppressIf  { 0A 82 }
0x54F31: 			EqIdVal QuestionId: 0xC02, Value: 0x0 { 12 06 02 0C 00 00 }
0x54F37: 			GrayOutIf  { 19 82 }
0x54F39: 				EqIdVal QuestionId: 0xC10, Value: 0x1 { 12 06 10 0C 01 00 }
0x54F3F: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xC03, VarStoreId: 0x6, VarOffset: 0x36C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 25 17 E5 0E 03 0C 06 00 6C 03 10 10 00 01 00 }
0x54F50: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x54F57: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x54F5E: 				End  { 29 02 }
0x54F60: 			End  { 29 02 }
0x54F62: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27E2, VarStoreId: 0x6, VarOffset: 0x120, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 7B 12 F5 0D E2 27 06 00 20 01 10 10 00 04 00 }
0x54F73: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54F7A: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x54F81: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x54F88: 			End  { 29 02 }
0x54F8A: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27E3, VarStoreId: 0x6, VarOffset: 0x2C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 97 12 AE 12 E3 27 06 00 C4 02 10 10 00 02 00 }
0x54F9B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54FA2: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x54FA9: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x54FB0: 			End  { 29 02 }
0x54FB2: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC04, VarStoreId: 0x6, VarOffset: 0x2E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 12 CD 12 04 0C 06 00 E0 02 10 10 00 01 00 }
0x54FC3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54FCA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54FD1: 			End  { 29 02 }
0x54FD3: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xC05, VarStoreId: 0x6, VarOffset: 0x2FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D3 12 A7 0E 05 0C 06 00 FC 02 10 10 00 01 00 }
0x54FE4: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x54FEB: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x54FF2: 			End  { 29 02 }
0x54FF4: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27E4, VarStoreId: 0x6, VarOffset: 0x318, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EF 12 06 13 E4 27 06 00 18 03 10 10 00 01 00 }
0x55005: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5500C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55013: 			End  { 29 02 }
0x55015: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC06, VarStoreId: 0x6, VarOffset: 0x334, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0C 13 23 13 06 0C 06 00 34 03 10 10 00 01 00 }
0x55026: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5502D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55034: 			End  { 29 02 }
0x55036: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC07, VarStoreId: 0x6, VarOffset: 0x350, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 29 13 40 13 07 0C 06 00 50 03 10 10 00 01 00 }
0x55047: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5504E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55055: 			End  { 29 02 }
0x55057: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC08, VarStoreId: 0x6, VarOffset: 0x13C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 13 99 13 08 0C 06 00 3C 01 10 10 00 01 00 }
0x55068: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5506F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55076: 			End  { 29 02 }
0x55078: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC09, VarStoreId: 0x6, VarOffset: 0x158, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 13 B6 13 09 0C 06 00 58 01 10 10 00 01 00 }
0x55089: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55090: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55097: 			End  { 29 02 }
0x55099: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC0A, VarStoreId: 0x6, VarOffset: 0x174, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 13 D3 13 0A 0C 06 00 74 01 10 10 00 01 00 }
0x550AA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x550B1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x550B8: 			End  { 29 02 }
0x550BA: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC0B, VarStoreId: 0x6, VarOffset: 0x190, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D9 13 F0 13 0B 0C 06 00 90 01 10 10 00 01 00 }
0x550CB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x550D2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x550D9: 			End  { 29 02 }
0x550DB: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC0C, VarStoreId: 0x6, VarOffset: 0x1E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 13 11 14 0C 0C 06 00 E4 01 10 10 00 01 00 }
0x550EC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x550F3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x550FA: 			End  { 29 02 }
0x550FC: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC0D, VarStoreId: 0x6, VarOffset: 0x200, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 17 14 2E 14 0D 0C 06 00 00 02 10 10 00 01 00 }
0x5510D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55114: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5511B: 			End  { 29 02 }
0x5511D: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC0E, VarStoreId: 0x6, VarOffset: 0x21C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 14 4B 14 0E 0C 06 00 1C 02 10 10 00 01 00 }
0x5512E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55135: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5513C: 			End  { 29 02 }
0x5513E: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC0F, VarStoreId: 0x6, VarOffset: 0x238, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 51 14 68 14 0F 0C 06 00 38 02 10 10 00 01 00 }
0x5514F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55156: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5515D: 			End  { 29 02 }
0x5515F: 			GrayOutIf  { 19 82 }
0x55161: 				EqIdVal QuestionId: 0xC03, Value: 0x0 { 12 06 03 0C 00 00 }
0x55167: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC10, VarStoreId: 0x6, VarOffset: 0x254, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 14 85 14 10 0C 06 00 54 02 10 10 00 01 00 }
0x55178: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5517F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55186: 				End  { 29 02 }
0x55188: 			End  { 29 02 }
0x5518A: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC11, VarStoreId: 0x6, VarOffset: 0x270, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 14 A2 14 11 0C 06 00 70 02 10 10 00 01 00 }
0x5519B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x551A2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x551A9: 			End  { 29 02 }
0x551AB: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xC12, VarStoreId: 0x6, VarOffset: 0x28C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 48 13 5F 13 12 0C 06 00 8C 02 10 10 00 04 00 }
0x551BC: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x551C3: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x551CA: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x551D1: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x551D8: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x551DF: 			End  { 29 02 }
0x551E1: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC13, VarStoreId: 0x6, VarOffset: 0x2A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CB 14 E2 14 13 0C 06 00 A8 02 10 10 00 01 00 }
0x551F2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x551F9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55200: 			End  { 29 02 }
0x55202: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xC14, VarStoreId: 0x6, VarOffset: 0x38D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E8 14 FF 14 14 0C 06 00 8D 03 00 11 00 00 FF FF 01 00 }
0x55216: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5521D: 			End  { 29 02 }
0x5521F: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC15, VarStoreId: 0x6, VarOffset: 0x524, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 05 15 1C 15 15 0C 06 00 24 05 00 10 00 07 01 }
0x55230: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x55236: 			End  { 29 02 }
0x55238: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xC16, VarStoreId: 0x6, VarOffset: 0x545, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 22 15 39 15 16 0C 06 00 45 05 00 11 01 00 14 00 01 00 }
0x5524C: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x55253: 			End  { 29 02 }
0x55255: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC17, VarStoreId: 0x6, VarOffset: 0x578, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 3F 15 56 15 17 0C 06 00 78 05 00 10 04 14 04 }
0x55266: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5526C: 			End  { 29 02 }
0x5526E: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x55275: 			End  { 29 02 }
0x55277: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5527E: 			End  { 29 02 }
0x55280: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC18, VarStoreId: 0x6, VarOffset: 0x3E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 15 7A 15 18 0C 06 00 E8 03 10 10 00 01 00 }
0x55291: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55298: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5529F: 			End  { 29 02 }
0x552A1: 			SuppressIf  { 0A 82 }
0x552A3: 				EqIdVal QuestionId: 0xC18, Value: 0x0 { 12 06 18 0C 00 00 }
0x552A9: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC19, VarStoreId: 0x6, VarOffset: 0x420, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 99 15 23 16 19 0C 06 00 20 04 10 10 00 02 00 }
0x552BA: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x552C1: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x552C8: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x552CF: 				End  { 29 02 }
0x552D1: 				SuppressIf  { 0A 82 }
0x552D3: 					EqIdVal QuestionId: 0xC19, Value: 0x1 { 12 86 19 0C 01 00 }
0x552D9: 						Not  { 17 02 }
0x552DB: 					End  { 29 02 }
0x552DD: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC1A, VarStoreId: 0x6, VarOffset: 0x495, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 9B 15 25 16 1A 0C 06 00 95 04 10 11 00 00 FF 03 01 00 }
0x552F1: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x552F8: 					End  { 29 02 }
0x552FA: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC1B, VarStoreId: 0x6, VarOffset: 0x43C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 9C 15 26 16 1B 0C 06 00 3C 04 10 10 00 05 00 }
0x5530B: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x55312: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x55319: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x55320: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x55327: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5532E: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x55335: 					End  { 29 02 }
0x55337: 				End  { 29 02 }
0x55339: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC1C, VarStoreId: 0x6, VarOffset: 0x458, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9A 15 24 16 1C 0C 06 00 58 04 10 10 00 02 00 }
0x5534A: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55351: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x55358: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5535F: 				End  { 29 02 }
0x55361: 				SuppressIf  { 0A 82 }
0x55363: 					EqIdVal QuestionId: 0xC1C, Value: 0x1 { 12 86 1C 0C 01 00 }
0x55369: 						Not  { 17 02 }
0x5536B: 					End  { 29 02 }
0x5536D: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC1D, VarStoreId: 0x6, VarOffset: 0x4CD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 9D 15 27 16 1D 0C 06 00 CD 04 10 11 00 00 FF 03 01 00 }
0x55381: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x55388: 					End  { 29 02 }
0x5538A: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC1E, VarStoreId: 0x6, VarOffset: 0x474, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 9E 15 28 16 1E 0C 06 00 74 04 10 10 00 05 00 }
0x5539B: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x553A2: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x553A9: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x553B0: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x553B7: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x553BE: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x553C5: 					End  { 29 02 }
0x553C7: 				End  { 29 02 }
0x553C9: 			End  { 29 02 }
0x553CB: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x553D2: 			End  { 29 02 }
0x553D4: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xC1F, VarStoreId: 0x6, VarOffset: 0x404, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 16 45 16 1F 0C 06 00 04 04 10 10 00 01 00 }
0x553E5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x553EC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x553F3: 			End  { 29 02 }
0x553F5: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC20, VarStoreId: 0x6, VarOffset: 0xC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 14 C3 14 20 0C 06 00 C3 00 10 10 00 01 00 }
0x55406: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5540D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55414: 			End  { 29 02 }
0x55416: 		End  { 29 02 }
0x55418: 	End  { 29 02 }
0x5541A: 	Form FormId: 0x2836, Title: "PCI Express Root Port 7" { 01 86 36 28 7C 16 }
0x55420: 		OneOf Prompt: "PCI Express Root Port 7", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xC21, VarStoreId: 0x6, VarOffset: 0x105, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 66 13 7C 13 21 0C 06 00 05 01 10 10 00 01 00 }
0x55431: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55438: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5543F: 		End  { 29 02 }
0x55441: 		SuppressIf  { 0A 82 }
0x55443: 			EqIdVal QuestionId: 0xC21, Value: 0x0 { 12 06 21 0C 00 00 }
0x55449: 			GrayOutIf  { 19 82 }
0x5544B: 				EqIdVal QuestionId: 0xC2F, Value: 0x1 { 12 06 2F 0C 01 00 }
0x55451: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xC22, VarStoreId: 0x6, VarOffset: 0x36D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 17 E5 0E 22 0C 06 00 6D 03 10 10 00 01 00 }
0x55462: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x55469: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x55470: 				End  { 29 02 }
0x55472: 			End  { 29 02 }
0x55474: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27E5, VarStoreId: 0x6, VarOffset: 0x121, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 7C 12 F5 0D E5 27 06 00 21 01 10 10 00 04 00 }
0x55485: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5548C: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x55493: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5549A: 			End  { 29 02 }
0x5549C: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27E6, VarStoreId: 0x6, VarOffset: 0x2C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 98 12 AE 12 E6 27 06 00 C5 02 10 10 00 02 00 }
0x554AD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x554B4: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x554BB: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x554C2: 			End  { 29 02 }
0x554C4: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC23, VarStoreId: 0x6, VarOffset: 0x2E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 12 CD 12 23 0C 06 00 E1 02 10 10 00 01 00 }
0x554D5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x554DC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x554E3: 			End  { 29 02 }
0x554E5: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xC24, VarStoreId: 0x6, VarOffset: 0x2FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D4 12 A7 0E 24 0C 06 00 FD 02 10 10 00 01 00 }
0x554F6: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x554FD: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55504: 			End  { 29 02 }
0x55506: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27E7, VarStoreId: 0x6, VarOffset: 0x319, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F0 12 06 13 E7 27 06 00 19 03 10 10 00 01 00 }
0x55517: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5551E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55525: 			End  { 29 02 }
0x55527: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC25, VarStoreId: 0x6, VarOffset: 0x335, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0D 13 23 13 25 0C 06 00 35 03 10 10 00 01 00 }
0x55538: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5553F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55546: 			End  { 29 02 }
0x55548: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC26, VarStoreId: 0x6, VarOffset: 0x351, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 13 40 13 26 0C 06 00 51 03 10 10 00 01 00 }
0x55559: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55560: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55567: 			End  { 29 02 }
0x55569: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC27, VarStoreId: 0x6, VarOffset: 0x13D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 83 13 99 13 27 0C 06 00 3D 01 10 10 00 01 00 }
0x5557A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55581: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55588: 			End  { 29 02 }
0x5558A: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC28, VarStoreId: 0x6, VarOffset: 0x159, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 13 B6 13 28 0C 06 00 59 01 10 10 00 01 00 }
0x5559B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x555A2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x555A9: 			End  { 29 02 }
0x555AB: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC29, VarStoreId: 0x6, VarOffset: 0x175, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 13 D3 13 29 0C 06 00 75 01 10 10 00 01 00 }
0x555BC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x555C3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x555CA: 			End  { 29 02 }
0x555CC: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC2A, VarStoreId: 0x6, VarOffset: 0x191, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DA 13 F0 13 2A 0C 06 00 91 01 10 10 00 01 00 }
0x555DD: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x555E4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x555EB: 			End  { 29 02 }
0x555ED: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC2B, VarStoreId: 0x6, VarOffset: 0x1E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FB 13 11 14 2B 0C 06 00 E5 01 10 10 00 01 00 }
0x555FE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55605: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5560C: 			End  { 29 02 }
0x5560E: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC2C, VarStoreId: 0x6, VarOffset: 0x201, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 18 14 2E 14 2C 0C 06 00 01 02 10 10 00 01 00 }
0x5561F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55626: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5562D: 			End  { 29 02 }
0x5562F: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC2D, VarStoreId: 0x6, VarOffset: 0x21D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 35 14 4B 14 2D 0C 06 00 1D 02 10 10 00 01 00 }
0x55640: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55647: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5564E: 			End  { 29 02 }
0x55650: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC2E, VarStoreId: 0x6, VarOffset: 0x239, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 52 14 68 14 2E 0C 06 00 39 02 10 10 00 01 00 }
0x55661: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55668: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5566F: 			End  { 29 02 }
0x55671: 			GrayOutIf  { 19 82 }
0x55673: 				EqIdVal QuestionId: 0xC22, Value: 0x0 { 12 06 22 0C 00 00 }
0x55679: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC2F, VarStoreId: 0x6, VarOffset: 0x255, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6F 14 85 14 2F 0C 06 00 55 02 10 10 00 01 00 }
0x5568A: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55691: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55698: 				End  { 29 02 }
0x5569A: 			End  { 29 02 }
0x5569C: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC30, VarStoreId: 0x6, VarOffset: 0x271, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 14 A2 14 30 0C 06 00 71 02 10 10 00 01 00 }
0x556AD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x556B4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x556BB: 			End  { 29 02 }
0x556BD: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xC31, VarStoreId: 0x6, VarOffset: 0x28D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 49 13 5F 13 31 0C 06 00 8D 02 10 10 00 04 00 }
0x556CE: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x556D5: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x556DC: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x556E3: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x556EA: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x556F1: 			End  { 29 02 }
0x556F3: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC32, VarStoreId: 0x6, VarOffset: 0x2A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CC 14 E2 14 32 0C 06 00 A9 02 10 10 00 01 00 }
0x55704: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5570B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55712: 			End  { 29 02 }
0x55714: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xC33, VarStoreId: 0x6, VarOffset: 0x38F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 E9 14 FF 14 33 0C 06 00 8F 03 00 11 00 00 FF FF 01 00 }
0x55728: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5572F: 			End  { 29 02 }
0x55731: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC34, VarStoreId: 0x6, VarOffset: 0x525, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 06 15 1C 15 34 0C 06 00 25 05 00 10 00 07 01 }
0x55742: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x55748: 			End  { 29 02 }
0x5574A: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xC35, VarStoreId: 0x6, VarOffset: 0x547, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 23 15 39 15 35 0C 06 00 47 05 00 11 01 00 14 00 01 00 }
0x5575E: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x55765: 			End  { 29 02 }
0x55767: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC36, VarStoreId: 0x6, VarOffset: 0x579, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 40 15 56 15 36 0C 06 00 79 05 00 10 04 14 04 }
0x55778: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5577E: 			End  { 29 02 }
0x55780: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x55787: 			End  { 29 02 }
0x55789: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x55790: 			End  { 29 02 }
0x55792: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC37, VarStoreId: 0x6, VarOffset: 0x3E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 64 15 7A 15 37 0C 06 00 E9 03 10 10 00 01 00 }
0x557A3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x557AA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x557B1: 			End  { 29 02 }
0x557B3: 			SuppressIf  { 0A 82 }
0x557B5: 				EqIdVal QuestionId: 0xC37, Value: 0x0 { 12 06 37 0C 00 00 }
0x557BB: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC38, VarStoreId: 0x6, VarOffset: 0x421, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9F 15 23 16 38 0C 06 00 21 04 10 10 00 02 00 }
0x557CC: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x557D3: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x557DA: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x557E1: 				End  { 29 02 }
0x557E3: 				SuppressIf  { 0A 82 }
0x557E5: 					EqIdVal QuestionId: 0xC38, Value: 0x1 { 12 86 38 0C 01 00 }
0x557EB: 						Not  { 17 02 }
0x557ED: 					End  { 29 02 }
0x557EF: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC39, VarStoreId: 0x6, VarOffset: 0x497, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 A1 15 25 16 39 0C 06 00 97 04 10 11 00 00 FF 03 01 00 }
0x55803: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5580A: 					End  { 29 02 }
0x5580C: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC3A, VarStoreId: 0x6, VarOffset: 0x43D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 A2 15 26 16 3A 0C 06 00 3D 04 10 10 00 05 00 }
0x5581D: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x55824: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5582B: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x55832: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x55839: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x55840: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x55847: 					End  { 29 02 }
0x55849: 				End  { 29 02 }
0x5584B: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC3B, VarStoreId: 0x6, VarOffset: 0x459, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A0 15 24 16 3B 0C 06 00 59 04 10 10 00 02 00 }
0x5585C: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55863: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5586A: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x55871: 				End  { 29 02 }
0x55873: 				SuppressIf  { 0A 82 }
0x55875: 					EqIdVal QuestionId: 0xC3B, Value: 0x1 { 12 86 3B 0C 01 00 }
0x5587B: 						Not  { 17 02 }
0x5587D: 					End  { 29 02 }
0x5587F: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC3C, VarStoreId: 0x6, VarOffset: 0x4CF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 A3 15 27 16 3C 0C 06 00 CF 04 10 11 00 00 FF 03 01 00 }
0x55893: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5589A: 					End  { 29 02 }
0x5589C: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC3D, VarStoreId: 0x6, VarOffset: 0x475, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 A4 15 28 16 3D 0C 06 00 75 04 10 10 00 05 00 }
0x558AD: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x558B4: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x558BB: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x558C2: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x558C9: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x558D0: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x558D7: 					End  { 29 02 }
0x558D9: 				End  { 29 02 }
0x558DB: 			End  { 29 02 }
0x558DD: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x558E4: 			End  { 29 02 }
0x558E6: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xC3E, VarStoreId: 0x6, VarOffset: 0x405, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 16 45 16 3E 0C 06 00 05 04 10 10 00 01 00 }
0x558F7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x558FE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55905: 			End  { 29 02 }
0x55907: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC3F, VarStoreId: 0x6, VarOffset: 0xC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 14 C3 14 3F 0C 06 00 C4 00 10 10 00 01 00 }
0x55918: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5591F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55926: 			End  { 29 02 }
0x55928: 		End  { 29 02 }
0x5592A: 	End  { 29 02 }
0x5592C: 	Form FormId: 0x2837, Title: "PCI Express Root Port 8" { 01 86 37 28 7D 16 }
0x55932: 		OneOf Prompt: "PCI Express Root Port 8", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xC40, VarStoreId: 0x6, VarOffset: 0x106, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 13 7C 13 40 0C 06 00 06 01 10 10 00 01 00 }
0x55943: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5594A: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55951: 		End  { 29 02 }
0x55953: 		SuppressIf  { 0A 82 }
0x55955: 			EqIdVal QuestionId: 0xC40, Value: 0x0 { 12 06 40 0C 00 00 }
0x5595B: 			GrayOutIf  { 19 82 }
0x5595D: 				EqIdVal QuestionId: 0xC4E, Value: 0x1 { 12 06 4E 0C 01 00 }
0x55963: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xC41, VarStoreId: 0x6, VarOffset: 0x36E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 17 E5 0E 41 0C 06 00 6E 03 10 10 00 01 00 }
0x55974: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5597B: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x55982: 				End  { 29 02 }
0x55984: 			End  { 29 02 }
0x55986: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27E8, VarStoreId: 0x6, VarOffset: 0x122, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 7D 12 F5 0D E8 27 06 00 22 01 10 10 00 04 00 }
0x55997: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5599E: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x559A5: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x559AC: 			End  { 29 02 }
0x559AE: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27E9, VarStoreId: 0x6, VarOffset: 0x2C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 99 12 AE 12 E9 27 06 00 C6 02 10 10 00 02 00 }
0x559BF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x559C6: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x559CD: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x559D4: 			End  { 29 02 }
0x559D6: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC42, VarStoreId: 0x6, VarOffset: 0x2E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 12 CD 12 42 0C 06 00 E2 02 10 10 00 01 00 }
0x559E7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x559EE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x559F5: 			End  { 29 02 }
0x559F7: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xC43, VarStoreId: 0x6, VarOffset: 0x2FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D5 12 A7 0E 43 0C 06 00 FE 02 10 10 00 01 00 }
0x55A08: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55A0F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55A16: 			End  { 29 02 }
0x55A18: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27EA, VarStoreId: 0x6, VarOffset: 0x31A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F1 12 06 13 EA 27 06 00 1A 03 10 10 00 01 00 }
0x55A29: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55A30: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55A37: 			End  { 29 02 }
0x55A39: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC44, VarStoreId: 0x6, VarOffset: 0x336, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 13 23 13 44 0C 06 00 36 03 10 10 00 01 00 }
0x55A4A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55A51: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55A58: 			End  { 29 02 }
0x55A5A: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC45, VarStoreId: 0x6, VarOffset: 0x352, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2B 13 40 13 45 0C 06 00 52 03 10 10 00 01 00 }
0x55A6B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55A72: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55A79: 			End  { 29 02 }
0x55A7B: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC46, VarStoreId: 0x6, VarOffset: 0x13E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 13 99 13 46 0C 06 00 3E 01 10 10 00 01 00 }
0x55A8C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55A93: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55A9A: 			End  { 29 02 }
0x55A9C: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC47, VarStoreId: 0x6, VarOffset: 0x15A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 13 B6 13 47 0C 06 00 5A 01 10 10 00 01 00 }
0x55AAD: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55AB4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55ABB: 			End  { 29 02 }
0x55ABD: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC48, VarStoreId: 0x6, VarOffset: 0x176, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 13 D3 13 48 0C 06 00 76 01 10 10 00 01 00 }
0x55ACE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55AD5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55ADC: 			End  { 29 02 }
0x55ADE: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC49, VarStoreId: 0x6, VarOffset: 0x192, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DB 13 F0 13 49 0C 06 00 92 01 10 10 00 01 00 }
0x55AEF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55AF6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55AFD: 			End  { 29 02 }
0x55AFF: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC4A, VarStoreId: 0x6, VarOffset: 0x1E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FC 13 11 14 4A 0C 06 00 E6 01 10 10 00 01 00 }
0x55B10: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55B17: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55B1E: 			End  { 29 02 }
0x55B20: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC4B, VarStoreId: 0x6, VarOffset: 0x202, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 19 14 2E 14 4B 0C 06 00 02 02 10 10 00 01 00 }
0x55B31: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55B38: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55B3F: 			End  { 29 02 }
0x55B41: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC4C, VarStoreId: 0x6, VarOffset: 0x21E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 36 14 4B 14 4C 0C 06 00 1E 02 10 10 00 01 00 }
0x55B52: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55B59: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55B60: 			End  { 29 02 }
0x55B62: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC4D, VarStoreId: 0x6, VarOffset: 0x23A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 53 14 68 14 4D 0C 06 00 3A 02 10 10 00 01 00 }
0x55B73: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55B7A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55B81: 			End  { 29 02 }
0x55B83: 			GrayOutIf  { 19 82 }
0x55B85: 				EqIdVal QuestionId: 0xC41, Value: 0x0 { 12 06 41 0C 00 00 }
0x55B8B: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC4E, VarStoreId: 0x6, VarOffset: 0x256, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 14 85 14 4E 0C 06 00 56 02 10 10 00 01 00 }
0x55B9C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55BA3: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55BAA: 				End  { 29 02 }
0x55BAC: 			End  { 29 02 }
0x55BAE: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC4F, VarStoreId: 0x6, VarOffset: 0x272, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8D 14 A2 14 4F 0C 06 00 72 02 10 10 00 01 00 }
0x55BBF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55BC6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55BCD: 			End  { 29 02 }
0x55BCF: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xC50, VarStoreId: 0x6, VarOffset: 0x28E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 4A 13 5F 13 50 0C 06 00 8E 02 10 10 00 04 00 }
0x55BE0: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x55BE7: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x55BEE: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x55BF5: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x55BFC: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x55C03: 			End  { 29 02 }
0x55C05: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC51, VarStoreId: 0x6, VarOffset: 0x2AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CD 14 E2 14 51 0C 06 00 AA 02 10 10 00 01 00 }
0x55C16: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55C1D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55C24: 			End  { 29 02 }
0x55C26: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xC52, VarStoreId: 0x6, VarOffset: 0x391, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 EA 14 FF 14 52 0C 06 00 91 03 00 11 00 00 FF FF 01 00 }
0x55C3A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x55C41: 			End  { 29 02 }
0x55C43: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC53, VarStoreId: 0x6, VarOffset: 0x526, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 07 15 1C 15 53 0C 06 00 26 05 00 10 00 07 01 }
0x55C54: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x55C5A: 			End  { 29 02 }
0x55C5C: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xC54, VarStoreId: 0x6, VarOffset: 0x549, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 24 15 39 15 54 0C 06 00 49 05 00 11 01 00 14 00 01 00 }
0x55C70: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x55C77: 			End  { 29 02 }
0x55C79: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC55, VarStoreId: 0x6, VarOffset: 0x57A, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 41 15 56 15 55 0C 06 00 7A 05 00 10 04 14 04 }
0x55C8A: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x55C90: 			End  { 29 02 }
0x55C92: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x55C99: 			End  { 29 02 }
0x55C9B: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x55CA2: 			End  { 29 02 }
0x55CA4: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC56, VarStoreId: 0x6, VarOffset: 0x3EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 15 7A 15 56 0C 06 00 EA 03 10 10 00 01 00 }
0x55CB5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55CBC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55CC3: 			End  { 29 02 }
0x55CC5: 			SuppressIf  { 0A 82 }
0x55CC7: 				EqIdVal QuestionId: 0xC56, Value: 0x0 { 12 06 56 0C 00 00 }
0x55CCD: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC57, VarStoreId: 0x6, VarOffset: 0x422, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A5 15 23 16 57 0C 06 00 22 04 10 10 00 02 00 }
0x55CDE: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55CE5: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x55CEC: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x55CF3: 				End  { 29 02 }
0x55CF5: 				SuppressIf  { 0A 82 }
0x55CF7: 					EqIdVal QuestionId: 0xC57, Value: 0x1 { 12 86 57 0C 01 00 }
0x55CFD: 						Not  { 17 02 }
0x55CFF: 					End  { 29 02 }
0x55D01: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC58, VarStoreId: 0x6, VarOffset: 0x499, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 A7 15 25 16 58 0C 06 00 99 04 10 11 00 00 FF 03 01 00 }
0x55D15: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x55D1C: 					End  { 29 02 }
0x55D1E: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC59, VarStoreId: 0x6, VarOffset: 0x43E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 A8 15 26 16 59 0C 06 00 3E 04 10 10 00 05 00 }
0x55D2F: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x55D36: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x55D3D: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x55D44: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x55D4B: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x55D52: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x55D59: 					End  { 29 02 }
0x55D5B: 				End  { 29 02 }
0x55D5D: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC5A, VarStoreId: 0x6, VarOffset: 0x45A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A6 15 24 16 5A 0C 06 00 5A 04 10 10 00 02 00 }
0x55D6E: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55D75: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x55D7C: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x55D83: 				End  { 29 02 }
0x55D85: 				SuppressIf  { 0A 82 }
0x55D87: 					EqIdVal QuestionId: 0xC5A, Value: 0x1 { 12 86 5A 0C 01 00 }
0x55D8D: 						Not  { 17 02 }
0x55D8F: 					End  { 29 02 }
0x55D91: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC5B, VarStoreId: 0x6, VarOffset: 0x4D1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 A9 15 27 16 5B 0C 06 00 D1 04 10 11 00 00 FF 03 01 00 }
0x55DA5: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x55DAC: 					End  { 29 02 }
0x55DAE: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC5C, VarStoreId: 0x6, VarOffset: 0x476, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 AA 15 28 16 5C 0C 06 00 76 04 10 10 00 05 00 }
0x55DBF: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x55DC6: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x55DCD: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x55DD4: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x55DDB: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x55DE2: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x55DE9: 					End  { 29 02 }
0x55DEB: 				End  { 29 02 }
0x55DED: 			End  { 29 02 }
0x55DEF: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x55DF6: 			End  { 29 02 }
0x55DF8: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xC5D, VarStoreId: 0x6, VarOffset: 0x406, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 16 45 16 5D 0C 06 00 06 04 10 10 00 01 00 }
0x55E09: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55E10: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55E17: 			End  { 29 02 }
0x55E19: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC5E, VarStoreId: 0x6, VarOffset: 0xC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 14 C3 14 5E 0C 06 00 C5 00 10 10 00 01 00 }
0x55E2A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55E31: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55E38: 			End  { 29 02 }
0x55E3A: 		End  { 29 02 }
0x55E3C: 	End  { 29 02 }
0x55E3E: 	Form FormId: 0x2838, Title: "PCI Express Root Port 9" { 01 86 38 28 7E 16 }
0x55E44: 		OneOf Prompt: "PCI Express Root Port 9", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xC5F, VarStoreId: 0x6, VarOffset: 0x107, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 13 7C 13 5F 0C 06 00 07 01 10 10 00 01 00 }
0x55E55: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55E5C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55E63: 		End  { 29 02 }
0x55E65: 		SuppressIf  { 0A 82 }
0x55E67: 			EqIdVal QuestionId: 0xC5F, Value: 0x0 { 12 06 5F 0C 00 00 }
0x55E6D: 			GrayOutIf  { 19 82 }
0x55E6F: 				EqIdVal QuestionId: 0xC6D, Value: 0x1 { 12 06 6D 0C 01 00 }
0x55E75: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xC60, VarStoreId: 0x6, VarOffset: 0x36F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 17 E5 0E 60 0C 06 00 6F 03 10 10 00 01 00 }
0x55E86: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x55E8D: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x55E94: 				End  { 29 02 }
0x55E96: 			End  { 29 02 }
0x55E98: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27EB, VarStoreId: 0x6, VarOffset: 0x123, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 7E 12 F5 0D EB 27 06 00 23 01 10 10 00 04 00 }
0x55EA9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55EB0: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x55EB7: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x55EBE: 			End  { 29 02 }
0x55EC0: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27EC, VarStoreId: 0x6, VarOffset: 0x2C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9A 12 AE 12 EC 27 06 00 C7 02 10 10 00 02 00 }
0x55ED1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55ED8: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x55EDF: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x55EE6: 			End  { 29 02 }
0x55EE8: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC61, VarStoreId: 0x6, VarOffset: 0x2E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 12 CD 12 61 0C 06 00 E3 02 10 10 00 01 00 }
0x55EF9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55F00: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55F07: 			End  { 29 02 }
0x55F09: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xC62, VarStoreId: 0x6, VarOffset: 0x2FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 12 A7 0E 62 0C 06 00 FF 02 10 10 00 01 00 }
0x55F1A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55F21: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55F28: 			End  { 29 02 }
0x55F2A: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27ED, VarStoreId: 0x6, VarOffset: 0x31B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F2 12 06 13 ED 27 06 00 1B 03 10 10 00 01 00 }
0x55F3B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55F42: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55F49: 			End  { 29 02 }
0x55F4B: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC63, VarStoreId: 0x6, VarOffset: 0x337, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0F 13 23 13 63 0C 06 00 37 03 10 10 00 01 00 }
0x55F5C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55F63: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55F6A: 			End  { 29 02 }
0x55F6C: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC64, VarStoreId: 0x6, VarOffset: 0x353, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 13 40 13 64 0C 06 00 53 03 10 10 00 01 00 }
0x55F7D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x55F84: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x55F8B: 			End  { 29 02 }
0x55F8D: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC65, VarStoreId: 0x6, VarOffset: 0x13F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 85 13 99 13 65 0C 06 00 3F 01 10 10 00 01 00 }
0x55F9E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55FA5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55FAC: 			End  { 29 02 }
0x55FAE: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC66, VarStoreId: 0x6, VarOffset: 0x15B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 13 B6 13 66 0C 06 00 5B 01 10 10 00 01 00 }
0x55FBF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55FC6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55FCD: 			End  { 29 02 }
0x55FCF: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC67, VarStoreId: 0x6, VarOffset: 0x177, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 13 D3 13 67 0C 06 00 77 01 10 10 00 01 00 }
0x55FE0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x55FE7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x55FEE: 			End  { 29 02 }
0x55FF0: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC68, VarStoreId: 0x6, VarOffset: 0x193, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 13 F0 13 68 0C 06 00 93 01 10 10 00 01 00 }
0x56001: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56008: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5600F: 			End  { 29 02 }
0x56011: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC69, VarStoreId: 0x6, VarOffset: 0x1E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 13 11 14 69 0C 06 00 E7 01 10 10 00 01 00 }
0x56022: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56029: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56030: 			End  { 29 02 }
0x56032: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC6A, VarStoreId: 0x6, VarOffset: 0x203, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1A 14 2E 14 6A 0C 06 00 03 02 10 10 00 01 00 }
0x56043: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5604A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56051: 			End  { 29 02 }
0x56053: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC6B, VarStoreId: 0x6, VarOffset: 0x21F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 37 14 4B 14 6B 0C 06 00 1F 02 10 10 00 01 00 }
0x56064: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5606B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56072: 			End  { 29 02 }
0x56074: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC6C, VarStoreId: 0x6, VarOffset: 0x23B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 54 14 68 14 6C 0C 06 00 3B 02 10 10 00 01 00 }
0x56085: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5608C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56093: 			End  { 29 02 }
0x56095: 			GrayOutIf  { 19 82 }
0x56097: 				EqIdVal QuestionId: 0xC60, Value: 0x0 { 12 06 60 0C 00 00 }
0x5609D: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC6D, VarStoreId: 0x6, VarOffset: 0x257, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 71 14 85 14 6D 0C 06 00 57 02 10 10 00 01 00 }
0x560AE: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x560B5: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x560BC: 				End  { 29 02 }
0x560BE: 			End  { 29 02 }
0x560C0: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC6E, VarStoreId: 0x6, VarOffset: 0x273, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 14 A2 14 6E 0C 06 00 73 02 10 10 00 01 00 }
0x560D1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x560D8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x560DF: 			End  { 29 02 }
0x560E1: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xC6F, VarStoreId: 0x6, VarOffset: 0x28F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 4B 13 5F 13 6F 0C 06 00 8F 02 10 10 00 04 00 }
0x560F2: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x560F9: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x56100: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x56107: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5610E: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x56115: 			End  { 29 02 }
0x56117: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC70, VarStoreId: 0x6, VarOffset: 0x2AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CE 14 E2 14 70 0C 06 00 AB 02 10 10 00 01 00 }
0x56128: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5612F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56136: 			End  { 29 02 }
0x56138: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xC71, VarStoreId: 0x6, VarOffset: 0x393, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 EB 14 FF 14 71 0C 06 00 93 03 00 11 00 00 FF FF 01 00 }
0x5614C: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x56153: 			End  { 29 02 }
0x56155: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC72, VarStoreId: 0x6, VarOffset: 0x527, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 08 15 1C 15 72 0C 06 00 27 05 00 10 00 07 01 }
0x56166: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5616C: 			End  { 29 02 }
0x5616E: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xC73, VarStoreId: 0x6, VarOffset: 0x54B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 25 15 39 15 73 0C 06 00 4B 05 00 11 01 00 14 00 01 00 }
0x56182: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x56189: 			End  { 29 02 }
0x5618B: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC74, VarStoreId: 0x6, VarOffset: 0x57B, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 42 15 56 15 74 0C 06 00 7B 05 00 10 04 14 04 }
0x5619C: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x561A2: 			End  { 29 02 }
0x561A4: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x561AB: 			End  { 29 02 }
0x561AD: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x561B4: 			End  { 29 02 }
0x561B6: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC75, VarStoreId: 0x6, VarOffset: 0x3EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 66 15 7A 15 75 0C 06 00 EB 03 10 10 00 01 00 }
0x561C7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x561CE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x561D5: 			End  { 29 02 }
0x561D7: 			SuppressIf  { 0A 82 }
0x561D9: 				EqIdVal QuestionId: 0xC75, Value: 0x0 { 12 06 75 0C 00 00 }
0x561DF: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC76, VarStoreId: 0x6, VarOffset: 0x423, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AB 15 23 16 76 0C 06 00 23 04 10 10 00 02 00 }
0x561F0: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x561F7: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x561FE: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x56205: 				End  { 29 02 }
0x56207: 				SuppressIf  { 0A 82 }
0x56209: 					EqIdVal QuestionId: 0xC76, Value: 0x1 { 12 86 76 0C 01 00 }
0x5620F: 						Not  { 17 02 }
0x56211: 					End  { 29 02 }
0x56213: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC77, VarStoreId: 0x6, VarOffset: 0x49B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 AD 15 25 16 77 0C 06 00 9B 04 10 11 00 00 FF 03 01 00 }
0x56227: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5622E: 					End  { 29 02 }
0x56230: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC78, VarStoreId: 0x6, VarOffset: 0x43F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 AE 15 26 16 78 0C 06 00 3F 04 10 10 00 05 00 }
0x56241: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x56248: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5624F: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x56256: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5625D: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x56264: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5626B: 					End  { 29 02 }
0x5626D: 				End  { 29 02 }
0x5626F: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC79, VarStoreId: 0x6, VarOffset: 0x45B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AC 15 24 16 79 0C 06 00 5B 04 10 10 00 02 00 }
0x56280: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56287: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5628E: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x56295: 				End  { 29 02 }
0x56297: 				SuppressIf  { 0A 82 }
0x56299: 					EqIdVal QuestionId: 0xC79, Value: 0x1 { 12 86 79 0C 01 00 }
0x5629F: 						Not  { 17 02 }
0x562A1: 					End  { 29 02 }
0x562A3: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC7A, VarStoreId: 0x6, VarOffset: 0x4D3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 AF 15 27 16 7A 0C 06 00 D3 04 10 11 00 00 FF 03 01 00 }
0x562B7: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x562BE: 					End  { 29 02 }
0x562C0: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC7B, VarStoreId: 0x6, VarOffset: 0x477, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 B0 15 28 16 7B 0C 06 00 77 04 10 10 00 05 00 }
0x562D1: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x562D8: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x562DF: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x562E6: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x562ED: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x562F4: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x562FB: 					End  { 29 02 }
0x562FD: 				End  { 29 02 }
0x562FF: 			End  { 29 02 }
0x56301: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x56308: 			End  { 29 02 }
0x5630A: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xC7C, VarStoreId: 0x6, VarOffset: 0x407, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 16 45 16 7C 0C 06 00 07 04 10 10 00 01 00 }
0x5631B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56322: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56329: 			End  { 29 02 }
0x5632B: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC7D, VarStoreId: 0x6, VarOffset: 0xC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AF 14 C3 14 7D 0C 06 00 C6 00 10 10 00 01 00 }
0x5633C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56343: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5634A: 			End  { 29 02 }
0x5634C: 		End  { 29 02 }
0x5634E: 	End  { 29 02 }
0x56350: 	Form FormId: 0x2839, Title: "PCI Express Root Port 10" { 01 86 39 28 7F 16 }
0x56356: 		OneOf Prompt: "PCI Express Root Port 10", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xC7E, VarStoreId: 0x6, VarOffset: 0x108, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 13 7C 13 7E 0C 06 00 08 01 10 10 00 01 00 }
0x56367: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5636E: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56375: 		End  { 29 02 }
0x56377: 		SuppressIf  { 0A 82 }
0x56379: 			EqIdVal QuestionId: 0xC7E, Value: 0x0 { 12 06 7E 0C 00 00 }
0x5637F: 			GrayOutIf  { 19 82 }
0x56381: 				EqIdVal QuestionId: 0xC8C, Value: 0x1 { 12 06 8C 0C 01 00 }
0x56387: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xC7F, VarStoreId: 0x6, VarOffset: 0x370, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 29 17 E5 0E 7F 0C 06 00 70 03 10 10 00 01 00 }
0x56398: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5639F: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x563A6: 				End  { 29 02 }
0x563A8: 			End  { 29 02 }
0x563AA: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27EE, VarStoreId: 0x6, VarOffset: 0x124, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 7F 12 F5 0D EE 27 06 00 24 01 10 10 00 04 00 }
0x563BB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x563C2: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x563C9: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x563D0: 			End  { 29 02 }
0x563D2: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27EF, VarStoreId: 0x6, VarOffset: 0x2C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9B 12 AE 12 EF 27 06 00 C8 02 10 10 00 02 00 }
0x563E3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x563EA: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x563F1: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x563F8: 			End  { 29 02 }
0x563FA: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC80, VarStoreId: 0x6, VarOffset: 0x2E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 12 CD 12 80 0C 06 00 E4 02 10 10 00 01 00 }
0x5640B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56412: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56419: 			End  { 29 02 }
0x5641B: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xC81, VarStoreId: 0x6, VarOffset: 0x300, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D7 12 A7 0E 81 0C 06 00 00 03 10 10 00 01 00 }
0x5642C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56433: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5643A: 			End  { 29 02 }
0x5643C: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27F0, VarStoreId: 0x6, VarOffset: 0x31C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F3 12 06 13 F0 27 06 00 1C 03 10 10 00 01 00 }
0x5644D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56454: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5645B: 			End  { 29 02 }
0x5645D: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC82, VarStoreId: 0x6, VarOffset: 0x338, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 10 13 23 13 82 0C 06 00 38 03 10 10 00 01 00 }
0x5646E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56475: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5647C: 			End  { 29 02 }
0x5647E: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xC83, VarStoreId: 0x6, VarOffset: 0x354, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 13 40 13 83 0C 06 00 54 03 10 10 00 01 00 }
0x5648F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56496: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5649D: 			End  { 29 02 }
0x5649F: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC84, VarStoreId: 0x6, VarOffset: 0x140, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 13 99 13 84 0C 06 00 40 01 10 10 00 01 00 }
0x564B0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x564B7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x564BE: 			End  { 29 02 }
0x564C0: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC85, VarStoreId: 0x6, VarOffset: 0x15C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A3 13 B6 13 85 0C 06 00 5C 01 10 10 00 01 00 }
0x564D1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x564D8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x564DF: 			End  { 29 02 }
0x564E1: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC86, VarStoreId: 0x6, VarOffset: 0x178, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 13 D3 13 86 0C 06 00 78 01 10 10 00 01 00 }
0x564F2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x564F9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56500: 			End  { 29 02 }
0x56502: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC87, VarStoreId: 0x6, VarOffset: 0x194, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DD 13 F0 13 87 0C 06 00 94 01 10 10 00 01 00 }
0x56513: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5651A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56521: 			End  { 29 02 }
0x56523: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC88, VarStoreId: 0x6, VarOffset: 0x1E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FE 13 11 14 88 0C 06 00 E8 01 10 10 00 01 00 }
0x56534: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5653B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56542: 			End  { 29 02 }
0x56544: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC89, VarStoreId: 0x6, VarOffset: 0x204, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1B 14 2E 14 89 0C 06 00 04 02 10 10 00 01 00 }
0x56555: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5655C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56563: 			End  { 29 02 }
0x56565: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC8A, VarStoreId: 0x6, VarOffset: 0x220, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 14 4B 14 8A 0C 06 00 20 02 10 10 00 01 00 }
0x56576: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5657D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56584: 			End  { 29 02 }
0x56586: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC8B, VarStoreId: 0x6, VarOffset: 0x23C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 55 14 68 14 8B 0C 06 00 3C 02 10 10 00 01 00 }
0x56597: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5659E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x565A5: 			End  { 29 02 }
0x565A7: 			GrayOutIf  { 19 82 }
0x565A9: 				EqIdVal QuestionId: 0xC7F, Value: 0x0 { 12 06 7F 0C 00 00 }
0x565AF: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC8C, VarStoreId: 0x6, VarOffset: 0x258, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 14 85 14 8C 0C 06 00 58 02 10 10 00 01 00 }
0x565C0: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x565C7: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x565CE: 				End  { 29 02 }
0x565D0: 			End  { 29 02 }
0x565D2: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC8D, VarStoreId: 0x6, VarOffset: 0x274, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 14 A2 14 8D 0C 06 00 74 02 10 10 00 01 00 }
0x565E3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x565EA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x565F1: 			End  { 29 02 }
0x565F3: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xC8E, VarStoreId: 0x6, VarOffset: 0x290, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 4C 13 5F 13 8E 0C 06 00 90 02 10 10 00 04 00 }
0x56604: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5660B: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x56612: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x56619: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x56620: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x56627: 			End  { 29 02 }
0x56629: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC8F, VarStoreId: 0x6, VarOffset: 0x2AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 14 E2 14 8F 0C 06 00 AC 02 10 10 00 01 00 }
0x5663A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56641: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56648: 			End  { 29 02 }
0x5664A: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xC90, VarStoreId: 0x6, VarOffset: 0x395, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 EC 14 FF 14 90 0C 06 00 95 03 00 11 00 00 FF FF 01 00 }
0x5665E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x56665: 			End  { 29 02 }
0x56667: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC91, VarStoreId: 0x6, VarOffset: 0x528, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 09 15 1C 15 91 0C 06 00 28 05 00 10 00 07 01 }
0x56678: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5667E: 			End  { 29 02 }
0x56680: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xC92, VarStoreId: 0x6, VarOffset: 0x54D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 26 15 39 15 92 0C 06 00 4D 05 00 11 01 00 14 00 01 00 }
0x56694: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5669B: 			End  { 29 02 }
0x5669D: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xC93, VarStoreId: 0x6, VarOffset: 0x57C, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 43 15 56 15 93 0C 06 00 7C 05 00 10 04 14 04 }
0x566AE: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x566B4: 			End  { 29 02 }
0x566B6: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x566BD: 			End  { 29 02 }
0x566BF: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x566C6: 			End  { 29 02 }
0x566C8: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC94, VarStoreId: 0x6, VarOffset: 0x3EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 15 7A 15 94 0C 06 00 EC 03 10 10 00 01 00 }
0x566D9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x566E0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x566E7: 			End  { 29 02 }
0x566E9: 			SuppressIf  { 0A 82 }
0x566EB: 				EqIdVal QuestionId: 0xC94, Value: 0x0 { 12 06 94 0C 00 00 }
0x566F1: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC95, VarStoreId: 0x6, VarOffset: 0x424, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 B1 15 23 16 95 0C 06 00 24 04 10 10 00 02 00 }
0x56702: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56709: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x56710: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x56717: 				End  { 29 02 }
0x56719: 				SuppressIf  { 0A 82 }
0x5671B: 					EqIdVal QuestionId: 0xC95, Value: 0x1 { 12 86 95 0C 01 00 }
0x56721: 						Not  { 17 02 }
0x56723: 					End  { 29 02 }
0x56725: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC96, VarStoreId: 0x6, VarOffset: 0x49D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 B3 15 25 16 96 0C 06 00 9D 04 10 11 00 00 FF 03 01 00 }
0x56739: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x56740: 					End  { 29 02 }
0x56742: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC97, VarStoreId: 0x6, VarOffset: 0x440, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 B4 15 26 16 97 0C 06 00 40 04 10 10 00 05 00 }
0x56753: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5675A: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x56761: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x56768: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5676F: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x56776: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5677D: 					End  { 29 02 }
0x5677F: 				End  { 29 02 }
0x56781: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xC98, VarStoreId: 0x6, VarOffset: 0x45C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 B2 15 24 16 98 0C 06 00 5C 04 10 10 00 02 00 }
0x56792: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56799: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x567A0: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x567A7: 				End  { 29 02 }
0x567A9: 				SuppressIf  { 0A 82 }
0x567AB: 					EqIdVal QuestionId: 0xC98, Value: 0x1 { 12 86 98 0C 01 00 }
0x567B1: 						Not  { 17 02 }
0x567B3: 					End  { 29 02 }
0x567B5: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC99, VarStoreId: 0x6, VarOffset: 0x4D5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 B5 15 27 16 99 0C 06 00 D5 04 10 11 00 00 FF 03 01 00 }
0x567C9: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x567D0: 					End  { 29 02 }
0x567D2: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xC9A, VarStoreId: 0x6, VarOffset: 0x478, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 B6 15 28 16 9A 0C 06 00 78 04 10 10 00 05 00 }
0x567E3: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x567EA: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x567F1: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x567F8: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x567FF: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x56806: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5680D: 					End  { 29 02 }
0x5680F: 				End  { 29 02 }
0x56811: 			End  { 29 02 }
0x56813: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5681A: 			End  { 29 02 }
0x5681C: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xC9B, VarStoreId: 0x6, VarOffset: 0x408, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 16 45 16 9B 0C 06 00 08 04 10 10 00 01 00 }
0x5682D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56834: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5683B: 			End  { 29 02 }
0x5683D: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xC9C, VarStoreId: 0x6, VarOffset: 0xC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 14 C3 14 9C 0C 06 00 C7 00 10 10 00 01 00 }
0x5684E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56855: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5685C: 			End  { 29 02 }
0x5685E: 		End  { 29 02 }
0x56860: 	End  { 29 02 }
0x56862: 	Form FormId: 0x283A, Title: "PCI Express Root Port 11" { 01 86 3A 28 80 16 }
0x56868: 		OneOf Prompt: "PCI Express Root Port 11", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xC9D, VarStoreId: 0x6, VarOffset: 0x109, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6A 13 7C 13 9D 0C 06 00 09 01 10 10 00 01 00 }
0x56879: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56880: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56887: 		End  { 29 02 }
0x56889: 		SuppressIf  { 0A 82 }
0x5688B: 			EqIdVal QuestionId: 0xC9D, Value: 0x0 { 12 06 9D 0C 00 00 }
0x56891: 			GrayOutIf  { 19 82 }
0x56893: 				EqIdVal QuestionId: 0xCAB, Value: 0x1 { 12 06 AB 0C 01 00 }
0x56899: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xC9E, VarStoreId: 0x6, VarOffset: 0x371, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 17 E5 0E 9E 0C 06 00 71 03 10 10 00 01 00 }
0x568AA: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x568B1: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x568B8: 				End  { 29 02 }
0x568BA: 			End  { 29 02 }
0x568BC: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27F1, VarStoreId: 0x6, VarOffset: 0x125, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 80 12 F5 0D F1 27 06 00 25 01 10 10 00 04 00 }
0x568CD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x568D4: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x568DB: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x568E2: 			End  { 29 02 }
0x568E4: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27F2, VarStoreId: 0x6, VarOffset: 0x2C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9C 12 AE 12 F2 27 06 00 C9 02 10 10 00 02 00 }
0x568F5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x568FC: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x56903: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5690A: 			End  { 29 02 }
0x5690C: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xC9F, VarStoreId: 0x6, VarOffset: 0x2E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 12 CD 12 9F 0C 06 00 E5 02 10 10 00 01 00 }
0x5691D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56924: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5692B: 			End  { 29 02 }
0x5692D: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xCA0, VarStoreId: 0x6, VarOffset: 0x301, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D8 12 A7 0E A0 0C 06 00 01 03 10 10 00 01 00 }
0x5693E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56945: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5694C: 			End  { 29 02 }
0x5694E: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27F3, VarStoreId: 0x6, VarOffset: 0x31D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F4 12 06 13 F3 27 06 00 1D 03 10 10 00 01 00 }
0x5695F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56966: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5696D: 			End  { 29 02 }
0x5696F: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCA1, VarStoreId: 0x6, VarOffset: 0x339, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 13 23 13 A1 0C 06 00 39 03 10 10 00 01 00 }
0x56980: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56987: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5698E: 			End  { 29 02 }
0x56990: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCA2, VarStoreId: 0x6, VarOffset: 0x355, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 13 40 13 A2 0C 06 00 55 03 10 10 00 01 00 }
0x569A1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x569A8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x569AF: 			End  { 29 02 }
0x569B1: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA3, VarStoreId: 0x6, VarOffset: 0x141, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 13 99 13 A3 0C 06 00 41 01 10 10 00 01 00 }
0x569C2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x569C9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x569D0: 			End  { 29 02 }
0x569D2: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA4, VarStoreId: 0x6, VarOffset: 0x15D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 13 B6 13 A4 0C 06 00 5D 01 10 10 00 01 00 }
0x569E3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x569EA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x569F1: 			End  { 29 02 }
0x569F3: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA5, VarStoreId: 0x6, VarOffset: 0x179, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 13 D3 13 A5 0C 06 00 79 01 10 10 00 01 00 }
0x56A04: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56A0B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56A12: 			End  { 29 02 }
0x56A14: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA6, VarStoreId: 0x6, VarOffset: 0x195, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 13 F0 13 A6 0C 06 00 95 01 10 10 00 01 00 }
0x56A25: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56A2C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56A33: 			End  { 29 02 }
0x56A35: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA7, VarStoreId: 0x6, VarOffset: 0x1E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FF 13 11 14 A7 0C 06 00 E9 01 10 10 00 01 00 }
0x56A46: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56A4D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56A54: 			End  { 29 02 }
0x56A56: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA8, VarStoreId: 0x6, VarOffset: 0x205, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1C 14 2E 14 A8 0C 06 00 05 02 10 10 00 01 00 }
0x56A67: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56A6E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56A75: 			End  { 29 02 }
0x56A77: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCA9, VarStoreId: 0x6, VarOffset: 0x221, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 14 4B 14 A9 0C 06 00 21 02 10 10 00 01 00 }
0x56A88: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56A8F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56A96: 			End  { 29 02 }
0x56A98: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCAA, VarStoreId: 0x6, VarOffset: 0x23D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 56 14 68 14 AA 0C 06 00 3D 02 10 10 00 01 00 }
0x56AA9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56AB0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56AB7: 			End  { 29 02 }
0x56AB9: 			GrayOutIf  { 19 82 }
0x56ABB: 				EqIdVal QuestionId: 0xC9E, Value: 0x0 { 12 06 9E 0C 00 00 }
0x56AC1: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCAB, VarStoreId: 0x6, VarOffset: 0x259, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 73 14 85 14 AB 0C 06 00 59 02 10 10 00 01 00 }
0x56AD2: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56AD9: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56AE0: 				End  { 29 02 }
0x56AE2: 			End  { 29 02 }
0x56AE4: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCAC, VarStoreId: 0x6, VarOffset: 0x275, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 14 A2 14 AC 0C 06 00 75 02 10 10 00 01 00 }
0x56AF5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56AFC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56B03: 			End  { 29 02 }
0x56B05: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xCAD, VarStoreId: 0x6, VarOffset: 0x291, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 4D 13 5F 13 AD 0C 06 00 91 02 10 10 00 04 00 }
0x56B16: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x56B1D: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x56B24: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x56B2B: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x56B32: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x56B39: 			End  { 29 02 }
0x56B3B: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCAE, VarStoreId: 0x6, VarOffset: 0x2AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 14 E2 14 AE 0C 06 00 AD 02 10 10 00 01 00 }
0x56B4C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56B53: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56B5A: 			End  { 29 02 }
0x56B5C: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xCAF, VarStoreId: 0x6, VarOffset: 0x397, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 ED 14 FF 14 AF 0C 06 00 97 03 00 11 00 00 FF FF 01 00 }
0x56B70: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x56B77: 			End  { 29 02 }
0x56B79: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xCB0, VarStoreId: 0x6, VarOffset: 0x529, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 0A 15 1C 15 B0 0C 06 00 29 05 00 10 00 07 01 }
0x56B8A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x56B90: 			End  { 29 02 }
0x56B92: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xCB1, VarStoreId: 0x6, VarOffset: 0x54F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 27 15 39 15 B1 0C 06 00 4F 05 00 11 01 00 14 00 01 00 }
0x56BA6: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x56BAD: 			End  { 29 02 }
0x56BAF: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xCB2, VarStoreId: 0x6, VarOffset: 0x57D, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 44 15 56 15 B2 0C 06 00 7D 05 00 10 04 14 04 }
0x56BC0: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x56BC6: 			End  { 29 02 }
0x56BC8: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x56BCF: 			End  { 29 02 }
0x56BD1: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x56BD8: 			End  { 29 02 }
0x56BDA: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xCB3, VarStoreId: 0x6, VarOffset: 0x3ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 15 7A 15 B3 0C 06 00 ED 03 10 10 00 01 00 }
0x56BEB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56BF2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56BF9: 			End  { 29 02 }
0x56BFB: 			SuppressIf  { 0A 82 }
0x56BFD: 				EqIdVal QuestionId: 0xCB3, Value: 0x0 { 12 06 B3 0C 00 00 }
0x56C03: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xCB4, VarStoreId: 0x6, VarOffset: 0x425, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 B7 15 23 16 B4 0C 06 00 25 04 10 10 00 02 00 }
0x56C14: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56C1B: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x56C22: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x56C29: 				End  { 29 02 }
0x56C2B: 				SuppressIf  { 0A 82 }
0x56C2D: 					EqIdVal QuestionId: 0xCB4, Value: 0x1 { 12 86 B4 0C 01 00 }
0x56C33: 						Not  { 17 02 }
0x56C35: 					End  { 29 02 }
0x56C37: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCB5, VarStoreId: 0x6, VarOffset: 0x49F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 B9 15 25 16 B5 0C 06 00 9F 04 10 11 00 00 FF 03 01 00 }
0x56C4B: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x56C52: 					End  { 29 02 }
0x56C54: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCB6, VarStoreId: 0x6, VarOffset: 0x441, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 BA 15 26 16 B6 0C 06 00 41 04 10 10 00 05 00 }
0x56C65: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x56C6C: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x56C73: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x56C7A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x56C81: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x56C88: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x56C8F: 					End  { 29 02 }
0x56C91: 				End  { 29 02 }
0x56C93: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xCB7, VarStoreId: 0x6, VarOffset: 0x45D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 B8 15 24 16 B7 0C 06 00 5D 04 10 10 00 02 00 }
0x56CA4: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56CAB: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x56CB2: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x56CB9: 				End  { 29 02 }
0x56CBB: 				SuppressIf  { 0A 82 }
0x56CBD: 					EqIdVal QuestionId: 0xCB7, Value: 0x1 { 12 86 B7 0C 01 00 }
0x56CC3: 						Not  { 17 02 }
0x56CC5: 					End  { 29 02 }
0x56CC7: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCB8, VarStoreId: 0x6, VarOffset: 0x4D7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 BB 15 27 16 B8 0C 06 00 D7 04 10 11 00 00 FF 03 01 00 }
0x56CDB: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x56CE2: 					End  { 29 02 }
0x56CE4: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCB9, VarStoreId: 0x6, VarOffset: 0x479, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 BC 15 28 16 B9 0C 06 00 79 04 10 10 00 05 00 }
0x56CF5: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x56CFC: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x56D03: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x56D0A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x56D11: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x56D18: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x56D1F: 					End  { 29 02 }
0x56D21: 				End  { 29 02 }
0x56D23: 			End  { 29 02 }
0x56D25: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x56D2C: 			End  { 29 02 }
0x56D2E: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xCBA, VarStoreId: 0x6, VarOffset: 0x409, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 16 45 16 BA 0C 06 00 09 04 10 10 00 01 00 }
0x56D3F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56D46: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56D4D: 			End  { 29 02 }
0x56D4F: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xCBB, VarStoreId: 0x6, VarOffset: 0xC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 14 C3 14 BB 0C 06 00 C8 00 10 10 00 01 00 }
0x56D60: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56D67: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56D6E: 			End  { 29 02 }
0x56D70: 		End  { 29 02 }
0x56D72: 	End  { 29 02 }
0x56D74: 	Form FormId: 0x283B, Title: "PCI Express Root Port 12" { 01 86 3B 28 81 16 }
0x56D7A: 		OneOf Prompt: "PCI Express Root Port 12", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xCBC, VarStoreId: 0x6, VarOffset: 0x10A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 13 7C 13 BC 0C 06 00 0A 01 10 10 00 01 00 }
0x56D8B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56D92: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56D99: 		End  { 29 02 }
0x56D9B: 		SuppressIf  { 0A 82 }
0x56D9D: 			EqIdVal QuestionId: 0xCBC, Value: 0x0 { 12 06 BC 0C 00 00 }
0x56DA3: 			GrayOutIf  { 19 82 }
0x56DA5: 				EqIdVal QuestionId: 0xCCA, Value: 0x1 { 12 06 CA 0C 01 00 }
0x56DAB: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xCBD, VarStoreId: 0x6, VarOffset: 0x372, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2B 17 E5 0E BD 0C 06 00 72 03 10 10 00 01 00 }
0x56DBC: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x56DC3: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x56DCA: 				End  { 29 02 }
0x56DCC: 			End  { 29 02 }
0x56DCE: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27F4, VarStoreId: 0x6, VarOffset: 0x126, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 81 12 F5 0D F4 27 06 00 26 01 10 10 00 04 00 }
0x56DDF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56DE6: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x56DED: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x56DF4: 			End  { 29 02 }
0x56DF6: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27F5, VarStoreId: 0x6, VarOffset: 0x2CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9D 12 AE 12 F5 27 06 00 CA 02 10 10 00 02 00 }
0x56E07: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56E0E: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x56E15: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x56E1C: 			End  { 29 02 }
0x56E1E: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCBE, VarStoreId: 0x6, VarOffset: 0x2E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 12 CD 12 BE 0C 06 00 E6 02 10 10 00 01 00 }
0x56E2F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56E36: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56E3D: 			End  { 29 02 }
0x56E3F: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xCBF, VarStoreId: 0x6, VarOffset: 0x302, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D9 12 A7 0E BF 0C 06 00 02 03 10 10 00 01 00 }
0x56E50: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56E57: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56E5E: 			End  { 29 02 }
0x56E60: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27F6, VarStoreId: 0x6, VarOffset: 0x31E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 12 06 13 F6 27 06 00 1E 03 10 10 00 01 00 }
0x56E71: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56E78: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56E7F: 			End  { 29 02 }
0x56E81: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCC0, VarStoreId: 0x6, VarOffset: 0x33A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 12 13 23 13 C0 0C 06 00 3A 03 10 10 00 01 00 }
0x56E92: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56E99: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56EA0: 			End  { 29 02 }
0x56EA2: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCC1, VarStoreId: 0x6, VarOffset: 0x356, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 13 40 13 C1 0C 06 00 56 03 10 10 00 01 00 }
0x56EB3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56EBA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56EC1: 			End  { 29 02 }
0x56EC3: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC2, VarStoreId: 0x6, VarOffset: 0x142, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 88 13 99 13 C2 0C 06 00 42 01 10 10 00 01 00 }
0x56ED4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56EDB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56EE2: 			End  { 29 02 }
0x56EE4: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC3, VarStoreId: 0x6, VarOffset: 0x15E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A5 13 B6 13 C3 0C 06 00 5E 01 10 10 00 01 00 }
0x56EF5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56EFC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56F03: 			End  { 29 02 }
0x56F05: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC4, VarStoreId: 0x6, VarOffset: 0x17A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 13 D3 13 C4 0C 06 00 7A 01 10 10 00 01 00 }
0x56F16: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56F1D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56F24: 			End  { 29 02 }
0x56F26: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC5, VarStoreId: 0x6, VarOffset: 0x196, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 13 F0 13 C5 0C 06 00 96 01 10 10 00 01 00 }
0x56F37: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56F3E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56F45: 			End  { 29 02 }
0x56F47: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC6, VarStoreId: 0x6, VarOffset: 0x1EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 00 14 11 14 C6 0C 06 00 EA 01 10 10 00 01 00 }
0x56F58: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56F5F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56F66: 			End  { 29 02 }
0x56F68: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC7, VarStoreId: 0x6, VarOffset: 0x206, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1D 14 2E 14 C7 0C 06 00 06 02 10 10 00 01 00 }
0x56F79: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56F80: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56F87: 			End  { 29 02 }
0x56F89: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC8, VarStoreId: 0x6, VarOffset: 0x222, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 14 4B 14 C8 0C 06 00 22 02 10 10 00 01 00 }
0x56F9A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56FA1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56FA8: 			End  { 29 02 }
0x56FAA: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCC9, VarStoreId: 0x6, VarOffset: 0x23E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 57 14 68 14 C9 0C 06 00 3E 02 10 10 00 01 00 }
0x56FBB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x56FC2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x56FC9: 			End  { 29 02 }
0x56FCB: 			GrayOutIf  { 19 82 }
0x56FCD: 				EqIdVal QuestionId: 0xCBD, Value: 0x0 { 12 06 BD 0C 00 00 }
0x56FD3: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCCA, VarStoreId: 0x6, VarOffset: 0x25A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 14 85 14 CA 0C 06 00 5A 02 10 10 00 01 00 }
0x56FE4: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x56FEB: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x56FF2: 				End  { 29 02 }
0x56FF4: 			End  { 29 02 }
0x56FF6: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCCB, VarStoreId: 0x6, VarOffset: 0x276, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 14 A2 14 CB 0C 06 00 76 02 10 10 00 01 00 }
0x57007: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5700E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57015: 			End  { 29 02 }
0x57017: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xCCC, VarStoreId: 0x6, VarOffset: 0x292, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 4E 13 5F 13 CC 0C 06 00 92 02 10 10 00 04 00 }
0x57028: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5702F: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x57036: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5703D: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x57044: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5704B: 			End  { 29 02 }
0x5704D: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCCD, VarStoreId: 0x6, VarOffset: 0x2AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 14 E2 14 CD 0C 06 00 AE 02 10 10 00 01 00 }
0x5705E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57065: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5706C: 			End  { 29 02 }
0x5706E: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xCCE, VarStoreId: 0x6, VarOffset: 0x399, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 EE 14 FF 14 CE 0C 06 00 99 03 00 11 00 00 FF FF 01 00 }
0x57082: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x57089: 			End  { 29 02 }
0x5708B: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xCCF, VarStoreId: 0x6, VarOffset: 0x52A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 0B 15 1C 15 CF 0C 06 00 2A 05 00 10 00 07 01 }
0x5709C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x570A2: 			End  { 29 02 }
0x570A4: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xCD0, VarStoreId: 0x6, VarOffset: 0x551, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 28 15 39 15 D0 0C 06 00 51 05 00 11 01 00 14 00 01 00 }
0x570B8: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x570BF: 			End  { 29 02 }
0x570C1: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xCD1, VarStoreId: 0x6, VarOffset: 0x57E, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 45 15 56 15 D1 0C 06 00 7E 05 00 10 04 14 04 }
0x570D2: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x570D8: 			End  { 29 02 }
0x570DA: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x570E1: 			End  { 29 02 }
0x570E3: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x570EA: 			End  { 29 02 }
0x570EC: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xCD2, VarStoreId: 0x6, VarOffset: 0x3EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 69 15 7A 15 D2 0C 06 00 EE 03 10 10 00 01 00 }
0x570FD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57104: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5710B: 			End  { 29 02 }
0x5710D: 			SuppressIf  { 0A 82 }
0x5710F: 				EqIdVal QuestionId: 0xCD2, Value: 0x0 { 12 06 D2 0C 00 00 }
0x57115: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xCD3, VarStoreId: 0x6, VarOffset: 0x426, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 BD 15 23 16 D3 0C 06 00 26 04 10 10 00 02 00 }
0x57126: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5712D: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x57134: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5713B: 				End  { 29 02 }
0x5713D: 				SuppressIf  { 0A 82 }
0x5713F: 					EqIdVal QuestionId: 0xCD3, Value: 0x1 { 12 86 D3 0C 01 00 }
0x57145: 						Not  { 17 02 }
0x57147: 					End  { 29 02 }
0x57149: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCD4, VarStoreId: 0x6, VarOffset: 0x4A1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 BF 15 25 16 D4 0C 06 00 A1 04 10 11 00 00 FF 03 01 00 }
0x5715D: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x57164: 					End  { 29 02 }
0x57166: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCD5, VarStoreId: 0x6, VarOffset: 0x442, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C0 15 26 16 D5 0C 06 00 42 04 10 10 00 05 00 }
0x57177: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5717E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x57185: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5718C: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x57193: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5719A: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x571A1: 					End  { 29 02 }
0x571A3: 				End  { 29 02 }
0x571A5: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xCD6, VarStoreId: 0x6, VarOffset: 0x45E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 BE 15 24 16 D6 0C 06 00 5E 04 10 10 00 02 00 }
0x571B6: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x571BD: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x571C4: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x571CB: 				End  { 29 02 }
0x571CD: 				SuppressIf  { 0A 82 }
0x571CF: 					EqIdVal QuestionId: 0xCD6, Value: 0x1 { 12 86 D6 0C 01 00 }
0x571D5: 						Not  { 17 02 }
0x571D7: 					End  { 29 02 }
0x571D9: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCD7, VarStoreId: 0x6, VarOffset: 0x4D9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 C1 15 27 16 D7 0C 06 00 D9 04 10 11 00 00 FF 03 01 00 }
0x571ED: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x571F4: 					End  { 29 02 }
0x571F6: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCD8, VarStoreId: 0x6, VarOffset: 0x47A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C2 15 28 16 D8 0C 06 00 7A 04 10 10 00 05 00 }
0x57207: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5720E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x57215: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5721C: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x57223: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5722A: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x57231: 					End  { 29 02 }
0x57233: 				End  { 29 02 }
0x57235: 			End  { 29 02 }
0x57237: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5723E: 			End  { 29 02 }
0x57240: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xCD9, VarStoreId: 0x6, VarOffset: 0x40A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 16 45 16 D9 0C 06 00 0A 04 10 10 00 01 00 }
0x57251: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57258: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5725F: 			End  { 29 02 }
0x57261: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xCDA, VarStoreId: 0x6, VarOffset: 0xC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 14 C3 14 DA 0C 06 00 C9 00 10 10 00 01 00 }
0x57272: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57279: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57280: 			End  { 29 02 }
0x57282: 		End  { 29 02 }
0x57284: 	End  { 29 02 }
0x57286: 	Form FormId: 0x283C, Title: "PCI Express Root Port 13" { 01 86 3C 28 82 16 }
0x5728C: 		OneOf Prompt: "PCI Express Root Port 13", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xCDB, VarStoreId: 0x6, VarOffset: 0x10B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 13 7C 13 DB 0C 06 00 0B 01 10 10 00 01 00 }
0x5729D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x572A4: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x572AB: 		End  { 29 02 }
0x572AD: 		SuppressIf  { 0A 82 }
0x572AF: 			EqIdVal QuestionId: 0xCDB, Value: 0x0 { 12 06 DB 0C 00 00 }
0x572B5: 			GrayOutIf  { 19 82 }
0x572B7: 				EqIdVal QuestionId: 0xCE9, Value: 0x1 { 12 06 E9 0C 01 00 }
0x572BD: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xCDC, VarStoreId: 0x6, VarOffset: 0x373, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 17 E5 0E DC 0C 06 00 73 03 10 10 00 01 00 }
0x572CE: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x572D5: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x572DC: 				End  { 29 02 }
0x572DE: 			End  { 29 02 }
0x572E0: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27F7, VarStoreId: 0x6, VarOffset: 0x127, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 82 12 F5 0D F7 27 06 00 27 01 10 10 00 04 00 }
0x572F1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x572F8: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x572FF: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x57306: 			End  { 29 02 }
0x57308: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27F8, VarStoreId: 0x6, VarOffset: 0x2CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9E 12 AE 12 F8 27 06 00 CB 02 10 10 00 02 00 }
0x57319: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57320: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x57327: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5732E: 			End  { 29 02 }
0x57330: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCDD, VarStoreId: 0x6, VarOffset: 0x2E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 12 CD 12 DD 0C 06 00 E7 02 10 10 00 01 00 }
0x57341: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57348: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5734F: 			End  { 29 02 }
0x57351: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xCDE, VarStoreId: 0x6, VarOffset: 0x303, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DA 12 A7 0E DE 0C 06 00 03 03 10 10 00 01 00 }
0x57362: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57369: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57370: 			End  { 29 02 }
0x57372: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27F9, VarStoreId: 0x6, VarOffset: 0x31F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F6 12 06 13 F9 27 06 00 1F 03 10 10 00 01 00 }
0x57383: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5738A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57391: 			End  { 29 02 }
0x57393: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCDF, VarStoreId: 0x6, VarOffset: 0x33B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 13 13 23 13 DF 0C 06 00 3B 03 10 10 00 01 00 }
0x573A4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x573AB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x573B2: 			End  { 29 02 }
0x573B4: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCE0, VarStoreId: 0x6, VarOffset: 0x357, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 13 40 13 E0 0C 06 00 57 03 10 10 00 01 00 }
0x573C5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x573CC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x573D3: 			End  { 29 02 }
0x573D5: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE1, VarStoreId: 0x6, VarOffset: 0x143, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 13 99 13 E1 0C 06 00 43 01 10 10 00 01 00 }
0x573E6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x573ED: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x573F4: 			End  { 29 02 }
0x573F6: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE2, VarStoreId: 0x6, VarOffset: 0x15F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A6 13 B6 13 E2 0C 06 00 5F 01 10 10 00 01 00 }
0x57407: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5740E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57415: 			End  { 29 02 }
0x57417: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE3, VarStoreId: 0x6, VarOffset: 0x17B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C3 13 D3 13 E3 0C 06 00 7B 01 10 10 00 01 00 }
0x57428: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5742F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57436: 			End  { 29 02 }
0x57438: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE4, VarStoreId: 0x6, VarOffset: 0x197, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 13 F0 13 E4 0C 06 00 97 01 10 10 00 01 00 }
0x57449: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57450: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57457: 			End  { 29 02 }
0x57459: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE5, VarStoreId: 0x6, VarOffset: 0x1EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 14 11 14 E5 0C 06 00 EB 01 10 10 00 01 00 }
0x5746A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57471: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57478: 			End  { 29 02 }
0x5747A: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE6, VarStoreId: 0x6, VarOffset: 0x207, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1E 14 2E 14 E6 0C 06 00 07 02 10 10 00 01 00 }
0x5748B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57492: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57499: 			End  { 29 02 }
0x5749B: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE7, VarStoreId: 0x6, VarOffset: 0x223, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3B 14 4B 14 E7 0C 06 00 23 02 10 10 00 01 00 }
0x574AC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x574B3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x574BA: 			End  { 29 02 }
0x574BC: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE8, VarStoreId: 0x6, VarOffset: 0x23F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 14 68 14 E8 0C 06 00 3F 02 10 10 00 01 00 }
0x574CD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x574D4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x574DB: 			End  { 29 02 }
0x574DD: 			GrayOutIf  { 19 82 }
0x574DF: 				EqIdVal QuestionId: 0xCDC, Value: 0x0 { 12 06 DC 0C 00 00 }
0x574E5: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCE9, VarStoreId: 0x6, VarOffset: 0x25B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 75 14 85 14 E9 0C 06 00 5B 02 10 10 00 01 00 }
0x574F6: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x574FD: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57504: 				End  { 29 02 }
0x57506: 			End  { 29 02 }
0x57508: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCEA, VarStoreId: 0x6, VarOffset: 0x277, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 14 A2 14 EA 0C 06 00 77 02 10 10 00 01 00 }
0x57519: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57520: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57527: 			End  { 29 02 }
0x57529: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xCEB, VarStoreId: 0x6, VarOffset: 0x293, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 4F 13 5F 13 EB 0C 06 00 93 02 10 10 00 04 00 }
0x5753A: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x57541: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x57548: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5754F: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x57556: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5755D: 			End  { 29 02 }
0x5755F: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCEC, VarStoreId: 0x6, VarOffset: 0x2AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D2 14 E2 14 EC 0C 06 00 AF 02 10 10 00 01 00 }
0x57570: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57577: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5757E: 			End  { 29 02 }
0x57580: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xCED, VarStoreId: 0x6, VarOffset: 0x39B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 EF 14 FF 14 ED 0C 06 00 9B 03 00 11 00 00 FF FF 01 00 }
0x57594: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5759B: 			End  { 29 02 }
0x5759D: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xCEE, VarStoreId: 0x6, VarOffset: 0x52B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 0C 15 1C 15 EE 0C 06 00 2B 05 00 10 00 07 01 }
0x575AE: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x575B4: 			End  { 29 02 }
0x575B6: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xCEF, VarStoreId: 0x6, VarOffset: 0x553, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 29 15 39 15 EF 0C 06 00 53 05 00 11 01 00 14 00 01 00 }
0x575CA: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x575D1: 			End  { 29 02 }
0x575D3: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xCF0, VarStoreId: 0x6, VarOffset: 0x57F, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 46 15 56 15 F0 0C 06 00 7F 05 00 10 04 14 04 }
0x575E4: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x575EA: 			End  { 29 02 }
0x575EC: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x575F3: 			End  { 29 02 }
0x575F5: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x575FC: 			End  { 29 02 }
0x575FE: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xCF1, VarStoreId: 0x6, VarOffset: 0x3EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6A 15 7A 15 F1 0C 06 00 EF 03 10 10 00 01 00 }
0x5760F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57616: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5761D: 			End  { 29 02 }
0x5761F: 			SuppressIf  { 0A 82 }
0x57621: 				EqIdVal QuestionId: 0xCF1, Value: 0x0 { 12 06 F1 0C 00 00 }
0x57627: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xCF2, VarStoreId: 0x6, VarOffset: 0x427, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C3 15 23 16 F2 0C 06 00 27 04 10 10 00 02 00 }
0x57638: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5763F: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x57646: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5764D: 				End  { 29 02 }
0x5764F: 				SuppressIf  { 0A 82 }
0x57651: 					EqIdVal QuestionId: 0xCF2, Value: 0x1 { 12 86 F2 0C 01 00 }
0x57657: 						Not  { 17 02 }
0x57659: 					End  { 29 02 }
0x5765B: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCF3, VarStoreId: 0x6, VarOffset: 0x4A3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 C5 15 25 16 F3 0C 06 00 A3 04 10 11 00 00 FF 03 01 00 }
0x5766F: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x57676: 					End  { 29 02 }
0x57678: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCF4, VarStoreId: 0x6, VarOffset: 0x443, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C6 15 26 16 F4 0C 06 00 43 04 10 10 00 05 00 }
0x57689: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x57690: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x57697: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5769E: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x576A5: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x576AC: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x576B3: 					End  { 29 02 }
0x576B5: 				End  { 29 02 }
0x576B7: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xCF5, VarStoreId: 0x6, VarOffset: 0x45F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C4 15 24 16 F5 0C 06 00 5F 04 10 10 00 02 00 }
0x576C8: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x576CF: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x576D6: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x576DD: 				End  { 29 02 }
0x576DF: 				SuppressIf  { 0A 82 }
0x576E1: 					EqIdVal QuestionId: 0xCF5, Value: 0x1 { 12 86 F5 0C 01 00 }
0x576E7: 						Not  { 17 02 }
0x576E9: 					End  { 29 02 }
0x576EB: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCF6, VarStoreId: 0x6, VarOffset: 0x4DB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 C7 15 27 16 F6 0C 06 00 DB 04 10 11 00 00 FF 03 01 00 }
0x576FF: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x57706: 					End  { 29 02 }
0x57708: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xCF7, VarStoreId: 0x6, VarOffset: 0x47B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C8 15 28 16 F7 0C 06 00 7B 04 10 10 00 05 00 }
0x57719: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x57720: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x57727: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5772E: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x57735: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5773C: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x57743: 					End  { 29 02 }
0x57745: 				End  { 29 02 }
0x57747: 			End  { 29 02 }
0x57749: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x57750: 			End  { 29 02 }
0x57752: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xCF8, VarStoreId: 0x6, VarOffset: 0x40B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 35 16 45 16 F8 0C 06 00 0B 04 10 10 00 01 00 }
0x57763: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5776A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57771: 			End  { 29 02 }
0x57773: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xCF9, VarStoreId: 0x6, VarOffset: 0xCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 14 C3 14 F9 0C 06 00 CA 00 10 10 00 01 00 }
0x57784: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5778B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57792: 			End  { 29 02 }
0x57794: 		End  { 29 02 }
0x57796: 	End  { 29 02 }
0x57798: 	Form FormId: 0x283D, Title: "PCI Express Root Port 14" { 01 86 3D 28 83 16 }
0x5779E: 		OneOf Prompt: "PCI Express Root Port 14", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xCFA, VarStoreId: 0x6, VarOffset: 0x10C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 13 7C 13 FA 0C 06 00 0C 01 10 10 00 01 00 }
0x577AF: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x577B6: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x577BD: 		End  { 29 02 }
0x577BF: 		SuppressIf  { 0A 82 }
0x577C1: 			EqIdVal QuestionId: 0xCFA, Value: 0x0 { 12 06 FA 0C 00 00 }
0x577C7: 			GrayOutIf  { 19 82 }
0x577C9: 				EqIdVal QuestionId: 0xD08, Value: 0x1 { 12 06 08 0D 01 00 }
0x577CF: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xCFB, VarStoreId: 0x6, VarOffset: 0x374, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 17 E5 0E FB 0C 06 00 74 03 10 10 00 01 00 }
0x577E0: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x577E7: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x577EE: 				End  { 29 02 }
0x577F0: 			End  { 29 02 }
0x577F2: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27FA, VarStoreId: 0x6, VarOffset: 0x128, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 83 12 F5 0D FA 27 06 00 28 01 10 10 00 04 00 }
0x57803: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5780A: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x57811: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x57818: 			End  { 29 02 }
0x5781A: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27FB, VarStoreId: 0x6, VarOffset: 0x2CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9F 12 AE 12 FB 27 06 00 CC 02 10 10 00 02 00 }
0x5782B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57832: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x57839: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x57840: 			End  { 29 02 }
0x57842: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xCFC, VarStoreId: 0x6, VarOffset: 0x2E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 12 CD 12 FC 0C 06 00 E8 02 10 10 00 01 00 }
0x57853: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5785A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57861: 			End  { 29 02 }
0x57863: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xCFD, VarStoreId: 0x6, VarOffset: 0x304, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DB 12 A7 0E FD 0C 06 00 04 03 10 10 00 01 00 }
0x57874: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5787B: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57882: 			End  { 29 02 }
0x57884: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27FC, VarStoreId: 0x6, VarOffset: 0x320, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F7 12 06 13 FC 27 06 00 20 03 10 10 00 01 00 }
0x57895: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5789C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x578A3: 			End  { 29 02 }
0x578A5: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCFE, VarStoreId: 0x6, VarOffset: 0x33C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 13 23 13 FE 0C 06 00 3C 03 10 10 00 01 00 }
0x578B6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x578BD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x578C4: 			End  { 29 02 }
0x578C6: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xCFF, VarStoreId: 0x6, VarOffset: 0x358, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 13 40 13 FF 0C 06 00 58 03 10 10 00 01 00 }
0x578D7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x578DE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x578E5: 			End  { 29 02 }
0x578E7: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD00, VarStoreId: 0x6, VarOffset: 0x144, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 13 99 13 00 0D 06 00 44 01 10 10 00 01 00 }
0x578F8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x578FF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57906: 			End  { 29 02 }
0x57908: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD01, VarStoreId: 0x6, VarOffset: 0x160, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A7 13 B6 13 01 0D 06 00 60 01 10 10 00 01 00 }
0x57919: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57920: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57927: 			End  { 29 02 }
0x57929: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD02, VarStoreId: 0x6, VarOffset: 0x17C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 13 D3 13 02 0D 06 00 7C 01 10 10 00 01 00 }
0x5793A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57941: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57948: 			End  { 29 02 }
0x5794A: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD03, VarStoreId: 0x6, VarOffset: 0x198, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 13 F0 13 03 0D 06 00 98 01 10 10 00 01 00 }
0x5795B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57962: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57969: 			End  { 29 02 }
0x5796B: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD04, VarStoreId: 0x6, VarOffset: 0x1EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 14 11 14 04 0D 06 00 EC 01 10 10 00 01 00 }
0x5797C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57983: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5798A: 			End  { 29 02 }
0x5798C: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD05, VarStoreId: 0x6, VarOffset: 0x208, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1F 14 2E 14 05 0D 06 00 08 02 10 10 00 01 00 }
0x5799D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x579A4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x579AB: 			End  { 29 02 }
0x579AD: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD06, VarStoreId: 0x6, VarOffset: 0x224, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 14 4B 14 06 0D 06 00 24 02 10 10 00 01 00 }
0x579BE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x579C5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x579CC: 			End  { 29 02 }
0x579CE: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD07, VarStoreId: 0x6, VarOffset: 0x240, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 59 14 68 14 07 0D 06 00 40 02 10 10 00 01 00 }
0x579DF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x579E6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x579ED: 			End  { 29 02 }
0x579EF: 			GrayOutIf  { 19 82 }
0x579F1: 				EqIdVal QuestionId: 0xCFB, Value: 0x0 { 12 06 FB 0C 00 00 }
0x579F7: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD08, VarStoreId: 0x6, VarOffset: 0x25C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 14 85 14 08 0D 06 00 5C 02 10 10 00 01 00 }
0x57A08: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57A0F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57A16: 				End  { 29 02 }
0x57A18: 			End  { 29 02 }
0x57A1A: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD09, VarStoreId: 0x6, VarOffset: 0x278, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 14 A2 14 09 0D 06 00 78 02 10 10 00 01 00 }
0x57A2B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57A32: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57A39: 			End  { 29 02 }
0x57A3B: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xD0A, VarStoreId: 0x6, VarOffset: 0x294, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 50 13 5F 13 0A 0D 06 00 94 02 10 10 00 04 00 }
0x57A4C: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x57A53: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x57A5A: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x57A61: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x57A68: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x57A6F: 			End  { 29 02 }
0x57A71: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD0B, VarStoreId: 0x6, VarOffset: 0x2B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D3 14 E2 14 0B 0D 06 00 B0 02 10 10 00 01 00 }
0x57A82: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57A89: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57A90: 			End  { 29 02 }
0x57A92: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xD0C, VarStoreId: 0x6, VarOffset: 0x39D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F0 14 FF 14 0C 0D 06 00 9D 03 00 11 00 00 FF FF 01 00 }
0x57AA6: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x57AAD: 			End  { 29 02 }
0x57AAF: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD0D, VarStoreId: 0x6, VarOffset: 0x52C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 0D 15 1C 15 0D 0D 06 00 2C 05 00 10 00 07 01 }
0x57AC0: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x57AC6: 			End  { 29 02 }
0x57AC8: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xD0E, VarStoreId: 0x6, VarOffset: 0x555, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 2A 15 39 15 0E 0D 06 00 55 05 00 11 01 00 14 00 01 00 }
0x57ADC: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x57AE3: 			End  { 29 02 }
0x57AE5: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD0F, VarStoreId: 0x6, VarOffset: 0x580, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 47 15 56 15 0F 0D 06 00 80 05 00 10 04 14 04 }
0x57AF6: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x57AFC: 			End  { 29 02 }
0x57AFE: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x57B05: 			End  { 29 02 }
0x57B07: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x57B0E: 			End  { 29 02 }
0x57B10: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD10, VarStoreId: 0x6, VarOffset: 0x3F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6B 15 7A 15 10 0D 06 00 F0 03 10 10 00 01 00 }
0x57B21: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57B28: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57B2F: 			End  { 29 02 }
0x57B31: 			SuppressIf  { 0A 82 }
0x57B33: 				EqIdVal QuestionId: 0xD10, Value: 0x0 { 12 06 10 0D 00 00 }
0x57B39: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD11, VarStoreId: 0x6, VarOffset: 0x428, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 C9 15 23 16 11 0D 06 00 28 04 10 10 00 02 00 }
0x57B4A: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57B51: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x57B58: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x57B5F: 				End  { 29 02 }
0x57B61: 				SuppressIf  { 0A 82 }
0x57B63: 					EqIdVal QuestionId: 0xD11, Value: 0x1 { 12 86 11 0D 01 00 }
0x57B69: 						Not  { 17 02 }
0x57B6B: 					End  { 29 02 }
0x57B6D: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD12, VarStoreId: 0x6, VarOffset: 0x4A5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 CB 15 25 16 12 0D 06 00 A5 04 10 11 00 00 FF 03 01 00 }
0x57B81: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x57B88: 					End  { 29 02 }
0x57B8A: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD13, VarStoreId: 0x6, VarOffset: 0x444, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 CC 15 26 16 13 0D 06 00 44 04 10 10 00 05 00 }
0x57B9B: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x57BA2: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x57BA9: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x57BB0: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x57BB7: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x57BBE: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x57BC5: 					End  { 29 02 }
0x57BC7: 				End  { 29 02 }
0x57BC9: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD14, VarStoreId: 0x6, VarOffset: 0x460, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 CA 15 24 16 14 0D 06 00 60 04 10 10 00 02 00 }
0x57BDA: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57BE1: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x57BE8: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x57BEF: 				End  { 29 02 }
0x57BF1: 				SuppressIf  { 0A 82 }
0x57BF3: 					EqIdVal QuestionId: 0xD14, Value: 0x1 { 12 86 14 0D 01 00 }
0x57BF9: 						Not  { 17 02 }
0x57BFB: 					End  { 29 02 }
0x57BFD: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD15, VarStoreId: 0x6, VarOffset: 0x4DD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 CD 15 27 16 15 0D 06 00 DD 04 10 11 00 00 FF 03 01 00 }
0x57C11: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x57C18: 					End  { 29 02 }
0x57C1A: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD16, VarStoreId: 0x6, VarOffset: 0x47C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 CE 15 28 16 16 0D 06 00 7C 04 10 10 00 05 00 }
0x57C2B: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x57C32: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x57C39: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x57C40: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x57C47: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x57C4E: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x57C55: 					End  { 29 02 }
0x57C57: 				End  { 29 02 }
0x57C59: 			End  { 29 02 }
0x57C5B: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x57C62: 			End  { 29 02 }
0x57C64: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xD17, VarStoreId: 0x6, VarOffset: 0x40C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 36 16 45 16 17 0D 06 00 0C 04 10 10 00 01 00 }
0x57C75: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57C7C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57C83: 			End  { 29 02 }
0x57C85: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD18, VarStoreId: 0x6, VarOffset: 0xCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 14 C3 14 18 0D 06 00 CB 00 10 10 00 01 00 }
0x57C96: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57C9D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57CA4: 			End  { 29 02 }
0x57CA6: 		End  { 29 02 }
0x57CA8: 	End  { 29 02 }
0x57CAA: 	Form FormId: 0x283E, Title: "PCI Express Root Port 15" { 01 86 3E 28 84 16 }
0x57CB0: 		OneOf Prompt: "PCI Express Root Port 15", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xD19, VarStoreId: 0x6, VarOffset: 0x10D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 13 7C 13 19 0D 06 00 0D 01 10 10 00 01 00 }
0x57CC1: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57CC8: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57CCF: 		End  { 29 02 }
0x57CD1: 		SuppressIf  { 0A 82 }
0x57CD3: 			EqIdVal QuestionId: 0xD19, Value: 0x0 { 12 06 19 0D 00 00 }
0x57CD9: 			GrayOutIf  { 19 82 }
0x57CDB: 				EqIdVal QuestionId: 0xD27, Value: 0x1 { 12 06 27 0D 01 00 }
0x57CE1: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xD1A, VarStoreId: 0x6, VarOffset: 0x375, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2E 17 E5 0E 1A 0D 06 00 75 03 10 10 00 01 00 }
0x57CF2: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x57CF9: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x57D00: 				End  { 29 02 }
0x57D02: 			End  { 29 02 }
0x57D04: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x27FD, VarStoreId: 0x6, VarOffset: 0x129, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 84 12 F5 0D FD 27 06 00 29 01 10 10 00 04 00 }
0x57D15: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57D1C: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x57D23: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x57D2A: 			End  { 29 02 }
0x57D2C: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x27FE, VarStoreId: 0x6, VarOffset: 0x2CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A0 12 AE 12 FE 27 06 00 CD 02 10 10 00 02 00 }
0x57D3D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57D44: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x57D4B: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x57D52: 			End  { 29 02 }
0x57D54: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD1B, VarStoreId: 0x6, VarOffset: 0x2E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 12 CD 12 1B 0D 06 00 E9 02 10 10 00 01 00 }
0x57D65: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57D6C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57D73: 			End  { 29 02 }
0x57D75: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xD1C, VarStoreId: 0x6, VarOffset: 0x305, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 12 A7 0E 1C 0D 06 00 05 03 10 10 00 01 00 }
0x57D86: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57D8D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57D94: 			End  { 29 02 }
0x57D96: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x27FF, VarStoreId: 0x6, VarOffset: 0x321, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F8 12 06 13 FF 27 06 00 21 03 10 10 00 01 00 }
0x57DA7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57DAE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57DB5: 			End  { 29 02 }
0x57DB7: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD1D, VarStoreId: 0x6, VarOffset: 0x33D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 15 13 23 13 1D 0D 06 00 3D 03 10 10 00 01 00 }
0x57DC8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57DCF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57DD6: 			End  { 29 02 }
0x57DD8: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD1E, VarStoreId: 0x6, VarOffset: 0x359, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 13 40 13 1E 0D 06 00 59 03 10 10 00 01 00 }
0x57DE9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57DF0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57DF7: 			End  { 29 02 }
0x57DF9: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD1F, VarStoreId: 0x6, VarOffset: 0x145, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 13 99 13 1F 0D 06 00 45 01 10 10 00 01 00 }
0x57E0A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57E11: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57E18: 			End  { 29 02 }
0x57E1A: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD20, VarStoreId: 0x6, VarOffset: 0x161, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 13 B6 13 20 0D 06 00 61 01 10 10 00 01 00 }
0x57E2B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57E32: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57E39: 			End  { 29 02 }
0x57E3B: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD21, VarStoreId: 0x6, VarOffset: 0x17D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 13 D3 13 21 0D 06 00 7D 01 10 10 00 01 00 }
0x57E4C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57E53: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57E5A: 			End  { 29 02 }
0x57E5C: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD22, VarStoreId: 0x6, VarOffset: 0x199, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 13 F0 13 22 0D 06 00 99 01 10 10 00 01 00 }
0x57E6D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57E74: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57E7B: 			End  { 29 02 }
0x57E7D: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD23, VarStoreId: 0x6, VarOffset: 0x1ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 03 14 11 14 23 0D 06 00 ED 01 10 10 00 01 00 }
0x57E8E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57E95: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57E9C: 			End  { 29 02 }
0x57E9E: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD24, VarStoreId: 0x6, VarOffset: 0x209, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 20 14 2E 14 24 0D 06 00 09 02 10 10 00 01 00 }
0x57EAF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57EB6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57EBD: 			End  { 29 02 }
0x57EBF: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD25, VarStoreId: 0x6, VarOffset: 0x225, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 14 4B 14 25 0D 06 00 25 02 10 10 00 01 00 }
0x57ED0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57ED7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57EDE: 			End  { 29 02 }
0x57EE0: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD26, VarStoreId: 0x6, VarOffset: 0x241, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5A 14 68 14 26 0D 06 00 41 02 10 10 00 01 00 }
0x57EF1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57EF8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57EFF: 			End  { 29 02 }
0x57F01: 			GrayOutIf  { 19 82 }
0x57F03: 				EqIdVal QuestionId: 0xD1A, Value: 0x0 { 12 06 1A 0D 00 00 }
0x57F09: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD27, VarStoreId: 0x6, VarOffset: 0x25D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 77 14 85 14 27 0D 06 00 5D 02 10 10 00 01 00 }
0x57F1A: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57F21: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57F28: 				End  { 29 02 }
0x57F2A: 			End  { 29 02 }
0x57F2C: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD28, VarStoreId: 0x6, VarOffset: 0x279, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 14 A2 14 28 0D 06 00 79 02 10 10 00 01 00 }
0x57F3D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x57F44: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x57F4B: 			End  { 29 02 }
0x57F4D: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xD29, VarStoreId: 0x6, VarOffset: 0x295, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 51 13 5F 13 29 0D 06 00 95 02 10 10 00 04 00 }
0x57F5E: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x57F65: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x57F6C: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x57F73: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x57F7A: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x57F81: 			End  { 29 02 }
0x57F83: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD2A, VarStoreId: 0x6, VarOffset: 0x2B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D4 14 E2 14 2A 0D 06 00 B1 02 10 10 00 01 00 }
0x57F94: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x57F9B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x57FA2: 			End  { 29 02 }
0x57FA4: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xD2B, VarStoreId: 0x6, VarOffset: 0x39F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F1 14 FF 14 2B 0D 06 00 9F 03 00 11 00 00 FF FF 01 00 }
0x57FB8: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x57FBF: 			End  { 29 02 }
0x57FC1: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD2C, VarStoreId: 0x6, VarOffset: 0x52D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 0E 15 1C 15 2C 0D 06 00 2D 05 00 10 00 07 01 }
0x57FD2: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x57FD8: 			End  { 29 02 }
0x57FDA: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xD2D, VarStoreId: 0x6, VarOffset: 0x557, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 2B 15 39 15 2D 0D 06 00 57 05 00 11 01 00 14 00 01 00 }
0x57FEE: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x57FF5: 			End  { 29 02 }
0x57FF7: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD2E, VarStoreId: 0x6, VarOffset: 0x581, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 48 15 56 15 2E 0D 06 00 81 05 00 10 04 14 04 }
0x58008: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5800E: 			End  { 29 02 }
0x58010: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58017: 			End  { 29 02 }
0x58019: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x58020: 			End  { 29 02 }
0x58022: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD2F, VarStoreId: 0x6, VarOffset: 0x3F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6C 15 7A 15 2F 0D 06 00 F1 03 10 10 00 01 00 }
0x58033: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5803A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58041: 			End  { 29 02 }
0x58043: 			SuppressIf  { 0A 82 }
0x58045: 				EqIdVal QuestionId: 0xD2F, Value: 0x0 { 12 06 2F 0D 00 00 }
0x5804B: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD30, VarStoreId: 0x6, VarOffset: 0x429, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 CF 15 23 16 30 0D 06 00 29 04 10 10 00 02 00 }
0x5805C: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58063: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5806A: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58071: 				End  { 29 02 }
0x58073: 				SuppressIf  { 0A 82 }
0x58075: 					EqIdVal QuestionId: 0xD30, Value: 0x1 { 12 86 30 0D 01 00 }
0x5807B: 						Not  { 17 02 }
0x5807D: 					End  { 29 02 }
0x5807F: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD31, VarStoreId: 0x6, VarOffset: 0x4A7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D1 15 25 16 31 0D 06 00 A7 04 10 11 00 00 FF 03 01 00 }
0x58093: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5809A: 					End  { 29 02 }
0x5809C: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD32, VarStoreId: 0x6, VarOffset: 0x445, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 D2 15 26 16 32 0D 06 00 45 04 10 10 00 05 00 }
0x580AD: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x580B4: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x580BB: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x580C2: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x580C9: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x580D0: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x580D7: 					End  { 29 02 }
0x580D9: 				End  { 29 02 }
0x580DB: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD33, VarStoreId: 0x6, VarOffset: 0x461, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D0 15 24 16 33 0D 06 00 61 04 10 10 00 02 00 }
0x580EC: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x580F3: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x580FA: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58101: 				End  { 29 02 }
0x58103: 				SuppressIf  { 0A 82 }
0x58105: 					EqIdVal QuestionId: 0xD33, Value: 0x1 { 12 86 33 0D 01 00 }
0x5810B: 						Not  { 17 02 }
0x5810D: 					End  { 29 02 }
0x5810F: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD34, VarStoreId: 0x6, VarOffset: 0x4DF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D3 15 27 16 34 0D 06 00 DF 04 10 11 00 00 FF 03 01 00 }
0x58123: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5812A: 					End  { 29 02 }
0x5812C: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD35, VarStoreId: 0x6, VarOffset: 0x47D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 D4 15 28 16 35 0D 06 00 7D 04 10 10 00 05 00 }
0x5813D: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x58144: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5814B: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x58152: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x58159: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x58160: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x58167: 					End  { 29 02 }
0x58169: 				End  { 29 02 }
0x5816B: 			End  { 29 02 }
0x5816D: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58174: 			End  { 29 02 }
0x58176: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xD36, VarStoreId: 0x6, VarOffset: 0x40D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 37 16 45 16 36 0D 06 00 0D 04 10 10 00 01 00 }
0x58187: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5818E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58195: 			End  { 29 02 }
0x58197: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD37, VarStoreId: 0x6, VarOffset: 0xCC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 14 C3 14 37 0D 06 00 CC 00 10 10 00 01 00 }
0x581A8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x581AF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x581B6: 			End  { 29 02 }
0x581B8: 		End  { 29 02 }
0x581BA: 	End  { 29 02 }
0x581BC: 	Form FormId: 0x283F, Title: "PCI Express Root Port 16" { 01 86 3F 28 85 16 }
0x581C2: 		OneOf Prompt: "PCI Express Root Port 16", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xD38, VarStoreId: 0x6, VarOffset: 0x10E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6F 13 7C 13 38 0D 06 00 0E 01 10 10 00 01 00 }
0x581D3: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x581DA: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x581E1: 		End  { 29 02 }
0x581E3: 		SuppressIf  { 0A 82 }
0x581E5: 			EqIdVal QuestionId: 0xD38, Value: 0x0 { 12 06 38 0D 00 00 }
0x581EB: 			GrayOutIf  { 19 82 }
0x581ED: 				EqIdVal QuestionId: 0xD46, Value: 0x1 { 12 06 46 0D 01 00 }
0x581F3: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xD39, VarStoreId: 0x6, VarOffset: 0x376, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2F 17 E5 0E 39 0D 06 00 76 03 10 10 00 01 00 }
0x58204: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5820B: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x58212: 				End  { 29 02 }
0x58214: 			End  { 29 02 }
0x58216: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2800, VarStoreId: 0x6, VarOffset: 0x12A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 85 12 F5 0D 00 28 06 00 2A 01 10 10 00 04 00 }
0x58227: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5822E: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x58235: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5823C: 			End  { 29 02 }
0x5823E: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2801, VarStoreId: 0x6, VarOffset: 0x2CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A1 12 AE 12 01 28 06 00 CE 02 10 10 00 02 00 }
0x5824F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58256: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5825D: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x58264: 			End  { 29 02 }
0x58266: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD3A, VarStoreId: 0x6, VarOffset: 0x2EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 12 CD 12 3A 0D 06 00 EA 02 10 10 00 01 00 }
0x58277: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5827E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58285: 			End  { 29 02 }
0x58287: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xD3B, VarStoreId: 0x6, VarOffset: 0x306, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DD 12 A7 0E 3B 0D 06 00 06 03 10 10 00 01 00 }
0x58298: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5829F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x582A6: 			End  { 29 02 }
0x582A8: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2802, VarStoreId: 0x6, VarOffset: 0x322, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 12 06 13 02 28 06 00 22 03 10 10 00 01 00 }
0x582B9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x582C0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x582C7: 			End  { 29 02 }
0x582C9: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD3C, VarStoreId: 0x6, VarOffset: 0x33E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 16 13 23 13 3C 0D 06 00 3E 03 10 10 00 01 00 }
0x582DA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x582E1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x582E8: 			End  { 29 02 }
0x582EA: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD3D, VarStoreId: 0x6, VarOffset: 0x35A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 13 40 13 3D 0D 06 00 5A 03 10 10 00 01 00 }
0x582FB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58302: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58309: 			End  { 29 02 }
0x5830B: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD3E, VarStoreId: 0x6, VarOffset: 0x146, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 13 99 13 3E 0D 06 00 46 01 10 10 00 01 00 }
0x5831C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58323: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5832A: 			End  { 29 02 }
0x5832C: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD3F, VarStoreId: 0x6, VarOffset: 0x162, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 13 B6 13 3F 0D 06 00 62 01 10 10 00 01 00 }
0x5833D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58344: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5834B: 			End  { 29 02 }
0x5834D: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD40, VarStoreId: 0x6, VarOffset: 0x17E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 13 D3 13 40 0D 06 00 7E 01 10 10 00 01 00 }
0x5835E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58365: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5836C: 			End  { 29 02 }
0x5836E: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD41, VarStoreId: 0x6, VarOffset: 0x19A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 13 F0 13 41 0D 06 00 9A 01 10 10 00 01 00 }
0x5837F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58386: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5838D: 			End  { 29 02 }
0x5838F: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD42, VarStoreId: 0x6, VarOffset: 0x1EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 04 14 11 14 42 0D 06 00 EE 01 10 10 00 01 00 }
0x583A0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x583A7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x583AE: 			End  { 29 02 }
0x583B0: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD43, VarStoreId: 0x6, VarOffset: 0x20A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 21 14 2E 14 43 0D 06 00 0A 02 10 10 00 01 00 }
0x583C1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x583C8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x583CF: 			End  { 29 02 }
0x583D1: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD44, VarStoreId: 0x6, VarOffset: 0x226, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 14 4B 14 44 0D 06 00 26 02 10 10 00 01 00 }
0x583E2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x583E9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x583F0: 			End  { 29 02 }
0x583F2: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD45, VarStoreId: 0x6, VarOffset: 0x242, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5B 14 68 14 45 0D 06 00 42 02 10 10 00 01 00 }
0x58403: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5840A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58411: 			End  { 29 02 }
0x58413: 			GrayOutIf  { 19 82 }
0x58415: 				EqIdVal QuestionId: 0xD39, Value: 0x0 { 12 06 39 0D 00 00 }
0x5841B: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD46, VarStoreId: 0x6, VarOffset: 0x25E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 14 85 14 46 0D 06 00 5E 02 10 10 00 01 00 }
0x5842C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58433: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5843A: 				End  { 29 02 }
0x5843C: 			End  { 29 02 }
0x5843E: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD47, VarStoreId: 0x6, VarOffset: 0x27A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 14 A2 14 47 0D 06 00 7A 02 10 10 00 01 00 }
0x5844F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58456: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5845D: 			End  { 29 02 }
0x5845F: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xD48, VarStoreId: 0x6, VarOffset: 0x296, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 52 13 5F 13 48 0D 06 00 96 02 10 10 00 04 00 }
0x58470: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x58477: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5847E: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x58485: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5848C: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x58493: 			End  { 29 02 }
0x58495: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD49, VarStoreId: 0x6, VarOffset: 0x2B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D5 14 E2 14 49 0D 06 00 B2 02 10 10 00 01 00 }
0x584A6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x584AD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x584B4: 			End  { 29 02 }
0x584B6: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xD4A, VarStoreId: 0x6, VarOffset: 0x3A1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F2 14 FF 14 4A 0D 06 00 A1 03 00 11 00 00 FF FF 01 00 }
0x584CA: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x584D1: 			End  { 29 02 }
0x584D3: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD4B, VarStoreId: 0x6, VarOffset: 0x52E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 0F 15 1C 15 4B 0D 06 00 2E 05 00 10 00 07 01 }
0x584E4: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x584EA: 			End  { 29 02 }
0x584EC: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xD4C, VarStoreId: 0x6, VarOffset: 0x559, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 2C 15 39 15 4C 0D 06 00 59 05 00 11 01 00 14 00 01 00 }
0x58500: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x58507: 			End  { 29 02 }
0x58509: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD4D, VarStoreId: 0x6, VarOffset: 0x582, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 49 15 56 15 4D 0D 06 00 82 05 00 10 04 14 04 }
0x5851A: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x58520: 			End  { 29 02 }
0x58522: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58529: 			End  { 29 02 }
0x5852B: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x58532: 			End  { 29 02 }
0x58534: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD4E, VarStoreId: 0x6, VarOffset: 0x3F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6D 15 7A 15 4E 0D 06 00 F2 03 10 10 00 01 00 }
0x58545: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5854C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58553: 			End  { 29 02 }
0x58555: 			SuppressIf  { 0A 82 }
0x58557: 				EqIdVal QuestionId: 0xD4E, Value: 0x0 { 12 06 4E 0D 00 00 }
0x5855D: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD4F, VarStoreId: 0x6, VarOffset: 0x42A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D5 15 23 16 4F 0D 06 00 2A 04 10 10 00 02 00 }
0x5856E: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58575: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5857C: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58583: 				End  { 29 02 }
0x58585: 				SuppressIf  { 0A 82 }
0x58587: 					EqIdVal QuestionId: 0xD4F, Value: 0x1 { 12 86 4F 0D 01 00 }
0x5858D: 						Not  { 17 02 }
0x5858F: 					End  { 29 02 }
0x58591: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD50, VarStoreId: 0x6, VarOffset: 0x4A9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D7 15 25 16 50 0D 06 00 A9 04 10 11 00 00 FF 03 01 00 }
0x585A5: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x585AC: 					End  { 29 02 }
0x585AE: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD51, VarStoreId: 0x6, VarOffset: 0x446, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 D8 15 26 16 51 0D 06 00 46 04 10 10 00 05 00 }
0x585BF: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x585C6: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x585CD: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x585D4: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x585DB: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x585E2: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x585E9: 					End  { 29 02 }
0x585EB: 				End  { 29 02 }
0x585ED: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD52, VarStoreId: 0x6, VarOffset: 0x462, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D6 15 24 16 52 0D 06 00 62 04 10 10 00 02 00 }
0x585FE: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58605: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5860C: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58613: 				End  { 29 02 }
0x58615: 				SuppressIf  { 0A 82 }
0x58617: 					EqIdVal QuestionId: 0xD52, Value: 0x1 { 12 86 52 0D 01 00 }
0x5861D: 						Not  { 17 02 }
0x5861F: 					End  { 29 02 }
0x58621: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD53, VarStoreId: 0x6, VarOffset: 0x4E1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 D9 15 27 16 53 0D 06 00 E1 04 10 11 00 00 FF 03 01 00 }
0x58635: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5863C: 					End  { 29 02 }
0x5863E: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD54, VarStoreId: 0x6, VarOffset: 0x47E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 DA 15 28 16 54 0D 06 00 7E 04 10 10 00 05 00 }
0x5864F: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x58656: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5865D: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x58664: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5866B: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x58672: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x58679: 					End  { 29 02 }
0x5867B: 				End  { 29 02 }
0x5867D: 			End  { 29 02 }
0x5867F: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58686: 			End  { 29 02 }
0x58688: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xD55, VarStoreId: 0x6, VarOffset: 0x40E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 16 45 16 55 0D 06 00 0E 04 10 10 00 01 00 }
0x58699: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x586A0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x586A7: 			End  { 29 02 }
0x586A9: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD56, VarStoreId: 0x6, VarOffset: 0xCD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 14 C3 14 56 0D 06 00 CD 00 10 10 00 01 00 }
0x586BA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x586C1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x586C8: 			End  { 29 02 }
0x586CA: 		End  { 29 02 }
0x586CC: 	End  { 29 02 }
0x586CE: 	Form FormId: 0x2840, Title: "PCI Express Root Port 17" { 01 86 40 28 86 16 }
0x586D4: 		OneOf Prompt: "PCI Express Root Port 17", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xD57, VarStoreId: 0x6, VarOffset: 0x10F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 13 7C 13 57 0D 06 00 0F 01 10 10 00 01 00 }
0x586E5: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x586EC: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x586F3: 		End  { 29 02 }
0x586F5: 		SuppressIf  { 0A 82 }
0x586F7: 			EqIdVal QuestionId: 0xD57, Value: 0x0 { 12 06 57 0D 00 00 }
0x586FD: 			GrayOutIf  { 19 82 }
0x586FF: 				EqIdVal QuestionId: 0xD65, Value: 0x1 { 12 06 65 0D 01 00 }
0x58705: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xD58, VarStoreId: 0x6, VarOffset: 0x377, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 30 17 E5 0E 58 0D 06 00 77 03 10 10 00 01 00 }
0x58716: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5871D: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x58724: 				End  { 29 02 }
0x58726: 			End  { 29 02 }
0x58728: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2803, VarStoreId: 0x6, VarOffset: 0x12B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 86 12 F5 0D 03 28 06 00 2B 01 10 10 00 04 00 }
0x58739: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58740: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x58747: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5874E: 			End  { 29 02 }
0x58750: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2804, VarStoreId: 0x6, VarOffset: 0x2CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A2 12 AE 12 04 28 06 00 CF 02 10 10 00 02 00 }
0x58761: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58768: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5876F: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x58776: 			End  { 29 02 }
0x58778: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD59, VarStoreId: 0x6, VarOffset: 0x2EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 12 CD 12 59 0D 06 00 EB 02 10 10 00 01 00 }
0x58789: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58790: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58797: 			End  { 29 02 }
0x58799: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xD5A, VarStoreId: 0x6, VarOffset: 0x307, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 12 A7 0E 5A 0D 06 00 07 03 10 10 00 01 00 }
0x587AA: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x587B1: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x587B8: 			End  { 29 02 }
0x587BA: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2805, VarStoreId: 0x6, VarOffset: 0x323, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 12 06 13 05 28 06 00 23 03 10 10 00 01 00 }
0x587CB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x587D2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x587D9: 			End  { 29 02 }
0x587DB: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD5B, VarStoreId: 0x6, VarOffset: 0x33F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 17 13 23 13 5B 0D 06 00 3F 03 10 10 00 01 00 }
0x587EC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x587F3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x587FA: 			End  { 29 02 }
0x587FC: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD5C, VarStoreId: 0x6, VarOffset: 0x35B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 13 40 13 5C 0D 06 00 5B 03 10 10 00 01 00 }
0x5880D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58814: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5881B: 			End  { 29 02 }
0x5881D: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD5D, VarStoreId: 0x6, VarOffset: 0x147, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8D 13 99 13 5D 0D 06 00 47 01 10 10 00 01 00 }
0x5882E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58835: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5883C: 			End  { 29 02 }
0x5883E: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD5E, VarStoreId: 0x6, VarOffset: 0x163, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 13 B6 13 5E 0D 06 00 63 01 10 10 00 01 00 }
0x5884F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58856: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5885D: 			End  { 29 02 }
0x5885F: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD5F, VarStoreId: 0x6, VarOffset: 0x17F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C7 13 D3 13 5F 0D 06 00 7F 01 10 10 00 01 00 }
0x58870: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58877: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5887E: 			End  { 29 02 }
0x58880: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD60, VarStoreId: 0x6, VarOffset: 0x19B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 13 F0 13 60 0D 06 00 9B 01 10 10 00 01 00 }
0x58891: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58898: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5889F: 			End  { 29 02 }
0x588A1: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD61, VarStoreId: 0x6, VarOffset: 0x1EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 05 14 11 14 61 0D 06 00 EF 01 10 10 00 01 00 }
0x588B2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x588B9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x588C0: 			End  { 29 02 }
0x588C2: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD62, VarStoreId: 0x6, VarOffset: 0x20B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 14 2E 14 62 0D 06 00 0B 02 10 10 00 01 00 }
0x588D3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x588DA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x588E1: 			End  { 29 02 }
0x588E3: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD63, VarStoreId: 0x6, VarOffset: 0x227, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3F 14 4B 14 63 0D 06 00 27 02 10 10 00 01 00 }
0x588F4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x588FB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58902: 			End  { 29 02 }
0x58904: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD64, VarStoreId: 0x6, VarOffset: 0x243, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5C 14 68 14 64 0D 06 00 43 02 10 10 00 01 00 }
0x58915: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5891C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58923: 			End  { 29 02 }
0x58925: 			GrayOutIf  { 19 82 }
0x58927: 				EqIdVal QuestionId: 0xD58, Value: 0x0 { 12 06 58 0D 00 00 }
0x5892D: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD65, VarStoreId: 0x6, VarOffset: 0x25F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 79 14 85 14 65 0D 06 00 5F 02 10 10 00 01 00 }
0x5893E: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58945: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5894C: 				End  { 29 02 }
0x5894E: 			End  { 29 02 }
0x58950: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD66, VarStoreId: 0x6, VarOffset: 0x27B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 96 14 A2 14 66 0D 06 00 7B 02 10 10 00 01 00 }
0x58961: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58968: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5896F: 			End  { 29 02 }
0x58971: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xD67, VarStoreId: 0x6, VarOffset: 0x297, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 53 13 5F 13 67 0D 06 00 97 02 10 10 00 04 00 }
0x58982: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x58989: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x58990: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x58997: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5899E: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x589A5: 			End  { 29 02 }
0x589A7: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD68, VarStoreId: 0x6, VarOffset: 0x2B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D6 14 E2 14 68 0D 06 00 B3 02 10 10 00 01 00 }
0x589B8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x589BF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x589C6: 			End  { 29 02 }
0x589C8: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xD69, VarStoreId: 0x6, VarOffset: 0x3A3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F3 14 FF 14 69 0D 06 00 A3 03 00 11 00 00 FF FF 01 00 }
0x589DC: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x589E3: 			End  { 29 02 }
0x589E5: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD6A, VarStoreId: 0x6, VarOffset: 0x52F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 10 15 1C 15 6A 0D 06 00 2F 05 00 10 00 07 01 }
0x589F6: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x589FC: 			End  { 29 02 }
0x589FE: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xD6B, VarStoreId: 0x6, VarOffset: 0x55B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 2D 15 39 15 6B 0D 06 00 5B 05 00 11 01 00 14 00 01 00 }
0x58A12: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x58A19: 			End  { 29 02 }
0x58A1B: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD6C, VarStoreId: 0x6, VarOffset: 0x583, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 4A 15 56 15 6C 0D 06 00 83 05 00 10 04 14 04 }
0x58A2C: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x58A32: 			End  { 29 02 }
0x58A34: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58A3B: 			End  { 29 02 }
0x58A3D: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x58A44: 			End  { 29 02 }
0x58A46: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD6D, VarStoreId: 0x6, VarOffset: 0x3F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6E 15 7A 15 6D 0D 06 00 F3 03 10 10 00 01 00 }
0x58A57: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58A5E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58A65: 			End  { 29 02 }
0x58A67: 			SuppressIf  { 0A 82 }
0x58A69: 				EqIdVal QuestionId: 0xD6D, Value: 0x0 { 12 06 6D 0D 00 00 }
0x58A6F: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD6E, VarStoreId: 0x6, VarOffset: 0x42B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DB 15 23 16 6E 0D 06 00 2B 04 10 10 00 02 00 }
0x58A80: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58A87: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x58A8E: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58A95: 				End  { 29 02 }
0x58A97: 				SuppressIf  { 0A 82 }
0x58A99: 					EqIdVal QuestionId: 0xD6E, Value: 0x1 { 12 86 6E 0D 01 00 }
0x58A9F: 						Not  { 17 02 }
0x58AA1: 					End  { 29 02 }
0x58AA3: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD6F, VarStoreId: 0x6, VarOffset: 0x4AB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 DD 15 25 16 6F 0D 06 00 AB 04 10 11 00 00 FF 03 01 00 }
0x58AB7: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x58ABE: 					End  { 29 02 }
0x58AC0: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD70, VarStoreId: 0x6, VarOffset: 0x447, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 DE 15 26 16 70 0D 06 00 47 04 10 10 00 05 00 }
0x58AD1: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x58AD8: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x58ADF: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x58AE6: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x58AED: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x58AF4: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x58AFB: 					End  { 29 02 }
0x58AFD: 				End  { 29 02 }
0x58AFF: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD71, VarStoreId: 0x6, VarOffset: 0x463, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 DC 15 24 16 71 0D 06 00 63 04 10 10 00 02 00 }
0x58B10: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58B17: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x58B1E: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58B25: 				End  { 29 02 }
0x58B27: 				SuppressIf  { 0A 82 }
0x58B29: 					EqIdVal QuestionId: 0xD71, Value: 0x1 { 12 86 71 0D 01 00 }
0x58B2F: 						Not  { 17 02 }
0x58B31: 					End  { 29 02 }
0x58B33: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD72, VarStoreId: 0x6, VarOffset: 0x4E3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 DF 15 27 16 72 0D 06 00 E3 04 10 11 00 00 FF 03 01 00 }
0x58B47: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x58B4E: 					End  { 29 02 }
0x58B50: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD73, VarStoreId: 0x6, VarOffset: 0x47F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 E0 15 28 16 73 0D 06 00 7F 04 10 10 00 05 00 }
0x58B61: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x58B68: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x58B6F: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x58B76: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x58B7D: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x58B84: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x58B8B: 					End  { 29 02 }
0x58B8D: 				End  { 29 02 }
0x58B8F: 			End  { 29 02 }
0x58B91: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58B98: 			End  { 29 02 }
0x58B9A: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xD74, VarStoreId: 0x6, VarOffset: 0x40F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 16 45 16 74 0D 06 00 0F 04 10 10 00 01 00 }
0x58BAB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58BB2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58BB9: 			End  { 29 02 }
0x58BBB: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD75, VarStoreId: 0x6, VarOffset: 0xCE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 14 C3 14 75 0D 06 00 CE 00 10 10 00 01 00 }
0x58BCC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58BD3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58BDA: 			End  { 29 02 }
0x58BDC: 		End  { 29 02 }
0x58BDE: 	End  { 29 02 }
0x58BE0: 	Form FormId: 0x2841, Title: "PCI Express Root Port 18" { 01 86 41 28 87 16 }
0x58BE6: 		OneOf Prompt: "PCI Express Root Port 18", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xD76, VarStoreId: 0x6, VarOffset: 0x110, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 71 13 7C 13 76 0D 06 00 10 01 10 10 00 01 00 }
0x58BF7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58BFE: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58C05: 		End  { 29 02 }
0x58C07: 		SuppressIf  { 0A 82 }
0x58C09: 			EqIdVal QuestionId: 0xD76, Value: 0x0 { 12 06 76 0D 00 00 }
0x58C0F: 			GrayOutIf  { 19 82 }
0x58C11: 				EqIdVal QuestionId: 0xD84, Value: 0x1 { 12 06 84 0D 01 00 }
0x58C17: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xD77, VarStoreId: 0x6, VarOffset: 0x378, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 31 17 E5 0E 77 0D 06 00 78 03 10 10 00 01 00 }
0x58C28: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x58C2F: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x58C36: 				End  { 29 02 }
0x58C38: 			End  { 29 02 }
0x58C3A: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2806, VarStoreId: 0x6, VarOffset: 0x12C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 87 12 F5 0D 06 28 06 00 2C 01 10 10 00 04 00 }
0x58C4B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58C52: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x58C59: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x58C60: 			End  { 29 02 }
0x58C62: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2807, VarStoreId: 0x6, VarOffset: 0x2D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A3 12 AE 12 07 28 06 00 D0 02 10 10 00 02 00 }
0x58C73: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58C7A: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x58C81: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x58C88: 			End  { 29 02 }
0x58C8A: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD78, VarStoreId: 0x6, VarOffset: 0x2EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 12 CD 12 78 0D 06 00 EC 02 10 10 00 01 00 }
0x58C9B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58CA2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58CA9: 			End  { 29 02 }
0x58CAB: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xD79, VarStoreId: 0x6, VarOffset: 0x308, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 12 A7 0E 79 0D 06 00 08 03 10 10 00 01 00 }
0x58CBC: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58CC3: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58CCA: 			End  { 29 02 }
0x58CCC: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2808, VarStoreId: 0x6, VarOffset: 0x324, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FB 12 06 13 08 28 06 00 24 03 10 10 00 01 00 }
0x58CDD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58CE4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58CEB: 			End  { 29 02 }
0x58CED: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD7A, VarStoreId: 0x6, VarOffset: 0x340, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 18 13 23 13 7A 0D 06 00 40 03 10 10 00 01 00 }
0x58CFE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58D05: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58D0C: 			End  { 29 02 }
0x58D0E: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD7B, VarStoreId: 0x6, VarOffset: 0x35C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 35 13 40 13 7B 0D 06 00 5C 03 10 10 00 01 00 }
0x58D1F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58D26: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58D2D: 			End  { 29 02 }
0x58D2F: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD7C, VarStoreId: 0x6, VarOffset: 0x148, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 13 99 13 7C 0D 06 00 48 01 10 10 00 01 00 }
0x58D40: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58D47: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58D4E: 			End  { 29 02 }
0x58D50: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD7D, VarStoreId: 0x6, VarOffset: 0x164, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AB 13 B6 13 7D 0D 06 00 64 01 10 10 00 01 00 }
0x58D61: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58D68: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58D6F: 			End  { 29 02 }
0x58D71: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD7E, VarStoreId: 0x6, VarOffset: 0x180, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 13 D3 13 7E 0D 06 00 80 01 10 10 00 01 00 }
0x58D82: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58D89: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58D90: 			End  { 29 02 }
0x58D92: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD7F, VarStoreId: 0x6, VarOffset: 0x19C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E5 13 F0 13 7F 0D 06 00 9C 01 10 10 00 01 00 }
0x58DA3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58DAA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58DB1: 			End  { 29 02 }
0x58DB3: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD80, VarStoreId: 0x6, VarOffset: 0x1F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 06 14 11 14 80 0D 06 00 F0 01 10 10 00 01 00 }
0x58DC4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58DCB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58DD2: 			End  { 29 02 }
0x58DD4: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD81, VarStoreId: 0x6, VarOffset: 0x20C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 23 14 2E 14 81 0D 06 00 0C 02 10 10 00 01 00 }
0x58DE5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58DEC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58DF3: 			End  { 29 02 }
0x58DF5: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD82, VarStoreId: 0x6, VarOffset: 0x228, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 14 4B 14 82 0D 06 00 28 02 10 10 00 01 00 }
0x58E06: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58E0D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58E14: 			End  { 29 02 }
0x58E16: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD83, VarStoreId: 0x6, VarOffset: 0x244, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5D 14 68 14 83 0D 06 00 44 02 10 10 00 01 00 }
0x58E27: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58E2E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58E35: 			End  { 29 02 }
0x58E37: 			GrayOutIf  { 19 82 }
0x58E39: 				EqIdVal QuestionId: 0xD77, Value: 0x0 { 12 06 77 0D 00 00 }
0x58E3F: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD84, VarStoreId: 0x6, VarOffset: 0x260, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 14 85 14 84 0D 06 00 60 02 10 10 00 01 00 }
0x58E50: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58E57: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58E5E: 				End  { 29 02 }
0x58E60: 			End  { 29 02 }
0x58E62: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD85, VarStoreId: 0x6, VarOffset: 0x27C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 14 A2 14 85 0D 06 00 7C 02 10 10 00 01 00 }
0x58E73: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58E7A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58E81: 			End  { 29 02 }
0x58E83: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xD86, VarStoreId: 0x6, VarOffset: 0x298, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 54 13 5F 13 86 0D 06 00 98 02 10 10 00 04 00 }
0x58E94: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x58E9B: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x58EA2: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x58EA9: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x58EB0: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x58EB7: 			End  { 29 02 }
0x58EB9: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD87, VarStoreId: 0x6, VarOffset: 0x2B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D7 14 E2 14 87 0D 06 00 B4 02 10 10 00 01 00 }
0x58ECA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x58ED1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x58ED8: 			End  { 29 02 }
0x58EDA: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xD88, VarStoreId: 0x6, VarOffset: 0x3A5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F4 14 FF 14 88 0D 06 00 A5 03 00 11 00 00 FF FF 01 00 }
0x58EEE: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x58EF5: 			End  { 29 02 }
0x58EF7: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD89, VarStoreId: 0x6, VarOffset: 0x530, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 11 15 1C 15 89 0D 06 00 30 05 00 10 00 07 01 }
0x58F08: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x58F0E: 			End  { 29 02 }
0x58F10: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xD8A, VarStoreId: 0x6, VarOffset: 0x55D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 2E 15 39 15 8A 0D 06 00 5D 05 00 11 01 00 14 00 01 00 }
0x58F24: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x58F2B: 			End  { 29 02 }
0x58F2D: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xD8B, VarStoreId: 0x6, VarOffset: 0x584, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 4B 15 56 15 8B 0D 06 00 84 05 00 10 04 14 04 }
0x58F3E: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x58F44: 			End  { 29 02 }
0x58F46: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x58F4D: 			End  { 29 02 }
0x58F4F: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x58F56: 			End  { 29 02 }
0x58F58: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD8C, VarStoreId: 0x6, VarOffset: 0x3F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 6F 15 7A 15 8C 0D 06 00 F4 03 10 10 00 01 00 }
0x58F69: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58F70: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x58F77: 			End  { 29 02 }
0x58F79: 			SuppressIf  { 0A 82 }
0x58F7B: 				EqIdVal QuestionId: 0xD8C, Value: 0x0 { 12 06 8C 0D 00 00 }
0x58F81: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD8D, VarStoreId: 0x6, VarOffset: 0x42C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E1 15 23 16 8D 0D 06 00 2C 04 10 10 00 02 00 }
0x58F92: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x58F99: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x58FA0: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x58FA7: 				End  { 29 02 }
0x58FA9: 				SuppressIf  { 0A 82 }
0x58FAB: 					EqIdVal QuestionId: 0xD8D, Value: 0x1 { 12 86 8D 0D 01 00 }
0x58FB1: 						Not  { 17 02 }
0x58FB3: 					End  { 29 02 }
0x58FB5: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD8E, VarStoreId: 0x6, VarOffset: 0x4AD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 E3 15 25 16 8E 0D 06 00 AD 04 10 11 00 00 FF 03 01 00 }
0x58FC9: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x58FD0: 					End  { 29 02 }
0x58FD2: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD8F, VarStoreId: 0x6, VarOffset: 0x448, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 E4 15 26 16 8F 0D 06 00 48 04 10 10 00 05 00 }
0x58FE3: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x58FEA: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x58FF1: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x58FF8: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x58FFF: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59006: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5900D: 					End  { 29 02 }
0x5900F: 				End  { 29 02 }
0x59011: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xD90, VarStoreId: 0x6, VarOffset: 0x464, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E2 15 24 16 90 0D 06 00 64 04 10 10 00 02 00 }
0x59022: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59029: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x59030: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x59037: 				End  { 29 02 }
0x59039: 				SuppressIf  { 0A 82 }
0x5903B: 					EqIdVal QuestionId: 0xD90, Value: 0x1 { 12 86 90 0D 01 00 }
0x59041: 						Not  { 17 02 }
0x59043: 					End  { 29 02 }
0x59045: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD91, VarStoreId: 0x6, VarOffset: 0x4E5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 E5 15 27 16 91 0D 06 00 E5 04 10 11 00 00 FF 03 01 00 }
0x59059: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x59060: 					End  { 29 02 }
0x59062: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xD92, VarStoreId: 0x6, VarOffset: 0x480, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 E6 15 28 16 92 0D 06 00 80 04 10 10 00 05 00 }
0x59073: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5907A: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59081: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x59088: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5908F: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59096: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5909D: 					End  { 29 02 }
0x5909F: 				End  { 29 02 }
0x590A1: 			End  { 29 02 }
0x590A3: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x590AA: 			End  { 29 02 }
0x590AC: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xD93, VarStoreId: 0x6, VarOffset: 0x410, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 16 45 16 93 0D 06 00 10 04 10 10 00 01 00 }
0x590BD: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x590C4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x590CB: 			End  { 29 02 }
0x590CD: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xD94, VarStoreId: 0x6, VarOffset: 0xCF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 14 C3 14 94 0D 06 00 CF 00 10 10 00 01 00 }
0x590DE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x590E5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x590EC: 			End  { 29 02 }
0x590EE: 		End  { 29 02 }
0x590F0: 	End  { 29 02 }
0x590F2: 	Form FormId: 0x2842, Title: "PCI Express Root Port 19" { 01 86 42 28 88 16 }
0x590F8: 		OneOf Prompt: "PCI Express Root Port 19", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xD95, VarStoreId: 0x6, VarOffset: 0x111, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 13 7C 13 95 0D 06 00 11 01 10 10 00 01 00 }
0x59109: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59110: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59117: 		End  { 29 02 }
0x59119: 		SuppressIf  { 0A 82 }
0x5911B: 			EqIdVal QuestionId: 0xD95, Value: 0x0 { 12 06 95 0D 00 00 }
0x59121: 			GrayOutIf  { 19 82 }
0x59123: 				EqIdVal QuestionId: 0xDA3, Value: 0x1 { 12 06 A3 0D 01 00 }
0x59129: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xD96, VarStoreId: 0x6, VarOffset: 0x379, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 32 17 E5 0E 96 0D 06 00 79 03 10 10 00 01 00 }
0x5913A: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x59141: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x59148: 				End  { 29 02 }
0x5914A: 			End  { 29 02 }
0x5914C: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2809, VarStoreId: 0x6, VarOffset: 0x12D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 88 12 F5 0D 09 28 06 00 2D 01 10 10 00 04 00 }
0x5915D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59164: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5916B: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x59172: 			End  { 29 02 }
0x59174: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x280A, VarStoreId: 0x6, VarOffset: 0x2D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A4 12 AE 12 0A 28 06 00 D1 02 10 10 00 02 00 }
0x59185: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5918C: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x59193: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5919A: 			End  { 29 02 }
0x5919C: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD97, VarStoreId: 0x6, VarOffset: 0x2ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C3 12 CD 12 97 0D 06 00 ED 02 10 10 00 01 00 }
0x591AD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x591B4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x591BB: 			End  { 29 02 }
0x591BD: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xD98, VarStoreId: 0x6, VarOffset: 0x309, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 12 A7 0E 98 0D 06 00 09 03 10 10 00 01 00 }
0x591CE: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x591D5: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x591DC: 			End  { 29 02 }
0x591DE: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x280B, VarStoreId: 0x6, VarOffset: 0x325, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FC 12 06 13 0B 28 06 00 25 03 10 10 00 01 00 }
0x591EF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x591F6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x591FD: 			End  { 29 02 }
0x591FF: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD99, VarStoreId: 0x6, VarOffset: 0x341, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 19 13 23 13 99 0D 06 00 41 03 10 10 00 01 00 }
0x59210: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59217: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5921E: 			End  { 29 02 }
0x59220: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xD9A, VarStoreId: 0x6, VarOffset: 0x35D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 36 13 40 13 9A 0D 06 00 5D 03 10 10 00 01 00 }
0x59231: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59238: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5923F: 			End  { 29 02 }
0x59241: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD9B, VarStoreId: 0x6, VarOffset: 0x149, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 13 99 13 9B 0D 06 00 49 01 10 10 00 01 00 }
0x59252: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59259: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59260: 			End  { 29 02 }
0x59262: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD9C, VarStoreId: 0x6, VarOffset: 0x165, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 13 B6 13 9C 0D 06 00 65 01 10 10 00 01 00 }
0x59273: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5927A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59281: 			End  { 29 02 }
0x59283: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD9D, VarStoreId: 0x6, VarOffset: 0x181, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C9 13 D3 13 9D 0D 06 00 81 01 10 10 00 01 00 }
0x59294: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5929B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x592A2: 			End  { 29 02 }
0x592A4: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD9E, VarStoreId: 0x6, VarOffset: 0x19D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E6 13 F0 13 9E 0D 06 00 9D 01 10 10 00 01 00 }
0x592B5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x592BC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x592C3: 			End  { 29 02 }
0x592C5: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xD9F, VarStoreId: 0x6, VarOffset: 0x1F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 07 14 11 14 9F 0D 06 00 F1 01 10 10 00 01 00 }
0x592D6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x592DD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x592E4: 			End  { 29 02 }
0x592E6: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDA0, VarStoreId: 0x6, VarOffset: 0x20D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 24 14 2E 14 A0 0D 06 00 0D 02 10 10 00 01 00 }
0x592F7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x592FE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59305: 			End  { 29 02 }
0x59307: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDA1, VarStoreId: 0x6, VarOffset: 0x229, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 41 14 4B 14 A1 0D 06 00 29 02 10 10 00 01 00 }
0x59318: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5931F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59326: 			End  { 29 02 }
0x59328: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDA2, VarStoreId: 0x6, VarOffset: 0x245, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5E 14 68 14 A2 0D 06 00 45 02 10 10 00 01 00 }
0x59339: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59340: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59347: 			End  { 29 02 }
0x59349: 			GrayOutIf  { 19 82 }
0x5934B: 				EqIdVal QuestionId: 0xD96, Value: 0x0 { 12 06 96 0D 00 00 }
0x59351: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDA3, VarStoreId: 0x6, VarOffset: 0x261, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7B 14 85 14 A3 0D 06 00 61 02 10 10 00 01 00 }
0x59362: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59369: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59370: 				End  { 29 02 }
0x59372: 			End  { 29 02 }
0x59374: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDA4, VarStoreId: 0x6, VarOffset: 0x27D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 98 14 A2 14 A4 0D 06 00 7D 02 10 10 00 01 00 }
0x59385: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5938C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59393: 			End  { 29 02 }
0x59395: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xDA5, VarStoreId: 0x6, VarOffset: 0x299, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 55 13 5F 13 A5 0D 06 00 99 02 10 10 00 04 00 }
0x593A6: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x593AD: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x593B4: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x593BB: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x593C2: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x593C9: 			End  { 29 02 }
0x593CB: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDA6, VarStoreId: 0x6, VarOffset: 0x2B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D8 14 E2 14 A6 0D 06 00 B5 02 10 10 00 01 00 }
0x593DC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x593E3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x593EA: 			End  { 29 02 }
0x593EC: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xDA7, VarStoreId: 0x6, VarOffset: 0x3A7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F5 14 FF 14 A7 0D 06 00 A7 03 00 11 00 00 FF FF 01 00 }
0x59400: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x59407: 			End  { 29 02 }
0x59409: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xDA8, VarStoreId: 0x6, VarOffset: 0x531, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 12 15 1C 15 A8 0D 06 00 31 05 00 10 00 07 01 }
0x5941A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x59420: 			End  { 29 02 }
0x59422: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xDA9, VarStoreId: 0x6, VarOffset: 0x55F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 2F 15 39 15 A9 0D 06 00 5F 05 00 11 01 00 14 00 01 00 }
0x59436: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5943D: 			End  { 29 02 }
0x5943F: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xDAA, VarStoreId: 0x6, VarOffset: 0x585, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 4C 15 56 15 AA 0D 06 00 85 05 00 10 04 14 04 }
0x59450: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x59456: 			End  { 29 02 }
0x59458: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5945F: 			End  { 29 02 }
0x59461: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x59468: 			End  { 29 02 }
0x5946A: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xDAB, VarStoreId: 0x6, VarOffset: 0x3F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 70 15 7A 15 AB 0D 06 00 F5 03 10 10 00 01 00 }
0x5947B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59482: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59489: 			End  { 29 02 }
0x5948B: 			SuppressIf  { 0A 82 }
0x5948D: 				EqIdVal QuestionId: 0xDAB, Value: 0x0 { 12 06 AB 0D 00 00 }
0x59493: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xDAC, VarStoreId: 0x6, VarOffset: 0x42D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E7 15 23 16 AC 0D 06 00 2D 04 10 10 00 02 00 }
0x594A4: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x594AB: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x594B2: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x594B9: 				End  { 29 02 }
0x594BB: 				SuppressIf  { 0A 82 }
0x594BD: 					EqIdVal QuestionId: 0xDAC, Value: 0x1 { 12 86 AC 0D 01 00 }
0x594C3: 						Not  { 17 02 }
0x594C5: 					End  { 29 02 }
0x594C7: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDAD, VarStoreId: 0x6, VarOffset: 0x4AF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 E9 15 25 16 AD 0D 06 00 AF 04 10 11 00 00 FF 03 01 00 }
0x594DB: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x594E2: 					End  { 29 02 }
0x594E4: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDAE, VarStoreId: 0x6, VarOffset: 0x449, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 EA 15 26 16 AE 0D 06 00 49 04 10 10 00 05 00 }
0x594F5: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x594FC: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59503: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5950A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x59511: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59518: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5951F: 					End  { 29 02 }
0x59521: 				End  { 29 02 }
0x59523: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xDAF, VarStoreId: 0x6, VarOffset: 0x465, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E8 15 24 16 AF 0D 06 00 65 04 10 10 00 02 00 }
0x59534: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5953B: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x59542: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x59549: 				End  { 29 02 }
0x5954B: 				SuppressIf  { 0A 82 }
0x5954D: 					EqIdVal QuestionId: 0xDAF, Value: 0x1 { 12 86 AF 0D 01 00 }
0x59553: 						Not  { 17 02 }
0x59555: 					End  { 29 02 }
0x59557: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDB0, VarStoreId: 0x6, VarOffset: 0x4E7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 EB 15 27 16 B0 0D 06 00 E7 04 10 11 00 00 FF 03 01 00 }
0x5956B: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x59572: 					End  { 29 02 }
0x59574: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDB1, VarStoreId: 0x6, VarOffset: 0x481, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 EC 15 28 16 B1 0D 06 00 81 04 10 10 00 05 00 }
0x59585: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5958C: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59593: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5959A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x595A1: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x595A8: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x595AF: 					End  { 29 02 }
0x595B1: 				End  { 29 02 }
0x595B3: 			End  { 29 02 }
0x595B5: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x595BC: 			End  { 29 02 }
0x595BE: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xDB2, VarStoreId: 0x6, VarOffset: 0x411, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3B 16 45 16 B2 0D 06 00 11 04 10 10 00 01 00 }
0x595CF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x595D6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x595DD: 			End  { 29 02 }
0x595DF: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xDB3, VarStoreId: 0x6, VarOffset: 0xD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 14 C3 14 B3 0D 06 00 D0 00 10 10 00 01 00 }
0x595F0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x595F7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x595FE: 			End  { 29 02 }
0x59600: 		End  { 29 02 }
0x59602: 	End  { 29 02 }
0x59604: 	Form FormId: 0x2843, Title: "PCI Express Root Port 20" { 01 86 43 28 89 16 }
0x5960A: 		OneOf Prompt: "PCI Express Root Port 20", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xDB4, VarStoreId: 0x6, VarOffset: 0x112, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 73 13 7C 13 B4 0D 06 00 12 01 10 10 00 01 00 }
0x5961B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59622: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59629: 		End  { 29 02 }
0x5962B: 		SuppressIf  { 0A 82 }
0x5962D: 			EqIdVal QuestionId: 0xDB4, Value: 0x0 { 12 06 B4 0D 00 00 }
0x59633: 			GrayOutIf  { 19 82 }
0x59635: 				EqIdVal QuestionId: 0xDC2, Value: 0x1 { 12 06 C2 0D 01 00 }
0x5963B: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xDB5, VarStoreId: 0x6, VarOffset: 0x37A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 33 17 E5 0E B5 0D 06 00 7A 03 10 10 00 01 00 }
0x5964C: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x59653: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5965A: 				End  { 29 02 }
0x5965C: 			End  { 29 02 }
0x5965E: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x280C, VarStoreId: 0x6, VarOffset: 0x12E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 89 12 F5 0D 0C 28 06 00 2E 01 10 10 00 04 00 }
0x5966F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59676: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5967D: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x59684: 			End  { 29 02 }
0x59686: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x280D, VarStoreId: 0x6, VarOffset: 0x2D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A5 12 AE 12 0D 28 06 00 D2 02 10 10 00 02 00 }
0x59697: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5969E: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x596A5: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x596AC: 			End  { 29 02 }
0x596AE: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDB6, VarStoreId: 0x6, VarOffset: 0x2EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 12 CD 12 B6 0D 06 00 EE 02 10 10 00 01 00 }
0x596BF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x596C6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x596CD: 			End  { 29 02 }
0x596CF: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xDB7, VarStoreId: 0x6, VarOffset: 0x30A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 12 A7 0E B7 0D 06 00 0A 03 10 10 00 01 00 }
0x596E0: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x596E7: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x596EE: 			End  { 29 02 }
0x596F0: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x280E, VarStoreId: 0x6, VarOffset: 0x326, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FD 12 06 13 0E 28 06 00 26 03 10 10 00 01 00 }
0x59701: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59708: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5970F: 			End  { 29 02 }
0x59711: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xDB8, VarStoreId: 0x6, VarOffset: 0x342, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1A 13 23 13 B8 0D 06 00 42 03 10 10 00 01 00 }
0x59722: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59729: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59730: 			End  { 29 02 }
0x59732: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xDB9, VarStoreId: 0x6, VarOffset: 0x35E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 37 13 40 13 B9 0D 06 00 5E 03 10 10 00 01 00 }
0x59743: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5974A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59751: 			End  { 29 02 }
0x59753: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDBA, VarStoreId: 0x6, VarOffset: 0x14A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 13 99 13 BA 0D 06 00 4A 01 10 10 00 01 00 }
0x59764: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5976B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59772: 			End  { 29 02 }
0x59774: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDBB, VarStoreId: 0x6, VarOffset: 0x166, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AD 13 B6 13 BB 0D 06 00 66 01 10 10 00 01 00 }
0x59785: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5978C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59793: 			End  { 29 02 }
0x59795: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDBC, VarStoreId: 0x6, VarOffset: 0x182, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 13 D3 13 BC 0D 06 00 82 01 10 10 00 01 00 }
0x597A6: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x597AD: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x597B4: 			End  { 29 02 }
0x597B6: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDBD, VarStoreId: 0x6, VarOffset: 0x19E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E7 13 F0 13 BD 0D 06 00 9E 01 10 10 00 01 00 }
0x597C7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x597CE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x597D5: 			End  { 29 02 }
0x597D7: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDBE, VarStoreId: 0x6, VarOffset: 0x1F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 14 11 14 BE 0D 06 00 F2 01 10 10 00 01 00 }
0x597E8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x597EF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x597F6: 			End  { 29 02 }
0x597F8: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDBF, VarStoreId: 0x6, VarOffset: 0x20E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 25 14 2E 14 BF 0D 06 00 0E 02 10 10 00 01 00 }
0x59809: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59810: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59817: 			End  { 29 02 }
0x59819: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDC0, VarStoreId: 0x6, VarOffset: 0x22A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 14 4B 14 C0 0D 06 00 2A 02 10 10 00 01 00 }
0x5982A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59831: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59838: 			End  { 29 02 }
0x5983A: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDC1, VarStoreId: 0x6, VarOffset: 0x246, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5F 14 68 14 C1 0D 06 00 46 02 10 10 00 01 00 }
0x5984B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59852: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59859: 			End  { 29 02 }
0x5985B: 			GrayOutIf  { 19 82 }
0x5985D: 				EqIdVal QuestionId: 0xDB5, Value: 0x0 { 12 06 B5 0D 00 00 }
0x59863: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDC2, VarStoreId: 0x6, VarOffset: 0x262, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7C 14 85 14 C2 0D 06 00 62 02 10 10 00 01 00 }
0x59874: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5987B: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59882: 				End  { 29 02 }
0x59884: 			End  { 29 02 }
0x59886: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDC3, VarStoreId: 0x6, VarOffset: 0x27E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 99 14 A2 14 C3 0D 06 00 7E 02 10 10 00 01 00 }
0x59897: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5989E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x598A5: 			End  { 29 02 }
0x598A7: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xDC4, VarStoreId: 0x6, VarOffset: 0x29A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 56 13 5F 13 C4 0D 06 00 9A 02 10 10 00 04 00 }
0x598B8: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x598BF: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x598C6: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x598CD: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x598D4: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x598DB: 			End  { 29 02 }
0x598DD: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDC5, VarStoreId: 0x6, VarOffset: 0x2B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D9 14 E2 14 C5 0D 06 00 B6 02 10 10 00 01 00 }
0x598EE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x598F5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x598FC: 			End  { 29 02 }
0x598FE: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xDC6, VarStoreId: 0x6, VarOffset: 0x3A9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F6 14 FF 14 C6 0D 06 00 A9 03 00 11 00 00 FF FF 01 00 }
0x59912: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x59919: 			End  { 29 02 }
0x5991B: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xDC7, VarStoreId: 0x6, VarOffset: 0x532, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 13 15 1C 15 C7 0D 06 00 32 05 00 10 00 07 01 }
0x5992C: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x59932: 			End  { 29 02 }
0x59934: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xDC8, VarStoreId: 0x6, VarOffset: 0x561, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 30 15 39 15 C8 0D 06 00 61 05 00 11 01 00 14 00 01 00 }
0x59948: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5994F: 			End  { 29 02 }
0x59951: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xDC9, VarStoreId: 0x6, VarOffset: 0x586, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 4D 15 56 15 C9 0D 06 00 86 05 00 10 04 14 04 }
0x59962: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x59968: 			End  { 29 02 }
0x5996A: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x59971: 			End  { 29 02 }
0x59973: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5997A: 			End  { 29 02 }
0x5997C: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xDCA, VarStoreId: 0x6, VarOffset: 0x3F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 71 15 7A 15 CA 0D 06 00 F6 03 10 10 00 01 00 }
0x5998D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59994: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5999B: 			End  { 29 02 }
0x5999D: 			SuppressIf  { 0A 82 }
0x5999F: 				EqIdVal QuestionId: 0xDCA, Value: 0x0 { 12 06 CA 0D 00 00 }
0x599A5: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xDCB, VarStoreId: 0x6, VarOffset: 0x42E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 ED 15 23 16 CB 0D 06 00 2E 04 10 10 00 02 00 }
0x599B6: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x599BD: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x599C4: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x599CB: 				End  { 29 02 }
0x599CD: 				SuppressIf  { 0A 82 }
0x599CF: 					EqIdVal QuestionId: 0xDCB, Value: 0x1 { 12 86 CB 0D 01 00 }
0x599D5: 						Not  { 17 02 }
0x599D7: 					End  { 29 02 }
0x599D9: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDCC, VarStoreId: 0x6, VarOffset: 0x4B1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 EF 15 25 16 CC 0D 06 00 B1 04 10 11 00 00 FF 03 01 00 }
0x599ED: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x599F4: 					End  { 29 02 }
0x599F6: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDCD, VarStoreId: 0x6, VarOffset: 0x44A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 F0 15 26 16 CD 0D 06 00 4A 04 10 10 00 05 00 }
0x59A07: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x59A0E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59A15: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x59A1C: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x59A23: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59A2A: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x59A31: 					End  { 29 02 }
0x59A33: 				End  { 29 02 }
0x59A35: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xDCE, VarStoreId: 0x6, VarOffset: 0x466, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 EE 15 24 16 CE 0D 06 00 66 04 10 10 00 02 00 }
0x59A46: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59A4D: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x59A54: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x59A5B: 				End  { 29 02 }
0x59A5D: 				SuppressIf  { 0A 82 }
0x59A5F: 					EqIdVal QuestionId: 0xDCE, Value: 0x1 { 12 86 CE 0D 01 00 }
0x59A65: 						Not  { 17 02 }
0x59A67: 					End  { 29 02 }
0x59A69: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDCF, VarStoreId: 0x6, VarOffset: 0x4E9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 F1 15 27 16 CF 0D 06 00 E9 04 10 11 00 00 FF 03 01 00 }
0x59A7D: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x59A84: 					End  { 29 02 }
0x59A86: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDD0, VarStoreId: 0x6, VarOffset: 0x482, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 F2 15 28 16 D0 0D 06 00 82 04 10 10 00 05 00 }
0x59A97: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x59A9E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59AA5: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x59AAC: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x59AB3: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59ABA: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x59AC1: 					End  { 29 02 }
0x59AC3: 				End  { 29 02 }
0x59AC5: 			End  { 29 02 }
0x59AC7: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x59ACE: 			End  { 29 02 }
0x59AD0: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xDD1, VarStoreId: 0x6, VarOffset: 0x412, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 16 45 16 D1 0D 06 00 12 04 10 10 00 01 00 }
0x59AE1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59AE8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59AEF: 			End  { 29 02 }
0x59AF1: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xDD2, VarStoreId: 0x6, VarOffset: 0xD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 14 C3 14 D2 0D 06 00 D1 00 10 10 00 01 00 }
0x59B02: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59B09: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59B10: 			End  { 29 02 }
0x59B12: 		End  { 29 02 }
0x59B14: 	End  { 29 02 }
0x59B16: 	Form FormId: 0x2844, Title: "PCI Express Root Port 21" { 01 86 44 28 8A 16 }
0x59B1C: 		OneOf Prompt: "PCI Express Root Port 21", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xDD3, VarStoreId: 0x6, VarOffset: 0x113, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 13 7C 13 D3 0D 06 00 13 01 10 10 00 01 00 }
0x59B2D: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59B34: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59B3B: 		End  { 29 02 }
0x59B3D: 		SuppressIf  { 0A 82 }
0x59B3F: 			EqIdVal QuestionId: 0xDD3, Value: 0x0 { 12 06 D3 0D 00 00 }
0x59B45: 			GrayOutIf  { 19 82 }
0x59B47: 				EqIdVal QuestionId: 0xDE1, Value: 0x1 { 12 06 E1 0D 01 00 }
0x59B4D: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xDD4, VarStoreId: 0x6, VarOffset: 0x37B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 34 17 E5 0E D4 0D 06 00 7B 03 10 10 00 01 00 }
0x59B5E: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x59B65: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x59B6C: 				End  { 29 02 }
0x59B6E: 			End  { 29 02 }
0x59B70: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x280F, VarStoreId: 0x6, VarOffset: 0x12F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8A 12 F5 0D 0F 28 06 00 2F 01 10 10 00 04 00 }
0x59B81: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59B88: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x59B8F: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x59B96: 			End  { 29 02 }
0x59B98: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2810, VarStoreId: 0x6, VarOffset: 0x2D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A6 12 AE 12 10 28 06 00 D3 02 10 10 00 02 00 }
0x59BA9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59BB0: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x59BB7: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x59BBE: 			End  { 29 02 }
0x59BC0: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDD5, VarStoreId: 0x6, VarOffset: 0x2EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 12 CD 12 D5 0D 06 00 EF 02 10 10 00 01 00 }
0x59BD1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59BD8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59BDF: 			End  { 29 02 }
0x59BE1: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xDD6, VarStoreId: 0x6, VarOffset: 0x30B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E2 12 A7 0E D6 0D 06 00 0B 03 10 10 00 01 00 }
0x59BF2: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59BF9: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59C00: 			End  { 29 02 }
0x59C02: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2811, VarStoreId: 0x6, VarOffset: 0x327, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FE 12 06 13 11 28 06 00 27 03 10 10 00 01 00 }
0x59C13: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59C1A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59C21: 			End  { 29 02 }
0x59C23: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xDD7, VarStoreId: 0x6, VarOffset: 0x343, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1B 13 23 13 D7 0D 06 00 43 03 10 10 00 01 00 }
0x59C34: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59C3B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59C42: 			End  { 29 02 }
0x59C44: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xDD8, VarStoreId: 0x6, VarOffset: 0x35F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 13 40 13 D8 0D 06 00 5F 03 10 10 00 01 00 }
0x59C55: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59C5C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59C63: 			End  { 29 02 }
0x59C65: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDD9, VarStoreId: 0x6, VarOffset: 0x14B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 13 99 13 D9 0D 06 00 4B 01 10 10 00 01 00 }
0x59C76: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59C7D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59C84: 			End  { 29 02 }
0x59C86: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDDA, VarStoreId: 0x6, VarOffset: 0x167, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 13 B6 13 DA 0D 06 00 67 01 10 10 00 01 00 }
0x59C97: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59C9E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59CA5: 			End  { 29 02 }
0x59CA7: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDDB, VarStoreId: 0x6, VarOffset: 0x183, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CB 13 D3 13 DB 0D 06 00 83 01 10 10 00 01 00 }
0x59CB8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59CBF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59CC6: 			End  { 29 02 }
0x59CC8: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDDC, VarStoreId: 0x6, VarOffset: 0x19F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 13 F0 13 DC 0D 06 00 9F 01 10 10 00 01 00 }
0x59CD9: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59CE0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59CE7: 			End  { 29 02 }
0x59CE9: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDDD, VarStoreId: 0x6, VarOffset: 0x1F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 09 14 11 14 DD 0D 06 00 F3 01 10 10 00 01 00 }
0x59CFA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59D01: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59D08: 			End  { 29 02 }
0x59D0A: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDDE, VarStoreId: 0x6, VarOffset: 0x20F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 14 2E 14 DE 0D 06 00 0F 02 10 10 00 01 00 }
0x59D1B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59D22: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59D29: 			End  { 29 02 }
0x59D2B: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDDF, VarStoreId: 0x6, VarOffset: 0x22B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 43 14 4B 14 DF 0D 06 00 2B 02 10 10 00 01 00 }
0x59D3C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59D43: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59D4A: 			End  { 29 02 }
0x59D4C: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDE0, VarStoreId: 0x6, VarOffset: 0x247, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 60 14 68 14 E0 0D 06 00 47 02 10 10 00 01 00 }
0x59D5D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59D64: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59D6B: 			End  { 29 02 }
0x59D6D: 			GrayOutIf  { 19 82 }
0x59D6F: 				EqIdVal QuestionId: 0xDD4, Value: 0x0 { 12 06 D4 0D 00 00 }
0x59D75: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDE1, VarStoreId: 0x6, VarOffset: 0x263, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7D 14 85 14 E1 0D 06 00 63 02 10 10 00 01 00 }
0x59D86: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59D8D: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59D94: 				End  { 29 02 }
0x59D96: 			End  { 29 02 }
0x59D98: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDE2, VarStoreId: 0x6, VarOffset: 0x27F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9A 14 A2 14 E2 0D 06 00 7F 02 10 10 00 01 00 }
0x59DA9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59DB0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59DB7: 			End  { 29 02 }
0x59DB9: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xDE3, VarStoreId: 0x6, VarOffset: 0x29B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 57 13 5F 13 E3 0D 06 00 9B 02 10 10 00 04 00 }
0x59DCA: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x59DD1: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x59DD8: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x59DDF: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x59DE6: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x59DED: 			End  { 29 02 }
0x59DEF: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDE4, VarStoreId: 0x6, VarOffset: 0x2B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DA 14 E2 14 E4 0D 06 00 B7 02 10 10 00 01 00 }
0x59E00: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59E07: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x59E0E: 			End  { 29 02 }
0x59E10: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xDE5, VarStoreId: 0x6, VarOffset: 0x3AB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F7 14 FF 14 E5 0D 06 00 AB 03 00 11 00 00 FF FF 01 00 }
0x59E24: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x59E2B: 			End  { 29 02 }
0x59E2D: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xDE6, VarStoreId: 0x6, VarOffset: 0x533, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 14 15 1C 15 E6 0D 06 00 33 05 00 10 00 07 01 }
0x59E3E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x59E44: 			End  { 29 02 }
0x59E46: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xDE7, VarStoreId: 0x6, VarOffset: 0x563, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 31 15 39 15 E7 0D 06 00 63 05 00 11 01 00 14 00 01 00 }
0x59E5A: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x59E61: 			End  { 29 02 }
0x59E63: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xDE8, VarStoreId: 0x6, VarOffset: 0x587, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 4E 15 56 15 E8 0D 06 00 87 05 00 10 04 14 04 }
0x59E74: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x59E7A: 			End  { 29 02 }
0x59E7C: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x59E83: 			End  { 29 02 }
0x59E85: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x59E8C: 			End  { 29 02 }
0x59E8E: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xDE9, VarStoreId: 0x6, VarOffset: 0x3F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 72 15 7A 15 E9 0D 06 00 F7 03 10 10 00 01 00 }
0x59E9F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59EA6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x59EAD: 			End  { 29 02 }
0x59EAF: 			SuppressIf  { 0A 82 }
0x59EB1: 				EqIdVal QuestionId: 0xDE9, Value: 0x0 { 12 06 E9 0D 00 00 }
0x59EB7: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xDEA, VarStoreId: 0x6, VarOffset: 0x42F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 F3 15 23 16 EA 0D 06 00 2F 04 10 10 00 02 00 }
0x59EC8: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59ECF: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x59ED6: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x59EDD: 				End  { 29 02 }
0x59EDF: 				SuppressIf  { 0A 82 }
0x59EE1: 					EqIdVal QuestionId: 0xDEA, Value: 0x1 { 12 86 EA 0D 01 00 }
0x59EE7: 						Not  { 17 02 }
0x59EE9: 					End  { 29 02 }
0x59EEB: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDEB, VarStoreId: 0x6, VarOffset: 0x4B3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 F5 15 25 16 EB 0D 06 00 B3 04 10 11 00 00 FF 03 01 00 }
0x59EFF: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x59F06: 					End  { 29 02 }
0x59F08: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDEC, VarStoreId: 0x6, VarOffset: 0x44B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 F6 15 26 16 EC 0D 06 00 4B 04 10 10 00 05 00 }
0x59F19: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x59F20: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59F27: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x59F2E: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x59F35: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59F3C: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x59F43: 					End  { 29 02 }
0x59F45: 				End  { 29 02 }
0x59F47: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xDED, VarStoreId: 0x6, VarOffset: 0x467, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 F4 15 24 16 ED 0D 06 00 67 04 10 10 00 02 00 }
0x59F58: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x59F5F: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x59F66: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x59F6D: 				End  { 29 02 }
0x59F6F: 				SuppressIf  { 0A 82 }
0x59F71: 					EqIdVal QuestionId: 0xDED, Value: 0x1 { 12 86 ED 0D 01 00 }
0x59F77: 						Not  { 17 02 }
0x59F79: 					End  { 29 02 }
0x59F7B: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDEE, VarStoreId: 0x6, VarOffset: 0x4EB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 F7 15 27 16 EE 0D 06 00 EB 04 10 11 00 00 FF 03 01 00 }
0x59F8F: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x59F96: 					End  { 29 02 }
0x59F98: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xDEF, VarStoreId: 0x6, VarOffset: 0x483, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 F8 15 28 16 EF 0D 06 00 83 04 10 10 00 05 00 }
0x59FA9: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x59FB0: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x59FB7: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x59FBE: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x59FC5: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x59FCC: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x59FD3: 					End  { 29 02 }
0x59FD5: 				End  { 29 02 }
0x59FD7: 			End  { 29 02 }
0x59FD9: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x59FE0: 			End  { 29 02 }
0x59FE2: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xDF0, VarStoreId: 0x6, VarOffset: 0x413, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 16 45 16 F0 0D 06 00 13 04 10 10 00 01 00 }
0x59FF3: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x59FFA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A001: 			End  { 29 02 }
0x5A003: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xDF1, VarStoreId: 0x6, VarOffset: 0xD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 14 C3 14 F1 0D 06 00 D2 00 10 10 00 01 00 }
0x5A014: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A01B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A022: 			End  { 29 02 }
0x5A024: 		End  { 29 02 }
0x5A026: 	End  { 29 02 }
0x5A028: 	Form FormId: 0x2845, Title: "PCI Express Root Port 22" { 01 86 45 28 8B 16 }
0x5A02E: 		OneOf Prompt: "PCI Express Root Port 22", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xDF2, VarStoreId: 0x6, VarOffset: 0x114, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 75 13 7C 13 F2 0D 06 00 14 01 10 10 00 01 00 }
0x5A03F: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A046: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A04D: 		End  { 29 02 }
0x5A04F: 		SuppressIf  { 0A 82 }
0x5A051: 			EqIdVal QuestionId: 0xDF2, Value: 0x0 { 12 06 F2 0D 00 00 }
0x5A057: 			GrayOutIf  { 19 82 }
0x5A059: 				EqIdVal QuestionId: 0xE00, Value: 0x1 { 12 06 00 0E 01 00 }
0x5A05F: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xDF3, VarStoreId: 0x6, VarOffset: 0x37C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 35 17 E5 0E F3 0D 06 00 7C 03 10 10 00 01 00 }
0x5A070: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5A077: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5A07E: 				End  { 29 02 }
0x5A080: 			End  { 29 02 }
0x5A082: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2812, VarStoreId: 0x6, VarOffset: 0x130, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8B 12 F5 0D 12 28 06 00 30 01 10 10 00 04 00 }
0x5A093: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A09A: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5A0A1: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5A0A8: 			End  { 29 02 }
0x5A0AA: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2813, VarStoreId: 0x6, VarOffset: 0x2D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A7 12 AE 12 13 28 06 00 D4 02 10 10 00 02 00 }
0x5A0BB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A0C2: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5A0C9: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5A0D0: 			End  { 29 02 }
0x5A0D2: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDF4, VarStoreId: 0x6, VarOffset: 0x2F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 12 CD 12 F4 0D 06 00 F0 02 10 10 00 01 00 }
0x5A0E3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A0EA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A0F1: 			End  { 29 02 }
0x5A0F3: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xDF5, VarStoreId: 0x6, VarOffset: 0x30C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E3 12 A7 0E F5 0D 06 00 0C 03 10 10 00 01 00 }
0x5A104: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A10B: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A112: 			End  { 29 02 }
0x5A114: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2814, VarStoreId: 0x6, VarOffset: 0x328, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FF 12 06 13 14 28 06 00 28 03 10 10 00 01 00 }
0x5A125: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A12C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A133: 			End  { 29 02 }
0x5A135: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xDF6, VarStoreId: 0x6, VarOffset: 0x344, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1C 13 23 13 F6 0D 06 00 44 03 10 10 00 01 00 }
0x5A146: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A14D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A154: 			End  { 29 02 }
0x5A156: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xDF7, VarStoreId: 0x6, VarOffset: 0x360, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 13 40 13 F7 0D 06 00 60 03 10 10 00 01 00 }
0x5A167: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A16E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A175: 			End  { 29 02 }
0x5A177: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDF8, VarStoreId: 0x6, VarOffset: 0x14C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 13 99 13 F8 0D 06 00 4C 01 10 10 00 01 00 }
0x5A188: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A18F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A196: 			End  { 29 02 }
0x5A198: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDF9, VarStoreId: 0x6, VarOffset: 0x168, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AF 13 B6 13 F9 0D 06 00 68 01 10 10 00 01 00 }
0x5A1A9: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A1B0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A1B7: 			End  { 29 02 }
0x5A1B9: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDFA, VarStoreId: 0x6, VarOffset: 0x184, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CC 13 D3 13 FA 0D 06 00 84 01 10 10 00 01 00 }
0x5A1CA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A1D1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A1D8: 			End  { 29 02 }
0x5A1DA: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDFB, VarStoreId: 0x6, VarOffset: 0x1A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 13 F0 13 FB 0D 06 00 A0 01 10 10 00 01 00 }
0x5A1EB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A1F2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A1F9: 			End  { 29 02 }
0x5A1FB: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDFC, VarStoreId: 0x6, VarOffset: 0x1F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0A 14 11 14 FC 0D 06 00 F4 01 10 10 00 01 00 }
0x5A20C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A213: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A21A: 			End  { 29 02 }
0x5A21C: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDFD, VarStoreId: 0x6, VarOffset: 0x210, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 27 14 2E 14 FD 0D 06 00 10 02 10 10 00 01 00 }
0x5A22D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A234: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A23B: 			End  { 29 02 }
0x5A23D: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDFE, VarStoreId: 0x6, VarOffset: 0x22C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 14 4B 14 FE 0D 06 00 2C 02 10 10 00 01 00 }
0x5A24E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A255: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A25C: 			End  { 29 02 }
0x5A25E: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xDFF, VarStoreId: 0x6, VarOffset: 0x248, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 61 14 68 14 FF 0D 06 00 48 02 10 10 00 01 00 }
0x5A26F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A276: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A27D: 			End  { 29 02 }
0x5A27F: 			GrayOutIf  { 19 82 }
0x5A281: 				EqIdVal QuestionId: 0xDF3, Value: 0x0 { 12 06 F3 0D 00 00 }
0x5A287: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE00, VarStoreId: 0x6, VarOffset: 0x264, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7E 14 85 14 00 0E 06 00 64 02 10 10 00 01 00 }
0x5A298: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A29F: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A2A6: 				End  { 29 02 }
0x5A2A8: 			End  { 29 02 }
0x5A2AA: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE01, VarStoreId: 0x6, VarOffset: 0x280, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9B 14 A2 14 01 0E 06 00 80 02 10 10 00 01 00 }
0x5A2BB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A2C2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A2C9: 			End  { 29 02 }
0x5A2CB: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xE02, VarStoreId: 0x6, VarOffset: 0x29C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 58 13 5F 13 02 0E 06 00 9C 02 10 10 00 04 00 }
0x5A2DC: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5A2E3: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5A2EA: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5A2F1: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5A2F8: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5A2FF: 			End  { 29 02 }
0x5A301: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE03, VarStoreId: 0x6, VarOffset: 0x2B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DB 14 E2 14 03 0E 06 00 B8 02 10 10 00 01 00 }
0x5A312: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A319: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A320: 			End  { 29 02 }
0x5A322: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xE04, VarStoreId: 0x6, VarOffset: 0x3AD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F8 14 FF 14 04 0E 06 00 AD 03 00 11 00 00 FF FF 01 00 }
0x5A336: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5A33D: 			End  { 29 02 }
0x5A33F: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE05, VarStoreId: 0x6, VarOffset: 0x534, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 15 15 1C 15 05 0E 06 00 34 05 00 10 00 07 01 }
0x5A350: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5A356: 			End  { 29 02 }
0x5A358: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xE06, VarStoreId: 0x6, VarOffset: 0x565, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 32 15 39 15 06 0E 06 00 65 05 00 11 01 00 14 00 01 00 }
0x5A36C: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5A373: 			End  { 29 02 }
0x5A375: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE07, VarStoreId: 0x6, VarOffset: 0x588, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 4F 15 56 15 07 0E 06 00 88 05 00 10 04 14 04 }
0x5A386: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5A38C: 			End  { 29 02 }
0x5A38E: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5A395: 			End  { 29 02 }
0x5A397: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5A39E: 			End  { 29 02 }
0x5A3A0: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE08, VarStoreId: 0x6, VarOffset: 0x3F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 73 15 7A 15 08 0E 06 00 F8 03 10 10 00 01 00 }
0x5A3B1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A3B8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A3BF: 			End  { 29 02 }
0x5A3C1: 			SuppressIf  { 0A 82 }
0x5A3C3: 				EqIdVal QuestionId: 0xE08, Value: 0x0 { 12 06 08 0E 00 00 }
0x5A3C9: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE09, VarStoreId: 0x6, VarOffset: 0x430, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 F9 15 23 16 09 0E 06 00 30 04 10 10 00 02 00 }
0x5A3DA: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A3E1: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5A3E8: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5A3EF: 				End  { 29 02 }
0x5A3F1: 				SuppressIf  { 0A 82 }
0x5A3F3: 					EqIdVal QuestionId: 0xE09, Value: 0x1 { 12 86 09 0E 01 00 }
0x5A3F9: 						Not  { 17 02 }
0x5A3FB: 					End  { 29 02 }
0x5A3FD: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE0A, VarStoreId: 0x6, VarOffset: 0x4B5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 FB 15 25 16 0A 0E 06 00 B5 04 10 11 00 00 FF 03 01 00 }
0x5A411: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5A418: 					End  { 29 02 }
0x5A41A: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE0B, VarStoreId: 0x6, VarOffset: 0x44C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 FC 15 26 16 0B 0E 06 00 4C 04 10 10 00 05 00 }
0x5A42B: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5A432: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5A439: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5A440: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5A447: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5A44E: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5A455: 					End  { 29 02 }
0x5A457: 				End  { 29 02 }
0x5A459: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE0C, VarStoreId: 0x6, VarOffset: 0x468, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 FA 15 24 16 0C 0E 06 00 68 04 10 10 00 02 00 }
0x5A46A: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A471: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5A478: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5A47F: 				End  { 29 02 }
0x5A481: 				SuppressIf  { 0A 82 }
0x5A483: 					EqIdVal QuestionId: 0xE0C, Value: 0x1 { 12 86 0C 0E 01 00 }
0x5A489: 						Not  { 17 02 }
0x5A48B: 					End  { 29 02 }
0x5A48D: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE0D, VarStoreId: 0x6, VarOffset: 0x4ED, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 FD 15 27 16 0D 0E 06 00 ED 04 10 11 00 00 FF 03 01 00 }
0x5A4A1: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5A4A8: 					End  { 29 02 }
0x5A4AA: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE0E, VarStoreId: 0x6, VarOffset: 0x484, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 FE 15 28 16 0E 0E 06 00 84 04 10 10 00 05 00 }
0x5A4BB: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5A4C2: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5A4C9: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5A4D0: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5A4D7: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5A4DE: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5A4E5: 					End  { 29 02 }
0x5A4E7: 				End  { 29 02 }
0x5A4E9: 			End  { 29 02 }
0x5A4EB: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5A4F2: 			End  { 29 02 }
0x5A4F4: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xE0F, VarStoreId: 0x6, VarOffset: 0x414, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 16 45 16 0F 0E 06 00 14 04 10 10 00 01 00 }
0x5A505: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A50C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A513: 			End  { 29 02 }
0x5A515: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE10, VarStoreId: 0x6, VarOffset: 0xD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 14 C3 14 10 0E 06 00 D3 00 10 10 00 01 00 }
0x5A526: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A52D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A534: 			End  { 29 02 }
0x5A536: 		End  { 29 02 }
0x5A538: 	End  { 29 02 }
0x5A53A: 	Form FormId: 0x2846, Title: "PCI Express Root Port 23" { 01 86 46 28 8C 16 }
0x5A540: 		OneOf Prompt: "PCI Express Root Port 23", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xE11, VarStoreId: 0x6, VarOffset: 0x115, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 13 7C 13 11 0E 06 00 15 01 10 10 00 01 00 }
0x5A551: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A558: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A55F: 		End  { 29 02 }
0x5A561: 		SuppressIf  { 0A 82 }
0x5A563: 			EqIdVal QuestionId: 0xE11, Value: 0x0 { 12 06 11 0E 00 00 }
0x5A569: 			GrayOutIf  { 19 82 }
0x5A56B: 				EqIdVal QuestionId: 0xE1F, Value: 0x1 { 12 06 1F 0E 01 00 }
0x5A571: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xE12, VarStoreId: 0x6, VarOffset: 0x37D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 36 17 E5 0E 12 0E 06 00 7D 03 10 10 00 01 00 }
0x5A582: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5A589: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5A590: 				End  { 29 02 }
0x5A592: 			End  { 29 02 }
0x5A594: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2815, VarStoreId: 0x6, VarOffset: 0x131, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8C 12 F5 0D 15 28 06 00 31 01 10 10 00 04 00 }
0x5A5A5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A5AC: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5A5B3: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5A5BA: 			End  { 29 02 }
0x5A5BC: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2816, VarStoreId: 0x6, VarOffset: 0x2D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A8 12 AE 12 16 28 06 00 D5 02 10 10 00 02 00 }
0x5A5CD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A5D4: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5A5DB: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5A5E2: 			End  { 29 02 }
0x5A5E4: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE13, VarStoreId: 0x6, VarOffset: 0x2F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C7 12 CD 12 13 0E 06 00 F1 02 10 10 00 01 00 }
0x5A5F5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A5FC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A603: 			End  { 29 02 }
0x5A605: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xE14, VarStoreId: 0x6, VarOffset: 0x30D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 12 A7 0E 14 0E 06 00 0D 03 10 10 00 01 00 }
0x5A616: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A61D: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A624: 			End  { 29 02 }
0x5A626: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2817, VarStoreId: 0x6, VarOffset: 0x329, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 00 13 06 13 17 28 06 00 29 03 10 10 00 01 00 }
0x5A637: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A63E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A645: 			End  { 29 02 }
0x5A647: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE15, VarStoreId: 0x6, VarOffset: 0x345, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1D 13 23 13 15 0E 06 00 45 03 10 10 00 01 00 }
0x5A658: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A65F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A666: 			End  { 29 02 }
0x5A668: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE16, VarStoreId: 0x6, VarOffset: 0x361, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 13 40 13 16 0E 06 00 61 03 10 10 00 01 00 }
0x5A679: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A680: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A687: 			End  { 29 02 }
0x5A689: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE17, VarStoreId: 0x6, VarOffset: 0x14D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 13 99 13 17 0E 06 00 4D 01 10 10 00 01 00 }
0x5A69A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A6A1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A6A8: 			End  { 29 02 }
0x5A6AA: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE18, VarStoreId: 0x6, VarOffset: 0x169, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B0 13 B6 13 18 0E 06 00 69 01 10 10 00 01 00 }
0x5A6BB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A6C2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A6C9: 			End  { 29 02 }
0x5A6CB: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE19, VarStoreId: 0x6, VarOffset: 0x185, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CD 13 D3 13 19 0E 06 00 85 01 10 10 00 01 00 }
0x5A6DC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A6E3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A6EA: 			End  { 29 02 }
0x5A6EC: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE1A, VarStoreId: 0x6, VarOffset: 0x1A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EA 13 F0 13 1A 0E 06 00 A1 01 10 10 00 01 00 }
0x5A6FD: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A704: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A70B: 			End  { 29 02 }
0x5A70D: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE1B, VarStoreId: 0x6, VarOffset: 0x1F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 14 11 14 1B 0E 06 00 F5 01 10 10 00 01 00 }
0x5A71E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A725: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A72C: 			End  { 29 02 }
0x5A72E: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE1C, VarStoreId: 0x6, VarOffset: 0x211, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 14 2E 14 1C 0E 06 00 11 02 10 10 00 01 00 }
0x5A73F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A746: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A74D: 			End  { 29 02 }
0x5A74F: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE1D, VarStoreId: 0x6, VarOffset: 0x22D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 45 14 4B 14 1D 0E 06 00 2D 02 10 10 00 01 00 }
0x5A760: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A767: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A76E: 			End  { 29 02 }
0x5A770: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE1E, VarStoreId: 0x6, VarOffset: 0x249, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 62 14 68 14 1E 0E 06 00 49 02 10 10 00 01 00 }
0x5A781: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A788: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A78F: 			End  { 29 02 }
0x5A791: 			GrayOutIf  { 19 82 }
0x5A793: 				EqIdVal QuestionId: 0xE12, Value: 0x0 { 12 06 12 0E 00 00 }
0x5A799: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE1F, VarStoreId: 0x6, VarOffset: 0x265, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7F 14 85 14 1F 0E 06 00 65 02 10 10 00 01 00 }
0x5A7AA: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A7B1: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A7B8: 				End  { 29 02 }
0x5A7BA: 			End  { 29 02 }
0x5A7BC: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE20, VarStoreId: 0x6, VarOffset: 0x281, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9C 14 A2 14 20 0E 06 00 81 02 10 10 00 01 00 }
0x5A7CD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A7D4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A7DB: 			End  { 29 02 }
0x5A7DD: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xE21, VarStoreId: 0x6, VarOffset: 0x29D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 59 13 5F 13 21 0E 06 00 9D 02 10 10 00 04 00 }
0x5A7EE: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5A7F5: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5A7FC: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5A803: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5A80A: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5A811: 			End  { 29 02 }
0x5A813: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE22, VarStoreId: 0x6, VarOffset: 0x2B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DC 14 E2 14 22 0E 06 00 B9 02 10 10 00 01 00 }
0x5A824: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5A82B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5A832: 			End  { 29 02 }
0x5A834: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xE23, VarStoreId: 0x6, VarOffset: 0x3AF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 F9 14 FF 14 23 0E 06 00 AF 03 00 11 00 00 FF FF 01 00 }
0x5A848: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5A84F: 			End  { 29 02 }
0x5A851: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE24, VarStoreId: 0x6, VarOffset: 0x535, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 16 15 1C 15 24 0E 06 00 35 05 00 10 00 07 01 }
0x5A862: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5A868: 			End  { 29 02 }
0x5A86A: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xE25, VarStoreId: 0x6, VarOffset: 0x567, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 33 15 39 15 25 0E 06 00 67 05 00 11 01 00 14 00 01 00 }
0x5A87E: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5A885: 			End  { 29 02 }
0x5A887: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE26, VarStoreId: 0x6, VarOffset: 0x589, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 50 15 56 15 26 0E 06 00 89 05 00 10 04 14 04 }
0x5A898: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5A89E: 			End  { 29 02 }
0x5A8A0: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5A8A7: 			End  { 29 02 }
0x5A8A9: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5A8B0: 			End  { 29 02 }
0x5A8B2: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE27, VarStoreId: 0x6, VarOffset: 0x3F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 74 15 7A 15 27 0E 06 00 F9 03 10 10 00 01 00 }
0x5A8C3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A8CA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5A8D1: 			End  { 29 02 }
0x5A8D3: 			SuppressIf  { 0A 82 }
0x5A8D5: 				EqIdVal QuestionId: 0xE27, Value: 0x0 { 12 06 27 0E 00 00 }
0x5A8DB: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE28, VarStoreId: 0x6, VarOffset: 0x431, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 FF 15 23 16 28 0E 06 00 31 04 10 10 00 02 00 }
0x5A8EC: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A8F3: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5A8FA: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5A901: 				End  { 29 02 }
0x5A903: 				SuppressIf  { 0A 82 }
0x5A905: 					EqIdVal QuestionId: 0xE28, Value: 0x1 { 12 86 28 0E 01 00 }
0x5A90B: 						Not  { 17 02 }
0x5A90D: 					End  { 29 02 }
0x5A90F: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE29, VarStoreId: 0x6, VarOffset: 0x4B7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 01 16 25 16 29 0E 06 00 B7 04 10 11 00 00 FF 03 01 00 }
0x5A923: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5A92A: 					End  { 29 02 }
0x5A92C: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE2A, VarStoreId: 0x6, VarOffset: 0x44D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 02 16 26 16 2A 0E 06 00 4D 04 10 10 00 05 00 }
0x5A93D: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5A944: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5A94B: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5A952: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5A959: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5A960: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5A967: 					End  { 29 02 }
0x5A969: 				End  { 29 02 }
0x5A96B: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE2B, VarStoreId: 0x6, VarOffset: 0x469, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 00 16 24 16 2B 0E 06 00 69 04 10 10 00 02 00 }
0x5A97C: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5A983: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5A98A: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5A991: 				End  { 29 02 }
0x5A993: 				SuppressIf  { 0A 82 }
0x5A995: 					EqIdVal QuestionId: 0xE2B, Value: 0x1 { 12 86 2B 0E 01 00 }
0x5A99B: 						Not  { 17 02 }
0x5A99D: 					End  { 29 02 }
0x5A99F: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE2C, VarStoreId: 0x6, VarOffset: 0x4EF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 03 16 27 16 2C 0E 06 00 EF 04 10 11 00 00 FF 03 01 00 }
0x5A9B3: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5A9BA: 					End  { 29 02 }
0x5A9BC: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE2D, VarStoreId: 0x6, VarOffset: 0x485, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 04 16 28 16 2D 0E 06 00 85 04 10 10 00 05 00 }
0x5A9CD: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5A9D4: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5A9DB: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5A9E2: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5A9E9: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5A9F0: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5A9F7: 					End  { 29 02 }
0x5A9F9: 				End  { 29 02 }
0x5A9FB: 			End  { 29 02 }
0x5A9FD: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5AA04: 			End  { 29 02 }
0x5AA06: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xE2E, VarStoreId: 0x6, VarOffset: 0x415, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3F 16 45 16 2E 0E 06 00 15 04 10 10 00 01 00 }
0x5AA17: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AA1E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AA25: 			End  { 29 02 }
0x5AA27: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE2F, VarStoreId: 0x6, VarOffset: 0xD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 14 C3 14 2F 0E 06 00 D4 00 10 10 00 01 00 }
0x5AA38: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AA3F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AA46: 			End  { 29 02 }
0x5AA48: 		End  { 29 02 }
0x5AA4A: 	End  { 29 02 }
0x5AA4C: 	Form FormId: 0x2847, Title: "PCI Express Root Port 24" { 01 86 47 28 8D 16 }
0x5AA52: 		OneOf Prompt: "PCI Express Root Port 24", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xE30, VarStoreId: 0x6, VarOffset: 0x116, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 77 13 7C 13 30 0E 06 00 16 01 10 10 00 01 00 }
0x5AA63: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AA6A: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5AA71: 		End  { 29 02 }
0x5AA73: 		SuppressIf  { 0A 82 }
0x5AA75: 			EqIdVal QuestionId: 0xE30, Value: 0x0 { 12 06 30 0E 00 00 }
0x5AA7B: 			GrayOutIf  { 19 82 }
0x5AA7D: 				EqIdVal QuestionId: 0xE3E, Value: 0x1 { 12 06 3E 0E 01 00 }
0x5AA83: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xE31, VarStoreId: 0x6, VarOffset: 0x37E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 37 17 E5 0E 31 0E 06 00 7E 03 10 10 00 01 00 }
0x5AA94: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5AA9B: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5AAA2: 				End  { 29 02 }
0x5AAA4: 			End  { 29 02 }
0x5AAA6: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2818, VarStoreId: 0x6, VarOffset: 0x132, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8D 12 F5 0D 18 28 06 00 32 01 10 10 00 04 00 }
0x5AAB7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AABE: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5AAC5: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5AACC: 			End  { 29 02 }
0x5AACE: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2819, VarStoreId: 0x6, VarOffset: 0x2D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A9 12 AE 12 19 28 06 00 D6 02 10 10 00 02 00 }
0x5AADF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AAE6: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5AAED: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5AAF4: 			End  { 29 02 }
0x5AAF6: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE32, VarStoreId: 0x6, VarOffset: 0x2F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 12 CD 12 32 0E 06 00 F2 02 10 10 00 01 00 }
0x5AB07: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AB0E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5AB15: 			End  { 29 02 }
0x5AB17: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xE33, VarStoreId: 0x6, VarOffset: 0x30E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E5 12 A7 0E 33 0E 06 00 0E 03 10 10 00 01 00 }
0x5AB28: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AB2F: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5AB36: 			End  { 29 02 }
0x5AB38: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x281A, VarStoreId: 0x6, VarOffset: 0x32A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 13 06 13 1A 28 06 00 2A 03 10 10 00 01 00 }
0x5AB49: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AB50: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5AB57: 			End  { 29 02 }
0x5AB59: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE34, VarStoreId: 0x6, VarOffset: 0x346, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1E 13 23 13 34 0E 06 00 46 03 10 10 00 01 00 }
0x5AB6A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AB71: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AB78: 			End  { 29 02 }
0x5AB7A: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE35, VarStoreId: 0x6, VarOffset: 0x362, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3B 13 40 13 35 0E 06 00 62 03 10 10 00 01 00 }
0x5AB8B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AB92: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5AB99: 			End  { 29 02 }
0x5AB9B: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE36, VarStoreId: 0x6, VarOffset: 0x14E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 13 99 13 36 0E 06 00 4E 01 10 10 00 01 00 }
0x5ABAC: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5ABB3: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5ABBA: 			End  { 29 02 }
0x5ABBC: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE37, VarStoreId: 0x6, VarOffset: 0x16A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 13 B6 13 37 0E 06 00 6A 01 10 10 00 01 00 }
0x5ABCD: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5ABD4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5ABDB: 			End  { 29 02 }
0x5ABDD: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE38, VarStoreId: 0x6, VarOffset: 0x186, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CE 13 D3 13 38 0E 06 00 86 01 10 10 00 01 00 }
0x5ABEE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5ABF5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5ABFC: 			End  { 29 02 }
0x5ABFE: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE39, VarStoreId: 0x6, VarOffset: 0x1A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EB 13 F0 13 39 0E 06 00 A2 01 10 10 00 01 00 }
0x5AC0F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AC16: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AC1D: 			End  { 29 02 }
0x5AC1F: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE3A, VarStoreId: 0x6, VarOffset: 0x1F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0C 14 11 14 3A 0E 06 00 F6 01 10 10 00 01 00 }
0x5AC30: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AC37: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AC3E: 			End  { 29 02 }
0x5AC40: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE3B, VarStoreId: 0x6, VarOffset: 0x212, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 29 14 2E 14 3B 0E 06 00 12 02 10 10 00 01 00 }
0x5AC51: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AC58: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AC5F: 			End  { 29 02 }
0x5AC61: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE3C, VarStoreId: 0x6, VarOffset: 0x22E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 14 4B 14 3C 0E 06 00 2E 02 10 10 00 01 00 }
0x5AC72: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AC79: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AC80: 			End  { 29 02 }
0x5AC82: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE3D, VarStoreId: 0x6, VarOffset: 0x24A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 63 14 68 14 3D 0E 06 00 4A 02 10 10 00 01 00 }
0x5AC93: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AC9A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5ACA1: 			End  { 29 02 }
0x5ACA3: 			GrayOutIf  { 19 82 }
0x5ACA5: 				EqIdVal QuestionId: 0xE31, Value: 0x0 { 12 06 31 0E 00 00 }
0x5ACAB: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE3E, VarStoreId: 0x6, VarOffset: 0x266, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 80 14 85 14 3E 0E 06 00 66 02 10 10 00 01 00 }
0x5ACBC: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5ACC3: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5ACCA: 				End  { 29 02 }
0x5ACCC: 			End  { 29 02 }
0x5ACCE: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE3F, VarStoreId: 0x6, VarOffset: 0x282, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 14 A2 14 3F 0E 06 00 82 02 10 10 00 01 00 }
0x5ACDF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5ACE6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5ACED: 			End  { 29 02 }
0x5ACEF: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xE40, VarStoreId: 0x6, VarOffset: 0x29E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5A 13 5F 13 40 0E 06 00 9E 02 10 10 00 04 00 }
0x5AD00: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5AD07: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5AD0E: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5AD15: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5AD1C: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5AD23: 			End  { 29 02 }
0x5AD25: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE41, VarStoreId: 0x6, VarOffset: 0x2BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DD 14 E2 14 41 0E 06 00 BA 02 10 10 00 01 00 }
0x5AD36: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AD3D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AD44: 			End  { 29 02 }
0x5AD46: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xE42, VarStoreId: 0x6, VarOffset: 0x3B1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 FA 14 FF 14 42 0E 06 00 B1 03 00 11 00 00 FF FF 01 00 }
0x5AD5A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5AD61: 			End  { 29 02 }
0x5AD63: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE43, VarStoreId: 0x6, VarOffset: 0x536, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 17 15 1C 15 43 0E 06 00 36 05 00 10 00 07 01 }
0x5AD74: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5AD7A: 			End  { 29 02 }
0x5AD7C: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xE44, VarStoreId: 0x6, VarOffset: 0x569, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 34 15 39 15 44 0E 06 00 69 05 00 11 01 00 14 00 01 00 }
0x5AD90: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5AD97: 			End  { 29 02 }
0x5AD99: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE45, VarStoreId: 0x6, VarOffset: 0x58A, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 51 15 56 15 45 0E 06 00 8A 05 00 10 04 14 04 }
0x5ADAA: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5ADB0: 			End  { 29 02 }
0x5ADB2: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5ADB9: 			End  { 29 02 }
0x5ADBB: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5ADC2: 			End  { 29 02 }
0x5ADC4: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE46, VarStoreId: 0x6, VarOffset: 0x3FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 75 15 7A 15 46 0E 06 00 FA 03 10 10 00 01 00 }
0x5ADD5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5ADDC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5ADE3: 			End  { 29 02 }
0x5ADE5: 			SuppressIf  { 0A 82 }
0x5ADE7: 				EqIdVal QuestionId: 0xE46, Value: 0x0 { 12 06 46 0E 00 00 }
0x5ADED: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE47, VarStoreId: 0x6, VarOffset: 0x432, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 05 16 23 16 47 0E 06 00 32 04 10 10 00 02 00 }
0x5ADFE: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AE05: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5AE0C: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5AE13: 				End  { 29 02 }
0x5AE15: 				SuppressIf  { 0A 82 }
0x5AE17: 					EqIdVal QuestionId: 0xE47, Value: 0x1 { 12 86 47 0E 01 00 }
0x5AE1D: 						Not  { 17 02 }
0x5AE1F: 					End  { 29 02 }
0x5AE21: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE48, VarStoreId: 0x6, VarOffset: 0x4B9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 07 16 25 16 48 0E 06 00 B9 04 10 11 00 00 FF 03 01 00 }
0x5AE35: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5AE3C: 					End  { 29 02 }
0x5AE3E: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE49, VarStoreId: 0x6, VarOffset: 0x44E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 08 16 26 16 49 0E 06 00 4E 04 10 10 00 05 00 }
0x5AE4F: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5AE56: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5AE5D: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5AE64: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5AE6B: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5AE72: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5AE79: 					End  { 29 02 }
0x5AE7B: 				End  { 29 02 }
0x5AE7D: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE4A, VarStoreId: 0x6, VarOffset: 0x46A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 06 16 24 16 4A 0E 06 00 6A 04 10 10 00 02 00 }
0x5AE8E: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AE95: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5AE9C: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5AEA3: 				End  { 29 02 }
0x5AEA5: 				SuppressIf  { 0A 82 }
0x5AEA7: 					EqIdVal QuestionId: 0xE4A, Value: 0x1 { 12 86 4A 0E 01 00 }
0x5AEAD: 						Not  { 17 02 }
0x5AEAF: 					End  { 29 02 }
0x5AEB1: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE4B, VarStoreId: 0x6, VarOffset: 0x4F1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 09 16 27 16 4B 0E 06 00 F1 04 10 11 00 00 FF 03 01 00 }
0x5AEC5: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5AECC: 					End  { 29 02 }
0x5AECE: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE4C, VarStoreId: 0x6, VarOffset: 0x486, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 0A 16 28 16 4C 0E 06 00 86 04 10 10 00 05 00 }
0x5AEDF: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5AEE6: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5AEED: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5AEF4: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5AEFB: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5AF02: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5AF09: 					End  { 29 02 }
0x5AF0B: 				End  { 29 02 }
0x5AF0D: 			End  { 29 02 }
0x5AF0F: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5AF16: 			End  { 29 02 }
0x5AF18: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xE4D, VarStoreId: 0x6, VarOffset: 0x416, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 40 16 45 16 4D 0E 06 00 16 04 10 10 00 01 00 }
0x5AF29: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AF30: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AF37: 			End  { 29 02 }
0x5AF39: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE4E, VarStoreId: 0x6, VarOffset: 0xD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 14 C3 14 4E 0E 06 00 D5 00 10 10 00 01 00 }
0x5AF4A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AF51: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5AF58: 			End  { 29 02 }
0x5AF5A: 		End  { 29 02 }
0x5AF5C: 	End  { 29 02 }
0x5AF5E: 	Form FormId: 0x2848, Title: "PCI Express Root Port 25" { 01 86 48 28 8E 16 }
0x5AF64: 		OneOf Prompt: "PCI Express Root Port 25", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xE4F, VarStoreId: 0x6, VarOffset: 0x117, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 13 7C 13 4F 0E 06 00 17 01 10 10 00 01 00 }
0x5AF75: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5AF7C: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5AF83: 		End  { 29 02 }
0x5AF85: 		SuppressIf  { 0A 82 }
0x5AF87: 			EqIdVal QuestionId: 0xE4F, Value: 0x0 { 12 06 4F 0E 00 00 }
0x5AF8D: 			GrayOutIf  { 19 82 }
0x5AF8F: 				EqIdVal QuestionId: 0xE5D, Value: 0x1 { 12 06 5D 0E 01 00 }
0x5AF95: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xE50, VarStoreId: 0x6, VarOffset: 0x37F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 38 17 E5 0E 50 0E 06 00 7F 03 10 10 00 01 00 }
0x5AFA6: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5AFAD: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5AFB4: 				End  { 29 02 }
0x5AFB6: 			End  { 29 02 }
0x5AFB8: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x281B, VarStoreId: 0x6, VarOffset: 0x133, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8E 12 F5 0D 1B 28 06 00 33 01 10 10 00 04 00 }
0x5AFC9: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5AFD0: 				OneOfOption Option: "L1" Value: 2 { 09 07 FC 0E 00 00 02 }
0x5AFD7: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5AFDE: 			End  { 29 02 }
0x5AFE0: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x281C, VarStoreId: 0x6, VarOffset: 0x2D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AA 12 AE 12 1C 28 06 00 D7 02 10 10 00 02 00 }
0x5AFF1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5AFF8: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5AFFF: 				OneOfOption Option: "L1.1 & L1.2" Value: 2 { 09 07 B0 12 00 00 02 }
0x5B006: 			End  { 29 02 }
0x5B008: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE51, VarStoreId: 0x6, VarOffset: 0x2F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C9 12 CD 12 51 0E 06 00 F3 02 10 10 00 01 00 }
0x5B019: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B020: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B027: 			End  { 29 02 }
0x5B029: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xE52, VarStoreId: 0x6, VarOffset: 0x30F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E6 12 A7 0E 52 0E 06 00 0F 03 10 10 00 01 00 }
0x5B03A: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B041: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B048: 			End  { 29 02 }
0x5B04A: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x281D, VarStoreId: 0x6, VarOffset: 0x32B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 13 06 13 1D 28 06 00 2B 03 10 10 00 01 00 }
0x5B05B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B062: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B069: 			End  { 29 02 }
0x5B06B: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE53, VarStoreId: 0x6, VarOffset: 0x347, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1F 13 23 13 53 0E 06 00 47 03 10 10 00 01 00 }
0x5B07C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B083: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B08A: 			End  { 29 02 }
0x5B08C: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE54, VarStoreId: 0x6, VarOffset: 0x363, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3C 13 40 13 54 0E 06 00 63 03 10 10 00 01 00 }
0x5B09D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B0A4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B0AB: 			End  { 29 02 }
0x5B0AD: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE55, VarStoreId: 0x6, VarOffset: 0x14F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 13 99 13 55 0E 06 00 4F 01 10 10 00 01 00 }
0x5B0BE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B0C5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B0CC: 			End  { 29 02 }
0x5B0CE: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE56, VarStoreId: 0x6, VarOffset: 0x16B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 13 B6 13 56 0E 06 00 6B 01 10 10 00 01 00 }
0x5B0DF: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B0E6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B0ED: 			End  { 29 02 }
0x5B0EF: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE57, VarStoreId: 0x6, VarOffset: 0x187, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CF 13 D3 13 57 0E 06 00 87 01 10 10 00 01 00 }
0x5B100: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B107: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B10E: 			End  { 29 02 }
0x5B110: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE58, VarStoreId: 0x6, VarOffset: 0x1A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EC 13 F0 13 58 0E 06 00 A3 01 10 10 00 01 00 }
0x5B121: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B128: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B12F: 			End  { 29 02 }
0x5B131: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE59, VarStoreId: 0x6, VarOffset: 0x1F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0D 14 11 14 59 0E 06 00 F7 01 10 10 00 01 00 }
0x5B142: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B149: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B150: 			End  { 29 02 }
0x5B152: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE5A, VarStoreId: 0x6, VarOffset: 0x213, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 14 2E 14 5A 0E 06 00 13 02 10 10 00 01 00 }
0x5B163: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B16A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B171: 			End  { 29 02 }
0x5B173: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE5B, VarStoreId: 0x6, VarOffset: 0x22F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 47 14 4B 14 5B 0E 06 00 2F 02 10 10 00 01 00 }
0x5B184: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B18B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B192: 			End  { 29 02 }
0x5B194: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE5C, VarStoreId: 0x6, VarOffset: 0x24B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 64 14 68 14 5C 0E 06 00 4B 02 10 10 00 01 00 }
0x5B1A5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B1AC: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B1B3: 			End  { 29 02 }
0x5B1B5: 			GrayOutIf  { 19 82 }
0x5B1B7: 				EqIdVal QuestionId: 0xE50, Value: 0x0 { 12 06 50 0E 00 00 }
0x5B1BD: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE5D, VarStoreId: 0x6, VarOffset: 0x267, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 81 14 85 14 5D 0E 06 00 67 02 10 10 00 01 00 }
0x5B1CE: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B1D5: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B1DC: 				End  { 29 02 }
0x5B1DE: 			End  { 29 02 }
0x5B1E0: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE5E, VarStoreId: 0x6, VarOffset: 0x283, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9E 14 A2 14 5E 0E 06 00 83 02 10 10 00 01 00 }
0x5B1F1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B1F8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B1FF: 			End  { 29 02 }
0x5B201: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xE5F, VarStoreId: 0x6, VarOffset: 0x29F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5B 13 5F 13 5F 0E 06 00 9F 02 10 10 00 04 00 }
0x5B212: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5B219: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5B220: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5B227: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5B22E: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5B235: 			End  { 29 02 }
0x5B237: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE60, VarStoreId: 0x6, VarOffset: 0x2BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DE 14 E2 14 60 0E 06 00 BB 02 10 10 00 01 00 }
0x5B248: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B24F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B256: 			End  { 29 02 }
0x5B258: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xE61, VarStoreId: 0x6, VarOffset: 0x3B3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 FB 14 FF 14 61 0E 06 00 B3 03 00 11 00 00 FF FF 01 00 }
0x5B26C: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5B273: 			End  { 29 02 }
0x5B275: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE62, VarStoreId: 0x6, VarOffset: 0x537, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 18 15 1C 15 62 0E 06 00 37 05 00 10 00 07 01 }
0x5B286: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5B28C: 			End  { 29 02 }
0x5B28E: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xE63, VarStoreId: 0x6, VarOffset: 0x56B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 35 15 39 15 63 0E 06 00 6B 05 00 11 01 00 14 00 01 00 }
0x5B2A2: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5B2A9: 			End  { 29 02 }
0x5B2AB: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE64, VarStoreId: 0x6, VarOffset: 0x58B, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 52 15 56 15 64 0E 06 00 8B 05 00 10 04 14 04 }
0x5B2BC: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5B2C2: 			End  { 29 02 }
0x5B2C4: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5B2CB: 			End  { 29 02 }
0x5B2CD: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5B2D4: 			End  { 29 02 }
0x5B2D6: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE65, VarStoreId: 0x6, VarOffset: 0x3FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 76 15 7A 15 65 0E 06 00 FB 03 10 10 00 01 00 }
0x5B2E7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B2EE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B2F5: 			End  { 29 02 }
0x5B2F7: 			SuppressIf  { 0A 82 }
0x5B2F9: 				EqIdVal QuestionId: 0xE65, Value: 0x0 { 12 06 65 0E 00 00 }
0x5B2FF: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE66, VarStoreId: 0x6, VarOffset: 0x433, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 0B 16 23 16 66 0E 06 00 33 04 10 10 00 02 00 }
0x5B310: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B317: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5B31E: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5B325: 				End  { 29 02 }
0x5B327: 				SuppressIf  { 0A 82 }
0x5B329: 					EqIdVal QuestionId: 0xE66, Value: 0x1 { 12 86 66 0E 01 00 }
0x5B32F: 						Not  { 17 02 }
0x5B331: 					End  { 29 02 }
0x5B333: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE67, VarStoreId: 0x6, VarOffset: 0x4BB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 0D 16 25 16 67 0E 06 00 BB 04 10 11 00 00 FF 03 01 00 }
0x5B347: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5B34E: 					End  { 29 02 }
0x5B350: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE68, VarStoreId: 0x6, VarOffset: 0x44F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 0E 16 26 16 68 0E 06 00 4F 04 10 10 00 05 00 }
0x5B361: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5B368: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5B36F: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5B376: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5B37D: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5B384: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5B38B: 					End  { 29 02 }
0x5B38D: 				End  { 29 02 }
0x5B38F: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE69, VarStoreId: 0x6, VarOffset: 0x46B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 0C 16 24 16 69 0E 06 00 6B 04 10 10 00 02 00 }
0x5B3A0: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B3A7: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5B3AE: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5B3B5: 				End  { 29 02 }
0x5B3B7: 				SuppressIf  { 0A 82 }
0x5B3B9: 					EqIdVal QuestionId: 0xE69, Value: 0x1 { 12 86 69 0E 01 00 }
0x5B3BF: 						Not  { 17 02 }
0x5B3C1: 					End  { 29 02 }
0x5B3C3: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE6A, VarStoreId: 0x6, VarOffset: 0x4F3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 0F 16 27 16 6A 0E 06 00 F3 04 10 11 00 00 FF 03 01 00 }
0x5B3D7: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5B3DE: 					End  { 29 02 }
0x5B3E0: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE6B, VarStoreId: 0x6, VarOffset: 0x487, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 10 16 28 16 6B 0E 06 00 87 04 10 10 00 05 00 }
0x5B3F1: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5B3F8: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5B3FF: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5B406: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5B40D: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5B414: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5B41B: 					End  { 29 02 }
0x5B41D: 				End  { 29 02 }
0x5B41F: 			End  { 29 02 }
0x5B421: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5B428: 			End  { 29 02 }
0x5B42A: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xE6C, VarStoreId: 0x6, VarOffset: 0x417, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 41 16 45 16 6C 0E 06 00 17 04 10 10 00 01 00 }
0x5B43B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B442: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B449: 			End  { 29 02 }
0x5B44B: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE6D, VarStoreId: 0x6, VarOffset: 0xD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 14 C3 14 6D 0E 06 00 D6 00 10 10 00 01 00 }
0x5B45C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B463: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B46A: 			End  { 29 02 }
0x5B46C: 		End  { 29 02 }
0x5B46E: 	End  { 29 02 }
0x5B470: 	Form FormId: 0x2849, Title: "PCI Express Root Port 26" { 01 86 49 28 8F 16 }
0x5B476: 		OneOf Prompt: "PCI Express Root Port 26", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xE6E, VarStoreId: 0x6, VarOffset: 0x118, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 79 13 7C 13 6E 0E 06 00 18 01 10 10 00 01 00 }
0x5B487: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B48E: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B495: 		End  { 29 02 }
0x5B497: 		SuppressIf  { 0A 82 }
0x5B499: 			EqIdVal QuestionId: 0xE6E, Value: 0x0 { 12 06 6E 0E 00 00 }
0x5B49F: 			GrayOutIf  { 19 82 }
0x5B4A1: 				EqIdVal QuestionId: 0xE7C, Value: 0x1 { 12 06 7C 0E 01 00 }
0x5B4A7: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xE6F, VarStoreId: 0x6, VarOffset: 0x380, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 17 E5 0E 6F 0E 06 00 80 03 10 10 00 01 00 }
0x5B4B8: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5B4BF: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5B4C6: 				End  { 29 02 }
0x5B4C8: 			End  { 29 02 }
0x5B4CA: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x281E, VarStoreId: 0x6, VarOffset: 0x134, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 8F 12 F5 0D 1E 28 06 00 34 01 10 10 00 04 00 }
0x5B4DB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B4E2: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5B4E9: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5B4F0: 			End  { 29 02 }
0x5B4F2: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x281F, VarStoreId: 0x6, VarOffset: 0x2D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AB 12 AE 12 1F 28 06 00 D8 02 10 10 00 02 00 }
0x5B503: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B50A: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5B511: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5B518: 			End  { 29 02 }
0x5B51A: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE70, VarStoreId: 0x6, VarOffset: 0x2F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 12 CD 12 70 0E 06 00 F4 02 10 10 00 01 00 }
0x5B52B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B532: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B539: 			End  { 29 02 }
0x5B53B: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xE71, VarStoreId: 0x6, VarOffset: 0x310, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E7 12 A7 0E 71 0E 06 00 10 03 10 10 00 01 00 }
0x5B54C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B553: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B55A: 			End  { 29 02 }
0x5B55C: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2820, VarStoreId: 0x6, VarOffset: 0x32C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 03 13 06 13 20 28 06 00 2C 03 10 10 00 01 00 }
0x5B56D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B574: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B57B: 			End  { 29 02 }
0x5B57D: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE72, VarStoreId: 0x6, VarOffset: 0x348, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 20 13 23 13 72 0E 06 00 48 03 10 10 00 01 00 }
0x5B58E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B595: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B59C: 			End  { 29 02 }
0x5B59E: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE73, VarStoreId: 0x6, VarOffset: 0x364, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 13 40 13 73 0E 06 00 64 03 10 10 00 01 00 }
0x5B5AF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B5B6: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B5BD: 			End  { 29 02 }
0x5B5BF: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE74, VarStoreId: 0x6, VarOffset: 0x150, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 96 13 99 13 74 0E 06 00 50 01 10 10 00 01 00 }
0x5B5D0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B5D7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B5DE: 			End  { 29 02 }
0x5B5E0: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE75, VarStoreId: 0x6, VarOffset: 0x16C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 13 B6 13 75 0E 06 00 6C 01 10 10 00 01 00 }
0x5B5F1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B5F8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B5FF: 			End  { 29 02 }
0x5B601: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE76, VarStoreId: 0x6, VarOffset: 0x188, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D0 13 D3 13 76 0E 06 00 88 01 10 10 00 01 00 }
0x5B612: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B619: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B620: 			End  { 29 02 }
0x5B622: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE77, VarStoreId: 0x6, VarOffset: 0x1A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 ED 13 F0 13 77 0E 06 00 A4 01 10 10 00 01 00 }
0x5B633: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B63A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B641: 			End  { 29 02 }
0x5B643: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE78, VarStoreId: 0x6, VarOffset: 0x1F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0E 14 11 14 78 0E 06 00 F8 01 10 10 00 01 00 }
0x5B654: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B65B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B662: 			End  { 29 02 }
0x5B664: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE79, VarStoreId: 0x6, VarOffset: 0x214, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2B 14 2E 14 79 0E 06 00 14 02 10 10 00 01 00 }
0x5B675: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B67C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B683: 			End  { 29 02 }
0x5B685: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE7A, VarStoreId: 0x6, VarOffset: 0x230, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 14 4B 14 7A 0E 06 00 30 02 10 10 00 01 00 }
0x5B696: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B69D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B6A4: 			End  { 29 02 }
0x5B6A6: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE7B, VarStoreId: 0x6, VarOffset: 0x24C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 14 68 14 7B 0E 06 00 4C 02 10 10 00 01 00 }
0x5B6B7: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B6BE: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B6C5: 			End  { 29 02 }
0x5B6C7: 			GrayOutIf  { 19 82 }
0x5B6C9: 				EqIdVal QuestionId: 0xE6F, Value: 0x0 { 12 06 6F 0E 00 00 }
0x5B6CF: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE7C, VarStoreId: 0x6, VarOffset: 0x268, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 14 85 14 7C 0E 06 00 68 02 10 10 00 01 00 }
0x5B6E0: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B6E7: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B6EE: 				End  { 29 02 }
0x5B6F0: 			End  { 29 02 }
0x5B6F2: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE7D, VarStoreId: 0x6, VarOffset: 0x284, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9F 14 A2 14 7D 0E 06 00 84 02 10 10 00 01 00 }
0x5B703: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B70A: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B711: 			End  { 29 02 }
0x5B713: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xE7E, VarStoreId: 0x6, VarOffset: 0x2A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5C 13 5F 13 7E 0E 06 00 A0 02 10 10 00 04 00 }
0x5B724: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5B72B: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5B732: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5B739: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5B740: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5B747: 			End  { 29 02 }
0x5B749: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE7F, VarStoreId: 0x6, VarOffset: 0x2BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 DF 14 E2 14 7F 0E 06 00 BC 02 10 10 00 01 00 }
0x5B75A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B761: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B768: 			End  { 29 02 }
0x5B76A: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xE80, VarStoreId: 0x6, VarOffset: 0x3B5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 FC 14 FF 14 80 0E 06 00 B5 03 00 11 00 00 FF FF 01 00 }
0x5B77E: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5B785: 			End  { 29 02 }
0x5B787: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE81, VarStoreId: 0x6, VarOffset: 0x538, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 19 15 1C 15 81 0E 06 00 38 05 00 10 00 07 01 }
0x5B798: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5B79E: 			End  { 29 02 }
0x5B7A0: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xE82, VarStoreId: 0x6, VarOffset: 0x56D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 36 15 39 15 82 0E 06 00 6D 05 00 11 01 00 14 00 01 00 }
0x5B7B4: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5B7BB: 			End  { 29 02 }
0x5B7BD: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xE83, VarStoreId: 0x6, VarOffset: 0x58C, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 53 15 56 15 83 0E 06 00 8C 05 00 10 04 14 04 }
0x5B7CE: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5B7D4: 			End  { 29 02 }
0x5B7D6: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5B7DD: 			End  { 29 02 }
0x5B7DF: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5B7E6: 			End  { 29 02 }
0x5B7E8: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE84, VarStoreId: 0x6, VarOffset: 0x3FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 77 15 7A 15 84 0E 06 00 FC 03 10 10 00 01 00 }
0x5B7F9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B800: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B807: 			End  { 29 02 }
0x5B809: 			SuppressIf  { 0A 82 }
0x5B80B: 				EqIdVal QuestionId: 0xE84, Value: 0x0 { 12 06 84 0E 00 00 }
0x5B811: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE85, VarStoreId: 0x6, VarOffset: 0x434, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 11 16 23 16 85 0E 06 00 34 04 10 10 00 02 00 }
0x5B822: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B829: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5B830: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5B837: 				End  { 29 02 }
0x5B839: 				SuppressIf  { 0A 82 }
0x5B83B: 					EqIdVal QuestionId: 0xE85, Value: 0x1 { 12 86 85 0E 01 00 }
0x5B841: 						Not  { 17 02 }
0x5B843: 					End  { 29 02 }
0x5B845: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE86, VarStoreId: 0x6, VarOffset: 0x4BD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 13 16 25 16 86 0E 06 00 BD 04 10 11 00 00 FF 03 01 00 }
0x5B859: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5B860: 					End  { 29 02 }
0x5B862: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE87, VarStoreId: 0x6, VarOffset: 0x450, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 14 16 26 16 87 0E 06 00 50 04 10 10 00 05 00 }
0x5B873: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5B87A: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5B881: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5B888: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5B88F: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5B896: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5B89D: 					End  { 29 02 }
0x5B89F: 				End  { 29 02 }
0x5B8A1: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xE88, VarStoreId: 0x6, VarOffset: 0x46C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 12 16 24 16 88 0E 06 00 6C 04 10 10 00 02 00 }
0x5B8B2: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B8B9: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5B8C0: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5B8C7: 				End  { 29 02 }
0x5B8C9: 				SuppressIf  { 0A 82 }
0x5B8CB: 					EqIdVal QuestionId: 0xE88, Value: 0x1 { 12 86 88 0E 01 00 }
0x5B8D1: 						Not  { 17 02 }
0x5B8D3: 					End  { 29 02 }
0x5B8D5: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE89, VarStoreId: 0x6, VarOffset: 0x4F5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 15 16 27 16 89 0E 06 00 F5 04 10 11 00 00 FF 03 01 00 }
0x5B8E9: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5B8F0: 					End  { 29 02 }
0x5B8F2: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xE8A, VarStoreId: 0x6, VarOffset: 0x488, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 16 16 28 16 8A 0E 06 00 88 04 10 10 00 05 00 }
0x5B903: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5B90A: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5B911: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5B918: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5B91F: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5B926: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5B92D: 					End  { 29 02 }
0x5B92F: 				End  { 29 02 }
0x5B931: 			End  { 29 02 }
0x5B933: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5B93A: 			End  { 29 02 }
0x5B93C: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xE8B, VarStoreId: 0x6, VarOffset: 0x418, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 16 45 16 8B 0E 06 00 18 04 10 10 00 01 00 }
0x5B94D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B954: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B95B: 			End  { 29 02 }
0x5B95D: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xE8C, VarStoreId: 0x6, VarOffset: 0xD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 14 C3 14 8C 0E 06 00 D7 00 10 10 00 01 00 }
0x5B96E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5B975: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5B97C: 			End  { 29 02 }
0x5B97E: 		End  { 29 02 }
0x5B980: 	End  { 29 02 }
0x5B982: 	Form FormId: 0x284A, Title: "PCI Express Root Port 27" { 01 86 4A 28 90 16 }
0x5B988: 		OneOf Prompt: "PCI Express Root Port 27", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xE8D, VarStoreId: 0x6, VarOffset: 0x119, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7A 13 7C 13 8D 0E 06 00 19 01 10 10 00 01 00 }
0x5B999: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B9A0: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5B9A7: 		End  { 29 02 }
0x5B9A9: 		SuppressIf  { 0A 82 }
0x5B9AB: 			EqIdVal QuestionId: 0xE8D, Value: 0x0 { 12 06 8D 0E 00 00 }
0x5B9B1: 			GrayOutIf  { 19 82 }
0x5B9B3: 				EqIdVal QuestionId: 0xE9B, Value: 0x1 { 12 06 9B 0E 01 00 }
0x5B9B9: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xE8E, VarStoreId: 0x6, VarOffset: 0x381, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3A 17 E5 0E 8E 0E 06 00 81 03 10 10 00 01 00 }
0x5B9CA: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5B9D1: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5B9D8: 				End  { 29 02 }
0x5B9DA: 			End  { 29 02 }
0x5B9DC: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2821, VarStoreId: 0x6, VarOffset: 0x135, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 90 12 F5 0D 21 28 06 00 35 01 10 10 00 04 00 }
0x5B9ED: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5B9F4: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5B9FB: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5BA02: 			End  { 29 02 }
0x5BA04: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2822, VarStoreId: 0x6, VarOffset: 0x2D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AC 12 AE 12 22 28 06 00 D9 02 10 10 00 02 00 }
0x5BA15: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BA1C: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5BA23: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5BA2A: 			End  { 29 02 }
0x5BA2C: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE8F, VarStoreId: 0x6, VarOffset: 0x2F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CB 12 CD 12 8F 0E 06 00 F5 02 10 10 00 01 00 }
0x5BA3D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BA44: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BA4B: 			End  { 29 02 }
0x5BA4D: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xE90, VarStoreId: 0x6, VarOffset: 0x311, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 12 A7 0E 90 0E 06 00 11 03 10 10 00 01 00 }
0x5BA5E: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BA65: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BA6C: 			End  { 29 02 }
0x5BA6E: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2823, VarStoreId: 0x6, VarOffset: 0x32D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 04 13 06 13 23 28 06 00 2D 03 10 10 00 01 00 }
0x5BA7F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BA86: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BA8D: 			End  { 29 02 }
0x5BA8F: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE91, VarStoreId: 0x6, VarOffset: 0x349, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 21 13 23 13 91 0E 06 00 49 03 10 10 00 01 00 }
0x5BAA0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BAA7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BAAE: 			End  { 29 02 }
0x5BAB0: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xE92, VarStoreId: 0x6, VarOffset: 0x365, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 13 40 13 92 0E 06 00 65 03 10 10 00 01 00 }
0x5BAC1: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BAC8: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BACF: 			End  { 29 02 }
0x5BAD1: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE93, VarStoreId: 0x6, VarOffset: 0x151, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 97 13 99 13 93 0E 06 00 51 01 10 10 00 01 00 }
0x5BAE2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BAE9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BAF0: 			End  { 29 02 }
0x5BAF2: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE94, VarStoreId: 0x6, VarOffset: 0x16D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 13 B6 13 94 0E 06 00 6D 01 10 10 00 01 00 }
0x5BB03: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BB0A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BB11: 			End  { 29 02 }
0x5BB13: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE95, VarStoreId: 0x6, VarOffset: 0x189, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D1 13 D3 13 95 0E 06 00 89 01 10 10 00 01 00 }
0x5BB24: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BB2B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BB32: 			End  { 29 02 }
0x5BB34: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE96, VarStoreId: 0x6, VarOffset: 0x1A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EE 13 F0 13 96 0E 06 00 A5 01 10 10 00 01 00 }
0x5BB45: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BB4C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BB53: 			End  { 29 02 }
0x5BB55: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE97, VarStoreId: 0x6, VarOffset: 0x1F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0F 14 11 14 97 0E 06 00 F9 01 10 10 00 01 00 }
0x5BB66: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BB6D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BB74: 			End  { 29 02 }
0x5BB76: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE98, VarStoreId: 0x6, VarOffset: 0x215, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2C 14 2E 14 98 0E 06 00 15 02 10 10 00 01 00 }
0x5BB87: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BB8E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BB95: 			End  { 29 02 }
0x5BB97: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE99, VarStoreId: 0x6, VarOffset: 0x231, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 49 14 4B 14 99 0E 06 00 31 02 10 10 00 01 00 }
0x5BBA8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BBAF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BBB6: 			End  { 29 02 }
0x5BBB8: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE9A, VarStoreId: 0x6, VarOffset: 0x24D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 66 14 68 14 9A 0E 06 00 4D 02 10 10 00 01 00 }
0x5BBC9: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BBD0: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BBD7: 			End  { 29 02 }
0x5BBD9: 			GrayOutIf  { 19 82 }
0x5BBDB: 				EqIdVal QuestionId: 0xE8E, Value: 0x0 { 12 06 8E 0E 00 00 }
0x5BBE1: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE9B, VarStoreId: 0x6, VarOffset: 0x269, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 83 14 85 14 9B 0E 06 00 69 02 10 10 00 01 00 }
0x5BBF2: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BBF9: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BC00: 				End  { 29 02 }
0x5BC02: 			End  { 29 02 }
0x5BC04: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE9C, VarStoreId: 0x6, VarOffset: 0x285, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 14 A2 14 9C 0E 06 00 85 02 10 10 00 01 00 }
0x5BC15: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BC1C: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BC23: 			End  { 29 02 }
0x5BC25: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xE9D, VarStoreId: 0x6, VarOffset: 0x2A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5D 13 5F 13 9D 0E 06 00 A1 02 10 10 00 04 00 }
0x5BC36: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5BC3D: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5BC44: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5BC4B: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5BC52: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5BC59: 			End  { 29 02 }
0x5BC5B: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xE9E, VarStoreId: 0x6, VarOffset: 0x2BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E0 14 E2 14 9E 0E 06 00 BD 02 10 10 00 01 00 }
0x5BC6C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BC73: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BC7A: 			End  { 29 02 }
0x5BC7C: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xE9F, VarStoreId: 0x6, VarOffset: 0x3B7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 FD 14 FF 14 9F 0E 06 00 B7 03 00 11 00 00 FF FF 01 00 }
0x5BC90: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5BC97: 			End  { 29 02 }
0x5BC99: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xEA0, VarStoreId: 0x6, VarOffset: 0x539, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 1A 15 1C 15 A0 0E 06 00 39 05 00 10 00 07 01 }
0x5BCAA: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5BCB0: 			End  { 29 02 }
0x5BCB2: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xEA1, VarStoreId: 0x6, VarOffset: 0x56F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 37 15 39 15 A1 0E 06 00 6F 05 00 11 01 00 14 00 01 00 }
0x5BCC6: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5BCCD: 			End  { 29 02 }
0x5BCCF: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xEA2, VarStoreId: 0x6, VarOffset: 0x58D, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 54 15 56 15 A2 0E 06 00 8D 05 00 10 04 14 04 }
0x5BCE0: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5BCE6: 			End  { 29 02 }
0x5BCE8: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5BCEF: 			End  { 29 02 }
0x5BCF1: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5BCF8: 			End  { 29 02 }
0x5BCFA: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xEA3, VarStoreId: 0x6, VarOffset: 0x3FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 78 15 7A 15 A3 0E 06 00 FD 03 10 10 00 01 00 }
0x5BD0B: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BD12: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BD19: 			End  { 29 02 }
0x5BD1B: 			SuppressIf  { 0A 82 }
0x5BD1D: 				EqIdVal QuestionId: 0xEA3, Value: 0x0 { 12 06 A3 0E 00 00 }
0x5BD23: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xEA4, VarStoreId: 0x6, VarOffset: 0x435, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 17 16 23 16 A4 0E 06 00 35 04 10 10 00 02 00 }
0x5BD34: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BD3B: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5BD42: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5BD49: 				End  { 29 02 }
0x5BD4B: 				SuppressIf  { 0A 82 }
0x5BD4D: 					EqIdVal QuestionId: 0xEA4, Value: 0x1 { 12 86 A4 0E 01 00 }
0x5BD53: 						Not  { 17 02 }
0x5BD55: 					End  { 29 02 }
0x5BD57: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEA5, VarStoreId: 0x6, VarOffset: 0x4BF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 19 16 25 16 A5 0E 06 00 BF 04 10 11 00 00 FF 03 01 00 }
0x5BD6B: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5BD72: 					End  { 29 02 }
0x5BD74: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEA6, VarStoreId: 0x6, VarOffset: 0x451, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 1A 16 26 16 A6 0E 06 00 51 04 10 10 00 05 00 }
0x5BD85: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5BD8C: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5BD93: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5BD9A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5BDA1: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5BDA8: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5BDAF: 					End  { 29 02 }
0x5BDB1: 				End  { 29 02 }
0x5BDB3: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xEA7, VarStoreId: 0x6, VarOffset: 0x46D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 18 16 24 16 A7 0E 06 00 6D 04 10 10 00 02 00 }
0x5BDC4: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BDCB: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5BDD2: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5BDD9: 				End  { 29 02 }
0x5BDDB: 				SuppressIf  { 0A 82 }
0x5BDDD: 					EqIdVal QuestionId: 0xEA7, Value: 0x1 { 12 86 A7 0E 01 00 }
0x5BDE3: 						Not  { 17 02 }
0x5BDE5: 					End  { 29 02 }
0x5BDE7: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEA8, VarStoreId: 0x6, VarOffset: 0x4F7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 1B 16 27 16 A8 0E 06 00 F7 04 10 11 00 00 FF 03 01 00 }
0x5BDFB: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5BE02: 					End  { 29 02 }
0x5BE04: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEA9, VarStoreId: 0x6, VarOffset: 0x489, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 1C 16 28 16 A9 0E 06 00 89 04 10 10 00 05 00 }
0x5BE15: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5BE1C: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5BE23: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5BE2A: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5BE31: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5BE38: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5BE3F: 					End  { 29 02 }
0x5BE41: 				End  { 29 02 }
0x5BE43: 			End  { 29 02 }
0x5BE45: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5BE4C: 			End  { 29 02 }
0x5BE4E: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xEAA, VarStoreId: 0x6, VarOffset: 0x419, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 43 16 45 16 AA 0E 06 00 19 04 10 10 00 01 00 }
0x5BE5F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BE66: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BE6D: 			End  { 29 02 }
0x5BE6F: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xEAB, VarStoreId: 0x6, VarOffset: 0xD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 14 C3 14 AB 0E 06 00 D8 00 10 10 00 01 00 }
0x5BE80: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BE87: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BE8E: 			End  { 29 02 }
0x5BE90: 		End  { 29 02 }
0x5BE92: 	End  { 29 02 }
0x5BE94: 	Form FormId: 0x284B, Title: "PCI Express Root Port 28" { 01 86 4B 28 91 16 }
0x5BE9A: 		OneOf Prompt: "PCI Express Root Port 28", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0xEAC, VarStoreId: 0x6, VarOffset: 0x11A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 7B 13 7C 13 AC 0E 06 00 1A 01 10 10 00 01 00 }
0x5BEAB: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BEB2: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BEB9: 		End  { 29 02 }
0x5BEBB: 		SuppressIf  { 0A 82 }
0x5BEBD: 			EqIdVal QuestionId: 0xEAC, Value: 0x0 { 12 06 AC 0E 00 00 }
0x5BEC3: 			GrayOutIf  { 19 82 }
0x5BEC5: 				EqIdVal QuestionId: 0xEBA, Value: 0x1 { 12 06 BA 0E 01 00 }
0x5BECB: 				OneOf Prompt: "Connection Type", Help: "Built-In: a built-in device is connected to this rootport. SlotImplemented bit will be clear. Slot: this rootport connects to user-accessible slot. SlotImplemented bit will be set.", QuestionFlags: 0x10, QuestionId: 0xEAD, VarStoreId: 0x6, VarOffset: 0x382, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3B 17 E5 0E AD 0E 06 00 82 03 10 10 00 01 00 }
0x5BEDC: 					OneOfOption Option: "Built-in" Value: 0 { 09 07 E6 0E 00 00 00 }
0x5BEE3: 					OneOfOption Option: "Slot" Value: 1, Default { 09 07 E7 0E 10 00 01 }
0x5BEEA: 				End  { 29 02 }
0x5BEEC: 			End  { 29 02 }
0x5BEEE: 			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x2824, VarStoreId: 0x6, VarOffset: 0x136, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 91 12 F5 0D 24 28 06 00 36 01 10 10 00 04 00 }
0x5BEFF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BF06: 				OneOfOption Option: "L1" Value: 2, Default { 09 07 FC 0E 10 00 02 }
0x5BF0D: 				OneOfOption Option: "Auto" Value: 4 { 09 07 90 00 00 00 04 }
0x5BF14: 			End  { 29 02 }
0x5BF16: 			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x2825, VarStoreId: 0x6, VarOffset: 0x2DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 AD 12 AE 12 25 28 06 00 DA 02 10 10 00 02 00 }
0x5BF27: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BF2E: 				OneOfOption Option: "L1.1" Value: 1 { 09 07 AF 12 00 00 01 }
0x5BF35: 				OneOfOption Option: "L1.1 & L1.2" Value: 2, Default, MfgDefault { 09 07 B0 12 30 00 02 }
0x5BF3C: 			End  { 29 02 }
0x5BF3E: 			OneOf Prompt: "L1 Low", Help: "PCI Express L1 Low Substate Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEAE, VarStoreId: 0x6, VarOffset: 0x2F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CC 12 CD 12 AE 0E 06 00 F6 02 10 10 00 01 00 }
0x5BF4F: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BF56: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BF5D: 			End  { 29 02 }
0x5BF5F: 			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0xEAF, VarStoreId: 0x6, VarOffset: 0x312, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 12 A7 0E AF 0E 06 00 12 03 10 10 00 01 00 }
0x5BF70: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BF77: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BF7E: 			End  { 29 02 }
0x5BF80: 			OneOf Prompt: "PTM", Help: "Enable/Disable Precision Time Measurement", QuestionFlags: 0x10, QuestionId: 0x2826, VarStoreId: 0x6, VarOffset: 0x32E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 05 13 06 13 26 28 06 00 2E 03 10 10 00 01 00 }
0x5BF91: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BF98: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BF9F: 			End  { 29 02 }
0x5BFA1: 			OneOf Prompt: "DPC", Help: "Enable/Disable Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xEB0, VarStoreId: 0x6, VarOffset: 0x34A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 22 13 23 13 B0 0E 06 00 4A 03 10 10 00 01 00 }
0x5BFB2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BFB9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5BFC0: 			End  { 29 02 }
0x5BFC2: 			OneOf Prompt: "EDPC", Help: "Enable/Disable Rootport extensions for Downstream Port Containment", QuestionFlags: 0x10, QuestionId: 0xEB1, VarStoreId: 0x6, VarOffset: 0x366, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3F 13 40 13 B1 0E 06 00 66 03 10 10 00 01 00 }
0x5BFD3: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5BFDA: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5BFE1: 			End  { 29 02 }
0x5BFE3: 			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB2, VarStoreId: 0x6, VarOffset: 0x152, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 98 13 99 13 B2 0E 06 00 52 01 10 10 00 01 00 }
0x5BFF4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5BFFB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C002: 			End  { 29 02 }
0x5C004: 			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB3, VarStoreId: 0x6, VarOffset: 0x16E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 13 B6 13 B3 0E 06 00 6E 01 10 10 00 01 00 }
0x5C015: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C01C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C023: 			End  { 29 02 }
0x5C025: 			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB4, VarStoreId: 0x6, VarOffset: 0x18A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 D2 13 D3 13 B4 0E 06 00 8A 01 10 10 00 01 00 }
0x5C036: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C03D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C044: 			End  { 29 02 }
0x5C046: 			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB5, VarStoreId: 0x6, VarOffset: 0x1A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 EF 13 F0 13 B5 0E 06 00 A6 01 10 10 00 01 00 }
0x5C057: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C05E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C065: 			End  { 29 02 }
0x5C067: 			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB6, VarStoreId: 0x6, VarOffset: 0x1FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 10 14 11 14 B6 0E 06 00 FA 01 10 10 00 01 00 }
0x5C078: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C07F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C086: 			End  { 29 02 }
0x5C088: 			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB7, VarStoreId: 0x6, VarOffset: 0x216, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2D 14 2E 14 B7 0E 06 00 16 02 10 10 00 01 00 }
0x5C099: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C0A0: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C0A7: 			End  { 29 02 }
0x5C0A9: 			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB8, VarStoreId: 0x6, VarOffset: 0x232, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4A 14 4B 14 B8 0E 06 00 32 02 10 10 00 01 00 }
0x5C0BA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C0C1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C0C8: 			End  { 29 02 }
0x5C0CA: 			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEB9, VarStoreId: 0x6, VarOffset: 0x24E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 67 14 68 14 B9 0E 06 00 4E 02 10 10 00 01 00 }
0x5C0DB: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5C0E2: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5C0E9: 			End  { 29 02 }
0x5C0EB: 			GrayOutIf  { 19 82 }
0x5C0ED: 				EqIdVal QuestionId: 0xEAD, Value: 0x0 { 12 06 AD 0E 00 00 }
0x5C0F3: 				OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEBA, VarStoreId: 0x6, VarOffset: 0x26A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 14 85 14 BA 0E 06 00 6A 02 10 10 00 01 00 }
0x5C104: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C10B: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C112: 				End  { 29 02 }
0x5C114: 			End  { 29 02 }
0x5C116: 			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEBB, VarStoreId: 0x6, VarOffset: 0x286, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 14 A2 14 BB 0E 06 00 86 02 10 10 00 01 00 }
0x5C127: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5C12E: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5C135: 			End  { 29 02 }
0x5C137: 			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0xEBC, VarStoreId: 0x6, VarOffset: 0x2A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 5E 13 5F 13 BC 0E 06 00 A2 02 10 10 00 04 00 }
0x5C148: 				OneOfOption Option: "Auto" Value: 0, Default { 09 07 06 00 10 00 00 }
0x5C14F: 				OneOfOption Option: "Gen1" Value: 1 { 09 07 EC 0E 00 00 01 }
0x5C156: 				OneOfOption Option: "Gen2" Value: 2 { 09 07 ED 0E 00 00 02 }
0x5C15D: 				OneOfOption Option: "Gen3" Value: 3 { 09 07 D6 0E 00 00 03 }
0x5C164: 				OneOfOption Option: "Gen4" Value: 4 { 09 07 D7 0E 00 00 04 }
0x5C16B: 			End  { 29 02 }
0x5C16D: 			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0xEBD, VarStoreId: 0x6, VarOffset: 0x2BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E1 14 E2 14 BD 0E 06 00 BE 02 10 10 00 01 00 }
0x5C17E: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C185: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C18C: 			End  { 29 02 }
0x5C18E: 			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0xEBE, VarStoreId: 0x6, VarOffset: 0x3B9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 FE 14 FF 14 BE 0E 06 00 B9 03 00 11 00 00 FF FF 01 00 }
0x5C1A2: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5C1A9: 			End  { 29 02 }
0x5C1AB: 			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xEBF, VarStoreId: 0x6, VarOffset: 0x53A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1 { 07 91 1B 15 1C 15 BF 0E 06 00 3A 05 00 10 00 07 01 }
0x5C1BC: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5C1C2: 			End  { 29 02 }
0x5C1C4: 			Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0xEC0, VarStoreId: 0x6, VarOffset: 0x571, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 38 15 39 15 C0 0E 06 00 71 05 00 11 01 00 14 00 01 00 }
0x5C1D8: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x5C1DF: 			End  { 29 02 }
0x5C1E1: 			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0xEC1, VarStoreId: 0x6, VarOffset: 0x58E, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4 { 07 91 55 15 56 15 C1 0E 06 00 8E 05 00 10 04 14 04 }
0x5C1F2: 				Default DefaultId: 0x0 Value: 4 { 5B 06 00 00 00 04 }
0x5C1F8: 			End  { 29 02 }
0x5C1FA: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5C201: 			End  { 29 02 }
0x5C203: 			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0 { 02 87 5D 15 00 00 00 }
0x5C20A: 			End  { 29 02 }
0x5C20C: 			OneOf Prompt: "LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xEC2, VarStoreId: 0x6, VarOffset: 0x3FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 79 15 7A 15 C2 0E 06 00 FE 03 10 10 00 01 00 }
0x5C21D: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5C224: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5C22B: 			End  { 29 02 }
0x5C22D: 			SuppressIf  { 0A 82 }
0x5C22F: 				EqIdVal QuestionId: 0xEC2, Value: 0x0 { 12 06 C2 0E 00 00 }
0x5C235: 				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xEC3, VarStoreId: 0x6, VarOffset: 0x436, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 1D 16 23 16 C3 0E 06 00 36 04 10 10 00 02 00 }
0x5C246: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5C24D: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5C254: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5C25B: 				End  { 29 02 }
0x5C25D: 				SuppressIf  { 0A 82 }
0x5C25F: 					EqIdVal QuestionId: 0xEC3, Value: 0x1 { 12 86 C3 0E 01 00 }
0x5C265: 						Not  { 17 02 }
0x5C267: 					End  { 29 02 }
0x5C269: 					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEC4, VarStoreId: 0x6, VarOffset: 0x4C1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 1F 16 25 16 C4 0E 06 00 C1 04 10 11 00 00 FF 03 01 00 }
0x5C27D: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5C284: 					End  { 29 02 }
0x5C286: 					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEC5, VarStoreId: 0x6, VarOffset: 0x452, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 20 16 26 16 C5 0E 06 00 52 04 10 10 00 05 00 }
0x5C297: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5C29E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5C2A5: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5C2AC: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5C2B3: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5C2BA: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5C2C1: 					End  { 29 02 }
0x5C2C3: 				End  { 29 02 }
0x5C2C5: 				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0xEC6, VarStoreId: 0x6, VarOffset: 0x46E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 1E 16 24 16 C6 0E 06 00 6E 04 10 10 00 02 00 }
0x5C2D6: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5C2DD: 					OneOfOption Option: "Manual" Value: 1 { 09 07 CA 07 00 00 01 }
0x5C2E4: 					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 90 00 30 00 02 }
0x5C2EB: 				End  { 29 02 }
0x5C2ED: 				SuppressIf  { 0A 82 }
0x5C2EF: 					EqIdVal QuestionId: 0xEC6, Value: 0x1 { 12 86 C6 0E 01 00 }
0x5C2F5: 						Not  { 17 02 }
0x5C2F7: 					End  { 29 02 }
0x5C2F9: 					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEC7, VarStoreId: 0x6, VarOffset: 0x4F9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1 { 07 94 21 16 27 16 C7 0E 06 00 F9 04 10 11 00 00 FF 03 01 00 }
0x5C30D: 						Default DefaultId: 0x0 Value: 60 { 5B 07 00 00 01 3C 00 }
0x5C314: 					End  { 29 02 }
0x5C316: 					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0xEC8, VarStoreId: 0x6, VarOffset: 0x48A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 22 16 28 16 C8 0E 06 00 8A 04 10 10 00 05 00 }
0x5C327: 						OneOfOption Option: "1 ns" Value: 0 { 09 07 57 15 00 00 00 }
0x5C32E: 						OneOfOption Option: "32 ns" Value: 1 { 09 07 58 15 00 00 01 }
0x5C335: 						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault { 09 07 59 15 30 00 02 }
0x5C33C: 						OneOfOption Option: "32768 ns" Value: 3 { 09 07 5A 15 00 00 03 }
0x5C343: 						OneOfOption Option: "1048576 ns" Value: 4 { 09 07 5B 15 00 00 04 }
0x5C34A: 						OneOfOption Option: "33554432 ns" Value: 5 { 09 07 5C 15 00 00 05 }
0x5C351: 					End  { 29 02 }
0x5C353: 				End  { 29 02 }
0x5C355: 			End  { 29 02 }
0x5C357: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5C35E: 			End  { 29 02 }
0x5C360: 			OneOf Prompt: "LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0xEC9, VarStoreId: 0x6, VarOffset: 0x41A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 44 16 45 16 C9 0E 06 00 1A 04 10 10 00 01 00 }
0x5C371: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C378: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C37F: 			End  { 29 02 }
0x5C381: 			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0xECA, VarStoreId: 0x6, VarOffset: 0xD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 14 C3 14 CA 0E 06 00 D9 00 10 10 00 01 00 }
0x5C392: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C399: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C3A0: 			End  { 29 02 }
0x5C3A2: 		End  { 29 02 }
0x5C3A4: 	End  { 29 02 }
0x5C3A6: 	Form FormId: 0x284C, Title: "PCIE clocks" { 01 86 4C 28 82 18 }
0x5C3AC: 		OneOf Prompt: "Clock0 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xECB, VarStoreId: 0x6, VarOffset: 0xDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 86 18 84 18 CB 0E 06 00 DB 00 10 10 00 02 00 }
0x5C3BD: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C3C4: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C3CB: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C3D2: 		End  { 29 02 }
0x5C3D4: 		OneOf Prompt: "ClkReq for Clock0", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xECC, VarStoreId: 0x6, VarOffset: 0xED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 98 18 85 18 CC 0E 06 00 ED 00 10 10 00 FF 00 }
0x5C3E5: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C3EC: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C3F3: 		End  { 29 02 }
0x5C3F5: 		OneOf Prompt: "Clock1 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xECD, VarStoreId: 0x6, VarOffset: 0xDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 87 18 84 18 CD 0E 06 00 DC 00 10 10 00 02 00 }
0x5C406: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C40D: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C414: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C41B: 		End  { 29 02 }
0x5C41D: 		OneOf Prompt: "ClkReq for Clock1", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xECE, VarStoreId: 0x6, VarOffset: 0xEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 99 18 85 18 CE 0E 06 00 EE 00 10 10 00 FF 00 }
0x5C42E: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C435: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C43C: 		End  { 29 02 }
0x5C43E: 		OneOf Prompt: "Clock2 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xECF, VarStoreId: 0x6, VarOffset: 0xDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 88 18 84 18 CF 0E 06 00 DD 00 10 10 00 02 00 }
0x5C44F: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C456: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C45D: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C464: 		End  { 29 02 }
0x5C466: 		OneOf Prompt: "ClkReq for Clock2", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xED0, VarStoreId: 0x6, VarOffset: 0xEF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9A 18 85 18 D0 0E 06 00 EF 00 10 10 00 FF 00 }
0x5C477: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C47E: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C485: 		End  { 29 02 }
0x5C487: 		OneOf Prompt: "Clock3 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xED1, VarStoreId: 0x6, VarOffset: 0xDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 89 18 84 18 D1 0E 06 00 DE 00 10 10 00 02 00 }
0x5C498: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C49F: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C4A6: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C4AD: 		End  { 29 02 }
0x5C4AF: 		OneOf Prompt: "ClkReq for Clock3", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xED2, VarStoreId: 0x6, VarOffset: 0xF0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9B 18 85 18 D2 0E 06 00 F0 00 10 10 00 FF 00 }
0x5C4C0: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C4C7: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C4CE: 		End  { 29 02 }
0x5C4D0: 		OneOf Prompt: "Clock4 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xED3, VarStoreId: 0x6, VarOffset: 0xDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8A 18 84 18 D3 0E 06 00 DF 00 10 10 00 02 00 }
0x5C4E1: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C4E8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C4EF: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C4F6: 		End  { 29 02 }
0x5C4F8: 		OneOf Prompt: "ClkReq for Clock4", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xED4, VarStoreId: 0x6, VarOffset: 0xF1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9C 18 85 18 D4 0E 06 00 F1 00 10 10 00 FF 00 }
0x5C509: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C510: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C517: 		End  { 29 02 }
0x5C519: 		OneOf Prompt: "Clock5 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xED5, VarStoreId: 0x6, VarOffset: 0xE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8B 18 84 18 D5 0E 06 00 E0 00 10 10 00 02 00 }
0x5C52A: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C531: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C538: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C53F: 		End  { 29 02 }
0x5C541: 		OneOf Prompt: "ClkReq for Clock5", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xED6, VarStoreId: 0x6, VarOffset: 0xF2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9D 18 85 18 D6 0E 06 00 F2 00 10 10 00 FF 00 }
0x5C552: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C559: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C560: 		End  { 29 02 }
0x5C562: 		OneOf Prompt: "Clock6 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xED7, VarStoreId: 0x6, VarOffset: 0xE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8C 18 84 18 D7 0E 06 00 E1 00 10 10 00 02 00 }
0x5C573: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C57A: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C581: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C588: 		End  { 29 02 }
0x5C58A: 		OneOf Prompt: "ClkReq for Clock6", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xED8, VarStoreId: 0x6, VarOffset: 0xF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9E 18 85 18 D8 0E 06 00 F3 00 10 10 00 FF 00 }
0x5C59B: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C5A2: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C5A9: 		End  { 29 02 }
0x5C5AB: 		OneOf Prompt: "Clock7 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xED9, VarStoreId: 0x6, VarOffset: 0xE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8D 18 84 18 D9 0E 06 00 E2 00 10 10 00 02 00 }
0x5C5BC: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C5C3: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C5CA: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C5D1: 		End  { 29 02 }
0x5C5D3: 		OneOf Prompt: "ClkReq for Clock7", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEDA, VarStoreId: 0x6, VarOffset: 0xF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 9F 18 85 18 DA 0E 06 00 F4 00 10 10 00 FF 00 }
0x5C5E4: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C5EB: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C5F2: 		End  { 29 02 }
0x5C5F4: 		OneOf Prompt: "Clock8 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEDB, VarStoreId: 0x6, VarOffset: 0xE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8E 18 84 18 DB 0E 06 00 E3 00 10 10 00 02 00 }
0x5C605: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C60C: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C613: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C61A: 		End  { 29 02 }
0x5C61C: 		OneOf Prompt: "ClkReq for Clock8", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEDC, VarStoreId: 0x6, VarOffset: 0xF5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A0 18 85 18 DC 0E 06 00 F5 00 10 10 00 FF 00 }
0x5C62D: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C634: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C63B: 		End  { 29 02 }
0x5C63D: 		OneOf Prompt: "Clock9 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEDD, VarStoreId: 0x6, VarOffset: 0xE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 8F 18 84 18 DD 0E 06 00 E4 00 10 10 00 02 00 }
0x5C64E: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C655: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C65C: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C663: 		End  { 29 02 }
0x5C665: 		OneOf Prompt: "ClkReq for Clock9", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEDE, VarStoreId: 0x6, VarOffset: 0xF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A1 18 85 18 DE 0E 06 00 F6 00 10 10 00 FF 00 }
0x5C676: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C67D: 			OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C684: 		End  { 29 02 }
0x5C686: 		SuppressIf  { 0A 82 }
0x5C688: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 06 12 11 02 00 }
0x5C68E: 			OneOf Prompt: "Clock10 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEDF, VarStoreId: 0x6, VarOffset: 0xE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 90 18 84 18 DF 0E 06 00 E5 00 10 10 00 02 00 }
0x5C69F: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C6A6: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C6AD: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C6B4: 			End  { 29 02 }
0x5C6B6: 			OneOf Prompt: "ClkReq for Clock10", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEE0, VarStoreId: 0x6, VarOffset: 0xF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A2 18 85 18 E0 0E 06 00 F7 00 10 10 00 FF 00 }
0x5C6C7: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C6CE: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C6D5: 			End  { 29 02 }
0x5C6D7: 			OneOf Prompt: "Clock11 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEE1, VarStoreId: 0x6, VarOffset: 0xE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 91 18 84 18 E1 0E 06 00 E6 00 10 10 00 02 00 }
0x5C6E8: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C6EF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C6F6: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C6FD: 			End  { 29 02 }
0x5C6FF: 			OneOf Prompt: "ClkReq for Clock11", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEE2, VarStoreId: 0x6, VarOffset: 0xF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A3 18 85 18 E2 0E 06 00 F8 00 10 10 00 FF 00 }
0x5C710: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C717: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C71E: 			End  { 29 02 }
0x5C720: 			OneOf Prompt: "Clock12 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEE3, VarStoreId: 0x6, VarOffset: 0xE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 92 18 84 18 E3 0E 06 00 E7 00 10 10 00 02 00 }
0x5C731: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C738: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C73F: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C746: 			End  { 29 02 }
0x5C748: 			OneOf Prompt: "ClkReq for Clock12", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEE4, VarStoreId: 0x6, VarOffset: 0xF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A4 18 85 18 E4 0E 06 00 F9 00 10 10 00 FF 00 }
0x5C759: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C760: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C767: 			End  { 29 02 }
0x5C769: 			OneOf Prompt: "Clock13 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEE5, VarStoreId: 0x6, VarOffset: 0xE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 93 18 84 18 E5 0E 06 00 E8 00 10 10 00 02 00 }
0x5C77A: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C781: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C788: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C78F: 			End  { 29 02 }
0x5C791: 			OneOf Prompt: "ClkReq for Clock13", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEE6, VarStoreId: 0x6, VarOffset: 0xFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A5 18 85 18 E6 0E 06 00 FA 00 10 10 00 FF 00 }
0x5C7A2: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C7A9: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C7B0: 			End  { 29 02 }
0x5C7B2: 			OneOf Prompt: "Clock14 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEE7, VarStoreId: 0x6, VarOffset: 0xE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 94 18 84 18 E7 0E 06 00 E9 00 10 10 00 02 00 }
0x5C7C3: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C7CA: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C7D1: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C7D8: 			End  { 29 02 }
0x5C7DA: 			OneOf Prompt: "ClkReq for Clock14", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEE8, VarStoreId: 0x6, VarOffset: 0xFB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A6 18 85 18 E8 0E 06 00 FB 00 10 10 00 FF 00 }
0x5C7EB: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C7F2: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C7F9: 			End  { 29 02 }
0x5C7FB: 			OneOf Prompt: "Clock15 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEE9, VarStoreId: 0x6, VarOffset: 0xEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 95 18 84 18 E9 0E 06 00 EA 00 10 10 00 02 00 }
0x5C80C: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C813: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C81A: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C821: 			End  { 29 02 }
0x5C823: 			OneOf Prompt: "ClkReq for Clock15", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEEA, VarStoreId: 0x6, VarOffset: 0xFC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A7 18 85 18 EA 0E 06 00 FC 00 10 10 00 FF 00 }
0x5C834: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C83B: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C842: 			End  { 29 02 }
0x5C844: 			OneOf Prompt: "Clock16 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEEB, VarStoreId: 0x6, VarOffset: 0xEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 96 18 84 18 EB 0E 06 00 EB 00 10 10 00 02 00 }
0x5C855: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C85C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C863: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C86A: 			End  { 29 02 }
0x5C86C: 			OneOf Prompt: "ClkReq for Clock16", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEEC, VarStoreId: 0x6, VarOffset: 0xFD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A8 18 85 18 EC 0E 06 00 FD 00 10 10 00 FF 00 }
0x5C87D: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C884: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C88B: 			End  { 29 02 }
0x5C88D: 			OneOf Prompt: "Clock17 assignment", Help: "Platform-POR = clock is assigned to PCIe port or LAN according to board layout. Enabled = keep clock enabledeven if unused. Disabled = Disable clock.", QuestionFlags: 0x10, QuestionId: 0xEED, VarStoreId: 0x6, VarOffset: 0xEC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 97 18 84 18 ED 0E 06 00 EC 00 10 10 00 02 00 }
0x5C89E: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C8A5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C8AC: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 04 00 00 00 02 }
0x5C8B3: 			End  { 29 02 }
0x5C8B5: 			OneOf Prompt: "ClkReq for Clock17", Help: "Platform-POR = CLKREQ signal is assigned to CLKSRC according to board layout. Disabled = CLKREQ will not be used.", QuestionFlags: 0x10, QuestionId: 0xEEE, VarStoreId: 0x6, VarOffset: 0xFE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 05 91 A9 18 85 18 EE 0E 06 00 FE 00 10 10 00 FF 00 }
0x5C8C6: 				OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x5C8CD: 				OneOfOption Option: "Disabled" Value: 255 { 09 07 04 00 00 00 FF }
0x5C8D4: 			End  { 29 02 }
0x5C8D6: 		End  { 29 02 }
0x5C8D8: 	End  { 29 02 }
0x5C8DA: 	Form FormId: 0x284D, Title: "THC Configuration" { 01 86 4D 28 08 12 }
0x5C8E0: 		SuppressIf  { 0A 82 }
0x5C8E2: 			EqIdVal QuestionId: 0x1123, Value: 0x0 { 12 06 23 11 00 00 }
0x5C8E8: 			Subtitle Prompt: "Touch Host Controller Configuration Settings", Help: "", Flags: 0x0 { 02 87 09 12 00 00 00 }
0x5C8EF: 			End  { 29 02 }
0x5C8F1: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5C8F8: 			End  { 29 02 }
0x5C8FA: 			OneOf Prompt: "THC Port Configuration", Help: "Assign Port to THC", QuestionFlags: 0x10, QuestionId: 0xEEF, VarStoreId: 0x6, VarOffset: 0x518, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 0B 12 0C 12 EF 0E 06 00 18 05 10 10 00 01 00 }
0x5C90B: 				OneOfOption Option: "None" Value: 0, Default, MfgDefault { 09 07 0D 12 30 00 00 }
0x5C912: 				OneOfOption Option: "THC0" Value: 1 { 09 07 0E 12 00 00 01 }
0x5C919: 			End  { 29 02 }
0x5C91B: 			SuppressIf  { 0A 82 }
0x5C91D: 				EqIdVal QuestionId: 0xEEF, Value: 0x0 { 12 06 EF 0E 00 00 }
0x5C923: 				OneOf Prompt: "Port Clock", Help: "SPI_DFX_CLK_EN BIT set to 0 or 1", QuestionFlags: 0x10, QuestionId: 0xEF0, VarStoreId: 0x6, VarOffset: 0x519, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 11 12 10 12 F0 0E 06 00 19 05 10 10 00 01 00 }
0x5C934: 					OneOfOption Option: "Functional" Value: 0, Default, MfgDefault { 09 07 12 12 30 00 00 }
0x5C93B: 					OneOfOption Option: "DFX" Value: 1 { 09 07 13 12 00 00 01 }
0x5C942: 				End  { 29 02 }
0x5C944: 				Numeric Prompt: "Active LTR", Help: "Expose Active LTR data through ACPI _DSM for OS driver to configure", QuestionFlags: 0x10, QuestionId: 0xEF1, VarStoreId: 0x6, VarOffset: 0x794, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 1A 12 1B 12 F1 0E 06 00 94 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5C95E: 					Default DefaultId: 0x0 Value: 4294967295 { 5B 09 00 00 02 FF FF FF FF }
0x5C967: 				End  { 29 02 }
0x5C969: 				Numeric Prompt: "Idle LTR", Help: "Expose Idle LTR data through ACPI _DSM for OS driver to configure", QuestionFlags: 0x10, QuestionId: 0xEF2, VarStoreId: 0x6, VarOffset: 0x79C, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 1C 12 1D 12 F2 0E 06 00 9C 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5C983: 					Default DefaultId: 0x0 Value: 4294967295 { 5B 09 00 00 02 FF FF FF FF }
0x5C98C: 				End  { 29 02 }
0x5C98E: 				Numeric Prompt: "HID Over SPI Limit Packet Size", Help: "When set, limits SPI read & write packet size to 64B. Otherwise, THC uses Max Soc packet size for SPI Read and Write 
0 - Max Soc Packet Size 
1 - 64 Bytes", QuestionFlags: 0x10, QuestionId: 0xEF3, VarStoreId: 0x6, VarOffset: 0x7A4, Flags: 0x22, Size: 32, Min: 0x0, Max: 0x1, Step: 0x1 { 07 9A 20 12 21 12 F3 0E 06 00 A4 07 10 22 00 00 00 00 01 00 00 00 01 00 00 00 }
0x5C9A8: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5C9B1: 				End  { 29 02 }
0x5C9B3: 				Numeric Prompt: "Hid Over Spi Performance Limitation", Help: "Minimum amount of delay the driver must wait between end of write operation and begin of read operation. This value shall be in 10us multiples
 0-Disabled
 1-65535 (0xFFFF) up to 655350us", QuestionFlags: 0x10, QuestionId: 0xEF4, VarStoreId: 0x6, VarOffset: 0x7AC, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 9A 22 12 23 12 F4 0E 06 00 AC 07 10 22 00 00 00 00 FF FF 00 00 01 00 00 00 }
0x5C9CD: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5C9D6: 				End  { 29 02 }
0x5C9D8: 				OneOf Prompt: "Wake On Touch", Help: "Based on this setting vGPIO for given THC will be in native mode, and additional _CRS for wake will be exposed in ACPI", QuestionFlags: 0x10, QuestionId: 0xEF5, VarStoreId: 0x6, VarOffset: 0x51A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 14 12 15 12 F5 0E 06 00 1A 05 10 10 00 01 00 }
0x5C9E9: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5C9F0: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5C9F7: 				End  { 29 02 }
0x5C9F9: 				OneOf Prompt: "THC Mode", Help: "Switch between Intel THC protcol and Industry standard HID Over SPI protocol.", QuestionFlags: 0x10, QuestionId: 0xEF6, VarStoreId: 0x6, VarOffset: 0x792, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 16 12 17 12 F6 0E 06 00 92 07 10 10 00 01 00 }
0x5CA0A: 					OneOfOption Option: "THC" Value: 0, Default, MfgDefault { 09 07 18 12 30 00 00 }
0x5CA11: 					OneOfOption Option: "HID over SPI" Value: 1 { 09 07 19 12 00 00 01 }
0x5CA18: 				End  { 29 02 }
0x5CA1A: 				SuppressIf  { 0A 82 }
0x5CA1C: 					EqIdVal QuestionId: 0xEF6, Value: 0x0 { 12 06 F6 0E 00 00 }
0x5CA22: 					Numeric Prompt: "Connection Speed", Help: "HID Over SPI Connection Speed in Hz", QuestionFlags: 0x10, QuestionId: 0xEF7, VarStoreId: 0x6, VarOffset: 0x7BC, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x2625A00, Step: 0x1 { 07 9A 1E 12 1F 12 F7 0E 06 00 BC 07 10 12 00 00 00 00 00 5A 62 02 01 00 00 00 }
0x5CA3C: 						Default DefaultId: 0x0 Value: 17000000 { 5B 09 00 00 02 40 66 03 01 }
0x5CA45: 					End  { 29 02 }
0x5CA47: 					OneOf Prompt: "Flags", Help: "HID Over SPI Flags", QuestionFlags: 0x10, QuestionId: 0xEF8, VarStoreId: 0x6, VarOffset: 0x7B4, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x8000, Step: 0x0 { 05 9A 24 12 25 12 F8 0E 06 00 B4 07 10 12 00 00 00 00 00 80 00 00 00 00 00 00 }
0x5CA61: 						OneOfOption Option: "Single SPI Mode" Value: 0, Default, MfgDefault { 09 0A 26 12 32 02 00 00 00 00 }
0x5CA6B: 						OneOfOption Option: "Dual SPI Mode" Value: 16384 { 09 0A 27 12 02 02 00 40 00 00 }
0x5CA75: 						OneOfOption Option: "Quad SPI Mode" Value: 32768 { 09 0A 28 12 02 02 00 80 00 00 }
0x5CA7F: 					End  { 29 02 }
0x5CA81: 					Numeric Prompt: "Input Report Body Address", Help: "HID Over SPI Input Report Body Address", QuestionFlags: 0x10, QuestionId: 0xEF9, VarStoreId: 0x6, VarOffset: 0x7C4, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 29 12 2A 12 F9 0E 06 00 C4 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CA9B: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CAA4: 					End  { 29 02 }
0x5CAA6: 					Numeric Prompt: "Input Report Header Address", Help: "HID Over SPI Input Report Header Address", QuestionFlags: 0x10, QuestionId: 0xEFA, VarStoreId: 0x6, VarOffset: 0x7CC, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 2B 12 2C 12 FA 0E 06 00 CC 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CAC0: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CAC9: 					End  { 29 02 }
0x5CACB: 					Numeric Prompt: "Output Report Address", Help: "HID Over SPI Output Report Address", QuestionFlags: 0x10, QuestionId: 0xEFB, VarStoreId: 0x6, VarOffset: 0x7D4, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 2D 12 2E 12 FB 0E 06 00 D4 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CAE5: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CAEE: 					End  { 29 02 }
0x5CAF0: 					Numeric Prompt: "Write Opcode", Help: "HID Over SPI Write Opcode", QuestionFlags: 0x10, QuestionId: 0xEFC, VarStoreId: 0x6, VarOffset: 0x7E4, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 2F 12 30 12 FC 0E 06 00 E4 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CB0A: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CB13: 					End  { 29 02 }
0x5CB15: 					Numeric Prompt: "Read Opcode", Help: "HID Over SPI Read Opcode", QuestionFlags: 0x10, QuestionId: 0xEFD, VarStoreId: 0x6, VarOffset: 0x7DC, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A 31 12 32 12 FD 0E 06 00 DC 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CB2F: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CB38: 					End  { 29 02 }
0x5CB3A: 					OneOf Prompt: "Reset Pad Trigger", Help: "HID Over SPI Reset Pad Trigger", QuestionFlags: 0x10, QuestionId: 0xEFE, VarStoreId: 0x6, VarOffset: 0x7EC, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x1, Step: 0x0 { 05 9A 33 12 34 12 FE 0E 06 00 EC 07 10 12 00 00 00 00 01 00 00 00 00 00 00 00 }
0x5CB54: 						OneOfOption Option: "Low" Value: 0, Default, MfgDefault { 09 0A 35 12 32 02 00 00 00 00 }
0x5CB5E: 						OneOfOption Option: "High" Value: 1 { 09 0A 36 12 02 02 01 00 00 00 }
0x5CB68: 					End  { 29 02 }
0x5CB6A: 				End  { 29 02 }
0x5CB6C: 			End  { 29 02 }
0x5CB6E: 			OneOf Prompt: "THC Port Configuration", Help: "Assign Port to THC", QuestionFlags: 0x10, QuestionId: 0xEFF, VarStoreId: 0x6, VarOffset: 0x51B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 A2 19 0C 12 FF 0E 06 00 1B 05 10 10 00 02 00 }
0x5CB7F: 				OneOfOption Option: "None" Value: 0, Default, MfgDefault { 09 07 0D 12 30 00 00 }
0x5CB86: 				OneOfOption Option: "THC1" Value: 2 { 09 07 0F 12 00 00 02 }
0x5CB8D: 			End  { 29 02 }
0x5CB8F: 			SuppressIf  { 0A 82 }
0x5CB91: 				EqIdVal QuestionId: 0xEFF, Value: 0x0 { 12 06 FF 0E 00 00 }
0x5CB97: 				OneOf Prompt: "Port Clock", Help: "SPI_DFX_CLK_EN BIT set to 0 or 1", QuestionFlags: 0x10, QuestionId: 0xF00, VarStoreId: 0x6, VarOffset: 0x51C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A3 19 10 12 00 0F 06 00 1C 05 10 10 00 01 00 }
0x5CBA8: 					OneOfOption Option: "Functional" Value: 0, Default, MfgDefault { 09 07 12 12 30 00 00 }
0x5CBAF: 					OneOfOption Option: "DFX" Value: 1 { 09 07 13 12 00 00 01 }
0x5CBB6: 				End  { 29 02 }
0x5CBB8: 				Numeric Prompt: "Active LTR", Help: "Expose Active LTR data through ACPI _DSM for OS driver to configure", QuestionFlags: 0x10, QuestionId: 0xF01, VarStoreId: 0x6, VarOffset: 0x798, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A A4 19 1B 12 01 0F 06 00 98 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CBD2: 					Default DefaultId: 0x0 Value: 4294967295 { 5B 09 00 00 02 FF FF FF FF }
0x5CBDB: 				End  { 29 02 }
0x5CBDD: 				Numeric Prompt: "Idle LTR", Help: "Expose Idle LTR data through ACPI _DSM for OS driver to configure", QuestionFlags: 0x10, QuestionId: 0xF02, VarStoreId: 0x6, VarOffset: 0x7A0, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A A5 19 1D 12 02 0F 06 00 A0 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CBF7: 					Default DefaultId: 0x0 Value: 4294967295 { 5B 09 00 00 02 FF FF FF FF }
0x5CC00: 				End  { 29 02 }
0x5CC02: 				Numeric Prompt: "HID Over SPI Limit Packet Size", Help: "When set, limits SPI read & write packet size to 64B. Otherwise, THC uses Max Soc packet size for SPI Read and Write 
0 - Max Soc Packet Size 
1 - 64 Bytes", QuestionFlags: 0x10, QuestionId: 0xF03, VarStoreId: 0x6, VarOffset: 0x7A8, Flags: 0x22, Size: 32, Min: 0x0, Max: 0x1, Step: 0x1 { 07 9A A6 19 21 12 03 0F 06 00 A8 07 10 22 00 00 00 00 01 00 00 00 01 00 00 00 }
0x5CC1C: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CC25: 				End  { 29 02 }
0x5CC27: 				Numeric Prompt: "Hid Over Spi Performance Limitation", Help: "Minimum amount of delay the driver must wait between end of write operation and begin of read operation. This value shall be in 10us multiples
 0-Disabled
 1-65535 (0xFFFF) up to 655350us", QuestionFlags: 0x10, QuestionId: 0xF04, VarStoreId: 0x6, VarOffset: 0x7B0, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 9A A7 19 23 12 04 0F 06 00 B0 07 10 22 00 00 00 00 FF FF 00 00 01 00 00 00 }
0x5CC41: 					Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CC4A: 				End  { 29 02 }
0x5CC4C: 				OneOf Prompt: "Wake On Touch", Help: "Based on this setting vGPIO for given THC will be in native mode, and additional _CRS for wake will be exposed in ACPI", QuestionFlags: 0x10, QuestionId: 0xF05, VarStoreId: 0x6, VarOffset: 0x51D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 19 15 12 05 0F 06 00 1D 05 10 10 00 01 00 }
0x5CC5D: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5CC64: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5CC6B: 				End  { 29 02 }
0x5CC6D: 				OneOf Prompt: "THC Mode", Help: "Switch between Intel THC protcol and Industry standard HID Over SPI protocol.", QuestionFlags: 0x10, QuestionId: 0xF06, VarStoreId: 0x6, VarOffset: 0x793, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A9 19 17 12 06 0F 06 00 93 07 10 10 00 01 00 }
0x5CC7E: 					OneOfOption Option: "THC" Value: 0, Default, MfgDefault { 09 07 18 12 30 00 00 }
0x5CC85: 					OneOfOption Option: "HID over SPI" Value: 1 { 09 07 19 12 00 00 01 }
0x5CC8C: 				End  { 29 02 }
0x5CC8E: 				SuppressIf  { 0A 82 }
0x5CC90: 					EqIdVal QuestionId: 0xF06, Value: 0x0 { 12 06 06 0F 00 00 }
0x5CC96: 					Numeric Prompt: "Connection Speed", Help: "HID Over SPI Connection Speed in Hz", QuestionFlags: 0x10, QuestionId: 0xF07, VarStoreId: 0x6, VarOffset: 0x7C0, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x2625A00, Step: 0x1 { 07 9A AA 19 1F 12 07 0F 06 00 C0 07 10 12 00 00 00 00 00 5A 62 02 01 00 00 00 }
0x5CCB0: 						Default DefaultId: 0x0 Value: 17000000 { 5B 09 00 00 02 40 66 03 01 }
0x5CCB9: 					End  { 29 02 }
0x5CCBB: 					OneOf Prompt: "Flags", Help: "HID Over SPI Flags", QuestionFlags: 0x10, QuestionId: 0xF08, VarStoreId: 0x6, VarOffset: 0x7B8, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x8000, Step: 0x0 { 05 9A AB 19 25 12 08 0F 06 00 B8 07 10 12 00 00 00 00 00 80 00 00 00 00 00 00 }
0x5CCD5: 						OneOfOption Option: "Single SPI Mode" Value: 0, Default, MfgDefault { 09 0A 26 12 32 02 00 00 00 00 }
0x5CCDF: 						OneOfOption Option: "Dual SPI Mode" Value: 16384 { 09 0A 27 12 02 02 00 40 00 00 }
0x5CCE9: 						OneOfOption Option: "Quad SPI Mode" Value: 32768 { 09 0A 28 12 02 02 00 80 00 00 }
0x5CCF3: 					End  { 29 02 }
0x5CCF5: 					Numeric Prompt: "Input Report Body Address", Help: "HID Over SPI Input Report Body Address", QuestionFlags: 0x10, QuestionId: 0xF09, VarStoreId: 0x6, VarOffset: 0x7C8, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A AC 19 2A 12 09 0F 06 00 C8 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CD0F: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CD18: 					End  { 29 02 }
0x5CD1A: 					Numeric Prompt: "Input Report Header Address", Help: "HID Over SPI Input Report Header Address", QuestionFlags: 0x10, QuestionId: 0xF0A, VarStoreId: 0x6, VarOffset: 0x7D0, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A AD 19 2C 12 0A 0F 06 00 D0 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CD34: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CD3D: 					End  { 29 02 }
0x5CD3F: 					Numeric Prompt: "Output Report Address", Help: "HID Over SPI Output Report Address", QuestionFlags: 0x10, QuestionId: 0xF0B, VarStoreId: 0x6, VarOffset: 0x7D8, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A AE 19 2E 12 0B 0F 06 00 D8 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CD59: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CD62: 					End  { 29 02 }
0x5CD64: 					Numeric Prompt: "Write Opcode", Help: "HID Over SPI Write Opcode", QuestionFlags: 0x10, QuestionId: 0xF0C, VarStoreId: 0x6, VarOffset: 0x7E8, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A AF 19 30 12 0C 0F 06 00 E8 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CD7E: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CD87: 					End  { 29 02 }
0x5CD89: 					Numeric Prompt: "Read Opcode", Help: "HID Over SPI Read Opcode", QuestionFlags: 0x10, QuestionId: 0xF0D, VarStoreId: 0x6, VarOffset: 0x7E0, Flags: 0x22, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1 { 07 9A B0 19 32 12 0D 0F 06 00 E0 07 10 22 00 00 00 00 FF FF FF FF 01 00 00 00 }
0x5CDA3: 						Default DefaultId: 0x0 Value: 0 { 5B 09 00 00 02 00 00 00 00 }
0x5CDAC: 					End  { 29 02 }
0x5CDAE: 					OneOf Prompt: "Reset Pad Trigger", Help: "HID Over SPI Reset Pad Trigger", QuestionFlags: 0x10, QuestionId: 0xF0E, VarStoreId: 0x6, VarOffset: 0x7F0, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x1, Step: 0x0 { 05 9A B1 19 34 12 0E 0F 06 00 F0 07 10 12 00 00 00 00 01 00 00 00 00 00 00 00 }
0x5CDC8: 						OneOfOption Option: "Low" Value: 0, Default, MfgDefault { 09 0A 35 12 32 02 00 00 00 00 }
0x5CDD2: 						OneOfOption Option: "High" Value: 1 { 09 0A 36 12 02 02 01 00 00 00 }
0x5CDDC: 					End  { 29 02 }
0x5CDDE: 				End  { 29 02 }
0x5CDE0: 			End  { 29 02 }
0x5CDE2: 		End  { 29 02 }
0x5CDE4: 		SuppressIf  { 0A 82 }
0x5CDE6: 			EqIdVal QuestionId: 0x1123, Value: 0x1 { 12 06 23 11 01 00 }
0x5CDEC: 			Subtitle Prompt: "THC is not available", Help: "", Flags: 0x0 { 02 87 0A 12 00 00 00 }
0x5CDF3: 			End  { 29 02 }
0x5CDF5: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5CDFC: 			End  { 29 02 }
0x5CDFE: 		End  { 29 02 }
0x5CE00: 	End  { 29 02 }
0x5CE02: 	Form FormId: 0x284E, Title: "HD Audio Configuration" { 01 86 4E 28 44 11 }
0x5CE08: 		Subtitle Prompt: "HD Audio Subsystem Configuration Settings", Help: "", Flags: 0x0 { 02 87 45 11 00 00 00 }
0x5CE0F: 		End  { 29 02 }
0x5CE11: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5CE18: 		End  { 29 02 }
0x5CE1A: 		OneOf Prompt: "HD Audio", Help: "Control Detection of the HD-Audio device.

Disabled = HDA will be unconditionally disabled

Enabled = HDA will be unconditionally enabled.", QuestionFlags: 0x10, QuestionId: 0xF0F, VarStoreId: 0x6, VarOffset: 0x58F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4A 11 4B 11 0F 0F 06 00 8F 05 10 10 00 01 00 }
0x5CE2B: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5CE32: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5CE39: 		End  { 29 02 }
0x5CE3B: 		SuppressIf  { 0A 82 }
0x5CE3D: 			EqIdVal QuestionId: 0xF0F, Value: 0x0 { 12 06 0F 0F 00 00 }
0x5CE43: 			GrayOutIf  { 19 82 }
0x5CE45: 				EqIdVal QuestionId: 0x1115, Value: 0x1 { 12 06 15 11 01 00 }
0x5CE4B: 				OneOf Prompt: " Audio DSP", Help: "Enable/Disable Audio DSP.", QuestionFlags: 0x10, QuestionId: 0xF10, VarStoreId: 0x6, VarOffset: 0x590, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4C 11 4D 11 10 0F 06 00 90 05 10 10 00 01 00 }
0x5CE5C: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5CE63: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5CE6A: 				End  { 29 02 }
0x5CE6C: 			End  { 29 02 }
0x5CE6E: 			SuppressIf  { 0A 82 }
0x5CE70: 				EqIdVal QuestionId: 0xF10, Value: 0x0 { 12 86 10 0F 00 00 }
0x5CE76: 					EqIdVal QuestionId: 0x1115, Value: 0x1 { 12 06 15 11 01 00 }
0x5CE7C: 					Or  { 16 02 }
0x5CE7E: 				End  { 29 02 }
0x5CE80: 				OneOf Prompt: " Audio DSP Compliance Mode", Help: "Specifies DSP enabled system compliance:
1. Non-UAA (IntelSST driver support only - CC_040100)
2. UAA (HD Audio Inbox or IntelSST driver support - CC_040380)

Note: NHLT (DMIC/BT/I2S configuration) is published for non-UAA only.", QuestionFlags: 0x10, QuestionId: 0xF11, VarStoreId: 0x6, VarOffset: 0x591, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4E 11 4F 11 11 0F 06 00 91 05 10 10 00 01 00 }
0x5CE91: 					OneOfOption Option: "Non-UAA (IntelSST)" Value: 0, Default, MfgDefault { 09 07 50 11 30 00 00 }
0x5CE98: 					OneOfOption Option: "UAA (HDA Inbox/IntelSST)" Value: 1 { 09 07 51 11 00 00 01 }
0x5CE9F: 				End  { 29 02 }
0x5CEA1: 			End  { 29 02 }
0x5CEA3: 			GrayOutIf  { 19 82 }
0x5CEA5: 				EqIdVal QuestionId: 0xF17, Value: 0x1 { 12 86 17 0F 01 00 }
0x5CEAB: 					EqIdVal QuestionId: 0xF1D, Value: 0x1 { 12 06 1D 0F 01 00 }
0x5CEB1: 					Or  { 16 02 }
0x5CEB3: 				End  { 29 02 }
0x5CEB5: 				SuppressIf  { 0A 82 }
0x5CEB7: 					EqIdVal QuestionId: 0x1122, Value: 0x0 { 12 06 22 11 00 00 }
0x5CEBD: 					OneOf Prompt: "  HDA Link", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF12, VarStoreId: 0x6, VarOffset: 0x594, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 53 11 52 11 12 0F 06 00 94 05 10 10 00 01 00 }
0x5CECE: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5CED5: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5CEDC: 					End  { 29 02 }
0x5CEDE: 				End  { 29 02 }
0x5CEE0: 			End  { 29 02 }
0x5CEE2: 			GrayOutIf  { 19 82 }
0x5CEE4: 				EqIdVal QuestionId: 0xF20, Value: 0x1 { 12 06 20 0F 01 00 }
0x5CEEA: 				SuppressIf  { 0A 82 }
0x5CEEC: 					EqIdVal QuestionId: 0x1121, Value: 0x0 { 12 06 21 11 00 00 }
0x5CEF2: 					OneOf Prompt: "  DMIC #0", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF13, VarStoreId: 0x6, VarOffset: 0x595, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 06 19 52 11 13 0F 06 00 95 05 10 10 00 01 00 }
0x5CF03: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5CF0A: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5CF11: 					End  { 29 02 }
0x5CF13: 					GrayOutIf  { 19 82 }
0x5CF15: 						EqIdVal QuestionId: 0xF1E, Value: 0x1 { 12 06 1E 0F 01 00 }
0x5CF1B: 						SuppressIf  { 0A 82 }
0x5CF1D: 							EqIdVal QuestionId: 0xF13, Value: 0x0 { 12 06 13 0F 00 00 }
0x5CF23: 							OneOf Prompt: "Dmic Clock Source Select", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0xF14, VarStoreId: 0x6, VarOffset: 0x597, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 07 19 7E 11 14 0F 06 00 97 05 10 10 00 02 00 }
0x5CF34: 								OneOfOption Option: "Both" Value: 0 { 09 07 7F 11 00 00 00 }
0x5CF3B: 								OneOfOption Option: "ClkA" Value: 1, Default, MfgDefault { 09 07 80 11 30 00 01 }
0x5CF42: 								OneOfOption Option: "ClkB" Value: 2 { 09 07 81 11 00 00 02 }
0x5CF49: 							End  { 29 02 }
0x5CF4B: 						End  { 29 02 }
0x5CF4D: 					End  { 29 02 }
0x5CF4F: 				End  { 29 02 }
0x5CF51: 			End  { 29 02 }
0x5CF53: 			GrayOutIf  { 19 82 }
0x5CF55: 				EqIdVal QuestionId: 0xF1F, Value: 0x1 { 12 06 1F 0F 01 00 }
0x5CF5B: 				SuppressIf  { 0A 82 }
0x5CF5D: 					EqIdVal QuestionId: 0x1120, Value: 0x0 { 12 06 20 11 00 00 }
0x5CF63: 					OneOf Prompt: "  DMIC #1", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF15, VarStoreId: 0x6, VarOffset: 0x596, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 08 19 52 11 15 0F 06 00 96 05 10 10 00 01 00 }
0x5CF74: 						OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5CF7B: 						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5CF82: 					End  { 29 02 }
0x5CF84: 					GrayOutIf  { 19 82 }
0x5CF86: 						EqIdVal QuestionId: 0xF1E, Value: 0x1 { 12 06 1E 0F 01 00 }
0x5CF8C: 						SuppressIf  { 0A 82 }
0x5CF8E: 							EqIdVal QuestionId: 0xF15, Value: 0x0 { 12 06 15 0F 00 00 }
0x5CF94: 							OneOf Prompt: "Dmic Clock Source Select", Help: "N/A", QuestionFlags: 0x10, QuestionId: 0xF16, VarStoreId: 0x6, VarOffset: 0x598, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 09 19 7E 11 16 0F 06 00 98 05 10 10 00 02 00 }
0x5CFA5: 								OneOfOption Option: "Both" Value: 0 { 09 07 7F 11 00 00 00 }
0x5CFAC: 								OneOfOption Option: "ClkA" Value: 1, Default, MfgDefault { 09 07 80 11 30 00 01 }
0x5CFB3: 								OneOfOption Option: "ClkB" Value: 2 { 09 07 81 11 00 00 02 }
0x5CFBA: 							End  { 29 02 }
0x5CFBC: 						End  { 29 02 }
0x5CFBE: 					End  { 29 02 }
0x5CFC0: 				End  { 29 02 }
0x5CFC2: 			End  { 29 02 }
0x5CFC4: 			GrayOutIf  { 19 82 }
0x5CFC6: 				EqIdVal QuestionId: 0xF12, Value: 0x1 { 12 06 12 0F 01 00 }
0x5CFCC: 				SuppressIf  { 0A 82 }
0x5CFCE: 					EqIdVal QuestionId: 0x111F, Value: 0x0 { 12 06 1F 11 00 00 }
0x5CFD4: 					OneOf Prompt: "  SSP #0", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF17, VarStoreId: 0x6, VarOffset: 0x59D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 56 11 52 11 17 0F 06 00 9D 05 10 10 00 01 00 }
0x5CFE5: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5CFEC: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5CFF3: 					End  { 29 02 }
0x5CFF5: 				End  { 29 02 }
0x5CFF7: 			End  { 29 02 }
0x5CFF9: 			SuppressIf  { 0A 82 }
0x5CFFB: 				EqIdVal QuestionId: 0x111E, Value: 0x0 { 12 06 1E 11 00 00 }
0x5D001: 				OneOf Prompt: "  SSP #1", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF18, VarStoreId: 0x6, VarOffset: 0x59E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 57 11 52 11 18 0F 06 00 9E 05 10 10 00 01 00 }
0x5D012: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D019: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D020: 				End  { 29 02 }
0x5D022: 			End  { 29 02 }
0x5D024: 			SuppressIf  { 0A 82 }
0x5D026: 				EqIdVal QuestionId: 0x111D, Value: 0x0 { 12 06 1D 11 00 00 }
0x5D02C: 				GrayOutIf  { 19 82 }
0x5D02E: 					StringRef1 String: "No" { 4E 84 C9 01 }
0x5D032: 						StringRef1 String: "No" { 4E 04 C8 01 }
0x5D036: 						Match  { 2A 02 }
0x5D038: 						Not  { 17 02 }
0x5D03A: 					End  { 29 02 }
0x5D03C: 					OneOf Prompt: "  SSP #2", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF19, VarStoreId: 0x6, VarOffset: 0x59F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 58 11 52 11 19 0F 06 00 9F 05 10 10 00 01 00 }
0x5D04D: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D054: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D05B: 					End  { 29 02 }
0x5D05D: 				End  { 29 02 }
0x5D05F: 			End  { 29 02 }
0x5D061: 			SuppressIf  { 0A 82 }
0x5D063: 				EqIdVal QuestionId: 0x111C, Value: 0x0 { 12 06 1C 11 00 00 }
0x5D069: 				OneOf Prompt: "  SSP #3", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF1A, VarStoreId: 0x6, VarOffset: 0x5A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 59 11 52 11 1A 0F 06 00 A0 05 10 10 00 01 00 }
0x5D07A: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D081: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D088: 				End  { 29 02 }
0x5D08A: 			End  { 29 02 }
0x5D08C: 			SuppressIf  { 0A 82 }
0x5D08E: 				EqIdVal QuestionId: 0x111B, Value: 0x0 { 12 06 1B 11 00 00 }
0x5D094: 				OneOf Prompt: "  SSP #4", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF1B, VarStoreId: 0x6, VarOffset: 0x5A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5A 11 52 11 1B 0F 06 00 A1 05 10 10 00 01 00 }
0x5D0A5: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D0AC: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D0B3: 				End  { 29 02 }
0x5D0B5: 			End  { 29 02 }
0x5D0B7: 			SuppressIf  { 0A 82 }
0x5D0B9: 				EqIdVal QuestionId: 0x111A, Value: 0x0 { 12 06 1A 11 00 00 }
0x5D0BF: 				OneOf Prompt: "  SSP #5", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF1C, VarStoreId: 0x6, VarOffset: 0x5A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 5B 11 52 11 1C 0F 06 00 A2 05 10 10 00 01 00 }
0x5D0D0: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D0D7: 					OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D0DE: 				End  { 29 02 }
0x5D0E0: 			End  { 29 02 }
0x5D0E2: 			GrayOutIf  { 19 82 }
0x5D0E4: 				EqIdVal QuestionId: 0xF12, Value: 0x1 { 12 06 12 0F 01 00 }
0x5D0EA: 				SuppressIf  { 0A 82 }
0x5D0EC: 					EqIdVal QuestionId: 0x1119, Value: 0x0 { 12 06 19 11 00 00 }
0x5D0F2: 					OneOf Prompt: "  SNDW #1", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF1D, VarStoreId: 0x6, VarOffset: 0x599, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F9 18 52 11 1D 0F 06 00 99 05 10 10 00 01 00 }
0x5D103: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D10A: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D111: 					End  { 29 02 }
0x5D113: 				End  { 29 02 }
0x5D115: 			End  { 29 02 }
0x5D117: 			GrayOutIf  { 19 82 }
0x5D119: 				EqIdVal QuestionId: 0xF13, Value: 0x1 { 12 86 13 0F 01 00 }
0x5D11F: 					EqIdVal QuestionId: 0xF14, Value: 0x0 { 12 06 14 0F 00 00 }
0x5D125: 					And  { 15 02 }
0x5D127: 					EqIdVal QuestionId: 0xF15, Value: 0x1 { 12 06 15 0F 01 00 }
0x5D12D: 					EqIdVal QuestionId: 0xF16, Value: 0x0 { 12 06 16 0F 00 00 }
0x5D133: 					And  { 15 02 }
0x5D135: 					Or  { 16 02 }
0x5D137: 					EqIdVal QuestionId: 0xF13, Value: 0x1 { 12 06 13 0F 01 00 }
0x5D13D: 					EqIdVal QuestionId: 0xF14, Value: 0x2 { 12 06 14 0F 02 00 }
0x5D143: 					And  { 15 02 }
0x5D145: 					Or  { 16 02 }
0x5D147: 					EqIdVal QuestionId: 0xF15, Value: 0x1 { 12 06 15 0F 01 00 }
0x5D14D: 					EqIdVal QuestionId: 0xF16, Value: 0x2 { 12 06 16 0F 02 00 }
0x5D153: 					And  { 15 02 }
0x5D155: 					Or  { 16 02 }
0x5D157: 				End  { 29 02 }
0x5D159: 				SuppressIf  { 0A 82 }
0x5D15B: 					EqIdVal QuestionId: 0x1118, Value: 0x0 { 12 06 18 11 00 00 }
0x5D161: 					OneOf Prompt: "  SNDW #2", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF1E, VarStoreId: 0x6, VarOffset: 0x59A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 18 52 11 1E 0F 06 00 9A 05 10 10 00 01 00 }
0x5D172: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D179: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D180: 					End  { 29 02 }
0x5D182: 				End  { 29 02 }
0x5D184: 			End  { 29 02 }
0x5D186: 			GrayOutIf  { 19 82 }
0x5D188: 				EqIdVal QuestionId: 0xF15, Value: 0x1 { 12 06 15 0F 01 00 }
0x5D18E: 				SuppressIf  { 0A 82 }
0x5D190: 					EqIdVal QuestionId: 0x1117, Value: 0x0 { 12 06 17 11 00 00 }
0x5D196: 					OneOf Prompt: "  SNDW #3", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF1F, VarStoreId: 0x6, VarOffset: 0x59B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FB 18 52 11 1F 0F 06 00 9B 05 10 10 00 01 00 }
0x5D1A7: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D1AE: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D1B5: 					End  { 29 02 }
0x5D1B7: 				End  { 29 02 }
0x5D1B9: 			End  { 29 02 }
0x5D1BB: 			GrayOutIf  { 19 82 }
0x5D1BD: 				EqIdVal QuestionId: 0xF13, Value: 0x1 { 12 06 13 0F 01 00 }
0x5D1C3: 				SuppressIf  { 0A 82 }
0x5D1C5: 					EqIdVal QuestionId: 0x1116, Value: 0x0 { 12 06 16 11 00 00 }
0x5D1CB: 					OneOf Prompt: "  SNDW #4", Help: "Muxed interfaces:
1) HDA/SSP0
2) HDA[SDI1]/SSP1
3) DMIC0/SNDW4
4) DMIC1/SNDW3
CNL only:
5) HDA/SNDW1
6) SSP1/SNDW2", QuestionFlags: 0x10, QuestionId: 0xF20, VarStoreId: 0x6, VarOffset: 0x59C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 60 11 52 11 20 0F 06 00 9C 05 10 10 00 01 00 }
0x5D1DC: 						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D1E3: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D1EA: 					End  { 29 02 }
0x5D1EC: 				End  { 29 02 }
0x5D1EE: 			End  { 29 02 }
0x5D1F0: 			Ref Prompt: "HD Audio Advanced Configuration", Help: "HD Audio Subsystem Advanced Configuration Settings", QuestionFlags: 0x0, QuestionId: 0xF21, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x284F { 0F 0F 46 11 47 11 21 0F 00 00 FF FF 00 4F 28 }
0x5D1FF: 			SuppressIf  { 0A 82 }
0x5D201: 				EqIdVal QuestionId: 0xF10, Value: 0x0 { 12 86 10 0F 00 00 }
0x5D207: 					EqIdVal QuestionId: 0x1115, Value: 0x1 { 12 06 15 11 01 00 }
0x5D20D: 					Or  { 16 02 }
0x5D20F: 				End  { 29 02 }
0x5D211: 				Ref Prompt: "HD Audio DSP Features Configuration", Help: "HD Audio Subsystem Features Configuration (ACPI)", QuestionFlags: 0x0, QuestionId: 0xF22, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2850 { 0F 0F 48 11 49 11 22 0F 00 00 FF FF 00 50 28 }
0x5D220: 			End  { 29 02 }
0x5D222: 		End  { 29 02 }
0x5D224: 		SuppressIf  { 0A 82 }
0x5D226: 			EqIdVal QuestionId: 0x1114, Value: 0x1 { 12 06 14 11 01 00 }
0x5D22C: 			OneOf Prompt: "HDA Codec ALC245 Configuration", Help: "Option for configuring DMIC connection to ALC245.", QuestionFlags: 0x10, QuestionId: 0xF23, VarStoreId: 0x6, VarOffset: 0x791, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 E6 11 E7 11 23 0F 06 00 91 07 10 20 00 02 00 }
0x5D23D: 				OneOfOption Option: "No Dmic to codec" Value: 0, Default, MfgDefault { 09 07 E9 11 30 00 00 }
0x5D244: 				OneOfOption Option: "4 Dmic to codec" Value: 1 { 09 07 E8 11 00 00 01 }
0x5D24B: 				OneOfOption Option: "2 Dmic to codec" Value: 2 { 09 07 EA 11 00 00 02 }
0x5D252: 			End  { 29 02 }
0x5D254: 		End  { 29 02 }
0x5D256: 	End  { 29 02 }
0x5D258: 	Form FormId: 0x284F, Title: "HD Audio Advanced Configuration" { 01 86 4F 28 46 11 }
0x5D25E: 		Subtitle Prompt: "HD Audio Subsystem Advanced Configuration Settings", Help: "", Flags: 0x0 { 02 87 47 11 00 00 00 }
0x5D265: 		End  { 29 02 }
0x5D267: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5D26E: 		End  { 29 02 }
0x5D270: 		OneOf Prompt: "iDisplay Audio Disconnect", Help: "Disconnects SDI2 signal to hide/disable iDisplay Audio Codec.", QuestionFlags: 0x10, QuestionId: 0xF24, VarStoreId: 0x6, VarOffset: 0x592, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 82 11 83 11 24 0F 06 00 92 05 10 10 00 01 00 }
0x5D281: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D288: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D28F: 		End  { 29 02 }
0x5D291: 		OneOf Prompt: "Codec Sx Wake Capability", Help: "Capability to detect wake initiated by a codec in Sx (eg by modem codec)", QuestionFlags: 0x10, QuestionId: 0xF25, VarStoreId: 0x6, VarOffset: 0x5A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 84 11 85 11 25 0F 06 00 A6 05 10 10 00 01 00 }
0x5D2A2: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D2A9: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D2B0: 		End  { 29 02 }
0x5D2B2: 		OneOf Prompt: "PME Enable", Help: "Enables PME wake of HD Audio controller during POST.", QuestionFlags: 0x10, QuestionId: 0xF26, VarStoreId: 0x6, VarOffset: 0x593, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 11 87 11 26 0F 06 00 93 05 10 10 00 01 00 }
0x5D2C3: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D2CA: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D2D1: 		End  { 29 02 }
0x5D2D3: 		Text Prompt: "Statically Switchable BCLK Clock Frequency Configuration:", Help: "Statically Switchable BCLK Clock Frequency Configuration:", Text: "" { 03 08 88 11 88 11 00 00 }
0x5D2DB: 		OneOf Prompt: " HD Audio Link Frequency", Help: "Selects HD Audio Link frequency.
Applicable only if HDA codec supports selected frequency.", QuestionFlags: 0x10, QuestionId: 0xF27, VarStoreId: 0x6, VarOffset: 0x5A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 89 11 8A 11 27 0F 06 00 A3 05 10 10 00 02 00 }
0x5D2EC: 			OneOfOption Option: "6 MHz" Value: 0 { 09 07 8D 11 00 00 00 }
0x5D2F3: 			OneOfOption Option: "12 MHz" Value: 1 { 09 07 8E 11 00 00 01 }
0x5D2FA: 			OneOfOption Option: "24 MHz" Value: 2, Default { 09 07 8F 11 10 00 02 }
0x5D301: 		End  { 29 02 }
0x5D303: 		OneOf Prompt: " iDisplay Audio Link Frequency", Help: "Selects iDisplay Link frequency.", QuestionFlags: 0x10, QuestionId: 0xF28, VarStoreId: 0x6, VarOffset: 0x5A4, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x4, Step: 0x0 { 05 91 8B 11 8C 11 28 0F 06 00 A4 05 10 10 03 04 00 }
0x5D314: 			OneOfOption Option: "48 MHz" Value: 3 { 09 07 90 11 00 00 03 }
0x5D31B: 			OneOfOption Option: "96 MHz" Value: 4, Default { 09 07 91 11 10 00 04 }
0x5D322: 		End  { 29 02 }
0x5D324: 		OneOf Prompt: " iDisplay Audio Link T-Mode", Help: "Indicates whether SDI is operating in 1T, 2T (CNL) or 2T, 4T, 8T mode (ICL).", QuestionFlags: 0x10, QuestionId: 0xF29, VarStoreId: 0x6, VarOffset: 0x5A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 92 11 93 11 29 0F 06 00 A5 05 10 10 00 04 00 }
0x5D335: 			OneOfOption Option: "1T Mode" Value: 1 { 09 07 94 11 00 00 01 }
0x5D33C: 			OneOfOption Option: "2T Mode" Value: 0 { 09 07 95 11 00 00 00 }
0x5D343: 			OneOfOption Option: "4T Mode" Value: 2 { 09 07 96 11 00 00 02 }
0x5D34A: 			OneOfOption Option: "8T Mode" Value: 3, Default, MfgDefault { 09 07 97 11 30 00 03 }
0x5D351: 			OneOfOption Option: "16T Mode" Value: 4 { 09 07 98 11 00 00 04 }
0x5D358: 		End  { 29 02 }
0x5D35A: 		OneOf Prompt: "Autonomous Clock Stop SNDW #1", Help: "Enable/Disable Autonomous Clock Stop for SoundWire LINK1", QuestionFlags: 0x10, QuestionId: 0xF2A, VarStoreId: 0x6, VarOffset: 0x5A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 02 19 67 11 2A 0F 06 00 A7 05 10 10 00 01 00 }
0x5D36B: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D372: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D379: 		End  { 29 02 }
0x5D37B: 		OneOf Prompt: "Autonomous Clock Stop SNDW #2", Help: "Enable/Disable Autonomous Clock Stop for SoundWire LINK2", QuestionFlags: 0x10, QuestionId: 0xF2B, VarStoreId: 0x6, VarOffset: 0x5A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 03 19 68 11 2B 0F 06 00 A8 05 10 10 00 01 00 }
0x5D38C: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D393: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D39A: 		End  { 29 02 }
0x5D39C: 		OneOf Prompt: "Autonomous Clock Stop SNDW #3", Help: "Enable/Disable Autonomous Clock Stop for SoundWire LINK3", QuestionFlags: 0x10, QuestionId: 0xF2C, VarStoreId: 0x6, VarOffset: 0x5A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 04 19 69 11 2C 0F 06 00 A9 05 10 10 00 01 00 }
0x5D3AD: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D3B4: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D3BB: 		End  { 29 02 }
0x5D3BD: 		OneOf Prompt: "Autonomous Clock Stop SNDW #4", Help: "Enable/Disable Autonomous Clock Stop for SoundWire LINK4", QuestionFlags: 0x10, QuestionId: 0xF2D, VarStoreId: 0x6, VarOffset: 0x5AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 65 11 6A 11 2D 0F 06 00 AA 05 10 10 00 01 00 }
0x5D3CE: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D3D5: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D3DC: 		End  { 29 02 }
0x5D3DE: 		OneOf Prompt: "Data On Active Interval Select SNDW #1", Help: "Data On Active Interval Select:
1) 6 clock periods
2) 7 clock periods
3) 8 clock periods
4) 11 clock periods
5)", QuestionFlags: 0x10, QuestionId: 0xF2E, VarStoreId: 0x6, VarOffset: 0x5AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 FC 18 70 11 2E 0F 06 00 AB 05 10 10 00 03 00 }
0x5D3EF: 			OneOfOption Option: "6 clock periods" Value: 0 { 09 07 71 11 00 00 00 }
0x5D3F6: 			OneOfOption Option: "7 clock periods" Value: 1 { 09 07 72 11 00 00 01 }
0x5D3FD: 			OneOfOption Option: "8 clock periods" Value: 2 { 09 07 73 11 00 00 02 }
0x5D404: 			OneOfOption Option: "11 clock periods" Value: 3, Default, MfgDefault { 09 07 74 11 30 00 03 }
0x5D40B: 		End  { 29 02 }
0x5D40D: 		OneOf Prompt: "Data On Active Interval Select SNDW #2", Help: "Data On Active Interval Select:
1) 6 clock periods
2) 7 clock periods
3) 8 clock periods
4) 11 clock periods
5)", QuestionFlags: 0x10, QuestionId: 0xF2F, VarStoreId: 0x6, VarOffset: 0x5AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 FD 18 70 11 2F 0F 06 00 AC 05 10 10 00 03 00 }
0x5D41E: 			OneOfOption Option: "6 clock periods" Value: 0 { 09 07 71 11 00 00 00 }
0x5D425: 			OneOfOption Option: "7 clock periods" Value: 1 { 09 07 72 11 00 00 01 }
0x5D42C: 			OneOfOption Option: "8 clock periods" Value: 2 { 09 07 73 11 00 00 02 }
0x5D433: 			OneOfOption Option: "11 clock periods" Value: 3, Default, MfgDefault { 09 07 74 11 30 00 03 }
0x5D43A: 		End  { 29 02 }
0x5D43C: 		OneOf Prompt: "Data On Active Interval Select SNDW #3", Help: "Data On Active Interval Select:
1) 6 clock periods
2) 7 clock periods
3) 8 clock periods
4) 11 clock periods
5)", QuestionFlags: 0x10, QuestionId: 0xF30, VarStoreId: 0x6, VarOffset: 0x5AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 FE 18 70 11 30 0F 06 00 AD 05 10 10 00 03 00 }
0x5D44D: 			OneOfOption Option: "6 clock periods" Value: 0 { 09 07 71 11 00 00 00 }
0x5D454: 			OneOfOption Option: "7 clock periods" Value: 1 { 09 07 72 11 00 00 01 }
0x5D45B: 			OneOfOption Option: "8 clock periods" Value: 2 { 09 07 73 11 00 00 02 }
0x5D462: 			OneOfOption Option: "11 clock periods" Value: 3, Default, MfgDefault { 09 07 74 11 30 00 03 }
0x5D469: 		End  { 29 02 }
0x5D46B: 		OneOf Prompt: "Data On Active Interval Select SNDW #4", Help: "Data On Active Interval Select:
1) 6 clock periods
2) 7 clock periods
3) 8 clock periods
4) 11 clock periods
5)", QuestionFlags: 0x10, QuestionId: 0xF31, VarStoreId: 0x6, VarOffset: 0x5AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 6F 11 70 11 31 0F 06 00 AE 05 10 10 00 03 00 }
0x5D47C: 			OneOfOption Option: "6 clock periods" Value: 0 { 09 07 71 11 00 00 00 }
0x5D483: 			OneOfOption Option: "7 clock periods" Value: 1 { 09 07 72 11 00 00 01 }
0x5D48A: 			OneOfOption Option: "8 clock periods" Value: 2 { 09 07 73 11 00 00 02 }
0x5D491: 			OneOfOption Option: "11 clock periods" Value: 3, Default, MfgDefault { 09 07 74 11 30 00 03 }
0x5D498: 		End  { 29 02 }
0x5D49A: 		OneOf Prompt: "Data On Delay Select SNDW #1", Help: "Data On Delay Select:
1) 2 clock periods
2) 3 clock periods
3)", QuestionFlags: 0x10, QuestionId: 0xF32, VarStoreId: 0x6, VarOffset: 0x5AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FF 18 7A 11 32 0F 06 00 AF 05 10 10 00 01 00 }
0x5D4AB: 			OneOfOption Option: "2 clock periods" Value: 0 { 09 07 7B 11 00 00 00 }
0x5D4B2: 			OneOfOption Option: "3 clock periods" Value: 1, Default, MfgDefault { 09 07 7C 11 30 00 01 }
0x5D4B9: 		End  { 29 02 }
0x5D4BB: 		OneOf Prompt: "Data On Delay Select SNDW #2", Help: "Data On Delay Select:
1) 2 clock periods
2) 3 clock periods
3)", QuestionFlags: 0x10, QuestionId: 0xF33, VarStoreId: 0x6, VarOffset: 0x5B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 00 19 7A 11 33 0F 06 00 B0 05 10 10 00 01 00 }
0x5D4CC: 			OneOfOption Option: "2 clock periods" Value: 0 { 09 07 7B 11 00 00 00 }
0x5D4D3: 			OneOfOption Option: "3 clock periods" Value: 1, Default, MfgDefault { 09 07 7C 11 30 00 01 }
0x5D4DA: 		End  { 29 02 }
0x5D4DC: 		OneOf Prompt: "Data On Delay Select SNDW #3", Help: "Data On Delay Select:
1) 2 clock periods
2) 3 clock periods
3)", QuestionFlags: 0x10, QuestionId: 0xF34, VarStoreId: 0x6, VarOffset: 0x5B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 01 19 7A 11 34 0F 06 00 B1 05 10 10 00 01 00 }
0x5D4ED: 			OneOfOption Option: "2 clock periods" Value: 0 { 09 07 7B 11 00 00 00 }
0x5D4F4: 			OneOfOption Option: "3 clock periods" Value: 1, Default, MfgDefault { 09 07 7C 11 30 00 01 }
0x5D4FB: 		End  { 29 02 }
0x5D4FD: 		OneOf Prompt: "Data On Delay Select SNDW #4", Help: "Data On Delay Select:
1) 2 clock periods
2) 3 clock periods
3)", QuestionFlags: 0x10, QuestionId: 0xF35, VarStoreId: 0x6, VarOffset: 0x5B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 79 11 7A 11 35 0F 06 00 B2 05 10 10 00 01 00 }
0x5D50E: 			OneOfOption Option: "2 clock periods" Value: 0 { 09 07 7B 11 00 00 00 }
0x5D515: 			OneOfOption Option: "3 clock periods" Value: 1, Default, MfgDefault { 09 07 7C 11 30 00 01 }
0x5D51C: 		End  { 29 02 }
0x5D51E: 		OneOf Prompt: "ACX SSID 305610EC Codecs Topology", Help: "Codecs: ALC711-VD1, ALC714-VC1, 2x ALC316", QuestionFlags: 0x10, QuestionId: 0xF36, VarStoreId: 0x6, VarOffset: 0x7FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E4 11 E5 11 36 0F 06 00 FF 07 10 10 00 01 00 }
0x5D52F: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D536: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D53D: 		End  { 29 02 }
0x5D53F: 	End  { 29 02 }
0x5D541: 	Form FormId: 0x2850, Title: "HD Audio DSP Features Configuration" { 01 86 50 28 48 11 }
0x5D547: 		Subtitle Prompt: "HD Audio Subsystem Features Configuration (ACPI)", Help: "", Flags: 0x0 { 02 87 49 11 00 00 00 }
0x5D54E: 		End  { 29 02 }
0x5D550: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5D557: 		End  { 29 02 }
0x5D559: 		GrayOutIf  { 19 82 }
0x5D55B: 			EqIdVal QuestionId: 0xF11, Value: 0x0 { 12 86 11 0F 00 00 }
0x5D561: 				Not  { 17 02 }
0x5D563: 			End  { 29 02 }
0x5D565: 			Text Prompt: "Audio DSP NHLT Endpoints Configuration:", Help: "Audio DSP NHLT Endpoints Configuration:", Text: "" { 03 08 99 11 99 11 00 00 }
0x5D56D: 			GrayOutIf  { 19 82 }
0x5D56F: 				EqIdVal QuestionId: 0xF13, Value: 0x0 { 12 86 13 0F 00 00 }
0x5D575: 					EqIdVal QuestionId: 0xF15, Value: 0x0 { 12 06 15 0F 00 00 }
0x5D57B: 					And  { 15 02 }
0x5D57D: 				End  { 29 02 }
0x5D57F: 				GrayOutIf  { 19 82 }
0x5D581: 					EqIdVal QuestionId: 0xF38, Value: 0x1 { 12 86 38 0F 01 00 }
0x5D587: 						EqIdVal QuestionId: 0xF39, Value: 0x1 { 12 06 39 0F 01 00 }
0x5D58D: 						Or  { 16 02 }
0x5D58F: 						EqIdVal QuestionId: 0xF3A, Value: 0x1 { 12 06 3A 0F 01 00 }
0x5D595: 						Or  { 16 02 }
0x5D597: 						EqIdVal QuestionId: 0xF3B, Value: 0x1 { 12 06 3B 0F 01 00 }
0x5D59D: 						Or  { 16 02 }
0x5D59F: 						EqIdVal QuestionId: 0xF3C, Value: 0x1 { 12 06 3C 0F 01 00 }
0x5D5A5: 						Or  { 16 02 }
0x5D5A7: 					End  { 29 02 }
0x5D5A9: 					OneOf Prompt: " Dmic Mono 38.4MHz", Help: "Enables/Disables 1 Mic Array Endpoint in NHLT ACPI table. XTAL: 38.4MHz.", QuestionFlags: 0x10, QuestionId: 0xF37, VarStoreId: 0x7, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9A 11 9B 11 37 0F 07 00 01 00 10 10 00 01 00 }
0x5D5BA: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D5C1: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D5C8: 					End  { 29 02 }
0x5D5CA: 				End  { 29 02 }
0x5D5CC: 				GrayOutIf  { 19 82 }
0x5D5CE: 					EqIdVal QuestionId: 0xF37, Value: 0x1 { 12 86 37 0F 01 00 }
0x5D5D4: 						EqIdVal QuestionId: 0xF39, Value: 0x1 { 12 06 39 0F 01 00 }
0x5D5DA: 						Or  { 16 02 }
0x5D5DC: 						EqIdVal QuestionId: 0xF3A, Value: 0x1 { 12 06 3A 0F 01 00 }
0x5D5E2: 						Or  { 16 02 }
0x5D5E4: 						EqIdVal QuestionId: 0xF3B, Value: 0x1 { 12 06 3B 0F 01 00 }
0x5D5EA: 						Or  { 16 02 }
0x5D5EC: 						EqIdVal QuestionId: 0xF3C, Value: 0x1 { 12 06 3C 0F 01 00 }
0x5D5F2: 						Or  { 16 02 }
0x5D5F4: 					End  { 29 02 }
0x5D5F6: 					OneOf Prompt: " Dmic Stereo 38.4MHz", Help: "Enables/Disables 2 Mic Array Endpoint in NHLT ACPI table. XTAL: 38.4MHz.", QuestionFlags: 0x10, QuestionId: 0xF38, VarStoreId: 0x7, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9C 11 9D 11 38 0F 07 00 02 00 10 10 00 01 00 }
0x5D607: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D60E: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D615: 					End  { 29 02 }
0x5D617: 				End  { 29 02 }
0x5D619: 				GrayOutIf  { 19 82 }
0x5D61B: 					EqIdVal QuestionId: 0xF37, Value: 0x1 { 12 86 37 0F 01 00 }
0x5D621: 						EqIdVal QuestionId: 0xF38, Value: 0x1 { 12 06 38 0F 01 00 }
0x5D627: 						Or  { 16 02 }
0x5D629: 						EqIdVal QuestionId: 0xF3A, Value: 0x1 { 12 06 3A 0F 01 00 }
0x5D62F: 						Or  { 16 02 }
0x5D631: 						EqIdVal QuestionId: 0xF3B, Value: 0x1 { 12 06 3B 0F 01 00 }
0x5D637: 						Or  { 16 02 }
0x5D639: 						EqIdVal QuestionId: 0xF3C, Value: 0x1 { 12 06 3C 0F 01 00 }
0x5D63F: 						Or  { 16 02 }
0x5D641: 					End  { 29 02 }
0x5D643: 					OneOf Prompt: " Dmic Quad 38.4MHz", Help: "Enables/Disables 4 Mic Array Endpoint in NHLT ACPI table. XTAL: 38.4MHz.", QuestionFlags: 0x10, QuestionId: 0xF39, VarStoreId: 0x7, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9E 11 9F 11 39 0F 07 00 03 00 10 10 00 01 00 }
0x5D654: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D65B: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D662: 					End  { 29 02 }
0x5D664: 				End  { 29 02 }
0x5D666: 				GrayOutIf  { 19 82 }
0x5D668: 					EqIdVal QuestionId: 0xF37, Value: 0x1 { 12 86 37 0F 01 00 }
0x5D66E: 						EqIdVal QuestionId: 0xF38, Value: 0x1 { 12 06 38 0F 01 00 }
0x5D674: 						Or  { 16 02 }
0x5D676: 						EqIdVal QuestionId: 0xF39, Value: 0x1 { 12 06 39 0F 01 00 }
0x5D67C: 						Or  { 16 02 }
0x5D67E: 						EqIdVal QuestionId: 0xF3B, Value: 0x1 { 12 06 3B 0F 01 00 }
0x5D684: 						Or  { 16 02 }
0x5D686: 						EqIdVal QuestionId: 0xF3C, Value: 0x1 { 12 06 3C 0F 01 00 }
0x5D68C: 						Or  { 16 02 }
0x5D68E: 					End  { 29 02 }
0x5D690: 					OneOf Prompt: " Dmic Mono 24MHz", Help: "Enables/Disables 1 Mic Array Endpoint in NHLT ACPI table. XTAL: 24MHz.", QuestionFlags: 0x10, QuestionId: 0xF3A, VarStoreId: 0x7, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A4 11 A5 11 3A 0F 07 00 06 00 10 10 00 01 00 }
0x5D6A1: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D6A8: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D6AF: 					End  { 29 02 }
0x5D6B1: 				End  { 29 02 }
0x5D6B3: 				GrayOutIf  { 19 82 }
0x5D6B5: 					EqIdVal QuestionId: 0xF37, Value: 0x1 { 12 86 37 0F 01 00 }
0x5D6BB: 						EqIdVal QuestionId: 0xF38, Value: 0x1 { 12 06 38 0F 01 00 }
0x5D6C1: 						Or  { 16 02 }
0x5D6C3: 						EqIdVal QuestionId: 0xF39, Value: 0x1 { 12 06 39 0F 01 00 }
0x5D6C9: 						Or  { 16 02 }
0x5D6CB: 						EqIdVal QuestionId: 0xF3A, Value: 0x1 { 12 06 3A 0F 01 00 }
0x5D6D1: 						Or  { 16 02 }
0x5D6D3: 						EqIdVal QuestionId: 0xF3C, Value: 0x1 { 12 06 3C 0F 01 00 }
0x5D6D9: 						Or  { 16 02 }
0x5D6DB: 					End  { 29 02 }
0x5D6DD: 					OneOf Prompt: " Dmic Stereo 24MHz", Help: "Enables/Disables 2 Mic Array Endpoint in NHLT ACPI table. XTAL: 24MHz.", QuestionFlags: 0x10, QuestionId: 0xF3B, VarStoreId: 0x7, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A6 11 A7 11 3B 0F 07 00 07 00 10 10 00 01 00 }
0x5D6EE: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D6F5: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D6FC: 					End  { 29 02 }
0x5D6FE: 				End  { 29 02 }
0x5D700: 				GrayOutIf  { 19 82 }
0x5D702: 					EqIdVal QuestionId: 0xF37, Value: 0x1 { 12 86 37 0F 01 00 }
0x5D708: 						EqIdVal QuestionId: 0xF38, Value: 0x1 { 12 06 38 0F 01 00 }
0x5D70E: 						Or  { 16 02 }
0x5D710: 						EqIdVal QuestionId: 0xF39, Value: 0x1 { 12 06 39 0F 01 00 }
0x5D716: 						Or  { 16 02 }
0x5D718: 						EqIdVal QuestionId: 0xF3A, Value: 0x1 { 12 06 3A 0F 01 00 }
0x5D71E: 						Or  { 16 02 }
0x5D720: 						EqIdVal QuestionId: 0xF3B, Value: 0x1 { 12 06 3B 0F 01 00 }
0x5D726: 						Or  { 16 02 }
0x5D728: 					End  { 29 02 }
0x5D72A: 					OneOf Prompt: " Dmic Quad 24MHz", Help: "Enables/Disables 4 Mic Array Endpoint in NHLT ACPI table. XTAL: 24MHz.", QuestionFlags: 0x10, QuestionId: 0xF3C, VarStoreId: 0x7, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A8 11 A9 11 3C 0F 07 00 08 00 10 10 00 01 00 }
0x5D73B: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D742: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D749: 					End  { 29 02 }
0x5D74B: 				End  { 29 02 }
0x5D74D: 			End  { 29 02 }
0x5D74F: 			GrayOutIf  { 19 82 }
0x5D751: 				EqIdVal QuestionId: 0xF17, Value: 0x0 { 12 86 17 0F 00 00 }
0x5D757: 					EqIdVal QuestionId: 0xF18, Value: 0x0 { 12 06 18 0F 00 00 }
0x5D75D: 					And  { 15 02 }
0x5D75F: 					EqIdVal QuestionId: 0xF19, Value: 0x0 { 12 06 19 0F 00 00 }
0x5D765: 					And  { 15 02 }
0x5D767: 					EqIdVal QuestionId: 0xF1A, Value: 0x0 { 12 06 1A 0F 00 00 }
0x5D76D: 					And  { 15 02 }
0x5D76F: 					EqIdVal QuestionId: 0xF1B, Value: 0x0 { 12 06 1B 0F 00 00 }
0x5D775: 					And  { 15 02 }
0x5D777: 					EqIdVal QuestionId: 0xF1C, Value: 0x0 { 12 06 1C 0F 00 00 }
0x5D77D: 					And  { 15 02 }
0x5D77F: 					StringRef1 String: "No" { 4E 04 C9 01 }
0x5D783: 					StringRef1 String: "No" { 4E 04 C8 01 }
0x5D787: 					Match  { 2A 02 }
0x5D789: 					And  { 15 02 }
0x5D78B: 				End  { 29 02 }
0x5D78D: 				GrayOutIf  { 19 82 }
0x5D78F: 					EqIdVal QuestionId: 0xF3E, Value: 0x1 { 12 06 3E 0F 01 00 }
0x5D795: 					OneOf Prompt: " Bluetooth 38.4MHz", Help: "Enables/Disables Bluetooth Endpoint in NHLT ACPI table. XTAL: 38.4MHz.
", QuestionFlags: 0x10, QuestionId: 0xF3D, VarStoreId: 0x7, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 11 A1 11 3D 0F 07 00 04 00 10 10 00 01 00 }
0x5D7A6: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D7AD: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D7B4: 					End  { 29 02 }
0x5D7B6: 				End  { 29 02 }
0x5D7B8: 				GrayOutIf  { 19 82 }
0x5D7BA: 					EqIdVal QuestionId: 0xF3D, Value: 0x1 { 12 06 3D 0F 01 00 }
0x5D7C0: 					OneOf Prompt: " Bluetooth 24MHz", Help: "Enables/Disables Bluetooth Endpoint in NHLT ACPI table. XTAL: 24MHz.
", QuestionFlags: 0x10, QuestionId: 0xF3E, VarStoreId: 0x7, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AA 11 AB 11 3E 0F 07 00 09 00 10 10 00 01 00 }
0x5D7D1: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D7D8: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D7DF: 					End  { 29 02 }
0x5D7E1: 				End  { 29 02 }
0x5D7E3: 			End  { 29 02 }
0x5D7E5: 			GrayOutIf  { 19 82 }
0x5D7E7: 				EqIdVal QuestionId: 0xF17, Value: 0x0 { 12 86 17 0F 00 00 }
0x5D7ED: 					EqIdVal QuestionId: 0xF18, Value: 0x0 { 12 06 18 0F 00 00 }
0x5D7F3: 					And  { 15 02 }
0x5D7F5: 					EqIdVal QuestionId: 0xF19, Value: 0x0 { 12 06 19 0F 00 00 }
0x5D7FB: 					And  { 15 02 }
0x5D7FD: 					EqIdVal QuestionId: 0xF1A, Value: 0x0 { 12 06 1A 0F 00 00 }
0x5D803: 					And  { 15 02 }
0x5D805: 					EqIdVal QuestionId: 0xF1B, Value: 0x0 { 12 06 1B 0F 00 00 }
0x5D80B: 					And  { 15 02 }
0x5D80D: 					EqIdVal QuestionId: 0xF1C, Value: 0x0 { 12 06 1C 0F 00 00 }
0x5D813: 					And  { 15 02 }
0x5D815: 				End  { 29 02 }
0x5D817: 				GrayOutIf  { 19 82 }
0x5D819: 					EqIdVal QuestionId: 0xF40, Value: 0x1 { 12 86 40 0F 01 00 }
0x5D81F: 						EqIdVal QuestionId: 0xF41, Value: 0x1 { 12 06 41 0F 01 00 }
0x5D825: 						Or  { 16 02 }
0x5D827: 					End  { 29 02 }
0x5D829: 					OneOf Prompt: " I2S Alc274 38.4MHz", Help: "Enables/Disables I2S Endpoint for ALC274 in NHLT ACPI table. XTAL: 38.4MHz.
", QuestionFlags: 0x10, QuestionId: 0xF3F, VarStoreId: 0x7, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A2 11 A3 11 3F 0F 07 00 05 00 10 10 00 01 00 }
0x5D83A: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D841: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D848: 					End  { 29 02 }
0x5D84A: 				End  { 29 02 }
0x5D84C: 				GrayOutIf  { 19 82 }
0x5D84E: 					EqIdVal QuestionId: 0xF3F, Value: 0x1 { 12 86 3F 0F 01 00 }
0x5D854: 						EqIdVal QuestionId: 0xF41, Value: 0x1 { 12 06 41 0F 01 00 }
0x5D85A: 						Or  { 16 02 }
0x5D85C: 					End  { 29 02 }
0x5D85E: 					OneOf Prompt: " I2S Alc274 24MHz", Help: "Enables/Disables I2S Endpoint for ALC274 in NHLT ACPI table. XTAL: 24MHz.
", QuestionFlags: 0x10, QuestionId: 0xF40, VarStoreId: 0x7, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AC 11 AD 11 40 0F 07 00 0A 00 10 10 00 01 00 }
0x5D86F: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D876: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D87D: 					End  { 29 02 }
0x5D87F: 				End  { 29 02 }
0x5D881: 				GrayOutIf  { 19 82 }
0x5D883: 					EqIdVal QuestionId: 0xF3F, Value: 0x1 { 12 86 3F 0F 01 00 }
0x5D889: 						EqIdVal QuestionId: 0xF40, Value: 0x1 { 12 06 40 0F 01 00 }
0x5D88F: 						Or  { 16 02 }
0x5D891: 					End  { 29 02 }
0x5D893: 					OneOf Prompt: " I2S Es8326 24MHz", Help: "Enables/Disables I2S Endpoint for Everest Codec 8326 and 8336 in NHLT ACPI table. XTAL: 24MHz.
", QuestionFlags: 0x10, QuestionId: 0xF41, VarStoreId: 0x7, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 AE 11 AF 11 41 0F 07 00 0B 00 10 10 00 01 00 }
0x5D8A4: 						OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5D8AB: 						OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5D8B2: 					End  { 29 02 }
0x5D8B4: 				End  { 29 02 }
0x5D8B6: 				OneOf Prompt: " I2S Codec Select", Help: "Selects I2S Audio Codec support.
Note: SerialIo UART0 must be disabled to enable external I2S codec (due to GPIO pin muxing).
", QuestionFlags: 0x10, QuestionId: 0xF42, VarStoreId: 0x6, VarOffset: 0x5B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 B0 11 B1 11 42 0F 06 00 B3 05 10 10 00 03 00 }
0x5D8C7: 					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5D8CE: 					OneOfOption Option: "Realtek ALC274" Value: 1 { 09 07 B2 11 00 00 01 }
0x5D8D5: 					OneOfOption Option: "Realtek ALC1308" Value: 2 { 09 07 B3 11 00 00 02 }
0x5D8DC: 					OneOfOption Option: "Everest ES8326" Value: 3 { 09 07 B4 11 00 00 03 }
0x5D8E3: 				End  { 29 02 }
0x5D8E5: 				OneOf Prompt: " I2S Codec Bus Number", Help: "Selectcs Codec Bus from Serial IO I2C0/1/2/3/4/5", QuestionFlags: 0x10, QuestionId: 0xF43, VarStoreId: 0x6, VarOffset: 0x5B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 B5 11 B6 11 43 0F 06 00 B4 05 10 10 00 05 00 }
0x5D8F6: 					OneOfOption Option: "I2C0 Controller" Value: 0, Default, MfgDefault { 09 07 88 17 30 00 00 }
0x5D8FD: 					OneOfOption Option: "I2C1 Controller" Value: 1 { 09 07 89 17 00 00 01 }
0x5D904: 					OneOfOption Option: "I2C2 Controller" Value: 2 { 09 07 8A 17 00 00 02 }
0x5D90B: 					OneOfOption Option: "I2C3 Controller" Value: 3 { 09 07 8B 17 00 00 03 }
0x5D912: 					OneOfOption Option: "I2C4 Controller" Value: 4 { 09 07 8C 17 00 00 04 }
0x5D919: 					OneOfOption Option: "I2C5 Controller" Value: 5 { 09 07 8D 17 00 00 05 }
0x5D920: 				End  { 29 02 }
0x5D922: 			End  { 29 02 }
0x5D924: 		End  { 29 02 }
0x5D926: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5D92D: 		End  { 29 02 }
0x5D92F: 		Text Prompt: "Audio DSP Feature Support:", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", Text: "" { 03 08 B7 11 B8 11 00 00 }
0x5D937: 		CheckBox Prompt: " WoV (Wake on Voice)", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF44, VarStoreId: 0x6, VarOffset: 0x800, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E B9 11 B8 11 44 0F 06 00 00 08 10 00 }
0x5D945: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x5D94B: 		End  { 29 02 }
0x5D94D: 		CheckBox Prompt: " Bluetooth Sideband", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x14, QuestionId: 0x2827, VarStoreId: 0x6, VarOffset: 0x801, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E BA 11 B8 11 27 28 06 00 01 08 14 00 }
0x5D95B: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x5D961: 		End  { 29 02 }
0x5D963: 		GrayOutIf  { 19 82 }
0x5D965: 			EqIdVal QuestionId: 0x2827, Value: 0x0 { 12 06 27 28 00 00 }
0x5D96B: 			CheckBox Prompt: " BT Intel HFP", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF45, VarStoreId: 0x6, VarOffset: 0x805, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E BC 11 B8 11 45 0F 06 00 05 08 10 00 }
0x5D979: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x5D97F: 			End  { 29 02 }
0x5D981: 			CheckBox Prompt: " BT Intel A2DP", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF46, VarStoreId: 0x6, VarOffset: 0x806, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E BD 11 B8 11 46 0F 06 00 06 08 10 00 }
0x5D98F: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x5D995: 			End  { 29 02 }
0x5D997: 			CheckBox Prompt: " BT Intel LE Audio", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF47, VarStoreId: 0x6, VarOffset: 0x809, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E C0 11 B8 11 47 0F 06 00 09 08 10 00 }
0x5D9A5: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5D9AB: 			End  { 29 02 }
0x5D9AD: 		End  { 29 02 }
0x5D9AF: 		CheckBox Prompt: " ACX/SDCA", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF48, VarStoreId: 0x6, VarOffset: 0x80A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E C1 11 B8 11 48 0F 06 00 0A 08 10 00 }
0x5D9BD: 		End  { 29 02 }
0x5D9BF: 		GrayOutIf  { 19 82 }
0x5D9C1: 			EqIdVal QuestionId: 0xF48, Value: 0x0 { 12 06 48 0F 00 00 }
0x5D9C7: 			CheckBox Prompt: " ACX/SDCA speaker aggregation", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF49, VarStoreId: 0x6, VarOffset: 0x80B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E C2 11 B8 11 49 0F 06 00 0B 08 10 00 }
0x5D9D5: 			End  { 29 02 }
0x5D9D7: 		End  { 29 02 }
0x5D9D9: 		CheckBox Prompt: " Codec based VAD", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF4A, VarStoreId: 0x6, VarOffset: 0x802, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E BB 11 B8 11 4A 0F 06 00 02 08 10 00 }
0x5D9E7: 		End  { 29 02 }
0x5D9E9: 		GrayOutIf  { 19 82 }
0x5D9EB: 			EqIdVal QuestionId: 0xF4C, Value: 0x1 { 12 06 4C 0F 01 00 }
0x5D9F1: 			CheckBox Prompt: " DSP based Speech
 Pre-Processing Disabled", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF4B, VarStoreId: 0x6, VarOffset: 0x807, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E BE 11 B8 11 4B 0F 06 00 07 08 10 00 }
0x5D9FF: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5DA05: 			End  { 29 02 }
0x5DA07: 		End  { 29 02 }
0x5DA09: 		OneOf Prompt: " Voice Activity Detection", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0xF4C, VarStoreId: 0x6, VarOffset: 0x808, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 11 B8 11 4C 0F 06 00 08 08 10 10 00 01 00 }
0x5DA1A: 			OneOfOption Option: "Intel Wake on Voice" Value: 0 { 09 07 C7 11 00 00 00 }
0x5DA21: 			OneOfOption Option: "Windows 10 Voice Activation" Value: 1, Default { 09 07 C8 11 10 00 01 }
0x5DA28: 		End  { 29 02 }
0x5DA2A: 		SuppressIf  { 0A 82 }
0x5DA2C: 			EqIdVal QuestionId: 0x1113, Value: 0x0 { 12 06 13 11 00 00 }
0x5DA32: 			OneOf Prompt: " Discrete BT HCI Audio Offload Support", Help: " Enables/Disables Discrete Bluetooth HCI Audio Offload Support", QuestionFlags: 0x10, QuestionId: 0xF4D, VarStoreId: 0x6, VarOffset: 0x80D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C3 11 C4 11 4D 0F 06 00 0D 08 10 10 00 01 00 }
0x5DA43: 				OneOfOption Option: "Disabled" Value: 0, Default { 09 07 04 00 10 00 00 }
0x5DA4A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DA51: 			End  { 29 02 }
0x5DA53: 			SuppressIf  { 0A 82 }
0x5DA55: 				EqIdVal QuestionId: 0xF4D, Value: 0x0 { 12 06 4D 0F 00 00 }
0x5DA5B: 				OneOf Prompt: " Discrete BT HCI Audio Offload Link", Help: " Selects used SSP port for the discrete BT HCI Audio Offload", QuestionFlags: 0x10, QuestionId: 0xF4E, VarStoreId: 0x6, VarOffset: 0x80E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0 { 05 91 C5 11 C6 11 4E 0F 06 00 0E 08 10 10 00 05 00 }
0x5DA6C: 					SuppressIf  { 0A 82 }
0x5DA6E: 						EqIdVal QuestionId: 0xF17, Value: 0x0 { 12 06 17 0F 00 00 }
0x5DA74: 						OneOfOption Option: "  SSP #0" Value: 0 { 09 07 56 11 00 00 00 }
0x5DA7B: 					End  { 29 02 }
0x5DA7D: 					SuppressIf  { 0A 82 }
0x5DA7F: 						EqIdVal QuestionId: 0xF18, Value: 0x0 { 12 06 18 0F 00 00 }
0x5DA85: 						OneOfOption Option: "  SSP #1" Value: 1 { 09 07 57 11 00 00 01 }
0x5DA8C: 					End  { 29 02 }
0x5DA8E: 					SuppressIf  { 0A 82 }
0x5DA90: 						EqIdVal QuestionId: 0xF19, Value: 0x0 { 12 06 19 0F 00 00 }
0x5DA96: 						OneOfOption Option: "  SSP #2" Value: 2 { 09 07 58 11 00 00 02 }
0x5DA9D: 					End  { 29 02 }
0x5DA9F: 					SuppressIf  { 0A 82 }
0x5DAA1: 						EqIdVal QuestionId: 0xF1A, Value: 0x0 { 12 06 1A 0F 00 00 }
0x5DAA7: 						OneOfOption Option: "  SSP #3" Value: 3 { 09 07 59 11 00 00 03 }
0x5DAAE: 					End  { 29 02 }
0x5DAB0: 					SuppressIf  { 0A 82 }
0x5DAB2: 						EqIdVal QuestionId: 0xF1B, Value: 0x0 { 12 06 1B 0F 00 00 }
0x5DAB8: 						OneOfOption Option: "  SSP #4" Value: 4 { 09 07 5A 11 00 00 04 }
0x5DABF: 					End  { 29 02 }
0x5DAC1: 					SuppressIf  { 0A 82 }
0x5DAC3: 						EqIdVal QuestionId: 0xF1C, Value: 0x0 { 12 06 1C 0F 00 00 }
0x5DAC9: 						OneOfOption Option: "  SSP #5" Value: 5 { 09 07 5B 11 00 00 05 }
0x5DAD0: 					End  { 29 02 }
0x5DAD2: 				End  { 29 02 }
0x5DAD4: 			End  { 29 02 }
0x5DAD6: 		End  { 29 02 }
0x5DAD8: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5DADF: 		End  { 29 02 }
0x5DAE1: 		Text Prompt: "Audio DSP Pre/Post-Processing Module Support:", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", Text: "" { 03 08 C9 11 CA 11 00 00 }
0x5DAE9: 		CheckBox Prompt: " Waves Post-process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF4F, VarStoreId: 0x6, VarOffset: 0x5BE, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CB 11 CA 11 4F 0F 06 00 BE 05 10 00 }
0x5DAF7: 		End  { 29 02 }
0x5DAF9: 		CheckBox Prompt: " DTS", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF50, VarStoreId: 0x6, VarOffset: 0x5BF, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CC 11 CA 11 50 0F 06 00 BF 05 10 00 }
0x5DB07: 		End  { 29 02 }
0x5DB09: 		CheckBox Prompt: " IntelSST Speech", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF51, VarStoreId: 0x6, VarOffset: 0x5C0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CD 11 CA 11 51 0F 06 00 C0 05 10 00 }
0x5DB17: 		End  { 29 02 }
0x5DB19: 		CheckBox Prompt: " Dolby", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF52, VarStoreId: 0x6, VarOffset: 0x5C1, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CE 11 CA 11 52 0F 06 00 C1 05 10 00 }
0x5DB27: 		End  { 29 02 }
0x5DB29: 		CheckBox Prompt: " Waves Pre-process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF53, VarStoreId: 0x6, VarOffset: 0x5C2, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E CF 11 CA 11 53 0F 06 00 C2 05 10 00 }
0x5DB37: 		End  { 29 02 }
0x5DB39: 		CheckBox Prompt: " Audyssey", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF54, VarStoreId: 0x6, VarOffset: 0x5C3, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D0 11 CA 11 54 0F 06 00 C3 05 10 00 }
0x5DB47: 		End  { 29 02 }
0x5DB49: 		CheckBox Prompt: " Maxim Smart AMP", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF55, VarStoreId: 0x6, VarOffset: 0x5C4, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D1 11 CA 11 55 0F 06 00 C4 05 10 00 }
0x5DB57: 		End  { 29 02 }
0x5DB59: 		CheckBox Prompt: " ForteMedia SAMSoft", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF56, VarStoreId: 0x6, VarOffset: 0x5C5, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D2 11 CA 11 56 0F 06 00 C5 05 10 00 }
0x5DB67: 		End  { 29 02 }
0x5DB69: 		CheckBox Prompt: " Sound Research IP", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF57, VarStoreId: 0x6, VarOffset: 0x5C7, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D3 11 CA 11 57 0F 06 00 C7 05 10 00 }
0x5DB77: 		End  { 29 02 }
0x5DB79: 		CheckBox Prompt: " Conexant Pre-Process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF58, VarStoreId: 0x6, VarOffset: 0x5C8, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D4 11 CA 11 58 0F 06 00 C8 05 10 00 }
0x5DB87: 		End  { 29 02 }
0x5DB89: 		CheckBox Prompt: " Conexant Smart Amp", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF59, VarStoreId: 0x6, VarOffset: 0x5C9, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D5 11 CA 11 59 0F 06 00 C9 05 10 00 }
0x5DB97: 		End  { 29 02 }
0x5DB99: 		CheckBox Prompt: " Realtek Post-Process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF5A, VarStoreId: 0x6, VarOffset: 0x5CA, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D6 11 CA 11 5A 0F 06 00 CA 05 10 00 }
0x5DBA7: 		End  { 29 02 }
0x5DBA9: 		CheckBox Prompt: " Realtek Smart Amp", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF5B, VarStoreId: 0x6, VarOffset: 0x5CB, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D7 11 CA 11 5B 0F 06 00 CB 05 10 00 }
0x5DBB7: 		End  { 29 02 }
0x5DBB9: 		CheckBox Prompt: " Icepower IP MFX sub module", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF5C, VarStoreId: 0x6, VarOffset: 0x5CC, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D8 11 CA 11 5C 0F 06 00 CC 05 10 00 }
0x5DBC7: 		End  { 29 02 }
0x5DBC9: 		CheckBox Prompt: " Icepower IP EFX sub module", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF5D, VarStoreId: 0x6, VarOffset: 0x5CD, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D9 11 CA 11 5D 0F 06 00 CD 05 10 00 }
0x5DBD7: 		End  { 29 02 }
0x5DBD9: 		CheckBox Prompt: " Icepower IP SFX sub module", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF5E, VarStoreId: 0x6, VarOffset: 0x5CE, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DA 11 CA 11 5E 0F 06 00 CE 05 10 00 }
0x5DBE7: 		End  { 29 02 }
0x5DBE9: 		CheckBox Prompt: " Voice Preprocessing", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF5F, VarStoreId: 0x6, VarOffset: 0x5CF, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DB 11 CA 11 5F 0F 06 00 CF 05 10 00 }
0x5DBF7: 		End  { 29 02 }
0x5DBF9: 		CheckBox Prompt: " Acoustic Context Awareness (ACA)", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF60, VarStoreId: 0x6, VarOffset: 0x5D0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DC 11 CA 11 60 0F 06 00 D0 05 10 00 }
0x5DC07: 		End  { 29 02 }
0x5DC09: 		CheckBox Prompt: " Custom Module 'Alpha'", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF61, VarStoreId: 0x6, VarOffset: 0x5DB, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DD 11 CA 11 61 0F 06 00 DB 05 10 00 }
0x5DC17: 		End  { 29 02 }
0x5DC19: 		SuppressIf  { 0A 82 }
0x5DC1B: 			EqIdVal QuestionId: 0xF61, Value: 0x0 { 12 06 61 0F 00 00 }
0x5DC21: 			String Prompt: " 'Alpha' GUID:", Help: "Input hex digit character in aabbccdd-eeff-gghh-iijj-kkllmmnnoopp format.", QuestionFlags: 0x10, QuestionId: 0xF62, VarStoreId: 0x6, VarStoreInfo: 0x5DE, MinSize: 0x24, MaxSize: 0x24, Flags: 0x0 { 1C 90 DE 11 E3 11 62 0F 06 00 DE 05 10 24 24 00 }
0x5DC31: 			End  { 29 02 }
0x5DC33: 		End  { 29 02 }
0x5DC35: 		CheckBox Prompt: " Custom Module 'Beta'", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF63, VarStoreId: 0x6, VarOffset: 0x5DC, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E DF 11 CA 11 63 0F 06 00 DC 05 10 00 }
0x5DC43: 		End  { 29 02 }
0x5DC45: 		SuppressIf  { 0A 82 }
0x5DC47: 			EqIdVal QuestionId: 0xF63, Value: 0x0 { 12 06 63 0F 00 00 }
0x5DC4D: 			String Prompt: " 'Beta'  GUID:", Help: "Input hex digit character in aabbccdd-eeff-gghh-iijj-kkllmmnnoopp format.", QuestionFlags: 0x10, QuestionId: 0xF64, VarStoreId: 0x6, VarStoreInfo: 0x628, MinSize: 0x24, MaxSize: 0x24, Flags: 0x0 { 1C 90 E0 11 E3 11 64 0F 06 00 28 06 10 24 24 00 }
0x5DC5D: 			End  { 29 02 }
0x5DC5F: 		End  { 29 02 }
0x5DC61: 		CheckBox Prompt: " Custom Module 'Gamma'", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0xF65, VarStoreId: 0x6, VarOffset: 0x5DD, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E E1 11 CA 11 65 0F 06 00 DD 05 10 00 }
0x5DC6F: 		End  { 29 02 }
0x5DC71: 		SuppressIf  { 0A 82 }
0x5DC73: 			EqIdVal QuestionId: 0xF65, Value: 0x0 { 12 06 65 0F 00 00 }
0x5DC79: 			String Prompt: " 'Gamma' GUID:", Help: "Input hex digit character in aabbccdd-eeff-gghh-iijj-kkllmmnnoopp format.", QuestionFlags: 0x10, QuestionId: 0xF66, VarStoreId: 0x6, VarStoreInfo: 0x672, MinSize: 0x24, MaxSize: 0x24, Flags: 0x0 { 1C 90 E2 11 E3 11 66 0F 06 00 72 06 10 24 24 00 }
0x5DC89: 			End  { 29 02 }
0x5DC8B: 		End  { 29 02 }
0x5DC8D: 	End  { 29 02 }
0x5DC8F: 	Form FormId: 0x2851, Title: "Security Configuration" { 01 86 51 28 37 12 }
0x5DC95: 		Subtitle Prompt: "Security Configuration", Help: "", Flags: 0x0 { 02 87 37 12 00 00 00 }
0x5DC9C: 		End  { 29 02 }
0x5DC9E: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5DCA5: 		End  { 29 02 }
0x5DCA7: 		OneOf Prompt: "RTC Memory Lock", Help: "Enable will lock bytes 38h-3Fh in the lower/upper 128-byte bank of RTC RAM", QuestionFlags: 0x10, QuestionId: 0xF67, VarStoreId: 0x6, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 39 12 3A 12 67 0F 06 00 1B 00 10 10 00 01 00 }
0x5DCB8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5DCBF: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5DCC6: 		End  { 29 02 }
0x5DCC8: 		SuppressIf  { 0A 82 }
0x5DCCA: 			True  { 46 02 }
0x5DCCC: 			OneOf Prompt: "BIOS Lock", Help: "Enable/Disable the PCH BIOS Lock Enable feature. Required to be enabled to ensure SMM protection of flash.", QuestionFlags: 0x10, QuestionId: 0xF68, VarStoreId: 0x6, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3B 12 3C 12 68 0F 06 00 1C 00 10 10 00 01 00 }
0x5DCDD: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5DCE4: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5DCEB: 			End  { 29 02 }
0x5DCED: 		End  { 29 02 }
0x5DCEF: 		OneOf Prompt: "Force unlock on all GPIO pads", Help: "If Enabled BIOS will force all GPIO pads to be in unlocked state", QuestionFlags: 0x10, QuestionId: 0xF69, VarStoreId: 0x6, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 12 3E 12 69 0F 06 00 1D 00 10 10 00 01 00 }
0x5DD00: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DD07: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DD0E: 		End  { 29 02 }
0x5DD10: 	End  { 29 02 }
0x5DD12: 	Form FormId: 0x7A, Title: "SerialIo Configuration" { 01 86 7A 00 7D 17 }
0x5DD18: 		Subtitle Prompt: "SerialIo Configuration", Help: "", Flags: 0x0 { 02 87 7D 17 00 00 00 }
0x5DD1F: 		End  { 29 02 }
0x5DD21: 		GrayOutIf  { 19 82 }
0x5DD23: 			EqIdVal QuestionId: 0xF6B, Value: 0x1 { 12 86 6B 0F 01 00 }
0x5DD29: 				EqIdVal QuestionId: 0xF6C, Value: 0x1 { 12 06 6C 0F 01 00 }
0x5DD2F: 				Or  { 16 02 }
0x5DD31: 				EqIdVal QuestionId: 0xF6D, Value: 0x1 { 12 06 6D 0F 01 00 }
0x5DD37: 				Or  { 16 02 }
0x5DD39: 			End  { 29 02 }
0x5DD3B: 			OneOf Prompt: "I2C0 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF6A, VarStoreId: 0x6, VarOffset: 0x705, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 88 17 84 17 6A 0F 06 00 05 07 10 10 00 01 00 }
0x5DD4C: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5DD53: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5DD5A: 			End  { 29 02 }
0x5DD5C: 		End  { 29 02 }
0x5DD5E: 		GrayOutIf  { 19 82 }
0x5DD60: 			EqIdVal QuestionId: 0xF6A, Value: 0x0 { 12 06 6A 0F 00 00 }
0x5DD66: 			OneOf Prompt: "I2C1 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF6B, VarStoreId: 0x6, VarOffset: 0x706, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 17 84 17 6B 0F 06 00 06 07 10 10 00 01 00 }
0x5DD77: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DD7E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DD85: 			End  { 29 02 }
0x5DD87: 		End  { 29 02 }
0x5DD89: 		GrayOutIf  { 19 82 }
0x5DD8B: 			EqIdVal QuestionId: 0xF6A, Value: 0x0 { 12 06 6A 0F 00 00 }
0x5DD91: 			OneOf Prompt: "I2C2 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF6C, VarStoreId: 0x6, VarOffset: 0x707, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8A 17 84 17 6C 0F 06 00 07 07 10 10 00 01 00 }
0x5DDA2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DDA9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DDB0: 			End  { 29 02 }
0x5DDB2: 		End  { 29 02 }
0x5DDB4: 		GrayOutIf  { 19 82 }
0x5DDB6: 			EqIdVal QuestionId: 0xF6A, Value: 0x0 { 12 06 6A 0F 00 00 }
0x5DDBC: 			OneOf Prompt: "I2C3 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF6D, VarStoreId: 0x6, VarOffset: 0x708, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8B 17 84 17 6D 0F 06 00 08 07 10 10 00 01 00 }
0x5DDCD: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DDD4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DDDB: 			End  { 29 02 }
0x5DDDD: 		End  { 29 02 }
0x5DDDF: 		OneOf Prompt: "I2C4 Controller", Help: "Enables/Disables SerialIo Controller
For I2C5 and UART2 to work this device has to be enabled", QuestionFlags: 0x10, QuestionId: 0xF6E, VarStoreId: 0x6, VarOffset: 0x709, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8C 17 85 17 6E 0F 06 00 09 07 10 10 00 01 00 }
0x5DDF0: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DDF7: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DDFE: 		End  { 29 02 }
0x5DE00: 		OneOf Prompt: "I2C5 Controller", Help: "Enables/Disables SerialIo Controller
For this device to work I2C4 has to be enabled", QuestionFlags: 0x10, QuestionId: 0xF6F, VarStoreId: 0x6, VarOffset: 0x70A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8D 17 86 17 6F 0F 06 00 0A 07 10 10 00 01 00 }
0x5DE11: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DE18: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DE1F: 		End  { 29 02 }
0x5DE21: 		OneOf Prompt: "I2C6 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF70, VarStoreId: 0x6, VarOffset: 0x70B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8E 17 84 17 70 0F 06 00 0B 07 10 10 00 01 00 }
0x5DE32: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DE39: 			SuppressIf  { 0A 82 }
0x5DE3B: 				EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x5DE41: 					Not  { 17 02 }
0x5DE43: 				End  { 29 02 }
0x5DE45: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DE4C: 			End  { 29 02 }
0x5DE4E: 		End  { 29 02 }
0x5DE50: 		OneOf Prompt: "I2C7 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF71, VarStoreId: 0x6, VarOffset: 0x70C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 8F 17 84 17 71 0F 06 00 0C 07 10 10 00 01 00 }
0x5DE61: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DE68: 			SuppressIf  { 0A 82 }
0x5DE6A: 				EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x5DE70: 					Not  { 17 02 }
0x5DE72: 				End  { 29 02 }
0x5DE74: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DE7B: 			End  { 29 02 }
0x5DE7D: 		End  { 29 02 }
0x5DE7F: 		OneOf Prompt: "SPI0 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF72, VarStoreId: 0x6, VarOffset: 0x6E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 90 17 84 17 72 0F 06 00 E0 06 10 10 00 01 00 }
0x5DE90: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DE97: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DE9E: 		End  { 29 02 }
0x5DEA0: 		OneOf Prompt: "SPI1 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF73, VarStoreId: 0x6, VarOffset: 0x6E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 91 17 84 17 73 0F 06 00 E1 06 10 10 00 01 00 }
0x5DEB1: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5DEB7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5DEBE: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DEC5: 		End  { 29 02 }
0x5DEC7: 		OneOf Prompt: "SPI2 Controller", Help: "Enables/Disables SerialIo SPI2 Controller
The following device depends from:
Thermal Subsystem in PCI mode
Otherwise SPI2 will not appear in the OS", QuestionFlags: 0x10, QuestionId: 0xF74, VarStoreId: 0x6, VarOffset: 0x6E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 92 17 87 17 74 0F 06 00 E2 06 10 10 00 01 00 }
0x5DED8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DEDF: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DEE6: 		End  { 29 02 }
0x5DEE8: 		OneOf Prompt: "SPI3 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF75, VarStoreId: 0x6, VarOffset: 0x6E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 93 17 84 17 75 0F 06 00 E3 06 10 10 00 01 00 }
0x5DEF9: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DF00: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DF07: 		End  { 29 02 }
0x5DF09: 		SuppressIf  { 0A 82 }
0x5DF0B: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x5DF11: 				Not  { 17 02 }
0x5DF13: 			End  { 29 02 }
0x5DF15: 			OneOf Prompt: "SPI4 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF76, VarStoreId: 0x6, VarOffset: 0x6E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 94 17 84 17 76 0F 06 00 E4 06 10 10 00 01 00 }
0x5DF26: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DF2D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DF34: 			End  { 29 02 }
0x5DF36: 		End  { 29 02 }
0x5DF38: 		SuppressIf  { 0A 82 }
0x5DF3A: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x5DF40: 				Not  { 17 02 }
0x5DF42: 			End  { 29 02 }
0x5DF44: 			OneOf Prompt: "SPI5 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF77, VarStoreId: 0x6, VarOffset: 0x6E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 95 17 84 17 77 0F 06 00 E5 06 10 10 00 01 00 }
0x5DF55: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DF5C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DF63: 			End  { 29 02 }
0x5DF65: 		End  { 29 02 }
0x5DF67: 		SuppressIf  { 0A 82 }
0x5DF69: 			EqIdVal QuestionId: 0x1112, Value: 0x2 { 12 86 12 11 02 00 }
0x5DF6F: 				Not  { 17 02 }
0x5DF71: 			End  { 29 02 }
0x5DF73: 			OneOf Prompt: "SPI6 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF78, VarStoreId: 0x6, VarOffset: 0x6E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 96 17 84 17 78 0F 06 00 E6 06 10 10 00 01 00 }
0x5DF84: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DF8B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DF92: 			End  { 29 02 }
0x5DF94: 		End  { 29 02 }
0x5DF96: 		GrayOutIf  { 19 82 }
0x5DF98: 			EqIdValList QuestionId: 0xF42, Values: [1, 2, 3] { 14 0C 42 0F 03 00 01 00 02 00 03 00 }
0x5DFA4: 			OneOf Prompt: "UART0 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF79, VarStoreId: 0x6, VarOffset: 0x6E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 99 17 84 17 79 0F 06 00 E9 06 10 10 00 03 00 }
0x5DFB5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DFBC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DFC3: 				OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5DFCA: 			End  { 29 02 }
0x5DFCC: 		End  { 29 02 }
0x5DFCE: 		OneOf Prompt: "UART1 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF7A, VarStoreId: 0x6, VarOffset: 0x6EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 9A 17 84 17 7A 0F 06 00 EA 06 10 10 00 03 00 }
0x5DFDF: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5DFE6: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5DFED: 			OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5DFF4: 		End  { 29 02 }
0x5DFF6: 		SuppressIf  { 0A 82 }
0x5DFF8: 			EqIdVal QuestionId: 0x505, Value: 0x3 { 12 06 05 05 03 00 }
0x5DFFE: 			OneOf Prompt: "UART2 Controller", Help: "Set UART2 mode
 - DBG used for BIOS log print and/or Kernel OS Debug 
 - COM - 16550 compatible serial port with Power Gating support", QuestionFlags: 0x10, QuestionId: 0xF7B, VarStoreId: 0x6, VarOffset: 0x6EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 9B 17 A1 17 7B 0F 06 00 EB 06 10 10 00 03 00 }
0x5E00F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E016: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5E01D: 				OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5E024: 			End  { 29 02 }
0x5E026: 		End  { 29 02 }
0x5E028: 		OneOf Prompt: "UART3 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF7C, VarStoreId: 0x6, VarOffset: 0x6EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 9C 17 84 17 7C 0F 06 00 EC 06 10 10 00 03 00 }
0x5E039: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E040: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5E047: 			OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5E04E: 		End  { 29 02 }
0x5E050: 		OneOf Prompt: "UART4 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF7D, VarStoreId: 0x6, VarOffset: 0x6ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 9D 17 84 17 7D 0F 06 00 ED 06 10 10 00 03 00 }
0x5E061: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E068: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5E06F: 			OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5E076: 		End  { 29 02 }
0x5E078: 		OneOf Prompt: "UART5 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF7E, VarStoreId: 0x6, VarOffset: 0x6EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 9E 17 84 17 7E 0F 06 00 EE 06 10 10 00 03 00 }
0x5E089: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E090: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5E097: 			OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5E09E: 		End  { 29 02 }
0x5E0A0: 		OneOf Prompt: "UART6 Controller", Help: "Enables/Disables SerialIo Controller
If given device is Function 0 PSF disabling is skipped. PSF default will remain and device PCI CFG Space will still be visible. This is needed to allow PCI enumerator access functions above 0 in a multifunction device.
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5

 UART 0 (00:30:00) cannot be disabled when:
1. Child device is enabled like CNVi Bluetooth (\_SB.PC00.UA00.BTH0)
 UART 0 (00:30:00) cannot be enabled when:
1. I2S Audio codec is enabled (\_SB.PC00.I2C0.HDAC)", QuestionFlags: 0x10, QuestionId: 0xF7F, VarStoreId: 0x6, VarOffset: 0x6EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 9F 17 84 17 7F 0F 06 00 EF 06 10 10 00 03 00 }
0x5E0B1: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E0B8: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5E0BF: 			OneOfOption Option: "Communication port (COM)" Value: 3 { 09 07 A0 17 00 00 03 }
0x5E0C6: 		End  { 29 02 }
0x5E0C8: 		SuppressIf  { 0A 82 }
0x5E0CA: 			EqIdVal QuestionId: 0x505, Value: 0x3 { 12 86 05 05 03 00 }
0x5E0D0: 				Not  { 17 02 }
0x5E0D2: 			End  { 29 02 }
0x5E0D4: 			Text Prompt: "UART2 Controller", Help: "", Text: "used as debug port" { 03 08 9B 17 C9 07 E7 17 }
0x5E0DC: 		End  { 29 02 }
0x5E0DE: 		OneOf Prompt: "GPIO IRQ Route", Help: "Route all GPIOs to one of the IRQ.", QuestionFlags: 0x10, QuestionId: 0xF80, VarStoreId: 0x6, VarOffset: 0x70F, Flags: 0x10, Size: 8, Min: 0xE, Max: 0xF, Step: 0x0 { 05 91 5D 17 5E 17 80 0F 06 00 0F 07 10 10 0E 0F 00 }
0x5E0EF: 			OneOfOption Option: "IRQ14" Value: 14, Default, MfgDefault { 09 07 5F 17 30 00 0E }
0x5E0F6: 			OneOfOption Option: "IRQ15" Value: 15 { 09 07 60 17 00 00 0F }
0x5E0FD: 		End  { 29 02 }
0x5E0FF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E106: 		End  { 29 02 }
0x5E108: 		SuppressIf  { 0A 82 }
0x5E10A: 			EqIdVal QuestionId: 0xF6A, Value: 0x0 { 12 06 6A 0F 00 00 }
0x5E110: 			Ref Prompt: "Serial IO I2C0 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF81, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x80 { 0F 0F CC 17 CB 17 81 0F 00 00 FF FF 00 80 00 }
0x5E11F: 		End  { 29 02 }
0x5E121: 		SuppressIf  { 0A 82 }
0x5E123: 			EqIdVal QuestionId: 0xF6B, Value: 0x0 { 12 06 6B 0F 00 00 }
0x5E129: 			Ref Prompt: "Serial IO I2C1 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF82, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x81 { 0F 0F CD 17 CB 17 82 0F 00 00 FF FF 00 81 00 }
0x5E138: 		End  { 29 02 }
0x5E13A: 		SuppressIf  { 0A 82 }
0x5E13C: 			EqIdVal QuestionId: 0xF6C, Value: 0x0 { 12 06 6C 0F 00 00 }
0x5E142: 			Ref Prompt: "Serial IO I2C2 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF83, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x87 { 0F 0F CE 17 CB 17 83 0F 00 00 FF FF 00 87 00 }
0x5E151: 		End  { 29 02 }
0x5E153: 		SuppressIf  { 0A 82 }
0x5E155: 			EqIdVal QuestionId: 0xF6D, Value: 0x0 { 12 06 6D 0F 00 00 }
0x5E15B: 			Ref Prompt: "Serial IO I2C3 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF84, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x88 { 0F 0F CF 17 CB 17 84 0F 00 00 FF FF 00 88 00 }
0x5E16A: 		End  { 29 02 }
0x5E16C: 		SuppressIf  { 0A 82 }
0x5E16E: 			EqIdVal QuestionId: 0xF6E, Value: 0x0 { 12 86 6E 0F 00 00 }
0x5E174: 				EqIdVal QuestionId: 0x1111, Value: 0x1 { 12 06 11 11 01 00 }
0x5E17A: 				Or  { 16 02 }
0x5E17C: 			End  { 29 02 }
0x5E17E: 			Ref Prompt: "Serial IO I2C4 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF85, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x89 { 0F 0F D0 17 CB 17 85 0F 00 00 FF FF 00 89 00 }
0x5E18D: 		End  { 29 02 }
0x5E18F: 		SuppressIf  { 0A 82 }
0x5E191: 			EqIdVal QuestionId: 0xF6F, Value: 0x0 { 12 06 6F 0F 00 00 }
0x5E197: 			Ref Prompt: "Serial IO I2C5 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF86, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x8A { 0F 0F D1 17 CB 17 86 0F 00 00 FF FF 00 8A 00 }
0x5E1A6: 		End  { 29 02 }
0x5E1A8: 		SuppressIf  { 0A 82 }
0x5E1AA: 			EqIdVal QuestionId: 0xF70, Value: 0x0 { 12 06 70 0F 00 00 }
0x5E1B0: 			Ref Prompt: "Serial IO I2C6 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF87, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x99 { 0F 0F D2 17 CB 17 87 0F 00 00 FF FF 00 99 00 }
0x5E1BF: 		End  { 29 02 }
0x5E1C1: 		SuppressIf  { 0A 82 }
0x5E1C3: 			EqIdVal QuestionId: 0xF71, Value: 0x0 { 12 06 71 0F 00 00 }
0x5E1C9: 			Ref Prompt: "Serial IO I2C7 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF88, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x9A { 0F 0F D3 17 CB 17 88 0F 00 00 FF FF 00 9A 00 }
0x5E1D8: 		End  { 29 02 }
0x5E1DA: 		SuppressIf  { 0A 82 }
0x5E1DC: 			EqIdVal QuestionId: 0xF72, Value: 0x0 { 12 06 72 0F 00 00 }
0x5E1E2: 			Ref Prompt: "Serial IO SPI0 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF89, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x82 { 0F 0F D4 17 CB 17 89 0F 00 00 FF FF 00 82 00 }
0x5E1F1: 		End  { 29 02 }
0x5E1F3: 		SuppressIf  { 0A 82 }
0x5E1F5: 			EqIdVal QuestionId: 0xF73, Value: 0x0 { 12 06 73 0F 00 00 }
0x5E1FB: 			Ref Prompt: "Serial IO SPI1 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF8A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x83 { 0F 0F D5 17 CB 17 8A 0F 00 00 FF FF 00 83 00 }
0x5E20A: 		End  { 29 02 }
0x5E20C: 		SuppressIf  { 0A 82 }
0x5E20E: 			EqIdVal QuestionId: 0xF74, Value: 0x0 { 12 06 74 0F 00 00 }
0x5E214: 			Ref Prompt: "Serial IO SPI2 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF8B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x8C { 0F 0F D6 17 CB 17 8B 0F 00 00 FF FF 00 8C 00 }
0x5E223: 		End  { 29 02 }
0x5E225: 		SuppressIf  { 0A 82 }
0x5E227: 			EqIdVal QuestionId: 0xF79, Value: 0x0 { 12 86 79 0F 00 00 }
0x5E22D: 				EqIdVal QuestionId: 0x505, Value: 0x1 { 12 06 05 05 01 00 }
0x5E233: 				Or  { 16 02 }
0x5E235: 			End  { 29 02 }
0x5E237: 			Ref Prompt: "Serial IO UART0 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF8C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x84 { 0F 0F D9 17 CB 17 8C 0F 00 00 FF FF 00 84 00 }
0x5E246: 		End  { 29 02 }
0x5E248: 		SuppressIf  { 0A 82 }
0x5E24A: 			EqIdVal QuestionId: 0xF7A, Value: 0x0 { 12 86 7A 0F 00 00 }
0x5E250: 				EqIdVal QuestionId: 0x505, Value: 0x2 { 12 06 05 05 02 00 }
0x5E256: 				Or  { 16 02 }
0x5E258: 			End  { 29 02 }
0x5E25A: 			Ref Prompt: "Serial IO UART1 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF8D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x85 { 0F 0F DA 17 CB 17 8D 0F 00 00 FF FF 00 85 00 }
0x5E269: 		End  { 29 02 }
0x5E26B: 		SuppressIf  { 0A 82 }
0x5E26D: 			EqIdVal QuestionId: 0xF7B, Value: 0x0 { 12 06 7B 0F 00 00 }
0x5E273: 			Ref Prompt: "Serial IO UART2 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xF8E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x8B { 0F 0F DB 17 CB 17 8E 0F 00 00 FF FF 00 8B 00 }
0x5E282: 		End  { 29 02 }
0x5E284: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E28B: 		End  { 29 02 }
0x5E28D: 		OneOf Prompt: "WITT/MITT Test Device", Help: "Choose if WITT Device is used and with which controller", QuestionFlags: 0x10, QuestionId: 0xF8F, VarStoreId: 0xF101, VarOffset: 0x5EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x0 { 05 91 A3 17 A4 17 8F 0F 01 F1 EF 05 10 10 00 09 00 }
0x5E29E: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E2A5: 			OneOfOption Option: "Enabled - I2C0" Value: 1 { 09 07 DC 17 00 00 01 }
0x5E2AC: 			OneOfOption Option: "Enabled - I2C1" Value: 2 { 09 07 DD 17 00 00 02 }
0x5E2B3: 			OneOfOption Option: "Enabled - I2C2" Value: 3 { 09 07 DE 17 00 00 03 }
0x5E2BA: 			OneOfOption Option: "Enabled - I2C3" Value: 4 { 09 07 DF 17 00 00 04 }
0x5E2C1: 			OneOfOption Option: "Enabled - I2C4" Value: 5 { 09 07 E0 17 00 00 05 }
0x5E2C8: 			OneOfOption Option: "Enabled - I2C5" Value: 6 { 09 07 E1 17 00 00 06 }
0x5E2CF: 			OneOfOption Option: "Enabled - SPI0" Value: 7 { 09 07 E2 17 00 00 07 }
0x5E2D6: 			OneOfOption Option: "Enabled - SPI1" Value: 8 { 09 07 E3 17 00 00 08 }
0x5E2DD: 			OneOfOption Option: "Enabled - SPI2" Value: 9 { 09 07 E4 17 00 00 09 }
0x5E2E4: 		End  { 29 02 }
0x5E2E6: 		SuppressIf  { 0A 82 }
0x5E2E8: 			EqIdVal QuestionId: 0xF8F, Value: 0x0 { 12 06 8F 0F 00 00 }
0x5E2EE: 			OneOf Prompt: "WITT/MITT Device selection", Help: "Change WITT Device version", QuestionFlags: 0x10, QuestionId: 0xF90, VarStoreId: 0xF101, VarOffset: 0x5F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A5 17 A6 17 90 0F 01 F1 F0 05 10 10 00 01 00 }
0x5E2FF: 				OneOfOption Option: "WITT" Value: 0 { 09 07 E5 17 00 00 00 }
0x5E306: 				OneOfOption Option: "MITT" Value: 1, Default, MfgDefault { 09 07 E6 17 30 00 01 }
0x5E30D: 			End  { 29 02 }
0x5E30F: 		End  { 29 02 }
0x5E311: 		OneOf Prompt: "UART Test Device", Help: "Choose if UART Test Device is used and with which controller", QuestionFlags: 0x10, QuestionId: 0xF91, VarStoreId: 0xF101, VarOffset: 0x5F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 97 17 98 17 91 0F 01 F1 F1 05 10 10 00 03 00 }
0x5E322: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5E329: 			OneOfOption Option: "Enabled - UART0" Value: 1 { 09 07 81 17 00 00 01 }
0x5E330: 			OneOfOption Option: "Enabled - UART1" Value: 2 { 09 07 82 17 00 00 02 }
0x5E337: 			OneOfOption Option: "Enabled - UART2" Value: 3 { 09 07 83 17 00 00 03 }
0x5E33E: 		End  { 29 02 }
0x5E340: 		CheckBox Prompt: "Additional Serial IO devices", Help: "When enabled, ACPI will report additional devices connected to Serial IO.", QuestionFlags: 0x10, QuestionId: 0xF92, VarStoreId: 0x6, VarOffset: 0x713, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E D7 17 D8 17 92 0F 06 00 13 07 10 00 }
0x5E34E: 		End  { 29 02 }
0x5E350: 		CheckBox Prompt: "SerialIO timing parameters", Help: "Enables additional timing parameters for all SeraialIO controllers.
Defaults can be changed in each controller setting.
Platform restart required to apply changes", QuestionFlags: 0x10, QuestionId: 0xF93, VarStoreId: 0xF101, VarOffset: 0x5F4, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E C4 17 C5 17 93 0F 01 F1 F4 05 10 00 }
0x5E35E: 		End  { 29 02 }
0x5E360: 	End  { 29 02 }
0x5E362: 	Form FormId: 0x80, Title: "Serial IO I2C0 Settings" { 01 86 80 00 CC 17 }
0x5E368: 		Subtitle Prompt: "Serial IO I2C0 Settings", Help: "", Flags: 0x0 { 02 87 CC 17 00 00 00 }
0x5E36F: 		End  { 29 02 }
0x5E371: 		SuppressIf  { 0A 82 }
0x5E373: 			True  { 46 02 }
0x5E375: 			Numeric Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xF94, VarStoreId: 0xF101, VarOffset: 0x5D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 03 18 04 18 94 0F 01 F1 D0 05 00 10 00 FF 00 }
0x5E386: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5E38C: 			End  { 29 02 }
0x5E38E: 		End  { 29 02 }
0x5E390: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E397: 		End  { 29 02 }
0x5E399: 		SuppressIf  { 0A 82 }
0x5E39B: 			EqIdValList QuestionId: 0xF94, Values: [1, 3, 5, 7] { 14 8E 94 0F 04 00 01 00 03 00 05 00 07 00 }
0x5E3A9: 				Not  { 17 02 }
0x5E3AB: 			End  { 29 02 }
0x5E3AD: 			Ref Prompt: "Serial IO Touch Pad Settings", Help: "Indicates what type of I2C Touch Pad is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xF95, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2855 { 0F 0F ED 17 EF 17 95 0F 00 00 FF FF 00 55 28 }
0x5E3BC: 		End  { 29 02 }
0x5E3BE: 		SuppressIf  { 0A 82 }
0x5E3C0: 			EqIdValList QuestionId: 0xF94, Values: [2, 3, 6, 7] { 14 8E 94 0F 04 00 02 00 03 00 06 00 07 00 }
0x5E3CE: 				Not  { 17 02 }
0x5E3D0: 			End  { 29 02 }
0x5E3D2: 			Ref Prompt: "Serial IO Touch Panel Settings", Help: "Indicates what type of I2C Touch Panel is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xF96, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2856 { 0F 0F F2 17 F4 17 96 0F 00 00 FF FF 00 56 28 }
0x5E3E1: 		End  { 29 02 }
0x5E3E3: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E3EA: 		End  { 29 02 }
0x5E3EC: 		SuppressIf  { 0A 82 }
0x5E3EE: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5E3F4: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5E3FB: 			End  { 29 02 }
0x5E3FD: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF97, VarStoreId: 0xF101, VarOffset: 0x5F5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 A7 17 A8 17 97 0F 01 F1 F5 05 00 11 00 00 FF FF 00 00 }
0x5E411: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5E418: 			End  { 29 02 }
0x5E41A: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF98, VarStoreId: 0xF101, VarOffset: 0x5F7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 AB 17 AC 17 98 0F 01 F1 F7 05 00 11 00 00 FF FF 00 00 }
0x5E42E: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5E435: 			End  { 29 02 }
0x5E437: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF99, VarStoreId: 0xF101, VarOffset: 0x5F9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 A9 17 AA 17 99 0F 01 F1 F9 05 00 11 00 00 FF FF 00 00 }
0x5E44B: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E452: 			End  { 29 02 }
0x5E454: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF9A, VarStoreId: 0xF101, VarOffset: 0x5FB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 AD 17 AE 17 9A 0F 01 F1 FB 05 00 11 00 00 FF FF 00 00 }
0x5E468: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5E46F: 			End  { 29 02 }
0x5E471: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF9B, VarStoreId: 0xF101, VarOffset: 0x5FD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B1 17 B2 17 9B 0F 01 F1 FD 05 00 11 00 00 FF FF 00 00 }
0x5E485: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5E48C: 			End  { 29 02 }
0x5E48E: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF9C, VarStoreId: 0xF101, VarOffset: 0x5FF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 AF 17 B0 17 9C 0F 01 F1 FF 05 00 11 00 00 FF FF 00 00 }
0x5E4A2: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E4A9: 			End  { 29 02 }
0x5E4AB: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF9D, VarStoreId: 0xF101, VarOffset: 0x601, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B3 17 B4 17 9D 0F 01 F1 01 06 00 11 00 00 FF FF 00 00 }
0x5E4BF: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5E4C6: 			End  { 29 02 }
0x5E4C8: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF9E, VarStoreId: 0xF101, VarOffset: 0x603, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B7 17 B8 17 9E 0F 01 F1 03 06 00 11 00 00 FF FF 00 00 }
0x5E4DC: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5E4E3: 			End  { 29 02 }
0x5E4E5: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xF9F, VarStoreId: 0xF101, VarOffset: 0x605, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B5 17 B6 17 9F 0F 01 F1 05 06 00 11 00 00 FF FF 00 00 }
0x5E4F9: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E500: 			End  { 29 02 }
0x5E502: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA0, VarStoreId: 0xF101, VarOffset: 0x607, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 B9 17 BA 17 A0 0F 01 F1 07 06 00 11 00 00 FF FF 00 00 }
0x5E516: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5E51D: 			End  { 29 02 }
0x5E51F: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA1, VarStoreId: 0xF101, VarOffset: 0x609, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 BD 17 BE 17 A1 0F 01 F1 09 06 00 11 00 00 FF FF 00 00 }
0x5E533: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5E53A: 			End  { 29 02 }
0x5E53C: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA2, VarStoreId: 0xF101, VarOffset: 0x60B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 BB 17 BC 17 A2 0F 01 F1 0B 06 00 11 00 00 FF FF 00 00 }
0x5E550: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5E557: 			End  { 29 02 }
0x5E559: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA3, VarStoreId: 0xF101, VarOffset: 0x685, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 BF 17 C0 17 A3 0F 01 F1 85 06 00 11 01 00 10 27 00 00 }
0x5E56D: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5E574: 			End  { 29 02 }
0x5E576: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA4, VarStoreId: 0xF101, VarOffset: 0x687, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 C1 17 C2 17 A4 0F 01 F1 87 06 00 11 01 00 10 27 00 00 }
0x5E58A: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5E591: 			End  { 29 02 }
0x5E593: 		End  { 29 02 }
0x5E595: 		SuppressIf  { 0A 82 }
0x5E597: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5E59D: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5E5A4: 			End  { 29 02 }
0x5E5A6: 		End  { 29 02 }
0x5E5A8: 	End  { 29 02 }
0x5E5AA: 	Form FormId: 0x81, Title: "Serial IO I2C1 Settings" { 01 86 81 00 CD 17 }
0x5E5B0: 		Subtitle Prompt: "Serial IO I2C1 Settings", Help: "", Flags: 0x0 { 02 87 CD 17 00 00 00 }
0x5E5B7: 		End  { 29 02 }
0x5E5B9: 		SuppressIf  { 0A 82 }
0x5E5BB: 			True  { 46 02 }
0x5E5BD: 			Numeric Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFA5, VarStoreId: 0xF101, VarOffset: 0x5D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 96 19 04 18 A5 0F 01 F1 D1 05 00 10 00 FF 00 }
0x5E5CE: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5E5D4: 			End  { 29 02 }
0x5E5D6: 		End  { 29 02 }
0x5E5D8: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E5DF: 		End  { 29 02 }
0x5E5E1: 		SuppressIf  { 0A 82 }
0x5E5E3: 			EqIdValList QuestionId: 0xFA5, Values: [1, 3, 5, 7] { 14 8E A5 0F 04 00 01 00 03 00 05 00 07 00 }
0x5E5F1: 				Not  { 17 02 }
0x5E5F3: 			End  { 29 02 }
0x5E5F5: 			Ref Prompt: "Serial IO Touch Pad Settings", Help: "Indicates what type of I2C Touch Pad is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFA6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2855 { 0F 0F 8A 19 EF 17 A6 0F 00 00 FF FF 00 55 28 }
0x5E604: 		End  { 29 02 }
0x5E606: 		SuppressIf  { 0A 82 }
0x5E608: 			EqIdValList QuestionId: 0xFA5, Values: [2, 3, 6, 7] { 14 8E A5 0F 04 00 02 00 03 00 06 00 07 00 }
0x5E616: 				Not  { 17 02 }
0x5E618: 			End  { 29 02 }
0x5E61A: 			Ref Prompt: "Serial IO Touch Panel Settings", Help: "Indicates what type of I2C Touch Panel is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFA7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2856 { 0F 0F 8D 19 F4 17 A7 0F 00 00 FF FF 00 56 28 }
0x5E629: 		End  { 29 02 }
0x5E62B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E632: 		End  { 29 02 }
0x5E634: 		SuppressIf  { 0A 82 }
0x5E636: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5E63C: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5E643: 			End  { 29 02 }
0x5E645: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA8, VarStoreId: 0xF101, VarOffset: 0x60D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 16 19 A8 17 A8 0F 01 F1 0D 06 00 11 00 00 FF FF 00 00 }
0x5E659: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5E660: 			End  { 29 02 }
0x5E662: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFA9, VarStoreId: 0xF101, VarOffset: 0x60F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 20 19 AC 17 A9 0F 01 F1 0F 06 00 11 00 00 FF FF 00 00 }
0x5E676: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5E67D: 			End  { 29 02 }
0x5E67F: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFAA, VarStoreId: 0xF101, VarOffset: 0x611, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 1B 19 AA 17 AA 0F 01 F1 11 06 00 11 00 00 FF FF 00 00 }
0x5E693: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E69A: 			End  { 29 02 }
0x5E69C: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFAB, VarStoreId: 0xF101, VarOffset: 0x613, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 25 19 AE 17 AB 0F 01 F1 13 06 00 11 00 00 FF FF 00 00 }
0x5E6B0: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5E6B7: 			End  { 29 02 }
0x5E6B9: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFAC, VarStoreId: 0xF101, VarOffset: 0x615, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 2F 19 B2 17 AC 0F 01 F1 15 06 00 11 00 00 FF FF 00 00 }
0x5E6CD: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5E6D4: 			End  { 29 02 }
0x5E6D6: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFAD, VarStoreId: 0xF101, VarOffset: 0x617, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 2A 19 B0 17 AD 0F 01 F1 17 06 00 11 00 00 FF FF 00 00 }
0x5E6EA: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E6F1: 			End  { 29 02 }
0x5E6F3: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFAE, VarStoreId: 0xF101, VarOffset: 0x619, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 34 19 B4 17 AE 0F 01 F1 19 06 00 11 00 00 FF FF 00 00 }
0x5E707: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5E70E: 			End  { 29 02 }
0x5E710: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFAF, VarStoreId: 0xF101, VarOffset: 0x61B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 3E 19 B8 17 AF 0F 01 F1 1B 06 00 11 00 00 FF FF 00 00 }
0x5E724: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5E72B: 			End  { 29 02 }
0x5E72D: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB0, VarStoreId: 0xF101, VarOffset: 0x61D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 39 19 B6 17 B0 0F 01 F1 1D 06 00 11 00 00 FF FF 00 00 }
0x5E741: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E748: 			End  { 29 02 }
0x5E74A: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB1, VarStoreId: 0xF101, VarOffset: 0x61F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 43 19 BA 17 B1 0F 01 F1 1F 06 00 11 00 00 FF FF 00 00 }
0x5E75E: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5E765: 			End  { 29 02 }
0x5E767: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB2, VarStoreId: 0xF101, VarOffset: 0x621, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 4D 19 BE 17 B2 0F 01 F1 21 06 00 11 00 00 FF FF 00 00 }
0x5E77B: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5E782: 			End  { 29 02 }
0x5E784: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB3, VarStoreId: 0xF101, VarOffset: 0x623, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 48 19 BC 17 B3 0F 01 F1 23 06 00 11 00 00 FF FF 00 00 }
0x5E798: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5E79F: 			End  { 29 02 }
0x5E7A1: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB4, VarStoreId: 0xF101, VarOffset: 0x689, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 52 19 C0 17 B4 0F 01 F1 89 06 00 11 01 00 10 27 00 00 }
0x5E7B5: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5E7BC: 			End  { 29 02 }
0x5E7BE: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB5, VarStoreId: 0xF101, VarOffset: 0x68B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 5D 19 C2 17 B5 0F 01 F1 8B 06 00 11 01 00 10 27 00 00 }
0x5E7D2: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5E7D9: 			End  { 29 02 }
0x5E7DB: 		End  { 29 02 }
0x5E7DD: 		SuppressIf  { 0A 82 }
0x5E7DF: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5E7E5: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5E7EC: 			End  { 29 02 }
0x5E7EE: 		End  { 29 02 }
0x5E7F0: 	End  { 29 02 }
0x5E7F2: 	Form FormId: 0x87, Title: "Serial IO I2C2 Settings" { 01 86 87 00 CE 17 }
0x5E7F8: 		Subtitle Prompt: "Serial IO I2C2 Settings", Help: "", Flags: 0x0 { 02 87 CE 17 00 00 00 }
0x5E7FF: 		End  { 29 02 }
0x5E801: 		SuppressIf  { 0A 82 }
0x5E803: 			True  { 46 02 }
0x5E805: 			Numeric Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFB6, VarStoreId: 0xF101, VarOffset: 0x5D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 97 19 04 18 B6 0F 01 F1 D2 05 00 10 00 FF 00 }
0x5E816: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5E81C: 			End  { 29 02 }
0x5E81E: 		End  { 29 02 }
0x5E820: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E827: 		End  { 29 02 }
0x5E829: 		SuppressIf  { 0A 82 }
0x5E82B: 			EqIdValList QuestionId: 0xFB6, Values: [1, 3, 5, 7] { 14 8E B6 0F 04 00 01 00 03 00 05 00 07 00 }
0x5E839: 				Not  { 17 02 }
0x5E83B: 			End  { 29 02 }
0x5E83D: 			Ref Prompt: "Serial IO Touch Pad Settings", Help: "Indicates what type of I2C Touch Pad is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFB7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2855 { 0F 0F 8B 19 EF 17 B7 0F 00 00 FF FF 00 55 28 }
0x5E84C: 		End  { 29 02 }
0x5E84E: 		SuppressIf  { 0A 82 }
0x5E850: 			EqIdValList QuestionId: 0xFB6, Values: [2, 3, 6, 7] { 14 8E B6 0F 04 00 02 00 03 00 06 00 07 00 }
0x5E85E: 				Not  { 17 02 }
0x5E860: 			End  { 29 02 }
0x5E862: 			Ref Prompt: "Serial IO Touch Panel Settings", Help: "Indicates what type of I2C Touch Panel is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFB8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2856 { 0F 0F 8E 19 F4 17 B8 0F 00 00 FF FF 00 56 28 }
0x5E871: 		End  { 29 02 }
0x5E873: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5E87A: 		End  { 29 02 }
0x5E87C: 		SuppressIf  { 0A 82 }
0x5E87E: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5E884: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5E88B: 			End  { 29 02 }
0x5E88D: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFB9, VarStoreId: 0xF101, VarOffset: 0x625, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 17 19 A8 17 B9 0F 01 F1 25 06 00 11 00 00 FF FF 00 00 }
0x5E8A1: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5E8A8: 			End  { 29 02 }
0x5E8AA: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFBA, VarStoreId: 0xF101, VarOffset: 0x627, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 21 19 AC 17 BA 0F 01 F1 27 06 00 11 00 00 FF FF 00 00 }
0x5E8BE: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5E8C5: 			End  { 29 02 }
0x5E8C7: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFBB, VarStoreId: 0xF101, VarOffset: 0x629, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 1C 19 AA 17 BB 0F 01 F1 29 06 00 11 00 00 FF FF 00 00 }
0x5E8DB: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E8E2: 			End  { 29 02 }
0x5E8E4: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFBC, VarStoreId: 0xF101, VarOffset: 0x62B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 26 19 AE 17 BC 0F 01 F1 2B 06 00 11 00 00 FF FF 00 00 }
0x5E8F8: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5E8FF: 			End  { 29 02 }
0x5E901: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFBD, VarStoreId: 0xF101, VarOffset: 0x62D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 30 19 B2 17 BD 0F 01 F1 2D 06 00 11 00 00 FF FF 00 00 }
0x5E915: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5E91C: 			End  { 29 02 }
0x5E91E: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFBE, VarStoreId: 0xF101, VarOffset: 0x62F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 2B 19 B0 17 BE 0F 01 F1 2F 06 00 11 00 00 FF FF 00 00 }
0x5E932: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E939: 			End  { 29 02 }
0x5E93B: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFBF, VarStoreId: 0xF101, VarOffset: 0x631, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 35 19 B4 17 BF 0F 01 F1 31 06 00 11 00 00 FF FF 00 00 }
0x5E94F: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5E956: 			End  { 29 02 }
0x5E958: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC0, VarStoreId: 0xF101, VarOffset: 0x633, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 3F 19 B8 17 C0 0F 01 F1 33 06 00 11 00 00 FF FF 00 00 }
0x5E96C: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5E973: 			End  { 29 02 }
0x5E975: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC1, VarStoreId: 0xF101, VarOffset: 0x635, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 3A 19 B6 17 C1 0F 01 F1 35 06 00 11 00 00 FF FF 00 00 }
0x5E989: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5E990: 			End  { 29 02 }
0x5E992: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC2, VarStoreId: 0xF101, VarOffset: 0x637, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 44 19 BA 17 C2 0F 01 F1 37 06 00 11 00 00 FF FF 00 00 }
0x5E9A6: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5E9AD: 			End  { 29 02 }
0x5E9AF: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC3, VarStoreId: 0xF101, VarOffset: 0x639, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 4E 19 BE 17 C3 0F 01 F1 39 06 00 11 00 00 FF FF 00 00 }
0x5E9C3: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5E9CA: 			End  { 29 02 }
0x5E9CC: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC4, VarStoreId: 0xF101, VarOffset: 0x63B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 49 19 BC 17 C4 0F 01 F1 3B 06 00 11 00 00 FF FF 00 00 }
0x5E9E0: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5E9E7: 			End  { 29 02 }
0x5E9E9: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC5, VarStoreId: 0xF101, VarOffset: 0x68D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 53 19 C0 17 C5 0F 01 F1 8D 06 00 11 01 00 10 27 00 00 }
0x5E9FD: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5EA04: 			End  { 29 02 }
0x5EA06: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFC6, VarStoreId: 0xF101, VarOffset: 0x68F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 5E 19 C2 17 C6 0F 01 F1 8F 06 00 11 01 00 10 27 00 00 }
0x5EA1A: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5EA21: 			End  { 29 02 }
0x5EA23: 		End  { 29 02 }
0x5EA25: 		SuppressIf  { 0A 82 }
0x5EA27: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5EA2D: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5EA34: 			End  { 29 02 }
0x5EA36: 		End  { 29 02 }
0x5EA38: 	End  { 29 02 }
0x5EA3A: 	Form FormId: 0x88, Title: "Serial IO I2C3 Settings" { 01 86 88 00 CF 17 }
0x5EA40: 		Subtitle Prompt: "Serial IO I2C3 Settings", Help: "", Flags: 0x0 { 02 87 CF 17 00 00 00 }
0x5EA47: 		End  { 29 02 }
0x5EA49: 		SuppressIf  { 0A 82 }
0x5EA4B: 			True  { 46 02 }
0x5EA4D: 			Numeric Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFC7, VarStoreId: 0xF101, VarOffset: 0x5D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 98 19 04 18 C7 0F 01 F1 D3 05 00 10 00 FF 00 }
0x5EA5E: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5EA64: 			End  { 29 02 }
0x5EA66: 		End  { 29 02 }
0x5EA68: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5EA6F: 		End  { 29 02 }
0x5EA71: 		SuppressIf  { 0A 82 }
0x5EA73: 			EqIdValList QuestionId: 0xFC7, Values: [1, 3, 5, 7] { 14 8E C7 0F 04 00 01 00 03 00 05 00 07 00 }
0x5EA81: 				Not  { 17 02 }
0x5EA83: 			End  { 29 02 }
0x5EA85: 			Ref Prompt: "Serial IO Touch Pad Settings", Help: "Indicates what type of I2C Touch Pad is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFC8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2855 { 0F 0F 8C 19 EF 17 C8 0F 00 00 FF FF 00 55 28 }
0x5EA94: 		End  { 29 02 }
0x5EA96: 		SuppressIf  { 0A 82 }
0x5EA98: 			EqIdValList QuestionId: 0xFC7, Values: [2, 3, 6, 7] { 14 8E C7 0F 04 00 02 00 03 00 06 00 07 00 }
0x5EAA6: 				Not  { 17 02 }
0x5EAA8: 			End  { 29 02 }
0x5EAAA: 			Ref Prompt: "Serial IO Touch Panel Settings", Help: "Indicates what type of I2C Touch Panel is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0xFC9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2856 { 0F 0F 8F 19 F4 17 C9 0F 00 00 FF FF 00 56 28 }
0x5EAB9: 		End  { 29 02 }
0x5EABB: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5EAC2: 		End  { 29 02 }
0x5EAC4: 		SuppressIf  { 0A 82 }
0x5EAC6: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5EACC: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5EAD3: 			End  { 29 02 }
0x5EAD5: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFCA, VarStoreId: 0xF101, VarOffset: 0x63D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 18 19 A8 17 CA 0F 01 F1 3D 06 00 11 00 00 FF FF 00 00 }
0x5EAE9: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5EAF0: 			End  { 29 02 }
0x5EAF2: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFCB, VarStoreId: 0xF101, VarOffset: 0x63F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 22 19 AC 17 CB 0F 01 F1 3F 06 00 11 00 00 FF FF 00 00 }
0x5EB06: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5EB0D: 			End  { 29 02 }
0x5EB0F: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFCC, VarStoreId: 0xF101, VarOffset: 0x641, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 1D 19 AA 17 CC 0F 01 F1 41 06 00 11 00 00 FF FF 00 00 }
0x5EB23: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EB2A: 			End  { 29 02 }
0x5EB2C: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFCD, VarStoreId: 0xF101, VarOffset: 0x643, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 27 19 AE 17 CD 0F 01 F1 43 06 00 11 00 00 FF FF 00 00 }
0x5EB40: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5EB47: 			End  { 29 02 }
0x5EB49: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFCE, VarStoreId: 0xF101, VarOffset: 0x645, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 31 19 B2 17 CE 0F 01 F1 45 06 00 11 00 00 FF FF 00 00 }
0x5EB5D: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5EB64: 			End  { 29 02 }
0x5EB66: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFCF, VarStoreId: 0xF101, VarOffset: 0x647, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 2C 19 B0 17 CF 0F 01 F1 47 06 00 11 00 00 FF FF 00 00 }
0x5EB7A: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EB81: 			End  { 29 02 }
0x5EB83: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD0, VarStoreId: 0xF101, VarOffset: 0x649, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 36 19 B4 17 D0 0F 01 F1 49 06 00 11 00 00 FF FF 00 00 }
0x5EB97: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5EB9E: 			End  { 29 02 }
0x5EBA0: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD1, VarStoreId: 0xF101, VarOffset: 0x64B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 40 19 B8 17 D1 0F 01 F1 4B 06 00 11 00 00 FF FF 00 00 }
0x5EBB4: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5EBBB: 			End  { 29 02 }
0x5EBBD: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD2, VarStoreId: 0xF101, VarOffset: 0x64D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 3B 19 B6 17 D2 0F 01 F1 4D 06 00 11 00 00 FF FF 00 00 }
0x5EBD1: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EBD8: 			End  { 29 02 }
0x5EBDA: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD3, VarStoreId: 0xF101, VarOffset: 0x64F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 45 19 BA 17 D3 0F 01 F1 4F 06 00 11 00 00 FF FF 00 00 }
0x5EBEE: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5EBF5: 			End  { 29 02 }
0x5EBF7: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD4, VarStoreId: 0xF101, VarOffset: 0x651, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 4F 19 BE 17 D4 0F 01 F1 51 06 00 11 00 00 FF FF 00 00 }
0x5EC0B: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5EC12: 			End  { 29 02 }
0x5EC14: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD5, VarStoreId: 0xF101, VarOffset: 0x653, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 4A 19 BC 17 D5 0F 01 F1 53 06 00 11 00 00 FF FF 00 00 }
0x5EC28: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5EC2F: 			End  { 29 02 }
0x5EC31: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD6, VarStoreId: 0xF101, VarOffset: 0x691, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 54 19 C0 17 D6 0F 01 F1 91 06 00 11 01 00 10 27 00 00 }
0x5EC45: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5EC4C: 			End  { 29 02 }
0x5EC4E: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD7, VarStoreId: 0xF101, VarOffset: 0x693, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 5F 19 C2 17 D7 0F 01 F1 93 06 00 11 01 00 10 27 00 00 }
0x5EC62: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5EC69: 			End  { 29 02 }
0x5EC6B: 		End  { 29 02 }
0x5EC6D: 		SuppressIf  { 0A 82 }
0x5EC6F: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5EC75: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5EC7C: 			End  { 29 02 }
0x5EC7E: 		End  { 29 02 }
0x5EC80: 	End  { 29 02 }
0x5EC82: 	Form FormId: 0x89, Title: "Serial IO I2C4 Settings" { 01 86 89 00 D0 17 }
0x5EC88: 		Subtitle Prompt: "Serial IO I2C4 Settings", Help: "", Flags: 0x0 { 02 87 D0 17 00 00 00 }
0x5EC8F: 		End  { 29 02 }
0x5EC91: 		SuppressIf  { 0A 82 }
0x5EC93: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5EC99: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5ECA0: 			End  { 29 02 }
0x5ECA2: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD8, VarStoreId: 0xF101, VarOffset: 0x655, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 19 19 A8 17 D8 0F 01 F1 55 06 00 11 00 00 FF FF 00 00 }
0x5ECB6: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5ECBD: 			End  { 29 02 }
0x5ECBF: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFD9, VarStoreId: 0xF101, VarOffset: 0x657, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 23 19 AC 17 D9 0F 01 F1 57 06 00 11 00 00 FF FF 00 00 }
0x5ECD3: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5ECDA: 			End  { 29 02 }
0x5ECDC: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFDA, VarStoreId: 0xF101, VarOffset: 0x659, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 1E 19 AA 17 DA 0F 01 F1 59 06 00 11 00 00 FF FF 00 00 }
0x5ECF0: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5ECF7: 			End  { 29 02 }
0x5ECF9: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFDB, VarStoreId: 0xF101, VarOffset: 0x65B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 28 19 AE 17 DB 0F 01 F1 5B 06 00 11 00 00 FF FF 00 00 }
0x5ED0D: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5ED14: 			End  { 29 02 }
0x5ED16: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFDC, VarStoreId: 0xF101, VarOffset: 0x65D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 32 19 B2 17 DC 0F 01 F1 5D 06 00 11 00 00 FF FF 00 00 }
0x5ED2A: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5ED31: 			End  { 29 02 }
0x5ED33: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFDD, VarStoreId: 0xF101, VarOffset: 0x65F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 2D 19 B0 17 DD 0F 01 F1 5F 06 00 11 00 00 FF FF 00 00 }
0x5ED47: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5ED4E: 			End  { 29 02 }
0x5ED50: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFDE, VarStoreId: 0xF101, VarOffset: 0x661, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 37 19 B4 17 DE 0F 01 F1 61 06 00 11 00 00 FF FF 00 00 }
0x5ED64: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5ED6B: 			End  { 29 02 }
0x5ED6D: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFDF, VarStoreId: 0xF101, VarOffset: 0x663, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 41 19 B8 17 DF 0F 01 F1 63 06 00 11 00 00 FF FF 00 00 }
0x5ED81: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5ED88: 			End  { 29 02 }
0x5ED8A: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE0, VarStoreId: 0xF101, VarOffset: 0x665, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 3C 19 B6 17 E0 0F 01 F1 65 06 00 11 00 00 FF FF 00 00 }
0x5ED9E: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EDA5: 			End  { 29 02 }
0x5EDA7: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE1, VarStoreId: 0xF101, VarOffset: 0x667, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 46 19 BA 17 E1 0F 01 F1 67 06 00 11 00 00 FF FF 00 00 }
0x5EDBB: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5EDC2: 			End  { 29 02 }
0x5EDC4: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE2, VarStoreId: 0xF101, VarOffset: 0x669, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 50 19 BE 17 E2 0F 01 F1 69 06 00 11 00 00 FF FF 00 00 }
0x5EDD8: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5EDDF: 			End  { 29 02 }
0x5EDE1: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE3, VarStoreId: 0xF101, VarOffset: 0x66B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 4B 19 BC 17 E3 0F 01 F1 6B 06 00 11 00 00 FF FF 00 00 }
0x5EDF5: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5EDFC: 			End  { 29 02 }
0x5EDFE: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE4, VarStoreId: 0xF101, VarOffset: 0x695, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 55 19 C0 17 E4 0F 01 F1 95 06 00 11 01 00 10 27 00 00 }
0x5EE12: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5EE19: 			End  { 29 02 }
0x5EE1B: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE5, VarStoreId: 0xF101, VarOffset: 0x697, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 60 19 C2 17 E5 0F 01 F1 97 06 00 11 01 00 10 27 00 00 }
0x5EE2F: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5EE36: 			End  { 29 02 }
0x5EE38: 		End  { 29 02 }
0x5EE3A: 		SuppressIf  { 0A 82 }
0x5EE3C: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5EE42: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5EE49: 			End  { 29 02 }
0x5EE4B: 		End  { 29 02 }
0x5EE4D: 	End  { 29 02 }
0x5EE4F: 	Form FormId: 0x8A, Title: "Serial IO I2C5 Settings" { 01 86 8A 00 D1 17 }
0x5EE55: 		Subtitle Prompt: "Serial IO I2C5 Settings", Help: "", Flags: 0x0 { 02 87 D1 17 00 00 00 }
0x5EE5C: 		End  { 29 02 }
0x5EE5E: 		SuppressIf  { 0A 82 }
0x5EE60: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5EE66: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5EE6D: 			End  { 29 02 }
0x5EE6F: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE6, VarStoreId: 0xF101, VarOffset: 0x66D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 1A 19 A8 17 E6 0F 01 F1 6D 06 00 11 00 00 FF FF 00 00 }
0x5EE83: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5EE8A: 			End  { 29 02 }
0x5EE8C: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE7, VarStoreId: 0xF101, VarOffset: 0x66F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 24 19 AC 17 E7 0F 01 F1 6F 06 00 11 00 00 FF FF 00 00 }
0x5EEA0: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5EEA7: 			End  { 29 02 }
0x5EEA9: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE8, VarStoreId: 0xF101, VarOffset: 0x671, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 1F 19 AA 17 E8 0F 01 F1 71 06 00 11 00 00 FF FF 00 00 }
0x5EEBD: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EEC4: 			End  { 29 02 }
0x5EEC6: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFE9, VarStoreId: 0xF101, VarOffset: 0x673, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 29 19 AE 17 E9 0F 01 F1 73 06 00 11 00 00 FF FF 00 00 }
0x5EEDA: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5EEE1: 			End  { 29 02 }
0x5EEE3: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFEA, VarStoreId: 0xF101, VarOffset: 0x675, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 33 19 B2 17 EA 0F 01 F1 75 06 00 11 00 00 FF FF 00 00 }
0x5EEF7: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5EEFE: 			End  { 29 02 }
0x5EF00: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFEB, VarStoreId: 0xF101, VarOffset: 0x677, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 2E 19 B0 17 EB 0F 01 F1 77 06 00 11 00 00 FF FF 00 00 }
0x5EF14: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EF1B: 			End  { 29 02 }
0x5EF1D: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFEC, VarStoreId: 0xF101, VarOffset: 0x679, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 38 19 B4 17 EC 0F 01 F1 79 06 00 11 00 00 FF FF 00 00 }
0x5EF31: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5EF38: 			End  { 29 02 }
0x5EF3A: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFED, VarStoreId: 0xF101, VarOffset: 0x67B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 42 19 B8 17 ED 0F 01 F1 7B 06 00 11 00 00 FF FF 00 00 }
0x5EF4E: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5EF55: 			End  { 29 02 }
0x5EF57: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFEE, VarStoreId: 0xF101, VarOffset: 0x67D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 3D 19 B6 17 EE 0F 01 F1 7D 06 00 11 00 00 FF FF 00 00 }
0x5EF6B: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5EF72: 			End  { 29 02 }
0x5EF74: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFEF, VarStoreId: 0xF101, VarOffset: 0x67F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 47 19 BA 17 EF 0F 01 F1 7F 06 00 11 00 00 FF FF 00 00 }
0x5EF88: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5EF8F: 			End  { 29 02 }
0x5EF91: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF0, VarStoreId: 0xF101, VarOffset: 0x681, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 51 19 BE 17 F0 0F 01 F1 81 06 00 11 00 00 FF FF 00 00 }
0x5EFA5: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5EFAC: 			End  { 29 02 }
0x5EFAE: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF1, VarStoreId: 0xF101, VarOffset: 0x683, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 4C 19 BC 17 F1 0F 01 F1 83 06 00 11 00 00 FF FF 00 00 }
0x5EFC2: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5EFC9: 			End  { 29 02 }
0x5EFCB: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF2, VarStoreId: 0xF101, VarOffset: 0x699, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 56 19 C0 17 F2 0F 01 F1 99 06 00 11 01 00 10 27 00 00 }
0x5EFDF: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5EFE6: 			End  { 29 02 }
0x5EFE8: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF3, VarStoreId: 0xF101, VarOffset: 0x69B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 61 19 C2 17 F3 0F 01 F1 9B 06 00 11 01 00 10 27 00 00 }
0x5EFFC: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5F003: 			End  { 29 02 }
0x5F005: 		End  { 29 02 }
0x5F007: 		SuppressIf  { 0A 82 }
0x5F009: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F00F: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F016: 			End  { 29 02 }
0x5F018: 		End  { 29 02 }
0x5F01A: 	End  { 29 02 }
0x5F01C: 	Form FormId: 0x99, Title: "Serial IO I2C6 Settings" { 01 86 99 00 D2 17 }
0x5F022: 		Subtitle Prompt: "Serial IO I2C6 Settings", Help: "", Flags: 0x0 { 02 87 D2 17 00 00 00 }
0x5F029: 		End  { 29 02 }
0x5F02B: 		SuppressIf  { 0A 82 }
0x5F02D: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5F033: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5F03A: 			End  { 29 02 }
0x5F03C: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF4, VarStoreId: 0xF101, VarOffset: 0xAFC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 62 19 A8 17 F4 0F 01 F1 FC 0A 00 11 00 00 FF FF 00 00 }
0x5F050: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5F057: 			End  { 29 02 }
0x5F059: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF5, VarStoreId: 0xF101, VarOffset: 0xAFE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 63 19 AC 17 F5 0F 01 F1 FE 0A 00 11 00 00 FF FF 00 00 }
0x5F06D: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5F074: 			End  { 29 02 }
0x5F076: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF6, VarStoreId: 0xF101, VarOffset: 0xB00, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 64 19 AA 17 F6 0F 01 F1 00 0B 00 11 00 00 FF FF 00 00 }
0x5F08A: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5F091: 			End  { 29 02 }
0x5F093: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF7, VarStoreId: 0xF101, VarOffset: 0xB02, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 65 19 AE 17 F7 0F 01 F1 02 0B 00 11 00 00 FF FF 00 00 }
0x5F0A7: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5F0AE: 			End  { 29 02 }
0x5F0B0: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF8, VarStoreId: 0xF101, VarOffset: 0xB04, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 66 19 B2 17 F8 0F 01 F1 04 0B 00 11 00 00 FF FF 00 00 }
0x5F0C4: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5F0CB: 			End  { 29 02 }
0x5F0CD: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFF9, VarStoreId: 0xF101, VarOffset: 0xB06, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 67 19 B0 17 F9 0F 01 F1 06 0B 00 11 00 00 FF FF 00 00 }
0x5F0E1: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5F0E8: 			End  { 29 02 }
0x5F0EA: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFFA, VarStoreId: 0xF101, VarOffset: 0xB08, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 68 19 B4 17 FA 0F 01 F1 08 0B 00 11 00 00 FF FF 00 00 }
0x5F0FE: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5F105: 			End  { 29 02 }
0x5F107: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFFB, VarStoreId: 0xF101, VarOffset: 0xB0A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 69 19 B8 17 FB 0F 01 F1 0A 0B 00 11 00 00 FF FF 00 00 }
0x5F11B: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5F122: 			End  { 29 02 }
0x5F124: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFFC, VarStoreId: 0xF101, VarOffset: 0xB0C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 6A 19 B6 17 FC 0F 01 F1 0C 0B 00 11 00 00 FF FF 00 00 }
0x5F138: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5F13F: 			End  { 29 02 }
0x5F141: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFFD, VarStoreId: 0xF101, VarOffset: 0xB0E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 6B 19 BA 17 FD 0F 01 F1 0E 0B 00 11 00 00 FF FF 00 00 }
0x5F155: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5F15C: 			End  { 29 02 }
0x5F15E: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFFE, VarStoreId: 0xF101, VarOffset: 0xB10, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 6C 19 BE 17 FE 0F 01 F1 10 0B 00 11 00 00 FF FF 00 00 }
0x5F172: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5F179: 			End  { 29 02 }
0x5F17B: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0xFFF, VarStoreId: 0xF101, VarOffset: 0xB12, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 6D 19 BC 17 FF 0F 01 F1 12 0B 00 11 00 00 FF FF 00 00 }
0x5F18F: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5F196: 			End  { 29 02 }
0x5F198: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1000, VarStoreId: 0xF101, VarOffset: 0xB14, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 57 19 C0 17 00 10 01 F1 14 0B 00 11 01 00 10 27 00 00 }
0x5F1AC: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F1B3: 			End  { 29 02 }
0x5F1B5: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1001, VarStoreId: 0xF101, VarOffset: 0xB16, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 6E 19 C2 17 01 10 01 F1 16 0B 00 11 01 00 10 27 00 00 }
0x5F1C9: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5F1D0: 			End  { 29 02 }
0x5F1D2: 		End  { 29 02 }
0x5F1D4: 		SuppressIf  { 0A 82 }
0x5F1D6: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F1DC: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F1E3: 			End  { 29 02 }
0x5F1E5: 		End  { 29 02 }
0x5F1E7: 	End  { 29 02 }
0x5F1E9: 	Form FormId: 0x9A, Title: "Serial IO I2C7 Settings" { 01 86 9A 00 D3 17 }
0x5F1EF: 		Subtitle Prompt: "Serial IO I2C7 Settings", Help: "", Flags: 0x0 { 02 87 D3 17 00 00 00 }
0x5F1F6: 		End  { 29 02 }
0x5F1F8: 		SuppressIf  { 0A 82 }
0x5F1FA: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5F200: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5F207: 			End  { 29 02 }
0x5F209: 			Numeric Prompt: "StandardSpeed SCL High", Help: "Default:
612 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1002, VarStoreId: 0xF101, VarOffset: 0xB19, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 6F 19 A8 17 02 10 01 F1 19 0B 00 11 00 00 FF FF 00 00 }
0x5F21D: 				Default DefaultId: 0x0 Value: 706 { 5B 07 00 00 01 C2 02 }
0x5F224: 			End  { 29 02 }
0x5F226: 			Numeric Prompt: "StandardSpeed SCL Low", Help: "Default:
706 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1003, VarStoreId: 0xF101, VarOffset: 0xB1B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 70 19 AC 17 03 10 01 F1 1B 0B 00 11 00 00 FF FF 00 00 }
0x5F23A: 				Default DefaultId: 0x0 Value: 612 { 5B 07 00 00 01 64 02 }
0x5F241: 			End  { 29 02 }
0x5F243: 			Numeric Prompt: "StandardSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1004, VarStoreId: 0xF101, VarOffset: 0xB1D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 71 19 AA 17 04 10 01 F1 1D 0B 00 11 00 00 FF FF 00 00 }
0x5F257: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5F25E: 			End  { 29 02 }
0x5F260: 			Numeric Prompt: "FastSpeed SCL High", Help: "Default:
110 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1005, VarStoreId: 0xF101, VarOffset: 0xB1F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 72 19 AE 17 05 10 01 F1 1F 0B 00 11 00 00 FF FF 00 00 }
0x5F274: 				Default DefaultId: 0x0 Value: 110 { 5B 07 00 00 01 6E 00 }
0x5F27B: 			End  { 29 02 }
0x5F27D: 			Numeric Prompt: "FastSpeed SCL Low", Help: "Default:
207 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1006, VarStoreId: 0xF101, VarOffset: 0xB21, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 73 19 B2 17 06 10 01 F1 21 0B 00 11 00 00 FF FF 00 00 }
0x5F291: 				Default DefaultId: 0x0 Value: 207 { 5B 07 00 00 01 CF 00 }
0x5F298: 			End  { 29 02 }
0x5F29A: 			Numeric Prompt: "FastSpeed SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1007, VarStoreId: 0xF101, VarOffset: 0xB23, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 74 19 B0 17 07 10 01 F1 23 0B 00 11 00 00 FF FF 00 00 }
0x5F2AE: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5F2B5: 			End  { 29 02 }
0x5F2B7: 			Numeric Prompt: "FastSpeedPlus SCL High", Help: "Default:
43 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1008, VarStoreId: 0xF101, VarOffset: 0xB25, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 75 19 B4 17 08 10 01 F1 25 0B 00 11 00 00 FF FF 00 00 }
0x5F2CB: 				Default DefaultId: 0x0 Value: 43 { 5B 07 00 00 01 2B 00 }
0x5F2D2: 			End  { 29 02 }
0x5F2D4: 			Numeric Prompt: "FastSpeedPlus SCL Low", Help: "Default:
76 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1009, VarStoreId: 0xF101, VarOffset: 0xB27, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 76 19 B8 17 09 10 01 F1 27 0B 00 11 00 00 FF FF 00 00 }
0x5F2E8: 				Default DefaultId: 0x0 Value: 76 { 5B 07 00 00 01 4C 00 }
0x5F2EF: 			End  { 29 02 }
0x5F2F1: 			Numeric Prompt: "FastSpeedPlus SDA Hold", Help: "Default:
30 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x100A, VarStoreId: 0xF101, VarOffset: 0xB29, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 77 19 B6 17 0A 10 01 F1 29 0B 00 11 00 00 FF FF 00 00 }
0x5F305: 				Default DefaultId: 0x0 Value: 30 { 5B 07 00 00 01 1E 00 }
0x5F30C: 			End  { 29 02 }
0x5F30E: 			Numeric Prompt: "HighSpeed SCL High", Help: "Default:
11 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x100B, VarStoreId: 0xF101, VarOffset: 0xB2B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 78 19 BA 17 0B 10 01 F1 2B 0B 00 11 00 00 FF FF 00 00 }
0x5F322: 				Default DefaultId: 0x0 Value: 11 { 5B 07 00 00 01 0B 00 }
0x5F329: 			End  { 29 02 }
0x5F32B: 			Numeric Prompt: "HighSpeed SCL Low", Help: "Default:
22 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x100C, VarStoreId: 0xF101, VarOffset: 0xB2D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 79 19 BE 17 0C 10 01 F1 2D 0B 00 11 00 00 FF FF 00 00 }
0x5F33F: 				Default DefaultId: 0x0 Value: 22 { 5B 07 00 00 01 16 00 }
0x5F346: 			End  { 29 02 }
0x5F348: 			Numeric Prompt: "HighSpeed SDA Hold", Help: "Default:
8 [DEC]

Minimum:
1 [DEC]

Maximum:
65535 [DEC]", QuestionFlags: 0x0, QuestionId: 0x100D, VarStoreId: 0xF101, VarOffset: 0xB2F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 7A 19 BC 17 0D 10 01 F1 2F 0B 00 11 00 00 FF FF 00 00 }
0x5F35C: 				Default DefaultId: 0x0 Value: 5 { 5B 07 00 00 01 05 00 }
0x5F363: 			End  { 29 02 }
0x5F365: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x100E, VarStoreId: 0xF101, VarOffset: 0xB31, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 58 19 C0 17 0E 10 01 F1 31 0B 00 11 01 00 10 27 00 00 }
0x5F379: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F380: 			End  { 29 02 }
0x5F382: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x100F, VarStoreId: 0xF101, VarOffset: 0xB33, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 7B 19 C2 17 0F 10 01 F1 33 0B 00 11 01 00 10 27 00 00 }
0x5F396: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5F39D: 			End  { 29 02 }
0x5F39F: 		End  { 29 02 }
0x5F3A1: 		SuppressIf  { 0A 82 }
0x5F3A3: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F3A9: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F3B0: 			End  { 29 02 }
0x5F3B2: 		End  { 29 02 }
0x5F3B4: 	End  { 29 02 }
0x5F3B6: 	Form FormId: 0x82, Title: "Serial IO SPI0 Settings" { 01 86 82 00 D4 17 }
0x5F3BC: 		Subtitle Prompt: "Serial IO SPI0 Settings", Help: "", Flags: 0x0 { 02 87 D4 17 00 00 00 }
0x5F3C3: 		End  { 29 02 }
0x5F3C5: 		OneOf Prompt: "ChipSelect 0 polarity", Help: "Sets initial polarity for ChipSelect signal. Active low is with initial idle polarity of low and vice versa", QuestionFlags: 0x10, QuestionId: 0x1010, VarStoreId: 0x6, VarOffset: 0x6D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E8 17 EA 17 10 10 06 00 D2 06 10 10 00 01 00 }
0x5F3D6: 			OneOfOption Option: "Active Low" Value: 0 { 09 07 EB 17 00 00 00 }
0x5F3DD: 			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault { 09 07 EC 17 30 00 01 }
0x5F3E4: 		End  { 29 02 }
0x5F3E6: 		OneOf Prompt: "ChipSelect 1 polarity", Help: "Sets initial polarity for ChipSelect signal. Active low is with initial idle polarity of low and vice versa", QuestionFlags: 0x10, QuestionId: 0x1011, VarStoreId: 0x6, VarOffset: 0x6D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 E9 17 EA 17 11 10 06 00 D3 06 10 10 00 01 00 }
0x5F3F7: 			OneOfOption Option: "Active Low" Value: 0 { 09 07 EB 17 00 00 00 }
0x5F3FE: 			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault { 09 07 EC 17 30 00 01 }
0x5F405: 		End  { 29 02 }
0x5F407: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F40E: 		End  { 29 02 }
0x5F410: 		SuppressIf  { 0A 82 }
0x5F412: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5F418: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5F41F: 			End  { 29 02 }
0x5F421: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1012, VarStoreId: 0xF101, VarOffset: 0x69D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 59 19 C0 17 12 10 01 F1 9D 06 00 11 01 00 10 27 00 00 }
0x5F435: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F43C: 			End  { 29 02 }
0x5F43E: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1013, VarStoreId: 0xF101, VarOffset: 0x69F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 7C 19 C2 17 13 10 01 F1 9F 06 00 11 01 00 10 27 00 00 }
0x5F452: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x5F459: 			End  { 29 02 }
0x5F45B: 		End  { 29 02 }
0x5F45D: 		SuppressIf  { 0A 82 }
0x5F45F: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F465: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F46C: 			End  { 29 02 }
0x5F46E: 		End  { 29 02 }
0x5F470: 	End  { 29 02 }
0x5F472: 	Form FormId: 0x83, Title: "Serial IO SPI1 Settings" { 01 86 83 00 D5 17 }
0x5F478: 		Subtitle Prompt: "Serial IO SPI1 Settings", Help: "", Flags: 0x0 { 02 87 D5 17 00 00 00 }
0x5F47F: 		End  { 29 02 }
0x5F481: 		OneOf Prompt: "ChipSelect 0 polarity", Help: "Sets initial polarity for ChipSelect signal. Active low is with initial idle polarity of low and vice versa", QuestionFlags: 0x10, QuestionId: 0x1014, VarStoreId: 0x6, VarOffset: 0x6D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 86 19 EA 17 14 10 06 00 D4 06 10 10 00 01 00 }
0x5F492: 			OneOfOption Option: "Active Low" Value: 0 { 09 07 EB 17 00 00 00 }
0x5F499: 			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault { 09 07 EC 17 30 00 01 }
0x5F4A0: 		End  { 29 02 }
0x5F4A2: 		OneOf Prompt: "ChipSelect 1 polarity", Help: "Sets initial polarity for ChipSelect signal. Active low is with initial idle polarity of low and vice versa", QuestionFlags: 0x10, QuestionId: 0x1015, VarStoreId: 0x6, VarOffset: 0x6D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 88 19 EA 17 15 10 06 00 D5 06 10 10 00 01 00 }
0x5F4B3: 			OneOfOption Option: "Active Low" Value: 0 { 09 07 EB 17 00 00 00 }
0x5F4BA: 			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault { 09 07 EC 17 30 00 01 }
0x5F4C1: 		End  { 29 02 }
0x5F4C3: 		SuppressIf  { 0A 82 }
0x5F4C5: 			True  { 46 02 }
0x5F4C7: 			Numeric Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0x1016, VarStoreId: 0xF101, VarOffset: 0x5E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 02 18 04 18 16 10 01 F1 E5 05 00 10 00 FF 00 }
0x5F4D8: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5F4DE: 			End  { 29 02 }
0x5F4E0: 		End  { 29 02 }
0x5F4E2: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F4E9: 		End  { 29 02 }
0x5F4EB: 		SuppressIf  { 0A 82 }
0x5F4ED: 			EqIdValList QuestionId: 0x1016, Values: [1] { 14 88 16 10 01 00 01 00 }
0x5F4F5: 				Not  { 17 02 }
0x5F4F7: 			End  { 29 02 }
0x5F4F9: 			Ref Prompt: "Serial IO Finger Print Settings", Help: "Select the HID to enable Finger Print Sensor", QuestionFlags: 0x0, QuestionId: 0x1017, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2857 { 0F 0F F7 17 F9 17 17 10 00 00 FF FF 00 57 28 }
0x5F508: 		End  { 29 02 }
0x5F50A: 	End  { 29 02 }
0x5F50C: 	Form FormId: 0x8C, Title: "Serial IO SPI2 Settings" { 01 86 8C 00 D6 17 }
0x5F512: 		Subtitle Prompt: "Serial IO SPI2 Settings", Help: "", Flags: 0x0 { 02 87 D6 17 00 00 00 }
0x5F519: 		End  { 29 02 }
0x5F51B: 		OneOf Prompt: "ChipSelect 0 polarity", Help: "Sets initial polarity for ChipSelect signal. Active low is with initial idle polarity of low and vice versa", QuestionFlags: 0x10, QuestionId: 0x1018, VarStoreId: 0x6, VarOffset: 0x6D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 87 19 EA 17 18 10 06 00 D6 06 10 10 00 01 00 }
0x5F52C: 			OneOfOption Option: "Active Low" Value: 0 { 09 07 EB 17 00 00 00 }
0x5F533: 			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault { 09 07 EC 17 30 00 01 }
0x5F53A: 		End  { 29 02 }
0x5F53C: 		OneOf Prompt: "ChipSelect 1 polarity", Help: "Sets initial polarity for ChipSelect signal. Active low is with initial idle polarity of low and vice versa", QuestionFlags: 0x10, QuestionId: 0x1019, VarStoreId: 0x6, VarOffset: 0x6D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 19 EA 17 19 10 06 00 D7 06 10 10 00 01 00 }
0x5F54D: 			OneOfOption Option: "Active Low" Value: 0 { 09 07 EB 17 00 00 00 }
0x5F554: 			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault { 09 07 EC 17 30 00 01 }
0x5F55B: 		End  { 29 02 }
0x5F55D: 		SuppressIf  { 0A 82 }
0x5F55F: 			True  { 46 02 }
0x5F561: 			Numeric Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x0, QuestionId: 0x101A, VarStoreId: 0xF101, VarOffset: 0x5E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 95 19 04 18 1A 10 01 F1 E6 05 00 10 00 FF 00 }
0x5F572: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x5F578: 			End  { 29 02 }
0x5F57A: 		End  { 29 02 }
0x5F57C: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F583: 		End  { 29 02 }
0x5F585: 		SuppressIf  { 0A 82 }
0x5F587: 			EqIdValList QuestionId: 0x101A, Values: [1] { 14 88 1A 10 01 00 01 00 }
0x5F58F: 				Not  { 17 02 }
0x5F591: 			End  { 29 02 }
0x5F593: 			Ref Prompt: "Serial IO Finger Print Settings", Help: "Select the HID to enable Finger Print Sensor", QuestionFlags: 0x0, QuestionId: 0x101B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2857 { 0F 0F 90 19 F9 17 1B 10 00 00 FF FF 00 57 28 }
0x5F5A2: 		End  { 29 02 }
0x5F5A4: 	End  { 29 02 }
0x5F5A6: 	Form FormId: 0x84, Title: "Serial IO UART0 Settings" { 01 86 84 00 D9 17 }
0x5F5AC: 		Subtitle Prompt: "Serial IO UART0 Settings", Help: "", Flags: 0x0 { 02 87 D9 17 00 00 00 }
0x5F5B3: 		End  { 29 02 }
0x5F5B5: 		OneOf Prompt: "Hardware Flow Control", Help: "When enabled configures additional 2 GPIO pads for use as RTS/CTS signals for UART", QuestionFlags: 0x10, QuestionId: 0x101C, VarStoreId: 0x6, VarOffset: 0x6F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 53 18 54 18 1C 10 06 00 F7 06 10 10 00 01 00 }
0x5F5C6: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F5CD: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5F5D4: 		End  { 29 02 }
0x5F5D6: 		OneOf Prompt: "DMA Enable", Help: "Enabled: UART OS driver will use DMA when possible. Disabled: OS driver will enforce PIO mode", QuestionFlags: 0x10, QuestionId: 0x101D, VarStoreId: 0x6, VarOffset: 0x6F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 57 18 58 18 1D 10 06 00 F0 06 10 10 00 01 00 }
0x5F5E7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F5EE: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5F5F5: 		End  { 29 02 }
0x5F5F7: 		SuppressIf  { 0A 82 }
0x5F5F9: 			EqIdVal QuestionId: 0xF79, Value: 0x3 { 12 86 79 0F 03 00 }
0x5F5FF: 				Not  { 17 02 }
0x5F601: 			End  { 29 02 }
0x5F603: 			OneOf Prompt: "Power Gating", Help: "Disabled:
 No _PS0 _PS3 support, device is left in D0, after initialization
Enabled:
 _PS0 _PS3 that supports getting device out of reset
Auto:
 _PS0 and _PS3 detection through ACPI if device was initialized prior to first PG. If it was used (DBG2) PG is disabled", QuestionFlags: 0x10, QuestionId: 0x101E, VarStoreId: 0x6, VarOffset: 0x6FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 55 18 56 18 1E 10 06 00 FE 06 10 10 00 02 00 }
0x5F614: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F61B: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5F622: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 06 00 30 00 02 }
0x5F629: 			End  { 29 02 }
0x5F62B: 		End  { 29 02 }
0x5F62D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F634: 		End  { 29 02 }
0x5F636: 		SuppressIf  { 0A 82 }
0x5F638: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5F63E: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5F645: 			End  { 29 02 }
0x5F647: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x101F, VarStoreId: 0xF101, VarOffset: 0x6A9, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 5A 19 C0 17 1F 10 01 F1 A9 06 00 11 01 00 10 27 00 00 }
0x5F65B: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F662: 			End  { 29 02 }
0x5F664: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1020, VarStoreId: 0xF101, VarOffset: 0x6AB, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 7D 19 C3 17 20 10 01 F1 AB 06 00 11 01 00 10 27 00 00 }
0x5F678: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F67F: 			End  { 29 02 }
0x5F681: 		End  { 29 02 }
0x5F683: 		SuppressIf  { 0A 82 }
0x5F685: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F68B: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F692: 			End  { 29 02 }
0x5F694: 		End  { 29 02 }
0x5F696: 	End  { 29 02 }
0x5F698: 	Form FormId: 0x85, Title: "Serial IO UART1 Settings" { 01 86 85 00 DA 17 }
0x5F69E: 		Subtitle Prompt: "Serial IO UART1 Settings", Help: "", Flags: 0x0 { 02 87 DA 17 00 00 00 }
0x5F6A5: 		End  { 29 02 }
0x5F6A7: 		OneOf Prompt: "Hardware Flow Control", Help: "When enabled configures additional 2 GPIO pads for use as RTS/CTS signals for UART", QuestionFlags: 0x10, QuestionId: 0x1021, VarStoreId: 0x6, VarOffset: 0x6F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9C 19 54 18 21 10 06 00 F8 06 10 10 00 01 00 }
0x5F6B8: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F6BF: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5F6C6: 		End  { 29 02 }
0x5F6C8: 		OneOf Prompt: "DMA Enable", Help: "Enabled: UART OS driver will use DMA when possible. Disabled: OS driver will enforce PIO mode", QuestionFlags: 0x10, QuestionId: 0x1022, VarStoreId: 0x6, VarOffset: 0x6F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A0 19 58 18 22 10 06 00 F1 06 10 10 00 01 00 }
0x5F6D9: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F6E0: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5F6E7: 		End  { 29 02 }
0x5F6E9: 		SuppressIf  { 0A 82 }
0x5F6EB: 			EqIdVal QuestionId: 0x1110, Value: 0x3 { 12 86 10 11 03 00 }
0x5F6F1: 				Not  { 17 02 }
0x5F6F3: 			End  { 29 02 }
0x5F6F5: 			OneOf Prompt: "Power Gating", Help: "Disabled:
 No _PS0 _PS3 support, device is left in D0, after initialization
Enabled:
 _PS0 _PS3 that supports getting device out of reset
Auto:
 _PS0 and _PS3 detection through ACPI if device was initialized prior to first PG. If it was used (DBG2) PG is disabled", QuestionFlags: 0x10, QuestionId: 0x1023, VarStoreId: 0x6, VarOffset: 0x6FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9E 19 56 18 23 10 06 00 FF 06 10 10 00 02 00 }
0x5F706: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F70D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5F714: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 06 00 30 00 02 }
0x5F71B: 			End  { 29 02 }
0x5F71D: 		End  { 29 02 }
0x5F71F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F726: 		End  { 29 02 }
0x5F728: 		SuppressIf  { 0A 82 }
0x5F72A: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5F730: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5F737: 			End  { 29 02 }
0x5F739: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1024, VarStoreId: 0xF101, VarOffset: 0x6AD, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 5B 19 C0 17 24 10 01 F1 AD 06 00 11 01 00 10 27 00 00 }
0x5F74D: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F754: 			End  { 29 02 }
0x5F756: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1025, VarStoreId: 0xF101, VarOffset: 0x6AF, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 7E 19 C3 17 25 10 01 F1 AF 06 00 11 01 00 10 27 00 00 }
0x5F76A: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F771: 			End  { 29 02 }
0x5F773: 		End  { 29 02 }
0x5F775: 		SuppressIf  { 0A 82 }
0x5F777: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F77D: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F784: 			End  { 29 02 }
0x5F786: 		End  { 29 02 }
0x5F788: 	End  { 29 02 }
0x5F78A: 	Form FormId: 0x8B, Title: "Serial IO UART2 Settings" { 01 86 8B 00 DB 17 }
0x5F790: 		Subtitle Prompt: "Serial IO UART2 Settings", Help: "", Flags: 0x0 { 02 87 DB 17 00 00 00 }
0x5F797: 		End  { 29 02 }
0x5F799: 		OneOf Prompt: "Hardware Flow Control", Help: "When enabled configures additional 2 GPIO pads for use as RTS/CTS signals for UART", QuestionFlags: 0x10, QuestionId: 0x1026, VarStoreId: 0x6, VarOffset: 0x6F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 9D 19 54 18 26 10 06 00 F9 06 10 10 00 01 00 }
0x5F7AA: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F7B1: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5F7B8: 		End  { 29 02 }
0x5F7BA: 		OneOf Prompt: "DMA Enable", Help: "Enabled: UART OS driver will use DMA when possible. Disabled: OS driver will enforce PIO mode", QuestionFlags: 0x10, QuestionId: 0x1027, VarStoreId: 0x6, VarOffset: 0x6F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 A1 19 58 18 27 10 06 00 F2 06 10 10 00 01 00 }
0x5F7CB: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F7D2: 			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x5F7D9: 		End  { 29 02 }
0x5F7DB: 		SuppressIf  { 0A 82 }
0x5F7DD: 			EqIdVal QuestionId: 0x110F, Value: 0x3 { 12 86 0F 11 03 00 }
0x5F7E3: 				Not  { 17 02 }
0x5F7E5: 			End  { 29 02 }
0x5F7E7: 			OneOf Prompt: "Power Gating", Help: "Disabled:
 No _PS0 _PS3 support, device is left in D0, after initialization
Enabled:
 _PS0 _PS3 that supports getting device out of reset
Auto:
 _PS0 and _PS3 detection through ACPI if device was initialized prior to first PG. If it was used (DBG2) PG is disabled", QuestionFlags: 0x10, QuestionId: 0x1028, VarStoreId: 0x6, VarOffset: 0x700, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9F 19 56 18 28 10 06 00 00 07 10 10 00 02 00 }
0x5F7F8: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5F7FF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5F806: 				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault { 09 07 06 00 30 00 02 }
0x5F80D: 			End  { 29 02 }
0x5F80F: 		End  { 29 02 }
0x5F811: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F818: 		End  { 29 02 }
0x5F81A: 		SuppressIf  { 0A 82 }
0x5F81C: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x5F822: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x5F829: 			End  { 29 02 }
0x5F82B: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1029, VarStoreId: 0xF101, VarOffset: 0x6B1, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 5C 19 C0 17 29 10 01 F1 B1 06 00 11 01 00 10 27 00 00 }
0x5F83F: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F846: 			End  { 29 02 }
0x5F848: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x102A, VarStoreId: 0xF101, VarOffset: 0x6B3, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 7F 19 C3 17 2A 10 01 F1 B3 06 00 11 01 00 10 27 00 00 }
0x5F85C: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x5F863: 			End  { 29 02 }
0x5F865: 		End  { 29 02 }
0x5F867: 		SuppressIf  { 0A 82 }
0x5F869: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x5F86F: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x5F876: 			End  { 29 02 }
0x5F878: 		End  { 29 02 }
0x5F87A: 	End  { 29 02 }
0x5F87C: 	Form FormId: 0x2853, Title: "ISH Configuration" { 01 86 53 28 65 17 }
0x5F882: 		SuppressIf  { 0A 82 }
0x5F884: 			EqIdVal QuestionId: 0x110E, Value: 0x0 { 12 06 0E 11 00 00 }
0x5F88A: 			OneOf Prompt: "ISH Controller", Help: "Enables/Disables Integrated Sensor Hub (ISH) Device", QuestionFlags: 0x10, QuestionId: 0x102B, VarStoreId: 0x6, VarOffset: 0x6C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 68 17 69 17 2B 10 06 00 C1 06 10 10 00 01 00 }
0x5F89B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5F8A2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x5F8A9: 			End  { 29 02 }
0x5F8AB: 			SuppressIf  { 0A 82 }
0x5F8AD: 				EqIdVal QuestionId: 0x102B, Value: 0x0 { 12 06 2B 10 00 00 }
0x5F8B3: 				CheckBox Prompt: "PDT Unlock Message", Help: "Checked = Sends PDT Unlock Message to ISH.
After the message is sent the field is set back to unchecked automatically.", QuestionFlags: 0x10, QuestionId: 0x102C, VarStoreId: 0x6, VarOffset: 0x6D1, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 6A 17 6B 17 2C 10 06 00 D1 06 10 00 }
0x5F8C1: 				End  { 29 02 }
0x5F8C3: 				Text Prompt: "ISH GPIO Assignment Configuration", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", Text: "" { 03 08 6C 17 6D 17 00 00 }
0x5F8CB: 				CheckBox Prompt: " SPI_0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x102D, VarStoreId: 0x6, VarOffset: 0x6C2, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 6E 17 6D 17 2D 10 06 00 C2 06 10 00 }
0x5F8D9: 				End  { 29 02 }
0x5F8DB: 				SuppressIf  { 0A 82 }
0x5F8DD: 					EqIdVal QuestionId: 0x102D, Value: 0x0 { 12 06 2D 10 00 00 }
0x5F8E3: 					CheckBox Prompt: " SPI_0 CS_0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x102E, VarStoreId: 0x6, VarOffset: 0x6C3, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 6F 17 6D 17 2E 10 06 00 C3 06 10 00 }
0x5F8F1: 					End  { 29 02 }
0x5F8F3: 				End  { 29 02 }
0x5F8F5: 				CheckBox Prompt: " UART0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x102F, VarStoreId: 0x6, VarOffset: 0x6C4, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 70 17 6D 17 2F 10 06 00 C4 06 10 00 }
0x5F903: 				End  { 29 02 }
0x5F905: 				CheckBox Prompt: " UART1", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1030, VarStoreId: 0x6, VarOffset: 0x6C5, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 71 17 6D 17 30 10 06 00 C5 06 10 00 }
0x5F913: 				End  { 29 02 }
0x5F915: 				CheckBox Prompt: " I2C0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1031, VarStoreId: 0x6, VarOffset: 0x6C6, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 72 17 6D 17 31 10 06 00 C6 06 10 01 }
0x5F923: 				End  { 29 02 }
0x5F925: 				CheckBox Prompt: " I2C1", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1032, VarStoreId: 0x6, VarOffset: 0x6C7, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 73 17 6D 17 32 10 06 00 C7 06 10 01 }
0x5F933: 				End  { 29 02 }
0x5F935: 				CheckBox Prompt: " I2C2", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1033, VarStoreId: 0x6, VarOffset: 0x6C8, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 74 17 6D 17 33 10 06 00 C8 06 10 01 }
0x5F943: 				End  { 29 02 }
0x5F945: 				CheckBox Prompt: " GP_0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1034, VarStoreId: 0x6, VarOffset: 0x6C9, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 75 17 6D 17 34 10 06 00 C9 06 10 01 }
0x5F953: 				End  { 29 02 }
0x5F955: 				CheckBox Prompt: " GP_1", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1035, VarStoreId: 0x6, VarOffset: 0x6CA, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 76 17 6D 17 35 10 06 00 CA 06 10 01 }
0x5F963: 				End  { 29 02 }
0x5F965: 				CheckBox Prompt: " GP_2", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1036, VarStoreId: 0x6, VarOffset: 0x6CB, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 77 17 6D 17 36 10 06 00 CB 06 10 01 }
0x5F973: 				End  { 29 02 }
0x5F975: 				CheckBox Prompt: " GP_3", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1037, VarStoreId: 0x6, VarOffset: 0x6CC, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 78 17 6D 17 37 10 06 00 CC 06 10 01 }
0x5F983: 				End  { 29 02 }
0x5F985: 				CheckBox Prompt: " GP_4", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1038, VarStoreId: 0x6, VarOffset: 0x6CD, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 79 17 6D 17 38 10 06 00 CD 06 10 01 }
0x5F993: 				End  { 29 02 }
0x5F995: 				CheckBox Prompt: " GP_5", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x1039, VarStoreId: 0x6, VarOffset: 0x6CE, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 7A 17 6D 17 39 10 06 00 CE 06 10 01 }
0x5F9A3: 				End  { 29 02 }
0x5F9A5: 				CheckBox Prompt: " GP_6", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x103A, VarStoreId: 0x6, VarOffset: 0x6CF, Flags: 0x1, Default: Enabled, MfgDefault: Disabled { 06 8E 7B 17 6D 17 3A 10 06 00 CF 06 10 01 }
0x5F9B3: 				End  { 29 02 }
0x5F9B5: 				CheckBox Prompt: " GP_7", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0x103B, VarStoreId: 0x6, VarOffset: 0x6D0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 7C 17 6D 17 3B 10 06 00 D0 06 10 00 }
0x5F9C3: 				End  { 29 02 }
0x5F9C5: 			End  { 29 02 }
0x5F9C7: 		End  { 29 02 }
0x5F9C9: 		SuppressIf  { 0A 82 }
0x5F9CB: 			EqIdVal QuestionId: 0x110E, Value: 0x1 { 12 06 0E 11 01 00 }
0x5F9D1: 			Subtitle Prompt: "ISH is not available", Help: "", Flags: 0x0 { 02 87 67 17 00 00 00 }
0x5F9D8: 			End  { 29 02 }
0x5F9DA: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x5F9E1: 			End  { 29 02 }
0x5F9E3: 		End  { 29 02 }
0x5F9E5: 	End  { 29 02 }
0x5F9E7: 	Form FormId: 0x2854, Title: "Pch Thermal Throttling Control" { 01 86 54 28 0A 18 }
0x5F9ED: 		OneOf Prompt: "Thermal Throttling Level", Help: "Determine if use Intel suggested setting", QuestionFlags: 0x10, QuestionId: 0x103C, VarStoreId: 0x6, VarOffset: 0x717, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 26 18 27 18 3C 10 06 00 17 07 10 10 00 01 00 }
0x5F9FE: 			OneOfOption Option: "Suggested Setting" Value: 1, Default { 09 07 2C 18 10 00 01 }
0x5FA05: 			OneOfOption Option: "Manual" Value: 0 { 09 07 94 16 00 00 00 }
0x5FA0C: 		End  { 29 02 }
0x5FA0E: 		SuppressIf  { 0A 82 }
0x5FA10: 			EqIdVal QuestionId: 0x103C, Value: 0x1 { 12 06 3C 10 01 00 }
0x5FA16: 			CheckBox Prompt: "Thermal Throttling", Help: "Enable/Disable the thermal throttling states control", QuestionFlags: 0x10, QuestionId: 0x103D, VarStoreId: 0x6, VarOffset: 0x71E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 0B 18 0C 18 3D 10 06 00 1E 07 10 00 }
0x5FA24: 			End  { 29 02 }
0x5FA26: 			CheckBox Prompt: "TT State 13", Help: "PMSync state 13 will force at least T2 state", QuestionFlags: 0x10, QuestionId: 0x103E, VarStoreId: 0x6, VarOffset: 0x71F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 13 18 14 18 3E 10 06 00 1F 07 10 00 }
0x5FA34: 			End  { 29 02 }
0x5FA36: 			CheckBox Prompt: "Thermal Throttling Lock", Help: "Lock the entire TL register", QuestionFlags: 0x10, QuestionId: 0x103F, VarStoreId: 0x6, VarOffset: 0x720, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 15 18 16 18 3F 10 06 00 20 07 10 00 }
0x5FA44: 			End  { 29 02 }
0x5FA46: 			Numeric Prompt: "T0 Level", Help: "If Trip Point Temperature <= T0Level, the system is in T0 state", QuestionFlags: 0x10, QuestionId: 0x1040, VarStoreId: 0x6, VarOffset: 0x718, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 0D 18 0E 18 40 10 06 00 18 07 10 11 00 00 FF FF 01 00 }
0x5FA5A: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5FA61: 			End  { 29 02 }
0x5FA63: 			Numeric Prompt: "T1 Level", Help: "If T1Level >= Trip Point Temperature > T0Level, the system is in T1 state", QuestionFlags: 0x10, QuestionId: 0x1041, VarStoreId: 0x6, VarOffset: 0x71A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 0F 18 10 18 41 10 06 00 1A 07 10 11 00 00 FF FF 01 00 }
0x5FA77: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5FA7E: 			End  { 29 02 }
0x5FA80: 			Numeric Prompt: "T2 Level", Help: "If T2Level >= Trip Point Temperature > T1Level, the system is in T2 state", QuestionFlags: 0x10, QuestionId: 0x1042, VarStoreId: 0x6, VarOffset: 0x71C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 11 18 12 18 42 10 06 00 1C 07 10 11 00 00 FF FF 01 00 }
0x5FA94: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x5FA9B: 			End  { 29 02 }
0x5FA9D: 		End  { 29 02 }
0x5FA9F: 		OneOf Prompt: "DMI Thermal Setting", Help: "Determine if use Intel suggested setting", QuestionFlags: 0x10, QuestionId: 0x1043, VarStoreId: 0x6, VarOffset: 0x721, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 18 29 18 43 10 06 00 21 07 10 10 00 01 00 }
0x5FAB0: 			OneOfOption Option: "Suggested Setting" Value: 1, Default { 09 07 2C 18 10 00 01 }
0x5FAB7: 			OneOfOption Option: "Manual" Value: 0 { 09 07 94 16 00 00 00 }
0x5FABE: 		End  { 29 02 }
0x5FAC0: 		SuppressIf  { 0A 82 }
0x5FAC2: 			EqIdVal QuestionId: 0x1043, Value: 0x1 { 12 06 43 10 01 00 }
0x5FAC8: 			CheckBox Prompt: "DMI Thermal Sensor Autonomous Width", Help: "Enable/Disable Thermal Sensor initiated Autonomous Width Negotiation", QuestionFlags: 0x10, QuestionId: 0x1044, VarStoreId: 0x6, VarOffset: 0x726, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 17 18 18 18 44 10 06 00 26 07 10 00 }
0x5FAD6: 			End  { 29 02 }
0x5FAD8: 			OneOf Prompt: "Thermal Sensor 0 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T0", QuestionFlags: 0x10, QuestionId: 0x1045, VarStoreId: 0x6, VarOffset: 0x722, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 19 18 1A 18 45 10 06 00 22 07 10 10 00 04 00 }
0x5FAE9: 				OneOfOption Option: "x1" Value: 0 { 09 07 21 18 00 00 00 }
0x5FAF0: 				OneOfOption Option: "x2" Value: 1 { 09 07 22 18 00 00 01 }
0x5FAF7: 				OneOfOption Option: "x4" Value: 2 { 09 07 23 18 00 00 02 }
0x5FAFE: 				OneOfOption Option: "x8" Value: 3, Default { 09 07 24 18 10 00 03 }
0x5FB05: 				OneOfOption Option: "x16" Value: 4 { 09 07 25 18 00 00 04 }
0x5FB0C: 			End  { 29 02 }
0x5FB0E: 			OneOf Prompt: "Thermal Sensor 1 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T1", QuestionFlags: 0x10, QuestionId: 0x1046, VarStoreId: 0x6, VarOffset: 0x723, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 1B 18 1C 18 46 10 06 00 23 07 10 10 00 04 00 }
0x5FB1F: 				OneOfOption Option: "x1" Value: 0 { 09 07 21 18 00 00 00 }
0x5FB26: 				OneOfOption Option: "x2" Value: 1 { 09 07 22 18 00 00 01 }
0x5FB2D: 				OneOfOption Option: "x4" Value: 2, Default { 09 07 23 18 10 00 02 }
0x5FB34: 				OneOfOption Option: "x8" Value: 3 { 09 07 24 18 00 00 03 }
0x5FB3B: 				OneOfOption Option: "x16" Value: 4 { 09 07 25 18 00 00 04 }
0x5FB42: 			End  { 29 02 }
0x5FB44: 			OneOf Prompt: "Thermal Sensor 2 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T2", QuestionFlags: 0x10, QuestionId: 0x1047, VarStoreId: 0x6, VarOffset: 0x724, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 1D 18 1E 18 47 10 06 00 24 07 10 10 00 04 00 }
0x5FB55: 				OneOfOption Option: "x1" Value: 0 { 09 07 21 18 00 00 00 }
0x5FB5C: 				OneOfOption Option: "x2" Value: 1, Default { 09 07 22 18 10 00 01 }
0x5FB63: 				OneOfOption Option: "x4" Value: 2 { 09 07 23 18 00 00 02 }
0x5FB6A: 				OneOfOption Option: "x8" Value: 3 { 09 07 24 18 00 00 03 }
0x5FB71: 				OneOfOption Option: "x16" Value: 4 { 09 07 25 18 00 00 04 }
0x5FB78: 			End  { 29 02 }
0x5FB7A: 			OneOf Prompt: "Thermal Sensor 3 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T3", QuestionFlags: 0x10, QuestionId: 0x1048, VarStoreId: 0x6, VarOffset: 0x725, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0 { 05 91 1F 18 20 18 48 10 06 00 25 07 10 10 00 04 00 }
0x5FB8B: 				OneOfOption Option: "x1" Value: 0, Default { 09 07 21 18 10 00 00 }
0x5FB92: 				OneOfOption Option: "x2" Value: 1 { 09 07 22 18 00 00 01 }
0x5FB99: 				OneOfOption Option: "x4" Value: 2 { 09 07 23 18 00 00 02 }
0x5FBA0: 				OneOfOption Option: "x8" Value: 3 { 09 07 24 18 00 00 03 }
0x5FBA7: 				OneOfOption Option: "x16" Value: 4 { 09 07 25 18 00 00 04 }
0x5FBAE: 			End  { 29 02 }
0x5FBB0: 		End  { 29 02 }
0x5FBB2: 		OneOf Prompt: "SATA Thermal Setting", Help: "Determine if use Intel suggested setting", QuestionFlags: 0x10, QuestionId: 0x1049, VarStoreId: 0x6, VarOffset: 0x727, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 2A 18 2B 18 49 10 06 00 27 07 10 10 00 01 00 }
0x5FBC3: 			OneOfOption Option: "Suggested Setting" Value: 1, Default { 09 07 2C 18 10 00 01 }
0x5FBCA: 			OneOfOption Option: "Manual" Value: 0 { 09 07 94 16 00 00 00 }
0x5FBD1: 		End  { 29 02 }
0x5FBD3: 		SuppressIf  { 0A 82 }
0x5FBD5: 			EqIdVal QuestionId: 0x1049, Value: 0x1 { 12 06 49 10 01 00 }
0x5FBDB: 			Subtitle Prompt: "Port 0", Help: "", Flags: 0x0 { 02 87 08 18 00 00 00 }
0x5FBE2: 			End  { 29 02 }
0x5FBE4: 			OneOf Prompt: "T1 Multipler", Help: "Determine the value of SATA Port T1 Multipler", QuestionFlags: 0x10, QuestionId: 0x104A, VarStoreId: 0x6, VarOffset: 0x728, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 2D 18 2F 18 4A 10 06 00 28 07 10 10 00 03 00 }
0x5FBF5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FBFC: 				OneOfOption Option: "x1" Value: 1, Default { 09 07 21 18 10 00 01 }
0x5FC03: 				OneOfOption Option: "x2" Value: 2 { 09 07 22 18 00 00 02 }
0x5FC0A: 				OneOfOption Option: "x4" Value: 3 { 09 07 23 18 00 00 03 }
0x5FC11: 			End  { 29 02 }
0x5FC13: 			OneOf Prompt: "T2 Multipler", Help: "Determine the value of SATA Port T2 Multipler", QuestionFlags: 0x10, QuestionId: 0x104B, VarStoreId: 0x6, VarOffset: 0x729, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 30 18 32 18 4B 10 06 00 29 07 10 10 00 03 00 }
0x5FC24: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FC2B: 				OneOfOption Option: "x1" Value: 1 { 09 07 21 18 00 00 01 }
0x5FC32: 				OneOfOption Option: "x2" Value: 2, Default { 09 07 22 18 10 00 02 }
0x5FC39: 				OneOfOption Option: "x4" Value: 3 { 09 07 23 18 00 00 03 }
0x5FC40: 			End  { 29 02 }
0x5FC42: 			OneOf Prompt: "T3 Multipler", Help: "Determine the value of SATA Port T3 Multipler", QuestionFlags: 0x10, QuestionId: 0x104C, VarStoreId: 0x6, VarOffset: 0x72A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 33 18 35 18 4C 10 06 00 2A 07 10 10 00 03 00 }
0x5FC53: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FC5A: 				OneOfOption Option: "x1" Value: 1 { 09 07 21 18 00 00 01 }
0x5FC61: 				OneOfOption Option: "x2" Value: 2 { 09 07 22 18 00 00 02 }
0x5FC68: 				OneOfOption Option: "x4" Value: 3, Default { 09 07 23 18 10 00 03 }
0x5FC6F: 			End  { 29 02 }
0x5FC71: 			CheckBox Prompt: "Alternate Fast Init Tdispatch", Help: "Enable/Disable SATA Port Alternate Fast Init Tdispatch", QuestionFlags: 0x10, QuestionId: 0x104D, VarStoreId: 0x6, VarOffset: 0x72D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 3C 18 3E 18 4D 10 06 00 2D 07 10 00 }
0x5FC7F: 			End  { 29 02 }
0x5FC81: 		End  { 29 02 }
0x5FC83: 		SuppressIf  { 0A 82 }
0x5FC85: 			EqIdVal QuestionId: 0x1049, Value: 0x1 { 12 06 49 10 01 00 }
0x5FC8B: 			OneOf Prompt: "Tdispatch", Help: "Determine the value of SATA Port Tdispatch", QuestionFlags: 0x10, QuestionId: 0x104E, VarStoreId: 0x6, VarOffset: 0x72B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 36 18 38 18 4E 10 06 00 2B 07 10 10 00 03 00 }
0x5FC9C: 				SuppressIf  { 0A 82 }
0x5FC9E: 					EqIdVal QuestionId: 0x104D, Value: 0x0 { 12 06 4D 10 00 00 }
0x5FCA4: 					OneOfOption Option: "~32us" Value: 0, Default { 09 07 42 18 10 00 00 }
0x5FCAB: 					OneOfOption Option: "~128us" Value: 1 { 09 07 43 18 00 00 01 }
0x5FCB2: 					OneOfOption Option: "~8us" Value: 3 { 09 07 44 18 00 00 03 }
0x5FCB9: 				End  { 29 02 }
0x5FCBB: 				SuppressIf  { 0A 82 }
0x5FCBD: 					EqIdVal QuestionId: 0x104D, Value: 0x1 { 12 06 4D 10 01 00 }
0x5FCC3: 					OneOfOption Option: "~32ms" Value: 0, Default { 09 07 3F 18 10 00 00 }
0x5FCCA: 					OneOfOption Option: "~128ms" Value: 1 { 09 07 40 18 00 00 01 }
0x5FCD1: 					OneOfOption Option: "~8ms" Value: 3 { 09 07 41 18 00 00 03 }
0x5FCD8: 				End  { 29 02 }
0x5FCDA: 			End  { 29 02 }
0x5FCDC: 			OneOf Prompt: "Tinactive", Help: "Determine the value of SATA Port Tinactive", QuestionFlags: 0x10, QuestionId: 0x104F, VarStoreId: 0x6, VarOffset: 0x72C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 39 18 3B 18 4F 10 06 00 2C 07 10 10 00 03 00 }
0x5FCED: 				SuppressIf  { 0A 82 }
0x5FCEF: 					EqIdVal QuestionId: 0x104D, Value: 0x0 { 12 06 4D 10 00 00 }
0x5FCF5: 					OneOfOption Option: "~32us" Value: 0, Default { 09 07 42 18 10 00 00 }
0x5FCFC: 					OneOfOption Option: "~128us" Value: 1 { 09 07 43 18 00 00 01 }
0x5FD03: 					OneOfOption Option: "~8us" Value: 3 { 09 07 44 18 00 00 03 }
0x5FD0A: 				End  { 29 02 }
0x5FD0C: 				SuppressIf  { 0A 82 }
0x5FD0E: 					EqIdVal QuestionId: 0x104D, Value: 0x1 { 12 06 4D 10 01 00 }
0x5FD14: 					OneOfOption Option: "~32ms" Value: 0, Default { 09 07 3F 18 10 00 00 }
0x5FD1B: 					OneOfOption Option: "~128ms" Value: 1 { 09 07 40 18 00 00 01 }
0x5FD22: 					OneOfOption Option: "~8ms" Value: 3 { 09 07 41 18 00 00 03 }
0x5FD29: 				End  { 29 02 }
0x5FD2B: 			End  { 29 02 }
0x5FD2D: 		End  { 29 02 }
0x5FD2F: 		SuppressIf  { 0A 82 }
0x5FD31: 			EqIdVal QuestionId: 0x1049, Value: 0x1 { 12 06 49 10 01 00 }
0x5FD37: 			Subtitle Prompt: "Port 1", Help: "", Flags: 0x0 { 02 87 09 18 00 00 00 }
0x5FD3E: 			End  { 29 02 }
0x5FD40: 			OneOf Prompt: "T1 Multipler", Help: "Determine the value of SATA Port T1 Multipler", QuestionFlags: 0x10, QuestionId: 0x1050, VarStoreId: 0x6, VarOffset: 0x72E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 2E 18 2F 18 50 10 06 00 2E 07 10 10 00 03 00 }
0x5FD51: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FD58: 				OneOfOption Option: "x1" Value: 1, Default { 09 07 21 18 10 00 01 }
0x5FD5F: 				OneOfOption Option: "x2" Value: 2 { 09 07 22 18 00 00 02 }
0x5FD66: 				OneOfOption Option: "x4" Value: 3 { 09 07 23 18 00 00 03 }
0x5FD6D: 			End  { 29 02 }
0x5FD6F: 			OneOf Prompt: "T2 Multipler", Help: "Determine the value of SATA Port T2 Multipler", QuestionFlags: 0x10, QuestionId: 0x1051, VarStoreId: 0x6, VarOffset: 0x72F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 31 18 32 18 51 10 06 00 2F 07 10 10 00 03 00 }
0x5FD80: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FD87: 				OneOfOption Option: "x1" Value: 1 { 09 07 21 18 00 00 01 }
0x5FD8E: 				OneOfOption Option: "x2" Value: 2, Default { 09 07 22 18 10 00 02 }
0x5FD95: 				OneOfOption Option: "x4" Value: 3 { 09 07 23 18 00 00 03 }
0x5FD9C: 			End  { 29 02 }
0x5FD9E: 			OneOf Prompt: "T3 Multipler", Help: "Determine the value of SATA Port T3 Multipler", QuestionFlags: 0x10, QuestionId: 0x1052, VarStoreId: 0x6, VarOffset: 0x730, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 34 18 35 18 52 10 06 00 30 07 10 10 00 03 00 }
0x5FDAF: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FDB6: 				OneOfOption Option: "x1" Value: 1 { 09 07 21 18 00 00 01 }
0x5FDBD: 				OneOfOption Option: "x2" Value: 2 { 09 07 22 18 00 00 02 }
0x5FDC4: 				OneOfOption Option: "x4" Value: 3, Default { 09 07 23 18 10 00 03 }
0x5FDCB: 			End  { 29 02 }
0x5FDCD: 			CheckBox Prompt: "Alternate Fast Init Tdispatch", Help: "Enable/Disable SATA Port Alternate Fast Init Tdispatch", QuestionFlags: 0x10, QuestionId: 0x1053, VarStoreId: 0x6, VarOffset: 0x733, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 3D 18 3E 18 53 10 06 00 33 07 10 00 }
0x5FDDB: 			End  { 29 02 }
0x5FDDD: 		End  { 29 02 }
0x5FDDF: 		SuppressIf  { 0A 82 }
0x5FDE1: 			EqIdVal QuestionId: 0x1049, Value: 0x1 { 12 06 49 10 01 00 }
0x5FDE7: 			OneOf Prompt: "Tdispatch", Help: "Determine the value of SATA Port Tdispatch", QuestionFlags: 0x10, QuestionId: 0x1054, VarStoreId: 0x6, VarOffset: 0x731, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 37 18 38 18 54 10 06 00 31 07 10 10 00 03 00 }
0x5FDF8: 				SuppressIf  { 0A 82 }
0x5FDFA: 					EqIdVal QuestionId: 0x1053, Value: 0x0 { 12 06 53 10 00 00 }
0x5FE00: 					OneOfOption Option: "~32us" Value: 0, Default { 09 07 42 18 10 00 00 }
0x5FE07: 					OneOfOption Option: "~128us" Value: 1 { 09 07 43 18 00 00 01 }
0x5FE0E: 					OneOfOption Option: "~8us" Value: 3 { 09 07 44 18 00 00 03 }
0x5FE15: 				End  { 29 02 }
0x5FE17: 				SuppressIf  { 0A 82 }
0x5FE19: 					EqIdVal QuestionId: 0x1053, Value: 0x1 { 12 06 53 10 01 00 }
0x5FE1F: 					OneOfOption Option: "~32ms" Value: 0, Default { 09 07 3F 18 10 00 00 }
0x5FE26: 					OneOfOption Option: "~128ms" Value: 1 { 09 07 40 18 00 00 01 }
0x5FE2D: 					OneOfOption Option: "~8ms" Value: 3 { 09 07 41 18 00 00 03 }
0x5FE34: 				End  { 29 02 }
0x5FE36: 			End  { 29 02 }
0x5FE38: 			OneOf Prompt: "Tinactive", Help: "Determine the value of SATA Port Tinactive", QuestionFlags: 0x10, QuestionId: 0x1055, VarStoreId: 0x6, VarOffset: 0x732, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0 { 05 91 3A 18 3B 18 55 10 06 00 32 07 10 10 00 03 00 }
0x5FE49: 				SuppressIf  { 0A 82 }
0x5FE4B: 					EqIdVal QuestionId: 0x1053, Value: 0x0 { 12 06 53 10 00 00 }
0x5FE51: 					OneOfOption Option: "~32us" Value: 0, Default { 09 07 42 18 10 00 00 }
0x5FE58: 					OneOfOption Option: "~128us" Value: 1 { 09 07 43 18 00 00 01 }
0x5FE5F: 					OneOfOption Option: "~8us" Value: 3 { 09 07 44 18 00 00 03 }
0x5FE66: 				End  { 29 02 }
0x5FE68: 				SuppressIf  { 0A 82 }
0x5FE6A: 					EqIdVal QuestionId: 0x1053, Value: 0x1 { 12 06 53 10 01 00 }
0x5FE70: 					OneOfOption Option: "~32ms" Value: 0, Default { 09 07 3F 18 10 00 00 }
0x5FE77: 					OneOfOption Option: "~128ms" Value: 1 { 09 07 40 18 00 00 01 }
0x5FE7E: 					OneOfOption Option: "~8ms" Value: 3 { 09 07 41 18 00 00 03 }
0x5FE85: 				End  { 29 02 }
0x5FE87: 			End  { 29 02 }
0x5FE89: 		End  { 29 02 }
0x5FE8B: 	End  { 29 02 }
0x5FE8D: 	Form FormId: 0x2855, Title: "Serial IO Touch Pad Settings" { 01 86 55 28 ED 17 }
0x5FE93: 		OneOf Prompt: "Touch Pad", Help: "Indicates what type of I2C Touch Pad is connected to this SerialIo controller", QuestionFlags: 0x10, QuestionId: 0x1056, VarStoreId: 0xF101, VarOffset: 0x5D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x0 { 05 91 EE 17 EF 17 56 10 01 F1 D8 05 10 10 00 09 00 }
0x5FEA4: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x5FEAB: 			OneOfOption Option: "Synaptics Precision Touchpad" Value: 1 { 09 07 C8 17 00 00 01 }
0x5FEB2: 			OneOfOption Option: "Synaptics Forcepad" Value: 2 { 09 07 05 18 00 00 02 }
0x5FEB9: 			OneOfOption Option: "ALPS Precision Touchpad ClickPad" Value: 6 { 09 07 C9 17 00 00 06 }
0x5FEC0: 			OneOfOption Option: "THAT Touchpad" Value: 7 { 09 07 CA 17 00 00 07 }
0x5FEC7: 			OneOfOption Option: "Sensel Forcepad" Value: 8 { 09 07 06 18 00 00 08 }
0x5FECE: 			OneOfOption Option: "Smart C Cover" Value: 9 { 09 07 07 18 00 00 09 }
0x5FED5: 			OneOfOption Option: "Custom device" Value: 5, Default, MfgDefault { 09 07 4B 18 30 00 05 }
0x5FEDC: 		End  { 29 02 }
0x5FEDE: 		SuppressIf  { 0A 82 }
0x5FEE0: 			EqIdVal QuestionId: 0x1056, Value: 0x0 { 12 86 56 10 00 00 }
0x5FEE6: 				EqIdVal QuestionId: 0xF94, Value: 0x1 { 12 06 94 0F 01 00 }
0x5FEEC: 				EqIdVal QuestionId: 0x1056, Value: 0x3 { 12 06 56 10 03 00 }
0x5FEF2: 				EqIdVal QuestionId: 0x1056, Value: 0x4 { 12 06 56 10 04 00 }
0x5FEF8: 				Or  { 16 02 }
0x5FEFA: 				And  { 15 02 }
0x5FEFC: 				Or  { 16 02 }
0x5FEFE: 			End  { 29 02 }
0x5FF00: 			OneOf Prompt: "Touch Pad Interrupt Mode", Help: "Selects different routing for interrupts from Touch Pad", QuestionFlags: 0x10, QuestionId: 0x1057, VarStoreId: 0xF101, VarOffset: 0x5D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F0 17 F1 17 57 10 01 F1 D9 05 10 10 00 01 00 }
0x5FF11: 				OneOfOption Option: "GPIO Interrupt" Value: 0, Default, MfgDefault { 09 07 80 17 30 00 00 }
0x5FF18: 				OneOfOption Option: "APIC Interrupt" Value: 1 { 09 07 7F 17 00 00 01 }
0x5FF1F: 			End  { 29 02 }
0x5FF21: 		End  { 29 02 }
0x5FF23: 		SuppressIf  { 0A 82 }
0x5FF25: 			EqIdVal QuestionId: 0x1056, Value: 0x5 { 12 86 56 10 05 00 }
0x5FF2B: 				Not  { 17 02 }
0x5FF2D: 			End  { 29 02 }
0x5FF2F: 			Numeric Prompt: "Device's bus address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0x1058, VarStoreId: 0xF101, VarOffset: 0x5DA, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 91 4C 18 52 18 58 10 01 F1 DA 05 10 20 00 7F 01 }
0x5FF40: 				Default DefaultId: 0x0 Value: 21 { 5B 06 00 00 00 15 }
0x5FF46: 			End  { 29 02 }
0x5FF48: 			Numeric Prompt: "Device's HID address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0x1059, VarStoreId: 0xF101, VarOffset: 0x5DB, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 4D 18 52 18 59 10 01 F1 DB 05 10 21 00 00 FF FF 01 00 }
0x5FF5C: 				Default DefaultId: 0x0 Value: 1 { 5B 07 00 00 01 01 00 }
0x5FF63: 			End  { 29 02 }
0x5FF65: 			OneOf Prompt: "Device's bus speed", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0x105A, VarStoreId: 0xF101, VarOffset: 0x5DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 4E 18 52 18 5A 10 01 F1 DD 05 10 10 00 02 00 }
0x5FF76: 				OneOfOption Option: "100kHz" Value: 0 { 09 07 4F 18 00 00 00 }
0x5FF7D: 				OneOfOption Option: "400kHz" Value: 1, Default, MfgDefault { 09 07 50 18 30 00 01 }
0x5FF84: 				OneOfOption Option: "1MHz" Value: 2 { 09 07 51 18 00 00 02 }
0x5FF8B: 			End  { 29 02 }
0x5FF8D: 		End  { 29 02 }
0x5FF8F: 	End  { 29 02 }
0x5FF91: 	Form FormId: 0x2856, Title: "Serial IO Touch Panel Settings" { 01 86 56 28 F2 17 }
0x5FF97: 		OneOf Prompt: "Touch Panel", Help: "Indicates what type of I2C Touch Panel is connected to this SerialIo controller", QuestionFlags: 0x10, QuestionId: 0x105B, VarStoreId: 0xF101, VarOffset: 0x5DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 F3 17 F4 17 5B 10 01 F1 DE 05 10 10 00 07 00 }
0x5FFA8: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 04 00 30 00 00 }
0x5FFAF: 			OneOfOption Option: "Atmel3432 TouchPanel" Value: 1 { 09 07 45 18 00 00 01 }
0x5FFB6: 			OneOfOption Option: "Atmel2952 TouchPanel" Value: 2 { 09 07 46 18 00 00 02 }
0x5FFBD: 			OneOfOption Option: "Elan9048 TouchPanel" Value: 3 { 09 07 47 18 00 00 03 }
0x5FFC4: 			OneOfOption Option: "N-Trig/Samsung 13.3"" Value: 4 { 09 07 48 18 00 00 04 }
0x5FFCB: 			OneOfOption Option: "N-Trig/Sharp 12.5"" Value: 5 { 09 07 49 18 00 00 05 }
0x5FFD2: 			OneOfOption Option: "WACOM TouchPanel" Value: 6 { 09 07 4A 18 00 00 06 }
0x5FFD9: 			OneOfOption Option: "Custom device" Value: 7 { 09 07 4B 18 00 00 07 }
0x5FFE0: 		End  { 29 02 }
0x5FFE2: 		SuppressIf  { 0A 82 }
0x5FFE4: 			EqIdVal QuestionId: 0x105B, Value: 0x0 { 12 06 5B 10 00 00 }
0x5FFEA: 			OneOf Prompt: "Touch Panel Interrupt Mode", Help: "Selects different routing for interrupts from Touch Panel", QuestionFlags: 0x10, QuestionId: 0x105C, VarStoreId: 0xF101, VarOffset: 0x5DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 F5 17 F6 17 5C 10 01 F1 DF 05 10 10 00 01 00 }
0x5FFFB: 				OneOfOption Option: "GPIO Interrupt" Value: 0, Default, MfgDefault { 09 07 80 17 30 00 00 }
0x60002: 				OneOfOption Option: "APIC Interrupt" Value: 1 { 09 07 7F 17 00 00 01 }
0x60009: 			End  { 29 02 }
0x6000B: 		End  { 29 02 }
0x6000D: 		SuppressIf  { 0A 82 }
0x6000F: 			EqIdVal QuestionId: 0x105B, Value: 0x7 { 12 86 5B 10 07 00 }
0x60015: 				Not  { 17 02 }
0x60017: 			End  { 29 02 }
0x60019: 			Numeric Prompt: "Device's bus address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0x105D, VarStoreId: 0xF101, VarOffset: 0x5E0, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1 { 07 91 99 19 52 18 5D 10 01 F1 E0 05 10 20 00 7F 01 }
0x6002A: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x60030: 			End  { 29 02 }
0x60032: 			Numeric Prompt: "Device's HID address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0x105E, VarStoreId: 0xF101, VarOffset: 0x5E1, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1 { 07 94 9A 19 52 18 5E 10 01 F1 E1 05 10 21 00 00 FF FF 01 00 }
0x60046: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x6004D: 			End  { 29 02 }
0x6004F: 		End  { 29 02 }
0x60051: 		SuppressIf  { 0A 82 }
0x60053: 			QuestionRef1 QuestionId: 0x105B { 40 84 5B 10 }
0x60057: 				Uint8 Value: 0x6 { 42 03 06 }
0x6005A: 				GreaterEqual  { 32 02 }
0x6005C: 				Not  { 17 02 }
0x6005E: 			End  { 29 02 }
0x60060: 			OneOf Prompt: "Device's bus speed", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0x105F, VarStoreId: 0xF101, VarOffset: 0x5E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 9B 19 52 18 5F 10 01 F1 E3 05 10 10 00 02 00 }
0x60071: 				SuppressIf  { 0A 82 }
0x60073: 					EqIdVal QuestionId: 0x105B, Value: 0x7 { 12 86 5B 10 07 00 }
0x60079: 						Not  { 17 02 }
0x6007B: 					End  { 29 02 }
0x6007D: 					OneOfOption Option: "100kHz" Value: 0 { 09 07 4F 18 00 00 00 }
0x60084: 				End  { 29 02 }
0x60086: 				OneOfOption Option: "400kHz" Value: 1, Default, MfgDefault { 09 07 50 18 30 00 01 }
0x6008D: 				OneOfOption Option: "1MHz" Value: 2 { 09 07 51 18 00 00 02 }
0x60094: 			End  { 29 02 }
0x60096: 		End  { 29 02 }
0x60098: 	End  { 29 02 }
0x6009A: 	Form FormId: 0x2857, Title: "Serial IO Finger Print Settings" { 01 86 57 28 F7 17 }
0x600A0: 		OneOf Prompt: "Finger Print Sensor", Help: "Select the HID to enable Finger Print Sensor", QuestionFlags: 0x10, QuestionId: 0x1060, VarStoreId: 0xF101, VarOffset: 0x5EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0 { 05 91 F8 17 F9 17 60 10 01 F1 EB 05 10 10 00 06 00 }
0x600B1: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x600B7: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x600BE: 			OneOfOption Option: "FPC1011" Value: 1 { 09 07 FC 17 00 00 01 }
0x600C5: 			OneOfOption Option: "FPC1020" Value: 2 { 09 07 FD 17 00 00 02 }
0x600CC: 			OneOfOption Option: "VFSI6101" Value: 3 { 09 07 FF 17 00 00 03 }
0x600D3: 			OneOfOption Option: "Synaptics VFSI7500" Value: 4 { 09 07 00 18 00 00 04 }
0x600DA: 			OneOfOption Option: "EGIS0300" Value: 5 { 09 07 01 18 00 00 05 }
0x600E1: 			OneOfOption Option: "FPC1021" Value: 6 { 09 07 FE 17 00 00 06 }
0x600E8: 		End  { 29 02 }
0x600EA: 		SuppressIf  { 0A 82 }
0x600EC: 			EqIdVal QuestionId: 0x1060, Value: 0x0 { 12 06 60 10 00 00 }
0x600F2: 			OneOf Prompt: "Finger Print Interrupt Mode", Help: "Selects different routing for interrupts from Finger Print", QuestionFlags: 0x10, QuestionId: 0x1061, VarStoreId: 0xF101, VarOffset: 0x5EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 FA 17 FB 17 61 10 01 F1 EC 05 10 10 00 01 00 }
0x60103: 				OneOfOption Option: "GPIO Interrupt" Value: 0 { 09 07 80 17 00 00 00 }
0x6010A: 				OneOfOption Option: "APIC Interrupt" Value: 1, Default, MfgDefault { 09 07 7F 17 30 00 01 }
0x60111: 			End  { 29 02 }
0x60113: 		End  { 29 02 }
0x60115: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x6011C: 		End  { 29 02 }
0x6011E: 		SuppressIf  { 0A 82 }
0x60120: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x60126: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x6012D: 			End  { 29 02 }
0x6012F: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1062, VarStoreId: 0xF101, VarOffset: 0x6A1, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 91 19 C0 17 62 10 01 F1 A1 06 00 11 01 00 10 27 00 00 }
0x60143: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x6014A: 			End  { 29 02 }
0x6014C: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1063, VarStoreId: 0xF101, VarOffset: 0x6A3, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 92 19 C2 17 63 10 01 F1 A3 06 00 11 01 00 10 27 00 00 }
0x60160: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x60167: 			End  { 29 02 }
0x60169: 		End  { 29 02 }
0x6016B: 		SuppressIf  { 0A 82 }
0x6016D: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x60173: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x6017A: 			End  { 29 02 }
0x6017C: 		End  { 29 02 }
0x6017E: 		SuppressIf  { 0A 82 }
0x60180: 			EqIdVal QuestionId: 0xF93, Value: 0x0 { 12 06 93 0F 00 00 }
0x60186: 			Subtitle Prompt: "Timing parameters", Help: "", Flags: 0x0 { 02 87 C6 17 00 00 00 }
0x6018D: 			End  { 29 02 }
0x6018F: 			Numeric Prompt: "D0->D3 idle timeout (screen off)", Help: "Default:
200 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1064, VarStoreId: 0xF101, VarOffset: 0x6A5, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 93 19 C0 17 64 10 01 F1 A5 06 00 11 01 00 10 27 00 00 }
0x601A3: 				Default DefaultId: 0x0 Value: 200 { 5B 07 00 00 01 C8 00 }
0x601AA: 			End  { 29 02 }
0x601AC: 			Numeric Prompt: "D0->D3 idle timeout (screen on)", Help: "Default:
2000 [DEC]

Minimum:
1 [DEC]

Maximum:
10000 [DEC]", QuestionFlags: 0x0, QuestionId: 0x1065, VarStoreId: 0xF101, VarOffset: 0x6A7, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0 { 07 94 94 19 C2 17 65 10 01 F1 A7 06 00 11 01 00 10 27 00 00 }
0x601C0: 				Default DefaultId: 0x0 Value: 2000 { 5B 07 00 00 01 D0 07 }
0x601C7: 			End  { 29 02 }
0x601C9: 		End  { 29 02 }
0x601CB: 		SuppressIf  { 0A 82 }
0x601CD: 			EqIdVal QuestionId: 0xF93, Value: 0x1 { 12 06 93 0F 01 00 }
0x601D3: 			Subtitle Prompt: "Timing parameters disabled", Help: "", Flags: 0x0 { 02 87 C7 17 00 00 00 }
0x601DA: 			End  { 29 02 }
0x601DC: 		End  { 29 02 }
0x601DE: 	End  { 29 02 }
0x601E0: 	Form FormId: 0x2858, Title: "FIVR Configuration" { 01 86 58 28 AA 18 }
0x601E6: 		Text Prompt: "VCCIN_AUX voltage rail timing configuration", Help: "VCCIN_AUX voltage rail timing configuration", Text: "" { 03 08 BF 18 BF 18 00 00 }
0x601EE: 		Numeric Prompt: "Off to High Current Mode", Help: "Transition time in microseconds from Off (0V) to High Current Mode Voltage. This field has 1us resolution. 0 = Transition to 0V is disabled. The value must be greater than or equal to VccST board FET ramp time", QuestionFlags: 0x10, QuestionId: 0x1066, VarStoreId: 0x6, VarOffset: 0x76B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FF, Step: 0x1 { 07 94 C6 18 C7 18 66 10 06 00 6B 07 10 11 00 00 FF 07 01 00 }
0x60202: 			Default DefaultId: 0x0 Value: 150 { 5B 07 00 00 01 96 00 }
0x60209: 		End  { 29 02 }
0x6020B: 	End  { 29 02 }
0x6020D: 	Form FormId: 0x2859, Title: "PMC Configuration" { 01 86 59 28 CC 18 }
0x60213: 		Ref Prompt: "PMC ADR Configuration", Help: "PMC ADR Configuration", QuestionFlags: 0x0, QuestionId: 0x1067, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x285A { 0F 0F CE 18 CE 18 67 10 00 00 FF FF 00 5A 28 }
0x60222: 	End  { 29 02 }
0x60224: 	Form FormId: 0x285A, Title: "PMC ADR Configuration" { 01 86 5A 28 CE 18 }
0x6022A: 		OneOf Prompt: "ADR enable", Help: "Enable asynchronous DRAM refresh", QuestionFlags: 0x10, QuestionId: 0x1068, VarStoreId: 0x6, VarOffset: 0x77F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 CF 18 D0 18 68 10 06 00 7F 07 10 10 00 02 00 }
0x6023B: 			OneOfOption Option: "Platform-POR" Value: 0, Default, MfgDefault { 09 07 59 18 30 00 00 }
0x60242: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 03 00 00 00 01 }
0x60249: 			OneOfOption Option: "Disabled" Value: 2 { 09 07 92 00 00 00 02 }
0x60250: 		End  { 29 02 }
0x60252: 		SuppressIf  { 0A 82 }
0x60254: 			EqIdVal QuestionId: 0x1068, Value: 0x2 { 12 06 68 10 02 00 }
0x6025A: 			OneOf Prompt: "Host Partition Reset ADR Enable", Help: "Enables/Disables ADR on Host Partition Reset", QuestionFlags: 0x10, QuestionId: 0x1069, VarStoreId: 0x6, VarOffset: 0x782, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 D3 18 D4 18 69 10 06 00 82 07 10 10 00 02 00 }
0x6026B: 				OneOfOption Option: "Platform-POR" Value: 0 { 09 07 59 18 00 00 00 }
0x60272: 				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault { 09 07 03 00 30 00 01 }
0x60279: 				OneOfOption Option: "Disabled" Value: 2 { 09 07 92 00 00 00 02 }
0x60280: 			End  { 29 02 }
0x60282: 			Numeric Prompt: "ADR timer 1 expire time", Help: "Type desired ADR timer expire time, valid values - <1, 256>. Entered time is scaled by ADR timer time unit.", QuestionFlags: 0x0, QuestionId: 0x106A, VarStoreId: 0x6, VarOffset: 0x780, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFF, Step: 0x0 { 07 91 D1 18 D2 18 6A 10 06 00 80 07 00 10 01 FF 00 }
0x60293: 				Default DefaultId: 0x0 Value: 32 { 5B 06 00 00 00 20 }
0x60299: 			End  { 29 02 }
0x6029B: 			OneOf Prompt: "ADR timer 1 time unit", Help: "Select ADR timer time unit.", QuestionFlags: 0x10, QuestionId: 0x106B, VarStoreId: 0x6, VarOffset: 0x781, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0 { 05 91 D5 18 D6 18 6B 10 06 00 81 07 10 10 00 07 00 }
0x602AC: 				OneOfOption Option: "1us" Value: 0 { 09 07 D7 18 00 00 00 }
0x602B3: 				OneOfOption Option: "10us" Value: 1 { 09 07 D8 18 00 00 01 }
0x602BA: 				OneOfOption Option: "100us" Value: 2 { 09 07 D9 18 00 00 02 }
0x602C1: 				OneOfOption Option: "1ms" Value: 3 { 09 07 DA 18 00 00 03 }
0x602C8: 				OneOfOption Option: "10ms" Value: 4 { 09 07 DB 18 00 00 04 }
0x602CF: 				OneOfOption Option: "100ms" Value: 5 { 09 07 DC 18 00 00 05 }
0x602D6: 				OneOfOption Option: "1s" Value: 6, Default { 09 07 DD 18 10 00 06 }
0x602DD: 				OneOfOption Option: "10s" Value: 7 { 09 07 DE 18 00 00 07 }
0x602E4: 			End  { 29 02 }
0x602E6: 		End  { 29 02 }
0x602E8: 	End  { 29 02 }
0x602EA: 	Form FormId: 0x28C5, Title: "SB Porting Configuration" { 01 86 C5 28 93 00 }
0x602F0: 		Subtitle Prompt: "SB Porting Configuration", Help: "", Flags: 0x0 { 02 87 94 00 00 00 00 }
0x602F7: 		End  { 29 02 }
0x602F9: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x60300: 		End  { 29 02 }
0x60302: 	End  { 29 02 }
0x60304: 	Form FormId: 0x28C6, Title: "Extra options " { 01 86 C6 28 95 00 }
0x6030A: 		GrayOutIf  { 19 82 }
0x6030C: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60312: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x106C, VarStoreId: 0xF101, VarOffset: 0xBD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B1 00 CD 00 6C 10 01 F1 D3 0B 10 10 00 01 00 }
0x60323: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x6032A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60331: 			End  { 29 02 }
0x60333: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x106D, VarStoreId: 0xF101, VarOffset: 0xBEF, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D0 00 EC 00 6D 10 01 F1 EF 0B 10 11 01 00 14 00 01 00 }
0x60347: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x6034E: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60355: 			End  { 29 02 }
0x60357: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x106E, VarStoreId: 0xF101, VarOffset: 0xC27, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 ED 00 09 01 6E 10 01 F1 27 0C 10 10 01 1F 01 }
0x60368: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6036E: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60374: 			End  { 29 02 }
0x60376: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x106F, VarStoreId: 0xF101, VarOffset: 0xC43, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 0A 01 26 01 6F 10 01 F1 43 0C 10 10 01 1F 01 }
0x60387: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6038D: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60393: 			End  { 29 02 }
0x60395: 		End  { 29 02 }
0x60397: 	End  { 29 02 }
0x60399: 	Form FormId: 0x28C7, Title: "Extra options " { 01 86 C7 28 96 00 }
0x6039F: 		GrayOutIf  { 19 82 }
0x603A1: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x603A7: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1070, VarStoreId: 0xF101, VarOffset: 0xBD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B2 00 CD 00 70 10 01 F1 D4 0B 10 10 00 01 00 }
0x603B8: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x603BF: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x603C6: 			End  { 29 02 }
0x603C8: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1071, VarStoreId: 0xF101, VarOffset: 0xBF1, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D1 00 EC 00 71 10 01 F1 F1 0B 10 11 01 00 14 00 01 00 }
0x603DC: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x603E3: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x603EA: 			End  { 29 02 }
0x603EC: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1072, VarStoreId: 0xF101, VarOffset: 0xC28, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 EE 00 09 01 72 10 01 F1 28 0C 10 10 01 1F 01 }
0x603FD: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60403: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60409: 			End  { 29 02 }
0x6040B: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1073, VarStoreId: 0xF101, VarOffset: 0xC44, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 0B 01 26 01 73 10 01 F1 44 0C 10 10 01 1F 01 }
0x6041C: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60422: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60428: 			End  { 29 02 }
0x6042A: 		End  { 29 02 }
0x6042C: 	End  { 29 02 }
0x6042E: 	Form FormId: 0x28C8, Title: "Extra options " { 01 86 C8 28 97 00 }
0x60434: 		GrayOutIf  { 19 82 }
0x60436: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x6043C: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1074, VarStoreId: 0xF101, VarOffset: 0xBD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B3 00 CD 00 74 10 01 F1 D5 0B 10 10 00 01 00 }
0x6044D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60454: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x6045B: 			End  { 29 02 }
0x6045D: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1075, VarStoreId: 0xF101, VarOffset: 0xBF3, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D2 00 EC 00 75 10 01 F1 F3 0B 10 11 01 00 14 00 01 00 }
0x60471: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60478: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x6047F: 			End  { 29 02 }
0x60481: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1076, VarStoreId: 0xF101, VarOffset: 0xC29, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 EF 00 09 01 76 10 01 F1 29 0C 10 10 01 1F 01 }
0x60492: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60498: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6049E: 			End  { 29 02 }
0x604A0: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1077, VarStoreId: 0xF101, VarOffset: 0xC45, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 0C 01 26 01 77 10 01 F1 45 0C 10 10 01 1F 01 }
0x604B1: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x604B7: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x604BD: 			End  { 29 02 }
0x604BF: 		End  { 29 02 }
0x604C1: 	End  { 29 02 }
0x604C3: 	Form FormId: 0x28C9, Title: "Extra options " { 01 86 C9 28 98 00 }
0x604C9: 		GrayOutIf  { 19 82 }
0x604CB: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x604D1: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1078, VarStoreId: 0xF101, VarOffset: 0xBD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B4 00 CD 00 78 10 01 F1 D6 0B 10 10 00 01 00 }
0x604E2: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x604E9: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x604F0: 			End  { 29 02 }
0x604F2: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1079, VarStoreId: 0xF101, VarOffset: 0xBF5, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D3 00 EC 00 79 10 01 F1 F5 0B 10 11 01 00 14 00 01 00 }
0x60506: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x6050D: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60514: 			End  { 29 02 }
0x60516: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x107A, VarStoreId: 0xF101, VarOffset: 0xC2A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F0 00 09 01 7A 10 01 F1 2A 0C 10 10 01 1F 01 }
0x60527: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6052D: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60533: 			End  { 29 02 }
0x60535: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x107B, VarStoreId: 0xF101, VarOffset: 0xC46, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 0D 01 26 01 7B 10 01 F1 46 0C 10 10 01 1F 01 }
0x60546: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6054C: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60552: 			End  { 29 02 }
0x60554: 		End  { 29 02 }
0x60556: 	End  { 29 02 }
0x60558: 	Form FormId: 0x28CA, Title: "Extra options " { 01 86 CA 28 99 00 }
0x6055E: 		GrayOutIf  { 19 82 }
0x60560: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60566: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x107C, VarStoreId: 0xF101, VarOffset: 0xBD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B5 00 CD 00 7C 10 01 F1 D7 0B 10 10 00 01 00 }
0x60577: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x6057E: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60585: 			End  { 29 02 }
0x60587: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x107D, VarStoreId: 0xF101, VarOffset: 0xBF7, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D4 00 EC 00 7D 10 01 F1 F7 0B 10 11 01 00 14 00 01 00 }
0x6059B: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x605A2: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x605A9: 			End  { 29 02 }
0x605AB: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x107E, VarStoreId: 0xF101, VarOffset: 0xC2B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F1 00 09 01 7E 10 01 F1 2B 0C 10 10 01 1F 01 }
0x605BC: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x605C2: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x605C8: 			End  { 29 02 }
0x605CA: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x107F, VarStoreId: 0xF101, VarOffset: 0xC47, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 0E 01 26 01 7F 10 01 F1 47 0C 10 10 01 1F 01 }
0x605DB: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x605E1: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x605E7: 			End  { 29 02 }
0x605E9: 		End  { 29 02 }
0x605EB: 	End  { 29 02 }
0x605ED: 	Form FormId: 0x28CB, Title: "Extra options " { 01 86 CB 28 9A 00 }
0x605F3: 		GrayOutIf  { 19 82 }
0x605F5: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x605FB: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1080, VarStoreId: 0xF101, VarOffset: 0xBD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B6 00 CD 00 80 10 01 F1 D8 0B 10 10 00 01 00 }
0x6060C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60613: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x6061A: 			End  { 29 02 }
0x6061C: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1081, VarStoreId: 0xF101, VarOffset: 0xBF9, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D5 00 EC 00 81 10 01 F1 F9 0B 10 11 01 00 14 00 01 00 }
0x60630: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60637: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x6063E: 			End  { 29 02 }
0x60640: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1082, VarStoreId: 0xF101, VarOffset: 0xC2C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F2 00 09 01 82 10 01 F1 2C 0C 10 10 01 1F 01 }
0x60651: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60657: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6065D: 			End  { 29 02 }
0x6065F: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1083, VarStoreId: 0xF101, VarOffset: 0xC48, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 0F 01 26 01 83 10 01 F1 48 0C 10 10 01 1F 01 }
0x60670: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60676: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6067C: 			End  { 29 02 }
0x6067E: 		End  { 29 02 }
0x60680: 	End  { 29 02 }
0x60682: 	Form FormId: 0x28CC, Title: "Extra options " { 01 86 CC 28 9B 00 }
0x60688: 		GrayOutIf  { 19 82 }
0x6068A: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60690: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1084, VarStoreId: 0xF101, VarOffset: 0xBD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B7 00 CD 00 84 10 01 F1 D9 0B 10 10 00 01 00 }
0x606A1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x606A8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x606AF: 			End  { 29 02 }
0x606B1: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1085, VarStoreId: 0xF101, VarOffset: 0xBFB, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D6 00 EC 00 85 10 01 F1 FB 0B 10 11 01 00 14 00 01 00 }
0x606C5: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x606CC: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x606D3: 			End  { 29 02 }
0x606D5: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1086, VarStoreId: 0xF101, VarOffset: 0xC2D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F3 00 09 01 86 10 01 F1 2D 0C 10 10 01 1F 01 }
0x606E6: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x606EC: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x606F2: 			End  { 29 02 }
0x606F4: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1087, VarStoreId: 0xF101, VarOffset: 0xC49, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 10 01 26 01 87 10 01 F1 49 0C 10 10 01 1F 01 }
0x60705: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6070B: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60711: 			End  { 29 02 }
0x60713: 		End  { 29 02 }
0x60715: 	End  { 29 02 }
0x60717: 	Form FormId: 0x28CD, Title: "Extra options " { 01 86 CD 28 9C 00 }
0x6071D: 		GrayOutIf  { 19 82 }
0x6071F: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60725: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1088, VarStoreId: 0xF101, VarOffset: 0xBDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B8 00 CD 00 88 10 01 F1 DA 0B 10 10 00 01 00 }
0x60736: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x6073D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60744: 			End  { 29 02 }
0x60746: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1089, VarStoreId: 0xF101, VarOffset: 0xBFD, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D7 00 EC 00 89 10 01 F1 FD 0B 10 11 01 00 14 00 01 00 }
0x6075A: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60761: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60768: 			End  { 29 02 }
0x6076A: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x108A, VarStoreId: 0xF101, VarOffset: 0xC2E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F4 00 09 01 8A 10 01 F1 2E 0C 10 10 01 1F 01 }
0x6077B: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60781: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60787: 			End  { 29 02 }
0x60789: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x108B, VarStoreId: 0xF101, VarOffset: 0xC4A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 11 01 26 01 8B 10 01 F1 4A 0C 10 10 01 1F 01 }
0x6079A: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x607A0: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x607A6: 			End  { 29 02 }
0x607A8: 		End  { 29 02 }
0x607AA: 	End  { 29 02 }
0x607AC: 	Form FormId: 0x28CE, Title: "Extra options " { 01 86 CE 28 9D 00 }
0x607B2: 		GrayOutIf  { 19 82 }
0x607B4: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x607BA: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x108C, VarStoreId: 0xF101, VarOffset: 0xBDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 B9 00 CD 00 8C 10 01 F1 DB 0B 10 10 00 01 00 }
0x607CB: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x607D2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x607D9: 			End  { 29 02 }
0x607DB: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x108D, VarStoreId: 0xF101, VarOffset: 0xBFF, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D8 00 EC 00 8D 10 01 F1 FF 0B 10 11 01 00 14 00 01 00 }
0x607EF: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x607F6: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x607FD: 			End  { 29 02 }
0x607FF: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x108E, VarStoreId: 0xF101, VarOffset: 0xC2F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F5 00 09 01 8E 10 01 F1 2F 0C 10 10 01 1F 01 }
0x60810: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60816: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6081C: 			End  { 29 02 }
0x6081E: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x108F, VarStoreId: 0xF101, VarOffset: 0xC4B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 12 01 26 01 8F 10 01 F1 4B 0C 10 10 01 1F 01 }
0x6082F: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60835: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6083B: 			End  { 29 02 }
0x6083D: 		End  { 29 02 }
0x6083F: 	End  { 29 02 }
0x60841: 	Form FormId: 0x28CF, Title: "Extra options " { 01 86 CF 28 9E 00 }
0x60847: 		GrayOutIf  { 19 82 }
0x60849: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x6084F: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1090, VarStoreId: 0xF101, VarOffset: 0xBDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BA 00 CD 00 90 10 01 F1 DC 0B 10 10 00 01 00 }
0x60860: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60867: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x6086E: 			End  { 29 02 }
0x60870: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1091, VarStoreId: 0xF101, VarOffset: 0xC01, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 D9 00 EC 00 91 10 01 F1 01 0C 10 11 01 00 14 00 01 00 }
0x60884: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x6088B: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60892: 			End  { 29 02 }
0x60894: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1092, VarStoreId: 0xF101, VarOffset: 0xC30, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F6 00 09 01 92 10 01 F1 30 0C 10 10 01 1F 01 }
0x608A5: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x608AB: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x608B1: 			End  { 29 02 }
0x608B3: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1093, VarStoreId: 0xF101, VarOffset: 0xC4C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 13 01 26 01 93 10 01 F1 4C 0C 10 10 01 1F 01 }
0x608C4: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x608CA: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x608D0: 			End  { 29 02 }
0x608D2: 		End  { 29 02 }
0x608D4: 	End  { 29 02 }
0x608D6: 	Form FormId: 0x28D0, Title: "Extra options " { 01 86 D0 28 9F 00 }
0x608DC: 		GrayOutIf  { 19 82 }
0x608DE: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x608E4: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1094, VarStoreId: 0xF101, VarOffset: 0xBDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BB 00 CD 00 94 10 01 F1 DD 0B 10 10 00 01 00 }
0x608F5: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x608FC: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60903: 			End  { 29 02 }
0x60905: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1095, VarStoreId: 0xF101, VarOffset: 0xC03, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 DA 00 EC 00 95 10 01 F1 03 0C 10 11 01 00 14 00 01 00 }
0x60919: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60920: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60927: 			End  { 29 02 }
0x60929: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1096, VarStoreId: 0xF101, VarOffset: 0xC31, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F7 00 09 01 96 10 01 F1 31 0C 10 10 01 1F 01 }
0x6093A: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60940: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60946: 			End  { 29 02 }
0x60948: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x1097, VarStoreId: 0xF101, VarOffset: 0xC4D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 14 01 26 01 97 10 01 F1 4D 0C 10 10 01 1F 01 }
0x60959: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6095F: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60965: 			End  { 29 02 }
0x60967: 		End  { 29 02 }
0x60969: 	End  { 29 02 }
0x6096B: 	Form FormId: 0x28D1, Title: "Extra options " { 01 86 D1 28 A0 00 }
0x60971: 		GrayOutIf  { 19 82 }
0x60973: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60979: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x1098, VarStoreId: 0xF101, VarOffset: 0xBDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BC 00 CD 00 98 10 01 F1 DE 0B 10 10 00 01 00 }
0x6098A: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60991: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60998: 			End  { 29 02 }
0x6099A: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x1099, VarStoreId: 0xF101, VarOffset: 0xC05, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 DB 00 EC 00 99 10 01 F1 05 0C 10 11 01 00 14 00 01 00 }
0x609AE: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x609B5: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x609BC: 			End  { 29 02 }
0x609BE: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x109A, VarStoreId: 0xF101, VarOffset: 0xC32, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F8 00 09 01 9A 10 01 F1 32 0C 10 10 01 1F 01 }
0x609CF: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x609D5: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x609DB: 			End  { 29 02 }
0x609DD: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x109B, VarStoreId: 0xF101, VarOffset: 0xC4E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 15 01 26 01 9B 10 01 F1 4E 0C 10 10 01 1F 01 }
0x609EE: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x609F4: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x609FA: 			End  { 29 02 }
0x609FC: 		End  { 29 02 }
0x609FE: 	End  { 29 02 }
0x60A00: 	Form FormId: 0x28D2, Title: "Extra options " { 01 86 D2 28 A1 00 }
0x60A06: 		GrayOutIf  { 19 82 }
0x60A08: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60A0E: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x109C, VarStoreId: 0xF101, VarOffset: 0xBDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BD 00 CD 00 9C 10 01 F1 DF 0B 10 10 00 01 00 }
0x60A1F: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60A26: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60A2D: 			End  { 29 02 }
0x60A2F: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x109D, VarStoreId: 0xF101, VarOffset: 0xC07, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 DC 00 EC 00 9D 10 01 F1 07 0C 10 11 01 00 14 00 01 00 }
0x60A43: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60A4A: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60A51: 			End  { 29 02 }
0x60A53: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x109E, VarStoreId: 0xF101, VarOffset: 0xC33, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 F9 00 09 01 9E 10 01 F1 33 0C 10 10 01 1F 01 }
0x60A64: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60A6A: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60A70: 			End  { 29 02 }
0x60A72: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x109F, VarStoreId: 0xF101, VarOffset: 0xC4F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 16 01 26 01 9F 10 01 F1 4F 0C 10 10 01 1F 01 }
0x60A83: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60A89: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60A8F: 			End  { 29 02 }
0x60A91: 		End  { 29 02 }
0x60A93: 	End  { 29 02 }
0x60A95: 	Form FormId: 0x28D3, Title: "Extra options " { 01 86 D3 28 A2 00 }
0x60A9B: 		GrayOutIf  { 19 82 }
0x60A9D: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60AA3: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10A0, VarStoreId: 0xF101, VarOffset: 0xBE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BE 00 CD 00 A0 10 01 F1 E0 0B 10 10 00 01 00 }
0x60AB4: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60ABB: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60AC2: 			End  { 29 02 }
0x60AC4: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10A1, VarStoreId: 0xF101, VarOffset: 0xC09, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 DD 00 EC 00 A1 10 01 F1 09 0C 10 11 01 00 14 00 01 00 }
0x60AD8: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60ADF: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60AE6: 			End  { 29 02 }
0x60AE8: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10A2, VarStoreId: 0xF101, VarOffset: 0xC34, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 FA 00 09 01 A2 10 01 F1 34 0C 10 10 01 1F 01 }
0x60AF9: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60AFF: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60B05: 			End  { 29 02 }
0x60B07: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10A3, VarStoreId: 0xF101, VarOffset: 0xC50, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 17 01 26 01 A3 10 01 F1 50 0C 10 10 01 1F 01 }
0x60B18: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60B1E: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60B24: 			End  { 29 02 }
0x60B26: 		End  { 29 02 }
0x60B28: 	End  { 29 02 }
0x60B2A: 	Form FormId: 0x28D4, Title: "Extra options " { 01 86 D4 28 A3 00 }
0x60B30: 		GrayOutIf  { 19 82 }
0x60B32: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60B38: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10A4, VarStoreId: 0xF101, VarOffset: 0xBE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 BF 00 CD 00 A4 10 01 F1 E1 0B 10 10 00 01 00 }
0x60B49: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60B50: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60B57: 			End  { 29 02 }
0x60B59: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10A5, VarStoreId: 0xF101, VarOffset: 0xC0B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 DE 00 EC 00 A5 10 01 F1 0B 0C 10 11 01 00 14 00 01 00 }
0x60B6D: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60B74: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60B7B: 			End  { 29 02 }
0x60B7D: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10A6, VarStoreId: 0xF101, VarOffset: 0xC35, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 FB 00 09 01 A6 10 01 F1 35 0C 10 10 01 1F 01 }
0x60B8E: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60B94: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60B9A: 			End  { 29 02 }
0x60B9C: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10A7, VarStoreId: 0xF101, VarOffset: 0xC51, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 18 01 26 01 A7 10 01 F1 51 0C 10 10 01 1F 01 }
0x60BAD: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60BB3: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60BB9: 			End  { 29 02 }
0x60BBB: 		End  { 29 02 }
0x60BBD: 	End  { 29 02 }
0x60BBF: 	Form FormId: 0x28D5, Title: "Extra options " { 01 86 D5 28 A4 00 }
0x60BC5: 		GrayOutIf  { 19 82 }
0x60BC7: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60BCD: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10A8, VarStoreId: 0xF101, VarOffset: 0xBE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C0 00 CD 00 A8 10 01 F1 E2 0B 10 10 00 01 00 }
0x60BDE: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60BE5: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60BEC: 			End  { 29 02 }
0x60BEE: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10A9, VarStoreId: 0xF101, VarOffset: 0xC0D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 DF 00 EC 00 A9 10 01 F1 0D 0C 10 11 01 00 14 00 01 00 }
0x60C02: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60C09: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60C10: 			End  { 29 02 }
0x60C12: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10AA, VarStoreId: 0xF101, VarOffset: 0xC36, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 FC 00 09 01 AA 10 01 F1 36 0C 10 10 01 1F 01 }
0x60C23: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60C29: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60C2F: 			End  { 29 02 }
0x60C31: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10AB, VarStoreId: 0xF101, VarOffset: 0xC52, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 19 01 26 01 AB 10 01 F1 52 0C 10 10 01 1F 01 }
0x60C42: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60C48: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60C4E: 			End  { 29 02 }
0x60C50: 		End  { 29 02 }
0x60C52: 	End  { 29 02 }
0x60C54: 	Form FormId: 0x28D6, Title: "Extra options " { 01 86 D6 28 A5 00 }
0x60C5A: 		GrayOutIf  { 19 82 }
0x60C5C: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60C62: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10AC, VarStoreId: 0xF101, VarOffset: 0xBE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C1 00 CD 00 AC 10 01 F1 E3 0B 10 10 00 01 00 }
0x60C73: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60C7A: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60C81: 			End  { 29 02 }
0x60C83: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10AD, VarStoreId: 0xF101, VarOffset: 0xC0F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E0 00 EC 00 AD 10 01 F1 0F 0C 10 11 01 00 14 00 01 00 }
0x60C97: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60C9E: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60CA5: 			End  { 29 02 }
0x60CA7: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10AE, VarStoreId: 0xF101, VarOffset: 0xC37, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 FD 00 09 01 AE 10 01 F1 37 0C 10 10 01 1F 01 }
0x60CB8: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60CBE: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60CC4: 			End  { 29 02 }
0x60CC6: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10AF, VarStoreId: 0xF101, VarOffset: 0xC53, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 1A 01 26 01 AF 10 01 F1 53 0C 10 10 01 1F 01 }
0x60CD7: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60CDD: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60CE3: 			End  { 29 02 }
0x60CE5: 		End  { 29 02 }
0x60CE7: 	End  { 29 02 }
0x60CE9: 	Form FormId: 0x28D7, Title: "Extra options " { 01 86 D7 28 A6 00 }
0x60CEF: 		GrayOutIf  { 19 82 }
0x60CF1: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60CF7: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10B0, VarStoreId: 0xF101, VarOffset: 0xBE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C2 00 CD 00 B0 10 01 F1 E4 0B 10 10 00 01 00 }
0x60D08: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60D0F: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60D16: 			End  { 29 02 }
0x60D18: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10B1, VarStoreId: 0xF101, VarOffset: 0xC11, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E1 00 EC 00 B1 10 01 F1 11 0C 10 11 01 00 14 00 01 00 }
0x60D2C: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60D33: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60D3A: 			End  { 29 02 }
0x60D3C: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10B2, VarStoreId: 0xF101, VarOffset: 0xC38, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 FE 00 09 01 B2 10 01 F1 38 0C 10 10 01 1F 01 }
0x60D4D: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60D53: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60D59: 			End  { 29 02 }
0x60D5B: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10B3, VarStoreId: 0xF101, VarOffset: 0xC54, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 1B 01 26 01 B3 10 01 F1 54 0C 10 10 01 1F 01 }
0x60D6C: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60D72: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60D78: 			End  { 29 02 }
0x60D7A: 		End  { 29 02 }
0x60D7C: 	End  { 29 02 }
0x60D7E: 	Form FormId: 0x28D8, Title: "Extra options " { 01 86 D8 28 A7 00 }
0x60D84: 		GrayOutIf  { 19 82 }
0x60D86: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60D8C: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10B4, VarStoreId: 0xF101, VarOffset: 0xBE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C3 00 CD 00 B4 10 01 F1 E5 0B 10 10 00 01 00 }
0x60D9D: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60DA4: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60DAB: 			End  { 29 02 }
0x60DAD: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10B5, VarStoreId: 0xF101, VarOffset: 0xC13, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E2 00 EC 00 B5 10 01 F1 13 0C 10 11 01 00 14 00 01 00 }
0x60DC1: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60DC8: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60DCF: 			End  { 29 02 }
0x60DD1: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10B6, VarStoreId: 0xF101, VarOffset: 0xC39, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 FF 00 09 01 B6 10 01 F1 39 0C 10 10 01 1F 01 }
0x60DE2: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60DE8: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60DEE: 			End  { 29 02 }
0x60DF0: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10B7, VarStoreId: 0xF101, VarOffset: 0xC55, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 1C 01 26 01 B7 10 01 F1 55 0C 10 10 01 1F 01 }
0x60E01: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60E07: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60E0D: 			End  { 29 02 }
0x60E0F: 		End  { 29 02 }
0x60E11: 	End  { 29 02 }
0x60E13: 	Form FormId: 0x28D9, Title: "Extra options " { 01 86 D9 28 A8 00 }
0x60E19: 		GrayOutIf  { 19 82 }
0x60E1B: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60E21: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10B8, VarStoreId: 0xF101, VarOffset: 0xBE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C4 00 CD 00 B8 10 01 F1 E6 0B 10 10 00 01 00 }
0x60E32: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60E39: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60E40: 			End  { 29 02 }
0x60E42: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10B9, VarStoreId: 0xF101, VarOffset: 0xC15, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E3 00 EC 00 B9 10 01 F1 15 0C 10 11 01 00 14 00 01 00 }
0x60E56: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60E5D: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60E64: 			End  { 29 02 }
0x60E66: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10BA, VarStoreId: 0xF101, VarOffset: 0xC3A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 00 01 09 01 BA 10 01 F1 3A 0C 10 10 01 1F 01 }
0x60E77: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60E7D: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60E83: 			End  { 29 02 }
0x60E85: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10BB, VarStoreId: 0xF101, VarOffset: 0xC56, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 1D 01 26 01 BB 10 01 F1 56 0C 10 10 01 1F 01 }
0x60E96: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60E9C: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60EA2: 			End  { 29 02 }
0x60EA4: 		End  { 29 02 }
0x60EA6: 	End  { 29 02 }
0x60EA8: 	Form FormId: 0x28DA, Title: "Extra options " { 01 86 DA 28 A9 00 }
0x60EAE: 		GrayOutIf  { 19 82 }
0x60EB0: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60EB6: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10BC, VarStoreId: 0xF101, VarOffset: 0xBE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C5 00 CD 00 BC 10 01 F1 E7 0B 10 10 00 01 00 }
0x60EC7: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60ECE: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60ED5: 			End  { 29 02 }
0x60ED7: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10BD, VarStoreId: 0xF101, VarOffset: 0xC17, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E4 00 EC 00 BD 10 01 F1 17 0C 10 11 01 00 14 00 01 00 }
0x60EEB: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60EF2: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60EF9: 			End  { 29 02 }
0x60EFB: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10BE, VarStoreId: 0xF101, VarOffset: 0xC3B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 01 01 09 01 BE 10 01 F1 3B 0C 10 10 01 1F 01 }
0x60F0C: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60F12: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60F18: 			End  { 29 02 }
0x60F1A: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10BF, VarStoreId: 0xF101, VarOffset: 0xC57, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 1E 01 26 01 BF 10 01 F1 57 0C 10 10 01 1F 01 }
0x60F2B: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60F31: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60F37: 			End  { 29 02 }
0x60F39: 		End  { 29 02 }
0x60F3B: 	End  { 29 02 }
0x60F3D: 	Form FormId: 0x28DB, Title: "Extra options " { 01 86 DB 28 AA 00 }
0x60F43: 		GrayOutIf  { 19 82 }
0x60F45: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60F4B: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10C0, VarStoreId: 0xF101, VarOffset: 0xBE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C6 00 CD 00 C0 10 01 F1 E8 0B 10 10 00 01 00 }
0x60F5C: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60F63: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60F6A: 			End  { 29 02 }
0x60F6C: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10C1, VarStoreId: 0xF101, VarOffset: 0xC19, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E5 00 EC 00 C1 10 01 F1 19 0C 10 11 01 00 14 00 01 00 }
0x60F80: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x60F87: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x60F8E: 			End  { 29 02 }
0x60F90: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10C2, VarStoreId: 0xF101, VarOffset: 0xC3C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 02 01 09 01 C2 10 01 F1 3C 0C 10 10 01 1F 01 }
0x60FA1: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60FA7: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60FAD: 			End  { 29 02 }
0x60FAF: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10C3, VarStoreId: 0xF101, VarOffset: 0xC58, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 1F 01 26 01 C3 10 01 F1 58 0C 10 10 01 1F 01 }
0x60FC0: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x60FC6: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x60FCC: 			End  { 29 02 }
0x60FCE: 		End  { 29 02 }
0x60FD0: 	End  { 29 02 }
0x60FD2: 	Form FormId: 0x28DC, Title: "Extra options " { 01 86 DC 28 AB 00 }
0x60FD8: 		GrayOutIf  { 19 82 }
0x60FDA: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x60FE0: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10C4, VarStoreId: 0xF101, VarOffset: 0xBE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C7 00 CD 00 C4 10 01 F1 E9 0B 10 10 00 01 00 }
0x60FF1: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x60FF8: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x60FFF: 			End  { 29 02 }
0x61001: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10C5, VarStoreId: 0xF101, VarOffset: 0xC1B, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E6 00 EC 00 C5 10 01 F1 1B 0C 10 11 01 00 14 00 01 00 }
0x61015: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x6101C: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x61023: 			End  { 29 02 }
0x61025: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10C6, VarStoreId: 0xF101, VarOffset: 0xC3D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 03 01 09 01 C6 10 01 F1 3D 0C 10 10 01 1F 01 }
0x61036: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6103C: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x61042: 			End  { 29 02 }
0x61044: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10C7, VarStoreId: 0xF101, VarOffset: 0xC59, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 20 01 26 01 C7 10 01 F1 59 0C 10 10 01 1F 01 }
0x61055: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6105B: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x61061: 			End  { 29 02 }
0x61063: 		End  { 29 02 }
0x61065: 	End  { 29 02 }
0x61067: 	Form FormId: 0x28DD, Title: "Extra options " { 01 86 DD 28 AC 00 }
0x6106D: 		GrayOutIf  { 19 82 }
0x6106F: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x61075: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10C8, VarStoreId: 0xF101, VarOffset: 0xBEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C8 00 CD 00 C8 10 01 F1 EA 0B 10 10 00 01 00 }
0x61086: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x6108D: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x61094: 			End  { 29 02 }
0x61096: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10C9, VarStoreId: 0xF101, VarOffset: 0xC1D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E7 00 EC 00 C9 10 01 F1 1D 0C 10 11 01 00 14 00 01 00 }
0x610AA: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x610B1: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x610B8: 			End  { 29 02 }
0x610BA: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10CA, VarStoreId: 0xF101, VarOffset: 0xC3E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 04 01 09 01 CA 10 01 F1 3E 0C 10 10 01 1F 01 }
0x610CB: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x610D1: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x610D7: 			End  { 29 02 }
0x610D9: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10CB, VarStoreId: 0xF101, VarOffset: 0xC5A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 21 01 26 01 CB 10 01 F1 5A 0C 10 10 01 1F 01 }
0x610EA: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x610F0: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x610F6: 			End  { 29 02 }
0x610F8: 		End  { 29 02 }
0x610FA: 	End  { 29 02 }
0x610FC: 	Form FormId: 0x28DE, Title: "Extra options " { 01 86 DE 28 AD 00 }
0x61102: 		GrayOutIf  { 19 82 }
0x61104: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x6110A: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10CC, VarStoreId: 0xF101, VarOffset: 0xBEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 C9 00 CD 00 CC 10 01 F1 EB 0B 10 10 00 01 00 }
0x6111B: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x61122: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x61129: 			End  { 29 02 }
0x6112B: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10CD, VarStoreId: 0xF101, VarOffset: 0xC1F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E8 00 EC 00 CD 10 01 F1 1F 0C 10 11 01 00 14 00 01 00 }
0x6113F: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x61146: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x6114D: 			End  { 29 02 }
0x6114F: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10CE, VarStoreId: 0xF101, VarOffset: 0xC3F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 05 01 09 01 CE 10 01 F1 3F 0C 10 10 01 1F 01 }
0x61160: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61166: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6116C: 			End  { 29 02 }
0x6116E: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10CF, VarStoreId: 0xF101, VarOffset: 0xC5B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 22 01 26 01 CF 10 01 F1 5B 0C 10 10 01 1F 01 }
0x6117F: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61185: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6118B: 			End  { 29 02 }
0x6118D: 		End  { 29 02 }
0x6118F: 	End  { 29 02 }
0x61191: 	Form FormId: 0x28DF, Title: "Extra options " { 01 86 DF 28 AE 00 }
0x61197: 		GrayOutIf  { 19 82 }
0x61199: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x6119F: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10D0, VarStoreId: 0xF101, VarOffset: 0xBEC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CA 00 CD 00 D0 10 01 F1 EC 0B 10 10 00 01 00 }
0x611B0: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x611B7: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x611BE: 			End  { 29 02 }
0x611C0: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10D1, VarStoreId: 0xF101, VarOffset: 0xC21, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 E9 00 EC 00 D1 10 01 F1 21 0C 10 11 01 00 14 00 01 00 }
0x611D4: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x611DB: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x611E2: 			End  { 29 02 }
0x611E4: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10D2, VarStoreId: 0xF101, VarOffset: 0xC40, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 06 01 09 01 D2 10 01 F1 40 0C 10 10 01 1F 01 }
0x611F5: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x611FB: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x61201: 			End  { 29 02 }
0x61203: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10D3, VarStoreId: 0xF101, VarOffset: 0xC5C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 23 01 26 01 D3 10 01 F1 5C 0C 10 10 01 1F 01 }
0x61214: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x6121A: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x61220: 			End  { 29 02 }
0x61222: 		End  { 29 02 }
0x61224: 	End  { 29 02 }
0x61226: 	Form FormId: 0x28E0, Title: "Extra options " { 01 86 E0 28 AF 00 }
0x6122C: 		GrayOutIf  { 19 82 }
0x6122E: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x61234: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10D4, VarStoreId: 0xF101, VarOffset: 0xBED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CB 00 CD 00 D4 10 01 F1 ED 0B 10 10 00 01 00 }
0x61245: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x6124C: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x61253: 			End  { 29 02 }
0x61255: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10D5, VarStoreId: 0xF101, VarOffset: 0xC23, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 EA 00 EC 00 D5 10 01 F1 23 0C 10 11 01 00 14 00 01 00 }
0x61269: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x61270: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x61277: 			End  { 29 02 }
0x61279: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10D6, VarStoreId: 0xF101, VarOffset: 0xC41, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 07 01 09 01 D6 10 01 F1 41 0C 10 10 01 1F 01 }
0x6128A: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61290: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x61296: 			End  { 29 02 }
0x61298: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10D7, VarStoreId: 0xF101, VarOffset: 0xC5D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 24 01 26 01 D7 10 01 F1 5D 0C 10 10 01 1F 01 }
0x612A9: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x612AF: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x612B5: 			End  { 29 02 }
0x612B7: 		End  { 29 02 }
0x612B9: 	End  { 29 02 }
0x612BB: 	Form FormId: 0x28E1, Title: "Extra options " { 01 86 E1 28 B0 00 }
0x612C1: 		GrayOutIf  { 19 82 }
0x612C3: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x612C9: 			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0x10D8, VarStoreId: 0xF101, VarOffset: 0xBEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 CC 00 CD 00 D8 10 01 F1 EE 0B 10 10 00 01 00 }
0x612DA: 				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 CF 00 30 00 00 }
0x612E1: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 CE 00 00 00 01 }
0x612E8: 			End  { 29 02 }
0x612EA: 			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0x10D9, VarStoreId: 0xF101, VarOffset: 0xC25, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1 { 07 94 EB 00 EC 00 D9 10 01 F1 25 0C 10 11 01 00 14 00 01 00 }
0x612FE: 				Default DefaultId: 0x0 Value: 10 { 5B 07 00 00 01 0A 00 }
0x61305: 				Default DefaultId: 0x1 Value: 10 { 5B 07 01 00 01 0A 00 }
0x6130C: 			End  { 29 02 }
0x6130E: 			Numeric Prompt: "Reserved Memory Alignment", Help: "Reserved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10DA, VarStoreId: 0xF101, VarOffset: 0xC42, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 08 01 09 01 DA 10 01 F1 42 0C 10 10 01 1F 01 }
0x6131F: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61325: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6132B: 			End  { 29 02 }
0x6132D: 			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0x10DB, VarStoreId: 0xF101, VarOffset: 0xC5E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1 { 07 91 25 01 26 01 DB 10 01 F1 5E 0C 10 10 01 1F 01 }
0x6133E: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61344: 				Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x6134A: 			End  { 29 02 }
0x6134C: 		End  { 29 02 }
0x6134E: 	End  { 29 02 }
0x61350: 	Form FormId: 0x28F7, Title: "PEG Port Feature Configuration" { 01 86 F7 28 87 00 }
0x61356: 		Subtitle Prompt: "PEG Port Feature Configuration", Help: "", Flags: 0x0 { 02 87 88 00 00 00 00 }
0x6135D: 		End  { 29 02 }
0x6135F: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61366: 		End  { 29 02 }
0x61368: 		OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device in PEG", QuestionFlags: 0x10, QuestionId: 0x10DC, VarStoreId: 0xF101, VarOffset: 0xC85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 89 00 8A 00 DC 10 01 F1 85 0C 10 10 00 01 00 }
0x61379: 			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault { 09 07 92 00 30 00 00 }
0x61380: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 91 00 00 00 01 }
0x61387: 		End  { 29 02 }
0x61389: 	End  { 29 02 }
0x6138B: 	Form FormId: 0x28F8, Title: "External Gfx Card Primary Display Configuration" { 01 86 F8 28 6C 00 }
0x61391: 		Subtitle Prompt: "External Gfx Card Primary Display Configuration", Help: "", Flags: 0x0 { 02 87 6D 00 00 00 00 }
0x61398: 		End  { 29 02 }
0x6139A: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x613A1: 		End  { 29 02 }
0x613A3: 		SuppressIf  { 0A 82 }
0x613A5: 			EqIdVal QuestionId: 0x676, Value: 0x0 { 12 86 76 06 00 00 }
0x613AB: 				EqIdVal QuestionId: 0x5AF, Value: 0x1 { 12 06 AF 05 01 00 }
0x613B1: 				Or  { 16 02 }
0x613B3: 				EqIdVal QuestionId: 0x2910, Value: 0x0 { 12 06 10 29 00 00 }
0x613B9: 				Or  { 16 02 }
0x613BB: 				EqIdVal QuestionId: 0x676, Value: 0x4 { 12 06 76 06 04 00 }
0x613C1: 				Or  { 16 02 }
0x613C3: 			End  { 29 02 }
0x613C5: 			OneOf Prompt: " Primary PEG", Help: "Select PEG0/PEG1/PEG2/PEG3 Graphics device should be Primary PEG.", QuestionFlags: 0x10, QuestionId: 0x10DD, VarStoreId: 0xF101, VarOffset: 0xC83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 6E 00 6F 00 DD 10 01 F1 83 0C 10 10 00 02 00 }
0x613D6: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 90 00 30 00 00 }
0x613DD: 				OneOfOption Option: "PEG11" Value: 1 { 09 07 72 00 00 00 01 }
0x613E4: 				OneOfOption Option: "PEG12" Value: 2 { 09 07 73 00 00 00 02 }
0x613EB: 			End  { 29 02 }
0x613ED: 		End  { 29 02 }
0x613EF: 		SuppressIf  { 0A 82 }
0x613F1: 			EqIdVal QuestionId: 0x676, Value: 0x0 { 12 86 76 06 00 00 }
0x613F7: 				EqIdVal QuestionId: 0x5AF, Value: 0x1 { 12 06 AF 05 01 00 }
0x613FD: 				Or  { 16 02 }
0x613FF: 				EqIdVal QuestionId: 0x2910, Value: 0x0 { 12 06 10 29 00 00 }
0x61405: 				Or  { 16 02 }
0x61407: 				EqIdVal QuestionId: 0x676, Value: 0x4 { 12 06 76 06 04 00 }
0x6140D: 				Or  { 16 02 }
0x6140F: 			End  { 29 02 }
0x61411: 			OneOf Prompt: " Primary PCIE", Help: "Select Auto/PCIE1/PCIE2/PCIE3/PCIE4/PCIE5/PCIE6/PCIE7 of D28:F0/F1/F2/F3/F4/F5/F6/F7, PCIE8/PCIE9/PCIE10/PCIE11/PCIE12/PCIE13/PCIE14/PCIE15 of D29:F0/F1/F2/F3/F4/F5/F6/F7, PCIE16/PCIE17/PCIE18/PCIE19 of D27:F0/F1/F2/F3, Graphics device should be Primary PCIE.", QuestionFlags: 0x10, QuestionId: 0x10DE, VarStoreId: 0xF101, VarOffset: 0xC84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x13, Step: 0x0 { 05 91 70 00 71 00 DE 10 01 F1 84 0C 10 10 00 13 00 }
0x61422: 				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault { 09 07 90 00 30 00 00 }
0x61429: 				OneOfOption Option: "PCIE1" Value: 1 { 09 07 74 00 00 00 01 }
0x61430: 				OneOfOption Option: "PCIE2" Value: 2 { 09 07 75 00 00 00 02 }
0x61437: 				OneOfOption Option: "PCIE3" Value: 3 { 09 07 76 00 00 00 03 }
0x6143E: 				OneOfOption Option: "PCIE4" Value: 4 { 09 07 77 00 00 00 04 }
0x61445: 				OneOfOption Option: "PCIE5" Value: 5 { 09 07 78 00 00 00 05 }
0x6144C: 				OneOfOption Option: "PCIE6" Value: 6 { 09 07 79 00 00 00 06 }
0x61453: 				OneOfOption Option: "PCIE7" Value: 7 { 09 07 7A 00 00 00 07 }
0x6145A: 				OneOfOption Option: "PCIE8" Value: 8 { 09 07 7B 00 00 00 08 }
0x61461: 				OneOfOption Option: "PCIE9" Value: 9 { 09 07 7C 00 00 00 09 }
0x61468: 				OneOfOption Option: "PCIE10" Value: 10 { 09 07 7D 00 00 00 0A }
0x6146F: 				OneOfOption Option: "PCIE11" Value: 11 { 09 07 7E 00 00 00 0B }
0x61476: 				OneOfOption Option: "PCIE12" Value: 12 { 09 07 7F 00 00 00 0C }
0x6147D: 				OneOfOption Option: "PCIE13" Value: 13 { 09 07 80 00 00 00 0D }
0x61484: 				OneOfOption Option: "PCIE14" Value: 14 { 09 07 81 00 00 00 0E }
0x6148B: 				OneOfOption Option: "PCIE15" Value: 15 { 09 07 82 00 00 00 0F }
0x61492: 				OneOfOption Option: "PCIE16" Value: 16 { 09 07 83 00 00 00 10 }
0x61499: 				OneOfOption Option: "PCIE17" Value: 17 { 09 07 84 00 00 00 11 }
0x614A0: 				OneOfOption Option: "PCIE18" Value: 18 { 09 07 85 00 00 00 12 }
0x614A7: 				OneOfOption Option: "PCIE19" Value: 19 { 09 07 86 00 00 00 13 }
0x614AE: 			End  { 29 02 }
0x614B0: 		End  { 29 02 }
0x614B2: 	End  { 29 02 }
0x614B4: 	Form FormId: 0x271A, Title: "Security" { 01 86 1A 27 3B 00 }
0x614BA: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x105E { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 BE 28 }
0x614CF: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x105F { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 BF 28 }
0x614E4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x614EB: 		End  { 29 02 }
0x614ED: 		Subtitle Prompt: "Password Description", Help: "", Flags: 0x0 { 02 87 3C 00 00 00 00 }
0x614F4: 		End  { 29 02 }
0x614F6: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x614FD: 		End  { 29 02 }
0x614FF: 		Subtitle Prompt: "If ONLY the Administrator's password is set,", Help: "", Flags: 0x0 { 02 87 3D 00 00 00 00 }
0x61506: 		End  { 29 02 }
0x61508: 		Subtitle Prompt: "then this only limits access to Setup and is", Help: "", Flags: 0x0 { 02 87 3E 00 00 00 00 }
0x6150F: 		End  { 29 02 }
0x61511: 		Subtitle Prompt: "only asked for when entering Setup.", Help: "", Flags: 0x0 { 02 87 3F 00 00 00 00 }
0x61518: 		End  { 29 02 }
0x6151A: 		Subtitle Prompt: "If ONLY the User's password is set, then this", Help: "", Flags: 0x0 { 02 87 40 00 00 00 00 }
0x61521: 		End  { 29 02 }
0x61523: 		Subtitle Prompt: "is a power on password and must be entered to", Help: "", Flags: 0x0 { 02 87 41 00 00 00 00 }
0x6152A: 		End  { 29 02 }
0x6152C: 		Subtitle Prompt: "boot or enter Setup. In Setup the User will", Help: "", Flags: 0x0 { 02 87 42 00 00 00 00 }
0x61533: 		End  { 29 02 }
0x61535: 		Subtitle Prompt: "have Administrator rights.", Help: "", Flags: 0x0 { 02 87 43 00 00 00 00 }
0x6153C: 		End  { 29 02 }
0x6153E: 		Subtitle Prompt: "The password length must be", Help: "", Flags: 0x0 { 02 87 44 00 00 00 00 }
0x61545: 		End  { 29 02 }
0x61547: 		Subtitle Prompt: "in the following range:", Help: "", Flags: 0x0 { 02 87 45 00 00 00 00 }
0x6154E: 		End  { 29 02 }
0x61550: 		Text Prompt: "Minimum length", Help: "", Text: "N/A" { 03 08 46 00 02 00 47 00 }
0x61558: 		Text Prompt: "Maximum length", Help: "", Text: "N/A" { 03 08 48 00 02 00 49 00 }
0x61560: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61567: 		End  { 29 02 }
0x61569: 		GrayOutIf  { 19 82 }
0x6156B: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 06 0A 11 01 00 }
0x61571: 			Password Prompt: "Administrator Password", Help: "Set Administrator Password", QuestionFlags: 0x0, QuestionId: 0x10DF, VarStoreId: 0xF013, VarStoreInfo: 0x28, MinSize: 0x3, MaxSize: 0x14 { 08 91 4A 00 4B 00 DF 10 13 F0 28 00 00 03 00 14 00 }
0x61582: 			End  { 29 02 }
0x61584: 		End  { 29 02 }
0x61586: 		Password Prompt: "User Password", Help: "Set User Password", QuestionFlags: 0x0, QuestionId: 0x10E0, VarStoreId: 0xF013, VarStoreInfo: 0x0, MinSize: 0x3, MaxSize: 0x14 { 08 91 4C 00 4D 00 E0 10 13 F0 00 00 00 03 00 14 00 }
0x61597: 		End  { 29 02 }
0x61599: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x615A0: 		End  { 29 02 }
0x615A2: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x1138 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 D0 2A }
0x615B7: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x1138 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 D0 2A }
0x615CC: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x615D3: 		End  { 29 02 }
0x615D5: 		Ref Prompt: "Secure Boot", Help: "Secure Boot configuration", QuestionFlags: 0x4, QuestionId: 0x29D5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29D6 { 0F 0F 15 22 16 22 D5 29 00 00 FF FF 04 D6 29 }
0x615E4: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x615EB: 		End  { 29 02 }
0x615ED: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x1136 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 CE 2A }
0x61602: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x1137 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 CF 2A }
0x61617: 	End  { 29 02 }
0x61619: 	Form FormId: 0x29D6, Title: "Secure Boot" { 01 86 D6 29 15 22 }
0x6161F: 		SuppressIf  { 0A 82 }
0x61621: 			EqIdVal QuestionId: 0x110D, Value: 0x1 { 12 86 0D 11 01 00 }
0x61627: 				Not  { 17 02 }
0x61629: 			End  { 29 02 }
0x6162B: 			Text Prompt: "System Mode", Help: "", Text: "Deployed" { 03 08 17 22 02 00 1A 22 }
0x61633: 		End  { 29 02 }
0x61635: 		SuppressIf  { 0A 82 }
0x61637: 			EqIdVal QuestionId: 0x110C, Value: 0x1 { 12 86 0C 11 01 00 }
0x6163D: 				Not  { 17 02 }
0x6163F: 			End  { 29 02 }
0x61641: 			Text Prompt: "System Mode", Help: "", Text: "Audit" { 03 08 17 22 02 00 19 22 }
0x61649: 		End  { 29 02 }
0x6164B: 		SuppressIf  { 0A 82 }
0x6164D: 			EqIdVal QuestionId: 0x110D, Value: 0x1 { 12 86 0D 11 01 00 }
0x61653: 				EqIdVal QuestionId: 0x110C, Value: 0x1 { 12 06 0C 11 01 00 }
0x61659: 				Or  { 16 02 }
0x6165B: 				EqIdVal QuestionId: 0x110B, Value: 0x0 { 12 06 0B 11 00 00 }
0x61661: 				Or  { 16 02 }
0x61663: 			End  { 29 02 }
0x61665: 			Text Prompt: "System Mode", Help: "", Text: "Setup" { 03 08 17 22 02 00 07 00 }
0x6166D: 		End  { 29 02 }
0x6166F: 		SuppressIf  { 0A 82 }
0x61671: 			EqIdVal QuestionId: 0x110D, Value: 0x1 { 12 86 0D 11 01 00 }
0x61677: 				EqIdVal QuestionId: 0x110C, Value: 0x1 { 12 06 0C 11 01 00 }
0x6167D: 				Or  { 16 02 }
0x6167F: 				EqIdVal QuestionId: 0x110B, Value: 0x1 { 12 06 0B 11 01 00 }
0x61685: 				Or  { 16 02 }
0x61687: 			End  { 29 02 }
0x61689: 			Text Prompt: "System Mode", Help: "", Text: "User" { 03 08 17 22 02 00 18 22 }
0x61691: 		End  { 29 02 }
0x61693: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x6169A: 		End  { 29 02 }
0x6169C: 		GrayOutIf  { 19 82 }
0x6169E: 			EqIdVal QuestionId: 0x110A, Value: 0x1 { 12 86 0A 11 01 00 }
0x616A4: 				EqIdVal QuestionId: 0x1109, Value: 0x0 { 12 06 09 11 00 00 }
0x616AA: 				Or  { 16 02 }
0x616AC: 			End  { 29 02 }
0x616AE: 			OneOf Prompt: "Secure Boot", Help: "Secure Boot feature is Active if Secure Boot is Enabled,
Platform Key(PK) is enrolled and the System is in User mode.
The mode change requires platform reset", QuestionFlags: 0x14, QuestionId: 0x29D7, VarStoreId: 0x1B, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 1D 22 1E 22 D7 29 1B 00 00 00 14 10 00 01 00 }
0x616BF: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x616C5: 				OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x616CC: 				OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x616D3: 			End  { 29 02 }
0x616D5: 			SuppressIf  { 0A 82 }
0x616D7: 				EqIdVal QuestionId: 0x1108, Value: 0x0 { 12 86 08 11 00 00 }
0x616DD: 					Not  { 17 02 }
0x616DF: 				End  { 29 02 }
0x616E1: 				Text Prompt: "", Help: "", Text: "Not Active" { 03 08 02 00 02 00 20 22 }
0x616E9: 			End  { 29 02 }
0x616EB: 			SuppressIf  { 0A 82 }
0x616ED: 				EqIdVal QuestionId: 0x1108, Value: 0x1 { 12 86 08 11 01 00 }
0x616F3: 					Not  { 17 02 }
0x616F5: 				End  { 29 02 }
0x616F7: 				Text Prompt: "", Help: "", Text: "Active" { 03 08 02 00 02 00 1F 22 }
0x616FF: 			End  { 29 02 }
0x61701: 			Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61708: 			End  { 29 02 }
0x6170A: 			OneOf Prompt: "Secure Boot Mode", Help: "Secure Boot mode options:
Standard or Custom.
In Custom mode, Secure Boot Policy variables can be configured by a physically present user without full authentication", QuestionFlags: 0x14, QuestionId: 0x29D8, VarStoreId: 0x1B, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 21 22 22 22 D8 29 1B 00 01 00 14 10 00 01 00 }
0x6171B: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61721: 				OneOfOption Option: "Standard" Value: 0, MfgDefault { 09 07 23 22 20 00 00 }
0x61728: 				OneOfOption Option: "Custom" Value: 1 { 09 07 24 22 00 00 01 }
0x6172F: 			End  { 29 02 }
0x61731: 			GrayOutIf  { 19 82 }
0x61733: 				EqIdVal QuestionId: 0x29D8, Value: 0x0 { 12 06 D8 29 00 00 }
0x61739: 				Ref Prompt: "Restore Factory Keys", Help: "Force System to User Mode.
Install factory default Secure Boot key databases", QuestionFlags: 0x14, QuestionId: 0x29D9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29D6 { 0F 0F 2C 22 2D 22 D9 29 00 00 FF FF 14 D6 29 }
0x61748: 				GrayOutIf  { 19 82 }
0x6174A: 					EqIdVal QuestionId: 0x1106, Value: 0x0 { 12 06 06 11 00 00 }
0x61750: 					Ref Prompt: "Reset To Setup Mode", Help: "Delete all Secure Boot key databases from NVRAM", QuestionFlags: 0x14, QuestionId: 0x29DA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29D6 { 0F 0F 2A 22 2B 22 DA 29 00 00 FF FF 14 D6 29 }
0x6175F: 				End  { 29 02 }
0x61761: 				Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61768: 				End  { 29 02 }
0x6176A: 				Ref Prompt: "Key Management", Help: "Enables expert users to modify Secure Boot Policy variables without variable authentication", QuestionFlags: 0x4, QuestionId: 0x29DE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 3B 22 3C 22 DE 29 00 00 FF FF 04 DF 29 }
0x61779: 			End  { 29 02 }
0x6177B: 		End  { 29 02 }
0x6177D: 	End  { 29 02 }
0x6177F: 	Form FormId: 0x29DF, Title: "Key Management" { 01 86 DF 29 3B 22 }
0x61785: 		SuppressIf  { 0A 82 }
0x61787: 			EqIdVal QuestionId: 0x1107, Value: 0x1 { 12 86 07 11 01 00 }
0x6178D: 				Not  { 17 02 }
0x6178F: 			End  { 29 02 }
0x61791: 			Text Prompt: "Vendor Keys", Help: "", Text: "Valid" { 03 08 1B 22 02 00 90 03 }
0x61799: 		End  { 29 02 }
0x6179B: 		SuppressIf  { 0A 82 }
0x6179D: 			EqIdVal QuestionId: 0x1107, Value: 0x0 { 12 86 07 11 00 00 }
0x617A3: 				Not  { 17 02 }
0x617A5: 			End  { 29 02 }
0x617A7: 			Text Prompt: "Vendor Keys", Help: "", Text: "Modified" { 03 08 1B 22 02 00 1C 22 }
0x617AF: 		End  { 29 02 }
0x617B1: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x617B8: 		End  { 29 02 }
0x617BA: 		OneOf Prompt: "Factory Key Provision", Help: "Install factory default Secure Boot keys after the platform reset and while the System is in Setup mode", QuestionFlags: 0x14, QuestionId: 0x29E0, VarStoreId: 0x1B, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3D 22 3E 22 E0 29 1B 00 02 00 14 10 00 01 00 }
0x617CB: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x617D1: 			OneOfOption Option: "Disabled" Value: 0 { 09 07 04 00 00 00 00 }
0x617D8: 			OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 03 00 20 00 01 }
0x617DF: 		End  { 29 02 }
0x617E1: 		Ref Prompt: "Restore Factory Keys", Help: "Force System to User Mode.
Install factory default Secure Boot key databases", QuestionFlags: 0x14, QuestionId: 0x29E1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 2C 22 2D 22 E1 29 00 00 FF FF 14 DF 29 }
0x617F0: 		GrayOutIf  { 19 82 }
0x617F2: 			EqIdVal QuestionId: 0x1106, Value: 0x0 { 12 06 06 11 00 00 }
0x617F8: 			Ref Prompt: "Reset To Setup Mode", Help: "Delete all Secure Boot key databases from NVRAM", QuestionFlags: 0x14, QuestionId: 0x29E2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 2A 22 2B 22 E2 29 00 00 FF FF 14 DF 29 }
0x61807: 		End  { 29 02 }
0x61809: 		Ref Prompt: "Enroll Efi Image", Help: "Allow Efi image to run in Secure Boot mode.
Enroll SHA256 Hash certificate of a PE image into Authorized Signature Database (db)", QuestionFlags: 0x4, QuestionId: 0x29E3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 4B 22 4C 22 E3 29 00 00 FF FF 04 DF 29 }
0x61818: 		GrayOutIf  { 19 82 }
0x6181A: 			EqIdVal QuestionId: 0x1106, Value: 0x0 { 12 86 06 11 00 00 }
0x61820: 				EqIdVal QuestionId: 0x1105, Value: 0x0 { 12 06 05 11 00 00 }
0x61826: 				And  { 15 02 }
0x61828: 				EqIdVal QuestionId: 0x1104, Value: 0x0 { 12 06 04 11 00 00 }
0x6182E: 				And  { 15 02 }
0x61830: 				EqIdVal QuestionId: 0x1103, Value: 0x0 { 12 06 03 11 00 00 }
0x61836: 				And  { 15 02 }
0x61838: 				EqIdVal QuestionId: 0x1102, Value: 0x0 { 12 06 02 11 00 00 }
0x6183E: 				And  { 15 02 }
0x61840: 				EqIdVal QuestionId: 0x1101, Value: 0x0 { 12 06 01 11 00 00 }
0x61846: 				And  { 15 02 }
0x61848: 			End  { 29 02 }
0x6184A: 			Ref Prompt: "Export Secure Boot variables", Help: "Save NVRAM content of Secure Boot variable to a file", QuestionFlags: 0x4, QuestionId: 0x29E4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 49 22 4A 22 E4 29 00 00 FF FF 04 DF 29 }
0x61859: 		End  { 29 02 }
0x6185B: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61862: 		End  { 29 02 }
0x61864: 		Subtitle Prompt: "Secure Boot variable      | Size| Keys| Key Source", Help: "", Flags: 0x0 { 02 87 55 22 00 00 00 }
0x6186B: 		End  { 29 02 }
0x6186D: 		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHAXXX
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,Modified,Mixed", QuestionFlags: 0x14, QuestionId: 0x29E5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 56 22 54 22 E5 29 00 00 FF FF 14 DF 29 }
0x6187C: 		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHAXXX
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,Modified,Mixed", QuestionFlags: 0x4, QuestionId: 0x29E6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 58 22 54 22 E6 29 00 00 FF FF 04 DF 29 }
0x6188B: 		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHAXXX
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,Modified,Mixed", QuestionFlags: 0x4, QuestionId: 0x29E7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 5A 22 54 22 E7 29 00 00 FF FF 04 DF 29 }
0x6189A: 		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHAXXX
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,Modified,Mixed", QuestionFlags: 0x4, QuestionId: 0x29E8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 5C 22 54 22 E8 29 00 00 FF FF 04 DF 29 }
0x618A9: 		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHAXXX
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,Modified,Mixed", QuestionFlags: 0x4, QuestionId: 0x29E9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 5E 22 54 22 E9 29 00 00 FF FF 04 DF 29 }
0x618B8: 		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHAXXX
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,Modified,Mixed", QuestionFlags: 0x4, QuestionId: 0x29EA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x29DF { 0F 0F 60 22 54 22 EA 29 00 00 FF FF 04 DF 29 }
0x618C7: 	End  { 29 02 }
0x618C9: 	Form FormId: 0x2AD4, Title: "TCG Storage device Security Configuration" { 01 86 D4 2A E4 22 }
0x618CF: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x1134 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 CC 2A }
0x618E4: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x1135 { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 CD 2A }
0x618F9: 	End  { 29 02 }
0x618FB: 	Form FormId: 0x2AD5, Title: "TCG Storage device Security Configuration" { 01 86 D5 2A E4 22 }
0x61901: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x113A { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 D2 2A }
0x61916: 		Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Label, LabelNumber: 0x113B { 5F 15 35 17 0B 0F A0 87 93 41 B2 66 53 8C 38 AF 48 CE 00 D3 2A }
0x6192B: 	End  { 29 02 }
0x6192D: 	Form FormId: 0x271B, Title: "Boot" { 01 86 1B 27 20 00 }
0x61933: 		Subtitle Prompt: "Boot Configuration", Help: "", Flags: 0x0 { 02 87 25 00 00 00 00 }
0x6193A: 		End  { 29 02 }
0x6193C: 		Numeric Prompt: "Setup Prompt Timeout", Help: "Number of seconds to wait for setup activation key. 65535(0xFFFF) means indefinite waiting.", QuestionFlags: 0x0, QuestionId: 0x10E1, VarStoreId: 0xF005, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1 { 07 94 26 00 27 00 E1 10 05 F0 00 00 00 11 01 00 FF FF 01 00 }
0x61950: 			Default DefaultId: 0x0 Value: 1 { 5B 07 00 00 01 01 00 }
0x61957: 			Default DefaultId: 0x1 Value: 1 { 5B 07 01 00 01 01 00 }
0x6195E: 		End  { 29 02 }
0x61960: 		OneOf Prompt: "Bootup NumLock State", Help: "Select the keyboard NumLock state", QuestionFlags: 0x10, QuestionId: 0x10E2, VarStoreId: 0xF101, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 28 00 29 00 E2 10 01 F1 00 00 10 10 00 01 00 }
0x61971: 			OneOfOption Option: "On" Value: 1 { 09 07 2A 00 00 00 01 }
0x61978: 			OneOfOption Option: "Off" Value: 0 { 09 07 2B 00 00 00 00 }
0x6197F: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x61985: 			Default DefaultId: 0x1 Value: 0 { 5B 06 01 00 00 00 }
0x6198B: 		End  { 29 02 }
0x6198D: 		CheckBox Prompt: "Quiet Boot", Help: "Enables or disables Quiet Boot option", QuestionFlags: 0x0, QuestionId: 0x10E3, VarStoreId: 0xF013, VarOffset: 0x50, Flags: 0x0, Default: Disabled, MfgDefault: Disabled { 06 8E 21 00 22 00 E3 10 13 F0 50 00 00 00 }
0x6199B: 			Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x619A1: 			Default DefaultId: 0x1 Value: 1 { 5B 06 01 00 00 01 }
0x619A7: 		End  { 29 02 }
0x619A9: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x619B0: 		End  { 29 02 }
0x619B2: 		Subtitle Prompt: "Boot Option Priorities", Help: "", Flags: 0x0 { 02 87 2C 00 00 00 00 }
0x619B9: 		End  { 29 02 }
0x619BB: 		SuppressIf  { 0A 82 }
0x619BD: 			EqIdValList QuestionId: 0x1100, Values: [65535] { 14 08 00 11 01 00 FF FF }
0x619C5: 			OneOf Prompt: "Boot Option #%d", Help: "Sets the system boot order", QuestionFlags: 0x0, QuestionId: 0x10E4, VarStoreId: 0xF006, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0 { 05 94 2D 00 2F 00 E4 10 06 F0 00 00 00 11 00 00 01 00 00 00 }
0x619D9: 				OneOfOption Option: "" Value: 0 { 09 08 02 00 01 01 00 00 }
0x619E1: 				OneOfOption Option: "" Value: 1 { 09 08 02 00 01 01 01 00 }
0x619E9: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x619F0: 				Default DefaultId: 0x1 Value: 0 { 5B 07 01 00 01 00 00 }
0x619F7: 			End  { 29 02 }
0x619F9: 		End  { 29 02 }
0x619FB: 		OneOf Prompt: "Fast Boot", Help: "Enables or disables boot with initialization of a minimal set of devices required to launch active boot option. Has no effect for BBS boot options.", QuestionFlags: 0x10, QuestionId: 0x10E5, VarStoreId: 0xF101, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 23 00 24 00 E5 10 01 F1 02 00 10 10 00 01 00 }
0x61A0C: 			Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x61A12: 			OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 85 1B 20 00 00 }
0x61A19: 			OneOfOption Option: "Enabled" Value: 1 { 09 07 4E 20 00 00 01 }
0x61A20: 		End  { 29 02 }
0x61A22: 		SuppressIf  { 0A 82 }
0x61A24: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61A2A: 			GrayOutIf  { 19 82 }
0x61A2C: 				EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61A32: 				OneOf Prompt: " SATA Support", Help: "If Last Boot SATA Devices Only, Only last boot SATA device will be available in Post. If All SATA Devices, all SATA devices will be available in OS and Post.", QuestionFlags: 0x10, QuestionId: 0x10E6, VarStoreId: 0xF101, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 3E 20 3F 20 E6 10 01 F1 03 00 10 10 00 01 00 }
0x61A43: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x61A49: 					OneOfOption Option: "Last Boot SATA Devices Only" Value: 0 { 09 07 54 20 00 00 00 }
0x61A50: 					OneOfOption Option: "All SATA Devices" Value: 1, MfgDefault { 09 07 53 20 20 00 01 }
0x61A57: 				End  { 29 02 }
0x61A59: 			End  { 29 02 }
0x61A5B: 		End  { 29 02 }
0x61A5D: 		SuppressIf  { 0A 82 }
0x61A5F: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61A65: 			GrayOutIf  { 19 82 }
0x61A67: 				EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61A6D: 				OneOf Prompt: " NVMe Support", Help: "If Disabled, NVMe device will be skipped.", QuestionFlags: 0x10, QuestionId: 0x10E7, VarStoreId: 0xF101, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4A 20 4B 20 E7 10 01 F1 0A 00 10 10 00 01 00 }
0x61A7E: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61A84: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x61A8B: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 4E 20 20 00 01 }
0x61A92: 				End  { 29 02 }
0x61A94: 			End  { 29 02 }
0x61A96: 		End  { 29 02 }
0x61A98: 		SuppressIf  { 0A 82 }
0x61A9A: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61AA0: 			GrayOutIf  { 19 82 }
0x61AA2: 				EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61AA8: 				OneOf Prompt: " UFS Support", Help: "If Disabled, UFS device will be skipped.", QuestionFlags: 0x10, QuestionId: 0x10E8, VarStoreId: 0xF101, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 4C 20 4D 20 E8 10 01 F1 0B 00 10 10 00 01 00 }
0x61AB9: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61ABF: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x61AC6: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 4E 20 20 00 01 }
0x61ACD: 				End  { 29 02 }
0x61ACF: 			End  { 29 02 }
0x61AD1: 		End  { 29 02 }
0x61AD3: 		SuppressIf  { 0A 82 }
0x61AD5: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61ADB: 			OneOf Prompt: " VGA Support", Help: "If Auto, only install Legacy OpRom with Legacy OS and logo would NOT be shown during post. Efi driver will still be installed with EFI OS.", QuestionFlags: 0x10, QuestionId: 0x10E9, VarStoreId: 0xF101, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 46 20 47 20 E9 10 01 F1 04 00 10 10 00 01 00 }
0x61AEC: 				Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61AF2: 				OneOfOption Option: "Auto" Value: 0 { 09 07 06 00 00 00 00 }
0x61AF9: 				OneOfOption Option: "EFI Driver" Value: 1, MfgDefault { 09 07 51 20 20 00 01 }
0x61B00: 			End  { 29 02 }
0x61B02: 		End  { 29 02 }
0x61B04: 		SuppressIf  { 0A 82 }
0x61B06: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61B0C: 			GrayOutIf  { 19 82 }
0x61B0E: 				EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61B14: 				OneOf Prompt: " USB Support", Help: "If Disabled, all USB devices will NOT be available until after OS boot. If Partial Initial, USB Mass Storage and specific USB port/device will NOT be available before OS boot. If Enabled, all USB devices will be available in OS and Post.", QuestionFlags: 0x10, QuestionId: 0x10EA, VarStoreId: 0xF101, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0 { 05 91 40 20 41 20 EA 10 01 F1 05 00 10 10 00 02 00 }
0x61B25: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61B2B: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x61B32: 					OneOfOption Option: "Full Initial" Value: 1, MfgDefault { 09 07 4F 20 20 00 01 }
0x61B39: 					OneOfOption Option: "Partial Initial" Value: 2 { 09 07 50 20 00 00 02 }
0x61B40: 				End  { 29 02 }
0x61B42: 			End  { 29 02 }
0x61B44: 		End  { 29 02 }
0x61B46: 		SuppressIf  { 0A 82 }
0x61B48: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61B4E: 			GrayOutIf  { 19 82 }
0x61B50: 				EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61B56: 				OneOf Prompt: " PS2 Devices Support", Help: "If Disabled, PS2 devices will be skipped.", QuestionFlags: 0x10, QuestionId: 0x10EB, VarStoreId: 0xF101, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 42 20 43 20 EB 10 01 F1 06 00 10 10 00 01 00 }
0x61B67: 					Default DefaultId: 0x0 Value: 1 { 5B 06 00 00 00 01 }
0x61B6D: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x61B74: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 4E 20 20 00 01 }
0x61B7B: 				End  { 29 02 }
0x61B7D: 			End  { 29 02 }
0x61B7F: 		End  { 29 02 }
0x61B81: 		SuppressIf  { 0A 82 }
0x61B83: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61B89: 			GrayOutIf  { 19 82 }
0x61B8B: 				EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61B91: 				OneOf Prompt: " Network Stack Driver Support", Help: "If Disabled, NetWork Stack Driver will be skipped.", QuestionFlags: 0x10, QuestionId: 0x10EC, VarStoreId: 0xF101, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 48 20 49 20 EC 10 01 F1 09 00 10 10 00 01 00 }
0x61BA2: 					Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x61BA8: 					OneOfOption Option: "Disabled" Value: 0 { 09 07 85 1B 00 00 00 }
0x61BAF: 					OneOfOption Option: "Enabled" Value: 1, MfgDefault { 09 07 4E 20 20 00 01 }
0x61BB6: 				End  { 29 02 }
0x61BB8: 			End  { 29 02 }
0x61BBA: 		End  { 29 02 }
0x61BBC: 		SuppressIf  { 0A 82 }
0x61BBE: 			EqIdVal QuestionId: 0x10E5, Value: 0x0 { 12 06 E5 10 00 00 }
0x61BC4: 			OneOf Prompt: "Redirection Support", Help: "If disable, Redirection function will be disabled.", QuestionFlags: 0x10, QuestionId: 0x10ED, VarStoreId: 0xF101, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0 { 05 91 55 20 56 20 ED 10 01 F1 08 00 10 10 00 01 00 }
0x61BD5: 				Default DefaultId: 0x0 Value: 0 { 5B 06 00 00 00 00 }
0x61BDB: 				OneOfOption Option: "Disabled" Value: 0, MfgDefault { 09 07 85 1B 20 00 00 }
0x61BE2: 				OneOfOption Option: "Enabled" Value: 1 { 09 07 4E 20 00 00 01 }
0x61BE9: 			End  { 29 02 }
0x61BEB: 		End  { 29 02 }
0x61BED: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61BF4: 		End  { 29 02 }
0x61BF6: 		SuppressIf  { 0A 82 }
0x61BF8: 			EqIdValList QuestionId: 0x10FF, Values: [0] { 14 08 FF 10 01 00 00 00 }
0x61C00: 			Subtitle Prompt: "Driver Option Priorities", Help: "", Flags: 0x0 { 02 87 F9 1F 00 00 00 }
0x61C07: 			End  { 29 02 }
0x61C09: 		End  { 29 02 }
0x61C0B: 		SuppressIf  { 0A 82 }
0x61C0D: 			EqIdValList QuestionId: 0x10FF, Values: [65535] { 14 08 FF 10 01 00 FF FF }
0x61C15: 			OneOf Prompt: "Driver Option #%d", Help: "Sets the system driver order", QuestionFlags: 0x0, QuestionId: 0x10EE, VarStoreId: 0x13, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0 { 05 94 FA 1F FB 1F EE 10 13 00 00 00 00 11 00 00 01 00 00 00 }
0x61C29: 				OneOfOption Option: "" Value: 0, Default, MfgDefault { 09 08 02 00 31 01 00 00 }
0x61C31: 				OneOfOption Option: "" Value: 1 { 09 08 02 00 01 01 01 00 }
0x61C39: 			End  { 29 02 }
0x61C3B: 		End  { 29 02 }
0x61C3D: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61C44: 		End  { 29 02 }
0x61C46: 		SuppressIf  { 0A 82 }
0x61C48: 			EqIdValList QuestionId: 0x10FE, Values: [65535] { 14 08 FE 10 01 00 FF FF }
0x61C50: 			Ref Prompt: "", Help: "Set the order of the legacy devices in this group", QuestionFlags: 0x0, QuestionId: 0x10EF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28C0 { 0F 0F 02 00 35 00 EF 10 00 00 FF FF 00 C0 28 }
0x61C5F: 		End  { 29 02 }
0x61C61: 	End  { 29 02 }
0x61C63: 	Form FormId: 0x28C0, Title: "Boot" { 01 86 C0 28 20 00 }
0x61C69: 		SuppressIf  { 0A 82 }
0x61C6B: 			EqIdValList QuestionId: 0x10FD, Values: [65535] { 14 08 FD 10 01 00 FF FF }
0x61C73: 			OneOf Prompt: "Boot Option #%d", Help: "Sets the system boot order", QuestionFlags: 0x0, QuestionId: 0x10F0, VarStoreId: 0xF008, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0 { 05 94 2E 00 2F 00 F0 10 08 F0 00 00 00 11 00 00 01 00 00 00 }
0x61C87: 				OneOfOption Option: "" Value: 0 { 09 08 02 00 01 01 00 00 }
0x61C8F: 				OneOfOption Option: "" Value: 1 { 09 08 02 00 01 01 01 00 }
0x61C97: 				Default DefaultId: 0x0 Value: 0 { 5B 07 00 00 01 00 00 }
0x61C9E: 				Default DefaultId: 0x1 Value: 0 { 5B 07 01 00 01 00 00 }
0x61CA5: 			End  { 29 02 }
0x61CA7: 		End  { 29 02 }
0x61CA9: 	End  { 29 02 }
0x61CAB: 	Form FormId: 0x271C, Title: "Save & Exit" { 01 86 1C 27 4E 00 }
0x61CB1: 		Subtitle Prompt: "Save Options", Help: "", Flags: 0x0 { 02 87 57 00 00 00 00 }
0x61CB8: 		End  { 29 02 }
0x61CBA: 		SuppressIf  { 0A 82 }
0x61CBC: 			EqIdVal QuestionId: 0x10FC, Value: 0x1 { 12 06 FC 10 01 00 }
0x61CC2: 			Ref Prompt: "Save Changes and Exit", Help: "Exit system setup after saving the changes.", QuestionFlags: 0x0, QuestionId: 0x10F1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 4F 00 50 00 F1 10 00 00 FF FF 00 1C 27 }
0x61CD1: 		End  { 29 02 }
0x61CD3: 		SuppressIf  { 0A 82 }
0x61CD5: 			EqIdVal QuestionId: 0x10FC, Value: 0x2 { 12 06 FC 10 02 00 }
0x61CDB: 			Ref Prompt: "Discard Changes and Exit", Help: "Exit system setup without saving any changes.", QuestionFlags: 0x0, QuestionId: 0x10F2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 51 00 52 00 F2 10 00 00 FF FF 00 1C 27 }
0x61CEA: 		End  { 29 02 }
0x61CEC: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61CF3: 		End  { 29 02 }
0x61CF5: 		SuppressIf  { 0A 82 }
0x61CF7: 			EqIdVal QuestionId: 0x10FC, Value: 0x9 { 12 06 FC 10 09 00 }
0x61CFD: 			Ref Prompt: "Save Changes and Reset", Help: "Reset the system after saving the changes.", QuestionFlags: 0x0, QuestionId: 0x10F3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 53 00 54 00 F3 10 00 00 FF FF 00 1C 27 }
0x61D0C: 		End  { 29 02 }
0x61D0E: 		SuppressIf  { 0A 82 }
0x61D10: 			EqIdVal QuestionId: 0x10FC, Value: 0xA { 12 06 FC 10 0A 00 }
0x61D16: 			Ref Prompt: "Discard Changes and Reset", Help: "Reset system setup without saving any changes.", QuestionFlags: 0x0, QuestionId: 0x10F4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 55 00 56 00 F4 10 00 00 FF FF 00 1C 27 }
0x61D25: 		End  { 29 02 }
0x61D27: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61D2E: 		End  { 29 02 }
0x61D30: 		SuppressIf  { 0A 82 }
0x61D32: 			EqIdVal QuestionId: 0x10FC, Value: 0x3 { 12 06 FC 10 03 00 }
0x61D38: 			Ref Prompt: "Save Changes", Help: "Save Changes done so far to any of the setup options.", QuestionFlags: 0x0, QuestionId: 0x10F5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 58 00 59 00 F5 10 00 00 FF FF 00 1C 27 }
0x61D47: 		End  { 29 02 }
0x61D49: 		SuppressIf  { 0A 82 }
0x61D4B: 			EqIdVal QuestionId: 0x10FC, Value: 0x4 { 12 06 FC 10 04 00 }
0x61D51: 			Ref Prompt: "Discard Changes", Help: "Discard Changes done so far to any of the setup options.", QuestionFlags: 0x0, QuestionId: 0x10F6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 5A 00 5B 00 F6 10 00 00 FF FF 00 1C 27 }
0x61D60: 		End  { 29 02 }
0x61D62: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61D69: 		End  { 29 02 }
0x61D6B: 		Subtitle Prompt: "Default Options", Help: "", Flags: 0x0 { 02 87 5C 00 00 00 00 }
0x61D72: 		End  { 29 02 }
0x61D74: 		SuppressIf  { 0A 82 }
0x61D76: 			EqIdVal QuestionId: 0x10FC, Value: 0x5 { 12 06 FC 10 05 00 }
0x61D7C: 			Ref Prompt: "Restore Defaults", Help: "Restore/Load Default values for all the setup options.", QuestionFlags: 0x0, QuestionId: 0x10F7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 5D 00 5E 00 F7 10 00 00 FF FF 00 1C 27 }
0x61D8B: 		End  { 29 02 }
0x61D8D: 		SuppressIf  { 0A 82 }
0x61D8F: 			EqIdVal QuestionId: 0x10FC, Value: 0x6 { 12 06 FC 10 06 00 }
0x61D95: 			Ref Prompt: "Save as User Defaults", Help: "Save the changes done so far as User Defaults.", QuestionFlags: 0x0, QuestionId: 0x10F8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 5F 00 60 00 F8 10 00 00 FF FF 00 1C 27 }
0x61DA4: 		End  { 29 02 }
0x61DA6: 		SuppressIf  { 0A 82 }
0x61DA8: 			EqIdVal QuestionId: 0x10FC, Value: 0x7 { 12 06 FC 10 07 00 }
0x61DAE: 			Ref Prompt: "Restore User Defaults", Help: "Restore the User Defaults to all the setup options.", QuestionFlags: 0x0, QuestionId: 0x10F9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 61 00 62 00 F9 10 00 00 FF FF 00 1C 27 }
0x61DBD: 		End  { 29 02 }
0x61DBF: 		Subtitle Prompt: "", Help: "", Flags: 0x0 { 02 87 02 00 00 00 00 }
0x61DC6: 		End  { 29 02 }
0x61DC8: 		Subtitle Prompt: "Boot Override", Help: "", Flags: 0x0 { 02 87 63 00 00 00 00 }
0x61DCF: 		End  { 29 02 }
0x61DD1: 		SuppressIf  { 0A 82 }
0x61DD3: 			EqIdValList QuestionId: 0x10FB, Values: [65535] { 14 08 FB 10 01 00 FF FF }
0x61DDB: 			Ref Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x10FA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x271C { 0F 0F 02 00 02 00 FA 10 00 00 FF FF 00 1C 27 }
0x61DEA: 		End  { 29 02 }
0x61DEC: 		DisableIf  { 1E 82 }
0x61DEE: 			True  { 46 02 }
0x61DF0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x10FB, VarStoreId: 0xF014, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 FB 10 14 F0 00 00 00 11 00 00 FF FF 00 00 }
0x61E04: 			End  { 29 02 }
0x61E06: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x10FC, VarStoreId: 0xF002, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 FC 10 02 F0 00 00 00 11 00 00 FF FF 00 00 }
0x61E1A: 			End  { 29 02 }
0x61E1C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x10FD, VarStoreId: 0xF016, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 FD 10 16 F0 00 00 00 11 00 00 FF FF 00 00 }
0x61E30: 			End  { 29 02 }
0x61E32: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x10FE, VarStoreId: 0xF007, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 FE 10 07 F0 00 00 00 11 00 00 FF FF 00 00 }
0x61E46: 			End  { 29 02 }
0x61E48: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x10FF, VarStoreId: 0x12, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 FF 10 12 00 00 00 00 11 00 00 FF FF 00 00 }
0x61E5C: 			End  { 29 02 }
0x61E5E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1100, VarStoreId: 0xF003, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 00 11 03 F0 00 00 00 11 00 00 FF FF 00 00 }
0x61E72: 			End  { 29 02 }
0x61E74: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1101, VarStoreId: 0x1C, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 01 11 1C 00 02 00 00 10 00 FF 00 }
0x61E85: 			End  { 29 02 }
0x61E87: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1102, VarStoreId: 0x1C, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 02 11 1C 00 01 00 00 10 00 FF 00 }
0x61E98: 			End  { 29 02 }
0x61E9A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1103, VarStoreId: 0x1C, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 03 11 1C 00 00 00 00 10 00 FF 00 }
0x61EAB: 			End  { 29 02 }
0x61EAD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1104, VarStoreId: 0x1C, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 04 11 1C 00 03 00 00 10 00 FF 00 }
0x61EBE: 			End  { 29 02 }
0x61EC0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1105, VarStoreId: 0x1C, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 05 11 1C 00 04 00 00 10 00 FF 00 }
0x61ED1: 			End  { 29 02 }
0x61ED3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1106, VarStoreId: 0x1C, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 06 11 1C 00 05 00 00 10 00 FF 00 }
0x61EE4: 			End  { 29 02 }
0x61EE6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1107, VarStoreId: 0x1D, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 07 11 1D 00 00 00 00 10 00 FF 00 }
0x61EF7: 			End  { 29 02 }
0x61EF9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1108, VarStoreId: 0x1F, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 08 11 1F 00 00 00 00 10 00 FF 00 }
0x61F0A: 			End  { 29 02 }
0x61F0C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1109, VarStoreId: 0x22, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 09 11 22 00 00 00 00 10 00 FF 00 }
0x61F1D: 			End  { 29 02 }
0x61F1F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x110A, VarStoreId: 0xF000, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0A 11 00 F0 00 00 00 10 00 FF 00 }
0x61F30: 			End  { 29 02 }
0x61F32: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x110B, VarStoreId: 0x1E, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0B 11 1E 00 00 00 00 10 00 FF 00 }
0x61F43: 			End  { 29 02 }
0x61F45: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x110C, VarStoreId: 0x20, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0C 11 20 00 00 00 00 10 00 FF 00 }
0x61F56: 			End  { 29 02 }
0x61F58: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x110D, VarStoreId: 0x21, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0D 11 21 00 00 00 00 10 00 FF 00 }
0x61F69: 			End  { 29 02 }
0x61F6B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x110E, VarStoreId: 0x27, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0E 11 27 00 0B 00 00 10 00 FF 00 }
0x61F7C: 			End  { 29 02 }
0x61F7E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x110F, VarStoreId: 0x6, VarOffset: 0x6EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0F 11 06 00 EB 06 00 10 00 FF 00 }
0x61F8F: 			End  { 29 02 }
0x61F91: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1110, VarStoreId: 0x6, VarOffset: 0x6EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 10 11 06 00 EA 06 00 10 00 FF 00 }
0x61FA2: 			End  { 29 02 }
0x61FA4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1111, VarStoreId: 0x6, VarOffset: 0x70D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 11 11 06 00 0D 07 00 10 00 FF 00 }
0x61FB5: 			End  { 29 02 }
0x61FB7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1112, VarStoreId: 0x27, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 12 11 27 00 03 00 00 10 00 FF 00 }
0x61FC8: 			End  { 29 02 }
0x61FCA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1113, VarStoreId: 0xF101, VarOffset: 0xBBE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 13 11 01 F1 BE 0B 00 10 00 FF 00 }
0x61FDB: 			End  { 29 02 }
0x61FDD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1114, VarStoreId: 0xF101, VarOffset: 0xBB0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 14 11 01 F1 B0 0B 00 10 00 FF 00 }
0x61FEE: 			End  { 29 02 }
0x61FF0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1115, VarStoreId: 0x27, VarOffset: 0x6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 15 11 27 00 6B 00 00 10 00 FF 00 }
0x62001: 			End  { 29 02 }
0x62003: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1116, VarStoreId: 0x27, VarOffset: 0x5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 16 11 27 00 5B 00 00 10 00 FF 00 }
0x62014: 			End  { 29 02 }
0x62016: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1117, VarStoreId: 0x27, VarOffset: 0x5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 17 11 27 00 5A 00 00 10 00 FF 00 }
0x62027: 			End  { 29 02 }
0x62029: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1118, VarStoreId: 0x27, VarOffset: 0x59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 18 11 27 00 59 00 00 10 00 FF 00 }
0x6203A: 			End  { 29 02 }
0x6203C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1119, VarStoreId: 0x27, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 19 11 27 00 58 00 00 10 00 FF 00 }
0x6204D: 			End  { 29 02 }
0x6204F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x111A, VarStoreId: 0x27, VarOffset: 0x57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1A 11 27 00 57 00 00 10 00 FF 00 }
0x62060: 			End  { 29 02 }
0x62062: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x111B, VarStoreId: 0x27, VarOffset: 0x56, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1B 11 27 00 56 00 00 10 00 FF 00 }
0x62073: 			End  { 29 02 }
0x62075: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x111C, VarStoreId: 0x27, VarOffset: 0x55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1C 11 27 00 55 00 00 10 00 FF 00 }
0x62086: 			End  { 29 02 }
0x62088: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x111D, VarStoreId: 0x27, VarOffset: 0x54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1D 11 27 00 54 00 00 10 00 FF 00 }
0x62099: 			End  { 29 02 }
0x6209B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x111E, VarStoreId: 0x27, VarOffset: 0x53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1E 11 27 00 53 00 00 10 00 FF 00 }
0x620AC: 			End  { 29 02 }
0x620AE: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x111F, VarStoreId: 0x27, VarOffset: 0x52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1F 11 27 00 52 00 00 10 00 FF 00 }
0x620BF: 			End  { 29 02 }
0x620C1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1120, VarStoreId: 0x27, VarOffset: 0x51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 20 11 27 00 51 00 00 10 00 FF 00 }
0x620D2: 			End  { 29 02 }
0x620D4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1121, VarStoreId: 0x27, VarOffset: 0x50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 21 11 27 00 50 00 00 10 00 FF 00 }
0x620E5: 			End  { 29 02 }
0x620E7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1122, VarStoreId: 0x27, VarOffset: 0x4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 22 11 27 00 4F 00 00 10 00 FF 00 }
0x620F8: 			End  { 29 02 }
0x620FA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1123, VarStoreId: 0x27, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 23 11 27 00 0A 00 00 10 00 FF 00 }
0x6210B: 			End  { 29 02 }
0x6210D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1124, VarStoreId: 0x27, VarOffset: 0x39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 24 11 27 00 39 00 00 10 00 FF 00 }
0x6211E: 			End  { 29 02 }
0x62120: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1125, VarStoreId: 0x27, VarOffset: 0x3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 25 11 27 00 3A 00 00 10 00 FF 00 }
0x62131: 			End  { 29 02 }
0x62133: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1126, VarStoreId: 0x27, VarOffset: 0x38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 26 11 27 00 38 00 00 10 00 FF 00 }
0x62144: 			End  { 29 02 }
0x62146: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1127, VarStoreId: 0x27, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 27 11 27 00 37 00 00 10 00 FF 00 }
0x62157: 			End  { 29 02 }
0x62159: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1128, VarStoreId: 0x27, VarOffset: 0x36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 28 11 27 00 36 00 00 10 00 FF 00 }
0x6216A: 			End  { 29 02 }
0x6216C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1129, VarStoreId: 0x27, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 29 11 27 00 35 00 00 10 00 FF 00 }
0x6217D: 			End  { 29 02 }
0x6217F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x112A, VarStoreId: 0x27, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2A 11 27 00 34 00 00 10 00 FF 00 }
0x62190: 			End  { 29 02 }
0x62192: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x112B, VarStoreId: 0x27, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2B 11 27 00 33 00 00 10 00 FF 00 }
0x621A3: 			End  { 29 02 }
0x621A5: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x112C, VarStoreId: 0x27, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2C 11 27 00 32 00 00 10 00 FF 00 }
0x621B6: 			End  { 29 02 }
0x621B8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x112D, VarStoreId: 0x27, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2D 11 27 00 31 00 00 10 00 FF 00 }
0x621C9: 			End  { 29 02 }
0x621CB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x112E, VarStoreId: 0x27, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2E 11 27 00 30 00 00 10 00 FF 00 }
0x621DC: 			End  { 29 02 }
0x621DE: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x112F, VarStoreId: 0x27, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2F 11 27 00 2F 00 00 10 00 FF 00 }
0x621EF: 			End  { 29 02 }
0x621F1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1130, VarStoreId: 0x27, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 30 11 27 00 2E 00 00 10 00 FF 00 }
0x62202: 			End  { 29 02 }
0x62204: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1131, VarStoreId: 0x27, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 31 11 27 00 2D 00 00 10 00 FF 00 }
0x62215: 			End  { 29 02 }
0x62217: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1132, VarStoreId: 0x27, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 32 11 27 00 2C 00 00 10 00 FF 00 }
0x62228: 			End  { 29 02 }
0x6222A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1133, VarStoreId: 0x27, VarOffset: 0x2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 33 11 27 00 2B 00 00 10 00 FF 00 }
0x6223B: 			End  { 29 02 }
0x6223D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1134, VarStoreId: 0x27, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 34 11 27 00 2A 00 00 10 00 FF 00 }
0x6224E: 			End  { 29 02 }
0x62250: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1135, VarStoreId: 0x27, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 35 11 27 00 29 00 00 10 00 FF 00 }
0x62261: 			End  { 29 02 }
0x62263: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1136, VarStoreId: 0x27, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 36 11 27 00 28 00 00 10 00 FF 00 }
0x62274: 			End  { 29 02 }
0x62276: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1137, VarStoreId: 0x27, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 37 11 27 00 27 00 00 10 00 FF 00 }
0x62287: 			End  { 29 02 }
0x62289: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1138, VarStoreId: 0x27, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 38 11 27 00 26 00 00 10 00 FF 00 }
0x6229A: 			End  { 29 02 }
0x6229C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1139, VarStoreId: 0x27, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 39 11 27 00 25 00 00 10 00 FF 00 }
0x622AD: 			End  { 29 02 }
0x622AF: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x113A, VarStoreId: 0x27, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 3A 11 27 00 24 00 00 10 00 FF 00 }
0x622C0: 			End  { 29 02 }
0x622C2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x113B, VarStoreId: 0x27, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 3B 11 27 00 23 00 00 10 00 FF 00 }
0x622D3: 			End  { 29 02 }
0x622D5: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x113C, VarStoreId: 0x27, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 3C 11 27 00 22 00 00 10 00 FF 00 }
0x622E6: 			End  { 29 02 }
0x622E8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x113D, VarStoreId: 0x27, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 3D 11 27 00 21 00 00 10 00 FF 00 }
0x622F9: 			End  { 29 02 }
0x622FB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x113E, VarStoreId: 0x27, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 3E 11 27 00 20 00 00 10 00 FF 00 }
0x6230C: 			End  { 29 02 }
0x6230E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x113F, VarStoreId: 0x27, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 3F 11 27 00 1F 00 00 10 00 FF 00 }
0x6231F: 			End  { 29 02 }
0x62321: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1140, VarStoreId: 0x27, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 40 11 27 00 1E 00 00 10 00 FF 00 }
0x62332: 			End  { 29 02 }
0x62334: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1141, VarStoreId: 0x27, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 41 11 27 00 1D 00 00 10 00 FF 00 }
0x62345: 			End  { 29 02 }
0x62347: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1142, VarStoreId: 0x27, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 42 11 27 00 02 00 00 10 00 FF 00 }
0x62358: 			End  { 29 02 }
0x6235A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1143, VarStoreId: 0x27, VarOffset: 0x5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 43 11 27 00 5C 00 00 10 00 FF 00 }
0x6236B: 			End  { 29 02 }
0x6236D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1144, VarStoreId: 0x27, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 44 11 27 00 08 00 00 10 00 FF 00 }
0x6237E: 			End  { 29 02 }
0x62380: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1145, VarStoreId: 0x27, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 45 11 27 00 07 00 00 10 00 FF 00 }
0x62391: 			End  { 29 02 }
0x62393: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1146, VarStoreId: 0x27, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 46 11 27 00 09 00 00 10 00 FF 00 }
0x623A4: 			End  { 29 02 }
0x623A6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1147, VarStoreId: 0x27, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 47 11 27 00 3D 00 00 10 00 FF 00 }
0x623B7: 			End  { 29 02 }
0x623B9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1148, VarStoreId: 0x27, VarOffset: 0x3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 48 11 27 00 3C 00 00 10 00 FF 00 }
0x623CA: 			End  { 29 02 }
0x623CC: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1149, VarStoreId: 0x27, VarOffset: 0x3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 49 11 27 00 3B 00 00 10 00 FF 00 }
0x623DD: 			End  { 29 02 }
0x623DF: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x114A, VarStoreId: 0x4, VarOffset: 0x174, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 4A 11 04 00 74 01 00 10 00 FF 00 }
0x623F0: 			End  { 29 02 }
0x623F2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x114B, VarStoreId: 0x4, VarOffset: 0x173, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 4B 11 04 00 73 01 00 10 00 FF 00 }
0x62403: 			End  { 29 02 }
0x62405: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x114C, VarStoreId: 0x4, VarOffset: 0x172, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 4C 11 04 00 72 01 00 10 00 FF 00 }
0x62416: 			End  { 29 02 }
0x62418: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x114D, VarStoreId: 0x4, VarOffset: 0x171, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 4D 11 04 00 71 01 00 10 00 FF 00 }
0x62429: 			End  { 29 02 }
0x6242B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x114E, VarStoreId: 0x4, VarOffset: 0x170, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 4E 11 04 00 70 01 00 10 00 FF 00 }
0x6243C: 			End  { 29 02 }
0x6243E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x114F, VarStoreId: 0x4, VarOffset: 0x16F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 4F 11 04 00 6F 01 00 10 00 FF 00 }
0x6244F: 			End  { 29 02 }
0x62451: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1150, VarStoreId: 0x4, VarOffset: 0x16E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 50 11 04 00 6E 01 00 10 00 FF 00 }
0x62462: 			End  { 29 02 }
0x62464: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1151, VarStoreId: 0x4, VarOffset: 0x16D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 51 11 04 00 6D 01 00 10 00 FF 00 }
0x62475: 			End  { 29 02 }
0x62477: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1152, VarStoreId: 0x4, VarOffset: 0x16C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 52 11 04 00 6C 01 00 10 00 FF 00 }
0x62488: 			End  { 29 02 }
0x6248A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1153, VarStoreId: 0x4, VarOffset: 0x16B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 53 11 04 00 6B 01 00 10 00 FF 00 }
0x6249B: 			End  { 29 02 }
0x6249D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1154, VarStoreId: 0x4, VarOffset: 0x16A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 54 11 04 00 6A 01 00 10 00 FF 00 }
0x624AE: 			End  { 29 02 }
0x624B0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1155, VarStoreId: 0x4, VarOffset: 0x169, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 55 11 04 00 69 01 00 10 00 FF 00 }
0x624C1: 			End  { 29 02 }
0x624C3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1156, VarStoreId: 0x4, VarOffset: 0x168, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 56 11 04 00 68 01 00 10 00 FF 00 }
0x624D4: 			End  { 29 02 }
0x624D6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1157, VarStoreId: 0x4, VarOffset: 0x167, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 57 11 04 00 67 01 00 10 00 FF 00 }
0x624E7: 			End  { 29 02 }
0x624E9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1158, VarStoreId: 0x4, VarOffset: 0x166, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 58 11 04 00 66 01 00 10 00 FF 00 }
0x624FA: 			End  { 29 02 }
0x624FC: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1159, VarStoreId: 0x4, VarOffset: 0x165, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 59 11 04 00 65 01 00 10 00 FF 00 }
0x6250D: 			End  { 29 02 }
0x6250F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x115A, VarStoreId: 0x4, VarOffset: 0x164, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 5A 11 04 00 64 01 00 10 00 FF 00 }
0x62520: 			End  { 29 02 }
0x62522: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x115B, VarStoreId: 0x4, VarOffset: 0x163, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 5B 11 04 00 63 01 00 10 00 FF 00 }
0x62533: 			End  { 29 02 }
0x62535: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x115C, VarStoreId: 0x4, VarOffset: 0x162, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 5C 11 04 00 62 01 00 10 00 FF 00 }
0x62546: 			End  { 29 02 }
0x62548: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x115D, VarStoreId: 0x4, VarOffset: 0x161, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 5D 11 04 00 61 01 00 10 00 FF 00 }
0x62559: 			End  { 29 02 }
0x6255B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x115E, VarStoreId: 0x4, VarOffset: 0x160, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 5E 11 04 00 60 01 00 10 00 FF 00 }
0x6256C: 			End  { 29 02 }
0x6256E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x115F, VarStoreId: 0x4, VarOffset: 0x15F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 5F 11 04 00 5F 01 00 10 00 FF 00 }
0x6257F: 			End  { 29 02 }
0x62581: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1160, VarStoreId: 0x4, VarOffset: 0x15E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 60 11 04 00 5E 01 00 10 00 FF 00 }
0x62592: 			End  { 29 02 }
0x62594: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1161, VarStoreId: 0x4, VarOffset: 0x15D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 61 11 04 00 5D 01 00 10 00 FF 00 }
0x625A5: 			End  { 29 02 }
0x625A7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1162, VarStoreId: 0x4, VarOffset: 0x15C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 62 11 04 00 5C 01 00 10 00 FF 00 }
0x625B8: 			End  { 29 02 }
0x625BA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1163, VarStoreId: 0x4, VarOffset: 0x15B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 63 11 04 00 5B 01 00 10 00 FF 00 }
0x625CB: 			End  { 29 02 }
0x625CD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1164, VarStoreId: 0x4, VarOffset: 0x15A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 64 11 04 00 5A 01 00 10 00 FF 00 }
0x625DE: 			End  { 29 02 }
0x625E0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1165, VarStoreId: 0x4, VarOffset: 0x159, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 65 11 04 00 59 01 00 10 00 FF 00 }
0x625F1: 			End  { 29 02 }
0x625F3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1166, VarStoreId: 0x4, VarOffset: 0x158, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 66 11 04 00 58 01 00 10 00 FF 00 }
0x62604: 			End  { 29 02 }
0x62606: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1167, VarStoreId: 0x4, VarOffset: 0x157, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 67 11 04 00 57 01 00 10 00 FF 00 }
0x62617: 			End  { 29 02 }
0x62619: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1168, VarStoreId: 0x4, VarOffset: 0x156, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 68 11 04 00 56 01 00 10 00 FF 00 }
0x6262A: 			End  { 29 02 }
0x6262C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1169, VarStoreId: 0xF101, VarOffset: 0x7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 69 11 01 F1 7C 00 00 10 00 FF 00 }
0x6263D: 			End  { 29 02 }
0x6263F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x116A, VarStoreId: 0xF101, VarOffset: 0x7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 6A 11 01 F1 7B 00 00 10 00 FF 00 }
0x62650: 			End  { 29 02 }
0x62652: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x116B, VarStoreId: 0x5, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 6B 11 05 00 05 00 00 10 00 FF 00 }
0x62663: 			End  { 29 02 }
0x62665: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x116C, VarStoreId: 0x5, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 6C 11 05 00 04 00 00 10 00 FF 00 }
0x62676: 			End  { 29 02 }
0x62678: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x116D, VarStoreId: 0x5, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 6D 11 05 00 03 00 00 10 00 FF 00 }
0x62689: 			End  { 29 02 }
0x6268B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x116E, VarStoreId: 0x5, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 6E 11 05 00 02 00 00 10 00 FF 00 }
0x6269C: 			End  { 29 02 }
0x6269E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x116F, VarStoreId: 0x27, VarOffset: 0x5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 6F 11 27 00 5F 00 00 10 00 FF 00 }
0x626AF: 			End  { 29 02 }
0x626B1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1170, VarStoreId: 0x4, VarOffset: 0x468, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 70 11 04 00 68 04 00 10 00 FF 00 }
0x626C2: 			End  { 29 02 }
0x626C4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1171, VarStoreId: 0x3, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 71 11 03 00 05 00 00 10 00 FF 00 }
0x626D5: 			End  { 29 02 }
0x626D7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1172, VarStoreId: 0x27, VarOffset: 0x5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 72 11 27 00 5D 00 00 10 00 FF 00 }
0x626E8: 			End  { 29 02 }
0x626EA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1173, VarStoreId: 0x2, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 73 11 02 00 18 00 00 10 00 FF 00 }
0x626FB: 			End  { 29 02 }
0x626FD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1174, VarStoreId: 0x27, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 74 11 27 00 05 00 00 10 00 FF 00 }
0x6270E: 			End  { 29 02 }
0x62710: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1175, VarStoreId: 0x9, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 75 11 09 00 04 00 00 10 00 FF 00 }
0x62721: 			End  { 29 02 }
0x62723: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1176, VarStoreId: 0x4, VarOffset: 0xF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 76 11 04 00 F7 00 00 10 00 FF 00 }
0x62734: 			End  { 29 02 }
0x62736: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1177, VarStoreId: 0x27, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 77 11 27 00 1C 00 00 10 00 FF 00 }
0x62747: 			End  { 29 02 }
0x62749: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1178, VarStoreId: 0x27, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 78 11 27 00 1B 00 00 10 00 FF 00 }
0x6275A: 			End  { 29 02 }
0x6275C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1179, VarStoreId: 0x27, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 79 11 27 00 1A 00 00 10 00 FF 00 }
0x6276D: 			End  { 29 02 }
0x6276F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x117A, VarStoreId: 0x27, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 7A 11 27 00 19 00 00 10 00 FF 00 }
0x62780: 			End  { 29 02 }
0x62782: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x117B, VarStoreId: 0x27, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 7B 11 27 00 18 00 00 10 00 FF 00 }
0x62793: 			End  { 29 02 }
0x62795: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x117C, VarStoreId: 0x27, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 7C 11 27 00 17 00 00 10 00 FF 00 }
0x627A6: 			End  { 29 02 }
0x627A8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x117D, VarStoreId: 0x27, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 7D 11 27 00 16 00 00 10 00 FF 00 }
0x627B9: 			End  { 29 02 }
0x627BB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x117E, VarStoreId: 0x27, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 7E 11 27 00 15 00 00 10 00 FF 00 }
0x627CC: 			End  { 29 02 }
0x627CE: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x117F, VarStoreId: 0x27, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 7F 11 27 00 14 00 00 10 00 FF 00 }
0x627DF: 			End  { 29 02 }
0x627E1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1180, VarStoreId: 0x27, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 80 11 27 00 13 00 00 10 00 FF 00 }
0x627F2: 			End  { 29 02 }
0x627F4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1181, VarStoreId: 0x27, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 81 11 27 00 12 00 00 10 00 FF 00 }
0x62805: 			End  { 29 02 }
0x62807: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1182, VarStoreId: 0x27, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 82 11 27 00 11 00 00 10 00 FF 00 }
0x62818: 			End  { 29 02 }
0x6281A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1183, VarStoreId: 0x27, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 83 11 27 00 10 00 00 10 00 FF 00 }
0x6282B: 			End  { 29 02 }
0x6282D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1184, VarStoreId: 0x27, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 84 11 27 00 0F 00 00 10 00 FF 00 }
0x6283E: 			End  { 29 02 }
0x62840: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1185, VarStoreId: 0x27, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 85 11 27 00 0E 00 00 10 00 FF 00 }
0x62851: 			End  { 29 02 }
0x62853: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1186, VarStoreId: 0x27, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 86 11 27 00 0D 00 00 10 00 FF 00 }
0x62864: 			End  { 29 02 }
0x62866: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1187, VarStoreId: 0x27, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 87 11 27 00 0C 00 00 10 00 FF 00 }
0x62877: 			End  { 29 02 }
0x62879: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1188, VarStoreId: 0x27, VarOffset: 0x6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 88 11 27 00 6A 00 00 10 00 FF 00 }
0x6288A: 			End  { 29 02 }
0x6288C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1189, VarStoreId: 0x26, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 89 11 26 00 00 00 00 11 00 00 FF FF 00 00 }
0x628A0: 			End  { 29 02 }
0x628A2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x118A, VarStoreId: 0x25, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 8A 11 25 00 00 00 00 11 00 00 FF FF 00 00 }
0x628B6: 			End  { 29 02 }
0x628B8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x118B, VarStoreId: 0x29D3, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 8B 11 D3 29 09 00 00 10 00 FF 00 }
0x628C9: 			End  { 29 02 }
0x628CB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x118C, VarStoreId: 0x29D3, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 8C 11 D3 29 01 00 00 10 00 FF 00 }
0x628DC: 			End  { 29 02 }
0x628DE: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x118D, VarStoreId: 0x29D3, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 8D 11 D3 29 08 00 00 10 00 FF 00 }
0x628EF: 			End  { 29 02 }
0x628F1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x118E, VarStoreId: 0x29D3, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 8E 11 D3 29 07 00 00 10 00 FF 00 }
0x62902: 			End  { 29 02 }
0x62904: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x118F, VarStoreId: 0x29D3, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 8F 11 D3 29 06 00 00 10 00 FF 00 }
0x62915: 			End  { 29 02 }
0x62917: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1190, VarStoreId: 0x29D3, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 90 11 D3 29 05 00 00 10 00 FF 00 }
0x62928: 			End  { 29 02 }
0x6292A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1191, VarStoreId: 0x29D3, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 91 11 D3 29 04 00 00 10 00 FF 00 }
0x6293B: 			End  { 29 02 }
0x6293D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1192, VarStoreId: 0x29D3, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 92 11 D3 29 03 00 00 10 00 FF 00 }
0x6294E: 			End  { 29 02 }
0x62950: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1193, VarStoreId: 0x29D3, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 93 11 D3 29 02 00 00 10 00 FF 00 }
0x62961: 			End  { 29 02 }
0x62963: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1194, VarStoreId: 0x17, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 94 11 17 00 1F 00 00 10 00 FF 00 }
0x62974: 			End  { 29 02 }
0x62976: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1195, VarStoreId: 0x17, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 95 11 17 00 1E 00 00 10 00 FF 00 }
0x62987: 			End  { 29 02 }
0x62989: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1196, VarStoreId: 0x17, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 96 11 17 00 1D 00 00 10 00 FF 00 }
0x6299A: 			End  { 29 02 }
0x6299C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1197, VarStoreId: 0x17, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 97 11 17 00 1C 00 00 10 00 FF 00 }
0x629AD: 			End  { 29 02 }
0x629AF: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1198, VarStoreId: 0x17, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 98 11 17 00 1B 00 00 10 00 FF 00 }
0x629C0: 			End  { 29 02 }
0x629C2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1199, VarStoreId: 0x17, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 99 11 17 00 1A 00 00 10 00 FF 00 }
0x629D3: 			End  { 29 02 }
0x629D5: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x119A, VarStoreId: 0x17, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 9A 11 17 00 19 00 00 10 00 FF 00 }
0x629E6: 			End  { 29 02 }
0x629E8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x119B, VarStoreId: 0x17, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 9B 11 17 00 18 00 00 10 00 FF 00 }
0x629F9: 			End  { 29 02 }
0x629FB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x119C, VarStoreId: 0x17, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 9C 11 17 00 17 00 00 10 00 FF 00 }
0x62A0C: 			End  { 29 02 }
0x62A0E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x119D, VarStoreId: 0x17, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 9D 11 17 00 16 00 00 10 00 FF 00 }
0x62A1F: 			End  { 29 02 }
0x62A21: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x119E, VarStoreId: 0x17, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 9E 11 17 00 15 00 00 10 00 FF 00 }
0x62A32: 			End  { 29 02 }
0x62A34: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x119F, VarStoreId: 0x17, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 9F 11 17 00 14 00 00 10 00 FF 00 }
0x62A45: 			End  { 29 02 }
0x62A47: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A0, VarStoreId: 0x17, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A0 11 17 00 13 00 00 10 00 FF 00 }
0x62A58: 			End  { 29 02 }
0x62A5A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A1, VarStoreId: 0x17, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A1 11 17 00 12 00 00 10 00 FF 00 }
0x62A6B: 			End  { 29 02 }
0x62A6D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A2, VarStoreId: 0x17, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A2 11 17 00 11 00 00 10 00 FF 00 }
0x62A7E: 			End  { 29 02 }
0x62A80: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A3, VarStoreId: 0x17, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A3 11 17 00 10 00 00 10 00 FF 00 }
0x62A91: 			End  { 29 02 }
0x62A93: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A4, VarStoreId: 0x17, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A4 11 17 00 0F 00 00 10 00 FF 00 }
0x62AA4: 			End  { 29 02 }
0x62AA6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A5, VarStoreId: 0x17, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A5 11 17 00 0E 00 00 10 00 FF 00 }
0x62AB7: 			End  { 29 02 }
0x62AB9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A6, VarStoreId: 0x17, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A6 11 17 00 0D 00 00 10 00 FF 00 }
0x62ACA: 			End  { 29 02 }
0x62ACC: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A7, VarStoreId: 0x17, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A7 11 17 00 0C 00 00 10 00 FF 00 }
0x62ADD: 			End  { 29 02 }
0x62ADF: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A8, VarStoreId: 0x17, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A8 11 17 00 0B 00 00 10 00 FF 00 }
0x62AF0: 			End  { 29 02 }
0x62AF2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11A9, VarStoreId: 0x17, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 A9 11 17 00 0A 00 00 10 00 FF 00 }
0x62B03: 			End  { 29 02 }
0x62B05: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11AA, VarStoreId: 0x17, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 AA 11 17 00 09 00 00 10 00 FF 00 }
0x62B16: 			End  { 29 02 }
0x62B18: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11AB, VarStoreId: 0x17, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 AB 11 17 00 08 00 00 10 00 FF 00 }
0x62B29: 			End  { 29 02 }
0x62B2B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11AC, VarStoreId: 0x17, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 AC 11 17 00 07 00 00 10 00 FF 00 }
0x62B3C: 			End  { 29 02 }
0x62B3E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11AD, VarStoreId: 0x17, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 AD 11 17 00 06 00 00 10 00 FF 00 }
0x62B4F: 			End  { 29 02 }
0x62B51: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11AE, VarStoreId: 0x17, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 AE 11 17 00 05 00 00 10 00 FF 00 }
0x62B62: 			End  { 29 02 }
0x62B64: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11AF, VarStoreId: 0x17, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 AF 11 17 00 04 00 00 10 00 FF 00 }
0x62B75: 			End  { 29 02 }
0x62B77: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B0, VarStoreId: 0x17, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B0 11 17 00 03 00 00 10 00 FF 00 }
0x62B88: 			End  { 29 02 }
0x62B8A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B1, VarStoreId: 0x17, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B1 11 17 00 02 00 00 10 00 FF 00 }
0x62B9B: 			End  { 29 02 }
0x62B9D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B2, VarStoreId: 0x17, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B2 11 17 00 01 00 00 10 00 FF 00 }
0x62BAE: 			End  { 29 02 }
0x62BB0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B3, VarStoreId: 0x17, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B3 11 17 00 00 00 00 10 00 FF 00 }
0x62BC1: 			End  { 29 02 }
0x62BC3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B4, VarStoreId: 0x16, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B4 11 16 00 00 00 00 10 00 FF 00 }
0x62BD4: 			End  { 29 02 }
0x62BD6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B5, VarStoreId: 0x18, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B5 11 18 00 03 00 00 10 00 FF 00 }
0x62BE7: 			End  { 29 02 }
0x62BE9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B6, VarStoreId: 0x18, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B6 11 18 00 02 00 00 10 00 FF 00 }
0x62BFA: 			End  { 29 02 }
0x62BFC: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B7, VarStoreId: 0x18, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B7 11 18 00 01 00 00 10 00 FF 00 }
0x62C0D: 			End  { 29 02 }
0x62C0F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B8, VarStoreId: 0x18, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B8 11 18 00 00 00 00 10 00 FF 00 }
0x62C20: 			End  { 29 02 }
0x62C22: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11B9, VarStoreId: 0x15, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 B9 11 15 00 01 00 00 10 00 FF 00 }
0x62C33: 			End  { 29 02 }
0x62C35: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11BA, VarStoreId: 0x15, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 BA 11 15 00 00 00 00 10 00 FF 00 }
0x62C46: 			End  { 29 02 }
0x62C48: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11BB, VarStoreId: 0x14, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 BB 11 14 00 01 00 00 10 00 FF 00 }
0x62C59: 			End  { 29 02 }
0x62C5B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11BC, VarStoreId: 0xF101, VarOffset: 0xC8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 BC 11 01 F1 8A 0C 00 10 00 FF 00 }
0x62C6C: 			End  { 29 02 }
0x62C6E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11BD, VarStoreId: 0xF, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 BD 11 0F 00 01 00 00 10 00 FF 00 }
0x62C7F: 			End  { 29 02 }
0x62C81: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11BE, VarStoreId: 0xF, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 BE 11 0F 00 00 00 00 10 00 FF 00 }
0x62C92: 			End  { 29 02 }
0x62C94: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11BF, VarStoreId: 0xF101, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 BF 11 01 F1 22 00 00 10 00 FF 00 }
0x62CA5: 			End  { 29 02 }
0x62CA7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C0, VarStoreId: 0xF101, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C0 11 01 F1 26 00 00 10 00 FF 00 }
0x62CB8: 			End  { 29 02 }
0x62CBA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C1, VarStoreId: 0xF101, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C1 11 01 F1 25 00 00 10 00 FF 00 }
0x62CCB: 			End  { 29 02 }
0x62CCD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C2, VarStoreId: 0xF101, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C2 11 01 F1 24 00 00 10 00 FF 00 }
0x62CDE: 			End  { 29 02 }
0x62CE0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C3, VarStoreId: 0xF101, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C3 11 01 F1 23 00 00 10 00 FF 00 }
0x62CF1: 			End  { 29 02 }
0x62CF3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C4, VarStoreId: 0xF101, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C4 11 01 F1 15 00 00 10 00 FF 00 }
0x62D04: 			End  { 29 02 }
0x62D06: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C5, VarStoreId: 0xF101, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C5 11 01 F1 14 00 00 10 00 FF 00 }
0x62D17: 			End  { 29 02 }
0x62D19: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C6, VarStoreId: 0xF101, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C6 11 01 F1 11 00 00 10 00 FF 00 }
0x62D2A: 			End  { 29 02 }
0x62D2C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C7, VarStoreId: 0x9, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C7 11 09 00 03 00 00 10 00 FF 00 }
0x62D3D: 			End  { 29 02 }
0x62D3F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C8, VarStoreId: 0x3, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 C8 11 03 00 00 00 00 11 00 00 FF FF 00 00 }
0x62D53: 			End  { 29 02 }
0x62D55: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11C9, VarStoreId: 0x3, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 C9 11 03 00 04 00 00 10 00 FF 00 }
0x62D66: 			End  { 29 02 }
0x62D68: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11CA, VarStoreId: 0x28B7, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 CA 11 B7 28 02 00 00 10 00 FF 00 }
0x62D79: 			End  { 29 02 }
0x62D7B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11CB, VarStoreId: 0x2, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 CB 11 02 00 22 00 00 10 00 FF 00 }
0x62D8C: 			End  { 29 02 }
0x62D8E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11CC, VarStoreId: 0x28B7, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 CC 11 B7 28 03 00 00 10 00 FF 00 }
0x62D9F: 			End  { 29 02 }
0x62DA1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11CD, VarStoreId: 0x2, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 CD 11 02 00 21 00 00 10 00 FF 00 }
0x62DB2: 			End  { 29 02 }
0x62DB4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11CE, VarStoreId: 0x1, VarOffset: 0x113, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 CE 11 01 00 13 01 00 10 00 FF 00 }
0x62DC5: 			End  { 29 02 }
0x62DC7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11CF, VarStoreId: 0x28B7, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 CF 11 B7 28 01 00 00 10 00 FF 00 }
0x62DD8: 			End  { 29 02 }
0x62DDA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D0, VarStoreId: 0x28B7, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D0 11 B7 28 00 00 00 10 00 FF 00 }
0x62DEB: 			End  { 29 02 }
0x62DED: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D1, VarStoreId: 0xF101, VarOffset: 0xADC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D1 11 01 F1 DC 0A 00 10 00 FF 00 }
0x62DFE: 			End  { 29 02 }
0x62E00: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D2, VarStoreId: 0xF101, VarOffset: 0x799, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D2 11 01 F1 99 07 00 10 00 FF 00 }
0x62E11: 			End  { 29 02 }
0x62E13: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D3, VarStoreId: 0x5, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D3 11 05 00 00 00 00 10 00 FF 00 }
0x62E24: 			End  { 29 02 }
0x62E26: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D4, VarStoreId: 0xF101, VarOffset: 0x7CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D4 11 01 F1 CA 07 00 10 00 FF 00 }
0x62E37: 			End  { 29 02 }
0x62E39: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D5, VarStoreId: 0x5, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D5 11 05 00 01 00 00 10 00 FF 00 }
0x62E4A: 			End  { 29 02 }
0x62E4C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D6, VarStoreId: 0xF101, VarOffset: 0x7C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D6 11 01 F1 C9 07 00 10 00 FF 00 }
0x62E5D: 			End  { 29 02 }
0x62E5F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D7, VarStoreId: 0xF101, VarOffset: 0x7C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D7 11 01 F1 C8 07 00 10 00 FF 00 }
0x62E70: 			End  { 29 02 }
0x62E72: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D8, VarStoreId: 0xF101, VarOffset: 0x7C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D8 11 01 F1 C7 07 00 10 00 FF 00 }
0x62E83: 			End  { 29 02 }
0x62E85: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11D9, VarStoreId: 0xF101, VarOffset: 0xB36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 D9 11 01 F1 36 0B 00 10 00 FF 00 }
0x62E96: 			End  { 29 02 }
0x62E98: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11DA, VarStoreId: 0xF101, VarOffset: 0xADA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 DA 11 01 F1 DA 0A 00 10 00 FF 00 }
0x62EA9: 			End  { 29 02 }
0x62EAB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11DB, VarStoreId: 0xF101, VarOffset: 0x79B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 DB 11 01 F1 9B 07 00 10 00 FF 00 }
0x62EBC: 			End  { 29 02 }
0x62EBE: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11DC, VarStoreId: 0xF101, VarOffset: 0xAF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 DC 11 01 F1 F3 0A 00 10 00 FF 00 }
0x62ECF: 			End  { 29 02 }
0x62ED1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11DD, VarStoreId: 0x27, VarOffset: 0x67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 DD 11 27 00 67 00 00 10 00 FF 00 }
0x62EE2: 			End  { 29 02 }
0x62EE4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11DE, VarStoreId: 0x27, VarOffset: 0x66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 DE 11 27 00 66 00 00 10 00 FF 00 }
0x62EF5: 			End  { 29 02 }
0x62EF7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11DF, VarStoreId: 0x27, VarOffset: 0x65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 DF 11 27 00 65 00 00 10 00 FF 00 }
0x62F08: 			End  { 29 02 }
0x62F0A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E0, VarStoreId: 0x27, VarOffset: 0x64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E0 11 27 00 64 00 00 10 00 FF 00 }
0x62F1B: 			End  { 29 02 }
0x62F1D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E1, VarStoreId: 0xF101, VarOffset: 0xBB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E1 11 01 F1 B1 0B 00 10 00 FF 00 }
0x62F2E: 			End  { 29 02 }
0x62F30: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E2, VarStoreId: 0x9, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E2 11 09 00 11 00 00 10 00 FF 00 }
0x62F41: 			End  { 29 02 }
0x62F43: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E3, VarStoreId: 0x3, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E3 11 03 00 07 00 00 10 00 FF 00 }
0x62F54: 			End  { 29 02 }
0x62F56: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E4, VarStoreId: 0x3, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E4 11 03 00 06 00 00 10 00 FF 00 }
0x62F67: 			End  { 29 02 }
0x62F69: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E5, VarStoreId: 0x1, VarOffset: 0x2AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E5 11 01 00 AB 02 00 10 00 FF 00 }
0x62F7A: 			End  { 29 02 }
0x62F7C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E6, VarStoreId: 0x2, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E6 11 02 00 2F 00 00 10 00 FF 00 }
0x62F8D: 			End  { 29 02 }
0x62F8F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E7, VarStoreId: 0x1, VarOffset: 0x27D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E7 11 01 00 7D 02 00 10 00 FF 00 }
0x62FA0: 			End  { 29 02 }
0x62FA2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E8, VarStoreId: 0x1, VarOffset: 0x1D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E8 11 01 00 D2 01 00 10 00 FF 00 }
0x62FB3: 			End  { 29 02 }
0x62FB5: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11E9, VarStoreId: 0x1, VarOffset: 0x1CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 E9 11 01 00 CE 01 00 10 00 FF 00 }
0x62FC6: 			End  { 29 02 }
0x62FC8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11EA, VarStoreId: 0x1, VarOffset: 0x233, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 EA 11 01 00 33 02 00 10 00 FF 00 }
0x62FD9: 			End  { 29 02 }
0x62FDB: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11EB, VarStoreId: 0x2, VarOffset: 0x36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 EB 11 02 00 36 00 00 10 00 FF 00 }
0x62FEC: 			End  { 29 02 }
0x62FEE: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11EC, VarStoreId: 0x2, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 EC 11 02 00 15 00 00 10 00 FF 00 }
0x62FFF: 			End  { 29 02 }
0x63001: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11ED, VarStoreId: 0x2, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 ED 11 02 00 37 00 00 10 00 FF 00 }
0x63012: 			End  { 29 02 }
0x63014: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11EE, VarStoreId: 0x2, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 EE 11 02 00 2E 00 00 10 00 FF 00 }
0x63025: 			End  { 29 02 }
0x63027: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11EF, VarStoreId: 0x1, VarOffset: 0x382, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 EF 11 01 00 82 03 00 10 00 FF 00 }
0x63038: 			End  { 29 02 }
0x6303A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F0, VarStoreId: 0x27, VarOffset: 0x68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F0 11 27 00 68 00 00 10 00 FF 00 }
0x6304B: 			End  { 29 02 }
0x6304D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F1, VarStoreId: 0x27, VarOffset: 0x6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F1 11 27 00 6C 00 00 10 00 FF 00 }
0x6305E: 			End  { 29 02 }
0x63060: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F2, VarStoreId: 0xF101, VarOffset: 0x70F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F2 11 01 F1 0F 07 00 10 00 FF 00 }
0x63071: 			End  { 29 02 }
0x63073: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F3, VarStoreId: 0xF101, VarOffset: 0x85D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F3 11 01 F1 5D 08 00 10 00 FF 00 }
0x63084: 			End  { 29 02 }
0x63086: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F4, VarStoreId: 0xF101, VarOffset: 0x817, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F4 11 01 F1 17 08 00 10 00 FF 00 }
0x63097: 			End  { 29 02 }
0x63099: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F5, VarStoreId: 0xF101, VarOffset: 0x54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F5 11 01 F1 54 00 00 10 00 FF 00 }
0x630AA: 			End  { 29 02 }
0x630AC: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F6, VarStoreId: 0xF101, VarOffset: 0xB86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F6 11 01 F1 86 0B 00 10 00 FF 00 }
0x630BD: 			End  { 29 02 }
0x630BF: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F7, VarStoreId: 0xF101, VarOffset: 0xB8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F7 11 01 F1 8D 0B 00 10 00 FF 00 }
0x630D0: 			End  { 29 02 }
0x630D2: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F8, VarStoreId: 0xF101, VarOffset: 0xA9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F8 11 01 F1 9B 0A 00 10 00 FF 00 }
0x630E3: 			End  { 29 02 }
0x630E5: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11F9, VarStoreId: 0xF101, VarOffset: 0x6E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 F9 11 01 F1 E7 06 00 10 00 FF 00 }
0x630F6: 			End  { 29 02 }
0x630F8: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11FA, VarStoreId: 0xF101, VarOffset: 0x6E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 FA 11 01 F1 E6 06 00 10 00 FF 00 }
0x63109: 			End  { 29 02 }
0x6310B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11FB, VarStoreId: 0xF101, VarOffset: 0x6E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 FB 11 01 F1 E5 06 00 10 00 FF 00 }
0x6311C: 			End  { 29 02 }
0x6311E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11FC, VarStoreId: 0xF101, VarOffset: 0x6E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 FC 11 01 F1 E4 06 00 10 00 FF 00 }
0x6312F: 			End  { 29 02 }
0x63131: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11FD, VarStoreId: 0xF101, VarOffset: 0x6E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 FD 11 01 F1 E3 06 00 10 00 FF 00 }
0x63142: 			End  { 29 02 }
0x63144: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11FE, VarStoreId: 0xF101, VarOffset: 0x6DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 FE 11 01 F1 DA 06 00 10 00 FF 00 }
0x63155: 			End  { 29 02 }
0x63157: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x11FF, VarStoreId: 0xF101, VarOffset: 0x6D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 FF 11 01 F1 D9 06 00 10 00 FF 00 }
0x63168: 			End  { 29 02 }
0x6316A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1200, VarStoreId: 0xF101, VarOffset: 0x6D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 00 12 01 F1 D8 06 00 10 00 FF 00 }
0x6317B: 			End  { 29 02 }
0x6317D: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1201, VarStoreId: 0x28B8, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 01 12 B8 28 0B 00 00 10 00 FF 00 }
0x6318E: 			End  { 29 02 }
0x63190: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1202, VarStoreId: 0x8, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 02 12 08 00 02 00 00 10 00 FF 00 }
0x631A1: 			End  { 29 02 }
0x631A3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1203, VarStoreId: 0x9, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 03 12 09 00 08 00 00 10 00 FF 00 }
0x631B4: 			End  { 29 02 }
0x631B6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1204, VarStoreId: 0x9, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 04 12 09 00 07 00 00 10 00 FF 00 }
0x631C7: 			End  { 29 02 }
0x631C9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1205, VarStoreId: 0x9, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 05 12 09 00 0D 00 00 10 00 FF 00 }
0x631DA: 			End  { 29 02 }
0x631DC: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1206, VarStoreId: 0x8, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 06 12 08 00 0F 00 00 10 00 FF 00 }
0x631ED: 			End  { 29 02 }
0x631EF: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1207, VarStoreId: 0x9, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 07 12 09 00 0C 00 00 10 00 FF 00 }
0x63200: 			End  { 29 02 }
0x63202: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1208, VarStoreId: 0x8, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 08 12 08 00 01 00 00 10 00 FF 00 }
0x63213: 			End  { 29 02 }
0x63215: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1209, VarStoreId: 0x2, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 09 12 02 00 35 00 00 10 00 FF 00 }
0x63226: 			End  { 29 02 }
0x63228: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x120A, VarStoreId: 0x2, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0A 12 02 00 34 00 00 10 00 FF 00 }
0x63239: 			End  { 29 02 }
0x6323B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x120B, VarStoreId: 0x2, VarOffset: 0x2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0B 12 02 00 2B 00 00 10 00 FF 00 }
0x6324C: 			End  { 29 02 }
0x6324E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x120C, VarStoreId: 0x3, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0C 12 03 00 0A 00 00 10 00 FF 00 }
0x6325F: 			End  { 29 02 }
0x63261: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x120D, VarStoreId: 0x2, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0D 12 02 00 32 00 00 10 00 FF 00 }
0x63272: 			End  { 29 02 }
0x63274: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x120E, VarStoreId: 0x3, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0E 12 03 00 08 00 00 10 00 FF 00 }
0x63285: 			End  { 29 02 }
0x63287: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x120F, VarStoreId: 0x2, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 0F 12 02 00 1D 00 00 10 00 FF 00 }
0x63298: 			End  { 29 02 }
0x6329A: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1210, VarStoreId: 0x1, VarOffset: 0x2AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 10 12 01 00 AC 02 00 10 00 FF 00 }
0x632AB: 			End  { 29 02 }
0x632AD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1211, VarStoreId: 0x2, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 11 12 02 00 03 00 00 10 00 FF 00 }
0x632BE: 			End  { 29 02 }
0x632C0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1212, VarStoreId: 0x2, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 12 12 02 00 20 00 00 10 00 FF 00 }
0x632D1: 			End  { 29 02 }
0x632D3: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1213, VarStoreId: 0x2, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 13 12 02 00 09 00 00 10 00 FF 00 }
0x632E4: 			End  { 29 02 }
0x632E6: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1214, VarStoreId: 0x2, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 14 12 02 00 0B 00 00 10 00 FF 00 }
0x632F7: 			End  { 29 02 }
0x632F9: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1215, VarStoreId: 0x2, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 15 12 02 00 01 00 00 10 00 FF 00 }
0x6330A: 			End  { 29 02 }
0x6330C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1216, VarStoreId: 0x2, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 16 12 02 00 33 00 00 10 00 FF 00 }
0x6331D: 			End  { 29 02 }
0x6331F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1217, VarStoreId: 0x2, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 17 12 02 00 13 00 00 10 00 FF 00 }
0x63330: 			End  { 29 02 }
0x63332: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1218, VarStoreId: 0x2, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 18 12 02 00 14 00 00 10 00 FF 00 }
0x63343: 			End  { 29 02 }
0x63345: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1219, VarStoreId: 0x2, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 19 12 02 00 12 00 00 10 00 FF 00 }
0x63356: 			End  { 29 02 }
0x63358: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x121A, VarStoreId: 0x2, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1A 12 02 00 28 00 00 10 00 FF 00 }
0x63369: 			End  { 29 02 }
0x6336B: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x121B, VarStoreId: 0x2, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1B 12 02 00 24 00 00 10 00 FF 00 }
0x6337C: 			End  { 29 02 }
0x6337E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x121C, VarStoreId: 0x2, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1C 12 02 00 26 00 00 10 00 FF 00 }
0x6338F: 			End  { 29 02 }
0x63391: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x121D, VarStoreId: 0x2, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1D 12 02 00 25 00 00 10 00 FF 00 }
0x633A2: 			End  { 29 02 }
0x633A4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x121E, VarStoreId: 0x2, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1E 12 02 00 23 00 00 10 00 FF 00 }
0x633B5: 			End  { 29 02 }
0x633B7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x121F, VarStoreId: 0x2, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 1F 12 02 00 31 00 00 10 00 FF 00 }
0x633C8: 			End  { 29 02 }
0x633CA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1220, VarStoreId: 0x2, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 20 12 02 00 2C 00 00 10 00 FF 00 }
0x633DB: 			End  { 29 02 }
0x633DD: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1221, VarStoreId: 0x2, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 21 12 02 00 04 00 00 10 00 FF 00 }
0x633EE: 			End  { 29 02 }
0x633F0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1222, VarStoreId: 0x1, VarOffset: 0xC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 22 12 01 00 C2 00 00 10 00 FF 00 }
0x63401: 			End  { 29 02 }
0x63403: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1223, VarStoreId: 0x2, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 23 12 02 00 08 00 00 10 00 FF 00 }
0x63414: 			End  { 29 02 }
0x63416: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1224, VarStoreId: 0x2, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 24 12 02 00 06 00 00 10 00 FF 00 }
0x63427: 			End  { 29 02 }
0x63429: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1225, VarStoreId: 0x2, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 25 12 02 00 1B 00 00 10 00 FF 00 }
0x6343A: 			End  { 29 02 }
0x6343C: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1226, VarStoreId: 0x6, VarOffset: 0x78C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 26 12 06 00 8C 07 00 10 00 FF 00 }
0x6344D: 			End  { 29 02 }
0x6344F: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1227, VarStoreId: 0x27, VarOffset: 0x62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 27 12 27 00 62 00 00 10 00 FF 00 }
0x63460: 			End  { 29 02 }
0x63462: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1228, VarStoreId: 0x24, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 28 12 24 00 00 00 00 11 00 00 FF FF 00 00 }
0x63476: 			End  { 29 02 }
0x63478: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x1229, VarStoreId: 0x23, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 29 12 23 00 00 00 00 11 00 00 FF FF 00 00 }
0x6348C: 			End  { 29 02 }
0x6348E: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x122A, VarStoreId: 0x14, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2A 12 14 00 00 00 00 10 00 FF 00 }
0x6349F: 			End  { 29 02 }
0x634A1: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x122B, VarStoreId: 0xF101, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2B 12 01 F1 16 00 00 10 00 FF 00 }
0x634B2: 			End  { 29 02 }
0x634B4: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x122C, VarStoreId: 0xF101, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2C 12 01 F1 1A 00 00 10 00 FF 00 }
0x634C5: 			End  { 29 02 }
0x634C7: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x122D, VarStoreId: 0xF101, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2D 12 01 F1 18 00 00 10 00 FF 00 }
0x634D8: 			End  { 29 02 }
0x634DA: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x122E, VarStoreId: 0xF00A, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0 { 07 94 00 00 00 00 2E 12 0A F0 00 00 00 11 00 00 FF FF 00 00 }
0x634EE: 			End  { 29 02 }
0x634F0: 			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x122F, VarStoreId: 0xF101, VarOffset: 0x6C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0 { 07 91 00 00 00 00 2F 12 01 F1 C5 06 00 10 00 FF 00 }
0x63501: 			End  { 29 02 }
0x63503: 		End  { 29 02 }
0x63505: 	End  { 29 02 }
0x63507: End  { 29 02 }
