Intel (R) Flash Programming Tool Version: 14.0.36.1158
Copyright (C) 2005 - 2020, Intel Corporation. All rights reserved.


Windows OS Version : 10.0

LPC Device Id: 68D.
Platform: Cometlake Platform 
General FW Information
FW Status Register1: 0x90000255
FW Status Register2: 0x80110106
FW Status Register3: 0x00000020
FW Status Register4: 0x00004000
FW Status Register5: 0x00000000
FW Status Register6: 0x00400000

    CurrentState:                              Normal
    ManufacturingMode:                         Enabled
    FlashPartition:                            Valid
    OperationalState:                          CM0 with UMA
    InitComplete:                              Complete
    BUPLoadState:                              Success
    ErrorCode:                                 No Error
    ModeOfOperation:                           Normal
    SPI Flash Log:                             Not Present
    Phase:                                     Maestro
    PhaseStatus:                               UNKNOWN
    ME File System Corrupted:                  No
    FPF and ME Config Status:                  Not committed
    RPMC status:                               OK
Initializing SPI utilities
Reading HSFSTS register... Flash Descriptor: Valid 

Region Limits as programmed into the SPI Registers 
    FREG0 -  DESC       Region:Base Address: 0x000000   Limit :  0x000FFF 
    FREG1 -  BIOS       Region:Base Address: 0x400000   Limit :  0xFFFFFF 
    FREG2 -  CSME       Region:Base Address: 0x001000   Limit :  0x3FFFFF 
    FREG3 -  GbE        Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG4 -  PDR        Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG5 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG6 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG7 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG8 -  EC         Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG9 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG10 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG11 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG12 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG13 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG14 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
    FREG15 -             Region:Base Address: 0x7FFF000   Limit :  0x000FFF 
Address Limit 0x1000000    Maximum Memory 16384kB 


    --- Flash Devices Found ---
    ID:0xEF4018    Size: 16384KB (131072Kb)

Using hardware sequencing.
Reading region information from flash descriptor.
Base: 0x00000000, Limit: 0x00000FFF
Base: 0x00400000, Limit: 0x00FFFFFF
Base: 0x00001000, Limit: 0x003FFFFF
DumpFlashToFile (All_regions.bin, 0x0, 0x0)...

- Reading Flash [0x0000040]     0KB of 16384KB -   0 percent complete.
- Reading Flash [0x0028F80]   163KB of 16384KB -   1 percent complete.
- Reading Flash [0x0051EC0]   327KB of 16384KB -   2 percent complete.
- Reading Flash [0x007AE40]   491KB of 16384KB -   3 percent complete.
- Reading Flash [0x00A3D80]   655KB of 16384KB -   4 percent complete.
- Reading Flash [0x00CCD00]   819KB of 16384KB -   5 percent complete.
- Reading Flash [0x00F5C40]   983KB of 16384KB -   6 percent complete.
- Reading Flash [0x011EBC0]  1146KB of 16384KB -   7 percent complete.
- Reading Flash [0x0147B00]  1310KB of 16384KB -   8 percent complete.
- Reading Flash [0x0170A40]  1474KB of 16384KB -   9 percent complete.
- Reading Flash [0x01999C0]  1638KB of 16384KB -  10 percent complete.
- Reading Flash [0x01C2900]  1802KB of 16384KB -  11 percent complete.
- Reading Flash [0x01EB880]  1966KB of 16384KB -  12 percent complete.
- Reading Flash [0x02147C0]  2129KB of 16384KB -  13 percent complete.
- Reading Flash [0x023D740]  2293KB of 16384KB -  14 percent complete.
- Reading Flash [0x0266680]  2457KB of 16384KB -  15 percent complete.
- Reading Flash [0x028F600]  2621KB of 16384KB -  16 percent complete.
- Reading Flash [0x02B8540]  2785KB of 16384KB -  17 percent complete.
- Reading Flash [0x02E1480]  2949KB of 16384KB -  18 percent complete.
- Reading Flash [0x030A400]  3113KB of 16384KB -  19 percent complete.
- Reading Flash [0x0333340]  3276KB of 16384KB -  20 percent complete.
- Reading Flash [0x035C2C0]  3440KB of 16384KB -  21 percent complete.
- Reading Flash [0x0385200]  3604KB of 16384KB -  22 percent complete.
- Reading Flash [0x03AE180]  3768KB of 16384KB -  23 percent complete.
- Reading Flash [0x03D70C0]  3932KB of 16384KB -  24 percent complete.
- Reading Flash [0x0400000]  4096KB of 16384KB -  25 percent complete.
- Reading Flash [0x0428F80]  4259KB of 16384KB -  26 percent complete.
- Reading Flash [0x0451EC0]  4423KB of 16384KB -  27 percent complete.
- Reading Flash [0x047AE40]  4587KB of 16384KB -  28 percent complete.
- Reading Flash [0x04A3D80]  4751KB of 16384KB -  29 percent complete.
- Reading Flash [0x04CCD00]  4915KB of 16384KB -  30 percent complete.
- Reading Flash [0x04F5C40]  5079KB of 16384KB -  31 percent complete.
- Reading Flash [0x051EBC0]  5242KB of 16384KB -  32 percent complete.
- Reading Flash [0x0547B00]  5406KB of 16384KB -  33 percent complete.
- Reading Flash [0x0570A40]  5570KB of 16384KB -  34 percent complete.
- Reading Flash [0x05999C0]  5734KB of 16384KB -  35 percent complete.
- Reading Flash [0x05C2900]  5898KB of 16384KB -  36 percent complete.
- Reading Flash [0x05EB880]  6062KB of 16384KB -  37 percent complete.
- Reading Flash [0x06147C0]  6225KB of 16384KB -  38 percent complete.
- Reading Flash [0x063D740]  6389KB of 16384KB -  39 percent complete.
- Reading Flash [0x0666680]  6553KB of 16384KB -  40 percent complete.
- Reading Flash [0x068F600]  6717KB of 16384KB -  41 percent complete.
- Reading Flash [0x06B8540]  6881KB of 16384KB -  42 percent complete.
- Reading Flash [0x06E1480]  7045KB of 16384KB -  43 percent complete.
- Reading Flash [0x070A400]  7209KB of 16384KB -  44 percent complete.
- Reading Flash [0x0733340]  7372KB of 16384KB -  45 percent complete.
- Reading Flash [0x075C2C0]  7536KB of 16384KB -  46 percent complete.
- Reading Flash [0x0785200]  7700KB of 16384KB -  47 percent complete.
- Reading Flash [0x07AE180]  7864KB of 16384KB -  48 percent complete.
- Reading Flash [0x07D70C0]  8028KB of 16384KB -  49 percent complete.
- Reading Flash [0x0800000]  8192KB of 16384KB -  50 percent complete.
- Reading Flash [0x0828F80]  8355KB of 16384KB -  51 percent complete.
- Reading Flash [0x0851EC0]  8519KB of 16384KB -  52 percent complete.
- Reading Flash [0x087AE40]  8683KB of 16384KB -  53 percent complete.
- Reading Flash [0x08A3D80]  8847KB of 16384KB -  54 percent complete.
- Reading Flash [0x08CCD00]  9011KB of 16384KB -  55 percent complete.
- Reading Flash [0x08F5C40]  9175KB of 16384KB -  56 percent complete.
- Reading Flash [0x091EBC0]  9338KB of 16384KB -  57 percent complete.
- Reading Flash [0x0947B00]  9502KB of 16384KB -  58 percent complete.
- Reading Flash [0x0970A40]  9666KB of 16384KB -  59 percent complete.
- Reading Flash [0x09999C0]  9830KB of 16384KB -  60 percent complete.
- Reading Flash [0x09C2900]  9994KB of 16384KB -  61 percent complete.
- Reading Flash [0x09EB880] 10158KB of 16384KB -  62 percent complete.
- Reading Flash [0x0A147C0] 10321KB of 16384KB -  63 percent complete.
- Reading Flash [0x0A3D740] 10485KB of 16384KB -  64 percent complete.
- Reading Flash [0x0A66680] 10649KB of 16384KB -  65 percent complete.
- Reading Flash [0x0A8F600] 10813KB of 16384KB -  66 percent complete.
- Reading Flash [0x0AB8540] 10977KB of 16384KB -  67 percent complete.
- Reading Flash [0x0AE1480] 11141KB of 16384KB -  68 percent complete.
- Reading Flash [0x0B0A400] 11305KB of 16384KB -  69 percent complete.
- Reading Flash [0x0B33340] 11468KB of 16384KB -  70 percent complete.
- Reading Flash [0x0B5C2C0] 11632KB of 16384KB -  71 percent complete.
- Reading Flash [0x0B85200] 11796KB of 16384KB -  72 percent complete.
- Reading Flash [0x0BAE180] 11960KB of 16384KB -  73 percent complete.
- Reading Flash [0x0BD70C0] 12124KB of 16384KB -  74 percent complete.
- Reading Flash [0x0C00000] 12288KB of 16384KB -  75 percent complete.
- Reading Flash [0x0C28F80] 12451KB of 16384KB -  76 percent complete.
- Reading Flash [0x0C51EC0] 12615KB of 16384KB -  77 percent complete.
- Reading Flash [0x0C7AE40] 12779KB of 16384KB -  78 percent complete.
- Reading Flash [0x0CA3D80] 12943KB of 16384KB -  79 percent complete.
- Reading Flash [0x0CCCD00] 13107KB of 16384KB -  80 percent complete.
- Reading Flash [0x0CF5C40] 13271KB of 16384KB -  81 percent complete.
- Reading Flash [0x0D1EBC0] 13434KB of 16384KB -  82 percent complete.
- Reading Flash [0x0D47B00] 13598KB of 16384KB -  83 percent complete.
- Reading Flash [0x0D70A40] 13762KB of 16384KB -  84 percent complete.
- Reading Flash [0x0D999C0] 13926KB of 16384KB -  85 percent complete.
- Reading Flash [0x0DC2900] 14090KB of 16384KB -  86 percent complete.
- Reading Flash [0x0DEB880] 14254KB of 16384KB -  87 percent complete.
- Reading Flash [0x0E147C0] 14417KB of 16384KB -  88 percent complete.
- Reading Flash [0x0E3D740] 14581KB of 16384KB -  89 percent complete.
- Reading Flash [0x0E66680] 14745KB of 16384KB -  90 percent complete.
- Reading Flash [0x0E8F600] 14909KB of 16384KB -  91 percent complete.
- Reading Flash [0x0EB8540] 15073KB of 16384KB -  92 percent complete.
- Reading Flash [0x0EE1480] 15237KB of 16384KB -  93 percent complete.
- Reading Flash [0x0F0A400] 15401KB of 16384KB -  94 percent complete.
- Reading Flash [0x0F33340] 15564KB of 16384KB -  95 percent complete.
- Reading Flash [0x0F5C2C0] 15728KB of 16384KB -  96 percent complete.
- Reading Flash [0x0F85200] 15892KB of 16384KB -  97 percent complete.
- Reading Flash [0x0FAE180] 16056KB of 16384KB -  98 percent complete.
- Reading Flash [0x0FD70C0] 16220KB of 16384KB -  99 percent complete.
- Reading Flash [0x1000000] 16384KB of 16384KB - 100 percent complete.

Writing flash contents to file "All_regions.bin"...
Memory Dump Complete
FPT Operation Successful.

