C:\Users\my pc\Downloads\Intel CSME System Tools v11 r14 (1)\Intel CSME System T

ools v11 r14\MEInfo\WIN64>meinfowin64

Intel(R) MEInfo Version: 11.8.55.3510

Copyright(C) 2005 - 2017, Intel Corporation. All rights reserved.

Intel(R) Manageability and Security Application code versions:

BIOS Version N11 Ver. 02.30

MEBx Version 11.0.0.0005

GbE Version 0.8

Vendor ID 8086

PCH Version 31

FW Version 11.6.20.1221 H

Security Version (SVN) 1

LMS Version Not Available

MEI Driver Version 11.0.0.1172

Wireless Hardware Version Not Available

Wireless Driver Version Not Available

FW Capabilities 0x5DFE5147

Intel(R) Active Management Technology - PRESENT/ENABLED

 Intel(R) Capability Licensing Service - PRESENT/ENABLED

Protect Audio Video Path - PRESENT/ENABLED

 Intel(R) Dynamic Application Loader - PRESENT/ENABLED

Service Advertisement & Discovery - PRESENT/ENABLED

Re-key needed False

Platform is re-key capable True

Intel(R) AMT State Enabled

TLS Enabled

Last ME reset reason Global system reset

Local FWUpdate Enabled

BIOS Config Lock Enabled

GbE Config Lock Enabled

Host Read Access to ME Disabled

Host Write Access to ME Disabled

Host Read Access to EC Enabled

Host Write Access to EC Enabled

SPI Flash ID 1 EF4018

SPI Flash ID 2 Unknown

BIOS boot State Post Boot

OEM ID 00000000-0000-0000-0000-000000000000

Link Status Link Down

System UUID 2dcc5296-50f9-11e7-9c43-bc00009c0000

MAC Address 00-25-ab-a8-2c-bd

IPv4 Address 0.0.0.0

IPv6 Enablement Disabled

Privacy/Security Level Default

Configuration State Not Started

Provisioning Mode PKI

Capability Licensing Service Enabled

OEM Tag 0x00000000

Slot 1 Board Manufacturer 0x00000000

Slot 2 System Assembler 0x00000000

Slot 3 Reserved 0x00000000

M3 Autotest Disabled

C-link Status Enabled

Wireless Micro-code Mismatch No

Wireless Micro-code ID in Firmware 0x24F3

Wireless LAN in Firmware Intel(R) Dual Band Wireless-AC 8260

Wireless Hardware ID No Intel WLAN card installed

Wireless LAN Hardware No Intel WLAN card installed

Localized Language English

Independent Firmware Recovery Disabled

EPID Group ID 0xFEB

LSPCON Ports None

5K Ports None

OEM Public Key Hash FPF 00000000000000000000000000000000000

00000000000000000000000000000

OEM Public Key Hash ME 00000000000000000000000000000000000

00000000000000000000000000000

ACM SVN FPF 0x0

KM SVN FPF 0x0

BSMM SVN FPF 0x0

GuC Encryption Key FPF 00000000000000000000000000000000000

00000000000000000000000000000

GuC Encryption Key ME 00000000000000000000000000000000000

00000000000000000000000000000

 FPF ME

 --- --

Force Boot Guard ACM Disabled Disabled

Protect BIOS Environment Disabled Disabled

CPU Debugging Enabled Enabled

BSP Initialization Enabled Enabled

Measured Boot Disabled Disabled

Verified Boot Disabled Disabled

Key Manifest ID 0x0 0x0

Enforcement Policy 0x0 0x0